# Nmap service detection probe list -*- mode: fundamental; -*-
# $Id: nmap-service-probes 24265 2011-06-23 06:19:48Z fyodor $ 
#
# This is a database of custom probes and expected responses that the
# Nmap Security Scanner ( http://nmap.org ) uses to
# identify what services (eg http, smtp, dns, etc.) are listening on
# open ports.  Contributions to this database are welcome.  We hope to
# create an automated submission system (as with OS fingerprints), but
# for now you can email fyodor any new probes you develop so that he
# can include them in the main Nmap distributon.  By sending new
# probe/matches to Fyodor or one the insecure.org development mailing
# lists, it is assumed that you are transfering any and all copyright
# interest in the data to Fyodor so that he can modify it, relicense
# it, incorporate it into programs, etc. This is important because the
# inability to relicense code has caused devastating problems for
# other Free Software projects (such as KDE and NASM).  Nmap will
# always be available Open Source.  If you wish to specify special
# license conditions of your contributions, just say so when you send
# them.
#
# This collection of probe data is (C) 1998-2010 by Insecure.Com
# LLC.  It is distributed under the Nmap Open Source license as
# provided in the COPYING file of the source distribution or at
# http://nmap.org/data/COPYING .  Note that this license
# requires you to license your own work under a compatable open source
# license.  If you wish to embed Nmap technology into proprietary
# software, we sell alternative licenses (contact sales@insecure.com).
# Dozens of software vendors already license Nmap technology such as
# host discovery, port scanning, OS detection, and version detection.
# For more details, see http://nmap.org/book/man-legal.html
#
# For details on how Nmap version detection works, why it was added,
# the grammar of this file, and how to detect and contribute new
# services, see http://nmap.org/book/vscan.html.

# The Exclude directive takes a comma separated list of ports.
# The format is exactly the same as the -p switch.
Exclude T:9100-9107

# This is the NULL probe that just compares any banners given to us
##############################NEXT PROBE##############################
Probe TCP NULL q||
# Wait for at least 6 seconds for data.  It used to be 5, but some
# smtp services have lately been instituting an artificial pause (see
# FEATURE('greet_pause') in Sendmail, for example)
totalwaitms 6000

match 4d-server m|^\0\0\0H\0\0\0\x02.[^\0]*\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0$|s p/4th Dimension database server/

match acap m|^\* ACAP \(IMPLEMENTATION \"CommuniGate Pro ACAP (\d[-.\w]+)\"\) | p/CommuniGate Pro ACAP server/ i/for mail client preference sharing/ v/$1/
match acmp m|^ACMP Server Version ([\w._-]+)\r\n| p/Aagon ACMP Inventory/ v/$1/
match activemq m|^\0\0\0.\x01ActiveMQ\0\0\0|s p/Apache ActiveMQ/

# Microsoft ActiveSync Version 3.7 Build 3083 (It's used for syncing
# my ipaq it disapears when you remove the ipaq.)
match activesync m|^.\0\x01\0[^\0]\0[^\0]\0[^\0]\0[^\0]\0[^\0]\0.*\0\0\0$|s p/Microsoft ActiveSync/ o/Windows/
match activesync m|^\(\0\0\0\x02\0\0\0\x03\0\0\0\+\0\0\x003\0\0\0\0\0\0\0\x04\0\0`\x01\0\0\xff\0\0\0\0\0\0\0\0\0\0\0$|s p/Citrix ActiveSync/ o/Windows/

match adabas-d m|^Adabas D Remote Control Server Version ([\d.]+) Date [\d-]+ \(key is [0-9a-f]+\)\r\nOK> | p/Adabas D database remote control/ v/$1/

match adobe-crossdomain m|^<cross-domain-policy><allow-access-from domain='[^']*' to-ports='\d+' /></cross-domain-policy>\0$| p/Adobe cross-domain policy/

match ipmi-advertiserd m|^\x0e\0\0\0\0\0\0$| p/SuperMicro IPMI advertiserd/ d/remote management/

match altiris-agent m|^<\0r\0e\0s\0p\0o\0n\0s\0e\0>\0C\0o\0n\0n\0e\0c\0t\0e\0d\0 \0t\0o\0 [\0\d.]*<\0/\0r\0e\0s\0p\0o\0n\0s\0e\0>\0$| p/Altiris remote monitoring agent/

# AMANDA index server 2.4.2p2 on Linux 2.4
match amanda m|^220 ([-.\w]+) AMANDA index server \((\d[-.\w ]+)\) ready\.\r\n| p/Amanda backup system index server/ v/$2/ h/$1/ o/Unix/
match amanda m|^501 Could not read config file [^!\r\n]+!\r\n220 ([-.\w]+) AMANDA index server \(([-\w_.]+)\) ready\.\r\n| p/Amanda backup system index server/ v/$2/ h/$1/ i/broken: config file not found/
match amanda m|^ld\.so\.1: amandad: fatal: (libsunmath\.so\.1): open failed: No such file or directory\n$| p/Amanda backup system index server/ i/broken: $1 not found/

match antivir m|^220 Symantec AntiVirus Scan Engine ready\.\r\n| p/Symantec AntiVirus Scan Engine/
match antivir m|^200 NOD32SS ([\d.]+) \((\d+)\)\r\n| p/NOD32 AntiVirus/ v/$1 ($2)/

match anyremote m|^Set\(icons,M,6,forward,7,prev,8,stop,9,next,\*,question,0,pause,#,no\);Set\(font,small\);Set\(menu,replace,Playlist,Toggle Shuffle,Toggle Repeat\);Set\(icons,MPD,1,vol_down,2,mute,3,vol_up,4,rewind,5,play,6,forward,7,prev,8,stop,9,next,\*,question,0,pause,#,no\);Set\(font,small\);Set\(menu,replace,Playlist,Toggle Shuffle,Toggle Repeat\);$| p/anyRemote remote control daemon/

match aplus m|^\x01\xff\0\xff\x01\x1d\0\xfd\0\n\x03\x05A\+ API \(([\d.]+)\) - CCS \(([\d.]+)\)\0| p/Cleo A+/ i/API $1; CSS $2/
match app m|^\0\x01\0\x08\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\x01\0\0\0\x02$| p/Cisco Application Peering Protocol/ d/load balancer/

# http://www.qosient.com/argus/
match argus m|^\x80\x01\0\x80\0\x80\0\0\xe5az\xcb\0\0\0\0J...............\x02\0\x01\0\0<\x01,.......\0...\0\0\0\0\x01\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\xff\xff\xff\xff\x01\x04\0.\0\x80\x08|s p/Argus network analyzer/ v/3.0/

match arkeia m|^\0`\0\x04\0\0\0\x1810\x000\x000\x00852224\0\0\0\0\0\0\0\0\0\0\0$| p/Arkeia Network Backup/
# arkstats (part of arkeia-light 5.1.12 Backup server) on Linux 2.4.20
match arkstats m|^\0`\0\x03\0\0\0\x1810\x000\x000\x00852224\0\0\0\0\0\0\0\0\0\0\0| p/Arkeia arkstats/
match artsd m|^MCOP\0\0\0.\0\0\0\x01\0\0\0\x10aRts/MCOP-([\d.]+)\0\0\0\0|s p/artsd/ i/MCOP $1/

# Asterisk call manager - port 5038
match asterisk m|^Asterisk Call Manager/([\d.]+)\r\n| p/Asterisk Call Manager/ v/$1/
match asterisk-proxy m|^Response: Follows\r\nPrivilege: Command\r\n--END COMMAND--\r\n| p/Asterisk Call Manager Proxy/

match audit m|^Visionsoft Audit on Demand Service\r\nVersion: ([\d.]+)\r\n\r\n| p/Visionsoft Audit on Demand Service/ v/$1/ o/Windows/
match autosys m|^([\w._-]+)\nListener for [\w._-]+ AutoSysAdapter\nEOS\nExit Code = 1001\nIP <[\d.]+> is not authorized for this request\. Please contact your Web Administrator\.\nEOS\n| p/CA AutoSys RCS Listener/ v/$1/ i/not authorized/
match avg m|^220-AVG7 Anti-Virus daemon mode scanner\r\n220-Program version ([\d.]+), engine (\d+)\r\n220-Virus Database: Version ([\d/.]+)  [-\d]+\r\n| p/AVG daemon mode/ v/$1 engine $2/ i/Virus DB $3/
match avg m=^220-AVG daemon mode scanner \((?:AVG|SMTP)\)\r\n220-Program version ([\w._-]+)\r\n220-Virus Database: Version ([\w._/ -]+)\r\n220 Ready\r\n= p/AVG daemon mode/ v/$1/ i/Virus DB $2/

match afbackup m|^afbackup ([\d.]+)\n\nAF's backup server ready\.\n| p/afbackup/ v/$1/
match afbackup m|^.*, Warning on encryption key file `/etc/afbackup/cryptkey': File not readable\.\n.*, Warning: Ignoring file `/etc/afbackup/cryptkey', using compiled-in key\.\nafbackup 3\.4\n\nAF's backup server ready\.\n\x9d\x84\x0bZ$| p/afbackup/ i/using compiled-in key/

match backdoor m|^220 jeem\.mail\.pv ESMTP\r\n| p/Jeem backdoor/ i/**BACKDOOR**/ o/Windows/
match backdoor m|^\r\nUser Access Verification\r\n\r\nYour PassWord:| p/Jeem backdoor/ i/**BACKDOOR**/ o/Windows/
match backdoor m|^ \r\n$| p/OptixPro backdoor/ i/**BACKDOOR**/ o/Windows/
match backdoor m|^echo o [\d.]+ \d+ >s\r\necho common>> s\r\necho common>> s\r\necho bin>> s\r\necho get m220\.exe| p/JTRAM backdoor/ i/**BACKDOOR**/ o/Windows/
match backdoor m|^220 Bot Server \(Win32\)\r\n$| p/Gaobot backdoor/ i/**BACKDOOR**/ o/Windows/
match backdoor m|^PWD$| p/Subseven backdoor/ i/**BACKDOOR**/ o/Windows/
match backdoor m|^\r\n\[RPL\]002\r\n$| p/Subseven backdoor/ i/**BACKDOOR**/
match backdoor m|^=+\n= +RBackdoor ([\d.]+) | p/RBackdoor/ v/$1/ i/**BACKDOOR**/ o/Windows/
match backdoor m|^220 Windrone Server \(Win32\)\r\n$| p/NerdBot backdoor/ i/**BACKDOOR**/ o/Windows/
match backdoor m|^Zadej heslo:$| p/Czech "zadej heslo" backdoor/ i/**BACKDOOR**/ o/Windows/
match backdoor m|^220 Reptile welcomes you\.\.\r\n| p/Darkmoon backdoor "reptile" ftpd/ i/**BACKDOOR**/ o/Windows/
match backdoor m|^Sifre_EDIT$| p/ProRat trojan/ i/**BACKDOOR**/ o/Windows/
match backdoor m|^MZ\x90\0\x03\0\0\0\x04\0\0\0\xff\xff\0\0\xb8\0\0\0\0\0\0\0@\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0fn\0\0\xd0\0\0\0\x0e\x1f\xba\x0e\0\xb4\t\xcd!\xb8\x01L\xcd!This program cannot be run in DOS mode\.| p/Korgo worm/ i/**BACKDOOR**/ o/Windows/
match backdoor m|^\xfa\xcb\xd9\xd9\xdd\xc5\xd8\xce\xd6| p/Theef trojan/ i/**BACKDOOR**/ o/Windows/
match backdoor m|^220 SSL Connection Established - Loading Protocol\.\.\.\.\r\n| p/dhcpse.exe/ i/**BACKDOOR**/ o/Windows/
match backdoor m|^A-311 Death welcome\x001| p/Haxdoor trojan/ i/**BACKDOOR**/ o/Windows/
match backdoor m|^220 CAFEiNi [-\w_.]+ FTP server\r\n$| p/CAFEiNi trojan/ i/**BACKDOOR**/ o/Windows/
match backdoor m/^220 (Stny|fuck)Ftpd 0wns j0\r?\n/ p/Kibuv.b worm/ i/**BACKDOOR**/ o/Windows/
match backdoor m|^220 [Sf.][tu.][nc.][yk.][.F][t.][p.][d.] [0.][w.][n.][s.] [j.][0.]\r?\n|i p/Generic Kibuv worm/ i/**BACKDOOR**/ o/Windows/
match backdoor m=^(?:ba|)sh-([\d.]+)\$ = p/Bourne shell/ i/**BACKDOOR**/ v/$1/
match backdoor m=^exec .* failed : No such file or directory\n$= p/netcat -e/ i/misconfigured/
match backdoor m=220-Welcome!\r\n220-\x1b\[30m/\x1b\[31m#\xa4#\xa4#\xa4#\xa4#\xa4#\xa4#\xa4#\xa4#\xa4#\xa4#\xa4#\xa4#\xa4#\xa4#\xa4#\xa4#\xa4#\xa4#\xa4#\xa4#\xa4#\xa4#\xa4#\xa4#\xa4#                                                         \r\n220-\x1b\[30m\|          Current Time:  \x1b\[35m[^\r\n]*\r\n220-\x1b\[30m\|          Current Date:  \x1b\[35m[^\r\n]*\r\n220-\x1b\[30m\\\r\n= p/Windows trojan/ i/**BACKDOOR**/ o/Windows/

match bandwidth-test m|^\x01\0\0\0$| p/Mikrotik bandwidth-test server/

match barracuda-dcagent m|^Invalid Client IP\0\0$| p/Barracuda Domain Controller Agent/

match bf2rcon m|^### Battlefield 2 ModManager Rcon v([\d.]+)\.\n### Digest seed: \w+\n\n| p/Battlefield 2 ModManager Remote Console/ v/$1/

# Version 0.3.19 protocol
#  4 bytes magic number:   "\xf9\xbe\xb4\xd9"
# 12 bytes command:        "version\0\0\0\0\0"
#  4 bytes length
#  4 bytes version
#  8 bytes nLocalServices: "\x01\0\0\0\0\0\0\0"
#  8 bytes nTime
#  8 bytes client nServices "\x01\0\0\0\0\0\0\0"
# 16 bytes IPv4-compatible client IP "\0\0\0\0\0\0\0\0\0\0\xff\xff...."
#  2 bytes client port
#  8 bytes server nServices "\x01\0\0\0\0\0\0\0"
# 16 bytes IPv4-compatible server IP "\0\0\0\0\0\0\0\0\0\0\xff\xff...."
#  2 bytes server port
#  8 bytes nonce
#  1 byte  SubVer length
# variable SubVer string
#  4 bytes nBestHeight

# Version 0xc8 -> 200 -> 0.2.0
match bitcoin m|^\xf9\xbe\xb4\xd9version\0\0\0\0\0\x51\0\0\0\xc8\0\0\0\x01\0\0\0\0\0\0\0........\x01\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\xff\xff......\x01\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\xff\xff..............\0$|s p/Bitcoin digital currency server/ v/0.2.0/
# Version 0x12c -> 300 -> 0.3.0
match bitcoin m|^\xf9\xbe\xb4\xd9version\0\0\0\0\0\x55\0\0\0\x2c\x01\0\0\x01\0\0\0\0\0\0\0........\x01\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\xff\xff......\x01\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\xff\xff..............\0....$|s p/Bitcoin digital currency server/ v/0.3.0/
# Version 0x136 -> 310 -> 0.3.10
match bitcoin m|^\xf9\xbe\xb4\xd9version\0\0\0\0\0\x57\0\0\0\x36\x01\0\0\x01\0\0\0\0\0\0\0........\x01\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\xff\xff......\x01\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\xff\xff..............\0....$|s p/Bitcoin digital currency server/ v/0.3.10/
match bitcoin m|^\xf9\xbe\xb4\xd9version\0\0\0\0\0\x57\0\0\0\x36\x01\0\0\x01\0\0\0\0\0\0\0........\x01\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\xff\xff......\x01\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\xff\xff..............\x02(\..)....$|s p/Bitcoin digital currency server/ v/0.3.10$1/
# Version 0x7c9c -> 31900 -> 0.3.19
match bitcoin m|^\xf9\xbe\xb4\xd9version\0\0\0\0\0\x55\0\0\0\x9c\x7c\0\0\x01\0\0\0\0\0\0\0........\x01\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\xff\xff......\x01\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\xff\xff..............\0....$|s p/Bitcoin digital currency server/ v/0.3.19/
match bitcoin m|^\xf9\xbe\xb4\xd9version\0\0\0\0\0\x55\0\0\0\x9c\x7c\0\0\x01\0\0\0\0\0\0\0........\x01\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\xff\xff......\x01\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\xff\xff..............\x02(\..)....$|s p/Bitcoin digital currency server/ v/0.3.19$1/

# Bittorrent Client 3.2.1b on Linux 2.4.X
match bittorrent m|^\x13BitTorrent protocol\0\0\0\0\0\0\0\0| p/Bittorrent P2P client/
# BMC Software Patrol Agent 3.45 and HP Patrol Agent
match softwarepatrol m|^\0\0\0\x17i\x02\x03..\0\x05\x02\0\x04\x02\x04\x03..\0\x03\x04\0\0\0|s p|BMC/HP Software Patrol Agent|
match scmbug m|^SCMBUG-SERVER RELEASE_([-\w_.]+) \d+\n| p/Scmbug bugtracker/ v/$1/

# Tolis BRU (Backup and Restore Utility)
match bru m|^0x[0-9a-fA-F]{32}L| p/Tolis BRU/ i/Backup and Restore Utility/

# Bruker AXS X-ray machines (how cool is that!?!?) (Brandon)
match bruker-axs m|^\[ANGLESTATUS.*\[XYZSTATUS.*\[ZOOMSTATUS.*\[INSTRUMENTSTATUS.*XRAYSON=1|s p/Bruker AXS X-ray controller status/ i/X-rays: On/ d/specialized/
match bruker-axs m|^\[ANGLESTATUS.*\[XYZSTATUS.*\[ZOOMSTATUS.*\[INSTRUMENTSTATUS.*XRAYSON=0|s p/Bruker AXS X-ray controller status/ i/X-rays: Off/ d/specialized/

match buildservice m|^200 HELLO - BuildForge Agent v([\w._-]+)\n| p/BuildForge Agent/ v/$1/
match buildservice m|^\$\0\0\0\$\0\0\x000RAR\0 \0\0.\xe2\x02\0\xc4G\x0f\0\0\0\0\0\0\0\0\0\0\0\0\0|s p/Xoreax IncrediBuild/ o/Windows/

match burk-autopilot m|^\x19\0\0\0\0\0\x0f\xbeB!\x012\x02\xd1\x02\x032\x02p\0\x062\x02\x80\0$| p/Burk AutoPilot Plus remote management/ d/remote management/

match bzfs m|BZFS\d{4}\0| p/BZFlag game server/

# CA Message Queueing Server (Tom Sellers)
match ca-mq m|^ACK\x01| p/CA Message Queuing Server/

match ca-unicenter m|^\x8d\0\0\0\x8d\0\0\0\x100\x81\x89\x02\x81\x81\0.*\x02\x03\x01\0\x01\0$| p/CA Unicenter remote control/

match caicci m|^\x02\x07\x04\0\xe0\0\0\0\0\0\0\0\0\0\0\0\x02\0\0\0\0\0\0\0\x04\x03\x02\x010\0\0\0\0\0\0\0\x01\0\0\0\x01\0\0\0\xe0\0\0\0\0\0\0\0\0\x80\0\0\0\x80\0\0\0ems-p-sp\0\0\0\0\0\0\0\0\x01\0\0\0\0\0\0\0\0\0\0\x12\x01\0\0EMS-P-SPO-01\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0EMS-P-SPO-01\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0$| p/CAI-CCI/

match cccam m|^Welcome to the CCcam information client\.\n| p/CCcam DVR card sharing system information/

match cddbp m|^201 ([-\w_.]+) CDDBP server v([-\w.]+) ready at .*\r\n| p/freedb cddbp server/ v/$2/ h/$1/
match chargen m|^!"#\$%\&'\(\)\*\+,-\./0123456789:;<=>\?\@ABCDEFGHIJKLMNOPQRSTUVWXYZ\[\\\]\^_`abcdefgh\r\n"#\$%\&'\(\)\*\+,-\./0123456789:;<=>\?\@ABCDEF| p/Linux chargen/ o/Linux/
# Redhat 7.2, xinetd 2.3.7 chargen
match chargen m|^\*\+,-\./0123456789:;<=>\?@ABCDEFGHIJKLMNOPQRSTUVWXYZ\[\\\]\^_`abcdefghijklmnopq\r\n\+,-\./| p/xinetd chargen/ o/Unix/
# Sun Solaris 9; Windows
match chargen m|^\ !"#\$%&'\(\)\*\+,-\./0123456789:;<=>\?@ABCDEFGHIJKLMNOPQRSTUVWXYZ\[\\\]\^_|
# Mandrake Linux 9.2, xinetd 2.3.11 chargen
match chargen m|NOPQRSTUVWXYZ\[\\\]\^_`abcdefghijklm| p/xinetd chargen/ o/Unix/
match chargen m|^\*\*\* Port V([\d.]+) !\"#\$%&'\(\)\*\+,-\./0123456789:| p/Lantronix chargen/ v/$1/
match chargen m|^The quick brown fox jumps over the lazy dog\. 1234567890\r\n| p/Tektronix Phaser chargen/ d/printer/

match chat m|^WebStart Chat Service Established\.\.\.\r\n\(C\) 2000-\d+ R Gabriel all Rights Reserved\r\n| p/WebStart Chat Service/
match chat m|^\*\x01..\0\x04\0\0\0\x01$|s p/AIM or ICQ server/
match chat-ctrl m|^InfoChat Server v([\d.]+) Remote Control ready\n\r| p/InfoChat Remote Control/ v/$1/
match chess m=^\n\r             _       __     __                             __      \n\r            \| \|     / /__  / /________  ____ ___  ___     / /_____ \n\r            \| \| /\| / / _ \\/ / ___/ __ \\/ __ `__ \\/ _ \\   / __/ __ \\\n\r= p/Lasker Internet Chess server/

match chilliworx m|^ChilliSVC ([\d.]+)\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0| p/ChilliWorx management console/ v/$1/ d/remote management/

# Citadel/UX. Maybe to change the service name and to move somewhere else? embyte
match citadel m|^200.*Citadel(?:/UX)?| p/Citadel (UX) messaging server/
# Citrix, Metaframe XP on Windows
match citrix-ica m|^\x7f\x7fICA\0\x7f\x7fICA\0| p/Citrix Metaframe XP ICA/ o/Windows/
# Citrix MetaFrame XP 1.0 implimented with ClassLink 2000 on NT4
match citrix-ima m|^.\0\0\0\x81\0\0\0\x01|s p/Citrix Metaframe XP IMA/ o/Windows/
match clsbd m|^\0\0\0\x10ClsBoolVersion 1$| p/Cadence IC design daemon/
match codeforge m|^CFMSERV\(1\)\n| p/CodeForge IDE/
match concertosendlog m|^Concerto Software\r\n\r\nEnsemblePro SendLog Server - Version (\d[-.\w]+)\r\n\r\nEnter Telnet Password\r\n#> | p/Concerto Software EnsemblePro CRM software SendLog Server/ v/$1/
match concertotimesync m|^Concerto Software\r\n\r\nContactPro TimeSync Server - Version (\d[-.\w]+)\r\n\r\nEnter Telnet Password\r\n#> | p/Concerto Software EnsemblePro CRM software TimeSync Server/ v/$1/
match conference m|^Conference, V([\d.]+)\r\n$| p/Forum Communcations conferenced/ v/$1/
match complex-link m|^\x06\x07\xd0\0\x01\0\0\0\x01\0\x02\x07\xd0\0\x01\0\0\x01\x0f\x01\xf4\0\0\0\0HP +LTO ULTRIUM| p/HP LTO Ultrium data port/ d/storage-misc/

# Commvault Backup Server (CommVault Galaxy(R) Data Protection)
match commvault m/^\0\0\0\t\0\0\0\|\0\0\0/ p/CommVault Galaxy data backup/

match compuware-lm m|^Hello, I don't understand your request\.  Good bye\.\.\.\. $| p/Compuware Distributed License Management/

# PacketCable COPS Client-Open
match cops m|^\x10\x06\x80\x08......\x0b\x01([\w._-]+)\0|s p/Common Open Policy Service (COPS)/ h/$1/

# This port uses a binary protocol: [esc]X@ query OS version, [esc]XA query hardware
match crestron-control m|^Crestron Terminal Protocol Console opened\r\n| p/Crestron Terminal Console/ i/Crestron CNMSX-AV automation system/
match crestron-control m|^\r\nCrestron Terminal Protocol Console Opened\r\n\r\n| p/Crestron Terminal Console/

# XSig allows communcation with a Crestron control system.
match crestron-xsig m|^\x0f\0\x01\x02$| p/Crestron PRO2 XSig communication/

match csync m|\* OK ([-.\w]+) Cyrus sync server v([-.\w]+)| p/Cyrus sync server/ h/$1/ v/$2/

match cvspserver m|^no repository configured in /| p/CVS pserver/ i/broken/
match cvspserver m|^/usr/sbin/cvs-pserver: line \d+: .*cvs: No such file or directory\n| p/CVS pserver/ i/broken/
match cvspserver m|^Unknown command: `pserver'\n\nCVS commands are:\n| p/CVS pserver/ i/broken/

match cvsup m|^OK \d+ \d+ ([-.\w]+) CVSup server ready\n| p/CVSup/ v/$1/

match damewaremr m|^0\x11\0\0...........@........\x01\0\0\0\x01\0\0\0\0\0\0\0.\0\0\0$|s p/DameWare Mini Remote Control/ o/Windows/
# Linux
match daytime m=^[0-3]\d [A-Z][A-Z][A-Z] (?:19|20)\d\d \d\d:\d\d:\d\d \S+\r\n=
# OpenBSD 3.2
match daytime m=^[A-Z][a-z]{2} [A-Z][a-z]{2} +\d{1,2} +\d\d:\d\d:\d\d (?:19|20)\d\d\r\n= o/Unix/
# Solaris 8,9
match daytime m=^[A-Z][a-z]{2} [A-Z][a-z]{2} +\d{1,2} +\d\d:\d\d:\d\d (?:19|20)\d\d\n\r= p/Sun Solaris daytime/ o/Solaris/
# Windows daytime
match daytime m=^\d+:\d\d:\d\d [AP]M \d+/\d+/(?:19|20)\d\d\n$= p/Microsoft Windows USA daytime/ o/Windows/
# Windows daytime - UK english I think (no AM/PM)
match daytime m=^\d\d:\d\d:\d\d \d\d?.\d\d?.(?:19|20)\d\d\n$= p/Microsoft Windows International daytime/ o/Windows/
# daytime on Windows 2000 Server
match daytime m=^.... \d{1,2}:\d{1,2}:\d{1,2} (?:19|20)\d\d-\d{1,2}-\d{1,2}\n$= p/Microsoft Windows daytime/ o/Windows/
# Windows NT daytime
match daytime m=^[A-Z][a-z]+day, [A-Z][a-z]+ \d{1,2}, (?:19|20)\d\d \d{1,2}:\d\d:\d\d\n\0$= p/Microsoft Windows daytime/ o/Windows/
# Windows 2000 Adv Server sp-4 daytime
match daytime m=^[A-Z][a-z][a-z] [A-Z][a-z][a-z] \d{1,2} \d{1,2}:\d{1,2}:\d{1,2} (?:19|20)\d\d\n= p/Microsoft Windows daytime/ o/Windows/
# Windows 2003 Server daytme
match daytime m=^\d{1,2}\.\d{1,2}\.\d{1,2} \d\d/\d\d/(?:19|20)\d\d\n= p/Microsoft Windows daytime/ o/Windows/
# Windows 2000 Prof. Central European format
match daytime m=^\d{1,2}:\d\d:\d\d \d{1,2}[/.]\d{1,2}[/.]\d{4}\n$= p/Microsoft Windows daytime/ o/Windows/
match daytime m=^\d{1,2}:\d\d:\d\d [ap]m \d{4}/\d\d/\d\d\n$= p/Microsoft Windows daytime/ o/Windows/
match daytime m=^\d{1,2}:\d\d:\d\d [ap]m \d{1,2}/\d{1,2}/\d{4}\n$= p/Microsoft Windows 2003 daytime/ o/Windows/
# South Africa localization.
match daytime m=^\d\d:\d\d:\d\d [AP]M \d\d\d\d/\d\d/\d\d\n$= p/Microsoft Windows 7 daytime/

# Windows International daytime
match daytime m|^\d\d:\d\d:\d\d \d\d.\d\d.20\d\d\n$| p/Microsoft Windows International daytime/ o/Windows/
# New Zealand format daytime - Windows 2000
match daytime m|^[01]\d:\d\d:\d\d [AP]M [0-3]\d/[01]\d/0\d\n$| p/Microsoft Windows daytime/ i/New Zealand style/ o/Windows/
# HP-UX B.11.00 A inetd daytime
match daytime m|^[A-Z][a-z]{2} [A-Z][a-z]{2} +\d{1,2} \d\d:\d\d:\d\d [A-Z]+ 20\d\d\r\n$| p/HP-UX daytime/ o/HP-UX/
# Tardis 2000 v1.4 on NT
match daytime m|^[A-Z][a-z]{2} [A-Z][a-z]{2} +\d{1,2} \d\d:\d\d:\d\d 20\d\d $| p/Tardis 2000 daytime/
match daytime m|^\d+ \d\d-\d\d-\d\d \d\d:\d\d:\d\d 50 0 4 \d+\.0 UTC\(NIST\) \*\r\n| p/Greyware Domain Time II daytime/

# TrueTime nts100 running WxWorks
match daytime m|^[A-Z][a-z]{2}, [A-Z][a-z]{2} \d{1,2}, 20\d\d, \d\d:\d\d:\d\d-UTC$| p/TrueTime nts100/

# Cisco router daytime
match daytime m|^[A-Z][a-z]+day, [A-Z][a-z]+ \d{1,2}, \d{4} \d\d:\d\d:\d\d-\w\w\w(-DST)?\r\n| p/Cisco router daytime/ o/IOS/

match diablo2 m|^\xaf\x01$| p/Diablo 2 game server/

match dict m|^530 access denied\r\n$| p/dictd/ i/access denied/
match dict m|^220 ([-.\w]+) dictd ([-.\w/]+) on ([-.+ \w]+) <auth\.mime>| p/dictd/ h/$1/ v/$2/ o/$3/
match dict m|^220 hello <> msg\r\n$| p/Serpento dictd/

match directconnect m/^\$MyNick ([-.\w]+)|\$Lock/ p/Direct Connect P2P/ i/User: $1/ o/Windows/
match directconnect m|^\r\nDConnect Daemon v([\d.]+)\r\nlogin: | p/Direct Connect P2P/ v/$1/ o/Windows/
match directconnect m=<Hub-Security> Your IP is temporarily banned for (\d+) minutes\.\|= p/Shadows DirectConnect hub/ i/Banned for $1 minutes/
match directconnect m=<Hub-Security> You are being banned for (\d+) minutes \(by SDCH Anti Hammering\)\.\|= p/Shadows DirectConnect hub/ i/Banned for $1 minutes/
match directconnect m=<Hub-Security> You are being redirected to ([\d.]+)\|\$ForceMove [\d.]+\|= p/PtokaX directconnect hub/ i/Redirected to $1/
match directconnect m=^server-version\$([\w._-]+)\|init-completion\$200\|port\$\d+\|= p/Shakespeer Direct Connect GUI/ o/Mac OS X/
match directconnect-admin m=^\r\nOpen DC Hub, version ([\d.]+), administrators port\.\r\nAll commands begin with '\$' and end with '\|'\.\r\nPlease supply administrators passord\.\r\n= p/OpenDCHub directconenct hub admin port/ v/$1/ o/Unix/

match directupdate m|^OK Welcome <[\d.]+> on DirectUpdate server ([\d.]+)\r\n| p/DirectUpdate dynamic IP updater/ v/$1/
match directupdate m|^OK Welcome <[\d.]+> on DirectUpdate engine VER=\[([\d.]+) \(Build (\d+)\)\]-0x\w+\r\n| p/DirectUpdate dynamic IP updater/ v/$1 build $2/

match diskmonitor m|^000001a2[0-9a-f]{410}\r\n| p/Active@ Hard Disk Monitor/
match diskmonitor m|^0000019a[0-9a-f]{402}\r\n| p/Active@ Hard Disk Monitor/

match dlmtp m|^220 DSPAM DLMTP ([\w._-]+) Authentication Required\r\n| p/DSPAM dlmtpd/ v/$1/

match durian m|^<c5>Durian Web Application Server III<c4> ([^<]+)<c0> for Win32\r| p/Durian Web Application Server III/ v/$1/ o/Windows/

match dnsix m|^DNSIX$|
match dragon m|^UNAUTHORIZED\n\r\n\r$| p/Dragon realtime shell/
match drweb m|^0 PROTOCOL 2 [23] AGENT,CONSOLE,INSTALL| p/DrWeb/

match dynast-solver m|^DYNAST server v(.*) \(Win32\) - Copyright\(c\) DYN| p/DYNAST solver/ v/$1/ o/Windows/

match echolink m|^[0-9a-f]{8}$| p/EchoLink/

match enemyterritory m|^Welcome [\d.]+\. You have 15 seconds to identify\.\r\n| p/Enemy Territory Admin Mod/

match efi-webtools m|^\?p\xf7/Zq\xa2\xf5\x03.......\xf4\xea.......B$| p/EFI Fiery WebTools communication/
match efi-workstation m|^\(m\xe9l@k\xb7\xf5\x03$| p/EFI Fiery Command WorkStation/
match efi-workstation m|^\(m\xe9l@k\xb3\xf7\x1e\xa5$| p/EFI Fiery Command WorkStation/
match efi-workstation m|^\(m\xe9l@k\xb1\xf1\x15\xa5$| p/EFI Fiery Command WorkStation/

match eftserv m|^\?\x008 \xc3p EFTSRV1                                 ([\d.]+) | p/Ingenico EFTSRVd/ v/$1/ o/Windows/
match ericom m|^Ericom GCS v([\d.]+)\0| p/Ericom PowerTermWebConnect/ v/$1/ o/Windows/
match eggdrop m=^\r\n\r\n([-`|.\w]+)  \(Eggdrop v(\d[-.\w+]+) +\([cC]\) *1997.*\r\n\r\n= p/Eggdrop irc bot console/ v/$2/ i/botname: $1/
# These 2 fallbacks are because many people customize their eggdrop
# banners.  These rules should always be well below the detailed rule
# above.
match eggdrop m|\(Eggdrop v([\d.]+) \(C\) 1997 Robey Pointer.*Eggheads|s p/Eggdrop IRC bot console/ v/$1/
match eggdrop m|\(Eggdrop v([\d.]+)\+ipv6 \(C\) 1997 Robey Pointer.*Eggheads|s p/Eggdrop IRC bot console with ipv6/ v/$1/
match eggdrop m|\(Eggdrop v([\d.]+)\+SSL \(C\) 1997 Robey Pointer.*Eggheads|s p/Eggdrop IRC bot console with SSL/ v/$1/
match eggdrop m|\(Eggdrop v([\d.]+)\+rc(\d+) \(C\) 1997 Robey Pointer.*Eggheads|s p/Eggdrop IRC bot console/ v/$1 rc $2/
match eggdrop m=\(Eggdrop v([\d.]+)\+(STEALER\.net|Gentoo) \(C\) 1997 Robey Pointer.*Eggheads=s p/Eggdrop IRC bot console with Gentoo patches/ v/$1/ o/Linux/ i/Gentoo/

match eggdrop m|Copyright \(C\) 1997 Robey Pointer\r\n.*Eggheads| p/Eggdrop IRC bot console/

match enistic-manager m|^WZ=AAAAAAAAAAByAAE=73\r0E0000000000cgAD83\r$| p/Enistic Energy Manager/

match epp m|^\x00\x00\x03\x72<\?xml version=\"1\.0\" encoding=\"UTF-8\" standalone=\"no\" \?>\n<epp xmlns=\"http://www\.yoursrs\.com/xml/epp/epp-1\.0\" xmlns:xsi=\"http://www\.w3\.org/2001/XMLSchema-instance\" xsi:schemaLocation=\"http://www\.yoursrs\.com/xml/epp/epp-1\.0 epp-1\.0\.xsd\">\n\n  <greeting>\n    <svID>([^<]+)</svID>\n    <svDate>.*</svDate>\n    <svcMenu>\n      <version>([\w._-]+)</version>\n| p/Extensible Provisioning Protocol/ v/$2/ i/server name: $1/

match eve-online m|^7\0\0\0~\0\0\0\0\x14\x06\x04\xe8\x99\x02\0\x05\xeb\0\x04\xdf\x92\0\0\n\xd7\xa3p=\n\xd7\x18@\x04\x95\xf1\x01\0\x13\x13EVE-EVE-RELEASE@ccp$| p/EVE Online game server/

match exec m|^\x01Where are you\?\n$| p/netkit-rsh rexecd/ o/Linux/

# \x04 is the length, \x07\x08 is the command, following two bytes are an
# offset into an XOR code book. http://titanfiesta.googlecode.com/svn/trunk/TitanFiesta/Common/XorTable.h.
match fiesta-online m|^\x04\x07\x08..$| p/Fiesta Online game server/

match finger m|\r\n {4}Line {5,8}User {6,8}Host\(s\) {13,18}Idle +Location\r\n| p/Cisco fingerd/ o/IOS/ d/router/
match finger m|^OpenLDAP Finger Service\.\.\.\r\n| p/OpenLDAP fingerd/
match finger m|^No cfingerd\.conf file present\.  Check your setup\.\n$| p/cfingerd/ i/Broken/
match finger m|^Windows NT Version ([\d.]+) build (\d+), \d+ processors? \(.*\)\r\nFingerDW V([\d.]+) - Hummingbird Ltd\.\n| p/Hummingbird fingerd/ v/$3/ i/WinNT $1 build $2/ o/Windows/
match finger m|^\r\nIntegrated port\r\nPrinter Type: Lexmark T642\r\nPrint Job Status:| p/Lexmark T642 printer fingerd/ d/printer/

match freevcs m|^Welcome to FreeVCS MSSQL NT Service\r\n| p/FreeVCS/ i/MSSQL/ o/Windows/
match freevcs m|^Welcome to FreeVCS DBISAM NT Service\r\n| p/FreeVCS/ i/DBISAM/ o/Windows/
match freevcs m|^Welcome to FreeVCS Test NT Service\r\n| p/FreeVCS/ o/Windows/

# http://www.frozen-bubble.org/servers/servers.php
match frozen-bubble m|^FB/([\d.]+) PUSH: SERVER_READY ([\w._-]+) (\w+)\n| p/Frozen Bubble game server/ v/$1/ h/$2/ i/language: $3/

match file-replication m|^>>\n\0\x0eFRP Node Ready>>\n\0\x0e| p/File Replication Pro/

match freedoko m|^FreeDoko server\n\d+\.\d+: name: ([^\n]+)\n| p/FreeDoko game server/ i/name: $1/

match ftp m|^220 ([-/.+\w]+) FTP server \(SecureTransport (\d[-.\w]+)\) ready\.\r\n| p/Tumbleweed SecureTransport ftpd/ h/$1/ v/$2/
match ftp m|^220 3Com 3CDaemon FTP Server Version (\d[-.\w]+)\r\n| p/3Com 3CDaemon ftpd/ v/$1/
match ftp m|^220 3Com FTP Server Version ([-\w_.]+)\r\n| p/3Com ftpd/ v/$1/
# GuildFTP 0.999.9 on Windows
match ftp m|^220-GuildFTPd FTP Server \(c\) \d\d\d\d(-\d\d\d\d)?\r\n220-Version (\d[-.\w]+)\r\n| p/Guild ftpd/ v/$2/ o/Windows/
match ftp m|^220-.*\r\n220 Please enter your name:\r\n| p/GuildFTPd/ o/Windows/
# Medusa Async V1.21 [experimental] on Linux 2.4
match ftp m|^220 ([-/.+\w]+) FTP server \(Medusa Async V(\d[^\)]+)\) ready\.\r\n| p/Medusa Async ftpd/ h/$1/ v/$2/
match ftp m|^220 ([-/.+\w]+)\((\d[-.\w]+)\) FTP server \(EPSON ([^\)]+)\) ready\.\r\n| p/Epson printer ftpd/ h/$1/ v/$2/ i/Epson $3/ d/printer/
match ftp m|^220 ([-/.+\w]+) IBM TCP/IP for OS/2 - FTP Server [Vv]er \d+:\d+:\d+ on [A-Z]| p|IBM OS/2 ftpd| h/$1/ o|OS/2|
match ftp m|^220 ([-/.+\w]+) IBM TCP/IP f\xfcr OS/2 - FTP-Server [Vv]er \d+:\d+:\d+ .* bereit\.\r\n| p|IBM OS/2 ftpd| h/$1/ o|OS/2| i/German/
match ftp m|^220 Internet Rex (\d[-.\w ]+) \(([-/.+\w]+)\) FTP server awaiting your command\.\r\n| p/Internet Rex ftpd/ v/$1/ i/$2/
match ftp m|^220 ([-.+\w]+) FTP server \(Version (\d[-.\w]+)\([^\)]+\) [A-Z][a-z][a-z] [A-Z].*200\d\) ready\.\r\n| p/HP-UX ftpd/ h/$1/ v/$2/ o/HP-UX/
match ftp m|^530 Connection refused, unknown IP address\.\r\n$| p/Microsoft IIS ftpd/ i/IP address rejected/ o/Windows/
match ftp m|^220 IIS ([\w._-]+) FTP\r\n| p/Microsoft IIS ftpd/ v/$1/ o/Windows/
match ftp m|^220 PizzaSwitch FTP server ready\r\n| p/Xylan PizzaSwitch ftpd/
match ftp m|^220 ([-.+\w]+) IronPort FTP server \(V([-.\w]+)\) ready\.\r\n| p/IronPort mail appliance ftpd/ h/$1/ v/$2/
match ftp m|^220 ([-.+\w]+) IronPort FTP server \(V([-.\w]+)\) ready\.\r\n| p/IronPort mail appliance ftpd/ h/$1/ v/$2/
match ftp m|^220 ([-.+\w]+) IronPort FTP server \(V([-.\w]+)\) ready\r\n| p/IronPort firewall ftpd/ h/$1/ v/$2/
match ftp m|^220 WFTPD (\d[-.\w]+) service \(by Texas Imperial Software\) ready for new user\r\n| p/Texas Imperial Software WFTPD/ v/$1/ o/Windows/
match ftp m|^220.*\r\n220 WFTPD (\d[-.\w]+) service \(by Texas Imperial Software\) ready for new user\r\n|s p/Texas Imperial Software WFTPD/ v/$1/ o/Windows/
match ftp m|^220 ([-.+\w]+) FTP server \(Version (MICRO-[-.\w:#+ ]+)\) ready\.\r\n| p/Bay Networks MicroAnnex terminal server ftpd/ h/$1/ v/$2/ d/terminal server/
match ftp m|^220 ([-.+\w]+) FTP server \(Digital UNIX Version (\d[-.\w]+)\) ready\.\r\n| p/Digital UNIX ftpd/ h/$1/ v/$2/ o/Digital UNIX/
match ftp m|^220 ([-.+\w]+) FTP server \(Version [\d.]+\+Heimdal (\d[-+.\w ]+)\) ready\.\r\n| p/Heimdal Kerberized ftpd/ h/$1/ v/$2/ o/Unix/
match ftp m|^500 OOPS: (could not bind listening IPv4 socket)\r\n$| p/vsftpd/ i/broken: $1/ o/Unix/
match ftp m|^500 OOPS: vsftpd: (.*)\r\n| p/vsftpd/ i/broken: $1/ o/Unix/
match ftp m|^220-QTCP at ([-.\w]+)\r\n220| p|IBM OS/400 FTPd| o|OS/400| h/$1/
match ftp m|^220[- ]FileZilla Server version (\d[-.\w ]+)\r\n| p/FileZilla ftpd/ v/$1/ o/Windows/
match ftp m|^220 ([-\w_.]+) running FileZilla Server version (\d[-.\w ]+)\r\n| p/FileZilla ftpd/ v/$2/ h/$1/ o/Windows/
match ftp m|^220 FTP Server - FileZilla\r\n| p/FileZilla ftpd/ o/Windows/
match ftp m|^220-Welcome to ([A-Z]+) FTP Service\.\r\n220 All unauthorized access is logged\.\r\n| p/FileZilla ftpd/ h/$1/ o/Windows/
match ftp m|^220.*\r\n220[- ]FileZilla Server version (\d[-.\w ]+)\r\n|s p/FileZilla ftpd/ v/$1/ o/Windows/
match ftp m|^220-.*\r\n220-\r\n220 using FileZilla FileZilla Server version ([^\r\n]+)\r\n|s p/FileZilla ftpd/ v/$1/ o/Windows/
match ftp m|^220-FileZilla Server\r\n| p/FileZilla ftpd/ o/Windows/
match ftp m|^431 Could not initialize SSL connection\r\n| p/FileZilla ftpd/ i/Mandatory SSL/ o/Windows/
match ftp m|^550 No connections allowed from your IP\r\n| p/FileZilla ftpd/ i/IP blocked/ o/Windows/
# Netgear RP114 switch with integrated ftp server or ZyXel P2302R VoIP
match ftp m|^220 ([-\w]+)? FTP version 1\.0 ready at | p/Netgear broadband router or ZyXel VoIP adapter ftpd/ v/1.0/
match ftp m|^220 ([-.\w]+) FTP server \(GNU inetutils (\d[-.\w ]+)\) ready\.\r\n| p/GNU Inetutils FTPd/ v/$2/ h/$1/
match ftp m|^220 .* \(glftpd (\d[-.0-9a-zA-Z]+)_(\w+)(\+TLS)?\) ready\.\r\n| p/glFTPd/ v/$1/ i/$2/ o/Unix/
match ftp m|^220 .* \(glFTPd (\d[-.0-9a-zA-Z]+)_(\w+) Linux\+TLS\) ready\.?\r\n| p/glFTPd/ v/$1/ i/$2/ o/Linux/
match ftp m|^220 .* \(glFTPd (\d[-.0-9a-zA-Z]+) Linux\+TLS\) ready\.\r\n| p/glFTPd/ v/$1/ o/Linux/
match ftp m|^220 .* \(glFTPd (\d[-.0-9a-zA-Z]+) FreeBSD\+TLS\) ready\.\r\n| p/glFTPd/ v/$1/ o/FreeBSD/
match ftp m|^220 ([-.\w]+) FTP server \(FirstClass v(\d[-.\w]+)\) ready\.\r\n| p/FirstClass FTP server/ h/$1/ v/$2/
match ftp m|^220 ([-.\w]+) FTP server \(Compaq Tru64 UNIX Version (\d[-.\w]+)\) ready\.\r\n| p/Compaq Tru64 ftp server/ h/$1/ v/$2/ o/Tru64 UNIX/

match ftp m|^220 Axis ([\w\s]+) Network Camera( version)? (\d\S+) \((.*)\) ready\.\r\n|i p/Axis $1 Network Camera ftpd/ v/$3/ i/$4/ d/webcam/
match ftp m|^220 Axis (.*) Network Camera ([\w._-]+) .* ready\.\r?\n| p/Axis $1 Network Camera ftpd/ v/$2/ d/webcam/
match ftp m|^220 AXIS ([-.\w]+) FTP Network Print Server V(\d[-.\w]+) [A-Z][a-z]| p/Axis network print server ftpd/ v/$2/ i/Model $1/ d/print server/
match ftp m|^220 AXIS ([\d\w]+)V(\d\S+) (.*?) ready\.\n| p/AXIS $1 Webcam ftpd/ v/$2/ i/$3/ d/webcam/
match ftp m|^220 AXIS ([+\d]+) Video Server ?(\d\S+) (.*?) ready\.| p/AXIS $1 Video Server ftpd/ v/$2/ i/$3/
match ftp m|^220 AXIS (\w+) Video Server (\d\S+) \(.*\) ready\.\r\n| p/AXIS $1 Video Server ftpd/ v/$2/
match ftp m|^220 AXIS 205 version ([\d.]+) \(.*\) ready\.\r\n| p/AXIS 205 Network Video ftpd/ v/$1/ d/webcam/
match ftp m|^220 AXIS 250S MPEG-2 Video Server ([\d.]+) \([^)]+\) ready\.\r\n| p/AXIS 250S Network Video ftpd/ v/$1/ d/webcam/
match ftp m|^220 AXIS (\w+) Video Server ([\d.]+) \([^)]+\) ready\.\r\n| p/AXIS $1 Video Server ftpd/ v/$2/ d/media device/
match ftp m|^220 AXIS (\w+) Video Server Blade ([\w._-]+) \([^)]+\) ready\.\r\n| p/AXIS $1 Video Server Blade ftpd/ v/$2/ d/media device/
match ftp m|^220 AXIS StorPoint CD E100 CD-ROM Server V([\d.]+) .*  ready\.\r\n| p/AXIS StorPoint E100 CD-ROM Server ftpd/ v/$1/ d/storage-misc/
match ftp m|^220 AXIS (.+) FTP Network Print Server V([-\w_.]+) | p/AXIS $1 print server ftpd/ v/$2/ d/print server/
match ftp m|^220 AXIS ([\d/+]+) FTP Print Server V([-\w_.]+) | p/AXIS $1 print server ftpd/ v/$2/ d/print server/
match ftp m|^220 AXIS (\w+) Network Fixed Dome Camera (.*) ready\.\r\n| p/AXIS $1 camera ftpd/ v/$2/ d/webcam/

match ftp m|^220-Cerberus FTP Server Personal Edition\r\n220-UNREGISTERED\r\n| p/Cerberus FTP Server/ i/Personal Edition; Unregistered/ o/Windows/
match ftp m|^220-Cerberus FTP Server - Personal Edition\r\n220-This is the UNLICENSED personal edition and may be used for home, personal use only\r\n220-Welcome to Cerberus FTP Server\r\n220 Created by Cerberus, LLC\r\n| p/Cerberus FTP Server/ i/Personal Edition; Unregistered/ o/Windows/
match ftp m|^220-Welcome to Cerberus FTP Server\r\n220 Created by Grant Averett\r\n| p/Cerberus ftpd/ o/Windows/
match ftp m|^421-Not currently accepting logins at this address\. Try back \r\n421 later\.\r\n| p/Cerberus ftpd/ o/Windows/ i/banned/
match ftp m|^220 FTP print service:V-(\d[-.\w]+)/Use the network password for the ID if updating\.\r\n| p|Brother/HP printer ftpd| v/$1/ d/printer/
match ftp m|^220- APC FTP server ready\.\r\n220 \r\n$| p/APC ftp server/ d/power-device/
# HP-UX 10.x or AIX
match ftp m|^220 ([-\w]+) FTP server \(Version (\d[\w._-]+) [A-Z][a-z]{2} [A-Z][a-z]{2} .*\) ready\.\r\n| p/HP-UX or AIX ftpd/ h/$1/ v/$2/ o/Unix/
match ftp m|^220[- ]Roxen FTP server running on Roxen (\d[-.\w]+)/Pike (\d[-.\w]+)\r\n| p/Roxen ftp server/ v/$1/ i/Pike $2/
# Debian packaged oftpd 0.3.6-51 on Linux 2.6.0-test4 Debian
match ftp m|^220 Service ready for new user\.\r\n| p/oftpd/ o/Unix/
# Mac OS X Client 10.2.6 built-in ftpd
match ftp m|^220[ -].*FTP server \(lukemftpd (\d[-. \w]+)\) ready\.\r\n|s p/LukemFTPD/ v/$1/ o/Mac OS X/
match ftp m/^220.*Microsoft FTP Service \(Version (\d[^)]+)/ p/Microsoft ftpd/ v/$1/ o/Windows/
# This lame version doesn't give a version number
# Windows 2003
match ftp m/^220[ -]Microsoft FTP Service\r\n/ p/Microsoft ftpd/ o/Windows/
match ftp m/^220[ -]Serv-U FTP[ -]Server v([\w._-]+) / p/Serv-U ftpd/ v/$1/ o/Windows/
match ftp m|^220-Serv-U FTP Server for Winsock\r\n| p/Serv-U ftpd/ o/Windows/
match ftp m|^220 Serv-U FTP-Server v([-\w_.]+ build \d+) for WinSock ready\.\.\.\r\n| p/Serv-U ftpd/ v/$1/ o/Windows/
match ftp m|^220-FTP Server v([\d.]+) for WinSock ready\.| p/Serv-U ftpd/ o/Windows/ v/$1/
match ftp m|^220-SECURE FTP SERVER VERSION ([\d.]+) \(([-\w_.]+)\)\r\n| p/Serv-U ftpd/ v/$1/ i/Name $2/ o/Windows/
match ftp m|^431 Unable to negotiate secure command connection\.\r\n| p/Serv-U ftpd/ i/SSL Required/ o/Windows/
match ftp m/^220-Sambar FTP Server Version (\d\S+)\x0d\x0a/ p/Sambar ftpd/ v/$1/
# Sambar server V5.3 on Windows NT
match ftp m|^220-FTP Server ready\r\n220-Use USER user@host for native FTP proxy\r\n220 Your FTP Session will expire after 300 seconds of inactivity\.\r\n| p/Sambar ftpd/
match ftp m/^220 JD FTP Server Ready/ p/HP JetDirect ftpd/ d/print server/
match ftp m/^220.*Check Point FireWall-1 Secure FTP server running on/s p/Check Point Firewall-1 ftpd/ d/firewall/
match ftp m/^220[- ].*FTP server \(Version (wu-[-.\w]+)/s p/WU-FTPD/ v/$1/ o/Unix/
match ftp m|^220-\r\n220 ([-.\w]+) FTP server \(Version ([-.+\w()]+)\) ready\.\r\n$| p/WU-FTPD/ h/$1/ v/$2/ o/Unix/
match ftp m|^220 ([-.\w]+) FTP server \(Revision ([\d.]+) Version wuftpd-([-.+\w()]+) [^)]*\) ready\.\r\n$| p/WU-FTPD/ h/$1/ v/$3/ i/revision $2/ o/Unix/
match ftp m|^220 ([-.\w]+) FTP server \(Version ([-.+\w()]+)\) ready\.\r\n$| p|WU-FTPD or MIT Kerberos ftpd| h/$1/ v/$2/ o/Unix/

# ProFTPd 1.2.5
match ftp m|^220  Server \(ProFTPD\) \[([-.\w]+)\]\r\n| p/ProFTPD/ h/$1/ o/Unix/
match ftp m/^220 ProFTPD (\d\S+) Server/ p/ProFTPD/ v/$1/ o/Unix/
match ftp m/^220 FTP Server \[([-\w_.]+)\]\r\n/ p/ProFTPD/ o/Unix/ h/$1/
match ftp m|^220 ([-\w_.]+) FTP server ready\r\n| p/ProFTPD/ o/Unix/ h/$1/
match ftp m/^220.*ProFTP[dD].*Server ready/ p/ProFTPD/ o/Unix/
match ftp m|^220 ProFTP Server Ready\r\n| p/ProFTPD/ o/Unix/
match ftp m|^220 ProFTP Ready\r\n| p/ProFTPD/ o/Unix/
match ftp m|^220 Welcome @ my\.ftp\.org\r\n$| p/ProFTPD/ o/Unix/
match ftp m|^220-.*\r\n220 ProFTPD ([\d.]+) Server|s p/ProFTPD/ v/$1/ o/Unix/
match ftp m|^220 .* FTP Server \(ProFTPD ([\d.]+) on Red Hat linux ([\d.]+)\) ready\.\r\n| p/ProFTPD/ v/$1/ i/RedHat $2/ o/Linux/
match ftp m|^220 ProFTP-Server auf ([-\w_.]+)\r\n| p/ProFTPD/ i/German/ o/Unix/
match ftp m|^220.*\r\n220 ProFTPD ([\w._-]+) Server \(ProFTPD\)|s p/ProFTPD/ o/Unix/ v/$1/
# Hope these aren't too general -Doug
match ftp m|^220 ([-\w_.]+) FTP server ready!\r\n| p/ProFTPD/ o/Unix/ h/$1/
match ftp m|^220 FTP Server ready\.\r\n$| p/ProFTPD/ o/Unix/

match ftp m/^220.*NcFTPd Server / p/NcFTPd/ o/Unix/
match ftp m/^220 ([-\w_.]+) FTP server \(SunOS 5\.([789])\) ready/ p/Sun Solaris $2 ftpd/ o/Solaris/ h/$1/
match ftp m/^220 ([-\w_.]+) FTP server \(SunOS (\S+)\) ready/ p/Sun SunOS ftpd/ v/$2/ o/Solaris/ h/$1/
match ftp m/^220-([-.\w]+) IBM FTP.*(V\d+R\d+)/ p|IBM OS/390 ftpd| h/$1/ v/$2/ o|OS/390|
match ftp m|^220-IBM FTP, .*\.\r\n220 Connection will close if idle for more than 120 minutes\.\r\n| p|IBM OS/390 ftpd| o|OS/390|
match ftp m/^220 VxWorks \((\d[^)]+)\) FTP server ready/ p/VxWorks ftpd/ v/$1/ o/VxWorks/
match ftp m/^220 VxWorks \(VxWorks(\d[^)]+)\) FTP server ready/ p/VxWorks ftpd/ v/$1/ o/VxWorks/
match ftp m|^220 VxWorks FTP server \(VxWorks ?([\d.]+) - Secure NetLinx version \(([\d.]+)\)\) ready\.\r\n| p|AMX NetLinx A/V control system ftpd| v/$2/ i/VxWorks $1/ o/VxWorks/ d/media device/
match ftp m|^220 VxWorks \(VxWorks ([\w._-]+)\) FTP server ready\r\n| p|AMX NetLinx A/V control system ftpd| i/VxWorks $1/ o/VxWorks/ d/media device/
match ftp m|^220 VxWorks FTP server \(VxWorks ?([\w._-]+)\) ready\.\r\n| p/VxWorks ftpd/ v/$1/ o/VxWorks/
match ftp m|^220 ABB Robotics FTP server \(VxWorks ([\d.]+) rev ([\d.]+)\) ready\.\r\n| p/ABB Robotics ftpd/ i/VxWorks $1 rev $2  **A ROBOT**/ o/VxWorks/ d/specialized/

# Pure-ftpd
match ftp m/^220.*Welcome to .*Pure-?FTPd (\d\S+\s*)/ p/Pure-FTPd/ v/$1/
match ftp m/^220.*Welcome to .*Pure-?FTPd[^(]+\r\n/ p/Pure-FTPd/
match ftp m|^220.*Bienvenue sur .*Pure-?FTPd.*\r\n| p/Pure-FTPd/ i/French/
match ftp m/^220.*Bienvenue sur .*Pure-?FTPd (\d[-.\w]+)/ p/Pure-FTPd/ v/$1/ i/French/
match ftp m|^220.*Velkommen til .*Pure-?FTPd.*\r\n| p/Pure-FTPd/ i/Danish/
match ftp m|^220.*Bem-vindo.*Pure-?FTPd.*\r\n| p/Pure-FTPd/ i/Portugese/
# pure-ftpd 1.0.12 on Linux 2.4
match ftp m|^220[- ]FTP server ready\.\r\n.*214 Pure-FTPd - http://pureftpd\.org/?\r\n|s p/Pure-FTPd/
# OpenBSD 3.4 beta running Pure-FTPd 1.0.16 with SSL/TLS
match ftp m|^220---------- Welcome to Pure-FTPd \[privsep\] \[TLS\] ----------\r\n220-You are user number| p/Pure-FTPd/ i|with SSL/TLS|
match ftp m|^220---------- .* Pure-FTPd ----------\r\n220-| p/Pure-FTPd/
match ftp m|^220.*214 Pure-FTPd - http://pureftpd\.org/?\r\n|s p/Pure-FTPd/

match ftp m/^220 vsFTPd (.*) ready\.\.\.\r\n/ p/vsftpd/ v/$1/
match ftp m/^220 vsFTPd (.*) ready\.\.\. \[charset=\w+\]\r\n/ p/vsftpd/ v/$1/
match ftp m/^220 ready, dude \(vsFTPd (\d[0-9.]+): beat me, break me\)\r\n/ p/vsftpd/ v/$1/ o/Unix/
match ftp m/^220 \(vsFTPd ([-.\w]+)\)\r\n$/ p/vsftpd/ v/$1/ o/Unix/
match ftp m/^220 Welcome to blah FTP service\.\r\n$/ p/vsftpd/ o/Unix/

match ftp m/^220 TYPSoft FTP Server (\d\S+) ready\.\.\.\r\n/ p/TYPSoft ftpd/ v/$1/ o/Windows/
match ftp m/^220-MegaBit Gear (\S+).*FTP server ready/ p/MegaBit Gear ftpd/ v/$1/
match ftp m/^220.*WS_FTP Server (\d\S+)/ p/WS FTPd/ v/$1/ o/Windows/
match ftp m/^220 Features: a p \.\r\n$/ p/publicfile ftpd/ o/Unix/
match ftp m/^220 ([-.\w]+) FTP server \(Version (\S+) VFTPD, based on Version (\S+)\) ready\.\r\n$/ p/Virtual FTPD/ h/$1/ v/$2/ i/based on $2/ o/Unix/
match ftp m|220 ([-.\w]+) FTP server \(Version (\S+)/OpenBSD, linux port (\S+)\) ready\.\r\n| p/OpenBSD ftpd/ h/$1/ v/$2/ i/Linux port $2/ o/Linux/
match ftp m|^220 ([-.\w]+) FTP server \(Version (\S+)/OpenBSD/Linux-ftpd-([-.\w]+)\) ready.\r\n$| p/OpenBSD ftpd/ h/$1/ v/$2/ i/Linux port $2/ o/Linux/
match ftp m/^220 Interscan Version ([-\w.]+)/i p/InterScan VirusWall ftpd/ v/$1/
match ftp m|^220 InterScan FTP VirusWall NT (\d[-.\w]+) \(([-.\w]+) Mode\), Virus scan (\w+)\r\n$| p/InterScan VirusWall NT/ v/$1/ i/Virus scan $3; $2 mode/ o/Windows/
match ftp m|^220 ([-.\w]+) FTP server \(Version ([-.\w]+)/OpenBSD\) ready\.\r\n$| p/OpenBSD ftpd/ h/$1/ v/$2/ o/OpenBSD/
match ftp m|^220 ([-.\w]+) FTP server \(Version (6.0\w+)\) ready.\r\n| p/FreeBSD ftpd/ h/$1/ v/$2/ o/FreeBSD/
match ftp m|^220  FTP server \(Version ([\w.]+)\) ready\.\r\n| p/FreeBSD ftpd/ v/$1/ o/FreeBSD/
# Trolltech Troll-FTPD 1.28 (Only runs on Linux)
match ftp m|^220-Setting memory limit to 1024\+1024kbytes\r\n220-Local time is now \d+:\d+ and the load is [.\d]+\.\r\n220 You will be disconnected after \d+ seconds of inactivity.\r\n$| p/Trolltech Troll-FTPd/ o/Linux/

match ftp m|^220  FTP server \(Hummingbird Ltd\. \(HCLFTPD\) Version (7.1.0.0)\) ready\.\r\n$| p/Hummingbird FTP server/ v/$1/
match ftp m|^220  FTP server \(Hummingbird Communications Ltd\. \(HCLFTPD\) Version ([\d.]+)\) ready\.\r\n| p/Hummingbird FTP server/ v/$1/

match ftp m|^220- .*\n220 ([-.\w]+) FTP server \(Version (.*)\) ready\.\r\n|s p/BSD ftpd/ h/$1/ v/$2/
# Xitami FTPd
match ftp m|^220- \r\n.*www\.imatix\.com --\r\n|s p/Xitami ftpd/
match ftp m|^220- Welcome to this Xitami FTP server, running version ([\d\w.]+) of Xitami\. \n You are user number (\d+) of a permitted (\d+) users\.| p/Xitami ftpd/ v/$1/ i|$2/$3 users|

# Netware 6 - NWFTPD.NLM FTP Server Version 5.01w
match ftp m|^220 Service Ready for new User\r\n$| p/NetWare NWFTPD/
match ftp m|^220-LRN\r\n220 Service Ready for new User\r\n| p/NetWare NWFTPD/
match ftp m|^220 ([-\w]+) FTP server \(NetWare (v[\d.]+)\) ready\.\r\n$| p/Novell NetWare ftpd/ h/$1/ v/$2/ o/NetWare/
match ftp m|220  FTP Server for NW 3.1x, 4.xx  \((v1.10)\), \(c\) 199[0-9] HellSoft\.\r\n$| p/HellSoft FTP server for NetWare 3.1x, 4.x/ v/$1/
match ftp m|^220 ([-.\w]+) MultiNet FTP Server Process V(\S+) at .+\r\n$| p/DEC OpenVMS MultiNet FTPd/ h/$1/ v/$2/
match ftp m|^220-\r\n220 ([-.\w]+) FTP server \(NetBSD-ftpd ([-.\w]+)\) ready.\r\n$| p/NetBSD lukemftpd/ h/$1/ v/$2/
match ftp m|^220 ([-.\w]+) Network Management Card AOS v([-.\w]+) FTP server ready.\r\n$| p/APC AOS ftpd/ v/$2/ i/on APC $1 network management card/ d/power-device/ o/AOS/
match ftp m|^220 FTP Server \(Version 1.0\) ready.\r\n$| p/GlobespanVirata ftpd/ v/1.0/ d/broadband router/
# HP-UX B.11.00
match ftp m|^220 ([-.\w ]+) FTP server \(Version (1.1.2[.\d]+) [A-Z][a-z]{2} [A-Z][a-z]{2} .*\) ready.\r\n| p/HP-UX ftpd/ h/$1/ v/$2/ o/HP-UX/
# 220 mirrors.midco.net FTP server ready.
# WarFTP Daemon 1.70 on Win2K
match ftp m=^220-.*\r\n(220-|)    WarFTPd (\d[-.\w]+) \([\w ]+\) Ready\r\n=s p/WarFTPd/ v/$2/
match ftp m|^220 ([-.+\w]+) FTP SERVICE ready\r\n500 Please enter a command\. Dunno how to interperet empty lines\.\.\.\r\n500 Please enter a command\. Dunno how to interperet empty lines\.\.\.\r\n$| p/WarFTPd/ h/$1/ o/Windows/
match ftp m|^220 Welcome to Windows FTP Server| p|Windows Ftp Server| i|Not from Microsoft - http://srv.nease.net/|
# UnixWare 7.11
match ftp m|^220 ([-\w_.]+) FTP server \(BSDI Version ([\w.]+)\) ready\.\r\n| p|BSDI/Unixware ftpd| v/$2/ h/$1/
match ftp m|^220  FTP server \(Hummingbird Ltd\. \(HCLFTPD\) Version ([\d.]+)\) ready\.\r\n| p/Hummingbird ftpd/ v/$1/
match ftp m|^220 OpenFTPD server ready\. .*\.\r\n| p/OpenFTPD/
match ftp m|^220 ([\w._-]+) FTP server \(NetBSD-ftpd 20\w+\) ready\.\r\n| p/NetBSD lukemftpd/ o/NetBSD/
match ftp m|^220-\r\n    Your connection logged!\r\n220 ([\w\d_.-]+) FTP server \(NetBSD-ftpd 200\d+\) ready\.\r\n| p/NetBSD lukemftpd/ i/Connection logged/
match ftp m|^220 CommuniGate Pro FTP Server ([\d.]+) ready\r\n| p/Communigate Pro ftpd/ v/$1/
match ftp m|^220 CommuniGate Pro FTP Server ready\r\n| p/Communigate Pro ftpd/
match ftp m|^421 Sorry you are not welcomed on this server\.\r\n$| p/BulletProof ftpd/ i/Banned/ o/Windows/
match ftp m|^220-BulletProof FTP Server ready \.\.\.\r\n| p/BulletProof ftpd/ o/Windows/
match ftp m|^(220.*\r\n)?220 [Ee]valine FTP server \(Version:  Mac OS X|s p/Evaline ftpd/ o/Mac OS X/
match ftp m|^220 WinGate Engine FTP Gateway ready\r\n| p/WinGate ftpd/ o/Windows/
match ftp m|^220 Welcome to Quick 'n Easy FTP Server\r\n| p/Quick 'n Easy ftpd/ o/Windows/
match ftp m|^220 Welcome to Quick 'n Easy FTP Server DEMO\r\n| p/Quick 'n Easy ftpd/ o/Windows/ i/DEMO/
match ftp m|^421 Too many connections for this IP address, please try again later\.\r\n| p/Quick 'n Easy ftpd/ o/Windows/
match ftp m|^220 Tornado-vxWorks \(VxWorks([\d.]+)\) FTP server ready\r\n| p/Tornado vxWorks ftpd/ v/$1/
match ftp m|^220 [-\w_.]+ FTP server \(UNIX\(r\) System V Release 4\.0\) ready\.\r\n| p/UNIX System V Release 4.0 ftpd/
match ftp m|^(?:220-.*\r\n)?220 ([-\w_.]+) FTP Server \(Oracle XML DB/Oracle9i Enterprise Edition Release ([\d.]+) - Production\) ready\.\r\n|s p/Oracle Enterprise XML DB ftpd/ v/$2/ h/$1/
match ftp m|^(?:220-.*\r\n)?220 ([-\w_.]+) FTP Server \(Oracle XML DB/Oracle9i Release ([\d.]+) - Production\) ready\.\r\n|s p/Oracle XML DB ftpd/ v/$2/ h/$1/
match ftp m|^(?:220-.*\r\n)?220 ([-\w_.]+) FTP Server \(Oracle XML DB/Oracle Database 10g Enterprise Edition Release ([\d.]+) - Production\) ready\.\r\n|s p/Oracle 10g Enterprise XML DB ftpd/ v/$2/ h/$1/
match ftp m|^(?:220-.*\r\n)?220 ([-\w_.]+) FTP Server \(Oracle XML DB/Personal Oracle9i Release ([\d.]+) - Production\) ready\.\r\n|s p/Personal Oracle XML DB ftpd/ v/$1/ h/$1/
match ftp m|^(?:220-.*\r\n)?220 ([\w._-]+) FTP Server \(Oracle XML DB/Oracle Database\) ready\.\r\n|s p/Oracle XML DB ftpd/ h/$1/
match ftp m|^220 ([-\w_.]+) PacketShaper FTP server ready\.\r\n| p/PacketShaper ftpd/ h/$1/ o/Windows/
match ftp m|^220 WfFTP server\(([\w.]+)\) ready\.\r\n| p/Nortel WfFTP/ v/$1/ d/router/
match ftp m|^220- (.*) WAR-FTPD ([-\w.]+) Ready\r\n220 Please enter your user name\.\r\n| p/WAR-FTPD/ v/$2/ i/Name $1/ o/Windows/
match ftp m|^220 Canon EB-65 FTP Print Server V([\d.]+) .* ready\.\r\n| p/Canon EB-65 FTP Print Server/ v/$1/ d/print server/
match ftp m|^500 OOPS: .*\r\n$| p/vsftpd/ i/Misconfigured/ o/Unix/
match ftp m|^500 OOPS: vsftpd: both local and anonymous access disabled!\r\n| p/vsftpd/ i/Access denied/ o/Unix/
match ftp m|^220 FTP Version ([\d.]+) on MPS100\r\n| p/Lantronix MPS100 ftpd/ v/$1/ d/print server/
match ftp m|^220.*bftpd ([\d.]+) at ([-\w_.]+) ready\.?\r\n|s p/bftpd/ v/$1/ h/$2/
match ftp m|^220 RICOH Aficio ([\w\d_ +-]+) FTP server \(([\d.]+)\w?\) ready\.\r\n| p/Ricoh Aficio $1 ftpd/ v/$2/ d/print server/
match ftp m|^220 RICOH Pro (\d+[a-zA-Z]{0,3}) FTP server \(([\d+.]+)\) ready\.\r\n| p/Ricoh Pro $1 ftpd/ v/$2/ d/printer/
match ftp m|^220 LANIER ([\w\d /-]+) FTP server \(([\d+.]+)\) ready\.\r\n| p/Lanier $1 ftpd/ v/$2/ d/printer/
match ftp m|^220 Welcome to Code-Crafters Ability FTP Server\.\r\n| p/Code-Crafters Ability ftpd/ o/Windows/
match ftp m|^220 Welcome to Code-Crafters - Ability Server ([\d.]+)\.| p/Code-Crafters Ability ftpd/ v/$1/ o/Windows/
match ftp m|^220 ([-\w_.]+)           FTP server \(ARM_BE - V([\w.]+)\) ready\.\r\n| p/NetComm NS4000 Network Camera/ h/$1/ i/ARM_BE $2/ d/webcam/
match ftp m|^220 MikroTik FTP server \(MikroTik v?([\w._-]+)\) ready\r\n| p/MikroTik router ftpd/ v/$1/ d/router/
match ftp m|^220 lankacom FTP server \(MikroTik v?([\w._-]+)\) ready\r\n| p/Lankacom router ftpd/ i/MikroTik/ v/$1/ d/router/
match ftp m|^220 (.+) FTP server \(MikroTik ([\w._-]+)\) ready\r\n| p/MikroTik router ftpd/ v/$2/ h/$1/ d/router/
match ftp m|^220 NetPresenz v([\d.]+) \(Unregistered\) awaits your command\.\r\n| p/NetPresenz/ v/$1/ i/Unregistered/ o/Mac OS/
match ftp m|^220 LP-8900-\w+ FTP server \(OEM FTPD version ([\d.]+)\) ready\.\r\n| p/EPSON Network Print Server ftpd/ i/runs OEM FTPD $1/ d/print server/
match ftp m|^220 StylusPhoto750-AF6788 FTP server \(OEM FTPD version ([\d.]+)\) ready\.\r\n| p/Epson StylusPhoto750 ftpd/ i/runs OEM FTPD $1/ d/print server/
match ftp m|^220 AL-C900-BB0200 FTP server \(OEM FTPD version ([\d.]+)\) ready\.\r\n| p/Epson AcuLaser C900 printer ftpd/ i/runs OEM FTPD $1/ d/printer/
match ftp m|^220 FTP Version ([\d.]+) on MSS100\r\n| p/Lantronix MSS100 serial interface ftpd/ v/$1/ d/specialized/
match ftp m|^220 Matrix FTP server \(Server \w+#\d\) ready\.\r\n| p/Matrix ftpd/
match ftp m|^220 Titan FTP Server ([\d.]+) Ready\.\r\n| p/Titan ftpd/ v/$1/ o/Windows/
match ftp m|^421-\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+=\+\r\n421-The evaluation period for this Titan FTP Server has expired\.\r\n| p/Titan ftpd/ i/Evaluation period expired/ o/Windows/
match ftp m|^220 ioFTPD \[www: http://www\.ioftpd\.com\] - \[version: ([-\w_. ]+)\] server ready\.\r\n| p/ioFTPD/ v/$1/ o/Windows/
match ftp m|^220 CesarFTP ([\w.]+) Server Welcome !\r\n| p/CesarFTPd/ v/$1/ o/Windows/
match ftp m|^220 CesarFTP ([\w.]+) \xb7\xfe\xce\xf1\xc6\xf7\xbb\xb6\xd3\xad !\r\n| p/CesarFTPd/ v/$1/ i/Chinese/ o/Windows/
match ftp m|^220-This site is running the BisonWare BisonFTP server product V([\d.]+)\r\n| p/BisonWare BisonFTPd/ v/$1/ o/Windows/
match ftp m=^220-Welcome to XBOX FileZilla( \(XBMC\)|)\r\n220-version: XBFileZilla version ([\d.]+), \(based on FileZilla Server ([\d.]+)\)\r\n220 http://sourceforge\.net/projects/xbfilezilla\r\n= p/XBFileZilla/ v/$2/ i/Based on FileZilla $3/
match ftp m=^220-Welcome to XBOX FileZilla( \(XBMC\)|)\r\n220-version: XBMC:FileZilla version ([\d.]+), \(based on FileZilla Server ([\d.]+)\)\r\n220 http://sourceforge\.net/projects/xbfilezilla\r\n= p/XBFileZilla/ v/$2/ i/Based on FileZilla $3/
match ftp m|^220 Session will be terminated after 600 seconds of inactivity\.\r\n| p/Cisco 3000 series VPN ftpd/ o/IOS/ d/security-misc/
match ftp m|^220-SlimFTPd ([\d.]+), by WhitSoft Development \(www\.whitsoftdev\.com\)\r\n| p/SlimFTPd/ v/$1/ o/Windows/
match ftp m|^220 BlackMoon FTP Server Version ([\d.]+ Release \d+) - Build \d+\. Free Edition\. Service Ready\r\n| p/BlackMoon ftpd/ i/Free edition/ v/$1/ o/Windows/
match ftp m|^220 BlackMoon FTP Server Version ([\d.]+ Release \d+) - Build \d+\. Chaos Edition\. Service Ready\r\n| p/BlackMoon ftpd/ i/Chaos edition/ v/$1/ o/Windows/
match ftp m|^220-BlackMoon FTP Server Version ([\d.]+ Release \d+) - Build \d+\r\n| p/BlackMoon ftpd/ v/$1/ o/Windows/
match ftp m|^220 BlackMoon FTP Server - Free Edition - Version ([\d.]+)\. Service Ready\r\n| p/BlackMoon ftpd/ i/Free edition/ v/$1/ o/Windows/
match ftp m|^220 netapp ftp server\r\n| p/netapp ftpd/
match ftp m|^220 Oracle Internet File System FTP Server ready\r\n| p/Oracle Internet File System ftpd/
match ftp m|^220 RICOH Aficio (\w+) FTP server \(([\d.]+)\) ready\.\r\n| p/Ricoh Aficio $1 printer ftpd/ v/$2/ d/printer/
match ftp m|^220 NRG 2205/2238/2212 FTP server \(([\d.]+)\) ready\.\r\n| p|NRG 2205/2238/2212 copier ftpd| v/$1/ d/printer/
match ftp m|^220 mandelbrot FTP server \(Version ([\d.]+) \(NeXT ([\d.]+)\) .*\) ready\.\r\n| p/mandelbrot ftpd/ v/$1/ i/NeXT $2/ o/NeXTStep/
# Microsoft Windows .NET Enterprise Server (build 3604-3790)
match ftp m|^220 Net Administration Divisions FTP Server Ready\.\.\.\r\n| p/Net Administration Divisions ftpd/
match ftp m|^220-\r\n220-\r\n220 Please enter your user name\.\r\n| p/MoreFTPd/
match ftp m|^220 ([-\w_.]+) FTP server \(OSF/1 Version ([\d.]+)\) ready\.\r\n| p|OSF/1 ftpd| i|OSF/1 $2| h/$1/ o/Unix/
match ftp m|^220 Qtopia ([\d.]+) FTP Server\n| p/Qtopia ftpd/ v/$1/ d/PDA/
match ftp m|^220[ -]Gene6 FTP Server v([\d.]+) +\(Build (\d+)\).* ready\.\.\.\r\n| p/Gene6 ftpd/ v/$1 build $2/ o/Windows/
match ftp m|^220 G6 FTP Server v([\d.]+) \(beta (\d+)\) ready \.\.\.\r\n| p/Gene6 ftpd/ v/$1 beta $2/ o/Windows/
match ftp m|^220 ([-\w_.]+) by G6 FTP Server ready \.\.\.\r\n| p/Gene6 ftpd/ h/$1/ o/Windows/
match ftp m|^220 .* by G6 FTP Server ready \.\.\.\r\n| p/Gene6 ftpd/ o/Windows/
match ftp m|^220.*Hello!  I'm Gene6 FTP Server v([-\w_.]+) \(Build (\d+)\)\.\r\n|s p/Gene6 ftpd/ v/$1 build $2/ o/Windows/
match ftp m|^220 ([\w._-]+) FTP server ready\.\.\.\r\n| p/Gene6 ftpd/ o/Windows/
match ftp m|^220 sftpd/([\d.]+) Server \[[-\w_.]+\]\r\n| p/sftpd/ v/$1/
match ftp m|^220-TYPSoft FTP Server ([\d.]+) ready\.\.\.\r\n| p/TYPSoft ftpd/ v/$1/ o/Windows/
match ftp m|^220 Welcome to Pablo's FTP Server\r\n| p/Pablo's ftpd/ o/Windows/
match ftp m|^220 PowerLogic FTP Server ready\.\r\n| p/PowerLogic embedded device ftpd/ d/specialized/
match ftp m|^220 INTERMEC 540\+/542\+ FTP Printer Server V([\d.]+) .* ready\.\r\n| p|Intermec 540+/542+ printer ftpd| v/$1/ d/printer/
match ftp m|^220 EthernetBoard OkiLAN 8100e Ver ([\d.]+) FTP server\.\r\n| p/OkiLAN 8100e print server/ v/$1/ d/print server/
match ftp m|^220 OKI-([\w+]+) Version ([\d.]+) ready\.\r\n| p/OkiData $1 printer ftpd/ v/$2/ d/printer/
# SpeedStream 5660 ADSL modem/router
match ftp m|^220 VxWorks \(ENI-ftpd ([\d.]+)\) FTP server ready\r\n| p/SpeedStream 5660 ADSL router/ i|Runs ENI-ftpd/$1 on VxWorks| d/router/

match ftp m|^220--------------------------------------------------------------------------------\r\n220-This is the \"Banner\" message for the Mac OS X Server's FTP server process\.\r\n.*220 ([-\w_.]+) FTP server \(Version:  Mac OS X Server ([\d.]+) - \+GSSAPI\) ready\.\r\n|s p/Mac OS X Server ftpd/ i/MacOS X $2/ h/$1/ o/Mac OS X/
match ftp m|^220--------------------------------------------------------------------------------\r\n220-This is the \"Banner\" message for the Mac OS X Server's FTP server process\.\r\n| p/Mac OS X Server ftpd/ o/Mac OS X/

match ftp m|^220 Welcome to U\.S\.Robotics SureConnect ADSL Ethernet/USB Router update FTP server v([\d.]+)\.\r\n| p/USRobotics SureConnect ADSL router ftpd/ v/$1/ d/router/
match ftp m|^220-Welcome to Xerver Free FTP Server ([\d.]+)\.\r\n220-\r\n220-You can login below now\.\r\n220 Features: \.\r\n| p/Xerver Free ftpd/ v/$1/
match ftp m|^220 ([-\w_.]+) FTP server \(tnftpd (\d+)\) ready\.\r\n| p/tnftpd/ v/$2/ h/$1/
match ftp m|^220 ([-\w_.]+) FTP server \(LundFTPD ([\d.]+) .*\) ready\.\r\n| p/LundFTPd/ v/$2/ h/$1/
match ftp m|^220 HD316\r FTP server\(Version([\d.]+)\) ready\.\r\n| p/Panasonic HD316 Digital Disk Recorder/ v/$1/ d/storage-misc/
match ftp m=^220 (\w+) IBM Infoprint (Color |)(\d+) FTP Server ([\w.]+) ready\.\r\n= p/IBM Infoprint $2$3 ftpd/ h/$1/ v/$4/ d/printer/
match ftp m=^220 ([\w._-]+) IBM Infoprint (\w+) FTP Server ([\w.]+) ready\.\r\n= p/IBM Infoprint $2 ftpd/ h/$1/ v/$3/ d/printer/
match ftp m|^220 ShareIt FTP Server ([\d.]+) \(WINCE\) Ready\.\r\n| p/ShareIt ftpd/ v/$1/ d/PDA/
match ftp m|^220 ShareIt FTP Pro ([\d.]+) \(WINCE\) Ready\.\r\n| p/ShareIt Pro ftpd/ v/$1/ d/PDA/
match ftp m|^220 ISOS FTP Server for Upgrade Purpose \(([\d.]+)\) ready\r\n| p/Billion 741GE ADSL router/ v/$1/ d/router/
match ftp m|^220 PV11 FTP Server ready\r\n| p/Unknown wireless acces point ftpd/ i/Runs Phar Lap RTOS/ d/router/
match ftp m|^220 Alize Session Manager FTP Server\r\n| p/Alcatel OmniPCX ftpd/ d/PBX/
match ftp m|^220-FTP Server ready\r\n220-Welcome to the Sambar FTP Server\r\r\n| p/Sambar ftpd/
match ftp m|^220 SINA FTPD \(Version ([-\d.]+)\).*\r\n| p/Sina ftpd/ v/$1/
match ftp m|^220 DataHive FTP Server ([\d.]+) Ready\.\r\n| p/DataHive ftpd/ v/$1/
match ftp m|^220--- AlterVista FTP, based on Pure-FTPd --\r\n| p/AlterVista ftpd/ i/Based on Pure-ftpd/
match ftp m|^220 Welcome to the ADI Convergence Galaxy update FTP server v([\d.]+)\.\r\n| p/ADI Convergence Galaxy update ftpd/ v/$1/
match ftp m|^421 You are not permitted to make this connection\.\r\n| p/Symantec Raptor Firewall ftpd/ d/firewall/
match ftp m|^220 copier2FTP server ready\.\r\n| p/Konica Minolta Di3510 Copier ftpd/ d/printer/
match ftp m|^220 DrayTek FTP version ([\d.]+)\r\n| p/DrayTek Vigor router ftpd/ v/$1/ d/router/
match ftp m|^220 ([-\w_.]+) FTP server ready \(mod_ftpd/([\d.]+)\)\r\n| p/Apache mod_ftpd/ v/$2/ h/$1/
match ftp m|^220 The Avalaunch FTP system -- enter user name\r\n| p/Avalaunch ftpd/ i/XBox/ d/game console/
match ftp m|^220 Server 47 FTP service\. Welcome\.\r\n| p/bftpd/ o/Unix/
match ftp m%^220-loading\.\.\r\n220-\|           W e L c O m E @ SFXP\|=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=\|\r\n% p/SwiftFXP/
match ftp m|^220 Z-FTP\r\n| p/Z-FTPd/
match ftp m|^220 DELL1700n Dell Laser Printer 1700n FTP Server ([\w.]+) ready\.\r\n| p/Dell 1700n laser printer ftpd/ v/$1/ d/printer/
match ftp m|^220 Dell Laser Printer 3100cn\r\n| p/Dell 3100cn laser printer ftpd/ d/printer/
match ftp m|^220 Dell Color Laser 5110cn\r\n| p/Dell Color Laser 5110cn printer ftpd/ d/printer/
match ftp m|^220 \w+ Dell Laser Printer M5200 FTP Server ([\d.]+) ready\.\r\n| p/Dell Laser Priner M5200 ftpd/ v/$1/ d/printer/
match ftp m|^220 Plan 9 FTP server ready\r\n| p/Plan 9 ftpd/ o/Plan 9/
match ftp m=^220-\+----------------------\[ UNREGISTERED VERSION \]-----------------------\+\r\n220-\|   This site is running unregistered copy of RaidenFTPD ftp server   \+\r\n= p/RaidenFTPd/ i/Unregistered/ o/Windows/
match ftp m|220 ([-\w_.]+) FTP server \(Version:  Mac OS X Server ([\d.]+) - \+GSSAPI\) ready\.\r\n|s p/MacOS X Server ftpd/ i/MacOS X Server $2/ h/$1/
match ftp m|^220 Fastream NETFile FTP Server( Ready)?\r\n| p/Fastream NETFile FTPd/ o/Windows/
match ftp m|^220 FTP 9500 server \(Version ([\d.]+)\) ready\.\r\n| p|Nokia Smartphone 9300/9500 ftpd| v/$1/ d/phone/ o/Symbian/
match ftp m|^220 [\d.]+ CVX FTP server \(([\d.]+)\) ready\.\r\n| p/CVX ftpd/ v/$1/
match ftp m|^220-\.:\.\r\n220-\.:+\r\n220-\.::::::::::\. e1137 FTP Server loading \.::::::::::::::\. WinSock ready \.| p/e1137 ftpd/ o/Windows/
match ftp m|^220 Connect\(active \d+, max active \d+\) session \d+ to RemoteScan Server ([\d.]+) on .*\r\n| p/RemoteScan ftpd/ v/$1/ o/Windows/
match ftp m|^220.ArGoSoft FTP Server for Windows NT/2000/XP, Version [\d.]+ \(([\d.]+)\)\r\n| p/ArGoSoft ftpd/ v/$1/ o/Windows/
match ftp m|^220.ArGoSoft FTP Server, Version [\d.]+ \(([\d.]+)\)\r\n| p/ArGoSoft ftpd/ v/$1/ o/Windows/
match ftp m|^220 ArGoSoft FTP Server \.NET v\.([\d.]+) at [^\r\n]*\r\n| p/ArGoSoft ftpd/ v/$1/ o/Windows/
match ftp m|^220 Welcome to the dvd2xbox ftp server\.\r\n| p/dvd2xbox built-in ftpd/ d/game console/
match ftp m|^220 Welcome To WinEggDrop Tiny FTP Server\r\n| p/WinEggDrop ftpd/ o/Windows/
match ftp m|^220-\n220-Welcome to the HOME Edition of GlobalSCAPE CuteFTP Server, which limits\n| p/GlobalSCAPE CuteFTPd/ i/HOME Edition/ o/Windows/
match ftp m|^220 Gestetner DSm622 FTP server \(([\d.]+)\) ready\.\r\n| p/Gestetner DSm622 copier ftpd/ v/$1/ d/printer/
match ftp m|^220 NRG (\w+) FTP server \(([\d.]+)\) ready\.\r\n| p/NRG $1 printer ftpd/ v/$2/ d/printer/
match ftp m|^220-<W\x80lC0ME T0 THE \xb0GP - FXP PubSTRO\xb0 by JACK>\r\n| p/Backdoor Pubstro ftpd/ o/Windows/
match ftp m|^220 wzd server ready\.\r\n| p/wzdftpd/
match ftp m|^500 Sorry, no server available to handle request on ([-\w_.:]+)\r\n| p/ProFTPD/ i/No server available/ h/$1/
match ftp m|^500 Sorry, no server available to handle request on ([-\w_.:]+)\.\r\n| p/ProFTPD/ i/No server available/ h/$1/
match ftp m|^220 Intel NetportExpress\(tm\) 10/100 Single-port FTP server ready\.\r\n| p/Intel NetportExpress print server ftpd/ d/print server/
match ftp m|^220 NET\+ARM FTP Server ([\d.]+) ready\.\r\n| p/NET+ARM ftpd/ v/$1/
match ftp m|^220- FTPshell Server Service \(Version ([-\w_.]+)\)\r\n220  \r\n| p/FTPshell ftpd/ v/$1/ o/Windows/
match ftp m|^220 Connected to ([-\w_.]+) ready\.\.\.\r\n| p/TYPSoft ftpd/ h/$1/ o/Windows/
match ftp m|^220 ([-\w_.]+) FTP Server \(LiteServe\) Ready!\r\n| p/Perception LiteServe ftpd/ h/$1/ o/Windows/
match ftp m|^220 BetaFTPD ([-\w_.]+) ready\.\r\n| p/BetaFTPd/ v/$1/
match ftp m|^220 NET Disk FTP Server ready\.\r\n| p|NET Disk/NetStore ftpd|
match ftp m|^421 Service not available, closing control connection\.\r\n| p|NET Disk/NetStore ftpd| i/Disabled/
match ftp m|^220 NETWORK HDD FTP Server ready\.\r\n| p/Argosy Research HD363N Network HDD ftpd/ d/storage-misc/
match ftp m|^220 Blue Coat FTP Service\r\n| p/Blue Coat ftpd/
# Can't find any info on this ftpd. Backdoor? -Doug
match ftp m|^220 Homer Ftp Server\r\n| p/Homer ftpd/ o/Windows/
match ftp m|^220 Personal FTP Server ready\r\n| p/Personal FTPd/ o/Windows/
match ftp m|^220 Personal FTP Professional Server ready\r\n| p/Personal FTPd Professional/ o/Windows/
match ftp m|^220-InterVations FileCOPA FTP Server Version ([\d.]+) .*\r\n220 Trial Version\. (\d+) days remaining\r\n| p/InterVations FileCOPA ftpd/ v/$1/ i/Trial: $2 days left/ o/Windows/
match ftp m|^220 cab Mach4/(\d+) FTP Server ready\.\r\n| p/CAB MACH 4 label printer ftpd/ d/printer/ i/$1 dpi/
match ftp m|^220 cab A4\+/(\d+) FTP Server ready\.\r\n| p/CAB A4+ label printer ftpd/ d/printer/ i/$1 dpi/
match ftp m|^220 (KM[\w+]+) FTP server \(KM FTPD version ([\d.]+)\) ready\.\r\n| p/Konica Minolta $1 ftpd/ v/$2/ d/printer/
match ftp m|^220 Golden FTP Server ready v([\d.]+)\r\n| p/Golden ftpd/ v/$1/ o/Windows/
match ftp m|^220 Golden FTP Server PRO ready v([\d.]+)\r\n| p/Golden PRO ftpd/ v/$1/ o/Windows/
match ftp m|^220 ITC Version  ([\d.]+) of [-\d]+  X Kyocera UIO UMC 10base OK \r\n| p/X Kyocera UIO UMC 10base print server ftpd/ v/$1/ d/print server/
match ftp m|^220 ActiveFax Version ([\d.]+) \(Build (\d+)\) - .*\r\n| p/ActiveFax ftpd/ v/$1 build $2/
match ftp m|^220-Welcome to CrushFTP!\r\n220 CrushFTP Server Ready[.!]\r\n| p/CrushFTPd/
match ftp m|^220-Welcome to CrushFTP([\w._-]+)!\r\n220 CrushFTP Server Ready\.\r\n| p/CrushFTP/ v/$1/
match ftp m|^220 DPO-7300 FTP Server ([\d.]+) ready\.\n| p/NetSilicon DPO-7300 ftpd/ v/$1/
match ftp m|^220 Welcome to WinFtp Server\.\r\n| p/WinFtpd/ o/Windows/
match ftp m|^220  IBM TCP/IP for OS/2 - FTP Server ver ([\d:.]+) on .* ready\.\r\n| p|IBM OS/2 ftpd| v/$1/ o|OS/2|
match ftp m|^220 AudioVAULT FTP server\r\n| p/AudioVault ftpd/ o/Windows/
match ftp m|^220 FTP/VPP Server ([\d.]+) / Current Date: [-\d]+ [\d:]+\r\n| p/Verteiltes Printen und Plotten ftpd/ v/$1/
match ftp m|^220 Xerox WorkCentre (\w+) Ver ([\d.]+) FTP server\.\r\n| p/Xerox WorkCentre $1 ftpd/ v/$2/ d/printer/
match ftp m|^220 .* Server \(vftpd ([\d.]+)\) ready\.\r\n| p/vftpd/ v/$1/ o/Windows/
match ftp m|^220 Welcome to Network Camera FTP Server\r\n| p/Vivotek 3102 Camera ftpd/ d/webcam/
match ftp m|^220-TwoFTPd server ready\.\r\n220 Authenticate first\.\r\n| p/TwoFTPd/ o/Unix/
match ftp m|^220  WEB TLC FTP SERVER READY TYPE HELP FOR HELP \r\n| p/Overland Storage Neo2000 ftpd/ d/storage-misc/
match ftp m|^220 ([-/.+\w_]+) Lexmark ([-/.+\w ]+) FTP Server ([-.\w]+) ready\.\r\n| p/Lexmark $2 printer ftpd/ v/$3/ h/$1/ d/printer/
match ftp m|^220 ([-/.+\w_]+) MarkNet ([-/.+\w ]+) FTP Server ([-.\w]+) ready\.\r\n| p/Lexmark $2 printer ftpd/ v/$3/ h/$1/ d/printer/
match ftp m|^220 ([-/.+\w_]+) Dell Laser Printer ([-/.+\w ]+) FTP Server ([-.\w]+) ready\.\r\n| p/Dell $2 printer ftpd/ v/$3/ h/$1/ d/printer/
match ftp m|^220 ([-/.+\w_]+) Dell ([-/.+\w ]+) FTP Server ([-.\w]+) ready\.\r\n| p/Dell $2 printer ftpd/ v/$3/ h/$1/ d/printer/
match ftp m|^500 ([\w._-]+) FTP server shut down -- please try again later\.\r\n| p/Mac OS X Server ftpd/ h/$1/ i/disabled/ o/Mac OS X/
match ftp m|^220  \(Ver\. ([^)]+)\) [A-Z][a-z]{2} \d+ 20\d+ ready\.\r\n| p|Canon VB-C10/VB-C10R webcam ftpd| v/$1/ d/webcam/
match ftp m|^220 Cisco \(([\d.]+)\) FTP server ready\r\n| p/Cisco ftpd/ v/$1/ o/IOS/
match ftp m|^220 \"Global Site Selector FTP\"\r\n| p/Cisco Site Selector ftpd/ d/security-misc/
match ftp m|^220 ISOS FTP Server \(([\d.]+)\) ready\r\n| p/Xavi 7768 WAP ftpd/ v/$1/ d/WAP/
match ftp m|^220- smallftpd ([\d.]+)\r\n220- check http://smallftpd\.free\.fr| p/smallftpd/ v/$1/ o/Windows/
match ftp m|^220 ([-\w_.]+) GridFTP Server ([\w._-]+) \((gcc\w+), [-\d]+\) ready\.\r\n| p/Globus GridFTPd/ v/$2/ i/$3/ h/$1/
match ftp m|^220 ([\w._-]+) GridFTP Server ([\w._-]+) \((gcc\w+), [-\d]+\) \[Globus Toolkit ([\w._-]+)\] ready\.\r\n| p/Globus GridFTPd/ v/$2/ i/Globus Toolkit $4; $3/ h/$1/
match ftp m|^220 ([-\w_.]+) ([A-Z]+ )?GridFTP Server ([\d.]+) (GSSAPI type Globus/GSI wu-\S+) \(gcc\w+, [-\d]+\) ready\.\r\n| p/Globus GridFTPd/ v/$3/ i/$4/ h/$1/
match ftp m|^220 ([-\w_.]+) FTP server \(GridFTP Server ([\d.]+) \[(GSI patch v[\d\.]+)\] (wu-\S+) .+\) ready\.\r\n| p/Globus GridFTPd/ v/$2/ i/$4 $3/ h/$1/
match ftp m|^220 Welcome to the OpenDreambox FTP service\.\r\n| p/Dreambox ftpd/ o/Linux/ d/media device/
match ftp m|^220 Willkomen auf Ihrer Dreambox\.\r\n| p/Dreambox ftpd/ o/Linux/ d/media device/ i/German/
match ftp m|^220 Welcome to the PLi dreambox FTP server\r\n| p/Dreambox ftpd/ i/PLi image/ o/Linux/ d/media device/
match ftp m|^220 Welcome to the Pli Jade Server >> OpenDreambox FTP service <<\.\r\n| p/Dreambox ftpd/ i/PLi Jade image/ o/Linux/ d/media device/
match ftp m|^220 ([-\w_.]+) FTP server \(KONICA FTPD version ([\d.]+)\) ready\.\r\n| p/Konica Minolta printer ftpd/ v/$2/ h/$1/ d/printer/
match ftp m|^220 KONICA MINOLTA FTP server ready\.\r\n| p/Konica Minolta bizhub printer ftpd/ d/printer/
match ftp m|^Error loading /etc/ssl/certs/ftpd\.pem:| p/Linux NetKit ftpd/ i/misconfigured/ o/Linux/
match ftp m|^500 OOPS: cannot locate user entry:([-\w_]+)\r\n500 OOPS: child died\r\n| p/vsftpd/ i/misconfigured; ftp user $1/
match ftp m|^220 Welcome to Freebox FTP Server\.\r\n| p/Freebox ftpd/ d/media device/
match ftp m|^220  FTP server \(Medusa Async V([\d.]+) \[experimental\]\) ready\.\r\n| p/Zope Medusa ftpd/ v/$1/
match ftp m|^220-  Novonyx FTP Server for NetWare, v([\d.]+) \(| p/Novonyx ftpd/ v/$1/ o/NetWare/
match ftp m|^220 ([-\w_.]+) \(Aironet (BR\w+) V([\d.]+)\) ready\r\n| p/Aironet $2 wireless bridge ftpd/ v/$3/ h/$1/ d/WAP/
match ftp m|^220-Welcome To Rumpus!\r\n220 Service ready for new user\r\n| p/Rumpus ftpd/ o/Mac OS X/
match ftp m|^220 Hello, I'm freeFTPd ([\d.]+)\r\n| p/FreeFTPd/ v/$1/ o/Windows/
match ftp m|^220 PrNET FTP server \(PrNET FTP ([\d.]+)\) ready\.\r\n| p/Panasonic WV-NP1000 webcam ftpd/ v/$1/ d/webcam/
match ftp m|^220-Looking up your hostname\.\.\.\r\n220-Welcome to SimpleFTPd v([\w.]+) by MagicalTux| p/SimpleFTPd/ v/$1/
match ftp m|^220 IB-21E Ver ([\d.]+) FTP server\.\r\n| p/Kyocera IB-21E print server ftpd/ v/$1/ d/print server/
match ftp m|^220 IB-23 Ver ([\d.]+) FTP server\.\r\n| p/Kyocera FS-1000D-series print server ftpd/ v/$1/ d/print server/
match ftp m|^220 SurgeFTP ([-\w_.]+) \(Version ([\w.]+)\)\r\n| p/SurgeFTPd/ v/$1/
match ftp m|^220 Disk Station FTP server at ([-\w_.]+) ready\.\r\n| p/Synolgy NAS ftpd/ h/$1/ d/storage-misc/
match ftp m|^220  FTP Merak ([\d.-]+)\r\n| p/Merak ftpd/ v/$1/ o/Windows/
match ftp m|^refused in\.ftpd from [-\w_.]+ logged\n| p/tcpwrapped ftpd/ i/refused/
match ftp m|^220 Ipswitch Notification Server| p/Ipswitch notification ftpd/ o/Windows/
match ftp m|^220-?\s+SSH-[\d.]+-([a-zA-Z]+)| p/FTP masquerading as $1/ i/**BACKDOOR**/
match ftp m|^220 Xlight FTP Server ([\d.]+) ready\.\.\.\r\n| p/Xlight ftpd/ v/$1/ o/Windows/
match ftp m|^220 Xlight Server ([\d.]+) ready\.\.\. \r\n| p/Xlight ftpd/ v/$1/ o/Windows/
match ftp m|^220 NetTerm FTP server ready \r\n| p/NetTerm ftpd/ o/Windows/
match ftp m|^220 SHARP ([\w-]+) FTP server ready\.\r\n| p|Sharp $1 printer ftpd| d/printer/
match ftp m|^220 SHARP ([\w-]+) Ver ([\w._-]+) FTP server\.\r\n| p/SHARP $1 printer ftpd/ v/$2/ d/printer/
match ftp m|^220 FS-3820N FTP server\.\r\n| p/Kyocera FS-3820N printer ftpd/ d/printer/
match ftp m|^220 Dell Laser Printer 5100cn\r\n| p/Dell Laser Printer 5100cn ftpd/ d/printer/
match ftp m|^220 Scala FTP \(\"Scala InfoChannel Player \d+\" ([\w/.]+)\)\r\n| p/Scala InfoChannel Player ftpd/ v/$1/ d/media device/
match ftp m|^220 ([-\w_.]+) Dell Wireless Printer Adapter 3300 FTP Server| p/Dell Wireless Printer Adapter 3300 ftpd/ h/$1/ d/print server/
match ftp m|^220 RICOH Aficio MP C2500 FTP server \(([\d.]+)\) ready\.\r\n| p/Ricoh Aficio MP C2500 ftpd/ v/$1/ d/printer/
match ftp m|^220 FTP Services for ClearPath MCP:  Server version ([\d.]+)\r\n| p/Unisys ClearPath MCP ftpd/ v/$1/
match ftp m|^220 Nut/OS FTP ([\d.]+) beta ready at| p|Nut/OS Demo ftpd| v/$1/ o|Nut/OS|
match ftp m|^ftpd - accept the connection from [\d.]+\n220-eDVR FTP Server v([\d.]+) \(c\)Copyright WebGate Inc\. \w+-\w+\r\n220-Welcome to (DS\w+)\r\n220 You will be disconnected after 180 seconds of inactivity\.\r\n| p/WebGate $2 eDVR camera ftpd/ v/$1/ d/webcam/
match ftp m|^220 Canon iN-E5 FTP Print Server V([-\w_.]+) | p/Canon iN-E5 print server ftpd/ v/$1/ d/print server/
match ftp m|^220 FTP-Backupspace\r\n$| p/STRATO backup ftpd/
match ftp m|^220-.* \(([-\w_.]+)\)\r\n Synchronet FTP Server ([-\w_.]+)-Win32 Ready\r\n| p/Synchronet ftpd/ h/$1/ v/$2/ o/Windows/
match ftp m|^220 Welcome to DCS-(\w+) FTP Server\r\n$| p/D-Link DCS-$1 webcam ftpd/ d/webcam/
match ftp m|^220 X5 FTP server \(version ([\d.]+)\) ready\.\r\n| p/Zoom ADSL modem/ i/X5 $1/ d/broadband router/
match ftp m|^220 zFTPServer v([-\w_.]+), build ([-\d]+)| p/zFTPServer/ v/$1 build $2/ o/Windows/
match ftp m|^220 Welcome to zFTPServer\r\n| p/zFTPServer/ o/Windows/
match ftp m|^220 FRITZ!BoxWLAN(\d+)(?:\(UI\))? FTP server ready\.\r\n| p/FRITZ!Box WLAN $1 WAP ftpd/ d/WAP/
match ftp m|^220 FRITZ!BoxFonWLAN(\d+)(?:\(UI\))? FTP server ready\.\r\n| p/FRITZ!Box Fon WLAN $1 WAP ftpd/ d/WAP/
match ftp m|^220 FRITZ!Box Fon WLAN (\d+) FTP server ready\.\r\n| p/FRITZ!Box Fon WLAN $1 WAP ftpd/ d/WAP/
match ftp m|^220 ([-\w_.]+) FTP Server \(Oracle XML DB/Oracle9i Enterprise Edition Release ([\d.]+) - 64bit Production\) ready\.\r\n| p/Oracle XML DB ftpd/ h/$1/ v/$2/ i/64 bits/
match ftp m|^220 RICOH Aficio MP 2510 FTP server \(([-\w_.]+)\) ready\.\r\n| p/Ricoh Aficio MP 2510 printer ftpd/ d/printer/ v/$1/
match ftp m|^220 Dell Color Laser (\w+)\r\n| p/Dell Color Laser $1 printer ftpd/ d/printer/
match ftp m|^220 Dell MFP Laser (\w+)\r\n| p/Dell MFP Laser $1 printer ftpd/ d/printer/
match ftp m|^220 CompuMaster SRL, WT-6500 Ftp Server \(Version ([\d.]+)\)\.\r\n| p/CompuMaster WT-6500 ThinClient ftpd/ v/$1/ o/Windows/
match ftp m|^211 Hello \[[-\w_.]+\], Secure/IP Authentication Server ([-\w_.]+) at your service\.\r\n| p|OpenVMS Secure/IP ftpd| v/$1/ o/OpenVMS/
match ftp m|^220  HP166XC V([-\w_.]+) FUSION FTP server \(Version ([-\w_.]+)\) ready\.\r\n| p/HP166XC $1 Logic Analyzer ftpd/ i/FUSION ftpd $2/ d/specialized/
match ftp m|^220 FTP Server, type 'quote help' for help\r\n$| p/Polycom VSX 8000 ftpd/ d/webcam/
match ftp m|^550 no more people, max connections is reached\r\n| p/Avalaunch XBOX ftpd/ d/game console/ i/Max connections reached/
match ftp m|^220 Fastream IQ FTP Server\r\n| p/Fastream IQ ftpd/ o/Windows/
match ftp m|^220 RICOH Aficio SP C811DN FTP server \(([-\w_.]+)\) ready\.\r\n| p/Ricoh Aficio SP C811DN printer ftpd/ v/$1/ d/printer/
match ftp m|^220 HIOKI ftp service v([\d.]+)\r\n| p/Hioki HiCorder 8855 ftpd/ v/$1/ d/specialized/
match ftp m|^220 Treck FTP server ready\.\r\n| p/Treck Embedded ftpd/
match ftp m|^220 Microtest SuperCD-cdserver FTP server \(Version V([\w._-]+)\) ready\.\r\n| p/Axonix SuperCD ftpd/ d/media device/ v/$1/
match ftp m|^220 FTP service \(Ftpd ([\d.]+)\) ready on ([\w._-]+) at| p/Minix ftpd/ v/$1/ h/$2/ o/Minix/
match ftp m|^220 Cube Station FTP server at ([\w._-]+) ready\.\r\n| p/Synology CubeStation ftpd/ h/$1/
match ftp m|^220 Xerox Phaser (\w+)\r\n421 Service not available, closing control connection\r\n| p/Xerox Phaser $1 ftpd/ d/printer/
match ftp m|^220 CrossFTP Server ready for new user\.\r\n| p/CrossFTP java ftpd/
match ftp m|^220 ATAboy2X-\d+ FTP V([\w._-]+) ready\n| p/ATAboy2X ftpd/ d/storage-misc/ v/$1/
match ftp m|^220 Belkin Network USB Hub Ver ([\w._-]+) FTP server\.\r\n| p/Belkin USB hub ftpd/ v/$1/
match ftp m|^220-TCP/IP for VSE FTP Daemon Version ([\w._-]+) | p/VSE ftpd/ v/$1/ o/VSE/
match ftp m|^220 FTP server: Lexmark Optra LaserPrinter ready\r\n| p/Lexmark Optra LaserPrinter ftpd/ d/printer/
match ftp m|^220 NSE \(AG 5000   v([\w._-]+)\) FTP server ready\r\n| p/Nomadix AG 5000 ftpd/ d/WAP/ v/$1/
match ftp m|^220 Welcome to Easy File Sharing FTP Server!\r\n| p/Easy File Sharing ftpd/ o/Windows/
match ftp m|^220- \*+\r\n220- \r\n220-      Welcome to Dream FTP Server\r\n220-      Copyright 2002 - 2004\r\n220-      BolinTech Inc\.\r\n| p/BolinTech Dream FTP Server/ o/Windows/
match ftp m|^220 Welcome to the Netburner FTP server\.\r\n| p/Netburner embedded device ftpd/ d/specialized/
match ftp m|^220 NetBotz FTP Server ([\w._-]+) ready\.\r\n| p/NetBotz network monitor ftpd/ d/security-misc/
match ftp m|^220 TOSHIBA e-STUDIO5500c FTP server \(([\w._-]+)\) ready\.\r\n| p/Toshiba e-STUDIO5500c printer ftpd/ d/printer/ v/$1/
match ftp m|^220  \(WJ-HD220 FTP Server version ([\w._-]+) Ready\)\r\n| p/Panasonic WJ-HD220 ftpd/ d/media device/ v/$1/
match ftp m|^220 ([\w._-]+) FTP server \(EMC-SNAS: ([\w._-]+)\) ready\.\r\n| p/EMC Scalable Network Accelerator ftpd/ h/$1/ v/$2/
match ftp m|^220-CentOS release ([\w._-]+) .*\r\n220 ProFTPD ([\w._-]+) Server \(ProFTPD Default Installation\)|s p/ProFTPD/ v/$2/ i/CentOS $1/ o/Linux/
match ftp m|^220 TCAdmin FTP Server\r\n| p/Balance Servers TCAdmin game hosting ftpd/ o/Windows/
match ftp m|^.* klogd: klogd started: BusyBox v([\w._-]+) \(.*\)\r\nDoing BRCTL \.\.\.\r\nsetfilter br0 0 \r\n/var/tmp/act_firewall: No such file or directory\r\n| p/Actiontec router ftpd/ i/firewall broken; BusyBox $1/ d/broadband router/
# these should be fine. embyte
match ftp m|^220 .*BlackJumboDog Version ([^ ]+)| p/Blackjumbodog FTPd/ v/$1/
match ftp m|^220[- ] ?[Cc]rob FTP [Ss]erver [Vv]?([-.\d\w]+)| p/Crob FTPd/ v/$1/
match ftp m|^220.* GlobalSCAPE Secure FTP Server \(v\. ([^\)]+)\)| p/GlobalSCAPE Secure FTPd/ v/$1/ o/Windows/
match ftp m|^220 GlobalSCAPE Secure FTP Server\r\n| p/GlobalSCAPE Secure FTPd/ o/Windows/
match ftp m|^220 Mollensoft FTP Server ([^ ]+) Ready\.| p/Mollensoft FTPd/ v/$1/
match ftp m|^220 Welcome to Ocean FTP Server.| p/Ocean FTPd/ 
match ftp m|^220 4dftp .* FTP Service \(Version ([^)]+)\)| p/WebStar 4dftp/ v/$1/
match ftp m|^220 IBM NPS 540\+/542\+ FTP Printer Server V([\w._-]+) | p|IBM NPS 540+/542+ print server ftpd| d/print server/ v/$1/
match ftp m|^220 ([\w._-]+) FTP server \(mmftpd \(([\w._/-]+)\)\) ready\r\n| p/mmftpd/ h/$1/ v/$2/
match ftp m|^220 C500 FTP Server ([\w._-]+) ready\.\n| p/Lexmark C500 printer ftpd/ d/printer/ v/$1/
match ftp m|^220-TiMOS-\w+-([\w._-]+) cpm/hops ALCATEL ESS 7450 Copyright \(c\) 2000-2007 Alcatel-Lucent\.\r\n| p|Alcatel-Lucent ESS 7450 router ftpd| d/router/ o/TiMOS/ v/$1/
match ftp m|^220 SAVIN 8055 FTP server \(([\w._-]+)\) ready\.\r\n| p/Savin 8055 printer ftpd/ d/printer/ v/$1/
match ftp m|^220  TANDBERG    Satellite Modulator SM6600\r\n| p/Tandberg SM6600 Satellite Modulator ftpd/ d/media device/
match ftp m|^220 SUN StorEdge 3511 RAID FTP server ready\.\r\n| p/Sun StorEdge 3511 ftpd/ d/storage-misc/
match ftp m|^220 IFT ([\w._-]+) RAID FTP server ready\.\r\n| p/Infortrend EonStor $1 ftpd/ d/storage-misc/
match ftp m|^421 Closing non-secure connections in Secure Mode\. \r\n| p/Polycom VSX 7000A VoIP phone ftpd/ d/VoIP phone/
match ftp m|^220-Sami FTP Server ([\w._-]+)\r\n| p/KarjaSoft Sami ftpd/ v/$1/ o/Windows/
match ftp m|^220 DrFTPD ([\w._-]+) http://drftpd\.org\r\n| p/DrFTPD/ v/$1/
match ftp m|^220 DrFTPD\+ ([\w._-]+) \(\+STABLE\+\) \$Revision: (\d+) \$ http://drftpd\.org\r\n| p/DrFTPD/ v/$1 revision $2/
match ftp m|^220 Conti FTP Server ready\r\n| p/Conti ftpd/ o/Windows/
match ftp m|^220 Welcome to Mobile File Service\r\n\r\n| p|HTC P4000 PDA/Phone ftpd| d/PDA/ o/Windows/
match ftp m|^220 Welcome to Topfield PVR FTP server\r\n| p/Topfield HDPVR satellite decoder ftpd/ d/media device/
match ftp m|^220 ([\w._-]+) FTP server \(WS2000 FTPD Server\) ready\.\r\n| p|Motorola/Symbol WS2000 WAP ftpd| d/WAP/ h/$1/
match ftp m|^220  ADH FTP SERVER READY TYPE HELP FOR HELP \r\n| p/AD Network Video Dedicated Micros DVR ftpd/ d/webcam/
match ftp m|^220 TDS400 FTP Service \(Version ([\w._-]+)\)\.\r\n| p/TDS400 printer ftpd/ d/printer/ v/$1/
match ftp m|^220 ---freeFTPd 1\.0---warFTPd 1\.65---\r\n| p/Nepenthes HoneyTrap fake vulnerable ftpd/
match ftp m|^Can't exec \"/usr/sbin/pure-ftpd\": No such file or directory| p/Pure-FTPd under inetd/ i/Broken/ o/Unix/
match ftp m|^220- \w+\r\n220 FTP Server powered by: Quick 'n Easy FTP Server\r\n| p/Quick 'n Easy FTP Server/ o/Windows/
match ftp m|^220-National Instruments FTP\r\n220 Service Ready \r\n| p/National Instruments LabVIEW ftpd/ d/specialized/
# The ASCII spells "FREETZ".
match ftp m#^220-   __  _   __  __ ___ __\r\n220-  \|__ \|_\) \|__ \|__  \|   /\r\n220-  \|   \|\\  \|__ \|__  \|  /_\r\n220-\r\n220-   The fun has just begun\.\.\.\r\n220 \r\n# p/vsftpd/ d/WAP/ i/Freetz firmware for AVM Fritz!Box/
match ftp m|Permission denied\.\(Please check access control list\)\r\nPermission denied\.\(Please check access control list\)\r\n\n\rSystem administrator is connecting from [\d.]+\n\rReject the connection request !!!\n\r\n\rSystem administrator is connecting from [\d.]+\n\rReject the connection request !!!\n\r| p/DrayTek Vigor 2820 ADSL router ftpd/ i/access denied/ d/broadband router/
match ftp m|^220-FTPSERVE IBM VM Level (\d)(\d+) at ([\w._-]+), [^\r\n]*\r\n220 Connection will close if idle for more than 5 minutes\.\r\n| p/IBM FTPSERVE/ o|z/VM $1.$2| h/$3/
match ftp m|^220 MeritFTP ([\d.]+) at ([\d.]+) ready\.\r\n| p/Merit Megatouch game device ftpd/ d/specialized/
match ftp m|^220 NET\+OS ([\d.]+) FTP server ready\.\r\n503 Bad sequence of commands\r\n| p/NET+OS ftpd/ o/NET+OS/ i/NET+OS $1/
match ftp m|^220 Welcome to the NSLU2 vsftp daemon\.\r\n| p/vsftpd/ o/storage-misc/ i/NSLU2 NAS device/
match ftp m|^220-  Menuet FTP Server v([\d.]+)\r\n220 Username and Password required\r\n| p/Menuet FTP Server/ v/$1/ o/MenuetOS/
match ftp m|^220 Xyratex (\w+) RAID FTP server ready\.\r\n| p/Xyratex $1 RAID NAS device ftpd/ d/storage-misc/
match ftp m|^220 MLT-57066 Version ([\w.]+) ready\.\r\n| p/Minolta PagePro 20 printer ftpd/ v/$1/
match ftp m|^220 tandem FTP SERVER \w+ \(Version ([\w.]+) TANDEM \w+\) ready\.\r\n| p/Tandem FTP server/ v/$1/ o/GuardianOS/ i/Tandem Himalaya K2000/
match ftp m|^220 ZBR-(\d+) Version ([\d.]+) ready\.\r\n| p/Zebra print server ftpd/ v/$2/ i/firmware $1/
match ftp m|^220 ([\w._-]+) pSOSystem FTP server \(@\(#\)\(#\)pVER IA/MIPS, Version ([\w._ -]+), Built on ([\d/]+)\) ready\.\r\n| p/pSOSystem ftpd/ v/$2/ h/$1/ i/MIPS; build date $3/ o/pSOS/
match ftp m|^220 ([\w._-]+) pSOSystem FTP server \(@\(#\)\(#\)pVER IA/PPC, Version ([\w._ -]+), Built on ([\d/]+)\) ready\.\r\n| p/pSOSystem ftpd/ v/$2/ h/$1/ i/PowerPC; build date $3/ o/pSOS/
match ftp m|^220 ([\w._-]+) pSOSystem FTP server \(Network Utilities for /68k-MRI/([\w._-]+) - Network Utility\) ready\.\r\n| p/pSOSystem ftpd/ v/$2/ h/$1/ i/m68k/ o/pSOS/
match ftp m|^220 Star IFBD-HE05/06 FTP Server\.\r\n| p/Star Micronics TSP828L printer ftpd/ d/printer/
match ftp m|^220 Welcome to Baby FTP Server\r\n| p/Baby FTP Server/ o/Windows/
match ftp m|^220 [\w_.-]+ FTP server \(witelcom ([\d.]+)\) ready\r\n| p/Witelcom router ftpd/ d/router/
match ftp m|^220 SwiFTP ready\r\n| p/SwiFTP/ o/Linux/ d/phone/ i/Android phone/
match ftp m|^220 EFI FTP Print server ready\.\r\n| p/EFI Fiery ftpd/ d/print server/
match ftp m|^220 infotec  IS (\d+) FTP server \(([\w.]+)\) ready\.\r\n| p/Infotec IS $1 ftpd/ v/$2/
match ftp m|^220- Print Server ([\d.]+ \([^)]*\))\r\n220  FTP server \(Version ([^)]*)\) ready\.\r\n| p/Roland plotter print server ftpd/ v/$2/ i/print server version $1/
match ftp m|^220 FTP Server \(ZyWALL (USG \w+)\) \[[\w._-]+\]\r\n| p/ZyWALL $1 firewall ftpd/ d/firewall/
match ftp m|^220 Connected to IndiFTPD\r\n| p/IndiFTPD/
match ftp m|^220 EasyCoder FTP Server v\.([\d.]+) ready\.\r\n| p/Intermec PM4i printer ftpd/ v/$1/ d/printer/
match ftp m|^220 ALFTP Server ready\.  \^-\^\)/~\r\n| p/ALFTP/
match ftp m|^220 ftp server corona \(([\w._-]+)\)\r\n| p/THEOS Corona ftpd/ v/$1/ o/THEOS/
match ftp m|^220 vxTarget FTP server \(VxWorks ([\d.]+)\) ready\.\r\n| p/vxTarget ftpd/ o/VxWorks/ i/VxWorks $1/
match ftp m|^220-Welcome to the S60 Dumb FTP Server \(dftpd\)\r\n| p/Dumb FTP Server (dftpd)/ o/SymbianOS/ d/phone/
match ftp m|^220-Local time is now [\d:]+\r\n220 You will be disconnected after 300 seconds of inactivity\.\r\n| p/DViCO TVIX 6500A set top box ftpd/ d/media device/
match ftp m|^220 ET(\w{2})(\w{2})(\w{2})(\w{2})(\w{2})(\w{2}) ([\w-]+) Series FTP Server ready\.\r\n| d/printer/ p/Lexmark $1 series printer ftpd/ i/MAC: $1:$2:$3:$4:$5:$6/
match ftp m|^220 aFTPServer ready \(cwd is /\)\r\n$| p/FTPServer/ o/Linux/ d/phone/
match ftp m|^220 BCB1COOL Server \(Proftpd FTP Server\) \[([\w._-]+)\]\r\n| p/Proftpd FTP Server/ h/$1/
match ftp m|^220 FTP version ([\w.]+)\r\n331 Enter PASS command\r\n$| p/DrayTek Vigor 2820 ADSL router ftpd/ v/$1/ d/broadband router/
match ftp m|^220 Core FTP Server Version ([\w._-]+, build \d+), installed (\d+ days ago) Registered\r\n| p/Core FTP Server/ v/$1/ i/installed $2/
match ftp m|^220-.*\r\n220 ([\w._-]+) FTP Server \(Apache/([\w._-]+) \(Linux/SUSE\)\) ready\.\r\n| p/Apache mod_ftpd/ v/$2/ h/$1/ o/Linux/
match ftp m|^220 pyftpdlib ([\w._-]+) ready\.\r\n214-The following commands are recognized:\r\n ABOR   ALLO   APPE   CDUP   CWD    DELE   EPRT   EPSV  \r\n FEAT   HELP   LIST   MDTM   MKD    MLSD   MLST   MODE  \r\n NLST   NOOP   OPTS   PASS   PASV   PORT   PWD    QUIT  \r\n REIN   REST   RETR   RMD    RNFR   RNTO   SIZE   STAT  \r\n STOR   STOU   STRU   SYST   TYPE   USER   XCUP   XCWD  \r\n XMKD   XPWD   XRMD  \r\n214 Help command successful\.\r\n$| p/pyftpdlib/ v/$1/
match ftp m|^220 Simple FTP daemon coming up!\r\n| p/A+V Link NVS-4000 surveillance system ftpd/ d/webcam/
match ftp m|^220 DiskStation FTP server ready\.\r\n| p/Synology DiskStation NAS ftpd/ d/storage-misc/
# "1.0" number doesn't seem to reflect the true version number.
match ftp m|^220- Ftp Site Powerd by BigFoolCat Ftp Server 1\.0 \(meishu1981@163\.com\)\r\n220- Welcome to my ftp server\r\n220 \r\n| p/EasyFTP Server ftpd/ o/Windows/
match ftp m|^220 (FS-\d+DN) FTP server\r\n| p/Kyocera $1 printer ftpd/ d/printer/
match ftp m|^220 <1e2400fc>  Tenor Multipath Switch FTP server \(Version VxWorks([\w._-]+)\) ready\.\r\n| p/Tenor Multipath Switch ftpd/ d/switch/ o/VxWorks $1/
match ftp m|^220 Imagistics ZB3500080 Ver ([\w._-]+) FTP server\.\r\n| p/Sharp AR-C260M or AR-M351N printer ftpd/ v/$1/ d/printer/
match ftp m|^220 ([\w._-]+) FTP SERVER T9552G07 \(Version ([\w._-]+) TANDEM ([\w._-]+)\) ready\.\r\n| p/HP Tandem NonStop ftpd/ v/$2 $3/ h/$1/
match ftp m|^220 iFTP server v([\w._-]+)\n| p/inLighten iBox digital signage ftpd/ v/$1/ d/media device/
match ftp m|^120 The user queue is full, please try again later\.\r\n| p/Huawei Quidway AR28-09 WAP ftpd/ d/WAP/ i/user queue is full/
match ftp m|^220 Mabry \(FtpServX COM Object\) server ready\.\r\n| p/Mabry FTPServX/
match ftp m|^220 ([\w._-]+) FTP server \(InterCon version ([\w._-]+)\) ready\.\r\n| p/Kyocera Mita TASKalfa 300ci printer ftpd/ v/$2/ h/$1/
match ftp m|^220 [\w._-]+Citizen_CLP([\w._-]+) FTP server \(InterCon version ([\w._-]+)\) ready\.\n| p/Citizen CLP-$1 label printer ftpd/ v/$2/ d/printer/
match ftp m|^220 FileApp - FTP Server\r\n| p/DigiDNA FileApp ftpd/ o/iOS/
match ftp m%^220 (?:SHARP|Sharp) ([\w._-]+) Ver ([\w._+-]+) FTP server\.\r\n% p/Sharp $1 printer ftpd/ v/$2/
match ftp m|^220 Nucleus FTP Server \(Version ([\w._-]+)\) ready\.\r\n| p/Nucleus ftpd/ v/$1/
match ftp m|^220 -= HyNetOS FTP Server =-\r\n500 Command \(null\) not understood\r\n| p/HyNetOS ftpd/

#(insert ftp)

# not already sure about the next. maybe too generic? it exists already above a signature for openftpd. embyte
match ftp m|^220 OpenFTPD server([^ ]+)?| p/OpenFTPD/ v/$1/

match ftp-proxy m|^220 Ftp service of Jana-Server ready\r\n| p/JanaServer ftp proxy/ o/Windows/
match ftp-proxy m|^220 FTP Gateway at Jana Server ready\r\n| p/JanaServer ftp proxy/ o/Windows/
match ftp-proxy m|^220 ([-.\w]+) FTP proxy \(Version (\d[-.\w]+)\) ready\.\r\n| p/Guantlet FTP proxy/ v/$1/
# Frox FTP Proxy (frox-0.6.5) on Linux 2.2.X - http://frox.sourceforge.net/
match ftp-proxy m|^220 Frox transparent ftp proxy\. Login with username\[@host\[:port\]\]\r\n| p/Frox ftp proxy/
match ftp-proxy m|^501 Proxy unable to contact ftp server\r\n| p/Frox ftp proxy/
match ftp-proxy m|^220 ([-.+\w]+) FTP AnalogX Proxy (\d[-.\w]+) \(Release\) ready\r\n| p/AnalogX FTP proxy/ h/$1/ v/$2/
match ftp-proxy m|^220 Secure Gateway FTP server| p/Symantec Enterprise Firewall FTP proxy/ d/firewall/
match ftp-proxy m/^220-Sidewinder ftp proxy\.  You must login to the proxy first/ p/Sidewinder FTP proxy/
match ftp-proxy m/^220-\r\x0a220-Sidewinder ftp proxy/s p/Sidewinder FTP proxy/
match ftp-proxy m|^220 webshield2 FTP proxy ready\.\r\n| p/Webshield2 FTP proxy/ o/Windows/
match ftp-proxy m|^220 WinProxy FTP Gateway ready, enter username@host\[:port\]\r\n| p/WinProxy FTP proxy/ o/Windows/
match ftp-proxy m|^220 WinProxy \(Version ([^)]+)\) ready\.\r\n| p/WinProxy FTP proxy/ v/$1/ o/Windows/
match ftp-proxy m|^220 Proxy602 Gateway ready, enter user@host\[:port\]\r\n| p/Proxy602 ftp proxy/ d/firewall/
match ftp-proxy m|^220 Java FTP Proxy Server \(usage: USERID=user@site\) ready\.\r\n| p/Java FTP Proxy/
match ftp-proxy m|^220 ([-\w_.]+) FTP proxy \(Version V([\d.]+)\) ready\.\r\n| p/Generic FTP proxy/ v/$2/ h/$1/
match ftp-proxy m|^220 CoolProxy FTP server & firewall\r\n| p/CoolProxy ftp proxy/ o/Windows/
match ftp-proxy m|^220 Finjan SurfinGate Proxy - Server Ready\.\r\n| p/Finjan SurfinGate ftp proxy/
match ftp-proxy m|^220 ([-\w_.]+) \(NetCache\) .*\r\n| p/NetApp NetCache ftp proxy/ h/$1/
match ftp-proxy m|^220 Welcome to ([-\w_.]+) Ftp Proxy Service\.\r\n| p/Proxy Suite ftp proxy/ h/$1/
match ftp-proxy m|^220 Hi! Welcome \w+ UserGate| p/UserGate ftpd/ o/Windows/
match ftp-proxy m|^220 Webwasher FTP Proxy ([\d.]+) build (\d+)\r\n| p/Webwasher ftp proxy/ v/$1 build $2/ o/Windows/
match ftp-proxy m|^220- ([-\w_.]+) PROXY-FTP server \(DeleGate/([\d.]+)\) ready\.\r\n| p/DeleGate ftp proxy/ v/$2/ h/$1/
match ftp-proxy m|^500 WinGate Engine Access Denied\r\n| p/WinGate ftp proxy/ i/access denied/ o/Windows/
match ftp-proxy m|^220 IWSS FTP proxy ready\r\n| p/Trend Micro InterScan Web Security Suite ftp proxy/
match ftp-proxy m|^220 ezProxy FTP Proxy Server Ready \r\n| p/ezProxy ftp proxy/ o/Windows/
match ftp-proxy m|^220 FTP proxy \(v([\d.]+)\) ready\r\n530 Login incorrect\. Expected USER command\r\n| p/jftpgw ftp proxy/ v/$1/
match ftp-proxy m|^220-Welcome to SpoonProxy V([\w._-]+) by Pi-Soft Consulting, LLC\r\n| p/Pi-Soft SpoonProxy ftp proxy/ v/$1/ o/Windows/
match ftp-proxy m|^220-CCProxy FTP Service\(Unregistered\)\r\n| p/CCProxy ftp proxy/ i/unregistered/ o/Windows/
match ftp-proxy m|^220 kingate\(([\w._-]+)-win32\) ftp proxy ready\r\n| p/kingate ftp proxy/ v/$1/ o/Windows/
match ftp-proxy m|^220 FileCatalyst Server Enterprise v([^\r\n]*)\r\n$| p/FileCatalyst ftp proxy/ v/$1/
match ftp-proxy m|^220 ([\w._-]+), KEN! DSL FTP-Gateway\r\n| p/AVM KEN! ftp proxy/ h/$1/
match ftp-proxy m|^220 ([\w._-]+), KEN! FTP-Gateway\r\n| p/AVM KEN! ftp proxy/ h/$1/

# TODO kerio?
#match ftp m|^421 Service not available \(The FTP server is not responding\.\)\n$| v/unknown FTP server//service not responding/
match vdr m|^220 (\S+) SVDRP VideoDiskRecorder (\d[^\;]+);| p/VDR/ h/$1/ v/$2/ d/media device/
match vdr m|^Access denied!\n$| p/VDR/ d/media device/

softmatch ftp m/^220 Welcome to ([-.\w]+) FTP.*\r\n$/i h/$1/
softmatch ftp m/^220 ([-.\w]+) [-.\w ]+ftp.*\r\n$/i h/$1/
softmatch ftp m/^220-([-.\w]+) [-.\w ]+ftp.*\r\n220/i h/$1/
softmatch ftp m/^220 [-.\w ]+ftp.*\r\n$/i
softmatch ftp m/^220-[-.\w ]+ftp.*\r\n220/i
softmatch ftp m/^220[- ].*ftp server.*\r\n/i
softmatch ftp m/^220-\r?\n220 - ftp/i

match freeswitch-event m|^Content-Type: auth/request\n\n| p/FreeSWITCH mod_event_socket/

match fsae m|^\0\0\0\\\x80\x06\0\0\0\n\x01\x03\0\x01\x86\xaf\0\0\0\n\x10\x03\0\0\0\x01\0\0\0\x15\x11\x05FSAE server ([\d.]+)\0\0\0\x16\x12\x01................\0\0\0\x17\x13\x01FSAE_SERVER_\d+$|s p/Fortinet Server Authentication Extension/ v/$1/

match fw1-rlogin m|^\0Check Point FireWall-1 authenticated RLogin server running on ([-.\w]+)\r\n\r| p/Check Point FireWall-1 authenticated RLogin server/ i/$1/

match fyre m|^220 Fyre rendering server ready\n| p/Fyre rendering cluster node/

match g15daemon m|^G15 daemon HELLO$| p/g15daemon/ i/Logitech G15 keyboard control/

match galaxy m|^\0\0\0\t\0\0\0\x80\0\0\0\0\0\0\0\0\0\0\x042\0\0\0\x01\0\0\t_\0\0\0h| p/Galaxy Client Event Manager/ o/Windows/

match gamebots m|^HELLO_BOT\r\n| p/GameBots for Unreal Tournament 2004/
match gamebots-control m|^HELLO_CONTROL_SERVER\r\n| p/GameBots for Unreal Tournament 2004 control server/

match geovision-mobile m|^D3\x22\x11\0\0\0\0\xc6\x11\0\0\xae\x15\0\0$| p/Geovision mobile device support/

match gnats m|^200 ([-.\w]+) GNATS server (\d[-.\w]+) ready\.\r\n| p/GNATS bugtracking system/ h/$1/ v/$2/

match ganglia m|^<\?xml version=\"1\.0\".*<!DOCTYPE GANGLIA_XML.*<GANGLIA_XML VERSION=\"([^\"]+)\" SOURCE=\"([^\"]+)\">.*<CLUSTER NAME=\"([^\"]+)\" LOCALTIME=\"\d+\" OWNER=\"([^\"]+)\"|s p/Ganglia XML Grid monitor/ v/$1/ i/Cluster name: $3; Owner: $4; Source: $2/ d/specialized/

match goldsync m|^%%QU%%QU%%QU$| p/GoldMine GoldSync synchronization/

# Probably not general enough...
match gnatbox m|^GBPK\xfb\xf7n\x93W\xaf\x86\x93x@\xa9\x0e\xca\*\x9bS\0| p/GNATBox firewall administration/ d/firewall/

softmatch gkrellm m|^<error>\nClient limit exceeded\.\n| p/GKrellM System Monitor/
softmatch gkrellm m|^<error>\nConnection not allowed from .*\n| p/GKrellM System Monitor/

match gopher m|^3Connection to [\d.]+ is denied -- no authorization\.\r\n$|
match g6-remote m|^200 1400\r\n$| p/G6 ftpd remote admin/ o/Windows/

match giop m|^GIOP\x01...\0\0\0\0|s p/CORBA naming service/

# CompTek AquaGateKeeper (Telephony package) http://aqua.comptek.ru
match H.323-gatekeeper m|^\x03\0\0.*@|s p/CompTek AquaGateKeeper/
# OpenH323 Gatekeeper 2.0.3
match H.323-gatekeeper m|^\xff\xfd\x03\xff\xfb\x05.*Version:\r\nGatekeeper\(GNU\) Version\(([\d.]+)\) Ext\(.*\) Build\(.*\) Sys\(Linux .*\)\r\n| p/OpenH323 Gatekeeper/ v/$1/ o/Linux/
# Causes false matches with telnet.
# match H.323-gatekeeper m|^\xff\xfd.$| p|GNU Gatekeeper|
match H.323-gatekeeper m|^\xff\xfd\x03\xff\xfb\x05\xff\xfe\x01\r\nAccess forbidden!\r\n$| p/GNU Gatekeeper/
match H.323-gatekeeper m|^\x03\0\0\.\x08\x02\0\0Z~\0\"\x05%\xc0\x06\0\x08\x91J\0\x02X\x08\x11\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\x02\x80\x01\0$| p/GNU Gatekeeper/

# Returns ASCII data in the following format:
# |HardDrive1DevName|HardDrive1HardwareID|HardDrive1Temp|TempUnit|
# |HardDrive2DevName|HardDrive2HardwareID|HardDrive2Temp|TempUnit|
match hddtemp m+^\|/dev/[hs]\w\w\|+ p/hddtemp hard drive info server/
match hddtemp m+^\|$+ p/hddtemp hard drive info server/

match helpdesklog m|^Helpdesk Advanced ([\d.]+) License Logging Service| p/Helpdesk Advanced license server/ v/$1/

match honeywell-ripsd m|^\0\x10\x03\x0c$| p/Honeywell ripsd power management server/

match hptsvr m|^\(\0\0\0hpt_stor\x01\xea\xe0\xbf\0\0\0\0\0\0\0\0XRiu\.\.\.E\0\0\0\0\0\0\0\0$| p/HighPoint RAID management service/
match hptsvr m|^\(\0\0\0\0\0\0\0..`\0\x01\xff\xff\xff\xcc\xfa\x85\0C\x1d\xe6whfnk\.\.\.E\0\0\0\0\0\0\0\0$| p/HighPoint RAID management service/

match hpiod m|^msg=MessageError\nresult-code=5\n$| p/HP Linux Imaging and Printing System/

# And now for some SORRY web servers that just blurt out an http "response" upon connection!!!
match http m|^HTTP/1\.1 200 OK\r\nContent-type: text/html\r\nExpires: .*\r\nDate: .*\r\nPragma: no-cache\r\nCache-Control: no-cache\r\n\r\n<HTML><TITLE>JAP</TITLE>\n| p/Java Anonymous Proxy/
match http m|^HTTP/1.0 500\r\nContent-type: text/plain\r\n\r\nNo Scan Capable Devices Found\r\n| p/HP Embedded Web Server remote scan service/ i/no scanner found/ d/printer/
# SMC Barricade 7004ABR
match http m|^HTTP/1\.0 301 Moved\r\nLocation: http://\d+\.\d+\.\d+\.\d+:88\r\n| p/SMC Barricade broadband router/ i/simply redirects to real web admin port 88/ d/broadband router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: SonicWALL\r\n| p/SonicWALL firewall http config/ d/firewall/
match http m|^HTTP/1\.0 500 Internal Server Error\r\nDate: .*\r\nContent-type: text/html\r\nExpires: .*\r\n\r\n<H1>500 Internal Server Error</H1>\r\n\r\n\r\n| p/Cisco Catalyst http config/ d/switch/ o/IOS/
match http m|^HTTP/1\.1 200 OK\nMax-Age: 0\nExpires: 0\nCache-Control: no-cache\nCache-Control: private\nPragma: no-cache\nContent-type: multipart/x-mixed-replace;boundary=BoundaryString\n\n--BoundaryString\n| p/Motion Webcam gateway httpd/
match http m|^HTTP/1\.[01] 200 OK\r\nServer: Motion/([\d.]+)\r\n| p/Motion Camera httpd/ v/$1/ d/webcam/
match http m|^HTTP/1\.1 200 OK\r\nServer: Motion-httpd/([\d.]+)\r\n| p/Motion-httpd/ v/$1/ d/webcam/
match http m|^HTTP/1\.1 \d\d\d .*\nServer: Motion/([\d.]+)\n.*\nContent-type: image/jpeg\n|s p/Motion webcam httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nContent-Type: text/plain\r\nServer: WPA/([-\w_.]+)\r\n\r\n| p/Glucose WeatherPop Advanced httpd/ v/$1/ o/Mac OS X/
match http m|^HTTP/1\.0 503 R\r\nContent-Type: text/html\r\n\r\nBusy$| p/D-Link router http config/ d/router/
match http m|^<HEAD><TITLE>501 Not Implemented</TITLE></HEAD>\n<BODY><H1>501 Not Implemented</H1>\nThe server has not implemented your request type\.<BR>\n</BODY>\r\n$| p/Hummingbird Document Manager httpd/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\n\r\n<html>\n<body>\n<ul><li>\n<i>[^<]+</i>\n<ul><li>\n<i>Nice</i>\n<ul><li>\nNumber: \d+</li></ul>\n<i>ProgramArguments</i>\n<ol>\n<li>String: [^<]+</li>\n| p/Apple lanuchd_debug httpd/ o/Mac OS X/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\n\r\n<html>\n<body>\n<ul><li>\n<i>com\.apple\.KernelEventAgent</i>\n| p/Apple launchd_debugd httpd/ o/Mac OS X/
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: Speed Touch WebServer/([\d.]+)\r\n| p|Alcatel/Thomson SpeedTouch ADSL http config| v/$1/ d/broadband router/
match http m|^HTTP/1\.1 408 Request Time-Out\r\nConnection: Close\r\n\r\n$| p/Konica Minolta bizhub printer http config/ d/printer/
match http m|^HTTP/1\.1 400 Bad Request\r\n.*\r\n\r\n<h1>Bad Request \(Invalid Verb\)</h1>|s p/Microsoft IIS httpd/ o/Windows/
match http m|^<HTML><BODY><CENTER>Authentication failed</CENTER></BODY></HTML>\r\n$| p/InterSect Alliance SNARE http config/
match http m|^HTTP/1\.1 408 Request Timeout\nContent-Length:0\nContent-Type:text/html;charset=UTF-8\n\n$| p/Finchsync PocketPC Synchonizer httpd/
match http m|^HTTP/1\.1 200 OK\nServer: NetSupport Gateway/([\d.]+) \(Windows NT\)\nContent-Type: application/x-www-form-urlencoded\nContent-Length:    14\nConnection: Keep-Alive\n\nCMD=HEARTBEAT\n$| p/NetSupport Gateway httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\nCache-Control: no-cache\r\nExpires: Thu, 26 Oct 1995 00:00:00 GMT\r\nTransfer-Encoding: chunked\r\nServer: Allegro-Software-RomPager/([\d.]+)\r\n\r\n| p/Allegro RomPager/ v/$1/ i/Dell DRAC config/ d/remote management/
# This can inhibit a more informative GetRequest.
# match http m|^HTTP/1\.1 400 Bad Request\r\nServer: micro_httpd\r\n| p/micro_httpd/ i/ADSL router/ d/broadband router/ o/Linux/
# http://code.google.com/p/free-android-apps/wiki/Project_LocalHTTPD
match http m|^HTTP/1\.0 500 Internal Server Error \r\nContent-Type: text/plain\r\nDate: .*\r\n\r\nSERVER INTERNAL ERROR: Invalid ip\.$| p/Local HTTPD/ i/based on NanoHTTPD/ d/phone/
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: httpd-impacct/([^\r\n]+)\r\nContent-type: text/html\r\n\r\n<HTML><HEAD><TITLE>400 Bad Request</TITLE></HEAD>\n<BODY BGCOLOR=\"#cc9999\"><H2>400 Bad Request</H2>\nYour request has bad syntax or is inherently impossible to satisfy\.\n<HR>\n</HTML>\n$| p/httpd-impacct/ v/$1/ i/Asotel Vector 1908 switch http config/ d/switch/
match http m|^HTTP/1\.1 200 OK\r\nServer: DVBViewer \(Windows\)\r\nContent-Type: video/mpeg2\r\n\r\n\r\n| p/DVBViewer digital TV viewer httpd/ o/Windows/
match http m|^HTTP/1\.1 400 Bad Request\r\nserver: kolibri-([\w._-]+)\r\ncontent-type: text/plain\r\ncontent-length: 11\r\n\r\nBad Request$| p/Kolibri web application framework/ v/$1/
match http m|^HTTP/1\.1 405 Method Not Allowed\r\nServer: remote-potato-v([\w._-]+)\r\n| p/Remote Potato media player/ v/$1/
# The date reveals the time zone instead of using GMT.
match http m|^HTTP/1\.1 405 Method Not Allowed\r\nDate: ([^\r]+)\r\nServer: Embedthis-Appweb/([\w._-]+)\r\n| p/Embedthis-Appweb/ v/$2/ i/date: $1/
match http m|^HTTP/1\.1 400 Bad Request\r\nServer: Microsoft-Cassini/([\w._-]+)\r\n| p/Microsoft Cassini httpd/ v/$1/
match http m|^HTTP/1\.1 408 Request Timeout\r\nServer: WebSphere Application Server/([\w._-]+)\r\nContent-Type: text/html\r\nContent-Length: 117\r\n| p/IBM WebSphere Application Server/ v/$1/
match http m|^HTTP/1\.0 200 Ok Welcome to VOC\r\nServer: Voodoo chat daemon ver ([\w._ -]+)\r\nContent-type: text/html\r\nExpires: Mon, 08 Apr 1976 19:30:00 GMT\+3\r\nConnection: close\r\nKeep-Alive: max=0\r\nCache-Control: no-store, no-cache, must-revalidate\r\nCache-Control: post-check=0, pre-check=0\r\nPragma: no-cache\r\n\r\n$| p/Voodoo http chat daemon/ v/$1/
match http m|^HTTP/1\.1 400 Bad Request\r\nServer: Cassini/([\w._-]+)\r\n.*<style type=\"text/css\">\r\n        \t          body {margin:0; padding:0; color:Black; background-color:#BABED1;}\r\n|s p/Cassini httpd/ v/$1/ i/Sonic Foundry Mediasite Service Manager/
match http m|^HTTP/1\.1 200 OK\r\nServer: Menuet\r\nConnection: close\r\nContent-Length: 0\d+\r\nContent-Type: image/bmp\r\n\r\n| p/MenuetOS webcam server/ o/MenuetOS/

# This is here for NULL probe cheat since several probes unpredictably trigger it -Doug
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: OfficeScan Client\r\nContent-Type: text/plain\r\nAccept-Ranges: bytes\r\nContent-Length: 4\r\n\r\nFail| p/Trend Micro OfficeScan Antivirus http config/ o/Windows/

match http-proxy m=^HTTP/1\.[01] \d\d\d .*\r\n(Server|Proxy-agent): iPlanet-Web-Proxy-Server/([\d.]+)\r\n=s p/iPlanet web proxy/ v/$2/

match hp-gsg m|^220 JetDirect GGW server \(version (\d[.\d]+)\) ready\r\n| p/HP JetDirect Generic Scan Gateway/ v/$1/ d/printer/
match hp-gsg m|^220 HP GGW server \(version ([\w._-]+)\) ready\r\n\0| p/HP Generic Scan Gateway/ v/$1/ d/printer/

# http://h20000.www2.hp.com/bizsupport/TechSupport/Document.jsp?objectID=bpj01014
match hp-gsg m|^00$| p/IEEE 1284.4 scan peripheral gateway/ d/printer/
match hp-gsg m|^01$| p/IEEE 1284.4 scan peripheral gateway/ d/printer/ i/in use/
match hp-gsg m|^02$| p/IEEE 1284.4 scan peripheral gateway/ d/printer/ i/connection error/

match hylafax m|^220 ([-.\w]+) server \(HylaFAX \(tm\) Version (\d[-.\w]+)\) ready\.\r\n$| p/HylaFAX/ h/$1/ v/$2/ o/Unix/
# Hylafax 4.1.6 on Linux 2.4
match hylafax m|^130 Warning, client address \"[\d.]+\" is not listed for host name \"([-.\w]+)\"\.\r\n| p/HylaFAX/ i/IP unauthorized/ h/$1/
match hylafax m|^130 Warning, no inverse address mapping for client host name \"[-\w_.]+\"\.\r\n220 ([-\w_.]+) server \(HylaFAX \(tm\) Version ([\d.]+)\) ready\.\r\n| p/HylaFAX/ i/Reverse DNS unauthorized/ h/$1/ v/$2/

match ichat m|^\r\n                                Welcome To\r\n                             ichat ROOMS (\d[-.\w]+)\r\n==| p|^iChat Rooms| v|$1|

match ice m|^IceP\x01\0\x01\0\x03\0\x0e\0\0\0| p/Internet Communications Engine/

match ident m|^flock\(\) on closed filehandle .*midentd| p/midentd/ i/broken/
match ident m|^nullidentd -- version (\d[-.\w]+)\nCopyright | p/Nullidentd/ v/$1/ i/broken/
match ident m|^\d+, \d+ : USERID : FreeBSD : \[x\]-\d+\r\n| p/FreeBSD authd/ o/FreeBSD/

match ilom-remote-console m|^IUSB    \0\0\0\x007\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\xf1\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\x01\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0$| p/Sun Interactive Lights Out Manager or SuperMicro IPMI remote console/ d/remote management/

match imap m|^\* OK ([-/.+\w]+) Solstice \(tm\) Internet Mail Server \(tm\) (\d[-.\w]+) IMAP4 service - at | p/Sun Solstice Internet Mail Server imapd/ h/$1/ v/$2/ o/Unix/
match imap m|^\* OK GroupWise IMAP4rev1 Server Ready\r\n| p/Novell GroupWise imapd/ o/Unix/
match imap m|^\* OK \[CAPABILITY IMAP4rev1 .*\] GroupWise Server Ready\r\n| p/Novell GroupWise imapd/ o/Unix/
match imap m|^\* OK dbmail imap \(protocol version 4r1\) server (\d[-.\w]+) ready to run\r\n| p/DBMail imapd/ v/$1/ i/imapd version may differ from overal dbmail version number/
match imap m|^\* OK ([-.+\w]+) NetMail IMAP4 Agent server ready | p/Novell NetMail imapd/ h/$1/ o/Unix/
match imap m|^\* OK IMAP4 Server \(IMail ([-.\w]+)\)| p/IMail imapd/ v/$1/
match imap m|^\* OK Merak (\d[-.\w]+) IMAP4rev1 |i p/Merak Mail Server imapd/ v/$1/ o/Windows/
match imap m|^\* OK ([-.+\w]+) IMAP4rev1 Mercury/32 v(\d[-.\w]+) server ready\.\r\n| p|Mercury/32 imapd| h/$1/ v/$2/ o/Windows/
match imap m|^\* OK ([-.\w]+) IMAP4 service \(Netscape Messaging Server (\d[-.\w ]+) \(built ([\w ]+)\)\)\r\n| p/Netscape Messaging Server Imapd/ h/$1/ v/$2/ i/built $3/
match imap m|^\* OK \[CAPABILITY .*\] ([-.\w]+) IMAP4rev1 (20[\w.]+) at | p/UW imapd/ h/$1/ v/$2/
match imap m|^\* OK eXtremail V(\d[-.\w]+) release (\d+) IMAP4 server started\r\n| p/eXtremail IMAP server/ v/$1.$2/
match imap m|^\* OK eXtremail V(\d[-.\w]+) release (\d+) rev(\d+) IMAP4 server started\r\n| p/eXtremail IMAP server/ v/$1.$2.$3/
match imap m|^\* OK ([-.\w]+) NetMail IMAP4 Agent server ready <.*>\r\n| p/Novell NetMail imapd/ h/$1/ o/Unix/
# Alt-N MDaemon 6.5.1 imap server on Windows XP
match imap m|^\* OK ([-.\w]+) IMAP4rev1 MDaemon (\d[-.\w]+) ready\r\n| p/Alt-N MDaemon imapd/ v/$2/ h/$1/ o/Windows/
match imap m|^\* OK ([-.\w]+) IMAP4rev1 MDaemon (\d[-.\w]+) listo\r\n| p/Alt-N MDaemon imapd/ v/$2/ h/$1/ i/Spanish/ o/Windows/
# Dovecot IMAP Server - http://dovecot.procontrol.fi/
match imap m|^\* OK [Dd]ovecot ready\.\r\n| p/Dovecot imapd/
match imap m|^\* OK [Dd]ovecot MUA ready\r\n| p/Dovecot MUA imapd/
match imap m|^\* OK \[CAPABILITY IMAP4rev1 SORT THREAD=REFERENCES MULTIAPPEND UNSELECT LITERAL\+ IDLE CHILDREN NAMESPACE LOGIN-REFERRALS [^\]]+\]| p/Dovecot imapd/
match imap m|^\* OK \[CAPABILITY IMAP4rev1 SASL-IR SORT THREAD=REFERENCES MULTIAPPEND UNSELECT LITERAL\+ IDLE CHILDREN NAMESPACE LOGIN-REFERRALS| p/Dovecot imapd/ i/SASL enabled/
match imap m|^\* OK \[[^\[]+\] Dovecot ready\.\r\n| p/Dovecot imapd/
match imap m|^\* OK Welcome to [^.]+\. Dovecot ready\.\r\n| p/Dovecot imapd/
match imap m|^\* OK Dovecot at ([-\w_.]+) is ready\.\r\n| p/Dovecot imapd/ h/$1/
match imap m|^\* OK.*?Courier-IMAP ready\. Copyright 1998-(\d+) Double Precision, Inc\.  See COPYING for distribution information\.\r\n| p/Courier Imapd/ i/released $1/
match imap m|^\* OK \[CAPABILITY IMAP4rev1 .*?Courier-IMAP ready\. Copyright 1998-\d+ Double Precision, Inc\.  See COPYING for distribution information\.\r\n| p/Courier IMAP4rev1 imapd/
match imap m|^\* OK CommuniGate Pro IMAP Server ([-.\w]+) at ([-.\w]+) ready\r\n$| p/CommuniGate Pro imapd/ h/$1/ v/$2/
# W-Imapd-SSL v2001adebian-6
match imap m|^\* OK \[CAPABILITY IMAP4REV1 X-NETSCAPE LOGIN-REFERRALS STARTTLS AUTH=LOGIN\](\S+) IMAP4rev1 ([-.\w]+) at| p/UW imapd/ h/$1/ v/$2/
match imap m|^\* OK Domino IMAP4 Server Release (\d[-.\w ]+) +ready +(.*)\r\n| p/Lotus Domino imapd/ v/$1/ i/date: $2/
match imap m|^\* OK Domino IMAP4 Server Build V([\w_]+ Beta \w+) ready .*\r\n| p/Lotus Domino imapd/ v/$1/
match imap m|^\* BYE Domino IMAP4 Server Unable to authenticate session\.| p/Lotus Domino imapd/ i/Unable to connect/
match imap m|^\* OK \[CAPABILITY IMAP4rev1 CHILDREN NAMESPACE\] Freemail ready - hit me with your rhythm stick\.\r\n| p/Freemail imapd/
match imap m|^\* OK AVM KEN!4 IMAP Server ready\r\n| p/AVM KEN! imapd/

# MS Exchange
match imap m|^\* OK Microsoft Exchange IMAP4rev1 server version ([-.\w]+) | p/Microsoft Exchange imapd/ v/$1/ o/Windows/
match imap m|^\* OK Microsoft Exchange 2000 IMAP4rev1 server version (\d[-.\w]+) \([-.\w]+\) ready\.\r\n| p/Microsoft Exchange 2000 imapd/ v/$1/ o/Windows/
match imap m|^\* BYE Connection refused\r\n| p/Microsoft Exchange imapd/ i/refused/ o/Windows/
match imap m|^\* OK Microsoft Exchange Server ([\d]+) IMAP4rev1 server version (\d[-.\w]+) \(([-.\w]+)\) ready\.\r\n| p/Microsoft Exchange Server $1 imapd/ v/$2/ o/Windows/ h/$3/
match imap m|^\* OK Der Microsoft Exchange Server \(IMAP4rev1, Version (\d[-.\w]+) \([-.\w]+\)\) steht zur Verf\xfcgung\.\r\n| p/Microsoft Exchange 2000 imapd/ v/$1/ o/Windows/ i/German/
match imap m|^\* OK Der Microsoft Exchange Server 2003 IMAP4rev1-Server, Version ([\d.]+) \(([-\w_.]+)\), steht zur Verf\xfcgung\.\r\n| p/Microsoft Exchange 2003 imapd/ v/$1/ h/$2/ o/Windows/ i/German/
match imap m|^\* OK Microsoft Exchange IMAP4rev1 kiszolg\xe1l\xf3 verzi\xf3 (\d[-.\w]+) \(([-.\w]+)\) k\xe9sz\r\n| p/Microsoft Exchange Server imapd/ v/$1/ o/Windows/ h/$2/ i/Hungarian/
match imap m|^\* OK Server Microsoft Exchange IMAP4rev1 verze ([\d.]+) \(([-\w_.]+)\) je p\xf8ipraven\.\r\n| p/Microsoft Exchange Server imapd/ v/$1/ o/Windows/ h/$2/ i/Czech/
match imap m|^\* OK La version ([\d.]+) \(([-\w_.]+)\) du serveur IMAP4rev1 Microsoft Exchange est pr\xeate\r\n| p/Microsoft Exchange Server imapd/ v/$1/ o/Windows/ h/$2/ i/French/
match imap m|^\* OK Microsoft Exchange Server 2003 IMAP4rev1 \xb7\xfe\xce\xf1\xc6\xf7\xb0\xe6\xb1\xbe ([\d.]+) \(([-\w_.]+)\)| p/Microsoft Exchange 2003 imapd/ v/$1/ o/Windows/ h/$2/ i/Korean/
match imap m|^\* OK Microsoft Exchange Server 2003 IMAP4rev1 \xbc\xad\xb9\xf6 \xb9\xf6\xc0\xfc ([\d.]+) \(([-\w_.]+)\)| p/Microsoft Exchange 2003 imapd/ v/$1/ o/Windows/ h/$2/ i/Korean/
match imap m|^\* OK Servidor IMAP4rev1de Microsoft Exchange Server 2003 versi\xf3n ([\w._-]+) \(([\w._-]+)\) listo\.\r\n| p/Microsoft Exchange Server 2003 imapd/ v/$1/ h/$2/ i/Spanish/ o/Windows/
match imap m|^\* OK Microsoft Exchange Server 2007 IMAP4 service ready\r\n| p/Microsoft Exchange 2007 imapd/ o/Windows/
match imap m|^\* OK The Microsoft Exchange IMAP4 service is ready\.\r\n| p/Microsoft Exchange 2007-2008 imapd/ o/Windows/
match imap m|^\* OK IMAP4rev1 Server DeskNow \(DeskNow ([\w._-]+)\) ready\r\n| p/DeskNow imapd/ v/$1/

match imap m|^\* OK \[CAPABILITY (IMAP4 )?IMAP4REV1 .*IMAP4rev1 (200\d\.[-.\w]+) at| p/UW imapd/ v/$2/
match imap m|^\* OK (?:\[CAPABILITY IMAP4[^\]]*?\] )?([-.\w]+) Cyrus IMAP4? v([-.\w\+]+) server ready\r\n| p/Cyrus imapd/ h/$1/ v/$2/
match imap m|^\* OK (?:\[CAPABILITY IMAP4[^\]]*?\] )?([-.\w]+) Cyrus IMAP4? v([-.\w\+]+) server ready\r\n| p/Cyrus imapd/ h/$1/ v/$2/
match imap m|^\* OK ([-.\w]+) Cyrus IMAP4 v([-.\w\+]+)-Red Hat [-.\w\+]+ server ready\r\n| p/Cyrus imapd/ h/$1/ v/$2/ i/RedHat/ o/Linux/
match imap m|^\* OK ([-\w_.]+) Cyrus IMAP4 v([-\w_.]+)-Debian| p/Cyrus imapd/ h/$1/ v/$2/ o/Linux/ i|Debian/Ubuntu|
match imap m|^\* OK ([-.\w]+) Cyrus IMAP4 v([\w_.]+)-OS X ([\d.]+) server ready\r\n| p/Cyrus imapd/ v/$2/ h/$1/ i/Mac OS X $3/ o/Mac OS X/
match imap m|^\* OK \[[^\]]+\] ([-\w_.]+) Cyrus IMAP4 v([-\w_.]+)-OS X Server ([\d.]+):| p/Cyrus imapd/ v/$2/ h/$1/ i/Mac OS X $3/ o/Mac OS X/
match imap m|^\* OK (?:\[CAPABILITY IMAP4[^\]]*?\] )?([-.\w]+) Cyrus IMAP4? Murder v([-.\w]+) server ready\r\n| p/Cyrus Murder imapd/ h/$1/ v/$2/

match imap m|^\* OK Welcome to Binc IMAP v(\d[-.\w]+)| p/Binc imapd/ v/$1/
match imap m|^\* OK ([-.\w]+) IMAP4rev1 AppleMailServer (\d[-.\w]+) ready\r\n| p/AppleMailServer imapd/ h/$1/ v/$2/
match imap m/^\* OK IMAP4rev1 Server Classic Hamster (Vr.|Version) [\d.]+ \(Build ([\d.]+)\) greets you!\r\n/ p/Classic Hamster imapd/ v/$2/ o/Windows/
match imap m|^\* OK ([-\w_.]+) Oracle Email Server esimap\t([\d.]+) \t  is ready\r\n| p/Oracle imapd/ v/$2/ h/$1/
match imap m|^\* OK Kerio MailServer ([\d.]+) IMAP4rev1 server ready\r\n| p/Kerio imapd/ v/$1/
match imap m|^\* OK Kerio MailServer ([\d.]+) patch (\d+) IMAP4rev1 server ready\r\n| p/Kerio imapd/ v/$1 patch $2/
match imap m|^\* OK Netscape IMAP4rev1 Service ([\d.]+) on ([-\w_.]+) at .*\r\n| p/Netscape imapd/ v/$1/ h/$2/
match imap m|^\* OK IMAP4 server ready \(Worldmail ([\d.]+)\)\r\n| p/Worldmail imapd/ v/$1/ o/Windows/
match imap m|^\* OK HT Mail Server v([\d.]+) IMAP4rev1 .*\r\n| p/IceWarp imapd/ v/$1/
match imap m|^\* OK Softalk IMAP Server ready\r\n| p/Softalk imapd/ o/Windows/
match imap m|^\* OK Welcome to Binc IMAP| p/Binc imapd/
match imap m|^\* OK ([-\w_.]+) Mirapoint IMAP4 ([-\w.]+) server ready\r\n| p/Mirapoint imapd/ v/$2/ h/$1/
match imap m|^\* OK FirstClass IMAP4rev1 server v([\d.]+) at ([-\w_.]+) ready\r\n| p/FirstClass imapd/ v/$1/ h/$2/
match imap m|^\* OK IMAP4rev1 DvISE Mail Access Server MA-([\w.]+) \(\w+\)\r\n| p/DvISE imapd/ v/$1/
match imap m|^\* OK IMAP4rev1 GNU mailutils ([\w.]+)\r\n| p/GNU mailutils imapd/ v/$1/
match imap m|^\* OK IMAP ([-\w_.]+) \(Version ([-\w.]+)\)\r\n| p/SurgeMail imapd/ v/$2/ h/$1/
match imap m|^\* OK Samsung Contact IMAP server ([\d.]+) ready on ([-\w_.]+)\r\n| p/Samsung contact imapd/ v/$1/ h/$2/
match imap m|^\* OK \[([-\w_.]+)\] IMAP4rev1 Mercury/32 v([\w.]+) server ready\.\r\n| p|Mercury/32 imapd| v/$2/ h/$1/ o/Windows/
match imap m|^\* OK \[CAPABILITY IMAP4 IMAP4rev1 ACL QUOTA LITERAL\+ NAMESPACE UIDPLUS CHILDREN BINARY(?: UNSELECT)? LANGUAGE XSENDER X-NETSCAPE XSERVERINFO AUTH=PLAIN\] ([-\w_.]+) IMAP4 service \(Sun Java\(tm\) System Messaging Server ([-\w. ]+) \(built .*\)\)\r\n| p/Sun Java System Messaging Server imapd/ v/$2/ h/$1/
match imap m|^\* OK \[CAPABILITY IMAP4 IMAP4rev1[\w+= -]*\] ([\w._-]+) IMAP4 service \(Sun Java\(tm\) System Messaging Server ([\w._-]+) (\d+)bit \(built .*\)\)\r\n| p/Sun Java System Messaging Server imapd/ v/$2/ h/$1/ i/$3 bits/
match imap m|^\* OK \[CAPABILITY IMAP4[^\]]*\] Messaging Multiplexor \(Sun Java\(tm\) System Messaging Server (\d[-\w_.]+) \(built .*\)\)\r\n| p/Sun Java System Messaging Multiplexor imapd/ v/$1/
match imap m|^\* OK ([-\w_.]+) IMAP4 service \(iPlanet Messaging Server ([\w. ]+) \(built .*\)\)\r\n| p/Sun iPlanet Messaging Server imapd/ v/$2/ i/HotFix $3/ h/$1/
match imap m|^\* OK Anonymous Mail Server v([\d.]+) IMAP4rev1 .*\r\n| p/Anonymous Mail Server imapd/ v/$1/
match imap m|^\* OK ([-\w_.]+) ModusMail IMAP4 Server ([\d.]+) ready\r\n| p/ModusMail imapd/ v/$2/ h/$1/ o/Windows/
match imap m|^\* OK IMAP4rev1 Service at Jana-Server ready\r\n| p/JanaServer imapd/ o/Windows/
match imap m|^\* OK \]-:\^:-\[ IMAP4rev1 .*\r\n| p/Merak Mail Server imapd/ o/Windows/
match imap m|^\* OK ([-\w_.]+) IMAP4 Service ([\d.()]+) at .*\r\n| p/SCO imapd/ v/$2/ h/$1/ o/SCO UNIX/
match imap m|^\* OK CommuniGate Pro IMAP Server ready\r\n| p/CommuniGate Pro imapd/
match imap m|^\* OK IMAPrev1 Service Ready - hMailServer ([\w.-]+)\r\n| p/hMailServer imapd/ v/$1/ o/Windows/
match imap m|^\* OK IMAP4rev1 SmartMax IMAPMax (\d+) Ready\r\n| p/IMAPMax/ v/$1/ o/Windows/
match imap m|^\+OK X1 ([-\w_.]+)\r\n| p/IMail imapd/ h/$1/
match imap m|^\* OK IMAP4rev1 SmarterMail\r\n| p/SmarterMail imapd/ o/Windows/
match imap m|^\* OK Scalix IMAP server ([\d.]+) ready on ([-\w_.]+)\r\n| p/Scalix imapd/ v/$1/ h/$2/
match imap m|^\* OK Scalix IMAP server ([\d.]+) on ([-\w_.]+)\r\n| p/Scalix imapd/ v/$1/ h/$2/
match imap m|^\* OK .* GoMail V([-\w_.]+) IMAP4rev1| p/GoMail mass mailing plugin imapd/ v/$1/ o/Windows/
match imap m|^\* OK IMAP4 ready! [-\w_.]+ Winmail Mail Server MagicWinmail Extend IMAP 101\r\n| p/Winmail imapd/ o/Windows/
match imap m|^\* OK ([-\w_.]+) IMAP4rev1 Mailtraq \(([\d.]+)\) ready\r\n| p/Mailtraq imapd/ v/$2/ h/$1/ o/Windows/
match imap m|^\* OK ([-\w_.]+) CallPilot IMAP4rev1 v([\d.]+) server ready\.?\r\n| p/Nortel CallPilot imapd/ v/$2/ h/$1/ d/telecom-misc/
match imap m|^\* OK ([-\w_.]+) Zimbra IMAP4rev1 service ready\r\n| p/Zimbra imapd/ h/$1/
match imap m|^\* OK ([-\w_.]+) Zimbra IMAP4rev1 server ready\r\n| p/Zimbra imapd/ h/$1/
match imap m|^\* OK ([-\w_.]+) DKIMAP4 IMAP Server\r\n| p/DBOX DKIMAP4 imapd/ h/$1/
match imap m|^\* OK IMAP Module of ArGoSoft Mail Server Pro for WinNT/2000/XP, Version [\d.]+ \(([\d.]+)\)\r\n| p/ArGoSoft Pro imapd/ v/$1/ o/Windows/
match imap m|^\* OK ArGoSoft Mail Server IMAP Module v\.([\w._-]+) at | p/ArGoSoft imapd/ v/$1/ o/Windows/
match imap m|^\* OK ([-\w_.]+) running Eudora Internet Mail Server X ([\d.]+)\r\n| p/Eudora Internet Mail Server X imapd/ v/$2/ h/$1/ o/Mac OS X/
match imap m|^\* OK ([-\w_.]+) running EIMS X ([\w.]+)\r\n| p/Eudora Internet Mail Server X imapd/ v/$2/ h/$1/ o/Mac OS X/
match imap m|^\* OK MERCUR IMAP4-Server \(v([\w.]+) \w+\) for Windows ready| p/Atrium Software's Mercur imapd/ v/$1/ o/Windows/
match imap m|^\* OK WebSTAR Mail ready\r\n| p/WebSTAR imapd/ o/Mac OS X/
match imap m|^\* OK \[CAPABILITY IMAP4rev1 UIDPLUS CHILDREN NAMESPACE THREAD=ORDEREDSUBJECT THREAD=REFERENCES SORT QUOTA IDLE AUTH=PLAIN ACL ACL2=UNION\] Atmail IMAP4 Server ready\. See COPYING for distribution information\.\r\n| p/Atmail imapd/
match imap m|^\* OK Dovecot DA ready\.\r\n| p/Dovecot DirectAdmin imapd/
match imap m|^\* OK AXIGEN ([\w._-]+) \(Linux/i686\) IMAP4rev1 service is ready\r\n| p/Axigen imapd/ i|Linux/i686| v/$1/ o/Linux/
match imap m|^\* BYE Hi This is the IMAP SSL Redirect\r\n| p/Lotus Domino secure imapd/ i/SSL redirect/
match imap m|^\* OK Hi This is the IMAP SSL Server .*\r\n| p/Lotus Domino secure imapd/
match imap m|^\* OK TeamXchange IMAP4rev1 server \(([\w._-]+)\) ready\.\r\n| p/TeamXchange imapd/ h/$1/
match imap m|^\* OK \[CAPABILITY IMAP4REV1[^\]]*?\] ([-.\w]+) IMAP4rev1 Citadel ([-.\w]+) ready\r\n| p/Citadel imapd/ h/$1/ v/$2/
match imap m|^\* BYE Domino IMAP4 Server Configured for SSL Connections only\. Please reconnect using SSL Port (\d+), .*\r\n| p/Lotus Domino imapd/ i/SSL-only; imaps on port $1/
match imap m|^\* OK Kerio Connect ([\w._-]+) IMAP4rev1 server ready\r\n| p/Kerio Connect imapd/ v/$1/
match imap m|^\* OK ([\w._-]+) IMAP4rev1 Server PMDF V([\w._-]+) at | p/PMDF imapd/ o/OpenVMS/ v/$2/ h/$1/
match ssl/imap m|^\* BYE Fatal error: tls_init\(\) failed\r\n| p/Cyrus imapd/
match imap m|^\* OK VisNetic\.MailServer\.v([\w._-]+) IMAP4rev1 .*\r\n| p/VisNetic MailServer imapd/ v/$1/
match imap m|^\* OK ([-\w_.]+)\s+IdeaImapServer ([^\s]+) ready\r\n| p/IdeaImapServer imapd/ v/$2/ h/$1/

# Fairly General
match imap m|^\* OK IMAP4rev1 server ready at \d\d/\d\d/\d\d \d\d:\d\d:\d\d \r\n| p/MailEnable Professional imapd/ o/Windows/
match imap m|^\* OK IMAP4 Ready ([-\w_.]+) \w+\r\n| p/Perdition imapd/ h/$1/
match imap m|^\* OK ([-\w_.]+) IMAP server ready\r\n| p/hMailServer imapd/ h/$1/ o/Windows/

match imap-proxy m|^\* OK IMAP4 proxy ready\r\n| p/imap proxy/
match imap-proxy m|^\* BYE PGP Universal no imap4 service here\r\n| p/PGP Universal imap proxy/ i/disabled/
match imap-proxy m|^\* OK PGP Universal IMAP4rev1 service ready \(proxied server greeted us with: ([^)]+)\)\r\n| p/PGP Universal imap proxy/ i/Banner: $1/
match imap-proxy m|^\* OK imapfront ready\.\r\n| p/Mailfront imapfront imap proxy/
match imap-proxy m|^\* OK imapfront ready\. \+ stunnel\r\n| p/Mailfront imapfront imap proxy/ i/with stunnel/
match imap-proxy m|^\* OK avast! IMAP Proxy\r\n| p/Avast! anti-virus imap proxy/ o/Windows/
match imap-proxy m|^\* OK \[CAPABILITY IMAP4rev1\] SpamPal for Windows\r\n| p/SpamPal imap proxy/ o/Windows/
match imap-proxy m|^\* OK Zarafa IMAP gateway ready\r\n| p/Zarafa imap proxy/ o/Unix/
match imap-proxy m|\* OK \[CAPABILITY IMAP4rev1 UIDPLUS CHILDREN NAMESPACE THREAD=ORDEREDSUBJECT THREAD=REFERENCES SORT QUOTA IDLE ACL ACL2=UNION\] Courier-IMAP ready\. Copyright 1998-2008 Double Precision, Inc\. See COPYING for distribution information\.\r\n| p/imapproxy/

softmatch imap m/^\* OK ([-.\w]+) [-.\w,:+ ]+imap[-.\w,:+ ]+\r\n$/i h/$1/
softmatch imap m/^\* OK [-.\w,:+ ]+imap[-.\w,:+ ]+\r\n$/i

# Cyrus IMSPD
match imsp m|^\* OK Cyrus IMSP version (\d[-.\w]+) ready\r\n$| p/Cyrus IMSPd/ v/$1/

match infopark m|^\d+{infopark tcl-Interface-Server} {CM ([\w._-]+)| p/Infopark Fiona TCL interface/ v/$1/

match instrument-manager m|^\r\n\x18\t$| p/Data Innovations Instrument Manager/

match intermapper m|^<KU_goodbye>Access not allowed for [\d.]+\. Check the InterMapper server&apos;s access restrictions\.</KU_goodbye>$| p/InterMapper network monitor/
match intermapper m|^<KU_goodbye>Protocol Error: XML data is not well-formed\.</KU_goodbye>$| p/InterMapper network monitor/

match intertel-ctl m|^\x1f\x19\x0e\x01\0\x01\x01\x01\x02\x02\x03\x02\x01\x04\x11\x05| p/InterTel IPRC VoIP management card control channel/ d/PBX/

match intranetchat m|^\d+\0FORWARD\0\x0b\xc2c\x0c\xc1a\x9f@| p/Intranet Chat Server/

match ipsi m|^\0\x0f\0/([\w._-]+)\0| p/Avaya $1 IPSI version/ d/PBX/

match ir-alerts m|^.\0\0\0\0Lexmark (\w+)\0| p/Lexmark $1 IR alerts/ d/printer/

# ircd-hybrid 7 on Linux
match irc m=^NOTICE AUTH :\*\*\* Looking up your hostname\.\.\.\r\nNOTICE AUTH :\*\*\* Checking Ident\r\nNOTICE AUTH :\*\*\* (No|Got) Ident response\r\nNOTICE AUTH :\*\*\* (Couldn't look up|Found) your hostname\r\n$= p/Hybrid-based ircd/
match irc m=^NOTICE AUTH :\*\*\* Looking up your hostname\.\.\.\r\nNOTICE AUTH :\*\*\* Checking Ident\r\nNOTICE AUTH :\*\*\* (Couldn't look up|Found) your hostname\r\nNOTICE AUTH :\*\*\* (No|Got) Ident response\r\n$= p/Hybrid-based ircd/
match irc m=^NOTICE AUTH :\*\*\* Looking up your hostname\.\.\.\r\nNOTICE AUTH :\*\*\* Checking Ident\r\nNOTICE AUTH :\*\*\* (Couldn't look up|Found) your hostname\r\n$= p/Hybrid-based ircd/

# ircu
match irc m|^NOTICE AUTH :\*\*\* Looking up your hostname\r\nNOTICE AUTH :\*\*\* Found your hostname, cached\r\nNOTICE AUTH :\*\*\* Checking Ident\r\n| p/ircu ircd/
match irc m|^NOTICE AUTH :\*\*\* Looking up your hostname\r\nNOTICE AUTH :\*\*\* Checking Ident\r\nNOTICE AUTH :\*\*\* No ident response\r\n| p/ircu ircd/
match irc m|^NOTICE AUTH :\*\*\* Looking up your hostname\r\nNOTICE AUTH :\*\*\* Checking Ident\r\nNOTICE AUTH :\*\*\* Couldn't look up your hostname\r\n| p/ircu ircd/
match irc m|^NOTICE AUTH :\*\*\* Looking up your hostname\r\nNOTICE AUTH :\*\*\* Checking Ident\r\nNOTICE AUTH :\*\*\* Got ident response\r\nNOTICE AUTH :\*\*\* Couldn't look up your hostname\r\n| p/ircu ircd/
match irc m|^ERROR..Your host is trying to \(re\)connect too fast -- throttled\r\n| p/ircu ircd/
match irc m|^NOTICE AUTH :\*\*\* Looking up your hostname\r\nNOTICE AUTH :\*\*\* Checking Ident\r\nNOTICE AUTH :\*\*\* Found your hostname\r\n| p/ircu ircd/

# Hybrid6/PTlink6.15.0 ircd on Linux
match irc m|^NOTICE AUTH :\*\*\* Looking up your hostname\.\.\.\r\nNOTICE AUTH :\*\*\* Found your hostname\r\n$| p/Hybrid ircd/
# ircd 2.8/hybrid-6.3.1 on Linux
match irc m|^NOTICE AUTH :\*\*\* Looking up your hostname\.\.\.\r\nNOTICE AUTH :\*\*\* Checking Ident\r\nNOTICE AUTH :\*\*\* No Ident response\r\nNOTICE AUTH :\*\*\* Found your hostname\r\n$| p/Hybrid ircd/
# ircd-hybrid-7.0 - apparently upset because Nmap reconnected too fast
match irc m|^ERROR :Trying to reconnect too fast\.\r\n| p/Hybrid ircd/
# Hybrid-IRCD 7.0 on Linux 2.4
match irc m|^NOTICE AUTH :\*\*\* Looking up your hostname\.\.\.\r\nNOTICE AUTH :\*\*\* Checking Ident\r\nNOTICE AUTH :\*\*\* Found your hostname\r\nNOTICE AUTH :\*\*\* Got Ident response\r\n| p/Hybrid ircd/

match irc m|^ERROR :Closing Link: \[[\d.]+\] \(Throttled: Reconnecting too fast\) -Email ([-\w_.]+@[-\w_.]+) for more information\.| p/Unreal ircd/ i/Admin email $1/
# Sometimes multiple emails are specified, bad emails, etc
match irc m|^ERROR :Closing Link: \[[\d.]+\] \(Throttled: Reconnecting too fast\) -Email .* for more information\.| p/Unreal ircd/ i/Admin email $1/
match irc m|^ERROR :Closing Link: \[[\d.]+\] \(Too many unknown connections from your IP\)\r\n| p/Unreal ircd/
match irc m|^ERROR :Reconnecting too fast, throttled\.\r\n$| p/ratbox, charybdis, or ircd-seven ircd/

match irc m|^NOTICE AUTH :\*\*\* Processing connection to ([-\w_.]+)\r\n| p/ratbox ircd/ h/$1/

# No, Thomas Graf, this isn't leet :)
match irc m|^PING :42\r\n$| p/iacd ircd/

# Many different ircds...
match irc m|^NOTICE AUTH :\*\*\* Checking Ident\r\n|
match irc m|^:([-\w_.]+) NOTICE \* :\*\*\* Looking up your hostname\.\.\.\r\n| h/$1/
match irc m|^:([-\w_.]+) NOTICE AUTH :\*\*\* Looking up your hostname\.\.\.\n| h/$1/

# dircproxy 1.0.3 on Linux 2.4.x
match irc-proxy m|^:dircproxy NOTICE AUTH :Looking up your hostname\.\.\.\r\n:dircproxy NOTICE AUTH :Got your hostname\.\r\n| p/dircproxy/
# dirkproxy (modificated dircproxy)
match irc-proxy m|^:dirkproxy NOTICE AUTH :Looking up your hostname\.\.\.\r\n:dirkproxy NOTICE AUTH :Got your hostname\.\r\n| p/dirkproxy/
# Unreal IRCD Server version 3.2 beta 17
match irc m|^:([-.\w]+) NOTICE AUTH :\*\*\* Looking up your hostname\.\.\.\r\n| p/Unreal ircd/ h/$1/

# dancer-ircd 1.0.31+maint8-1
match irc m|^NOTICE AUTH :\*\*\* Looking up your hostname\.\.\.\r\nNOTICE AUTH :\*\*\* Checking ident\r\nNOTICE AUTH :\*\*\* No identd \(auth\) response\r\nNOTICE AUTH :\*\*\* Found your hostname\r\n$| p/Dancer ircd/
match irc m|^NOTICE AUTH :\*\*\* Looking up your hostname\.\.\.\r\nNOTICE AUTH :\*\*\* Couldn't look up your hostname\r\n| p/Dancer ircd/
match irc m|^NOTICE AUTH :\*\*\* Looking up your hostname\.\.\.\r\nNOTICE AUTH :\*\*\* Found your hostname, welcome back\r\nNOTICE AUTH :\*\*\* Checking ident\r\nNOTICE AUTH :\*\*\* No identd \(auth\) response\r\n| p/Dancer ircd/
match irc m|^NOTICE AUTH :\*\*\* Looking up your hostname\.\.\.\r\nNOTICE AUTH :\*\*\* Checking ident\r\nNOTICE AUTH :\*\*\* Got ident response\r\nNOTICE AUTH :\*\*\* Found your hostname\r\n| p/Dancer ircd/
match irc m|^NOTICE AUTH :\*\*\* Looking up your hostname\.\.\.\r\nNOTICE AUTH :\*\*\* Found your hostname, welcome back\r\nNOTICE AUTH :\*\*\* Checking ident\r\nNOTICE AUTH :\*\*\* Got ident response\r\n| p/Dancer ircd/
match irc m|^NOTICE AUTH :\*\*\* Looking up your hostname\.\.\.\r\nNOTICE AUTH :\*\*\* Checking ident\r\nNOTICE AUTH :\*\*\* No identd \(auth\) response\r\n| p/Dancer ircd/
match irc m|^NOTICE AUTH :\*\*\* Looking up your hostname\.\.\.\r\nNOTICE AUTH :\*\*\* Checking ident\r\nNOTICE AUTH :\*\*\*| p/Dancer ircd/

match irc m|^NOTICE AUTH :\*\*\* Checking Ident\r\nNOTICE AUTH :\*\*\* Got ident response\r\n| p/ircu Undernet IRCd/
# Bitlbee ircd 0.80
match irc m|(^:[-.\w]+) NOTICE AUTH :BitlBee-IRCd initialized, please go on\r\n| p/BitlBee IRCd/ h/$1/
match irc m|^Warning: Unable to read configuration file `.*/bitlbee\.conf'\.\n:[-\w_.]+\. NOTICE AUTH :BitlBee-IRCd initialized, please go on\r\n| p/BitlBee IRCd/

match irc m|^:([-\w_.]+) NOTICE Auth :Looking up your hostname\.\.\.\r\n| p/InspIRCd/ h/$1/
match irc m|^:([-\w_.]+) NOTICE Auth :\*\*\* Looking up your hostname\.\.\.\r\n| p/InspIRCd/ h/$1/
match irc m|^:([-\w_.]+) NOTICE \w+ :\*\*\* .*\r\nERROR :Closing link: \([\w._-]+@[\w._-]+\) \[Z-Lined: Your IP range has been attempting to connect too many times in too short a duration\. Wait a while, and you will be able to connect\.\]\r\n$| p/InspIRCd/ h/$1/
match inspircd-spanning-tree m|^CAPAB START\r\nCAPAB MODULES [\w_-]+\.so,| p/InspIRCd spanning tree/
match inspircd-spanning-tree m|^CAPAB START 1202\r\n$| p/InspIRCd spanning tree/

# PTlink6.15.2 on Linux 2.4
match irc m|^NOTICE AUTH :\*\*\* Hostname lookup disabled, using your numeric IP\r\nNOTICE AUTH :\*\*\* Checking Ident\r\n| p/PTlink ircd/
match irc m|(^:[-.+\w]+) NOTICE AUTH :\*\*\* Looking up your hostname\.\.\.\n:[-.+\w]+ NOTICE AUTH :\*\*\* Checking Ident\n:[-.+\w]+ NOTICE AUTH :\*\*\* Found your hostname\n| p/Bahamut Dalnet ircd/ i/derived from DreamForge and Hybrid/ h/$1/
match irc m|^:([\w._-]+) NOTICE ZUSR :You have been throttled for 2 minutes for too many connections in a short period of time\. Further connections in this period will reset your throttle and you will have to wait longer\.\r\n| p/Bahamut ircd/ h/$1/

match irc m|^ERROR Your host is trying to \(re\)connect too fast -- throttled\r\n| p/IRC2000 Pro ircd/
match irc m|^IRCXPRO ([\w._-]+)\r\nAUTHREQUEST :Authentication Required\r\n| p/IRCXPRO admin ircd/ v/$1/

match irc m|^:([\w._-]+) 451 \* HELP :No te has registrado\r\n| p/ConferenceRoom ircd/ i/Spanish/ h/$1/
match irc m|^:([\w._-]+) NOTICE AUTH :Minbif-IRCd initialized, please go on\r\n| p/Minbif ircd/ h/$1/

match irc-proxy m|^:.*!psyBNC@lam3rz\.de NOTICE \* :psyBNC([-.\w]+)\r\n| p/psyBNC/ v/$1/
match irc-proxy m|^:.*!pb@lam3rz\.de NOTICE \* :pb([-.\w]+)\r\n| p/psyBNC/ v/$1/
match irc-proxy m|^:.*!psyBNC@lam3rz\.de NOTICE \* :| p/psyBNC/
match irc-proxy m|^:.*!psyBNC@[-\w_.]+ NOTICE \* :psyBNC on ([-\w_.]+)\r\n| p/psyBNC/ h/$1/
match irc-proxy m|^:.*!psyBNC@([-\w_.]+) NOTICE \* :psyBNC([-\w_.]+)\r\n| p/psyBNC/ h/$1/ v/$2/

match irc-proxy m|^:sbnc!sbnc@sbnc\.soohrt\.org NOTICE \* :Wellcum\r\n| p/sbnc/
match irc-proxy m|^NOTICE AUTH :\*\*\* .*\r\nNOTICE AUTH :\*\*\* \[BNC ([\d.]+) | p/BNC irc-proxy/ v/$1/
match irc-proxy m|^:[-\w_.!@]+ NOTICE \S+ :\*\*\* shroudBNC *([\d.]+) .Revision: (\d+)| p/ShroudBNC irc-proxy/ v/$1 revision $2/

match iscsi m|^\x1b\[2JStarWind iSCSI Target v([\w._-]+) \(Build (0x\w+), Win32, Alcohol Edition\)\r\n| p/StarWind iSCSI/ v/$1 build $2/ o/Windows/ i/Alcohol Edition/
match iscsi m|^\x1b\[2JStarWind Alcohol Edition iSCSI Target v([\w._-]+) \(Build (\d+), Win32, Alcohol Edition\)\r\n| p/StarWind iSCSI/ v/$1 build $2/ o/Windows/ i/Alcohol Edition/
match iscsi m|^\x1b\[2JStarWind Alcohol Edition iSCSI Target v([\w._-]+) \(Build (\d+), Win32\)\r\n| p/StarWind iSCSI/ v/$1 build $2/ o/Windows/
match iscsi m|^\x1b\[2JStarWind iSCSI SAN Software v([\w._-]+) \(Build (\d+), Win32\)\r\nCopyright \(c\) StarWind Software 2003-2009\. All rights reserved\.\r\n\r\n\r\n$| p/StarWind iSCSI/ v/$1 build $2/ o/Windows/

match issc m|^\rYou do not have permission to connect to the builder port\.\r\nTalk to an admin at port \d+ for entry\.\r\n| p/ISS System Scanner Console/

# ISS RealSecure Server Sensor for Windows 6.5 on Windows NT 4.0 Server SP6a
# ISS RealSecure ServerSensor 7.0 on Windows 2000 Server
# ISS RealSecure Server Sensor 6.0 on Windows NT 4.0 Server SP6a
# ISS RealSecure Server Sensor 7.0 issdaemon on Microsoft Windows NT Workstation with SP6a
match iss-realsecure m|^\0\0\0.\x08\x01\x03\x01\0.\x02\0\0..\0\0.\0\0\0..\0\0\x80\x04..\0.\0\xa0|s p/ISS RealSecure IDS/ o/Windows/
match iss-realsecure m|^\0\0\0.\x08\x01\x04\x01\0..\0\0..\0\0.\0\0\0..\0\0\x80\x04..\0.\0\xa0\0\0|s p/ISS RealSecure IDS ServerSensor/ v/6.0 - 7.0/ o/Windows/
# I've only seen 1 example of the following. Probably not general enough
match iss-realsecure m|^\0\0\x01/\x08\x01\x03\x01\x01'\x04\0\0\0\x18\0\0\xa4\0\0\0f\x02\0\0\x80\x04\x06\0\0\x80\0\xa05Microsoft Enhanced RSA and AES Cryptographic Provider|s p/ISS Realsecure Workgroup Manager/ o/Windows/

match ixia-unknown m|^Enter port cpu supported card port number and hit Enter\. For example \"3 4\"\r\n| p/Ixia 400T traffic QA/
match ixia-unknown m|^.*\0\x18Ixia Hardware I/O Server\x13Ixia Communications\x18Ixia Hardware I/O Server\x0b([\d.]+)|s p/Ixia 400T traffic QA/
match ixia-unknown m|^\r\nWelcome to the Ixia Socket/Serial TCL Server\r\nPress Ctrl-C to reset Tcl Session\r\nIxia>| p/Ixia TCL server/

match java-message-service m|^101 imqbroker ([^\n]+)\n| p/Java Message Service/ v/$1/

match java-rmi m#^\x80c\0\0\x00622996\|com\.code42\.messaging\.security\.DHPublicKeyMessageY\xd4\0\0\0.0\x81.0\x81.\x06\t\*\x86H\x86\xf7\r\x01\x03\x010\x81.\x02A\0#s p/Java RMI/ i/CrashPlan online backup/

# Samsung ML-2850 port 2000
match jetdirect m|^ $| p/JetDirect/ d/printer/

match jmond m|^cpu: *[\d.]+ mem: *[\d.]+ swp: *[\d.]+\0| p/jmond unix resource monitor/ o/Unix/

match jtag m|^\0%\rJTAG Server\r\n\0\0\0\x08\0\0\0\xf0| p/Altera Quartus JTAG service/

match junoscript m|^<\?xml version=\"1\.0\"[^<]+<junoscript.*release=\"([^\"]+)\" hostname=\"([^\"]+)\"| p/Junoscript XML Interface/ v/Release $1/ d/router/ o/JUNOS $1/ h/$2/

match kguard m|^inv2W\x04\x0f\0\0\0\x01\0\t\0\0\x00| p/Kguard Security DVR/ d/webcam/

match klogin m|^\x01klogind: (All authentication systems disabled; connection refused)\.\.\r\n| p/MIT Kerberos klogin/ i/broken - $1/

match kismet m|^\*KISMET: 0\.0\.0 \d+ \x01Kismet\x01 \d+ \d+ (\S+) \n\*PROTOCOLS:| p/Kismet server/ v/$1/
match kismet m|^\*KISMET: ([\d.]+) \d+ \x01Kismet\x01 \d+ \n\*PROTOCOLS:| p/Kismet server/ v/$1/
match kismet-drone m#^\xde\xca\xfb\xad\x01\0\0\0\x04\0\t\0[\x07\x10]# p/Kismet drone/

match ksystemguard m|^ksysguardd ([\d.]+)\n\(c\)| p/ksystemguardd/ v/$1/

match landesk m|^TDMM\x1c\0\0\0\x14\0\0\0| p/LANDesk Management Suite/ i/Targeted Multicast Service/

match ldap m|^unable to set certificate file\n6292:error:02001002:system library:fopen:No such file or directory:bss_file\.c:| p/OpenLDAP over SSL/ i/broken/

match lisa m|^\d+ \*+\n.*\x000 succeeded\n\0$|s p/LAN Information Server/ i/Sanitized/
match lisa m|^\d+ ([-\w_.]+)\n.*\x000 succeeded\n\0$|s p/LAN Information Server/ h/$1/
match lisa m|^\d+ .*\n\x000 succeeded\n\0$|s p/LAN Information Server/
match lisa m|^0 succeeded\n\0$| p/LAN Information Server/

match lmtp m|^220 ([-.\w]+) LMTP Cyrus v(\d[-.\w]+) ready\r\n| p/Cyrus Imap Daemon lmtpd/ h/$1/ v/$2/
match lmtp m|^220 ([\w._-]+) Cyrus LMTP Murder v([\w._-]+) server ready\r\n| p/Cyrus lmtpd Murder/ v/$2/ h/$1/
match lmtp m|^220 ([-\w_.]+) LMTP Cyrus v([\d.]+)-Red Hat [\d.-]+ ready\r\n| p/Cyrus Imap Daemon lmtpd/ h/$1/ v/$2/ o/Linux/ i/on Red Hat/
match lmtp m|^220 ([-\w_.]+) DBMail LMTP service ready to rock\r\n| p/DBMail lmtpd/ h/$1/
match lmtp m|^220 DSPAM LMTP ([-\w_.]+) Ready\r\n| p/DSPAM lmtpd/ v/$1/
match lmtp m|^220 ([\w._-]+) Zimbra LMTP ready\r\n| p/Zimbra lmtpd/ h/$1/

match logevent m|^\x01\*Nsure Audit Novell NetWare \[\w+:\w+\]\r\n| p/Nsure Audit logeventd/ o/NetWare/

match lns m|^LNS READY<>$| p/Legalis Intranet legal information server/

# LSMS VPN Firewall GUI admin port
# LSMS Redundancy port
match lucent-fwadm m|^0001;2$| p/Lucent Secure Management Server/
match mailq m|^version zmailer ([\d.]+)\n220 MAILQ-V2-CHALLENGE: | p/ZMailer/ v/$1/ o/Unix/
match maya m|^\([\w._-]+:\d+\) : updateShowMenu MayaWindow| p/Autodesk Maya command port/
match mediad m|^\x80\0\0\$\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\xff\xff\xff\xff\xff\xff\xff\xff\0\0\0\0\0\0\0\0\0\0\0\0$| p/IRIX mediad/ o/IRIX/
match meetingmaker m/^\xc1,$/ p/Meeting Maker calendaring/
match melange m|^\+\+\+Online\r\n>> Melange Chat Server \(Version (\d[-.\w]+)\), Apr-25-1999\r\n\nWelcome | p/Melange Chat Server/ v/$1/
match metasploit m|^\n.*=\[ msf v([^\r\n]+)\r?\n.*\d+ exploits.*\d+ payloads.*\d+ encoders.*\d+ nops.*msf > $|s p/Metasploit Framework msfd/ v/$1/
match midas m|^MIDASd v([\w.]+) connection accepted\n\xff| p/midasd/ v/$1/
match minecraft m|^\xff\0\x17Took too long to log in$| p/Minecraft game server/
match misys-loaniq m|^Loan IQ %1 Request Server - Ready for Request\0| p/Misys Loan IQ/
match mpd m|^OK MPD ([\d.]+)\n$| p/Music Player Daemon/ v/$1/
match mpich2 m|^([\d.]+) \d+\0{240,250}$| p/MPICH2/ v/$1/
# lopster 1.2.0.1 on Linux 1.1
match mserv m|^200 Mserv (\d[-.\w]+) \(c\) James Ponder [-\d]+ - Type: USER <username>\r\n\.\r\n| p/Mserv music server/ v/$1/

match mudnames m|^MudNames ([\d.]+) - \(C\) 1997-2001 Ragnar Hojland Espinosa <ragnar@ragnar-hojland\.com>\n\r| p/MudNames/ v/$1/
match munin m|^# munin node at ([-\w_.]+)\n$| p/Munin/ h/$1/

match multiplicity m|^MULTIPLICITYP$| p/Stardock Multiplicity KVM daemon/ o/Windows/

match mu-connect m|^\x7f\xba\xbe\xbf$| p/Webzen MU Online role-playing game connect/
match mu-game m|^\x7f\xb2O\xbe\xbf\xad.\x8f\x8e\x8e\x8f\x88$| p/Webzen MU Online role-playing game server/

# The "^(?:\* [^\r\n]+\r\n)*?" construct on these matches is much faster
# than just using the matches without an anchor.  -- Brandon
match mupdate m|^(?:\* [^\r\n]+\r\n)*?\* OK MUPDATE \"([-.\w]+)\" \"Cyrus Murder\" \"v([-.\w]+)\" \"\(master\)\"\r\n| p/Cyrus Murder Master/ h/$1/ v/$2/
match mupdate m|^(?:\* [^\r\n]+\r\n)*?\* OK MUPDATE \"([-.\w]+)\" \"Cyrus Murder\" \"v([-.\w]+)\" \"mupdate://([-.\w]+)\"\r\n| p/Cyrus Murder Slave/ h/$1/ v/$2/ i/Master: $3/

match mwti-rpc m%^Welcome MWTI RPC Communication Server Version ([\w._-]+) \[(?:Administrator|SYSTEM)\]\r\n% p/MWTI RPC Communication Server/ v/$1/

softmatch napster m|^1$|

# Ncat --chat mode, since 4.85BETA4
match ncat-chat m|^<announce> [\d.:a-f]+ is connected as <\w+>\.\n<announce> already connected: (.*?)\.\n| p/Ncat chat/ i/users: $1/

match netop m|^\xd6\x81\x81\0\0\xf9\0\xf9\xee\xe3\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0| p/NetOp Remote Control/

match netrek m|^<>=======================================================================<>\n  Pl: Rank       Name             Login      Host name                Type\n| p/Netrek game server player information interface/

# Nping echo mode -- added in Nmap 5.36TEST1
match nping-echo m|^\x01\x01\0\x18.{8}\0\0\0\0.{32}\0{16}.{32}$|s p/Nping echo/

match nrpep m|^nrpep - ([\d.]+)\n$| p|NetSaint Remote Plugin Executor/Perl| v/$1/

# The four wildcard bytes are a timestamp.
match ndmp m|^\x80\0\0L\0\0\0\0....\0\0\0\0\0\0\x05\x02\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\x04\0\0\0%Connected to BlueArc NDMP session \d+\n\0\0\0|s p/BlueArc ndmp/
# Wireshark dissection: NOTIFY_CONNECTED
# Multiple versions: 6.0, 11, 12, 13, 2010.
match ndmp m|^\x80\0\0\$\0\0\0\x01....\0\0\0\0\0\0\x05\x02\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\x03\0\0\0\0$|s p|Symantec/Veritas Backup Exec ndmp|

match nngs m|^>>messages/login\r\n----- Welcome to the No Name Go Server \(NNGS\) -----\r\n\r\n| p/No Name Go Server/

match omniback m|^HP Data Protector ([\w.]+): INET, internal build 611, built on .*\n$| p/HP Data Protector/ v/$1/

match outpost-ctl m|^\[\xb0`\x81\x91\xd3\x9eI\xa2\*\x0f\x99\xff\x8a_\x12................\x01\0$|s p/Agnitum Outpost Firewall control/ d/firewall/

match precomd m|^nduid: \x00([0-9a-f]{40})$| p/WebOS precomd/ o/Linux/ i/nduid $1/ d/phone/

match donkey m|^.*\0\0\0\x06\0Donkey\x01\x0c\0\./donkey\.ini\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0|s p/MLdonkey multi-network P2P GUI port/
match donkey m|^\xff\xfd\x1f[\r\n* ]+Welcome to MLdonkey          \r\n| p/MLDonkey multi-network P2P GUI port/
match donkey m|^\xff\xfd\x1f\n\n\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\n\n                         Welcome to MLdonkey chrooted| p/MLDonkey multi-network P2P GUI port/ i/chrooted/
match donkey m|^\xff\xfd\x1f ?Welcome to MLdonkey ?\n\x1b\[34mWelcome on mldonkey command-line\x1b\[2;37;0m\n\nUse \x1b\[31m\?\x1b\[2;37;0m for help\n\n\x1b\[7mMLdonkey command-line:\x1b\[2;37;0m\n> | p/MLDonkey multi-network P2P server control port/
match donkey m|^\xff\xfd\x1fWelcome to MLDonkey ([\d.]+)\n\x1b\[3.mWelcome on mldonkey command-line\x1b\[2;37;0m\n\nUse \x1b\[31m\?\x1b\[2;37;0m for help\n\n\x1b\[7mMLdonkey command-line:\x1b\[2;37;0m\n> | p/MLDonkey multi-network P2P server control port/ v/$1/
match donkey m|^\xff\xfd\x1f\n\x1b\[34mWelcome on mldonkey command-line\x1b\[2;37;0m\n\nUse \x1b\[31m\?\x1b\[2;37;0m for help\n\n\x1b\[7mMLdonkey command-line:\x1b\[2;37;0m\n> | p/MLDonkey multi-network P2P server control port/
match donkey m|^\xff\xfd\x1fWelcome to MLdonkey, visit http://mldonkey\.dyndns\.info for new Versions\n\x1b\[34mWelcome on mldonkey command-line\x1b\[2;37;0m\n\nUse \x1b\[31m\?\x1b\[2;37;0m for help\n\n\x1b\[7mMLdonkey command-line:\x1b\[2;37;0m\n> | p/MLDonkey multi-network P2P server control port/
match donkey m|^\xff\xfd\x1f([^']+)'s mlDonkey\n\x1b\[34mWelcome on mldonkey command-line\x1b\[2;37;0m\n\nUse \x1b\[31m\?\x1b\[2;37;0m for help\n\n\x1b\[7mMLdonkey command-line:\x1b\[2;37;0m\n>| p/MLDonkey multi-network P2P server control port/ i/name $1/
match donkey m|^ADDDOWNLOAD\(\d+\)\nhash\(\d+\)\nstate\([\w ]+\)\ntransmit\(\d+\)\nsize\(\d+\)\nfile\(\w+\)\nshared\(\d+\)\nthroughput\(\d+\)\nelapsed\(\d+\)\n;| p/MLDonkey multi-network P2P server information port/
match donkey m|^[\x00-\x10]\0\0\0\0\0[^\0]\0\0\0| p/MLDonkey multi-network P2P server/

match donkey m|^Telnet connection from [\d.]+ rejected \(see allowed_ips setting\)\n| p/MLDonkey multi-network P2P server control port/ i/IP disallowed/
match donkey m|^HTTP/1\.1 404 Not Found\r\nDate: .*\r\nServer: eserver ([\d.]+)\r\nAccept-Ranges: bytes\r\nContent-Type: text/html\r\nContent-Length: \d+\r\n\r\n<html><head><title>404 File not found - eserver is not a HTTP server</title>| p/Lugdunum eserver/ v/$1/

match lanforge m|^\0<@\0\0\x0c\0\0\n\nWelcome to LANforge\.  Enter 'help' for more information\.\n\0\x01W@\0\0\x0c\0\0Licenses: Shelves: \d+  Cards: \d+  Ports: \d+  Active Ports: \d+\n  WanLinks: \d+  Wl-2m: \d+  Wl-45m: \d+  Wl-155m: \d+  Wl-1g: \d+\n  WanPaths: \d+  Armageddon: \d+  VOIP: \d+\n\nThese licenses will never expire\.\nCurrent use: Ports: \d+  WL-2m: \d+  WL-45m: \d+  WL-155m: \d+  WL-1G: \d+\n  Armageddon: \d+  VOIP: \d+\nLANforge Support and Software Upgrades expire in: ([^.]*)\.\n\0| p/LANforge management/ i/support expires in $1/

match login m|^A connection was attempted on an illegal port\.\r\n| p/Ataman ATRLS rlogind/ o/Windows/

# L2J loginserver. http://l2jserver.com/. Packets are obfuscated and encrypted
# but preceded by a 16-bit length.
match loginserver m|^\x0b\0\0......\0\0$|s p/L2J loginserver/
match loginserver m|^\x9b\0\0\xfd\x8a\"\0Zx\0.{129}\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0$|s p/L2J loginserver/
match loginserver m|^\xba\0.{184}$|s p/L2J loginserver/

match meterpreter m|^\0.\x0b\0MZ\xe8\0\0\0\0\x5b\x52\x45\x55\x89\xe5\x81\xc3..\0\0\xff\xd3\x89\xc3Wh\x04\0\0\0P\xff\xd0h\xf0\xb5\xa2Vh\x05\0\0\0P\xff\xd3\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\xe0\0\0\0\x0e\x1f\xba\x0e\0\xb4\t\xcd!\xb8\x01L\xcd!This program cannot be run in DOS mode\.\r\r\n\$\0\0\0\0\0\0\0|s p/Metasploit meterpreter/ i/**BACKDOOR**/
match meterpreter m|^\x16\x03\0\0\x59\x01\0\0\x55\x03\0\x4c\xaa..............................\0\0\(\x00\x39\x00\x38\x00\x35\0\x16\0\x13\0\x0a\x00\x33\x00\x32\0\x2f\0\x07\0\x05\0\x04\0\x15\0\x12\0\x09\0\x14\0\x11\0\x08\0\x06\0\x03\x01\0\0\x04\0\x23\0\0$|s p/Metasploit meterpreter metsvc/ i/**BACKDOOR**/

match millennium-ils m|^\"Thread-15\"  prio=5 \(RUNNABLE\)\r\n------------------------------\r\njava\.lang\.ProcessImpl\.waitFor\(Native Method\)\r\ncom\.iii\.miltoolbarpanel\$ToolbarProcess\$1\.run\(miltoolbarpanel\.java:1168\)\r\n\r\n| p/III Millennium Integrated Library System/

match monalisa m|^\xac\xed\0\x05sr\0\x1elia\.Monitor\.monitor\.monMessage\x8e\xf8\xad\xb0\x14\xe6`!\x02\0\x03L\0\x05identt\0\x12Ljava/lang/Object;L\0\x06resultq\0~\0\x01L\0\x03tagt\0\x12Ljava/lang/String| p/MonALISA monitoring service/

# Monopoly game server
match monopd m|^<monopd><server version=\"([\d.]+)\"/>.*</monopd>\n| p/monopd/ v/$1/ o/Unix/

match mud m|^\n\r\xff\xfbUDo you want ANSI color\? \(Y/n\) $| p|ROM-based MUD| i|http://rrp.rom.org/|

match myproxy m|^VERSION=MYPROXYv([\w._-]+)\nRESPONSE=1\nERROR=authentication failed\n\0$| p/MyProxy credential management/ v/$1/

match mysql m/^.\0\0\0\xff.*Host .* is not allowed to connect to this MySQL server$/s p/MySQL/ i/unauthorized/
match mysql m|^.\0\0\0\xff.\x04Too many connections|s p/MySQL/ i/Too many connections/
match mysql m|^.\0\0\0\xff.\x04Host '[-.\w]+' is blocked because of many connection errors; unblock with 'mysqladmin flush-hosts'|s p/MySQL/ i/Host blocked because of too many connections/
match mysql m|^.\0\0\0\xff.\x04Le h\xf4te '[-.\w]+' n'est pas authoris\xe9 \xe0 se connecter \xe0 ce serveur MySQL$| p/MySQL/ i/unauthorized; French/
match mysql m|^.\0\0\0\xffj\x04Host hat keine Berechtigung, eine Verbindung zu diesem MySQL Server herzustellen\.|s p/MySQL/ i/unauthorized; German/
match mysql m|^.\0\0\0.*Host '[-\w_.]+' hat keine Berechtigung, sich mit diesem MySQL-Server zu verbinden|s p/MySQL/ i/Unauthorized; German/
match mysql m/^.\0\0\0...Al sistema '[-.\w]+' non e` consentita la connessione a questo server MySQL$/s p/MySQL/ i/unauthorized; Italian/
match mysql m|^.\0\0\0\xffi?\x04?Host .* is blocked because of many connection errors\.|s p/MySQL/ i/blocked - too many connection errors/
match mysql m|^.\0\0\0...Servidor '[-.\w]+' est\xe1 bloqueado por muchos errores de conexi\xf3n\.  Desbloquear con 'mysqladmin flush-hosts'|s p/MySQL/ i/Spanish; blocked - too many connection errors/
match mysql m|^.\0\0\0...'Host' '[-.\w]+' n\xe3o tem permiss\xe3o para se conectar com este servidor MySQL| p/MySQL/ i/Spanish; unauthorized/
match mysql m|^.\0\0\0\x0a([\w._-]+)\0............\0\x5f\xd3\x2d\x02\0\0\0\0\0\0\0\0\0\0\0\0\0\0............\0$|s p/Drizzle/ v/$1/
match mysql m|^.\0\0\0\x0a([\w._-]+)\0............\0\x5f\xd1\x2d\x02\0\0\0\0\0\0\0\0\0\0\0\0\0\0............\0$|s p/Drizzle/ v/$1/

match minisql m|^.\0\0\x000:23:([\d.]+)\n$|s p/Mini SQL/ v/$1/

# MySQL 4.0.13
match mysql m/^.\0\0\0.(3\.[-_~.+\w]+)\0.*\x08\x02\0\0\0\0\0\0\0\0\0\0\0\0\0\0$/s p/MySQL/ v/$1/
match mysql m/^.\0\0\0\n(3\.[-_~.+\w]+)\0...\0/s p/MySQL/ v/$1/
match mysql m/^.\0\0\0\n(4\.[-_~.+\w]+)\0/s p/MySQL/ v/$1/
match mysql m|^.\0\0\0\n(5\.[-_~.+\w]+)\0|s p/MySQL/ v/$1/
match mysql m|^.\0\0\0\n(6\.[-_~.+\w]+)\0...\0|s p/MySQL/ v/$1/
match mysql m|^.\0\0\0\xffj\x04'[\d.]+' .* MySQL|s p/MySQL/

match mysql m|^.\0\0\0\n(0[\w._-]+)\0| p/MySQL instance manager/ v/$1/

# TIME
# This is a random 128-byte IV followed by a four-byte timestamp.
# 0x46000000 = Tue Mar 20 09:38:40 2007
# 0x53FFFFFF = Thu Aug 28 22:22:23 2014
match nagios-nsca m|^.{128}[\x46-\x53]...$|s p/Nagios NSCA/

match nbd m|^NBDMAGIC\0\0B| p/Network Block Device/

match ncacn_http m|^ncacn_http/([\d.]+)$| p/Microsoft Windows RPC over HTTP/ v/$1/ o/Windows/
# NCD Thinstar 300 running NCD Software 2.31 build 6
match ncd-diag m|^WinCE/WBT Diagnostic port\n\rSerial Number: (\w+)  MAC Address: 0000(\w+)\s+.*CPU info: ([ -.+\w/ ]+)\r\n.*(Windows CE Kernel[-.+:\w ]+)\r|s p|NCD Thinster Terminal Diagnostic port| i|Serial# $1; MAC: $2; CPU: $3; $4|

match netdevil m|^pass_pleaz$| p/Net-Devil backdoor/ i/**TROJAN**/ o/Windows/
match netsaint m|^Sorry, you \(\d{1,3}\.\d{1,3}\.\d{1,3}\.\d{1,3}\) are not among the allowed hosts\.\.\.\n$| p/Netsaint status daemon/
match netsaint m|^ERROR Client is not among hosts allowed to connect\.| p/Nagios Statd Server/
# I love this service:
match netstat m|^Active Internet connections \(.*\)\nProto Recv-Q Send-Q Local Address           Foreign Address         State      \n| o/Linux/
match netstat m|^Active Internet connections\nProto Recv-Q Send-Q  Local Address          Foreign Address        \(state\)\n| o/QNX/
match netstat m|^netstat: invalid option -- f\nusage: netstat \[-veenNcCF\]| p/Linux netstat/ i/broken/ o/Linux/
match netstat m|^Process Software MultiNet V([\d.]+) Rev A-X, AlphaServer ([\d/ ]+), OpenVMS AXP V([\d.]+)\r\n\r\nProduct                      License    Authorization        Expiration Date\r\n| p/OpenVMS netstatd/ i/PSM $1; AlphaServer $2; OpenVMS AXP $3/ o/OpenVMS/

match netsupport-dna m|^\x01\0\0\0\x01\0\0\0\0\0\0\0\n\x0c00\d{10}$| p/NetSupport DNA asset management/

match netsync m|^\x06\x02...([\w._@-]+)..|s p/Netsync/ v/6/ i/Monotone VCS; key name $1/
match netsync m|^\x00\x64\x01\x00$| p/Netsync/ i/Monotone VCS/

match netbios-ssn m|^smbd: error while loading shared libraries: libattr\.so\.1: cannot open shared object file: No such file or directory\n| p/Samba smbd/ i/Broken/
match netbus m|^NetBus ([\d.]+).*\r$| p/NetBus trojan/ v/$1/ o/Windows/

match nntp m|^nnrpd: invalid option -- S\nUsage error\.\n| p/INN NNTPd/ i/broken/
match nntp m|^502 You have no permission to talk\.  Goodbye.\r\n$| p/INN NNTPd/ i/unauthorized/
match nntp m|^200 ([-.\w]+) NNTP Service Ready - ([-.\w]+@[-.\w]+) \(DIABLO (\d[-.\w ]+)\)\r\n| p/Diablo NNTP service/ h/$1/ v/$3/ i/Admin: $2/
match nntp m|^200 NNTP Service (\d[-.\w ]+) Version: (\d[-.\w ]+) Posting Allowed \r\n| p/Microsoft NNTP Service/ v/$2/ i/posting ok/ o/Windows/
match nntp m|^200 Service NNTP (\d[-.\w ]+) Version: (\d[-.\w ]+) Posting Allowed \r\n| p/Microsoft NNTP Service/ v/$2/ i/posting ok/ o/Windows/
match nntp m|^200 Servicio NNTP (\d[-.\w ]+) Version: (\d[-.\w ]+) Posting Allowed \r\n| p/Microsoft NNTP Service/ v/$2/ i/Spanish; posting ok/ o/Windows/

match nntp m|^200 ([-.\w]+) DNEWS Version *(\d[-.\w]+).*posting OK \r\n| p/Netwinsite DNEWS/ h/$1/ v/$2/ i/posting OK/
match nntp m|^200 Leafnode NNTP Daemon, version (\d[-.\w]+) running at| p/Leafnode NNTPd/ v/$1/
match nntp m|^200 Lotus Domino NNTP Server for ([-./\w]+) \(Release (\d[-.\w]+), .*\) - Not OK to post\r\n$| p/Lotus Domino nntpd/ v/$2/ i/posting denied/ o/$1/
match nntp m|^200 Lotus Domino NNTP Server for ([-./\w]+) \(Release (\d[-.\w]+), .*\) - OK to post\r\n$| p/Lotus Domino nntpd/ v/$2/ i/posting ok/ o/$1/

match nntp m|^200 NNTP Service 5\.00\.0984 Version: (5\.0\.2159.1) Posting Allowed \r\n| p/Microsoft NNTP Service/ v/$1/ i/posting OK/ o/Windows 2000/
match nntp m|^200 NNTP Service Microsoft\xae Internet Services (\d[-.\w]+) Version: (\d[-.\w]+) Posting Allowed \r\n| p/Microsoft NNTP Service $1/ v/$2/ i/posting OK/ o/Windows/
match nntp m|^502 Connection refused\r\n| p/Microsoft NNTP Service/ i/refused/ o/Windows/
# Windows NT 4.0 SP5-SP6 
match nntp m|^20[01] Microsoft Exchange Internet News Service Version (\d\.\d\.[.\d]+) \((.*)\)\r\n| p/Microsoft Exchange Internet News Service/ v/$1/ i/$2/ o/Windows/
match nntp m|^20. ([-.\w]+) InterNetNews NNRP server INN (\d[-.\w ]+) ready \(posting ok\)\.\r\n| p/InterNetNews (INN)/ h/$1/ v/$2/ i/posting ok/
match nntp m|^20. ([-.\w]+) InterNetNews NNRP server INN (\d[-.\w ]+) ready \(no posting\)\.\r\n| p/InterNetNews (INN)/ h/$1/ v/$2/ i/no posting/
match nntp m|^200 ArGoSoft News Server for WinNT/2000/XP v ([\d.]+) ready\r\n| p/ArGoSoft nntpd/ v/$1/ o/Windows/
match nntp m|^400 No space left on device writing SMstore file -- throttling\r\n| p/InterNetNews (INN)/ i/HDD full/
match nntp m/^200 NNTP-Server Classic Hamster (Vr\.|Version) \d[-.\w ]+ \(Build (\d[-.\w ]+)\) \(post ok\) says: Hi!\r\n/ p/Classic Hamster NNTPd/ v/$2/ i/posting ok/ o/Windows/
# Netware News Server
match nntp m|^200 ([\w.-_]+) NetWare-News-Server/([\d.]+) 'LDNUM' NNRP ready \(posting ok\)\.\r\n| p/NetWare nntpd/ v/$2/ h/$1/
match nntp m|^200 Leafnode NNTP daemon, version ([\w.]+) at ([-\w_.]+) \r\n| p/Leafnode nntpd/ v/$1/ h/$2/
match nntp m|^\nLeafnode must have a fully-qualified and globally unique domain name,\nnot just \"([-\w_.]+)\"\.\n| p/Leadnode nntpd/ h/$1/ i/misconfigured/
match nntp m|^20\d ([\w.-_]+) NNTPCache server V([\d.]+) \[see www\.nntpcache\.org\]| p/NNTPCache/ v/$2/ h/$1/
match nntp m|^502 access denied <[-\w_.]+@[-\w_.]+>, you do not have connect permissions in the nntpcache\.access file\.\r\n| p/NNTPCache/ i/Access denied/
match nntp m|^200 ([-\w_.]+) InterNetNews NNRP server INN ([\d.]+) .* \(Debian\) ready \(posting ok\)\.\r\n| p/INN nntpd/ v/$2/ h/$1/ o/Linux/ i/on Debian; posting ok/
match nntp m|^200 ([-\w_.]+) InterNetNews (NNRP )?server INN ([\d.]+) .* ready \(posting ok\)\.\r\n| p/INN nntpd/ v/$3/ h/$1/ i/posting ok/
match nntp m|^201 ([-\w_.]+) InterNetNews (NNRP )?server INN ([\d.]+) .* ready \(no posting\)\.\r\n| p/INN nntpd/ v/$3/ h/$1/ i/no posting/
match nntp m|^200 ([-\w_.]+) InterNetNews (NNRP )?server INN ([\d.]+) .* ready\r\n| p/INN nntpd/ v/$3/ h/$1/
#atch nntp m|^200 ([-\w_.]+) InterNetNews server INN 2\.4\.2 \(20040820 prerelease\) ready\r\n
match nntp m|^200 ([-\w_.]+) NNRP Service Ready - [-\w_.]+@[-\w_.]+ \(posting ok\)\.\r\n| p/INN nntpd/ h/$1/ i/posting ok/
match nntp m|^200 ([-\w_.]+) InterNetNews server INN ([\d.]+) ready\r\n| p/INN nntpd/ v/$2/ h/$1/
match nntp m|^200 nntp//rss v([\d.]+) news server ready\r\n| p|nntp//rss nntpd| v/$1/
match nntp m|^200 Hi, you can post \(sn version ([\w.]+)\)\r\n| p/sn nntpd/ v/$1/ i/posting ok/
match nntp m|^200 ([-\w_.]+) NNTP Service Ready, posting permitted\r\n| p/JAMES nntpd/ h/$1/ i/posting ok/
match nntp m|^200 Jana news server ready - posting allowed\r\n| p/Jana nntpd/ i/posting ok/ o/Windows/
match nntp m|^200 NNTP server NOFFLE ([\w.]+)\r\n| p/NOFFLE nntpd/ v/$1/
match nntp m|^200 Servizio NNTP [\d.]+ Version: ([\d.]+) Posting Allowed \r\n| p/Servizio nntpd/ v/$1/ i/posting ok/
match nntp m|^502 Could not get your access name\.  Goodbye\.\r\n| p/inn2 nntpd/ i/unauthorized/
match nntp m|^201 NNTP server ready \(no posting\)\r\n502 No permission\r\n| p/Symantic Enterprise Firewall nntpd/ i/unauthorized/ d/firewall/
match nntp m|^502 ([-\w_.]+): Transfer permission denied to [\d.]+ - [-\w_.@]+ \(DIABLO ([-\w_.]+)\)\r\n| p/Diablo nntpd/ v/$2/ h/$1/ o/Unix/
match nntp m|^200 ([-\w_.]+) - colobus ([\d.]+) ready - \(posting ok\)\.\r\n| p/Colobus nntpd/ v/$1/ i/posting ok/
match nntp m|^200 Welcome to .* \(Typhoon v([\d.]+)\)\r\n| p/Typhoon nntpd/ v/$1/
match nntp m|^200 +Kerio MailServer ([\d.]+) +NNTP server ready\r\n| p/Kerio MailServer nntpd/ v/$1/
match nntp m|^200 NewsCache ([-\w_.]+), accepting NNRP commands\r\n| p/Newscache nntp cache/ v/$1/
match nntp m|^200 ([\w._-]+) Cyrus NNTP v([\w._-]+) server ready, posting allowed\r\n| p/Cyrus nntpd/ h/$1/ v/$2/ i/posting ok/
match nntp m|^200 ([-\w_.]+) ready for action \(Mailtraq ([\d.]+)/NNTP\)\r\n| p/Mailtraq nntpd/ v/$2/ h/$1/ o/Windows/
match nntp m|^200 Service available, posting allowed\r\n| p/Freenet Message System nntpd/
match nntp m|^200 NNTP-service [\d.]+ Version: ([\d.]+) Posting Allowed \r\n| p/Microsoft NNTP service/ v/$1/
match nntp m|^200 ([-\w._]+) InterNetNews NNRP server INN (.*) ready \(posting ok\)\r\n| p/InterNetNews NNRP server/ h/$1/ v/$2/

match nntp-proxy m|^200 CCProxy NNTP Service\r\n| p/CCProxy NNTP proxy/ o/Windows/
match nntp-proxy m|^200 avast! NNTP proxy ready\.\r\n$| p/Avast! anti-virus NNTP proxy/ o/Windows/

softmatch nntp m|^200 [-\[\]\(\)!,/+:<>@.\w ]*nntp[-\[\]\(\)!,/+:<>@.\w ]*\r\n$|

match novastor-backup m|^\x02\0\0\0\0\0\0#\x01\x80\x01.([\w._-]+)\x02\x13(\d\d/\d\d/\d\d\d\d \d\d:\d\d:\d\d)\0\0|s p/NovaNET-WEB backup/ v/$1/ i/$2/

# Windows 2000 Server Windows Media Unicast Service (NsUnicast) - Nsum.exe
match nsunicast m|^4\0\0\0V4\x12\0\0\0\0\0\0\0\0\x004\0\0\0\x04\0\xf0\0.\x07.\0.\0.\0.\0.\0.\0..\0\0\0\0.\0\0\0.\0\0\0\x02\0|s p/Microsoft Windows Media Unicast Service/ i/nsum.exe/ o/Windows/
match nsunicast m|^[4f]\0\0\0V4\x12\0\0\0\0\0\0\0\0\x00[4f]\0\0\0.\0\xf0\0\xd3\x07\t\0.\0.\0.\0.\0.\0..\0\0\0\0.\0\0\0..\0\0.\0|s p/Microsoft Windows Media Unicast Service/ i/nsum.exe/ o/Windows/

match netsupport m|^.\0\x02\0([^\0]+)\0+.\0\x01\0|s p/NetSupport PC remote control/ i/Name $1/

match oftp m|^\x10\0\0\x17IODETTE FTP READY \r$| p/ODETTE File Transfer Protocol/

match openlookup m|^\d+:d7:smethod,6:shello,8:soptions,\d+:d10:shttp_port,\d+:i\d+,5:sname,\d+:s([\w._-]+),10:ssync_port,\d+:i\d+,10:stimestamp,\d+:f[\d.]+,8:sversion,\d+:s([\w._-]+),| p/OpenLookup/ v/$2/ h/$1/

match parallels-server m|^PRLT\x06\0\0\x00([\w._-]+ \(\w\w\w, \d\d \w\w\w \d\d\d\d \d\d:\d\d:\d\d\))\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0$| p/Parallels Server/ v/$1/

# *B1E1 is magic. Protocol implementation at
# http://www.papouch.com/shop/scripts/soft/tmedotnet/readme.asp
match papouch-tme m|^\*B1E1([\+-]\d\d\d\.\d)\r$| p/Papouch TME Ethernet thermometer/ i/temperature: $1 C/

match partimage m|^([\d.]+) SSL( LOG)?\0            +\0$| p/Partimage+SSL/ v/$1/ o/Linux/

match patrol m|^\0\0\0\r..Who are you\?\n\0|s p/BMC Patrol Agent/ o/Unix/
match pcanywheredata m/^\0X\x08\0\}\x08\r\n\0\.\x08.*\.\.\.\r\n/s p/PCAnywhere/ o/Windows/
match pbmasterd m|^pbmasterd(\d[-.\w]+)@[-.+\w]+: | p/Symark Power Broker pbmasterd/ v/$1/ i/privilege separation software/
match pblocald m|^pblocald(\d[-.\w]+)@[-.+\w]+: | p/Symark Power Broker pblocald/ v/$1/ i/privilege separation software/
match p4d m|^..\0\0\0xfiles\0\x01\0\0\x005\0server\0\x01\0\0\x003\0server2\0\x02\0\0\x00..\0|s p/Perforce configuration daemon/
# Pharos Notify 7.1
match pharos m/^PSCOM(\xb6|\$)\0\0.*AUTHENTICATE/s p/Pharos Notify/ i/printing client/
match pjlink m|^PJLINK 0\r$| p/PJLink projector control/ d/media device/
match pjlink m|^PJLINK 1 [0-9a-f]{8}\r$| p/PJLink projector control/ d/media device/

match poweroff m|^201 Welcome to Poweroff ([\d.]+) created by Jorgen Bosman\r\n| p/Poweroffd/ v/$1/ o/Windows/

match prelude-manager m|^\x01\x04\0\0\0\0\0\rD| p/Prelude IDS manager/
match polycom-mgc m|^NotAuthorized\0\0\0\0\0\0\0\0\0\0\0\0| p/Polycom VSX 8000 MGC Manager/ d/webcam/

# This one is probably too specific... need more submissions
match pyro m|^PYRO\0\x04\0\x12\0\0\0\x10\0\0\0\0\0\0| p/Python Remote Object Nameserver/

match pksd m|^usage: [/\w]*/etc/pksd\.conf conf_file\n$| p/PGP Public Key Server/ i/broken/

match pioneers m|^version report\n| p/Pioneers game server/
match pioneers-meta m|^welcome to the pioneers-meta-server version ([\d.]+)\n| p/Pioneers game meta server/ v/$1/

# UW POP2 server on Linux 2.4.18
match pop2 m|^\+ POP2 [-\[\].\w]+ v([-.\w]+) server ready\r\n$| p/UW POP2 server/ v/$1/

# Novell Groupwise 6.0.1
match pop3 m|^\+OK GroupWise POP3 server ready\r\n$| p/Novell GroupWise pop3d/ o/Unix/
match pop3 m|^\+OK Ready when you are <200\d+\.| p/Hotmail Popper hotmail to pop3 gateway/
match pop3 m|^\+OK Internet Rex POP3 server ready <| p/Internet Rex Pop3 server/
match pop3 m|^\+OK DBMAIL pop3 server ready to rock <| p/DBMail pop3d/
match pop3 m|^\+OK POP3 POPFile \(v(\d[-.\w]+)\) server ready\r\n| p/POPFile pop3d/ v/$1/
# Dots in Revision to prevent MY CVS from screwing it up
match pop3 m|^\+OK ([-.+\w]+) NetMail POP3 Agent \$Re..sion: ([\d.]+) \$\r\n| p/Novell NetMail pop3d/ h/$1/ v/$2/ o/Unix/
match pop3 m|^\+OK ([-.+\w]+) Merak (\d[-.\w]+) POP3 | p/Merak Mail server pop3d/ h/$1/ v/$2/ o/Windows/
match pop3 m|^\+OK \]-:\^:-\[ \]-:\^:-\[ POP3| p/Merak Mail Server pop3d/ o/Windows/
match pop3 m|^\+OK ([-\w_.]+) [-\w_.]+ Mail Server ([\d.]+) POP3 .*\d:\d\d:\d\d \+| p/Merak Mail Server pop3d/ v/$2/ h/$1/ o/Windows/
# Mercury/32 3.32 pop3 Server module on Windows XP
match pop3 m|^\+OK <\d{6,10}\.\d{4,6}@([-.+\w]+)>, POP3 server ready\.\r\n| p|Mercury/32 pop3d| o|Windows| h|$1|
# gnu/mailutils pop3d 0.3.2 on Linux
match pop3 m|^\+OK POP3 Ready <\d{3,6}\.1[012]\d{8}@([-.\w]+)>\r\n| p|GNU mailutils pop3d| h|$1|
# Solid POP3 Server 0.15 on Linux 2.4
match pop3 m|^\+OK Solid POP3 server ready\r\n| p/Solid pop3d/
match pop3 m|^\+OK Solid POP3 server ready <\d{3,6}\.1[012]\d{8}@([-.\w]+)>\r\n| p/Solid pop3d/ h/$1/
# Cyrus POP3 v2.0.16
match pop3 m|^\+OK ([-.\w]+) Cyrus POP3 v(\d[-.\w\+]+) server ready ?\r\n| p/Cyrus POP3/ h/$1/ v/$2/
match pop3 m|^\+OK  ?([-.\w]+) Cyrus POP3 Murder v(\d[-.\w\+]+) server ready ?\r\n| p/Cyrus POP3 Murder/ h/$1/ v/$2/
#  pop3d (GNU Mailutils 0.3) on Linux 2.4
match pop3 m|^\+OK POP3 Ready <\d{3,6}\.1[012]\d{8}@(\w+)>\r\n| p/GNU Mailutils pop3d/ h/$1/
# Solid POP3 Server 0.15_1 on FreeBSD
match pop3 m|^\+OK ([\w\d_-]+\.[\w\d_.-]+) POP3 <\d{3,6}\.1[012]\d{8}@[-.\w]+>\r\n| p/Solid pop3d/ h/$1/
#  pop3d (GNU Mailutils 0.3) on Linux 2.4
match pop3 m|^\+OK POP3 Ready <\d{3,6}\.1[012]\d{8}@\w+>\r\n| p/GNU Mailutils pop3d/
# dovecot 0.99.10 on Linux 2.4
match pop3 m|^\+OK [Dd]ovecot ready\.\r\n| p/Dovecot pop3d/
match pop3 m|^\+OK dovecot MUA ready\r\n| p/Dovecot MUA pop3d/
match pop3 m|^\+OK [Dd]ovecot ready\. ?<.*@([-\w_.]+)>\r\n| p/Dovecot pop3d/ h/$1/
match pop3 m|^\+OK [Dd]ovecot on ([\w._-]+) ready\.\r\n| p/Dovecot pop3d/ h/$1/
match pop3 m|^\+OK Dovecot ready -| p/Dovecot pop3d/
match pop3 m|^\+OK (.*) Dovecot ready\.\r\n$| p/Dovcot pop3d/ i/$1/
match pop3 m|\+OK E-mail server ready\.\r\n| p/Dovecot pop3d/
match pop3 m|^\+OK Dovecot at ([-\w_.]+) ready\.\r\n| p/Dovecot pop3d/ h/$1/
# teapop 0.3.5 on Linux 2.4
match pop3 m|^\+OK Teapop \[v?(\d[-.\w ]+)\] - Teaspoon stirs around again .*\r\n| p/Teapop pop3d/ v/$1/
# Qpopper v4.0.5 on Linux 2.4.19
match pop3 m|^\+OK ready  \r\n$| p/Qpopper pop3d/
# Jana Server 1.45 on Win98
match pop3 m|^\+OK POP3 server ready <Jana-Server>\r\n| p/Jana POP3 server/ o/Windows/
match pop3 m|^\+OK AppleMailServer (\d[-.\w]+) POP3 server at ([-.\w]+) ready <\d| p/AppleMailServer pop3d/ h/$1/ v/$2/
match pop3 m|\+OK <10\d+\.\d+@([-.\w]+)> \[XMail (\d[-.\w]+) \(([-./\w]+)\) POP3 Server\] service ready; | p/XMail pop3 server/ h/$1/ v/$2/ o/$3/
# Mail-Enable pop3 server 1.704
match pop3 m|^\+OK Welcome to MailEnable POP3 Server| p/MailEnable POP3 Server/ o/Windows/
match pop3 m|^\+OK ([-.\w]+) running Eudora Internet Mail Server (\d[-.\w]+) <.*>\r\n| p/Eudora Internet Mail Server pop3d/ h/$1/ v/$2/
# Qpopper 4.0.3 on Linux
# QPopper 4.0.4 FreeBSD
match pop3 m|^\+OK ready  <\d{1,5}\.10\d{8}@([-.\w]+)>\r\n| p/Qualcomm Qpopper pop3d/ h/$1/
match pop3 m|^\+OK POP3 Welcome to GNU POP3 Server Version (\d[-.\w]+) <.*>\r\n| p/GNU POP3 Server/ v/$1/
match pop3 m|^\+OK eXtremail V(\d[-.\w]+) release (\d+) POP3 server ready <[\d.]+@([-\w_.]+)>\r\n| p/eXtremail pop3d/ v/$1 rel$2/ h/$3/
match pop3 m|^\+OK eXtremail V(\d[-.\w]+) release (\d+) rev(\d+) POP3 server ready <[\d.]+@([-\w_.]+)>\r\n| p/eXtrememail pop3d/ v/$1 rel$2 rev$3/ h/$4/
match pop3 m|^\+OK POP3 Welcome to vm-pop3d (\d[-.\w]+)| p/vm-pop3d/ v/$1/ i/derived from gnu-pop3d/
# tpop3d v1.4.2 on Linux - http://www.ex-parrot.com/~chris/tpop3d/
match pop3 m|^\+OK <[\da-f]{32}@([-.\w]+)>\r\n| p/tpop3d/ h/$1/
match pop3 m|^\+OK UCB based pop server \(version (\d[-.\w]+) at sionisten\) starting\.\r\n| p/Heimdal kerberized pop3/ v/$1/ i/UCB-pop3 derived/
# VPOP3 (Virtual POP3 server) 2.0.0d on Windows 2000
match pop3 m|^\+OK VPOP3 Server Ready <.*>\r\n| p/PSCS VPop3/
match pop3 m|^\+OK Lotus Notes POP3 server version ([-.\w]+) ready .* on ([^/]+)/([^\.]+)\.\r\n| p/Lotus Domino POP3 server/ v/$1/ i/CN=$2;Org=$3/
match pop3 m|^\+OK Lotus Notes POP3 server version ([-.\w]+) ready on | p/Lotus Domino POP3 server/ v/$1/
match pop3 m|^\+OK Lotus Notes POP3 server version Release ([-.\w]+) ready on | p/Lotus Domino POP3 server/ v/$1/
match pop3 m|^\+OK POP3 hotwayd v(\d[-.\w]+) -> The POP3-HTTPMail Gateway\.| p/hotwayd pop3d/ v/$1/
match pop3 m|^\+OK ([-.\w]+) POP3 service \(Netscape Messaging Server (\d[^(]+) \(built ([\w ]+)\)\)\r\n| p/Netscape Messenging Server pop3/ h/$1/ v/$2/ i/built on $3/
match pop3 m/^\+OK ([-.\w]+) Cyrus POP3 v(\d[-.\w]+) server ready </ p/Cyrus pop3d/ h/$1/ v/$2/
match pop3 m|^\+OK ([-.\w]+) Cyrus POP3 v(\d[-.\w]+)-Red Hat [-\d.]+ server ready <| p/Cyrus pop3d/ h/$1/ v/$2/ i/Red Hat/ o/Linux/
match pop3 m|^\+OK ([-.\w]+) Cyrus POP3 v(\d[-.\w]+)-OS X ([\d.]+) server ready <| p/Cyrus pop3d/ v/$2/ h/$1/ i/Mac OS X $3/ o/Mac OS X/
match pop3 m|^\+OK ([-\w_.]+) Cyrus POP3 v(\S+Debian\S+) server ready| p/Cyrus pop3d/ v/$2/ h/$1/ i/Debian/ o/Linux/
match pop3 m|^\+OK <[\d.]+@([\w._-]+)> [\w._-]+ Cyrus POP3 v([\w._-]+) server ready\r\n| p/Cyrus pop3d/ h/$1/ v/$2/
match pop3 m/^\+OK X1 NT-POP3 Server ([-\w.]+) \(IMail ([^)]+)\)\r\n/ p/IMail pop3d/ h/$1/ v/$2/
match pop3 m/^\+OK POP3 \[cppop (\d[^]]+)\] at \[/ p/cppop pop3d/ v/$1/
match pop3 m|^\+OK POP3 ([-\w_.]+) \[cppop (\d[^]]+)\] at \[| p/cppop pop3d/ v/$2/ h/$1/
match pop3 m|^\+OK Gpop ready for requests from [\d\.]+ ([\w\d]+)| p/Google Gmail pop3d/ i/$1/

# MS Exchange
match pop3 m|^\+OK Microsoft Exchange Server 2003 POP3 server version ([\d.]+) \(([-\w_.]+)\) ready\.\r\n| p/MS Exchange 2003 pop3d/ v/$1/ h/$2/ o/Windows/
match pop3 m/^\+OK Microsoft Exchange 2000 POP3 server version (\S+).* ready\.\r\n/ p/MS Exchange 2000 pop3d/ v/$1/ o/Windows/
match pop3 m/^\+OK Microsoft Exchange POP3 server version (\S+) ready\r\n/ p/MS Exchange pop3d/ v/$1/ o/Windows/
match pop3 m|^\+OK Microsoft Exchange POP3 server version ([\d.]+) ready  <[\d.]+@([-\w_.]+)>\r\n| p/MS Exchange pop3d/ v/$1/ h/$2/ o/Windows/
match pop3 m/^\+OK Der Microsoft Exchange POP3-Server \(Version ([\d\.]+)\) ist betriebsbereit\.\r\n/ p/MS Exchange pop3d/ v/$1/ i/German/ o/Windows/
match pop3 m|^\+OK Der Microsoft Exchange Server 2003 POP3-Server, Version ([\d.]+) \(([-\w_.]+)\), steht zur Verf\xfcgung\.\r\n| p/MS Exchange 2003 pop3d/ v/$1/ h/$2/ i/German/ o/Windows/
match pop3 m|^\+OK Microsoft Exchange Server 2003 POP3 \xb7\xfe\xce\xf1\xc6\xf7\xb0\xe6\xb1\xbe ([\d.]+) \(([-\w_.]+)\)| p/MS Exchange 2003 pop3d/ v/$1/ h/$2/ i/Chinese/ o/Windows/
match pop3 m|^\+OK Microsoft Exchange Server 2003 POP3 \xbc\xad\xb9\xf6 \xb9\xf6\xc0\xfc ([\d.]+) \(([-\w_.]+)\)| p/MS Exchange 2003 pop3d/ v/$1/ h/$2/ i/Korean/ o/Windows/
match pop3 m/^\+OK Microsoft Exchange POP3-server versie ([\d.]+) is gereed\.\r\n/ p/MS Exchange pop3d/ v/$1/ i/Dutch/
match pop3 m|^\+OK \xd1\xe5\xf0\xe2\xe5\xf0 Microsoft Exchange POP3 \xe2\xe5\xf0\xf1\xe8\xe8 ([\d.]+)  \xe3\xee\xf2\xee\xe2\r\n| p/MS Exchange pop3d/ v/$1/ i/Unknown language/
match pop3 m|^\+OK Microsoft Exchange POP3 kiszolg\xe1l\xf3 verzi\xf3 ([\d.]+) k\xe9sz\r\n| p/MS Exchange pop3d/ v/$1/ i/Hungarian/
match pop3 m|^\+OK Le serveur POP3 Microsoft Exchange Server 2003 version ([\d.]+) \(([-\w_.]+)\) est pr\xeat\.\r\n| p/MS Exchange 2003 pop3d/ v/$1/ h/$2/ i/French/
match pop3 m|^\+OK Le serveur POP3 Microsoft Exchange version ([\d.]+) est pr\xeat\r\n| p/MS Exchange pop3d/ v/$1/ i/French/
match pop3 m|^\+OK Microsoft Exchange POP3 server verze ([\d.]+) je p\xf8ipraven\.\r\n| p/MS Exchange pop3d/ v/$1/ i/Czech/ o/Windows/
match pop3 m|^\+OK Microsoft Exchange Server 2003 POP3 \xa6\xf8\xaaA\xbe\xb9\xaa\xa9\xa5\xbb ([\d.]+) \(([-\w_.]+)\) \xa5i\xa5H\xa8\xcf\xa5\xce\xa1C\r\n| p/MS Exchange 2003 pop3d/ v/$1/ i/Taiwanese?/ h/$2/ o/Windows/
match pop3 m|^\+OK Servidor POP3 de Microsoft Exchange Server 2003 versi\xf3n ([\d.]+) \(([\w._-]+)\) listo\.\r\n| p/MS Exchange 2003 pop3d/ v/$1/ i/Spanish/ h/$2/ o/Windows/
match pop3 m|^\+OK Server POP3 di Microsoft Exchange Server 2003 versione ([\w._-]+) \(([\w._-]+)\) pronto\.\r\n| p/MS Exchange 2003 pop3d/ v/%1/ i/Italian/ h/$2/ o/Windows/

match pop3 m|^\+OK Microsoft Exchange Server 2007 POP3 service ready\r\n| p/MS Exchange 2007 pop3d/ o/Windows/
match pop3 m|^\+OK Microsoft Exchange Server 2007 POP3 HIROC service ready\r\n| p/MS Exchange 2007 pop3d/ o/Windows/
match pop3 m|^\+OK The Microsoft Exchange POP3 service is ready\.\r\n| p/MS Exchange 2007 pop3d/ o/Windows/
match pop3 m/^\+OK QPOP \(version ([^)]+)\) at .*starting\./ p/Qpop pop3d/ v/$1/
match pop3 m/^\+OK QPOP Modified by Compaq \(version ([^)]+)\) at .*starting\./ p/QPop pop3d/ v/$1/
match pop3 m/^\+OK Qpopper .*\(version ([^)]+)\) at .*starting\./ p/Qpopper pop3d/ v/$1/
match pop3 m/^\+OK ([-.\w]+) POP3 server \(Netscape Mail Server v(\d[-.\w])\) ready/ p/Netscape Mail Server pop3d/ h/$1/ v/$2/
match pop3 m/^\+OK Cubic Circle's v(\d[-.\w]+) .* POP3 ready/ p/Cubic Circle Cucipop pop3d/ v/$1/
match pop3 m/^\+OK ArGoSoft Mail Server Freeware, Version \S+ \(([^)]+)\)\r\n$/ p/ArGoSoft freeware pop3d/ v/$1/
match pop3 m|^\+OK ArGoSoft Mail Server, Version [-.\w]+ \(([-.\w]+)\)\r\n$| p/ArGoSoft Mail Server pop3d/ v/$1/
match pop3 m|^\+OK ArGoSoft Mail Server POP3 Module v\.([\w._-]+) at | p/ArGoSoft Mail Server pop3d/ v/$1/ o/Windows/
match pop3 m|^\+OK ArGoSoft Mail Server Pro for WinNT/2000/XP, Version [-.\w]+ \(([-.\w]+)\)\r\n$| p/ArGoSoft Mail Server Pro pop3d/ v/$1/ o/Windows/
match pop3 m|^\+OK ([-\w.]+) ArGoSoft Mail Server Pro for WinNT/2000/XP, Version [\d.]+ \(([\d.]+)\)\r\n| p/ArGoSoft Pro/ v/$2/ h/$1/ o/Windows/
match pop3 m|^\+OK ArGoSoft Mail Server Plus for WinNT/2000, Version [\d.]+ \(([\d.]+)\)\r\n| p/ArGoSoft Plus/ v/$1/ o/Windows/
match pop3 m/^\+OK ([-.\w]+) Execmail POP3 \((\d[^)]+)\)/ p/Execmail pop3d/ h/$1/ v/$2/
match pop3 m/^\+OK MailSite POP3 Server (\S+) Ready </ p/MailSite pop3d/ v/$1/
match pop3 m/^\+OK ([-.\w]+) POP3? MDaemon (\S+) ready <MDAEMON/ p/MDaemon pop3d/ h/$1/ v/$2/ o/Windows/
match pop3 m|^\+OK ([-.\w]+) POP MDaemon ready using UNREGISTERED SOFTWARE ([\d.]+) <MDAEMON| h/$1/ v/$2/ o/Windows/ i/unregistered/
match pop3 m|^\+OK ([-\w_.]+) POP MDaemon ([\d.]+) listo <MDAEMON-[\w.]+@[-\w_.]+>\r\n| p/MDaemon pop3d/ v/$2/ i/Spanish/ h/$1/ o/Windows/
match pop3 m|^\+OK ([-\w_.]+) POP MDaemon ([\d.]+) \xd7\xbc\xb1\xb8\xba\xc3 <MDAEMON-[\w.]+@[-\w_.]+>\r\n| p/MDaemon pop3d/ v/$2/ i/Chinese/ h/$1/ o/Windows/
match pop3 m|^\+OK ([-\w_.]+) POP MDaemon ([\d.]+) ready\r\n| p/MDaemon pop3d/ v/$2/ h/$1/ o/Windows/

# qmail-pop3d 1.03-1
match pop3 m/^\+OK <\d{1,5}\.10\d{8}@[-.\w]+>\r\n$/ p/qmail-pop3d/ o/Unix/
# Courier Pop3 courier-pop3d-0.42.0-1.7.3
match pop3 m|^\+OK Hello there\.\r\n$| p/Courier pop3d/
match pop3 m|^\+OK Hello there\. <[\d.]+@([-\w_.]+)>\r\n$| p/Courier pop3d/ h/$1/
match pop3 m/^\+OK ([-.\w]+) VisNetic.MailServer.v([-.\w]+) POP3 / p/VisNetic MailServer pop3d/ h/$1/ v/$2/
match pop3 m/^\+OK ([-.\w]+) POP3 server \(Post\.Office v([-.\w]+) release ([-.\w]+) with ZPOP version ([-.\w]+)/ p|Post.Office pop3d| h|$1| v|$2 release $3| i|w/ZPOP $4|
match pop3 m/^\+OK CommuniGate Pro POP3 Server ([-.\w]+) ready/ p/CommuniGate Pro/ v/$1/
match pop3 m|^\+OK CommuniGate Pro POP3 Server ready <[\d.]+@([-\w_.]+)>\r\n| p/CommuniGate Pro/ h/$1/
match pop3 m/^\+OK\r\n$/ p/Openwall popa3d/
match pop3 m|^\+OK ([-.\w]+) MultiNet POP3 Server Process V(\S+) at| p/DEC OpenVMS MultiNet pop3d/ h/$1/ v/$2/
match pop3 m|^\+OK <.*>, MercuryP/NLM v(\d[-.\w]+) ready.\r\n$| p/Mercury POP3 server/ v/$1/ o/NetWare/
match pop3 m|^\+OK Microsoft Windows POP3 Service Version 1.0 <| p/Microsoft Windows 2003 POP3 Service/ v/1.0/ o/Windows 2000/
match pop3 m|^\+OK POP3 ([-.\w]+) v?(200\d\w?\.[-.\w]+) server ready\r\n| p/UW Imap pop3d/ h/$1/ v/$2/
match pop3 m|^\+OK POP3 v?([\d.]+) server ready <[\w.]+@([-\w_.]+)>\r\n| p/UW Imap pop3d/ v/$1/ h/$2/
match pop3 m|^\+OK POP3 \[([-\w_.]+)\] v([\d.]+) server ready\r\n| p/UW Imap pop3d/ h/$1/ v/$2/
match pop3 m|^\+OK POP3 server ready <\w{11}>\r\n$| p/WebSTAR pop3 server/
match pop3 m|^\+OK Kerio MailServer (\d[-.\w]+) POP3 server ready <([-.\w@:]+)>\r\n$| p/Kerio MailServer POP3 Server/ v/$1/ i/$2/
match pop3 m|^\+OK Kerio MailServer (\d[-.\w]+) POP3 server ready <| p/Kerio MailServer POP3 Server/ v/$1/
match pop3 m|^\+OK Kerio MailServer (\d[-.\w]+) patch ([\d.]+) POP3 server ready <[\d.]+@\(null\)>\r\n| p/Kerio MailServer POP3 Server/ v/$1 patch $2/
match pop3 m|^\+OK Kerio MailServer (\d[-.\w]+) patch ([\d.]+) POP3 server ready <[\d.]+@([-\w_.]+)>\r\n| p/Kerio MailServer POP3 Server/ v/$1 patch $2/ h/$3/
match pop3 m/^\+OK POP3-Server Classic Hamster (Vr\.|Version) [\d.]+ \(Build ([\d.]+)\) greets you! <.*>\r\n/ p/Classic Hamster pop3d/ v/$2/ o/Windows/
match pop3 m|^\+OK Stalker POP3 Server ([\w.]+) at ([-\w_.]+) ready <.*>\r\n| p/Stalker pop3d/ v/$1/ h/$2/ o/Mac OS/
match pop3 m|^\+OK ([-\w_.]+) POP3 service \(iPlanet Messaging Server ([-\w_.\s]+) \(built .*\)\)\r\n| p/iPlanet pop3d/ v/$2/ h/$2/
match pop3 m|^\+OK Messaging Multiplexor \(iPlanet Messaging Server ([-\w_.\s]+) \(built .*\)\)\r\n| p/iPlanet messaging multiplexor/ v/$1/
match pop3 m|^\+OK WinGate Engine POP3 Gateway ready\r\n| p/WinGate pop3d/ o/Windows/
match pop3 m|^\+OK ([-\w_.]+) Oracle Email Server espop3\t([\d.]+) \t  is ready\r\n| p/Oracle pop3d/ v/$2/ h/$1/
match pop3 m|^\+OK InterMail POP3 server ready\.\r\n| p/InterMail pop3d/
match pop3 m|^\+OK WinRoute Pro ([\d.]+) POP3 server ready <[-\w_.]+@unspecified.host>\r\n| p/WinRoute Pro pop3/ v/$1/
match pop3 m|^\+OK WinRoute Pro ([\d.]+) POP3 server ready <[-\w_.]+@([-\w_.]+)>\r\n| p/WinRoute Pro pop3/ v/$1/ h/$2/
match pop3 m|^\+OK ([-\w_.]+) POP3 server \(Netscape Messaging Server - Version ([\d.]+)\) ready .*\r\n| p/Netscape Messaginging Server pop3d/ v/$2/ h/$1/
match pop3 m|^\+OK [-\w_.]+ PopMax version ([\d. ]+) POP3 Mail Server Ready, Willing, and Waiting\r\n| p/MailMax PopMax pop3d/ v/$1/ o/Windows/
match pop3 m|^\+OK POP3 Welcome to GNU POP3 ([-\d.]+) <[\d.]+@([-\w_.]+)>\r\n| p/GNU POP3/ v/$1/ h/$2/
match pop3 m|^\+OK popserver ([\d.]+) pop3 server ready\r\n| p/LiberoPops pop3d/ v/$1/
match pop3 m|^\+OK ([-\w_.]+) POP3 server \(JAMES POP3 Server ([\w.]+)\) ready \r\n| p/JAMES pop3d/ v/$2/ h/$1/
match pop3 m|^\+OK ([-\w_.]+) NetMail POP3 Agent \$R...sion:   ([\d.]+)  \$\r\n| p/NetMail pop3d/ v/$2/ h/$1/
match pop3 m|^\+OK POP3 server ready \(Worldmail ([\d.]+)\) <[\w.]+@([-\w_.]+)>\r\n| p/Eudora Worldmail pop3d/ v/$1/ h/$2/ o/Windows/
match pop3 m|^\+OK ([-\w_.]+) POP3 WorkgroupMail ([\d.]+) .*\r\n| p/WorkgroupMail pop3d/ v/$2/ h/$1/ o/Windows/
match pop3 m|^\+OK POP3 server ready \(LSMTP v([\w.]+)\) <[\w.]+@([-\w_.]+)>\r\n| p/LSMTP pop3d/ v/$1/ h/$2/
match pop3 m|^\+OK ([-\w_.]+) Mirapoint POP3 ([\d.]+) server ready\r\n| p/Mirapoint RazorGate pop3d/ v/$2/ h/$1/
match pop3 m|^\+OK K9 - ([\d.]+) - http://keir\.net ready <[\w.]+>\r\n| p/K9 pop3d from keir.net/ v/$1/ o/Windows/
match pop3 m|^\+OK MERCUR POP3-Server \(v([\d.]+) \w+\) for Windows NT ready <[\d.]+@([-\w_.]+)>\r\n| p/MERCUR pop3d/ v/$1/ i/Windows NT/ o/Windows/
match pop3 m|^\+OK POP3 server ready QuickMail Pro Server for MacOS ([\d.]+) <[\w.]+@([-\w_.]+)>\r\n| p/QuickMail Pro pop3d/ v/$1/ h/$2/ o/Mac OS/
match pop3 m|^\+OK ready\r\n| p/602LAN Suite pop3/ o/Windows/
match pop3 m|^\+OK DvISE Mail Access Server Server ready \(Tobit Software, Germany\)\r\n| p/DvISE pop3d/
match pop3 m|^\+OK POP3 ([-\w_.]+) \(Version ([-\w.]+)\) http://surgemail\.com\r\n| p/SurgeMail pop3d/ v/$2/ h/$1/
match pop3 m|^\+OK ([-\w_.]+) running Eudora Internet Mail Server X ([\d.]+) <| p/Eudora Internet Mail Server X pop3d/ v/$2/ h/$1/ o/Mac OS X/
match pop3 m|^\+OK <[\d.]+@([-\w_.]+)> \[XMail ([\d.]+) POP3 Server\] service ready; | p/XMail pop3d/ v/$2/ h/$1/
match pop3 m|^\+OK <[\d.]+@([-\w_.]+)> \[XMail ([\d.]+) \(Linux/Ix86\) POP3 Server\] service ready; | p/XMail pop3d/ v/$2/ h/$1/ o/Linux/
match pop3 m|^\+OK Samsung Contact POP3 interface ready on: ([-\w_.]+)\r\n| p/Samsung Contact pop3d/ h/$1/
match pop3 m|^\+OK ([-\w_.]+) POP3 service \(Sun Java\(tm\) System Messaging Server ([-\d.]+) \(built .*\)| p/Sun Java System Messaging Server pop3d/ v/$2/ h/$1/
match pop3 m|^\+OK Messaging Multiplexor \(Sun Java\(tm\) System Messaging Server (\d[-\w_.]+) \(built .*\)\)\r\n| p/Sun Java System Messaging Multiplexor pop3d/ v/$1/
match pop3 m|^\+OK POP3 Greetings from minipop ([\d.]+) <[\d.]+@([-\w_.]+)>\r\n| p/minipop pop3d/ v/$1/ h/$2/
match pop3 m|^\+OK Hermes ([\w. ]+) POP3 Ready\. <[\d.]+@([-\w_.]+)>\r\n| p/Hermes pop3d/ v/$1/ h/$2/ o/Windows/
match pop3 m|^\+OK ModusMail POP3 Server ([\d.]+) Ready <[\d.]+@([-\w_.]+)>\r\n| p/ModusMail pop3d/ v/$1/ h/$2/ o/Windows/
match pop3 m|^\+OK ([-\w_.]+) POP3 server \(DeskNow POP3 Server ([\d.]+)\) ready \r\n| p/DeskNow pop3d/ v/$2/ h/$1/
match pop3 m|^\+OK POP3 SINA \(([-\d.]+)\) Server Ready\r\n| p/SINA pop3d/ v/$1/
match pop3 m|^\+OK ([-\w_.]+) SpearMail POP3 server ready\r\n| p/Spearmail pop3d/ h/$1/ o/Windows/
match pop3 m|^\+OK SCO POP3 server \(version ([-\w.]+)\) at ([-\w_.]+) starting\.\r\n| p/SCO pop3d/ v/$1/ h/$2/ o/SCO UNIX/
match pop3 m|^\+OK QPOP modified by SCO \(version ([-\w.]+)\) at ([-\w_.]+) starting\.  \r\n| p/SCO-modified QPOP pop3d/ v/$1/ h/$2/ o/SCO UNIX/
match pop3 m|^\+OK POP3 on WebEasyMail \[([\d.]+)\] ready\.  http://www\.51webmail\.com\r\n| p/WebEasyMail pop3d/ v/$1/ o/Windows/
match pop3 m|^\+OK \(POP3\) hMailServer ([-\w.]+)\r\n| p/hMailServer pop3d/ v/$1/ o/Windows/
match pop3 m|^\+OK Hi\r\n| p/Zoe Java pop3d/
match pop3 m|^\+OK Pop server at ([-\w_.]+) starting\.\r\n| p/BorderWare firewall pop3d/ h/$1/ d/firewall/
match pop3 m|^\+OK localhost Winmail Mail Server POP3 ready\r\n| p/Winmail pop3d/ o/Windows/
match pop3 m|^\+OK Welcome to ([-\w_.]+), with Ability Mail Server ([\d.]+) by Code-Crafters\.\r\n| p/Code-Crafters pop3d/ v/$2/ h/$1/ o/Windows/
match pop3 m|^\+OK DAWKCo POP3 Server v([-\w_.]+) ready <| p/DAWKCo pop3d/ v/$1/ o/Windows/
match pop3 m|^\+OK Welcome to ([-\w_.]+), powered by Ocean Mail Server ([\d.]+) <[\d.]+@[-\w_.]+>\r\n| p/Ocean Mail Server pop3d/ v/$2/ h/$1/ o/Windows/
match pop3 m|^\+OK <[\w.]+@([-\w_.]+)> ready for action \(Mailtraq ([\d.]+)/POP3\)\r\n| p/Mailtraq pop3d/ v/$2/ h/$1/ o/Windows/
match pop3 m|^\+OK ([-\w_.]+) Solstice \(tm\) Internet Mail Server \(tm\) POP3 ([\d.]+)| p/Sun Solstice Internet Mail Server pop3d/ v/$2/ h/$1/ o/Unix/
match pop3 m|^\+OK Welcome to RaidenMAILD POP3 service v([\d.]+),| p/RaidenMAILD pop3d/ v/$1/ o/Windows/
match pop3 m|^\+OK POP3 FTGate4 server ready| p/Floosietek FTGate4 pop3d/ o/Windows/
match pop3 m|^\+OK DBOX POP3 Server ([\d.]+) ready\r\n| p/DBOX TCL pop3d/ v/$1/
match pop3 m|^\+OK POP3 on WinWebMail \[([\d.]+)\] ready\.  http://www\.winwebmail\.com\r\n| p/WinWebMail pop3d/ v/$1/ o/Windows/
match pop3 m|^\+OK ([-\w_.]+) POP3 Server Version ([\d.]+) Copyright \d{4} International Messaging Associates\r\n| p/IMA pop3d/ v/$2/ h/$1/
match pop3 m|^\+OK MERCUR POP3-Server \(v([-\w_.]+) \w+\) for Windows ready <[\d.]+@([-\w_.]+)>\r\n| p/Atrium Software's Mercur pop3d/ v/$1/ h/$2/ o/Windows/
match pop3 m|^\+OK 4D Mail ([-\w_.]+) ready <| p/WebSTAR 4D pop3d/ v/$1/ o/Mac OS X/
match pop3 m|^\+OK ([-\w_.]+) POP3 ([-\w_.()]+) w/IMAP client at| p/SCO pop3d/ o/SCO UNIX/
match pop3 m|^\+OK Server Ready\r\n| p/Cisco VPN 3000 Concentrator pop3d/ d/security-misc/
match pop3 m|^\+OK Citadel POP3 server <\d+@([-\w_.]+)>\r\n| p/Citadel pop3d/ h/$1/
match pop3 m|^\+OK <-?[\d.]+@([-\w_.]+)>, POP3 server ready\.\r\n| p/Mercury Mail Transport System pop3d/ h/$1/
match pop3 m|^\+OK POP3 server ready <[-0-9a-f]+@([-\w_.]+)>\r\n| p/SmarterMail pop3d/ o/Windows/ h/$1/
match pop3 m|^\+OK mdpop3 ([\w.]+ \([\w ]+\)) ready\r\n| p/mdpop3/ v/$1/
match pop3 m|^\+OK ([-\w_.]+)\s+IdeaPop3Server ([^\s]+) ready\.\r\n| p/IdeaPop3Server pop3d/ v/$2/ h/$1/

# These are fairly general
match pop3 m|^\+OK POP3 Server ready\r\n$| p/zpop3d/
match pop3 m|^\+OK POP3 server ready\r\n$| p/qpoppper pop3d/
match pop3 m|^\+OK POP3 server ([-\w_.]+) ready <[\d.]+@[-\w_.]+>\r\n| p/BVRP Software SLMAIL pop3d/ h/$1/
match pop3 m|^\+OK ([-\w_.]+) POP3 Server \(Version ([\w.]+)\) ready at <.*>\r\n| p/BSD-based in.pop3d/ v/$2/ h/$1/
match pop3 m|^\+OK popd-([\d.]+) ready \r\n| p/FreeBSD popd/ v/$1/
match pop3 m|^\+OK POP3 server at ([-\w_.]+) ready <[\d.]+@| p/FirstClass pop3d/ h/$1/
match pop3 m|^\+OK POP3 Server OK <[\d.]+@([-\w_.]+)>\r\n| p/Communigate Pro pop3d/ h/$1/
match pop3 m|^-ERR Permission denied - closing connection\.\r\n$| p/Classic Hamster pop3d/ i/Permission denied/ o/Windows/
match pop3 m|^\+OK ([-\w_.]+) <[\d.]+@[-\w_.]+>\r\n| p/IA MailServer pop3d/ h/$1/ o/Windows/
match pop3 m|^\+OK <[\d.]+@([-\w_.]+)>\r\n| p/qmail pop3d/ h/$1/
match pop3 m|^\+OK POP3 server ready <[\d.]+@([-\w_.]+)>\r\n| p/MailMax pop3d/ h/$1/ o/Windows/
match pop3 m|^\+OK ready  <[\d.]+@([-\w_.]+)>\r\n| p/qpopper/ h/$1/
match pop3 m|^\+OK Scalix POP3 interface ready on: ([-\w_.]+)\r\n| p/Scalix pop3d/ h/$1/
match pop3 m|^\+OK ([-\w_.]+) .* GoMail V([\d.]+) POP3| p/GoMail mass mailing plugin pop3d/ v/$2/ h/$1/ o/Windows/
match pop3 m|^\+OK POP3 Welcome to ([-\w_.]+) using the Internet Anywhere Mail Server Version: ([\d.]+)\. Build: (\d+) by True North Software, Inc\.| p/True North Internet Anywhere pop3d/ v/$2 build $3/ h/$1/ o/Windows/
match pop3 m|^\+OK Authorized Users Only! \(([-\w_.]+)\)\r\n| p/Microsoft Exchange pop3d/ h/$1/ o/Windows/
match pop3 m|^\+OK Welcome to mpopd V([\d.]+)\.\.\.\. :\)\r\n| p/mpopd perl pop3d/ v/$1/
match pop3 m|^\+OK POP3 thats cool man\r\n| p/Mozilla Thunderbird webmail plugin pop3d/
match pop3 m|^\+OK [-\w_.]+ Welcome to the mail server\.\r\n| p/Ipswitch iMail pop3d/ o/Windows/
match pop3 m|^\+OK CMailServer ([\d.]+) POP3 Service Ready\r\n| p/CMailServer pop3d/ v/$1/ o/Windows/
match pop3 m|^\+OK ([-\w_.]+) running EIMS X ([\w.]+) <| p/Eudora Internet Mail Server X pop3d/ v/$2/ h/$1/ o/Mac OS X/
match pop3 m|^\+OK ([-\w_.]+) DynFX POP3 Server ([-\w_.]+) <| p/DynFX pop3d/ v/$2/ h/$1/ o/Windows/
match pop3 m|^\+OK POP3 on WinWebMail \[([-\w_.]+)\] ready\.  http://www\.winwebmail\.net\r\n| p/WinWebMail pop3d/ v/$1/ o/Windows/
match pop3 m|^\+OK POP3 server \(Neon Mail Server System Advance ([-\w_.]+), [^)]*\) ready ([-\w_.]+)\. <| p/Neon Mail Server pop3d/ v/$1/ h/$2/
match pop3 m|^\+OK WorldMail POP3 Server ([-\w_.]+) Ready <[\d.]+@([-\w_.]+)>\r\n| p/Eudora Worldmail pop3d/ v/$1/ h/$2/ o/Windows/
match pop3 m|^\+OK Welcome to the Atmail POP3 server - Login with user@domain\.\r\n| p/Atmail pop3d/
match pop3 m|^\+OK Atmail IMAP/POP3 server ready\r\n| p/Atmail pop3d/
match pop3 m|^\+OK Dovecot DA ready\. <[\w._=-]+@([\w._-]+)>\r\n| p/Dovecot DirectAdmin pop3d/ h/$1/
match pop3 m|^\+OK Dovecot DA ready\.\r\n| p/Dovecot DirectAdmin pop3d/
match pop3 m|^Unable to open trace file \"/var/spool/popper/| p/popper pop3d/ i/Misconfigured/
match pop3 m|^\+OK SocketMail v ([-\w_.]+) SocketMail POP3 Server Ready\r\n| p/SocketMail pop3d/ v/$1/
match pop3 m|^\+OK ([-\w_.]+) Zimbra POP3 server ready\r\n| p/Zimbra pop3d/ h/$1/
match pop3 m|^\+OK TMSOFT POP3 Server v([\w._-]+) ready <\w+>\r\n| p/TMSOFT pop3d/ o/Windows/ v/$1/
match pop3 m|^\+OK POP3D\(\*\) Server PMDFV([\w._-]+) at .* <\w+@([\w._-]+)>\r\n| p/PMDF pop3d/ o/OpenVMS/ v/$1/ h/$2/
match pop3 m|^\+OK POP3D\(\*\) Server PMDFV([\w._-]+) at .* \(APOP disabled\)\r\n| p/PMDF pop3d/ o/OpenVMS/ v/$1/
match pop3 m|^\+OK Dovecot POP3 at ([\w._-]+) ready\.\r\n| p/Dovecot pop3d/ h/$1/
# Debian lenny 5.0 Dovecot 1.0.rc15
match pop3 m|^\+OK Pop3 ready\.\r\n| p/Dovecot pop3d/
# embyte
match pop3 m|^\+OK E-POST POP3 Server \(([^\)]+)| p/E-Post POP3 Server/ v/$1/
match pop3 m|^\+OK ([\w._-]+) Cyrus POP3 v([\w._-]+)-OS X Server ([\w._-]+):\t9L1 server ready <[\d.]+@[\w._-]+>\r\n$| p/Cyrus pop3d/ v/$2/ h/$1/ o/Mac OS X/ i/OS X Server $3/
match pop3 m|^\+OK Kerio Connect ([\w._ -]+) POP3 server ready <[\d.]+@([\w._-]+)>\r\n$| p/Kerio Connect pop3d/ v/$1/ h/$2/
match pop3 m|^\+OK Welcome NewsGator Online Services POP3 Server version ([\w._-]+)\r\n$| p/NewsGator Enterprise Server pop3d/ v/$1/
match pop3 m|^-ERR \[SYS/PERM\] Fatal error: tls_init\(\) failed\r\n| p/Cyrus pop3d/
match pop3 m|^\+OK Quick 'n Easy Mail Server ready\r\n| p/Quick 'n Easy pop3d/ o/Windows/

match pop3-proxy m|^\+OK POP3 AnalogX Proxy (\d[-.\w]+) \(Release\) ready\.\n$| p/AnalogX POP3 proxy/ v/$1/
match pop3-proxy m/^\+OK CCProxy (\S+) POP3 Service Ready\r\n/ p/CCProxy pop3d/ v/$1/
match pop3-proxy m/^Proxy\+ POP3 server\. Insecure access - terminating\.\r\n/ p/Proxy+ pop3d/ o/Windows/
match pop3-proxy m|^\+OK TrendMicro IMSS (\d[-.\w ]+) POP3 Proxy at ([-.\w]+)\r\n| p/Trend Micro IMSS virus scanning POP3 proxy/ h/$1/ v/$2/
match pop3-proxy m|^\+OK Proxy-POP server \(DeleGate/([\d.]+) by ysato AT delegate DOT org\) at ([-\w_.]+) starting\.\r\n| p/DeleGate pop3 proxy/ v/$1/ h/$2/
match pop3-proxy m|^\+OK Jana-Server POP3 ready <[\w.]+@([-\w_.]+)>\r\n| p/JanaServer pop3 proxy/ h/$1/ o/Windows/
match pop3-proxy m|^\+OK POP3 Y(ahoo)?POPs! proxy ready\r\n| p/YahooPOPs! pop3 proxy/
match pop3-proxy m|^\+OK POP3 \(Spampal\) server ready \(USER command must include mailserver name\)\r\n| p/Spampal pop3 proxy/ o/Windows/
match pop3-proxy m|^\+OK Mirapoint POP3PROXY ([-\w.]+) server ready\r\n| p/Mirapoint pop3 proxy/ v/$1/
match pop3-proxy m|^\+OK AVG POP3 Proxy Server Beta - ([\d/.]+) \[[\d.]+\]\r\n| p/AVG pop3 proxy/ v/$1 Beta/ o/Windows/
match pop3-proxy m|^\+OK AVG POP3 Proxy Server ([\d/.]+) \[[\w/.]+\]\r\n| p/AVG pop3 proxy/ v/$1/ o/Windows/
match pop3-proxy m|^\+OK AVG POP3 Proxy Server <[\w.]+@[-\w_.]+> ([\d/.]+) \[[\d/.]+\]\r\n| p/AVG pop3 proxy/ v/$1/ o/Windows/
match pop3-proxy m|^-ERR AVG POP3 Proxy Server: Cannot connect to the mail server!\r\n| p/AVG pop3 proxy/ i/broken/ o/Windows/
match pop3-proxy m|^\+OK FreePOPs/([\d.]+) pop3 server ready\r\n| p/FreePOPs pop3 proxy/ v/$1/
match pop3-proxy m|^\+OK POP3 Spam Inspector Spam Filter Gateway Version ([\d.]+) Ready\.\r\n| p/Spam Inspector pop3 proxy/ v/$1/ o/Windows/
match pop3-proxy m|^\+OK MailMarshal\(([\d.]+)\) POP3 server ready <[\d.]+@([-\w_.]+)>\r\n| p/MailMarshal pop3d/ v/$1/ h/$2/
match pop3-proxy m|^\+OK HTML2POP3 server ready \(([\d.]+)\)\r\n| p/HTML2POP3 pop3 proxy/ v/$1/
match pop3-proxy m|^\+OK ([-\w_.]+) POP3 proxy ready\r\n| p/pop3gwd pop3 proxy/ h/$1/
match pop3-proxy m|^\+OK AVG POP3 Proxy Server <[\d.]+@([-\w_.]+)> ([\d.]+)/[\d.]+ \[[\d/.]+\]\r\n| p/GriSoft anti-virus pop3 proxy/ v/$2/ h/$1/ o/Windows/
match pop3-proxy m|^\+OK InterScan VirusWall POP3 Proxy\r\n| p/InterScan VirusWall pop3 proxy/ o/Windows/
match pop3-proxy m|^\+OK WinProxy POP3 Proxy Ready\r\n| p/WinProxy pop3 proxy/ o/Windows/
match pop3-proxy m|^-ERR 403 The requested host is forbidden by WinProxy\.  See your network administrator\.\n| p/WinProxy pop3 proxy/ i/IP forbidden/ o/Windows/
match pop3-proxy m|^\+OK MrPostman webmail proxy ready\r\n| p/MrPostman webmail pop3 proxy/
match pop3-proxy m|^\+OK (.*) \(PGP Universal service is proxying this connection\)\r\n| p/PGP Universal pop3 proxy/ i/Proxied greeting: $1/
match pop3-proxy m|^\+OK F-Secure/fsigk_pop/\d+/[-\w_.]+ starting\.\r\n| p/F-Secure Internet Gateway pop3 proxy/
match pop3-proxy m|^\+OK hello from popgate\(([\d.]+)\)\r\n| p/POPgate pop3 proxy/ v/$1/
match pop3-proxy m|^\+OK \[ISafe POP3 Proxy\] \r\n| p/ISafe pop3 proxy/
match pop3-proxy m|^\+OK <[\d.]+@([-\w_.]+)> \[ISafe POP3 Proxy\] \r\n| p/ISafe pop3 proxy/ h/$1/
match pop3-proxy m|^\+OK UserGate: forward ready\r\n-ERR UserGate: Mistake of the protocol\r\n| p/UserGate pop3 proxy/ o/Windows/
match pop3-proxy m|^\+OK kingate pop3 proxy\r\n| p/kingate pop3-proxy/
match pop3-proxy m|^\+OK POP3 Proxy Server Ready\r\n| p/IronMail pop3-proxy/
match pop3-proxy m|^\+OK avast! POP3 proxy ready\.\r\n| p/Avast! anti-virus pop3 proxy/ o/Windows/
match pop3-proxy m|^\+OK O3SIS UMA Proxy POP3 Server ([\w._-]+)\r\n| p/O3SIS UMA pop3 proxy/
match pop3-proxy m|^\+OK Zarafa POP3 gateway ready\r\n| p/Zarafa pop3 proxy/ o/Unix/

# http://echelon.pl/pubs/poppassd.html
# you give it username, present password and new password, and
# it changes the password of the user.
# poppassd 1.8.1
match pop3pw m|^200 ([-._\w]+ )?poppassd v?([-._\w]+) | p/poppassd/ v|$2|
match pop3pw m|^200 poppassd hello, who are you\?\r\n| p/poppassd/
match pop3pw m|^200 hello there, who are you\?\r\n| p/poppassd/
match pop3pw m|^200 hello there, please tell me who you are\r\n| p/poppassd/
match pop3pw m|^200 poppassd v([\w.]+) for Digital Unix with C2 security Hello, who are you\?\r\n| p/poppassd/ i/Digital Unix with C2 security/ v/$1/ o/Digital UNIX/
match pop3pw m|^200 courierpassd v(\d[-.\w]+) hello, who are you\?\r\n| p/Courierpassd pop3 password change daemon/
match pop3pw m|^200 ([-.+\w]+) MercuryW PopPass server ready\.\r\n| p|Mercury/32 poppass service| o|Windows| h|$1|
match pop3pw m|^200 X1 NT-PWD Server ([-.+\w]+) \(IMail (\d[-.\w]+)\)\r\n| p/Ipswitch IMail pop3 password change daemon/ h/$1/ v/$2/ o/Windows/
match pop3pw m|^200 CommuniGate Pro PWD Server (\d[-.\w]+) ready <| p/CommuniGate Pro pop3 password change daemon/ v/$1/
match pop3pw m|^\+OK ApplePasswordServer (\d[-.\w]+) password server at | p/ApplePasswordServer pop3 password change daemon/ v/$1/
match pop3pw m|^200 Stalker Internet Password Server ready\. V\.([\w.]+)\r\n| p/Stalker Mail Server password change daemon/ v/$1/ o/Mac OS/
match pop3pw m|^550 Login failed - already \d+/\d+ users connected sorry \(use G_CON_PERIP_EXCEPT to bypass\) \(IP=[\d.]+\)\r\n| p/Qualcomm poppassd/ i/Maximum users connected/
match pop3pw m|^200 hello and welcome to SchoolsNET SINA poppassd \[([-\d.]+)\]\r\n| p/SINA pop3pw/ v/$1/
match pop3pw m|^200 Post\.Office v([\d.]+) password server ready\r\n| p/Post.Office pop3pw/ v/$1/
match pop3pw m|^200 MERCUR Password service for Windows NT ready\r\n| p/Atrium Software's Mercur pop3pw/ o/Windows/

softmatch pop3 m|^\+OK [-\[\]\(\)!,/+:<>@.\w ]+\r\n$|

match pptp m|^\0\x10\0\x01\x1a\+<M\0\x05\0\0\0\0\0\x01$| p/Point to Point Tunneling Protocol/

match pmud m|^pmud (\d[-.\w]+) \d+\n| p|pmud| i|http://sf.net/projects/apmud|
match printer m|^lpd \[@([-.\w]+)\]: Print-services are not available to your host \([-.\w]+\)\.\n| p/BSD lpd/ i/Unauthorized host/ h/$1/
# BSD lpr/lpd line printer spooling system (lpr v1:2000.05.07) on Linux 2.6.0-test5
match printer m|^([-.\w]+): lpd: Your host does not have line printer access\n| p|BSD/Linux lpd| h|$1| i|hostname denied|
match printer m|^lpd \[@([-\w_.]+)\]: connected from invalid port \(\d+\)\n| p|BSD/Linux lpd| h|$1| i|source port denied|
# Linux 2.4.18 lpr 2000.05.07-4.2
match printer m|^lpd: Host name for your address \(\d+\.\d+\.\d+\.\d+\) unknown\n$| p/Linux lpd/ i/client IP must resolve/ o/Linux/
match printer m|^([/\w]+/)?lpd: (.*)\n| p/lpd/ i/error: $2/
# Mac OS X?
match printer m|^([-\w_.]+): lpd: hostname for your address \([\d.]+\) unknown\n| p/lpd/ h/$1/
match printer m|^[-\w_.]+: lpd: address for your hostname \([\d.]+\) not matched\n| p/lpd/
# Redhat Linux 7.3 LPRng-3.8.9
match printer m|^\x01no connect permissions\n$| p/LPRng/ i/Not authorized/
match printer m|^([-\w_.]+): lpsched: Malformed from address\n| p/lpsched/ h/$1/
match printer m|^([-\w_.]+): lpsched: Your host does not have line printer access\n| p/lpsched/ h/$1/ i/host denied/
match printer m|^([-\w_.]+): lpsched: Host name for your address \([\d.]+\) unknown\n| p/lpsched/ h/$1/ i/Unauthorized/
match printer m|^([-\w_.]+): /usr/lib/lpd: Malformed from address\n| p/lpd/ h/$1/
match printer m|^Printer Status ---> (.*)                    \nno entries\n| p/QMC DeskLaser printer/ i/Status $1/ d/printer/
match printer m|^\d+-202 your host does not have line printer access\.| p/AIX lpd/ i/Unauthorized/ o/AIX/
match printer m|^\d+-201 ill-formed FROM address\.$| p/AIX lpd/ o/AIX/
match printer-admin m|^LXK: $| p/Lexmark printer admin/ d/printer/

match pwdgen m|^\w+ \(\w+(-\w+)+\)\r\n$| p/pwdgen/

match pycharm m|^\0\.[\w._/-]+/Library/Preferences/PyCharm([\w._-]+)\0\)[\w._/-]+/Library/Caches/PyCharm[\w._-]+$| p/PyCharm/ v/$1/ o/Mac OS X/

match qaweb m|^QAS2$| p/QuickAddress Pro for the Web/

match qconn m|^QCONN\r\n\xff\xfd\"$| p/qconn remote IDE support/ o/QNX/

match qsp-proxy m|^\x01\x01\0\x08\x1c\xee\x01\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0$| p/Symantec ManHunt/

# Windows QOTD service only has 12 quotes.  Found on Windows XP in
# %systemroot%\system32\drivers\etc\quotes
match qotd m/^"(My spelling is Wobbly\.|Man can climb to the highest summits,|In Heaven an angel is nobody in particular\.|Assassination is the extreme form of censorship\.|When a stupid man is doing|We have no more right to consume happiness without|We want a few mad people now.|The secret of being miserable is to have leisure to|Here's the rule for bargains:|Oh the nerves, the nerves; the mysteries of this machine called man|A wonderful fact to reflect upon,|It was as true as taxes is\.)/ p/Windows qotd/ o/Windows/
match qotd m/^"(Mi ortograf\xeda tiembla\. Es bueno revisarla,|un hombre puede escalar a las m\xe1s altas cumbre|Algo maravilloso a poner de manifiesto:|Cuando un necio hace algo de lo que se aveg\xfcenza,|En el cielo, un \xe1ngel no es nadie en concreto|Traigamos unos cuantos locos ahora\.|Era tan verdad como los impuestos\. Y no|Hay libros cortos que, para entenderlos como se merecen,|La prosperidad hace amistades, y la adversidad las|El uso principal de un PC es confirmar la ley de|Quedarse en lo conocido por miedo a lo desconocido,|Cuando las leyes son injustas, no obligan en el fuero|Magia equivale a cualquier avance en la ciencia\.|Vale mejor consumir vanidades de la vida,)/ p/Windows qotd/ i/Spanish/ o/Windows/
# Some Italian qotds start with a space instead of a "
match qotd m/^.(Voce dal sen fuggita|Semel in anno licet insanire|Cosa bella e mortal passa e non dura|Quando uno stupido compie qualcosa di cui si vergogna,|Se tu pagare come dici tu,|Fatti non foste a viver come bruti,|Sperare senza far niente e` come)/ p/Windows qotd/ i/Italian/ o/Windows/
match qotd m/^"(Prazos longos sao f\xa0ceis de subscrever\.|Deus, para a felicidade do homem, inventou a f\x82 e o amor\.|Ao vencido, \xa2dio ou compaixao, ao vencedor, as batatas\.|Quem nao sabe que ao p\x82 de cada bandeira p\xa3blica,|Nao te irrites se te pagarem mal um benef\xa1cio; antes cair|A vida, como a antiga Tebas, tem cem portas\.)/ p/Windows qotd/ i/Portugese/ o/Windows/
# The German version doesn't start with "
match qotd m/^(Wer wirklich Autorit\xe4t hat, wird sich nicht scheuen,|Moral ist immer die Zuflucht der Leute,|Beharrlichkeit wird zuweilen mit Eigensinn|Wer den Tag mit Lachen beginnt, hat ihn|Wenn uns keine Ausweg mehr bleibt,|Gesichter sind die Leseb\xfccher des Lebens|Grosse Ereignisse werfen mitunter ihre Schatten|Dichtung ist verpflichtet, sich nach den|Ohne Freihet geht das Leben|Liebe ist wie ein Verkehrsunfall\. Man wird angefahren)/ p/Windows qotd/ i/German/ o/Windows/
match qotd m/^"(Clovek ma tri cesty, jak moudre jednat\. Nejprve premyslenim|Co je vubec hodno toho, aby to bylo vykonano,|Fantazie je dulezitejsi nez vedeni\.|Potize narustaji, cim vice se clovek blizi|Kdo nezna pristav, do ktereho se chce plavit,|Lidske mysleni ztraci smysl,|Nikdo nevi, co muze vykonat,|Nic neprekvapi lidi vice nez zdravy rozum|Zadny cil neni tak vysoky,)/ p/Windows qotd/ o/Windows/ i/Czech/
match qotd m/^"(L'art de persuader consiste autant|Le peu que je sais, c'est \x85 mon ignorance|Certaines \x83mes vont \x85 l'absolu comme l'eau|Le m\x82rite a sa pudeur comme la chastet|Rien de plus futile, de plus faux, de plus|\xb7 vaincre sans p\x82ril, on triomphe|Le comble de l'orgueil, c'est de se)/ p/Windows qotd/ o/Windows/ i/French/

match quagga m|^\r\nHello, this is [Qq]uagga \(version (\d[-.\w]+)\)\.\r\nCopyright 1996-200| p/Quagga routing software/ v/$1/ i/Derivative of GNU Zebra/

match qtopia-transfer m|^220 Qtopia transfer service ready!\n| p/Qtopia transfer daemon/ d/PDA/

match radmind m|^200-?RAP 1 ([-\w_.]+) ([-\w_.]+) radmind access protocol\r\n| p/radmind/ v/$2/ h/$1/
match rationalsoft m|^\0\0\0\x10ip_infilter=true$| p/Rational Soft Hidden Administrator Server/ o/Windows/ i/ha_server.exe/
match razor2 m|^sn=\w&srl=\d+&ep4=[-\w]+&a=\w&a=\w+\r\n$| p/Vipul's Razor2 anti-spam service/
match renderer m|^250 backburner ([\d.]+) Ready\.\r\nbackburner>| p/Discreet Backburner network renderer/ v/$1/
match rgpsp m|^last pid: \d+  <linux><special> rgpsp poller ! ! !\n| p/Remote GPS Poller/ o/Linux/
# Remote Console via RCONJ - RCONJ is a java utility that allows one
# to remote console into a Novell server. It uses 2034 (unsecure) or
# 2036 (secure) by default but can be changed.
# The unknown token looks like it might be signifigant but I can't
# find any protocol descriptions. -Doug
match rconj m|^\0.\0\x01\0\0\0\0.*\x0b\0\0\0\0([-\w_]+)\x00437|s p/Novell rconj/ i/Unknown token: $1/ o/Unix/
match realplayfavs m|^_realplayfavs_::([\w\s]+)::connected\0$| p/RealPlayer Shared Favorites/ i/name: $1/
match realplayfavs m|^_realplayfavs_::| p/RealPlayer Shared Favorites/
match resvc m|^\{\w+\} NODEINFO \(\d+\) \{\d+\}Version: (\d[-.\w ]+) Microsoft Routing Server ready\r\n  | p/Microsoft Exchange routing server/ v/$1/ o/Windows/
match remoteanything m|^(\d+\.\d+\.\d+) G\0\0\0\xb6\0.\t| p/TWD RemoteAnything/ v/$1/ o/Windows/
match rifa-dvr m|^RIFA\0\0\0\0| p/Rifatron DVR/ d/webcam/

match righteous-backup m|^\xe1\xe7\xef\xf0\0\0\x00.\(Righteous Backup Linux Agent\) ([^\xe1]+)\xe1\xe7\xe6\x07\0\x01\0 $| p/R1Soft Righteous Backup Linux Agent/ v/$1/ o/Linux/
match righteous-backup m|^\xe1\xe7\xe6\x07\0\x01\0 $| p/R1Soft Righteous Backup/

match roku m|^roku: ready\r\n| p/Roku SoundBridge/ d/media device/

match rowmote m|^KEY UNAUTHORIZED\r\nKEY UNAUTHORIZED\r\n| p/Rowmote remote media controller/ o/Mac OS X/

# RedHat 7.3 - rsync server version 2.5.4  protocol version 26
# Redhat Linux 7.1
# rsync 2.5.5-0.1 with custom banner on Debian Woody
match rsync m|^@RSYNCD: (\d+)| i/protocol version $1/

match rpacd m|^\0\x01\0\n\0\0\0=The host is not in the allowed host list\. Connection refused\.$| p/WinPcap Remote Capture Packet daemon/ o/Windows/
match rpd m|^\+host=cashew version=([\d.]+) uptime=[\d+:]+ audio-bits=\d+ audio-byte-order=\w+-endian| p/Remote Play Daemon/ v/$1/ o/Linux/

match runes-of-magic m|^\x10\0\0\0\x03| p/Runes of Magic game server/

# Simple Asynchronous File Transfer (SAFT)
match saft m|^220 ([-\w.]+) SAFT server \(sendfiled ([\w.]+) on ([\w]+)\) ready\.\r\n| p/sendfiled/ v/$2/ h/$1/ o/$3/
match scalix-ual m|^\x02\x1c50\x1c\x03\0\0\0\0$| p/Scalix UAL/
match scanager m|^\*\*\* ITSO_DB_FAIL \*\*\* invalid request\r\n| p/Indiana University Scanager DB/
# This sdmsvc was matching HP printers.  May be bogus, so removed.
# match sdmsvc m|^[\xaa\xff]$| p/LANDesk Software Distribution/ i/sdmsvc.exe/ o/Windows/
# http://www.ietf.org/internet-drafts/draft-martin-managesieve-04.txt
match sieve m|^NO Fatal error: Error initializing actions\r\n$| p|Cyrus timsieved| i|included w/cyrus imap|
match sieve m|^\"IMPLEMENTATION\" \"Cyrus timsieved v([\d.]+)-Red Hat [\d.-]+\"\r\n| p|Cyrus timsieved| v/$1/ i|Red Hat; included w/cyrus imap| o/Linux/
match sieve m|^\"IMPLEMENTATION\" \"Cyrus timsieved v([\d.]+)-Debian[- ]([\w._+-]+)\"\r\n| p|Cyrus timsieved| v/$1/ i|Debian| o/Linux/
match sieve m|^\"IMPLEMENTATION\" \"Cyrus timsieved \(Murder\) v([-.\w]+)\"\r\n| p/Cyrus timsieved Murder/ v/$1/
match sieve m|^\"IMPLEMENTATION\" \"Cyrus timsieved v([\w_.]+)-OS X ([^"]+)\"\r\n| p/Cyrus timsieved/ v/$1/ o/Mac OS X $2/
match sieve m|^\"IMPLEMENTATION\" \"Cyrus timsieved v(\d[-.\w]+)\"\r\n| p|Cyrus timsieved| v/$1/ i|included w/cyrus imap|
match sieve m|^\"IMPLEMENTATION\" \"dovecot\"\r\n| p/Dovecot timsieved/
match sieve m|^\"IMPLEMENTATION\" \"DBMail timsieved ([\w._-]+)\"\r\n| p/DBMail timsieved/ v/$1/
match sieve m|^\"IMPLEMENTATION\" \"CITADEL Sieve ([\d.]+)\"\r\n| p/Citadel timsieved/ v/$1/
match sieve m|^/usr/share/pysieved/plugins/dovecot\.py:27: DeprecationWarning: The popen2 module is deprecated\.  Use the subprocess module\.\n  import popen2\n\"IMPLEMENTATION\" \"pysieved ([\w._+-]+)\"\r\n| p/pysieved/ v/$1/
match sieve m|^\"IMPLEMENTATION\" \"pysieved ([\w._-]+)\"\r\n| p/pysieved/ v/$1/
match sieve m|^\"IMPLEMENTATION\" \"Dovecot Pigeonhole\"\r\n\"SIEVE\" \"comparator-i;octet comparator-i;ascii-casemap fileinto reject envelope encoded-character vacation subaddress comparator-i;ascii-numeric relational regex imap4flags copy include variables body enotify environment mailbox date spamtest spamtestplus virustest\"\r\n\"NOTIFY\" \"mailto\"\r\n\"SASL\" \"PLAIN LOGIN DIGEST-MD5 CRAM-MD5\"\r\n\"STARTTLS\"\r\n\"VERSION\" \"([\w._-]+)\"\r\nOK\ \"Dovecot ready\.\"\r\n$| p/Dovegot Pigeonhole sieve/ v/$1/

match sftp m|^\+Shiva SFTP Service\0$| p/Shiva LanRover SFTP service/
match sftp m=^SSH-2\.0-mod_sftp/([\w._-]+)\r\n= p/ProFTPD mod_sftp/ v/$1/

match sgms m|^SGMS Scheduler SGMS (\d+) ([\d.]+) .*\n>| p/Sonicwall Viewpoint SGMSd/ v/$2/ i/SGMS protocol $1/ d/firewall/

match sharefolder m|^t\x03\0\0$| p/Public ShareFolder mailbox synchronization/

# HP-UX B.11.00 A 9000/785
match shell m|^\x01remshd: getservbyname\n$| p/HP-UX Remshd/ o/HP-UX/
match shell m|^\x01remshd: Kerberos Authentication not enabled\.\n| p/HP-UX Remshd/ i/Kerberos disabled/ o/HP-UX/
match shell m|^\x01remshd: Error! Kerberos authentication failed| p/HP-UX Remshd/ i/Kerberos broken/ o/HP-UX/
match shell m|^\* You are not welcome to use rshd from .*\n| p/FreeBSD rshd/ i/Access denied/ o/Unix/

# Backdoor shell!
match shell m|^(ba)?sh-\d\.\d\d\w?# $| p/ROOT SHELL/ o/Unix/ i/**BACKDOOR**/
match shell m|^:: w4ck1ng-shell \(Private Build v([\w._-]+)\) bind shell backdoor :: \n\n| p/w4ck1ng-shell/ i/**BACKDOOR**/

match satstrat m|^VERSION ([\d.]+)\r\nJOIN 0\r\nNICK 0 !SaCkS\r\nJOIN 1\r\n| p/SatStrat/ v/$1/
match securepath m|^GENERAL: \d+ \d+<EoM>\n$| p/HP StorageWorks SecurePath/ o/Windows/
match securepath m|^Unauthorized client; connection refused<EoM>\n| p/HP StorageWorks SecurePath/ i/unauthorized/ o/Windows/
match service-monitor m|^\0\0\0\x18\0\0..\0\0..\xff\xff\xff\xff\xff\xff\xff\xff\0\0\0\x02\0\0\0\0\0\0\0.([^\0]+)\0|s p/CA Spectrum/ i/User $1/
match service-monitor m|^550 Bad syntax\. Go away\.\n$| p/CA Spectrum/

match slnp m|^220 SLNP (\w+)@[vV]ersion:[\s]?V?([^@]+)@((user:[^@]+@)?pid:[\d]+)\n$| p/Sisis $1/ v/$2/ i/$3/ o/Unix/

match starutil m|^star-v3 utility server\n\0| p/StarUTIL router config/ v/3/ d/router/

# good SMTP banner regexps can be found here:
# http://www.tty1.net/smtp-survey/measurement_en.html

# Goes at the top because some general match lines (Exim)
# will match the replayed greeting of the proxied server!
match smtp-proxy m|^220 ([-\w_.]+) PGP Universal service ready \(proxied server greeted us with: (.*)\)\r\n| p/PGP Universal smtp proxy/ h/$1/ i/Proxied greeting: $2/

match smtp m|^220 ([-/.+\w]+) MailGate ready for ESMTP on | p/MailGate smtpd/ h/$1/ o/Windows/
match smtp m|^220 ([-/.+\w]+) SMTP ready to roll\r\n| p/Hotmail Popper hotmail to smtp gateway/ h/$1/
match smtp m|^220 ([-/.+\w]+) AvMailGate-(\d[-.\w]+)\r\n| p/AvMailGate smtp anti-virus mail gateway/ h/$1/ v/$2/
match smtp m|^220 ([-/.+\w]+) Internet Rex ESMTP daemon at your service\.\r\n| p/Internet Rex smtpd/ h/$1/
match smtp m|^220 ([-.+\w]+) ESMTP NetIQ MailMarshal \(v(\d[-.\w]+)\) Ready\r\n| p/MailMarshal/ h/$1/ v/$2/
match smtp m|^220 ([-.+\w]+) ESMTP NetIQ MailMarshal \d[-.\w]+ Service Pack (\w+) \(v(\d[-.\w]+)\) Ready\r\n| p/MailMarshal/ h/$1/ v/$3 Service Pack $2/
match smtp m|^220 ([-\w_.]+) ESMTP MailMarshal \(v([\d.]+)\) Ready\r\n| p/MailMarshal/ h/$1/ v/$2/
# I think the revision number is different than the official product version number
# Dots in Revision to prevent MY CVS from screwing it up
match smtp m|^220 ([-.+\w]+) Novonyx SMTP ready \$Re..sion: *([\d.]+) *\$\r\n| p|Novonyx Novell NetMail smtpd| h|$1| v|$2|
match smtp m|^554-([-.+\w]+)\.us\r\n554 Access denied\r\n$| p/IronPort appliance mail rejector/ h/$1/
match smtp m|^220 eSafe@([-.+\w]+) Service ready\r\n| p/eSafe mail gateway/ h/$1/
match smtp m|^220[ -](\S+) ESMTP Merak (\d[^;]+);|i p/Merak Mail Server smtpd/ h/$1/ v/$2/ o/Windows/
match smtp m|^220[ -]\]-:\^:-\[ ESMTP \]-:\^:-\[; .*\r\n| p/Merak Mail Server smtpd/ o/Windows/
match smtp m|^220.*?MERCUR SMTP[\s-]Server \(v([^)]+)\) for ([-.\w ]+) ready at | p/LAN-ACES MERCUR smtp server/ v/$1/ o/$2/
match smtp m|^220 ([-.+\w]+) MasqMail (\d[-.\w]+) ESMTP\r\n| p/MasqMail smtpd/ h/$1/ v/$2/
# Barracuda Networks "Spam Firewall" embedded spam appliances
match smtp m|^220 ([-.\w\d]+) ESMTP \([a-fA-F0-9]{32}\)\r\n| p/Barracuda Networks Spam Firewall smtpd/ h/$1/
match smtp m|^554 Service unavailable; Client host \[[\w._-]+\] blocked using Barracuda Reputation;| p/Barracuda Networks Spam Firewall smtpd/ i/client blocked by Barracuda Reputation/
# Cisco NetWorks ESMTP server IOS (tm) 5300 Software (C5300-IS-M) on Cisco 5300 Access Server
match smtp m|^220 ([-.+\w]+) Cisco NetWorks ESMTP server\r\n| p/Cisco IOS NetWorks smtp server/ h/$1/ d/terminal server/ o/IOS/
match smtp m|^220 ([-.+\w]+) Mercury/32 v(\d[-.\w]+) ESMTP server ready\.\r\n| p|Mercury/32 smtpd| h|$1| v|$2| o|Windows|
# Canon ImageRunner SMTP server (network scanner/copier/printer)
match smtp m|^220 Canon[-.\w]+ ESMTP Ready\r\n| p/Canon printer smtp server/ d/printer/
match smtp m|^220 .*?eSafe E?SMTP Service (\d\S+) ready| p/eSafe mail gateway/ v/$1/
match smtp m|^220 .*?eSafe E?SMTP Service ready| p/eSafe mail gateway/
match smtp m|^520 Connection not authorised from this address\.\r\n| p|Mercury smtpd| i|Connection not authorised|
# Exim 3.36 on Linux 2.4 blocking the given IP
match smtp m|^554 SMTP service not available\r\n$| p/Exim smtpd/ i/Serviced refused (IP block)/
# Jana Server 1.45 on Win98
match smtp m|^220 Jana-Server Simple Mail Transfer Service ready\r\n| p/JanaServer mail server/ o/Windows/
match smtp m|^220 <1\d+\.\d+@([-.\w]+)> \[XMail (\d[-.\w]+) ESMTP Server\] service ready; | p/XMail SMTP server/ h/$1/ v/$2/
match smtp m|^220 <1\d+\.\d+@([-.\w]+)> \[XMail (\d[-.\w]+) \(([-./\w]+)\) ESMTP Server\] service ready; | p/XMail SMTP server/ h/$1/ v/$2/ i/on $3/
match smtp m|^220 ([-\w_.]+) <1\d+\.\d+@[-\w_.]+> \[XMail (\d[-.\w]+) ESMTP Server\] service ready| p/XMail SMTP server/ h/$1/ v/$2/
match smtp m|^421 \[XMail ([\d.]+) \(Linux/Ix86\) ESMTP Server\] - Server does not like Your IP\r\n| p/XMail SMTP server/ v/$1/ i|Linux/x86| o/Linux/
match smtp m|^220 ([-.\w]+) FirstClass ESMTP Mail Server v(\d[-.\w]+) ready\r\n| p/FirstClass SMTP server/ h/$1/ v/$2/
match smtp m|^220 ([-.\w]+) AppleMailServer (\d[-.\w]+) SMTP Server Ready\r\n| p/AppleMailServer/ h/$1/ v/$2/
match smtp m|^220 ([-.\w]+) ESMTP CommuniGate Pro (\d[-.\w]+)\r\n| p/Communigate Pro SMTP/ h/$1/ v/$2/
match smtp m|^220[- ]([-.\w]+) MailSite ESMTP Receiver Version (\d[-.\w]+) Ready\r\n| p/Rockliffe MailSite/ h/$1/ v/$2/
match smtp m|^220 ([-.\w]+) eXtremail V(\d[-.\w]+) release (\d+) ESMTP server ready \.\.\.\r\n| p/eXtremail smtpd/ h/$1/ v/$2.$3/
match smtp m|^220 ([-.\w]+) eXtremail V(\d[-.\w]+) release (\d+) rev(\d+) ESMTP server ready \.\.\.\r\n| p/eXtremail smtpd/ h/$1/ v/$2.$3.$4/
match smtp m|^220 Welcome to ([-.\w]+) - VisNetic MailScan ESMTP Server BUILD (\d[-.\w]+)\r\n| p/VisNetic MailScan ESMTP server/ h/$1/ v/$2/
# HP Service Desk 4.5 SMTP Server
match smtp m|^220 ([-.\w]+) service desk (\d[-.\w]+) SMTP Service Ready for input\.\r\n| p/HP Service Desk SMTP server/ h/$1/ v/$2/
# VPOP3 SMTP server 2.0.0d
match smtp m|^220 ([-.\w]+) VPOP3 SMTP Server Ready\r\n| p/PSCS VPOP3 mail server/ h/$1/
# CommuniGate Pro 4.1.3 on Mac OS X 10.2.6
match smtp m|^220 ([-.\w]+) ESMTP CommuniGate Pro (\d[-.\w]+) is glad to see you!\r\n| p/CommuniGate Pro mail server/ h/$1/ v/$2/
match smtp m|^220[ -]([-.\w]+) ESMTP MDaemon (\d[-.\w]+); | p/Alt-N MDaemon mail server/ h/$1/ v/$2/ o/Windows/
match smtp m/^220 ([-.+\w]+) \(IMail ([^)]+)\) NT-ESMTP Server/ p/IMail NT-ESMTP/ h/$1/ v/$2/ o/Windows/
match smtp m/^220 X1 NT-ESMTP Server ([-.+\w]+) \(IMail ([^)]+)\)\r\n/ p/IMail NT-ESMTP/ h/$1/ v/$2/ o/Windows/
match smtp m|^421  Insufficient System Storage\.\(IMail ([\d.]+)\)\r\n| p/IMail smtpd/ v/$1/ i/Storage full/ o/Windows/
match smtp m/^220-([-.+\w]+) Microsoft SMTP MAIL ready at.*Version: ([-\w.]+)\r\n/ p/Microsoft SMTP/ h/$1/ v/$2/ o/Windows/
match smtp m/^220 \[?([-.+\w]+)\]? Microsoft ESMTP MAIL Service, Version: ([-\w.]+) ready/ p/Microsoft ESMTP/ h/$1/ v/$2/ o/Windows/
match smtp m|^220 ([-\w_.]+) Microsoft ESMTP MAIL Service ready at| p/Microsoft Exchange ESMTP/ h/$1/ o/Windows/
match smtp m|^220 ([\w._-]+) Microsoft ESMTP MAIL Service Version: ([\w._-]+)\r\n| p/Microsoft Exchange 2010 smtpd/ v/$2/ h/$1/
match smtp m/^220 ([-.+\w]+) ESMTP Server \(Microsoft Exchange Internet Mail Service ([-\w.]+)\) ready/ p/Microsoft Exchange/ h/$1/ v/$2/ o/Windows/
match smtp m|^220 ([-\w_.]+) Microsoft Exchange Internet Mail Service ([-\w_.]+) ready\r\n| p/Microsoft Exchange/ h/$1/ v/$2/ o/Windows/
match smtp m|^220 \+OK Microsoft Exchange SMTP server version ([\d.]+)| p/Microsoft Exchange/ v/$1/ o/Windows/
match smtp m|^421 [\d.]+ Service not available, closing transmission channel\r\n| p/Microsoft Exchange smtpd/ o/Windows/ i/disabled/
match smtp m|^220[\s-](\S+) E?SMTP Sendmail (\d[^; ]+)| p/Sendmail/ h/$1/ v/$2/ o/Unix/
match smtp m|^220[\s-](\S+) E?SMTP Sendmail AIX([\d.]+)/(\d[^; ]+)| p/Sendmail/ h/$1/ v/$3/ i/AIX $2/ o/AIX/
match smtp m|^220[\s-](\S+) E?SMTP Sendmail AIX([\d.]+)/UCB (\d[^; ]+);| p/Sendmail/ h/$1/ v/$3/ i/AIX $2/ o/AIX/
match smtp m|^220[\s-](\S+) E?SMTP Sendmail @\(#\)Sendmail version (\d[^; ]+) - Revision ([\d.]+) | p/Sendmail/ h/$1/ v/$2 rev $3/ o/HP-UX/
match smtp m|^220[\s-](\S+) E?SMTP Sendmail @\(#\)Sendmail version (\d[^; ]+) - Revision ([\d.]+):: HP-UX([\d.]+)| p/Sendmail/ h/$1/ v/$2 rev $3/ o/HP-UX $4/
match smtp m|^220[\s-](\S+) Sendmail (SMI-\S+) ready at .*\r\n$| p/Sendmail/ h/$1/ v/$2/ o/Unix/
match smtp m|^220[\s-]([-\w_.]+) Sendmail (\S+) ready at .*\r\n| p/Sendmail/ h/$1/ v/$2/ o/Unix/
match smtp m|^220[\s-]([-\w_.]+) ESMTP Sendmail SGI-(\d[^; ]+)| p/Sendmail/ h/$1/ v/$2/ o/IRIX/
match smtp m|^421 4\.3\.2 Connection rate limit exceeded\.\r\n$| p/Sendmail/
match smtp m/^220[- ]([^\r\n]+) ESMTP Exim (V?\d\S+)/ p/Exim smtpd/ h/$1/ v/$2/
match smtp m/^220[- ].*\r\n220[- ]([^\r\n]+) ESMTP Exim /s p/Exim smtpd/ h/$1/
match smtp m/^220 CheckPoint FireWall-1 secure ESMTP server\r\n$/ p/Checkpoint FireWall-1 smtpd/ d/firewall/
match smtp m/^220 CheckPoint FireWall-1 secure SMTP server\r\n$/ p/Checkpoint FireWall-1 smtpd/ d/firewall/
match smtp m|^220 ([-.+\w]+) running IBM AS/400 SMTP V([\w]+)| p|IBM AS/400 smtpd| h|$1| v|$2|
match smtp m|^220 ([-.+\w]+) ESMTP MailEnable Service, Version: (\d[.\w]+)- ready at | p/MailEnable smptd/ h/$1/ v/$2/ o/Windows/
match smtp m/^220 ([-.+\w]+) ESMTP Mail Enable SMTP Service, Version: (\d[\w.]+)-- ready at/ p/MailEnable smptd/ h/$1/ v/$2/ o/Windows/
# Enterprise version number seems to be preceeded by "0--"; Professional with "0-"
match smtp m|^220 ([-.+\w]+) ESMTP MailEnable Service, Version: \d+--([\d.]+) ready at| p/MailEnable Enterprise smptd/ h/$1/ v/$2/ o/Windows/
# Catch-alls. Hyphens aren't making sense -Doug
match smtp m|^220 ([-.+\w]+) ESMTP MailEnable Service, Version: ([\w._-]+) ready at| p/MailEnable smptd/ h/$1/ v/$2/ o/Windows/
match smtp m|^530 ([-.+\w]+) ESMTP MailEnable Service, Version: ([\w._-]+) denied access at| p/MailEnable smptd/ h/$1/ v/$2/ i/Denied access/ o/Windows/
match smtp m/^220 ([-.+\w]+) ESMTP CPMTA-([-.+\w]+) - NO UCE\r\n/ p/CPMTA/ h/$1/ v/$2/ i/qmail-derived/
match smtp m|^220 ([-.+\w]+) SMTP/smap Ready\.\r\n| p/Smap/ i/from firewall toolkit/ h/$1/
match smtp m|^220 ([-.+\w]+) ESMTP service \(Netscape Messaging Server ([-.+ \w]+) \(built| p/Netscape Messaging Server/ h/$1/ v/$2/
match smtp m|^220-InterScan Version (\S+) .*Ready\r\n220 ([-.+\w]+) NTMail \(v([-.+\w]+)/.* ready| p/Trend Micro InterScan/ h/$2/ v/$1/ i/on NTMail $3/ o/Windows/
match smtp m|^220-InterScan Version (\S+) .*Ready\r\n220 ([-.+\w]+) ESMTP Postfix\r\n| p/Trend Micro InterScan/ h/$2/ v/$1/ i/on Postfix/ o/Unix/
match smtp m|^220-InterScan Version (\S+) .*Ready\r\n220 ([-.+\w]+) Microsoft ESMTP MAIL Service, Version: ([\d.]+) ready at| p/Trend Micro InterScan/ h/$2/ v/$1/ i/on Microsoft ESMTP $3/ o/Windows/
match smtp m|^220-InterScan Version (\S+) .*Ready\r\n| p/Trend Micro InterScan/ v/$1/
match smtp m|^220 ([-.\w]+) InterScan VirusWall NT ESMTP (\d[-.\w]+) \(build (\d+)\) ready at | p/Trend Micro InterScan VirusWall SMTP/ h/$1/ v/$2 build $3/  o/Windows/
match smtp m|^220 ([-.+\w]+) GroupWise Internet Agent (\S+) .*Novell, Inc\..*\r\n| p/Novell GroupWise/ h/$1/ v/$2/
match smtp m|^220 \S+ \S+ ESMTP receiver fssmtpd(\d+) ready| p/fssmtpd/ v/$1/
match smtp m/Failed to open configuration file.*exim/ p/Exim smtpd/ i/broken/
match smtp m/^220 Trend Micro ESMTP ([-.+\w]+) ready\.\r\n$/ p/Trend Micro ESMTP/ v/$1/
match smtp m|^220 Matrix SMTP Mail Server v([\w.]+) on <MATRIX_([\w]+)> Simple Mail Transfer Service Ready\r\n| p/Matrix SMTP Mail Server/ v/$1/ i/on Matrix $2/
match smtp m|^220(\S+) WebShield SMTP V(\d\S.*?) Network Associates, Inc\. Ready at| p/Network Associates WebShield/ h/$1/ v/$2/
match smtp m|^220(\S+) WebShielde(\w+)/SMTP Ready.| p/WebShielde$2 smtpd/ h/$1/
match smtp m|^220 ([-.+\w]+) ESMTP MailMasher ready to boogie\r\n| p/MailMasher smtpd/ h/$1/
# 220 example.com ESMTP Postfix (2.0.13) (Mandrake Linux)
match smtp m|^220 ([-.\w]+) ESMTP Postfix \(([-.\w]+)\) \(([-.\w ]+)\)| p/Postfix smtpd/ h/$1/ v/$2/ i/$3/
# 220 Example LLC example.com ESMTP Postfix (2.6.1)
match smtp m|^220 (.*) ([\w._-]+) ESMTP Postfix \(([\w._-]+)\)\r\n| p/Postfix smtpd/ h/$2/ v/$3/ i/$1/
# postfix 1.1.11-0.woody2
match smtp m|^220([\s-]\S+) ESMTP Postfix| p/Postfix smtpd/ h/$1/
match smtp m|^220 [\*\d\ ]{2,300}\r\n| p|Cisco PIX sanitized smtpd| d|firewall|
match smtp m|^220 ArGoSoft Mail Server Pro for WinNT/2000/XP, Version ([-.\w]+) \(([-.\w]+)\)\r\n| p/ArGoSoft Mail Server Pro/ v/$1/ i/$2/ o/Windows/
match smtp m|^220 ([-\w.]+) ArGoSoft Mail Server Pro for WinNT/2000/XP, Version [\d.]+ \(([\d.]+)\)\r\n| p/ArGoSoft Mail Server Pro/ v/$2/ h/$1/ o/Windows/
match smtp m|^220 ([-\w.]+) ArGoSoft Mail Server, Version [\d.]+ \(([\d.]+)\)\r\n| p/ArGoSoft Mail Server/ v/$2/ h/$1/ o/Windows/
match smtp m|^220 ([-\w_.]+) ArGoSoft Mail Server Freeware, Version [\d.]+ \(([\d.]+)\)\r\n| p/ArGoSoft Mail Server Freeware/ v/$2/ h/$1/ o/Windows/
match smtp m|^220 ArGoSoft Mail Server Plus for WinNT/2000, Version [\d.]+ \(([\d.]+)\)\r\n| p/ArGoSoft Mail Server Plus/ v/$1/ o/Windows/
match smtp m|^220 ([-.\w]+) ESMTP server \([Pp]ost.[Oo]ffice v([-.\w]+) release ([-.\w]+) ID# | p/Post.Office/ h/$1/ v/$2 release $3/
match smtp m|^220 ([-.\w]+) ESMTP VisNetic.MailServer.v([-.\w]+); | p/VisNetic MailServer/ h/$1/ v/$2/
# CommuniGate Pro 4.0.5
match smtp m|^220 ([-.\w]+) ESMTP Service. Welcome.\r\n$| p/CommuniGate Pro smtpd/ h/$1/
match smtp m|^220 ([-.\w]+) Process Software ESMTP service V([-.\w]+) ready| p/Process Software smtpd/ h/$1/ v/$2/ o/OpenVMS/
match smtp m|^220 ([-.\w]+) Mercury (\d[-.\w]+) ESMTP server ready\.\r\n$| p/Mercury Mail smtpd/ h/$1/ v/$2/
match smtp m|^220   ESMTP Service \(Lotus Domino Release ([\w._-]+)\) ready at | p/Lotus Domino smtpd/ v/$1/
match smtp m|^220 ([-.\w]+) ESMTP Service \(Lotus Domino Release (\d[-.\w ]+)\) ready| p/Lotus Domino smtpd/ h/$1/ v/$2/
match smtp m|^220 ([-.\w]+) ESMTP Service \(Lotus Domino (\d[-.\w ]+)\) ready at| p/Lotus Domino smtpd/ h/$1/ v/$2/
match smtp m|^220  ESMTP Service \(Lotus Domino Release (\d[-.\w ]+)\) ready at | p/Lotus Domino smtpd/ v/$1/
match smtp m|^220 ([-.\w]+) ESMTP Service \(Lotus Domino Build V([\w_]+) Beta (\w+)\) ready at | p/Lotus Domino smtpd/ h/$1/ v/$2 Beta $3/
match smtp m|^220  ESMTP Service \(Lotus Domino Build V([\w_]+) Beta (\w+)\) ready at | p/Lotus Domino smtpd/ v/$1 Beta $2/
match smtp m|^220 ([-.\w]+) ESMTP Service \(Lotus Domino Versione ([\w._ -]+)\) ready| p/Lotus Domino smtpd/ v/$2/ h/$1/ i/Italian/
match smtp m|^220 ([-.\w]+) Lotus SMTP MTA Service Ready\r\n$| p/Lotus Notes SMTP/ h/$1/
match smtp m|^220 ([-.\w]+) WebSTAR Mail Simple Mail Transfer Service Ready\r\n| p/WebSTAR SMTP server/ h/$1/
match smtp m|^220 ([-.\w]+) SMTP NAVGW (\d[-.\w]+);| p/Norton Antivirus Gateway NAVGW/ h/$1/ v/$2/
match smtp m|^220 ([-.\w]+) Kerio MailServer (\d[-.\w]+) ESMTP ready\r\n| p/Kerio MailServer/ h/$1/ v/$2/
match smtp m|^220 ([-.\w]+) Kerio MailServer (\d[-.\w]+ patch \d+) ESMTP ready\r\n| p/Kerio MailServer/ h/$1/ v/$2/
match smtp m|^220 YSmtp(\S+) ESMTP service ready| p/Yahoo! smtpd/ h/$1/
match smtp m|^220 (\S+) GMX Mailservices ESMTP| p/GMX smtpd/ h/$1/
match smtp m|^220 (\S+) ESMTP MailMax (\d[-.\w\d]+)| p/MailMax smtpd/ h/$1/ v/$2/
match smtp m|^220 (\S+) ESMTP WEB.DE V([^\s\;]+)| p/Web.de smtpd/ h/$1/ v/$2/
match smtp m|^relaylock: Error: PRODUCT_ROOT_D not defined\nrelaylock: Error: PRODUCT_ROOT_D not defined\n1\n$| p/Plesk relaylock smtp wrapper/ i/broken/
match smtp m|^220 Compuserve Office Mail Service \(lnxc-(\d+)\) ESMTP| p/Compuserve smtpd/ v/$1/
match smtp m|^220 Welcome to Nemesis ESMTP server on \S+| p/Nemesis smtpd/
match smtp m|^220 Welcome to the INDY SMTP Server\r\n$| p/INDY smtpd/
match smtp m|^220 Postini E?SMTP (\d+) [\w\d_+/:-]+ ready| p/Postini smtpd/ v/$1/
match smtp m|^220 ([\w\d-]+)\.hotmail\.com Sending unsolicited commercial| p/Hotmail smtpd/ h/$1/
match smtp m|^220[-\s](\S+) \(IntraStore TurboSendmail\) E?SMTP Service ready| p/TurboSendmail smtpd/ h/$1/
match smtp m|^220[-\s](\S+) E?SMTP Mirapoint (\d[^\;]+);| p/Mirapoint smtpd/ h/$1/ v/$2/
match smtp m|^220 ([\w._-]+) ESMTP Mirapoint Messaging Server MOS ([^;\r\n]+)[;\r\n]| p/Mirapoint Messaging Server MOS smtpd/ h/$1/ v/$2/
match smtp m|^220[-\s](\S+) Trend Micro InterScan Messaging Security Suite, Version: (\d\S+) ready| p/Trend Micro InterScan smtpd/ h/$1/ v/$2/
match smtp m|^220[-\s](\S+).*?Server ESMTP \(iPlanet Messaging Server (\d[^\(\)]+)| p/Sun iPlanet smtpd/ h/$1/ v/$2/
match smtp m|^220[-\s](\S+) running Eudora Internet Mail Server (\d\S+)| p/Eudora smtpd/ h/$1/ v/$2/ o/Windows/
match smtp m|^220[-\s](\S+) running Eudora Internet Mail Server X (\d\S+)\r\n| p/Eudora smtpd/ h/$1/ v/$2/ o/Mac OS X/
match smtp m|^220 (\S+) - Maillennium E?SMTP| p/Maillennium smtpd/ h/$1/
match smtp m|^220 (\S+).*?SMTP \(Sun Internet Mail Server sims.(\d[^\)]+)\)| p/Sun sims smtpd/ h/$1/ v/$2/
match smtp m|^220 (\S+) ESMTP qpsmtpd (\d\S+) ready;| p/qpsmtpd/ h/$1/ v/$2/
match smtp m|^220 (\S+) ESMTP XWall v(\d\S+)| p/XWall smtpd/ h/$1/ v/$2/
match smtp m|^220 (\S+) ESMTP Service \(Worldmail (\d[^\)]+)\) ready| p/Worldmail smtpd/ h/$1/ v/$2/ o/Windows/
match smtp m|^220 (\S+) eMail Sentinel (\d+) ESMTP Service ready| p/eMail Sentinel smtpd/ v/$1/
match smtp m|^220 (\S+) ESMTP mxl_mta-(\d[^\;]+);| p/mxl smtpd/ h/$1/ v/$2/
match smtp m|^220 (\S+) -- Server ESMTP \(SUN JES MTA 6\.x\)| p/SUN JES smtpd/ h/$1/ v/6.x/
match smtp m|^220 (\S+) Service ready by DvISE PostMan \((\d+)\) ESMTP Server| p/DvISE PostMan smtpd/ h/$1/ v/$2/
match smtp m|^220 ([-\w_.]+) Service ready by DvISE PostMan \((\d+)\) ESMTP Server \(Tobit Software, Germany\)\r\n| p/DvISE PostMan smtpd/ h/$1/ v/$2/
match smtp m|^220 (\S+) F-Secure Anti-Virus for Internet Mail ready| p/F-Secure AV SMTP Proxy/ h/$1/
match smtp m|^220 (\S+) Welcome to SpamFilter for ISP SMTP Server v(\d\S+)| p/LogSat SMTP Proxy/ h/$1/ v/$2/
match smtp m|^220-TrendMicro IMSS SMTP proxy\r\n| p/Trend Micro SMTP Proxy/
match smtp m|^220 ?(\S+) ESMTP server \(InterMail v(\S+)| p/InterMail smtpd/ h/$1/ v/$2/
match smtp m|^220 ([-\w_.]+) -- Server ESMTP \(Sun Java\(tm\) System Messaging Server ([\w._-]+) \(built .*; (\d+)bit\)| p/Sun Java System Messaging Server smtpd/ v/$2/ h/$1/ i/$3 bits/
match smtp m|^220 ([-\w_.]+) -- Server ESMTP \(Sun Java\(tm\) System Messaging Server ([\w._-]+) \(built .*; (\d+)bit\)| p/Sun Java System Messaging Server smtpd/ v/$2/ h/$1/ i/$3 bits/
match smtp m|^220 ([-\w_.]+) -- Server ESMTP \(Sun Java\(tm\) System Messaging Server ([\w._-]+) (\d+)bit \(built .*\)\)\r\n| p/Sun Java System Messaging Server smtpd/ v/$3/ h/$1/ i/$2 bits/
match smtp m|^220 ([-\w_.]+) -- Server ESMTP \(Sun Java System Messaging Server ([\d.]+) \(built .*\)\)\r\n| p/Sun Java System Messaging Server smtpd/ v/$2/ h/$1/
match smtp m|^220 (\S+) -- Server ESMTP \(Sun Java System Messaging Server (\d[^\(\)]+)| p/Sun Java System Messaging Server smtpd/ h/$1/ v/$2/
match smtp m|^220 jMailer SMTP Server\r\n$| p/jMailer smtpd/
match smtp m/^220[- ][^ ]+ Smail-([^ ]+) .*ESMTP/s p/Smail-ESMTP/ v/$1/
match smtp m/^220[- ][^ ]+ Smail-([^ ]+) / p/Smail/ v/$1/
match smtp m|^220 \[([-\w_.]+)\] ESMTP amavisd-new service ready\r\n| p/amavisd smtpd/ h/$1/
match smtp m/^220 SMTP-Server Classic Hamster (Vr\.|Version) [\d.]+ \(Build ([\d.]+)\)\r\n/ p/Classic Hamster smtpd/ v/$2/ o/Windows/
match smtp m|^220-Stalker Internet Mail Server V.([\w.]+) is ready\.\r\n| p/Stalker smtpd/ v/$1/ o/Mac OS/
match smtp m|^220-([-\w_.]+) Stalker Internet Mail Server V\.([\w.]+) is ready\.\r\n| p/Stalker smtpd/ v/$2/ h/$1/ o/Mac OS/
match smtp m|^220 ([-\w_.]+) ESMTP MailMax ([\d.]+) [A-Z][a-z][a-z].*\r\n| p/MailMax smtpd/ v/$2/ h/$1/ o/Windows/
match smtp m|^220 ([-\w_.]+) Mailmax version ([\d. ]+) ESMTP Mail Server Ready \r\n| p/MailMax smtpd/ v/$2/ h/$1/
match smtp m|^220 ([-\w_.]+) running IBM MVS SMTP CS V2R10 on .*\r\n| p/IBM MVS smtpd/ h/$1/ o/MVS/
match smtp m|^220 [-\w_]+ ESMTP ([-\w_.]+) \(Debian/GNU\)\r\n| p/Postfix smtpd/ h/$1/ o/Linux/ i/Debian/
match smtp m|^220 ESMTP \(Debian/GNU Mewwwwwww\)\r\n| p/Postfix smtpd/ o/Linux/ i/Debian/
match smtp m|^220 ([\w._-]+) [\w._-]+ ESMTP Postfix \(Debian/GNU\)| p/Postfix smtpd/ o/Linux/ i/Debian/
match smtp m|^220 ([-\w_.]+) ESMTP postfix NO UCE\r\n| p/Postfix smtpd/ h/$1/ i/whoson patch/
match smtp m|^220 ([-\w_.]+) SMTPD Server - Postfix\r\n| p/Postfix smtpd/ h/$1/
match smtp m|^220 ([-\w_.]+) ESMTP PostFix ([\d.]+)\r\n| p/Postfix smtpd/ h/$1/ v/$2/
match smtp m|^220 ([-\w_.]+) ESMTP Oracle Email Server SMTP Inbound Server\t([\d.]+) \t  Ready\r\n| p/Oracle smtpd/ v/$2/ h/$1/
match smtp m|^220 ([-\w_.]+) Mail essentials  server \(([\d.]+)\) ready for ESMTP transfer\r\n| p/Mail essentials for Exchange smtpd/ v/$2/ h/$1/ o/Windows/
match smtp m|^220 ([-\w_.]+) ESMTP - WinRoute Pro ([\d.]+)\r\n| p/WinRoute Pro smtpd/ v/$2/ h/$1/ o/Windows/
match smtp m|^220 ([-\w_.]+) ESMTP Lyris ListManager service ready\r\n| p/Lyris ListManager smtpd/ h/$1/
match smtp m|^220  ESMTP Lyris service ready\r\n| p/Lyris smtpd/
match smtp m|^220  ESMTP Lyris ListManager service ready\r\n| p/Lyris ListManager smtpd/
match smtp m|^220-([-\w_.]+) ESMTP\r\n220 [-\w_.]+ AsyncOS\r\n| p/IronPort C-60 smtpd/ o/AsyncOS/ d/specialized/
match smtp m|^220 ([-\w_.]+) SMTP Ready 12\.\r\n| p/Tunix firewall smtpd/ h/$1/ d/firewall/
match smtp m|^220 ([-\w_.]+) ESMTP server \(Netscape Messaging Server - Version ([\d.]+)\) ready .*\r\n| p/Netscape Messaging Server/ v/$2/ h/$1/
match smtp m|^220 ([-\w_.]+) ESMTP SMTPBeamer v([\d.]+)\r\n| p/SMTPBeamer smtpd/ v/$2/ h/$1/ o/Windows/
match smtp m|^220 ([-\w_.]+) ZMailer Server ([\w.]+) #\d+ ESMTP ready at .*\r\n| p/ZMailer smtpd/ v/$2/ h/$1/ o/Unix/
match smtp m|^220 - zeus SMTPS Sendmail ([-\w_.]+)/[-\w_.]+; .*\n| p/Zeus SMTPS smtpd/ v/$1/
match smtp m|^220 Coremail SMTP\(Anti Spam\) System \(\w+\[(\d+)\]\)\r\n| p/Coremail smtpd/ v/$1/
match smtp m|^220 ([-\w_.]+) ESMTP WorkgroupMail ([\d.]+) .*\r\n| p/WorkgroupMail smtpd/ v/$2/ h/$1/ o/Windows/
match smtp m|^220 ([-\w_.]+) \(PowerMTA(?:\(TM\)) v([\w.]+)\) ESMTP service ready\r\n| p/PowerMTA smtpd/ v/$2/ h/$1/
match smtp m|^220 ([-\w_.]+) ESMTP BorderWare MXtreme Mail Firewall\r\n| p/BorderWare MXtreme smtpd/ h/$1/ d/firewall/
match smtp m|^220 ([-\w_.]+) SMTP Server \(JAMES SMTP Server ([\w.]+)\) ready| p/JAMES smtpd/ v/$2/ h/$1/
match smtp m|^220 ([-\w_.]+) ESMTP MDaemon ([\d.]+) ready\r\n| p/MDaemon smtpd/ v/$2/ h/$1/ o/Windows/
match smtp m|^220 ([-\w_.]+)\s+ESMTP MDaemon ([\d.]+); .*\r\n| p/MDaemon smtpd/ v/$2/ h/$1/ o/Windows/
match smtp m|^220 ([-\w_.]+) ESMTP MDaemon ([\d.]+) UNREGISTERED; .*\r\n| p/MDaemon smtpd/ v/$2/ h/$1/ i/Unregistered/ o/Windows/
match smtp m|^220[ -]([-\w_.]+) ESMTP MSA MDaemon ([\d.]+);| p/MDaemon smtpd/ i/MSA support/ v/$2/ h/$1/ o/Windows/
match smtp m|^421 Sorry, SMTP server too busy right now \(193\); try again later\r\n| p/MDaemon smtpd/ i/Server too busy error/ o/Windows/
match smtp m|^220 ([-\w_.]+) ESMTP HT Mail Server v([\d.]+); .*\r\n| p/IceWarp smtpd/ v/$2/ h/$1/
match smtp m|^220 ([-\w_.]+) ESMTP IceWarp ([\d.]+)[; ]| p/IceWarp smtpd/ v/$2/ h/$1/
match smtp m|^220 ([-\w_.]+) ESMTP Gruponet IE2020 ([\d./]+);\r\n| p/Gruponet mail appliance smtpd/ v/$2/ h/$1/ d/specialized/
match smtp m|^220 ([-\w_.]+) mailfront ESMTP\r\n| p/mailfront smtpd/ h/$1/
match smtp m|^220 ([-\w_.]+) SMTP Server SLmail ([\d.]+) Ready ESMTP spoken here\r\n| p/SLmail smtpd/ v/$2/ h/$1/ o/Windows/
match smtp m|^220 ([-\w_.]+) VaMailArmor-([\d.]+)\r\n| p/VaMailArmor smtpd/ v/$2/ h/$1/
match smtp m|^220 ([-\w_.]+) ESMTP MailFrontier \(([\d.]+)\)\r\n| p/MailFrontier smtpd/ v/$2/ h/$1/ d/firewall/
match smtp m|^220 ([-\w_.]+) WindowsNT SMTP Server v([\w/.]+) ESMTP ready at .*\r\n| p/Windows NT SMTP Server smtpd/ h/$1/ o/Windows/
match smtp m|^220 ([-\w_.]+) \(LSMTP for Windows NT v([\w.]+)\) ESMTP server ready\r\n| p/LSMTP smtpd/ v/$2/ h/$1/ o/Windows/
match smtp m|^220 ([-\w_.]+) SMTP Mandamail ([\d.]+)/[\d.]+\r\n| p/Mandamail smtpd/ v/$2/ h/$1/
match smtp m|^220 Welcome to the QK SMTP Server\r\n| p/QK smtpd/ o/Windows/
match smtp m|^220 PostCast SMTP server \(http://www\.postcastserver\.com/\) ready at .*\r\n| p/PostCast smtpd/ o/Windows/
match smtp m|^220 ([-\w_.]+) running IBM MVS SMTP CS (\w+) on .*\r\n| p/IBM MVS smtpd/ v/$2/ h/$1/ o/MVS/
match smtp m|^Permission denied - do not try again\.\r\n| p/Hamster smtpd/ i/Access denied/ o/Windows/
match smtp m|^500 Permission denied - closing connection\.\r\n| p/Hamster smtpd/ i/Access denied/ o/Windows/
match smtp m|^220 \(SMTP\) hMailServer ([\d.]+) - Up since .*\r\n| p/hMailServer smtpd/ v/$1/ o/Windows/
match smtp m|^220 ([-\w_.]+) ESMTP hMailServer ([\w.-]+)\r\n| p/hMailServer/ v/$2/ h/$1/ o/Windows/
match smtp m|^220 ([-\w_.]+) Ready for action \(Mailtraq ([\d.]+)/E?SMTP\)\r\n| p/Mailtraq smtpd/ v/$2/ h/$1/ o/Windows/
match smtp m|^220 ([-\w_.]+) SMTP Service Ready \(QuickMail Pro Server for MacOS ([\d.]+)\)\r\n| p/QuickMail Pro smtpd/ v/$2/ h/$1/ o/Mac OS/
match smtp m|^220 ([-\w_.]+) HP Sendmail \(([\d/.]+) .*\) ready at .*\r\n| p/HP Sendmail/ v/$2/ h/$1/ o/HP-UX/
match smtp m|^220-([-\w_.]+) Bluecat Networks Inc\. Meridius Security Gateway\r\n220 | p/Bluecat Meridius smtpd/ d/firewall/
match smtp m|^220 ([-\w_.]+) SurgeSMTP \(Version ([\w.-]+)\) http://surgemail\.com\r\n| p/Surgemail smtpd/ v/$2/ h/$1/
match smtp m|^220 ([-\w_.]+) Hermes ([\d.]+) ML SMTP Ready\.\r\n| p/Hermes smtpd/ v/$2/ h/$1/ o/Windows/
match smtp m|^220 LiteMail SMTP Server Ready\.\r\n| p/LiteMail smtpd/ o/Windows/
match smtp m|^220 ([-\w_.]+) SMTP Server \(DeskNow SMTP Server ([\d.]+)\) ready .*\r\n| p/DeskNow smtpd/ v/$2/ h/$1/
match smtp m|^220 ([-\w_.]+) SMTP Server \(DeskNow\) ready| p/DeskNow smtpd/ h/$1/
match smtp m|^220 network-box ESMTP\r\n| p/Network Box smtpd/ d/firewall/
match smtp m|^220-\S+ Sendmail ([\d.]+)/A/UX ([\d.]+) ready at .*\r\n220 ESMTP spoken here\r\n| p/Sendmail/ v/$1/ i|on A/UX $2| o|A/UX|
match smtp m|^220 ([-\w_.]+) sina_smtpd \(([\d.-]+)\) id=\d+\r\n| p/SINA smtpd/ v/$2/ h/$1/
match smtp m|^220 ([-\w_.]+) SpearMail SMTP Daemon ready\.\r\n| p/SpearMail smtpd/ h/$1/ o/Windows/
match smtp m|^220 ESMTP on WebEasyMail \[([\d.]+)\] ready\.  http://www\.51webmail\.com\r\n| p/WebEasyMail smtpd/ v/$1/ o/Windows/
match smtp m|^220 ([-\w_.]+) AntiVir MailGate\r\n| p/AntiVir MailGate smtpd/ h/$1/
match smtp m|^220 server ESMTP KEN! v([\d.]+); .*\r\n| p/AVM KEN! smtpd/ v/$1/ o/Windows/
match smtp m|^220 ([-\w_.]+) NTMail \(v([\d.]+)/[\w.]+\) ready for ESMTP transfer   \r\n| p/NTMail smtpd/ v/$2/ h/$1/ o/Windows/
match smtp m|^220-([-\w_.]+) Sendmail IBM OS/2 SENDMAIL VERSION ([\w./]+) ready at .*\r\n220 ESMTP spoken here\r\n| p/Sendmail smtpd/ v/$2/ h/$1/ o|OS/2|
match smtp m|^220 imss-2 ESMTP ready at .*\r\n| p/Trend IMSS smtpd/ o/Windows/
match smtp m|^220 ([-\w_.]+) Service ready\.\r\n214- Valid commands are:\r\n214- HELO  MAIL  RCPT  DATA  RSET  QUIT  NOOP\r\n214- HELP  VRFY\r\n214- Commands not valid are:\r\n214- SEND  SOML  SAML  TURN\r\n.*214- [-\w_.]+ is running the OS/400 operating system\.\r\n|s p|OS/400 smtpd| o|OS/400|
match smtp m|^220 shttp\.srv Simple Mail Transfer Service Ready\r\n| p/Small Home Server smtpd/ o/Windows/
match smtp m|^501 Domain must resolve\r\n$| p/odmrd/
match smtp m|^220 ([-\w_.]+) ModusMail ESMTP Receiver Version ([\d.]+) Ready\r\n| p/ModusMail smtpd/ v/$2/ h/$1/ o/Windows/
match smtp m|^220 mailmatrix SMTP Server \(Mail Matrix Server\) ready| p/Mail Matrix smtpd/ o/Windows/
match smtp m|^220-([-\w_.]+) ESMTP .* GoMail V([\d.]+);| p/GoMail mass mailing plugin smtpd/ v/$2/ h/$1/ o/Windows/
match smtp m|^220 [-\w_.]+ Winmail Mail Server ESMTP ready\r\n| p/Winmail smtpd/ o/Windows/
match smtp m|^220 ([-\w_.]+) ESMTP \(Code-Crafters Ability Mail Server ([\d.]+)\)\r\n| p/Code-Crafters Ability smtpd/ v/$2/ h/$1/ o/Windows/
match smtp m|^220 ([-\w_.]+) SMTP Welcome to the Internet Anywhere Mail Server Version: ([\d.]+)\. Build: (\d+) by True North Software, Inc\.\r\n| p/True North Internet Anywhere smtpd/ v/$2/ i/Build $3/ h/$1/ o/Windows/
# Notice the ; immediatley after the host
match smtp m|^220 ([-\w_.]+); .* \+\d+\r\n| p/Webwasher CSM Suite smtpd/ h/$1/ o/Windows/
match smtp m|^451 Temporary local problem - please try later\r\n| p/qmail smtpd/ o/Unix/
match smtp m|^421 unable to read controls \(#4\.3\.0\)\r\n| p/qmail smtpd/ i/qmail-smtpd-auth 0.31/ o/Unix/
match smtp m|^220 ([-\w_.]+) Miralix SMSGwSMTP Ready\r\n| p/Miralix SMTP2SMS Gateway/ h/$1/ o/Windows/
match smtp m|^554 Please check your SMTP server is set to [-\w_.]+\.co\.uk\. Further help is available at| i/Wanadoo blocks smtp - NOT A REAL smtpd!/
match smtp m|^554 Please check that your outgoing mail server settings are correct\. Contact your service provider's technical support for assistance\.\n| i/Wanadoo blocks smtp - NOT A REAL smtpd!/
match smtp m|^220 ([-\w_.]+) V([\w._-]+), OpenVMS V([\w._-]+) Alpha ready at .* \r\n| p/OpenVMS smtpd/ v/$2/ h/$1/ i/OpenVMS $3; Alpha/ o/OpenVMS/
match smtp m|^220 rblsmtpd\.local\r\n| p/rblsmtpd wrapped smtpd/ i/Connecting from banned IP/
match smtp m|^rblsmtpd: [\d.]+ pid \d+:.*220 rblsmtpd\.local\r\n|s p/rblsmtpd wrapped smtpd/ i/Connecting from banned IP/
match smtp m|^220 Welcome to the Advanced SMTP Server\r\n| p/SoftStack Advanced smtpd/ o/Windows/
match smtp m|^220  SurgeSMTP \(Version ([-\w_.]+)\) http://surgemail\.com\r\n| p/Netwin Surgemail smtpd/ v/$1/
match smtp m|^220 HMailServer ESMTP\r\n| p/HMailServer smtpd/ o/Windows/
match smtp m|^220 SMTP-Server The Croatian Classic Hamster Ver\. [\d.]+ \(Podverzija ([\d.]+)\)\r\n| p/Classic Hamster smtpd/ v/$1/ i/Croatian/
match smtp m|^220 I, CALLPILOT\[[\d.]+\], speak ESMTP\.  Talk to me\.\r\n| p/Nortel CallPilot imapd/ d/telecom-misc/
match smtp m|^220 ([-\w_.]+) Welcome to RaidenMAILD E?SMTP service v([\d.]+),| p/RaidenMAILD smtpd/ v/$2/ h/$1/ o/Windows/
match smtp m|^220 ESMTP [^ ]+ CMailServer ([\d.]+) SMTP Service Ready\r\n| p/Youngzsoft CMailServer smtpd/ v/$1/ o/Windows/
match smtp m|^220 ESMTP on WinWebMail \[([\d.]+)\] ready\.  http://www\.winwebmail| p/WinWebMail smtpd/ v/$1/ o/Windows/
match smtp m|^220-W E L C O M E   T O   Q U A R K M A I L   S M T P   S E R V I C E !\r\n220 ([-\w_.]+) ESMTP server \(quarkmail server - version ([\d.]+)\) ready| p/Quarkmail smtpd/ v/$2/ h/$1/
match smtp m|^220 ([-\w_.]+) ESMTP Sendmail Switch-([\d.]+)/Switch-([\d.]+);| p/Sendmail Switch smtpd/ v/$2/ i/Switch $3/ h/$1/
# This is a fall-back line for other probes when postfix banner is stripped
match smtp m|^220 .*\r\n221 2\.7\.0 Error: I can break rules, too\. Goodbye\.\r\n| p/Postfix smtpd/
match smtp m|^220 ([-\w_.]+) running EIMS X ([\w.]+)\r\n| p/Eudora EIMS X smtpd/ h/$1/ v/$2/ o/Mac OS X/
match smtp m|^220  DP-3510\r\n| p/Panasonic DP-3500 smtpd/
match smtp m|^220 ([-\w_.]+) Axigen ESMTP ready\r\n| p/Axigen smtpd/ h/$1/ o/Unix/
match smtp m|^421 Unexpected log failure, please try later\r\n| p/Postfix smtpd/
match smtp m|^220 ([-\w_.]+) DynFX ESMTP Server ([-\w_.]+) \(| p/DynFX smtpd/ h/$1/ v/$2/ o/Windows/
match smtp m|^220 ;; ESMTP connection timed out; no servers could be reached Sendmail ([-\w_.]+)/| p/Sendmail/ v/$1/ i/broken/
match smtp m|^554 ([-\w_.]+) ESMTP not accepting messages\r\n| p/Sendmail/ h/$1/ i/Not accepting mail/
match smtp m|^220 ([-\w_.]+) L-Soft HDMail SMTP Service Version: ([-\w_.()]+) ready| p/L-Soft HDMail smtpd/ o/Linux/ h/$1/ v/$2/
match smtp m|^220 ([-\w_.]+) Synchronet SMTP Server ([\d.]+)-Win32 Ready\r\n| p/Synchronet smtpd/ v/$2/ h/$1/ o/Windows/
match smtp m|^220 ShareMailPro SMTP Server Ready \r\n| p/LavaSoftware ShareMailPro smtpd/ o/Windows/
match smtp m|^220 ([-\w_.]+) ESMTP Service\(Mail2000 ESMTP Server V([-\w_.]+)\) ready| p/Mail2000 smtpd/ v/$1/
match smtp m|^220 ([-\w_.]+) 4D WebSTAR V Mail \(([-\w_.]+)\) Ready for action\r\n| p/4D WebSTAR smtpd/ h/$1/ v/$2/ o/Mac OS X/
match smtp m|^220 ([-\w_.]+) ESMTP server \(Neon Mail Server System Advance ([-\w_.]+),| p/Neon Mail Server smtpd/ v/$2/ h/$1/
match smtp m|^553 Requested action not taken; No permission\.\r\n$| p/Mitel 3300 PBX smtpd/ i/Access denied/ d/PBX/
match smtp m|^421 [-\w_.]+ - Your name, '\[[-\w_.]+\]', is unknown to me\.\r\n| p/SCO smtpd/ i/Unknown host/ o/SCO UNIX/
match smtp m|^220 Service ready KMC252 smtpd\r\n| p/Konica Minolta bizhub KMC252 printer smtpd/ d/printer/
match smtp m|^220 ([\w_.-]+) cqgreylist - minimal smptd\r\n| p/cqgreylist minimal smtpd/ h/$1/
match smtp m|^220 ([\w_.-]+) ESMTP AnNyungSMTP ([\w._-]+);| p/AnNyung smtpd/ h/$1/ v/$2/
match smtp m|^220 DP-1820E\r\n| p/Panasonic DP-1820E printer smtpd/ d/printer/
match smtp m|^220 ([\w_.-]+) -- Server ESMTP \(PMDF V([\d.]+)-| p/PMDF smtpd/ o/OpenVMS/ h/$1/ v/$2/
match smtp m|^220 ([\w_.-]+) ESMTP SecurityGateway ([0-9]+.[0-9]+.[0-9]+)| p/ALT-N SecurityGateway smtpd/ h/$1/ v/$2/
match smtp m|^220 ([\w_.-]+) VHCS2 [\w._-]+ (\w+) Managed ESMTP ([\w._-]+)\r\n| p/Postfix smtpd/ i/Virtual Hosting Control System $3 $2/ h/$1/
match smtp m|^220 ([\w_.-]+) ESMTP ispCP (.*) OMEGA Managed\r\n| p/Postfix smtpd/ i/ispCP OMEGA $2/ h/$1/
# embyte
match smtp m|^220.*Simple Mail Transfer Service Ready\. Version ([\d.]+)| p/Goodtech smtpd/ v/$1/
match smtp m|^220.*SMTP Welcome to the IA eMailServer Corporate Edition Version: ([\d.]+ Build: [\d]+)| p/IA eMailServer Corporate/ v/$1/
match smtp m|^220.*SMTP Welcome to the IA eMailServer Standard Edition Version: ([\d.]+ Build: [\d]+)| p/IA eMailServer Standard/ v/$1/
match smtp m|^220 ([\w_.-]+) bizsmtp ESMTP server ready\r\n| p/Bizanga bizsmtp smtpd/ h/$1/
match smtp m|^220 ([\w_.-]+) ESMTP NetBox\(tm\)\r\n| p/NetBox smtpd/ h/$1/
match smtp m|^220 ([\w_.-]+) StrongMail SMTP Service Version: (\S+) ready| p/StrongMail smtpd/ v/$2/ h/$1/
match smtp m|^421 Service not available, closing transmission channel\r\n$| p/Oki 3200N laser printer smtpd/ i/service disabled/ d/printer/
match smtp m|^421 Service not available, closing transmission channel \r\n$| p/Konica Minolta bizhub smtpd/ i/service disabled/ d/printer/
match smtp m|^220 ([\w_.-]+) ESMTP OpenSMTPD\r\n| p/OpenSMTPD/ h/$1/
match smtp m|^220 Merak MAILSRV\r\n| p/Merak Mail Server smptd/
match smtp m|^220 ([\w_.-]+) ESMTP Citadel server ready\.\r\n| p/Citadel smtpd/ h/$1/
match smtp m|^220 ([\w_.-]+) Epiphany CME SMTP Server Version ([\d.]+) ready at [^\r\n]*\r\n| p/Epiphany Campaign Manager for Email (CME) smtpd/ v/$2/ h/$1/
match smtp m|^220 ([\w_.-]+) \(\w+\) Welcome to Nemesis ESMTP server\r\n| p/Nemesis smtpd/ h/$1/
match smtp m|^220 BEJY V([\w._-]+)  SMTP ([\w._-]+)  \(c\) \d+-\d+ by BebboSoft, Stefan \"Bebbo\" Franke, all rights reserved ready\r\n$| p/BEJY smtpd/ v/$2/ i/BEJY $1/
match smtp m|^220 Welcome NGOS SMTP Server version ([\w._-]+)\r\n$| p/NewsGator Enterprise Server smtpd/ v/$1/
match smtp m|^220 ([\w._-]+) Kerio Connect ([\w._-]+) ESMTP ready\r\n| p/Kerio Connect smtpd/ v/$2/ h/$1/
match smtp m|^220 Service ready (KMBT[0-9A-F]+) smtpd\r\n| p/Konica Minolta printer smtpd/ h/$1/
match smtp m|^220 ([\w._-]+) running IBM VM SMTP Level (\d+) on | p/IBM VM smtpd/ v/Level $2/ h/$1/
match smtp m|^220 DavMail SMTP ready at | p/DavMail smtpd/
match smtp m|^421 4\.3\.2 Service not available\r\n| p/Microsoft Exchange 2010 smtpd/ i/not available/
match smtp m|^220 ([\w._-]+) InSciTek OIS Ready here ESMTP\r\n| p/Allworx 6x VoIP phone smtpd/ d/VoIP phone/
match smtp m|^220 ([-\w_.]+)\s+ESMTP IdeaSmtpServer ([^\s]+) ready\.\r\n| p/IdeaSmtpServer smtpd/ v/$2/ h/$1/

#(insert smtp)

match smtp-proxy m|^220 ([-\w_.]+) SMTP/DeleGate/([\d.]+) ready at .*\r\n| p/DeleGate smtpd/ v/$2/ h/$1/
match smtp-proxy m|^220 ([-/.+\w]+) SMTP AnalogX Proxy (\d[-.\w]+) \(Release\) ready\r\n| p/AnalogX SMTP proxy/ h/$1/ v/$2/
match smtp-proxy m|^220 ([-\w_.]+) ESMTP spamd IP-based SPAM blocker; .*\r\n| p/spamd smtpd/ h/$1/
match smtp-proxy m|^220 YahooPOPs! Simple Mail Transfer Service Ready\r\n| p/YahooPOPs! smtpd/
match smtp-proxy m|^220  ESMTP smtprelay service ready\.\r\n| p/GeNUGate firewall smtp relay/ d/firewall/
match smtp-proxy m|^220 ([-\w_.]+) Tumbleweed MMS SMTP Relay Service ready\r\n| p/Tumbleweed smtp proxy/ h/$1/ d/firewall/
match smtp-proxy m|^220 ([-\w_.]+) SMTP hotsmtpd v([\d.]+)\. ESMTP-HTTPMail Gateway based on hotwayd\.\r\n| p/hotsmtpd based on hotwayd/ v/$2/ h/$1/
match smtp-proxy m|^220 ([-\w_.]+) Welcome SpamFilter for ISP SMTP Server v([\d.]+) - Unlicensed Evaluation Copy\r\n| p/SpamFilter for ISP smtpd/ v/$2/ h/$1/ i/Unregistered/ o/Windows/
match smtp-proxy m|^220 Welcome to the 1st SMTP Server\r\n| p/1st SMTP relay/ o/Windows/
match smtp-proxy m|^421 proxyplus\.universe SMTP server\. Insecure access - terminating\.\r\n| p/Proxy+ smtp proxy/ i/Access denied/ o/Windows/
match smtp-proxy m|^220 AVG ESMTP Proxy Server Beta - ([\d./]+) \[[\d.]+\]\r\n| p/GriSoft anti-virus smtp proxy/ v/$1/ o/Windows/
match smtp-proxy m|^220 AVG ESMTP Proxy Server ([\d./]+) \[[\d./]+\]\r\n| p/GriSoft anti-virus smtp proxy/ v/$1/ o/Windows/
match smtp-proxy m|^554 ([\d.]+) ([-\w_.]+) No mail service\r\n| p/Symantec SGS smtp proxy/ v/$1/ h/$2/
match smtp-proxy m|^220 ([-\w_.]+) ESMTP Scalix SMTP Relay ([\d.]+); .*\r\n| p/Scalix smtp relay/ v/$2/ h/$1/
match smtp-proxy m|^220 Traffic Inspector SMTP Gate \(SPAM protected\), ver\. ([\w._-]+), ready at.*\r\n| p/Smart-Soft spam filtering smtp-proxy/ v/$1/ o/Windows/
match smtp-proxy m|^220 mailwall SMTP Server \(Ikarus MailWall by David Grabenweger\) ready\r\n| p/Ikarus MailWall smtp-proxy/
match smtp-proxy m|^220 ([-\w_.]+) ESMTP - eXpurgate ([\d.]+) \(| p/eXpurgate smtp proxy/ v/$2/ h/$1/
match smtp-proxy m|^220 CCProxy ([\d.]+) SMTP Service Ready\(Unregistered\)\r\n| p/CCProxy smtp proxy/ v/$1/ i/Unregistered/ o/Windows/
match smtp-proxy m|^220 CCProxy ([\d.]+) SMTP Service Ready\r\n| p/CCProxy smtp proxy/ v/$1/ o/Windows/
match smtp-proxy m|^220 ([-\w_.]+) F-Secure/fsigk_smtp/\d+/[-\w_.]+\r\n| p/F-Secure Internet Gateway SMTP proxy/ h/$1/
match smtp-proxy m|^521 Host does not accept mail from you, closing transmission channel\.\.\.\r\n| p/F-Secure Internet Gatekeeper smtp proxy/
match smtp-proxy m|^NoSpamToday! SMTP Proxy Monitoring Service Ready\.\r\n| p/Byteplant NoSpamToday! smtp proxy/
match smtp-proxy m|^220 ([-\w_.]+) ESMTP bitdefender| p/BitDefender anti-virus mail gateway/ h/$1/ o/Windows/
match smtp-proxy m|^220 ([-\w_.]+) ESMTP BitDefender Proxy version ([^\r\n]+)\r\n| p/BitDefender anti-virus mail gateway/ h/$1/ v/$2/ o/Windows/
match smtp-proxy m|^220 ([-\w_.]+) ESMTP BitDefender Proxy\r\n| p/BitDefender anti-virus mail gateway/ h/$1/ o/Windows/
match smtp-proxy m|^220 Proxy\+ SMTP server at ([-\w_.]+)\. Authentication required\.\r\n| p/Proxy+ smtp proxy/ h/$1/ o/Windows/
match smtp-proxy m|^220 [-\w_.]+ avast! SMTP proxy ready\.\r\n| p/Avast! anti-virus smtp proxy/ o/Windows/
match smtp-proxy m|^220 UserGate: SMTP service ready\r\n| p/UserGate smtp proxy/ o/Windows/
match smtp-proxy m|^220 ([\w._-]+) WebShielde1000/SMTP Ready\.\r\n| p/McAfee WebShield e1000 smtp proxy/ v/$1/ d/security-misc/
match smtp-proxy m|^220 ([-\w_.]+) (SCM\d+)/SMTP Ready\.\r\n| p/McAfee $2 smtp proxy/ d/security-misc/ h/$1/
match smtp-proxy m|^220 ([\w._-]+) Welcome to SpamFilterISP SMTP Server v([\w._-]+) - Unlicensed Evaluation Copy\r\n| p/SpamFilterISP smtp proxy/ h/$1/ v/$2/ i/evaluation copy/
match smtp-proxy m|^220 arkoon Sendmail ready\. \r\n| p/Arkoon smtp proxy/
match smtp-proxy m|^554 You are not allowed to connect\.\r\n| p/Symantec Brightmail smtp proxy/
match smtp-proxy m|^220 ([\w._-]+) ESMTP Symantec Brightmail Gateway\r\n| p/Symantec Brightmail smtp proxy/
match smtp-proxy m|^220 ([\w._-]+) \[ESMTP Server\] service ready;Bonjour; [^\r\n]*\r\n| p/Trend Micro InterScan Messaging Security smtp proxy/ d/proxy server/ h/$1/
match smtp-proxy m|^220 ([\w._-]+) ESMTP server ready \(Alligate v([\w._-]+)\)(?: AUTH ONLY)?\r\n| p/Alligate smtp proxy/ v/$2/ h/$1/
match smtp-proxy m|^220 Alligate Greylisting Server ready\r\n| p/Alligate smtp proxy greylisting server/
match smtp-proxy m|^220 ([\w._-]+)\.ARK Sendmail ready\. \r\n| p/Arkoon smtp replay/ i/Sendmail/ h/$1/
match smtp-proxy m|^421 too many connections\r\n| p/Barracuda 300 spam filter/
match smtp-proxy m|^220 ([-\w_.]+) ESMTP Service ready\r\n| p/ESET NOD32 anti-virus smtp proxy/
match smtp-proxy m|^220 ([\w._-]+) MAILFOUNDRY ESMTP\r\n| p/MailFoundry antispam smtp proxy/ h/$1/
match smtp-proxy m|^220 ([\w._-]+) EWSA(\w+)/SMTP Ready\.\r\n| p/McAfee EWSA $2 smtp proxy/ h/$1/

match fw1-topology m|^[QY]\0\0\0$| p/Checkpoint FW1 Topology/ d/firewall/


softmatch smtp m|^220[\s-].*?E?SMTP[^\r]*\r\n|
softmatch smtp m|^572 Relay not authorized\r\n| i/Relay not authorized/
# This is likely Cisco specific, but making it generic just in case - Tom S.
softmatch smtp m|^550 (\d.\d.\d) ([^\r\n]+)| p/Unrecognized SMTP service/ i/$1 $2/

match smtp-stats m|^Statistics from .*\n M   msgsfr  bytes_from   msgsto    bytes_to  msgsrej msgsdis  Mailer\n| p/Multi Router Traffic Grapher smtp statistics/

match snapmirror m|^\x80\0\0\x24\0\0\0\x01\x4c\xb4\x21\xd2\0\0\0\0\0\0\x05\x02\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\x04\0\0\0\0$| p/SnapMirror replication/ o/Data ONTAP/ d/storage-misc/

match snpp m|^220 ([-.\w]+) SNPP server \(HylaFAX \(tm\) Version ([-.\w]+)\) ready.\r\n| p/HylaFAX SNPP/ h/$1/ v/$2/
match snpp m|^220 QuickPage v(\d[-.\w]+) SNPP server ready at | p/QuickPage SNPP/ v/$1/
match snpp m|^220 ([-.\w]+) SNPP Sendpage ([-\w_.]+) | p/Sendpage SNPP/ h/$1/ v/$2/

match sobby m|^obby_welcome:\d+\nnet6_encryption:\d+\n| p/Sobby collaborative editing/

match socks-proxy m|^Unauthorized \.\.\.\r\nIP Address: [\d.]+\r\nMAC Address: \r\nServer Time: \d\d\d\d-\d\d-\d\d \d{1,2}:\d\d:\d\d\r\nAuth Result: Invalid user\.$| p/CCProxy socks proxy/ i/unauthorized/

match sophos m|^IOR:[a-zA-Z0-9]{32}| p/Sophos Message Router/ i/Interroperable Object Reference Service/

match sourceviewerserver m|^OK SourceViewerService v1\.0\r\n| p/NetBeans Source Viewer Service/

# http://udk.openoffice.org/common/man/spec/urp.html
match urp m|^\0\0\0\x60\0\0\0\x01\xf8\x04\x96\0\0'com\.sun\.star\.bridge\.XProtocolProperties\x15UrpProtocolProperties\0\0\x14\r\0\0\0\x85\xfbc\x80\x9e\xca@\$\xbc\xc7\x9e\xbb#\x0f\xfc\xd6\0\0\x92\]\xe4\xb8$| p/UNO Remote Protocol (URP)/

match sourceoffice m|^200\r\nProtocol-Version:(\d[.\d]+)\r\nMessage-ID:\d+\r\nDatabase .*\r\nContent-Length:\d+\r\n\r\n(\w:\\.*ini)\r\n\r\n| p/Sourcegear SourceOffSite/ i/Protocol $1; INI file: $2/
match sourceoffice m|^250\r\nProtocol-Version:(\d[.\d]+)\r\nMessage-ID:\d+\r\nDatabase .*\r\nContent-Length:\d+\r\nKey Length:(\d+)\r\n\r\n.*(\w:\\.*ini)\r\n\r\n|s p/Sourcegear SourceOffSite/ i/Protocol $1; Key len: $2; INI file: $3/

match spmd m|^SPMD_ACK\0\0\x01\0\x01$| p/Softimage XSI SPMD license server/ o/Windows/

# F-Secure/WRQ
match ssh m|^SSH-([\d.]+)-([\d.]+) F-Secure SSH Windows NT Server\r?\n| p/F-Secure WinNT sshd/ v/$2/ i/protocol $1/ o/Windows/
match ssh m|^SSH-([\d.]+)-([\d.]+) dss F-SECURE SSH\r?\n| p/F-Secure sshd/ v/$2/ i/dss-only; protocol $1/
match ssh m|^SSH-([\d.]+)-([\d.]+) F-SECURE SSH.*\r?\n| p/F-Secure sshd/ v/$2/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-ReflectionForSecureIT_([-\w_.]+) - Process Software MultiNet\r\n| p/WRQ Reflection for Secure IT sshd/ v/$2/ i/OpenVMS MultiNet; protocol $1/ o/OpenVMS/
match ssh m|^SSH-([\d.]+)-ReflectionForSecureIT_([-\w_.]+)\r?\n| p/WRQ Reflection for Secure IT sshd/ v/$2/ i/protocol $1/

# SCS
match ssh m|^SSH-(\d[.\d]+)-SSH Protocol Compatible Server SCS (\d[-.\w]+)\r?\n| p/SCS NetScreen sshd/ v/$2/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-SSH Compatible Server\r?\n| p/SCS NetScreen sshd/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-([\d.]+) SSH Secure Shell Tru64 UNIX\r?\n| p/SCS sshd/ v/$2/ i/protocol $1/ o/Tru64 UNIX/
match ssh m/^SSH-([.\d]+)-(\d+\.\d+\.\d+) SSH Secure Shell/ p/SCS sshd/ v/$2/ i/protocol $1/
match ssh m|^sshd: SSH Secure Shell (\d[-.\w]+) on ([-.\w]+)\nSSH-(\d[.\d]+)-| p/SCS SSH Secure Shell/ v/$1/ i/on $2; protocol $3/
match ssh m|^sshd: SSH Secure Shell (\d[-.\w]+) \(([^\r\n\)]+)\) on ([-.\w]+)\nSSH-(\d[.\d]+)-| p/SCS sshd/ v/$1/ i/$2; on $3; protocol $4/
match ssh m|^sshd2\[\d+\]: .*\r\nSSH-(\d[\d.]+)-(\d[-.\w]+) SSH Secure Shell \(([^\r\n\)]+)\)\r?\n| p/SCS sshd/ v/$2/ i/protocol $1/
match ssh m/^SSH-([.\d]+)-(\d+\.\d+\.[-.\w]+)/ p/SCS sshd/ v/$2/ i/protocol $1/

# OpenSSH
match ssh m|^SSH-([\d.]+)-OpenSSH_([\w._-]+) Debian-(\S*maemo\S*)\r?\n| p/OpenSSH/ v/$2 Debian $1/ i/Nokia Maemo tablet; protocol $1/ o/Linux/
match ssh m|^SSH-([\d.]+)-OpenSSH_([\w._-]+)[ -]{1,2}Debian[ -_]([^\r\n]+)\r?\n| p/OpenSSH/ v/$2 Debian $3/ i/protocol $1/ o/Linux/
match ssh m|^SSH-([\d.]+)-OpenSSH_[\w.]+-FC-([\w.-]+)\.fc(\d+)\r\n| p/OpenSSH/ v/$2 Fedora/ i/Fedora Core $3; protocol $1/ o/Linux/
match ssh m|^SSH-([\d.]+)-OpenSSH_([\w._-]+) FreeBSD-([\d]+)\r?\n| p/OpenSSH/ v/$2/ i/FreeBSD $3; protocol $1/ o/FreeBSD/
match ssh m|^SSH-([\d.]+)-OpenSSH_([\w._-]+) FreeBSD localisations (\d+)\r?\n| p/OpenSSH/ v/$2/ i/FreeBSD $3; protocol $1/ o/FreeBSD/
match ssh m|^SSH-([\d.]+)-OpenSSH_([\w._-]+) FreeBSD-openssh-portable-([\w.,]+)\r?\n| p/OpenSSH/ v/$2/ i/protocol $1/ o/FreeBSD/
match ssh m|^SSH-([\d.]+)-OpenSSH_([\w._-]+) FreeBSD-openssh-portable-overwrite-base| p/OpenSSH/ v/$2/ i/protocol $1; overwrite base SSH/ o/FreeBSD/
match ssh m|^SSH-([\d.]+)-OpenSSH_([\w._-]+) FreeBSD-openssh-gssapi-| p/OpenSSH/ v/$2/ i/gssapi; protocol $1/ o/FreeBSD/
match ssh m|^SSH-([\d.]+)-OpenSSH_([\w._-]+) FreeBSD\n| p/OpenSSH/ v/$2/ i/protocol $1/ o/FreeBSD/
match ssh m|^SSH-([\d.]+)-OpenSSH_([\w._-]+) miniBSD-([\d]+)\r?\n| p/OpenSSH/ v/$2/ i/MiniBSD $3; protocol $1/ o/MiniBSD/
match ssh m|^SSH-([\d.]+)-OpenSSH_([\w._-]+) NetBSD_Secure_Shell-([\w._-]+)\r?\n| p/OpenSSH/ v/$2/ i/NetBSD $3; protocol $1/ o/NetBSD/
match ssh m|^SSH-([\d.]+)-OpenSSH_([\w.-]+)_Mikrotik_v([\d.]+)\r?\n| p/OpenSSH/ v/$2 mikrotik $3/ i/protocol $1/ d/router/
match ssh m|^SSH-([\d.]+)-OpenSSH_([\w._-]+) in RemotelyAnywhere ([\d.]+)\r?\n| p/OpenSSH/ v/$2/ i/RemotelyAnywhere $3; protocol $1/ o/Windows/
match ssh m|^SSH-([\d.]+)-OpenSSH_([\w._-]+)\+CAN-2004-0175\r?\n| p/OpenSSH/ v/$2+CAN-2004-0175/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-OpenSSH_([\w._-]+) NCSA_GSSAPI_20040818 KRB5\r?\n| p/OpenSSH/ v/$2 NCSA_GSSAPI_20040818 KRB5/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-OpenSSH_([\w.]+)-(hpn[\dv]+)\r?\n| p/OpenSSH/ v/$2-$3/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-OpenSSH_([\w.]+\+sftpfilecontrol-v[\d.]+-hpn\w+)\r?\n| p/OpenSSH/ v/$2/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-OpenSSH_([\w.]+-hpn) NCSA_GSSAPI_\d+ KRB5\r?\n| p/OpenSSH/ v/$2/ i/protocol $1; kerberos support/
match ssh m|^SSH-([\d.]+)-OpenSSH_3\.4\+p1\+gssapi\+OpenSSH_3\.7\.1buf_fix\+2006100301\r?\n| p/OpenSSH/ v/3.4p1 with CMU Andrew patches/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-OpenSSH_([\w.]+)\.RL\r?\n| p/OpenSSH/ v/$2.RL Allied Telesis/ i/protocol $1/ d/switch/
match ssh m|^SSH-([\d.]+)-OpenSSH_([\w.]+)-(CERN\d+)\r?\n| p/OpenSSH/ v/$2-$3/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-OpenSSH_([-\w.]+)\.cern-hpn| p/OpenSSH/ v/$2-cern-hpn/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-OpenSSH_([-\w.]+-hpn)\r?\n| p/OpenSSH/ v/$2/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-OpenSSH_([-\w.]+-pwexp\d+)\r?\n| p/OpenSSH/ v/$2/ i/protocol $1/ o/AIX/
match ssh m|^SSH-([\d.]+)-Nortel\r?\n| p/Nortel SSH/ d/switch/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-OpenSSH_([-\w_.]+) DragonFly-\d+\r?\n| p/OpenSSH/ v/$2/ i/protocol $1/ o/DragonFlyBSD/
match ssh m|^SSH-([\d.]+)-OpenSSH_([-\w_.]+) FIPS\n| p/OpenSSH/ v/$2/ i/protocol $1; Imperva SecureSphere firewall/ d/firewall/
match ssh m|^SSH-([\d.]+)-OpenSSH_([-\w_.]+) NCSA_GSSAPI_GPT_([-\w_.]+) GSI\n| p/OpenSSH/ v/$2/ i/protocol $1; NCSA GSSAPI authentication patch/

# Choose 1 of the following:
# 1) Match all OpenSSHs:
#match ssh m/^SSH-([.\d]+)-OpenSSH[_-]([\S ]+)/i p/OpenSSH/ v/$2/ i/protocol $1/
# 2) Don't match unknown SSHs (and generate fingerprints)
match ssh m/^SSH-([.\d]+)-OpenSSH[_-]([\w.]+)\r?\n/i p/OpenSSH/ v/$2/ i/protocol $1/

# These are strange ones. These routers pretend to be OpenSSH, but don't do it that well (see the \r):
match ssh m|^SSH-2\.0-OpenSSH\r?\n| p/Linksys WRT45G modified dropbear sshd/ i/protocol 2.0/ d/router/
match ssh m|^SSH-2\.0-OpenSSH_3\.6p1\r?\n| p|D-Link/Netgear DSL router modified dropbear sshd| i/protocol 2.0/ d/router/

match ssh m|^\0\0\0\$\0\0\0\0\x01\0\0\0\x1bNo host key is configured!\n\r!\"v| p/Foundry Networks switch sshd/ i/broken: No host key configured/
match ssh m|^SSH-(\d[\d.]+)-SSF-(\d[-.\w]+)\r?\n| p/SSF French SSH/ v/$2/ i/protocol $1/
match ssh m|^SSH-(\d[\d.]+)-lshd_(\d[-.\w]+) lsh - a free ssh\r\n\0\0| p/lshd secure shell/ v/$2/ i/protocol $1/
match ssh m|^SSH-(\d[\d.]+)-lshd-(\d[-.\w]+) lsh - a GNU ssh\r\n\0\0| p/lshd secure shell/ v/$2/ i/protocol $1/
match ssh m/^SSH-([.\d]+)-Sun_SSH_(\S+)/ p/SunSSH/ v/$2/ i/protocol $1/
match ssh m/^SSH-([.\d]+)-meow roototkt by rebel/ p/meow SSH ROOTKIT/ i/protocol $1/
# Akamai hosted systems tend to run this - found on www.microsoft.com
match ssh m|^SSH-(\d[.\d]*)-(AKAMAI-I*)\r?\n$| p/Akamai SSH/ v/$2/ i/protocol $1/
match ssh m|^SSH-(\d[.\d]*)-(Server-V)\r?\n$| p/Akamai SSH/ v/$2/ i/protocol $1/
match ssh m|^SSH-(\d[.\d]*)-(Server-VI)\r?\n$| p/Akamai SSH/ v/$2/ i/protocol $1/
match ssh m|^SSH-(\d[.\d]*)-(Server-VII)\r?\n| p/Akamai SSH/ v/$2/ i/protocol $1/
match ssh m|^SSH-(\d[.\d]+)-Cisco-(\d[.\d]+)\r?\n$| p/Cisco SSH/ v/$2/ i/protocol $1/ o/IOS/
match ssh m|^SSH-(\d[.\d]+)-CiscoIOS_([\d.]+)XA\r?\n| p/Cisco SSH/ v/$2/ i/protocol $1; Chinese IOS XA/ o/IOS/
match ssh m|^\r\nDestination server does not have Ssh activated\.\r\nContact Cisco Systems, Inc to purchase a\r\nlicense key to activate Ssh\.\r\n| p/Cisco CSS SSH/ i/Unlicensed/
match ssh m|^SSH-(\d[.\d]+)-VShell_(\d[._\d]+) VShell\r?\n$| p/VanDyke VShell sshd/ v/$SUBST(2,"_",".")/ i/protocol $1/
match ssh m|^SSH-2\.0-0\.0 \r?\n| p/VanDyke VShell sshd/ i/version info hidden; protocol 2.0/
match ssh m|^SSH-([\d.]+)-([\w.]+) VShell\r?\n| p/VanDyke VShell/ v/$2/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-([\w.]+) \(beta\) VShell\r?\n| p/VanDyke VShell/ v/$2 beta/ i/protocol $1/
match ssh m/^SSH-([.\d]+)-(\d[-.\w]+) sshlib: WinSSHD (\d[-.\w]+)\r?\n/ p/Bitvise WinSSHD/ v/$3/ i/sshlib $2; protocol $1/ o/Windows/
match ssh m/^SSH-([.\d]+)-(\d[-.\w]+) sshlib: WinSSHD\r?\n/ p/Bitvise WinSSHD/ i/sshlib $2; protocol $1; server version hidden/ o/Windows/
match ssh m|^SSH-([.\d]+)-([\w._-]+) sshlib: sshlibSrSshServer ([\w._-]+)\r\n| p/SrSshServer/ i/sshlib $2; protocol $1/ v/$3/
match ssh m|^SSH-([\d.]+)-([\w._-]+) sshlib: GlobalScape\r?\n| p/GlobalScape CuteFTP sshd/ i/sshlib $2; protocol $1/ o/Windows/
match ssh m|^SSH-([\d.]+)-([\w._-]+) sshlib: EdmzSshDaemon ([\w._-]+)\r\n| p/EdmzSshDaemon/ v/$3/ i/sshlib $2; protocol $1/
match ssh m|^SSH-([.\d]+)-([\w._-]+) FlowSsh: WinSSHD ([\w._-]+)\r\n| p/Bitvise WinSSHD/ i/FlowSsh $2; protocol $1/ v/$3/ o/Windows/
match ssh m|^SSH-([.\d]+)-([\w._-]+) FlowSsh: WinSSHD ([\w._-]+): free only for personal non-commercial use\r\n| p/Bitvise WinSSHD/ i/FlowSsh $2; protocol $1; non-commercial use/ v/$3/ o/Windows/
match ssh m|^SSH-([.\d]+)-([\w._-]+) FlowSsh: WinSSHD: free only for personal non-commercial use\r\n| p/Bitvise WinSSHD/ i/FlowSsh $2; protocol $1; non-commercial use/ o/Windows/
# Cisco VPN 3000 Concentrator
# Cisco VPN Concentrator 3005 - Cisco Systems, Inc./VPN 3000 Concentrator Version 4.0.1.B Jun 20 2003
match ssh m/^SSH-([.\d]+)-OpenSSH\r?\n$/ p/OpenSSH/ i/protocol $1/ d/terminal server/
match ssh m|^SSH-1\.5-X\r?\n| p/Cisco VPN Concentrator SSHd/ i/protocol 1.5/ d/terminal server/
match ssh m|^SSH-([\d.]+)-NetScreen\r?\n| p/NetScreen sshd/ i/protocol $1/ d/firewall/
match ssh m|^SSH-1\.5-FucKiT RootKit by Cyrax\r?\n| p/FucKiT RootKit sshd/ i/**BACKDOOR** protocol 1.5/ o/Linux/
match ssh m|^SSH-2\.0-dropbear_([-\w.]+)\r?\n| p/Dropbear sshd/ v/$1/ i/protocol 2.0/ o/Linux/
match ssh m|^Access to service sshd from [-\w_.]+@[-\w_.]+ has been denied\.\r\n| p/libwrap'd OpenSSH/ i/Access denied/
match ssh m|^SSH-([\d.]+)-FortiSSH_([\d.]+)\r?\n| p/FortiSSH/ v/$2/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-cryptlib\r?\n| p/APC AOS cryptlib sshd/ i/protocol $1/ o/AOS/
match ssh m/^SSH-([.\d]+)-([.\d]+) Radware\r?\n$/ p/Radware Linkproof SSH/ v/$2/ i/protocol $1/ d/terminal server/
match ssh m|^SSH-2\.0-1\.0 Radware SSH \r?\n| p/Radware sshd/ i|protocol 2.0| d/firewall/
match ssh m|^SSH-([\d.]+)-Radware_([\d.]+)\r?\n| p/Radware sshd/ v/$2/ i/protocol $1/ d/firewall/
match ssh m|^SSH-1\.5-By-ICE_4_All \( Hackers Not Allowed! \)\r?\n| p/ICE_4_All backdoor sshd/ i/**BACKDOOR** protocol 1.5/
match ssh m|^SSH-2\.0-mpSSH_([\d.]+)\r?\n| p/HP Integrated Lights-Out mpSSH/ v/$1/ i/protocol 2.0/
match ssh m|^SSH-2\.0-Unknown\r?\n| p/Allot Netenforcer OpenSSH/ i/protocol 2.0/
match ssh m|^SSH-2\.0-FrSAR ([\d.]+) TRUEX COMPT 32/64\r?\n| p/FrSAR truex compt sshd/ v/$1/ i/protocol 2.0/
match ssh m|^SSH-2\.0-(\d{8,12})\r?\n| p/Netpilot config access/ v/$1/ i/protocol 2.0/
match ssh m|^SSH-([\d.]+)-RomCliSecure_([\d.]+)\r?\n| p/Adtran Netvanta RomCliSecure sshd/ v/$2/ i/protocol $1/
match ssh m|^SSH-2\.0-APSSH_([\w.]+)\r?\n| p/APSSHd/ v/$1/ i/protocol 2.0/
match ssh m|^SSH-2\.0-Twisted\r?\n| p/Kojoney SSH honeypot/ i/protocol 2.0/
match ssh m|^SSH-([\d.]+)-OpenSSH_([\w.]+)\r?\n.*aes256|s p/Kojoney SSH honeypot/ i/Pretending to be $2; protocol $1/
match ssh m|^SSH-2\.0-Mocana SSH \r?\n| p/Mocanada embedded SSH/ i/protocol 2.0/
match ssh m|^SSH-1\.99-InteropSecShell_([\d.]+)\r?\n| p/InteropSystems SSH/ v/$1/ i/protocol 1.99/ o/Windows/
match ssh m|^SSH-2\.0-WeOnlyDo(-wodFTPD)? ([\d.]+)\r?\n| p/WeOnlyDo sshd/ v/$2/ i/protocol 2.0/ o/Windows/
match ssh m|^SSH-2\.0-WeOnlyDo-([\d.]+)\r?\n| p/WeOnlyDo sshd/ v/$1/ i/protocol 2.0/ o/Windows/
match ssh m|^SSH-2\.0-PGP\r?\n| p/PHP Universal sshd/ i/protocol 2.0/
match ssh m|^SSH-([\d.]+)-libssh-([-\w.]+)\r?\n| p/libssh/ v/$2/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-HUAWEI-VRP([\d.]+)\r?\n| p/Huawei VRP sshd/ v/$2/ i/protocol $1/ o/VRP/ d/router/
match ssh m|^SSH-([\d.]+)-VRP-([\d.]+)\r?\n| p/Huawei VRP sshd/ v/$2/ i/protocol $1/ o/VRP/ d/router/
match ssh m|^SSH-([\d.]+)-lancom\r?\n| p/lancom sshd/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-xxxxxxx\r?\n| p|Fortinet VPN/firewall sshd| i/protocol $1/ d/firewall/
match ssh m|^SSH-([\d.]+)-AOS_SSH\r?\n| p/AOS sshd/ i/protocol $1/ o/AOS/
match ssh m|^SSH-([\d.]+)-RedlineNetworksSSH_([\d.]+) Derived_From_OpenSSH-([\d.])+\r?\n| p/RedLineNetworks sshd/ v/$2/ i/Derived from OpenSSH $3; protocol $1/
match ssh m|^SSH-([\d.]+)-DLink Corp\. SSH server ver ([\d.]+)\r?\n| p/D-Link sshd/ v/$2/ i/protocol $1/ d/router/
match ssh m|^SSH-([\d.]+)-FreSSH\.([\d.]+)\r?\n| p/FreSSH/ v/$2/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-Neteyes-C-Series_([\d.]+)\r?\n| p/Neteyes C Series load balancer sshd/ v/$2/ i/protocol $1/ d/load balancer/
match ssh m|^SSH-([\d.]+)-IPSSH-([\d.]+)\r?\n| p|Cisco/3com IPSSHd| v/$2/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-DigiSSH_([\d.]+)\r?\n| p/Digi CM sshd/ v/$2/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-0 Tasman Networks Inc\.\r?\n| p/Tasman router sshd/ i/protocol $1/ d/router/
match ssh m|^SSH-([\d.]+)-([\w.]+)rad\r?\n| p/Rad Java SFTPd/ v/$2/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-OpenSSH_([\d.]+) in DesktopAuthority ([\d.]+)\r?\n| p/DesktopAuthority OpenSSH/ v/$2/ i/DesktopAuthority $3; protocol $1/ o/Windows/
match ssh m|^SSH-([\d.]+)-NOS-SSH_([\d.]+)\r?\n| p/3Com WX2200 or WX4400 NOS sshd/ v/$2/ i/protocol $1/ d/WAP/
match ssh m|^SSH-1\.5-SSH\.0\.1\r?\n| p/Dell PowerConnect sshd/ i/protocol 1.5/ d/power-device/
match ssh m|^SSH-([\d.]+)-Ingrian_SSH\r?\n| p/Ingrian SSH/ i/protocol $1/ d/security-misc/
match ssh m|^SSH-([\d.]+)-PSFTPd PE\. Secure FTP Server ready\r?\n| p/PSFTPd sshd/ i/protocol $1/ o/Windows/
match ssh m|^SSH-([\d.]+)-BlueArcSSH_([\d.]+)\r?\n| p/BlueArc sshd/ v/$2/ i/protocol $1/ d/storage-misc/
match ssh m|^SSH-([.\d]+)-Zyxel SSH server\r?\n| p/ZyXEL ZyWALL sshd/ o/ZyNOS/ d/security-misc/ i/protocol $1/
match ssh m|^SSH-([.\d]+)-paramiko_([\w._-]+)\r?\n| p/Paramiko Python sshd/ v/$2/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-USHA SSHv([\w._-]+)\r?\n| p/USHA SSH/ v/$2/ i/protocol $1/ d/power-device/
match ssh m|^SSH-2\.0-SSH_0\.2\r?\n$| p/3com WAP sshd/ d/WAP/ v/0.2/ i/protocol 2.0/
match ssh m|^SSH-([\d.]+)-CoreFTP-([\w._-]+)\r?\n| p/CoreFTP sshd/ v/$2/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-RomSShell_([\w._-]+)\r\n| p/AllegroSoft RomSShell sshd/ v/$2/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-IFT SSH server BUILD_VER\n| p/Sun StorEdge 3511 sshd/ i/IFT SSH/ d/storage-misc/
match ssh m|^Could not load host key\. Closing connection\.\.\.$| p/Cisco switch sshd/ i/misconfigured/ o/IOS/ d/switch/
match ssh m|^SSH-([\d.]+)-WS_FTP-SSH_([\w._-]+)\r\n| p/WS_FTP sshd/ i/protocol $1/ v/$2/ o/Windows/
match ssh m|^SSH-([\d.]+)-http://www\.sshtools\.com J2SSH \[SERVER\]\r\n| p/SSHTools J2SSH/ i/protocol $1/
match ssh m|^SSH-([\d.]+)-DraySSH_([\w._-]+)\n\n\rNo connection is available now\. Try again later!$| p/DrayTek Vigor 2820 ADSL router sshd/ v/$2/ i/protocol $1/ d/broadband router/
match ssh m|^SSH-([\d.]+)-Pragma FortressSSH ([\d.]+)\n| p/Pragma FortessSSH/ v/$2/ i/protocol $1/ o/Windows/
match ssh m|^SSH-([\d.]+)-SysaxSSH_([\d.]+)\r\n| p/Sysax Multi Server sshd/ v/$2/ i/protocol $1/ o/Windows/
match ssh m|^SSH-2\.0-1\.00\r\n$| p/Cisco IP Phone CP-7900G-series sshd/ d/VoIP phone/
match ssh m|^SSH-([\d.]+)-Foxit-WAC-Server-([\d.]+ Build \d+)\n| p/Foxit WAC Server sshd/ v/$2/ i/protocol $1/ o/Windows/
match ssh m|^SSH-([\d.]+)-ROSSSH\r\n| p/MikroTik RouterOS sshd/ i/protocol $1/ o/Linux/ d/router/
match ssh m|^SSH-([\d.]+)-3Com OS-([\w._-]+ Release \w+)\n| p/3Com switch sshd/ d/switch/ v/$2/ i/protocol $1/
match ssh m|^SSH-2\.0-XXXX\r\n| p/Cyberoam firewall sshd/ d/firewall/
match ssh m|^SSH-2\.0-Tc6l51-sD1m-m_\n| p/Fortinet FortiWifi 60C firewall sshd/ d/firewall/

softmatch ssh m/^SSH-([.\d]+)-/ i/protocol $1/


match soldat m|^Soldat Admin Connection Established\.\.\.\r\nAdmin connected\.\r\n| p/Soldat multiplayer-game server/
match solproxy m|^The solproxy is used by [\d.]+\n\rThe client is closed!\n\r| p/Dell Serial Over LAN proxy/

match synchroedit m|^SynchroEdit ([\d.]+) running on ([\w._-]+)\n$| p/SynchroEdit request server/ v/$1/ h/$1/

match teamspeak m|^TS3\n\r$| p/TeamSpeak voice communication/ v/3/
match teamspeak m|^TS3\n\rWelcome to the TeamSpeak 3 ServerQuery interface, type \"help\" for a list of commands and \"help <command>\" for information on a specific command\.\n\r$| p/TeamSpeak voice communication/ v/3/

match teamviewer m|^\x17\x24\x0a\x20\x00....\x08\x13\x80\0\0\0\0\0\x01\0\0\0\x11\x80\0\0\0\0\0\0\0\0\0\0\0\0\0\0$| p/TeamViewer/
match teamviewer m|^\x17\x24\x0a\x20\x00....\x88\x13\x80\0\0\0\0\0\x01\0\0\0\x11\x80\0\0\0\0\0\0\0\0\0\0\0\0\0\0$| p/TeamViewer/ v/5/
match teamviewer m|^\x17\x24\x0a\x20\x00....\xe8\x42\0\0\0\0\0\0\x01\0\0\0\x10\x80\0\0\0\0\0\0\0\0\0\0\0\0\0\0$| p/TeamViewer/
match teamviewer m|^\x17\x24\x0a\x20\x00....\x68\x42\0\0\0\0\0\0\x01\0\0\0\x11\x80\0\0\0\0\0\0\0\0\0\0\0\0\0\0$| p/TeamViewer/

# BEEP/ANTP protocol uses RPY (reply) much like HTTP
# See http://www.ietf.org/rfc/rfc3080.txt
# and http://simp.mitre.org/drafts/antp.html
# for details
match beep m|^RPY \d \d \. \d \d+\r\nContent-Type: application/beep\+xml\r\n\r\n<greeting><profile uri=\"http://www\.codingmonkeys\.de/BEEP/SubEthaEditHandshake\"| p/SubEthaEdit collaborative text editor/ o/Mac OS X/
match beep m|^RPY \d \d \. \d \d+\r\nContent-Type: application/beep\+xml\r\n\r\n<greeting.<profile uri=\"http://www\.apple\.com/beep/GSS\"/>.*/beep/xgrid/controller/|s p/Apple Xgrid Controller/ d/specialized/ o/Mac OS X/
softmatch beep m|^RPY \d \d \. \d \d+\r\nContent-Type: application/beep\+xml\r\n|

match kvm m|^\0\0\0\x0bSynergy\0\x01\0| p/Synergy KVM/
match kvm m|^\0\0\0\x0b<CSC/>\0| p/Raritan KVM/
match kvm m|^LFB 1\.0[56]$| p/IBM BladeCenter KVM/

match syncsort-nibbler m|^\x80\0\0\$\0\0\0\x01I\xae\xeb\xc1\0\0\0\0\0\0\x05\x02\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\x04\0\0\0\"$| p/Syncsort Backup Express nibbler/

# Redhat Linux 7.1 - HAHAHAHAHAHA!!!! I love this service :) 
match systat m|^USER       PID %CPU %MEM   VSZ  RSS TTY      STAT START   TIME COMMAND\n| p/Linux systat/ o/Linux/
match systat m|^  PID  PGRP SID PRI STATE   BLK  SIZE COMMAND\n| p/QNX systat/ o/QNX/

match tcpwrapped m|^You are not welcome to use (\w+) from [\w._-]+\.\n$| p/BSD TCP Wrappers/ i/$1/

match tdm m|^\x01\0\0\0\x03$| p/Turbine Download Manager/

match teamtalk m|^welcome userid=\d+ servername=\"([^"]+)\" motd=\"\" forwarding=\d+ channels=\d+ operators=\d+ maxusers=\d+ protocol=\"([\d.]+)\"\r\n| p/Bearware TeamTalk/ i/Server Name $1; protocol $2/

# Cisco router running IOS 12.1.5-12.2.13a
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f$| p/Cisco router/ d/router/ o/IOS/
# Draytek Vigor 2600 aDSL router
match telnet m|^\xff\xfd\x18\xff\xfb\x01\n\r\n\rPassword: | p/Draytek Vigor ADSL router telnetd/  d/broadband router/
# IBM Infoprint 12 printer with JetDirect
match telnet m|^\xff\xfc\x01\r\nPlease type \[Return\] two times, to initialize telnet configuration\r\nFor HELP type \"\?\"\r\n> | p/HP JetDirect printer telnetd/ d/printer/
# HP JetDirect 300X print server
match telnet m|^\xff\xfc\x01\r\nHP JetDirect\r\n\r\nPassword:$| p/HP JetDirect printer telnetd/ d/printer/
# IBM High Performace Switch - Model 8275-416, Software version 1.1, Manufacturer IBM068
match telnet m|^\x1b\[1;1H\x1b\[2J\x1b\[8;38H\x1b\[1;1H\x1b\[2;1H\(C\) Copyright IBM Corp\. 1999\x1b\[3;1HAll Rights Reserved\.| p/IBM switch telnetd/
match telnet m|^\x1b\[H\x1b\[2JYou have connected to a FirstClass System\. Please login\.\.\.\r\nUserID: | p/FirstClass messaging system telnetd/
# Cisco Catalyst management console
# 3Com 3Com SuperStack II Switch 3300
match telnet m|^\xff\xfd\x03\xff\xfb\x03\xff\xfb\x01| i|Usually a Cisco/3com switch| d|switch| o/IOS/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\nSun\(tm\) Advanced Lights Out Manager (\d[-.\w]+) \(v(\d+)\)\r\n\r\nPlease login: | p/Sun Advanced Lights Out Manager/ v/$1/ i/on Sun v$2; for remote system control/ d/remote management/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\nCopyright \d+ Sun Microsystems, Inc\.  All rights reserved\.\r\nUse is subject to license terms\.\r\n\r\n\r\nSun\(tm\) Advanced Lights Out Manager ([\d.]+) \(([\w._-]+)\)\r\n\r\nPlease login: | p/Sun Advanced Lights Out Manager telnetd/ v/$1/ o/Solaris/ h/$2/ d/remote management/
# Epson Stylus Color 900N telnet
match telnet m|^\xff\xfb\x01\xff\xfb\x01Connected to [-/.+\w]+!\r\n\r\nPassword: | p/Epson printer telnetd/ d/printer/
# This one may not technically be considered telnet protocol, but you seem to use it via telnet
match telnet m|^220 SL4NT viewer service ready\r\n250 Currently connected channels: | p/Netal SLANT viewer/
match telnet m|^\xff\xfb\x03\xff\xfb\0\xff\xfb\0\xff\xfd\0\xff.*\r\rFrontDoor (\d[-.\w]+)/|s p/FrontDoor FIDONet Mailer telnetd/ v/$1/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\nOK\r\n$| p/Motorola Vanguard router telnetd/ d/router/
match telnet m|^\xff\xfb\x03\xff\xfd\x03\xff\xfc\x06.*\nPrecidia Technologies\r\n([-.+\w]+) Remote Configuration\r\n\nPassword\? |s p/Precidia serial2ethernet gateway telnetd/ i/model $1/
match telnet m|^\xff\xfb\x01\n\r.*Welcome to the Xylan PizzaSwitch! Version (\d[-.\w]+)\n\rlogin   : |s p/Xylan PizzaSwitch telnetd/ v/$1/ d/switch/
# Bay Networks Accelar 1100 (version 2.0.5.5) switch
match telnet m|^\xff\xfb\x01\r\n\r\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\n\r\r\* Bay Networks,Inc\..*(Accelar [-.+\w]+).*Software Release (\d[-.\w]+) |s p/Bay Networks Accelar switch telnetd/ v/$2/ i/$1/ d/switch/
match telnet m|^\xff\xfb\x01\r\n\r\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\n\r\r\* Nortel Networks,Inc\..*\n\r\r\* Passport ([-.\w]+) .*\r\* Software Release (\d[-.\w]+) |s p/Nortel Networks Passport switch telnetd/ v/$2/ i/Passport $1/ d/switch/
# NCD Thinstar 300 running NCD Software 2.31 build 6
match telnet m|^\xff\xfb\x03\xff\xfd\x03\xff\xfb\x01WinCE/WBT Command Shell Version (\d[-.\w]+)\r\nSerial Number: (\w+)  MAC Address: 0000(\w+)\r\nUUID: [-\w]+\r\nPassword: | p/NCD Thinster terminal command shell/ v/$1/ i/Serial# $2; MAC $3/ d/terminal/
# Netopia 4542 aDSL router telnetd
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\x1b\[2J\x1b\[Hname:| p/Netopia ADSL router telnetd/ d/broadband router/
match telnet m|^\xff\xfb\x01\n\r-> \x08\x08\x08\x08        \*\*\*  EPSON Network Scanner Server \((.*)\)  \*\*\*\n\r\n\r\x08\x08\x08\x08        \n\r| p/Epson Network Scanner Server/ i/$1/

# NetportExpress PRO/100 3 port print server
match telnet m|^\xff\xfb\x01\r\nNetportExpress\(tm\) ([-/.+\w]+)\r\n.*\r\n\r\nlogin: | p/Intel NetportExpress print server telnetd/ i/Model $1/ d/print server/
# 3Com OfficeConnect 812 Router telnetd
match telnet m|^login: \xff\xfd\x03\xff\xfb\x03\xff\xfb\x01| p/3Com OfficeConnect router telnetd/ d/router/
# Nortel Networks Instant Internet 100
match telnet m|^\xff\xfb\x01\r\npassword: | p/Nortel Networks Instant Internet broadband router telnetd/ d/broadband router/
# Network Appliance ONTAP 6.3.3 telnet
match telnet m|^\xff\xfb\x01\xff\xfd\x18\xff\xfd#| p/Network Appliance Ontap telnetd/
# Netgear RP114 broadband router or ZyXel P2302R VoIP adapter
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\nPassword: | p/Netgear broadband router or ZyXel VoIP adapter telnetd/
match telnet m|^\xff\xfd\x18\xff\xfb\x01\x1b\[2J\x1b\[\?7l\x1b.*HP ([-.\w]+) ProCurve Switch ([-.\w]+)\r\n\rFirmware revision ([-.\w]+)\r\n\r\r| p/HP ProCurve $2 Switch telnetd/ i/JetDirect $2; firmware: $3/ d/switch/
match telnet m|^\x1b\[20;1H\r\n\r\x1b\[\?25h\x1b\[20;11H\x1b\[21;1HSession Terminated, Connect again\r\n\r\x1b\[\?25h\x1b\[21;1H\xff\xfd\x18\xff\xfb\x01\x1b\[2J\x1b\[\?7l\x1b\[[34];23r\x1b\[\?6l\x1b\[1;1H\x1b\[\?25l\x1b\[1;1HHP (J\w+) ProCurve Switch ([-.\w]+)\r\n\rFirmware revision ([-.\w]+)\r\n\r\r| p/HP ProCurve $2 Switch telnetd/ i/JetDirect $2; firmware: $3/ d/switch/
match telnet m|^\xff\xfd\x18\xff\xfb\x01\x1b\[2J\x1b\[\?7l\x1b.*ProCurve ([\w._-]+) Switch ([\w._-]+)\r\r\nSoftware revision ([\w._-]+)\r\r\n|s p/HP ProCurve $1 $2 switch telnetd/ i/Firmware $3/ d/switch/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\r\n\r.*Procurve Wireless Access Point (\d+)\r\n|s p/HP ProCurve Access Point $1 WAP telnetd/ d/WAP/
match telnet m|^Check Point FireWall-1 Client Authentication Server running on [-.\w]+\r\n\r\xff\xfb\x01\xff\xfe\x01\xff\xfb\x03User: | p/Check Point FireWall-1 Client Authenticaton Server/
# Enterasys XP-8600 running E9.0.5.0
match telnet m|^\xff\xfb\x03\xff\xfd\x01\xff\xfd\x1f\xff\xfb\x05\xff\xfd!| p/Enterasys XSR Security Router telnetd/ d/router/
# Windows 2000 telnetd
match telnet m|^\xff\xfd%\xff\xfb\x01\xff\xfd\x03\xff\xfd\x1f\xff\xfd\0\xff\xfb\0$| p/Microsoft Windows 2000 telnetd/ o/Windows/
match telnet m|^\xff\xfd\x03\xff\xfb\x03\xff\xfd'\xff\xfd\x18\xff\xfb\0\xff\xfd\0\xff\xfb\x01\xff\xfe\x01GUI START\n| p/Microsoft Windows 2000 telnetd/ o/Windows/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd'\xff\xfd\x1f\xff\xfd\0\xff\xfb\0Welcome to Microsoft Telnet Service \r\n| p/Microsoft Windows 2000 telnetd/ o/Windows/
match telnet m#^\xff\xfb\x01\xff\xfd\x03\xff\xfd\x1f\xff\xfd\0\xff\xfb\0Microsoft \(R\) Windows (NT |)\(TM\) Version (\d[-.\w]+) \(Build (\d+)\)\r\nWelcome to Microsoft Telnet Service \r\nTelnet Server Build (\d[-.\w]+)\n\rlogin: # p/Microsoft Windows $1telnetd/ v/$4/ i/OS version $2 build $3/ o/Windows/
# Windows XP telnetd
match telnet m|^\xff\xfd%\xff\xfb\x01\xff\xfb\x03\xff\xfd'\xff\xfd\x1f\xff\xfd\0\xff\xfb\0| p/Microsoft Windows XP telnetd/ o/Windows XP/
match telnet m|^\r\nNo more connections are allowed to telnet server\. Please try again later\.\0| p/Microsoft Windows XP telnetd/ o/Windows XP/ i/no more connections allowed/
# IRIX 6.5.18f telnetd
match telnet m|^\xff\xfd\x18\xff\xfd \xff\xfd#\xff\xfd\$| p/IRIX telnetd/ v/6.X/ o/IRIX/
# OS 400 V4R4M0
# OS/400 V5R1M0
match telnet m|^\xff\xfd'\xff\xfd\x18$| p|IBM OS/400 telnetd| o|OS/400|
# JetDirect Model: J4169A Firmware: L.21.11
match telnet m|^\xff\xfb\x03\xff\xfb\x01\x07HP JetDirect\r\nPassword is not set\r\n| p/HP JetDirect printer telnetd/ i/No password/ d/printer/
# HP Jetdirect telnet with password protection
match telnet m|^\xff\xfb\x03\xff\xfb\x01\x07HP JetDirect\r\n\r\nEnter username: | p/HP JetDirect printer telnetd/ d/printer/
# HP MPE/iX 5.5 on HP 3000 telnet service
match telnet m|^\xff\xfd\x03\xff\xfb\x01\xff\xfd!| p|HP MPE/iX telnetd|
# Brother 1870N Printer
match telnet m|^\x1b\[2J\x1b\[1;1f\xff\xfb\x01\xff\xfb\x03\xff\xfd\x03| p|Brother/HP printer telnetd| d/printer/
# AIX 4.3.3.0
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\r\n\nIQinVision IQeye3 Version ([vV].*)\n\r\nType HELP| p/IQinVision IQeye3 telnetd/ v/version $1/ d/webcam/
match telnet m|^\xff\xfe%\xff\xfd\x18$| p/AIX telnetd/ o/AIX/
match telnet m|^\r\nEfficient ([-.\w ]+) Router \(([-.\d/]+)\) v(\d[-.\w]+) Ready\r\n\xff\xfb\x01\xff\xfb\x03\xff\xfd\x01\xff\xfe\x01Login: | p/Efficient router telnetd/ v/$3/ i/Model $1 - $2/ d/router/
# http://mldonkey.berlios.de/
# mldonkey-2.5-3 telnet port
match telnet m|^\xff\xfd\x1f\n\n\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\n\n                         Welcome to MLdonkey          \n| p/MLDonkey multi-network P2P admin port/
match telnet m|^\r\nRaptor Firewall Secure Gateway\.\r\n| p/Symantec Raptor firewall secure gateway telnetd/
match telnet m|^\r\nSynchronet BBS for Win32  Version (\d[-.\w]+)\r\n| p/Synchronet BBS/ v/$1/ i/on Win32/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\nlogin: $| p/Orinoco WAP telnetd/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\xff\xfb\x03\x1b\[1;1H\x1b\[2K\x1b\[2;1H\x1b\[2K\x1b\[3;1H\x1b.*Nortel Networks.*BayStack ([-.\w]+).*Versions: ([.: \w]+)|s p/Nortel Networks telnetd/ i/Baystack $1; Versions: $2/ d/switch/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\xff\xfb\x03\x1b\[1;1H\x1b\[2K\x1b\[2;1H\x1b\[2K\x1b\[3;1H\x1b.*BayStack ([-\w_.]+) .*HW:(\w+)  FW:V([\d.]+) SW:V([\d.]+)\x1b|s p/BayStack switch $1 telnetd/ v/HW:$2 FW:$3 SW:$4/ d/switch/
# ASCII art banner that says "BAYSTACK"
match telnet m|^\xff\xfb\x01\x1b\[2J\x1b\[58259456;1H\x1b\[0m\x1b\[1;1H \*\*\*\*\*      \*\*\*     \*     \*    \*\*\*\*\*   \*\*\*\*\*\*\*\*\*     \*\*\*       \*\*\*\*\*  \*      \*\x1b\[2;1H| p/BayStack switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\n\r\n.*Bay Networks (Bay[-.: \w]+)\n\r|s p/Bay Networks telnetd/ i/$1/
match telnet m/^Check Point FireWall-1 authenticated Telnet server running on/ p/Check Point Firewall-1 telnetd/
match telnet m/^\r\nSpeedStream ([^(\r\n]+) \(.*\) v(\S+) Ready\r\n\xff\xfb\x01\xff\xfb\x03\xff\xfd/ p/SpeedStream $1/ v/$2/
match telnet m|^\xff\xfb\x01\r\n\rType \"\?\" at the command prompt for a list of commands\.\n\r.*Command-> |s p/SpeedStream 5660 router telnetd/ d/router/
# Alcatel SpeedTouch 510 ADSL router - Admin Interface, version 4.0.2.0.0
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfb\x01\xff\xfb\x03Username : | p|Alcatel/Thomson SpeedTouch DSL router admin interface| d/broadband router/
match telnet m/^\r\nRaptor Firewall Secure Gateway\.\r\n\r\nAccess denied\.\r\n/ p/Symantec Raptor Firewall Secure Gateway telnetd/ i/Access Denied/
match telnet m/^\*\*\*\*\*\*\* System Image Boot \*\*\*\*\*\*\*\n\r\n\rVina Technologies (.*) \((\d[-.\w]+ build \d+)\)\n\r/ p/Vina Technologies $1 telnetd/ v/$2/
match telnet m/^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\x1b\[0m\x1b\[2J\x1b\[01;00H\r\0Gigalink ([-+ \w]+)/ p/Gigalink telnetd/ i/on $1/
match telnet m/^\xff\xfb\x03\xff\xfb.*D-Link.*Telnet Console.*Model\s+: ([-+\w]+)/s p/D-Link telnetd/ i/on $1/
match telnet m|^\xff\xfb\x01\x1b\[0m\x1b\[2J\x1b\[0m\x1b\[9;20HCopyright\(C\) 1995-99 D-Link Systems Inc\.\x1b\[13;30HUser Name\x1b\[14;30HPassword\x1b\[23;10HMAC Address:\x1b\[8;29H([-.\w]+) Console Program\x1b\[13;41H| p/D-Link switch telnetd/ i/D-Link $1/
match telnet m/^\xff\xfa\x18\x01\xff\xf0\xff\xfb\x01\xff\xfb\x03Ambit Cable Router\r\n\r\nLogin: / p/Ambit Cable Router telnetd/ d/broadband router/
match telnet m|^\xff\xfc\x01\r\nHP JetDirect\r\n\r\nPlease type \"?\" for HELP, or \"/\" for current settings\r\n> $| p/HP JetDirect telnetd/ d/printer/
match telnet m/^\n\rVina Technologies (.*) \((\d[-.\w]+ build \d+)\)/ p/Vina Technologies $1 telnetd/ v/$2/
match telnet m/^\xff\xfd\x03\xff\xfb\x03\xff\xfb\x01\x1b\[0m\x1b\[1;1H\x1b\[2J\rD\r           \n\r             (DES-.*) Command Line Interface\n\r\n/ p/D-Link $1 telnetd/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\r\n<< Command Line Interface V ([\w._-]+) >>\r\n\r\nUser: | p/D-Link DVG-series VoIP gateway telnetd/ v/$1/ d/VoIP adapter/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\x1b\[0m\x1b\[2J\x1b\[0m\x1b\[2J\x1b\[21;1H\x1b\[0m\*+\x1b\[22;1H\x1b\[0mMessage Area:\x1b\[24;1H\x1b\[7mCTRL\+R = Refresh +\x1b\[9;16H\x1b\[0mDES-3624 Stackable Fast Ethernet Switch Console Management\x1b| p/D-Link DES-3624 switch telnetd/ d/switch/

match telnet m/^\xff\xfb\x01\xff\xfb\x03\xff\xfc\x1f\n\r\n\rUser Access Verification\n\r\n\r\n\r\n\r\n\rShell version (\d\S+).*Maipu Communication Technology Co\./ p/Maipu Router/ i/shell v$1/ d/router/
match telnet m/^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x03\x1b.*Intel Corporation, ([-+. \w()]+)/s p/Intel telnetd/ i/on $1/
match telnet m|^\r\nFlowPoint/(.*) Ready\r\n.*\xff\xfb\x01\xff\xfb| p/Flowpoint telnet/ i/on $1/
match telnet m/Welcome to Tenor Multipath Switch Telnet Server.*Type: (\S+)/s p/Tenor telnetd/ v/$1/ i/on Multipath Switch/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x01\x0d\x0a\x0d\x0aCisco\x20Systems.*Console/Telnet Access of the ([-. \w]+) for Configuration Purposes|s p/Cisco $1 telnetd/
# Cisco 350 Series Wireless AP 11.05
match telnet m|^\xff\xfb\x01\n\r\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08                           \x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08\x08| p/Cisco WAP telnetd/ d/WAP/
# Cisco 678 DSL router
match telnet m|^\r\n\r\nUser Access Verification\r\nPassword:\xff\xfb\x01$| p/Cisco DSL router telnetd/ d/broadband router/
# Cisco 3640, 12406/PRP
match telnet m|^\r\n\r\nUser Access Verification\r\n\r\nUsername: | p/Cisco router telnetd/ d/router/
#  Cisco 2900 Catalyst switch, IOS 12.0(5)XU
# Cisco 3600 router running IOS 12.X
# Cisco 2600 IOS 12.0
match telnet m/^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f.*User Access Verification\r\n\r\n(Username|Password): $/s p/Cisco IOS telnetd/ d/switch/ o/IOS/
# Cisco Pix 501 PIX IOS 6.3(1) telnet
match telnet m/^\xff\xfb\x03\xff\xfb\x01\xff\xfb\x03\xff\xfb\x01.*\r\nUser Access Verification\r\n\r\nPassword: /s p/Cisco telnetd/ i/IOS 6.X/ o/IOS/ d/firewall/
match telnet m|^\xff\xfb\x01\r\r\nUser Access Verification\r\r\n\r\r\nUsername:| p/Cisco PIX 500 series telnetd/ d/firewall/ o/IOS/
# Cisco Catalyst 6509 - WS-C6509 Software, Version NmpSW: 5.5(1)
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x01\r\n\r\nCisco Systems Console\r\n| p/Cisco Catalyst switch telnetd/ d/switch/ o/IOS/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\n\r\nPassword required, but none set\r\n| p/Cisco router telnetd/ i/password required but not set/ d/router/
match telnet m|^Access not permitted\. Closing connection\.\.\.\n$|s p/Cisco catalyst switch telnetd/ i/access denied/ d/switch/
# The match below matches Cisco microswitch devices and also Edge-core ES3526XA
match telnet m|^\xff\xfd\x18$| p|Cisco or Edge-core switch telnetd| d/switch/
# OpenBSD 2.3
# FreeBSD 5.1
match telnet m|^\xff\xfd%$| p/BSD-derived telnetd/
# Solaris 9
match telnet m|^\xff\xfd\x18\xff\xfd\x1f\xff\xfd#\xff\xfd'\xff\xfd\$$| p/Sun Solaris telnetd/ o/Solaris/
# Redhat Linux 7.3 telnet
match telnet m|\xff\xfd\x18\xff\xfd \xff\xfd#\xff\xfd'$| p/Linux telnetd/ o/Linux/
match telnet m|^\xff\xfb\x01\n\rUser Name : $| p/APC network management card telnetd/ d/power-device/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x03\n\rUser Name : | p|APC telnetd| i|Power/UPS device| d|power-device|
# G-Net BB0060 ADSL Modem
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\n\r                         \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\n\r.*GlobespanVirata Inc\., Software Release ([-.\w]+)\n\r|s p/GlobespanVirata telnetd/ v/$1/ d/broadband router/
# HP-UX B.11.00 A
match telnet m|^\xff\xfd\$$| p/HP-UX telnetd/ o/HP-UX/
# Cayman-DSL Model 3220-H, DMT-ADSL (Alcatel) OS version 6.3.0
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfe\x01\n\rlogin: $| p/Cayman-DSL router telnetd/ d/broadband router/
# Blue Coat Port 80 Security Appliance  Model: Blue Coat SG400  Software Version: SGOS 2.1.6044 Software Release id: 19480 Service Pack 4
# Maybe I should call this SGOS telnetd instead
match telnet m|^\xff\xfb\x03\xff\xfb\x01\xff\xfd\x1f\r\n\r\nUsername: $| p/Blue Coat telnetd/ o/SGOS/
match telnet m|^\xff\xfb\x01@ Userid: | p/Shiva LanRover telnetd/
# Netscreen ScreenOS 4.0.1r1.0 telnetd on a netscreen 5XT running firmware 4.0.1r1.0
match telnet m|^\xff\xfd\x18\xff\xfb\x01(\xff\xfe\x01)?(\xff.\x03)?[\w ]*Remote Management Console\r\n(\r\n)?login: $| p/Netscreen ScreenOS telnetd/ d/firewall/
# Note that openwall telnetd is derived from OpenBSD telnetd
match telnet m|^\xff\xfd\x18\xff\xfd \xff\xfd#\xff\xfd'\xff\xfd\$$| p|Openwall GNU/*/Linux telnetd| o|Linux|
match telnet m|^\xff\xfc\x01\r\nHP JetDirect\r\n\r\nPlease type \"\?\" for HELP, or \"/\" for current settings\r\n> $| p/HP Jet Direct printer telnetd/ d/printer/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\nAXIS (\S+) TELNET| p/AXIS Webcam/ v/$1/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\n\r\nTelebit\'s NetBlazer Version (\S+)\r\n| p/Telebit NetBlazer/ v/$1/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x03.*?FORE\x20Systems,\x20FORE\x20ES-2810.*?Version (\d[\d\.-]+)| p/FORE Systems ES-2810/ v/$1/
match telnet m|^\xff\xfb\x03\xff\xfb\x01.*ForeRunner ES-3810.*Enter Username: | p/FORE Systems ES-3810/
match telnet m|^\xff\xfb\x01\r\nCopyright \(C\) 1999 by  Extreme Networks\r\r\n| p/Extreme Networks telnetd/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03.*?ES-1000\x20Fast\x20Ethernet\x20Switch\x20Console| p/Marconi ES-1000/
match telnet m|^\xff\xfb\x01login:\x20$| p/telnet/ i/generic/
match telnet m|^\xff\xfb\x01\xff\xfd\x01\xff\xfb\x03\xff\xfd\x03\xff\xfb\x05\xff\xfd\x05Welcome to ([-\w_]+) Debug Terminal - \d*\n\r\n\r\n\rlogin:| p/HP StorageWorks SSL1016 tape autoloader telnetd/ i/Name: $1/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\r\n\r\nWelcome to Print Server\r\n\r\nPS>| p|Generic print server telnetd| d/print server/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n\n\*+\r\n\*  Welcome to Print Server  \*\r\n\*     Telnet Console +\*\r\n\*+\r\n\r\nServer Name    :  ([-\w_.]+)\0\0\0\0\0\0\0\0\r\nServer Model   :  USB Print Server\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\r\nF/W Version    :  ([\d.]+)  \0\0\0\0\r\nMAC Address    :  ([\w ]+)\r\nUptime         :  ([^\r\n]+)\r\n| p/TRENDnet TE4100-PS1U telnetd/ v/$2/ h/$1/ i/MAC: $3; Uptime $4/ d/print server/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n\r\n\*+\r\n\*  Welcome to TRENDnet Print Server  \*\r\n\*          Telnet Console            \*\r\n\*+\r\n\r\nServer Name    : *([\w._-]+) *\0\0\0\0\0\0\r\nServer Model   : *([\w._-]+) *\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\r\nF/W Version    : *([\w._-]+) *\0\0\0\0\r\nMAC Address    : *([0-9A-F ]+) *\r\nUptime         : *([^\r\n]*)\r\n\nPlease Enter Password: | p/TRENDnet $2 print server telnetd/ v/$3/ h/$1/ i/MAC: $4; Uptime $5/ d/print server/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n\n\*+\r\n\*  Welcome to Print Server  \*\r\n\*     Telnet Console        \*\r\n\*+\r\n\r\nServer Name    :  ([-\w_.]+)\r\nServer Model   :  Pocket Size Print Server\0\0\0\0\0\0\0\0\r\nF/W Version    :  ([\d.]+)  \0\0\0\0\r\nMAC Address    :  ([\w ]+)\r\nUptime         :  ([^\r\n]+)\r\n\nPlease Enter Password:| p/Lexmark W810 telnetd/ v/$2/ i/Name $1; MAC $3; Uptime $4/ d/printer/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n\n\*+\r\n\*  Welcome to Print Server  \*\r\n\*     Telnet Console        \*\r\n\*+\r\n\r\nServer Name    :  ([-\w_.]+)\0*\r\nServer Model   :  3Port Print Server\0\0\0\0\0\0\0\0\0\0\0\0\0\0\r\nF/W Version    :  ([-\w_.]+)  \0*\r\nMAC Address    :  ([\w ]+)\r\nUptime         :  ([^\r\n]+)\r\n\nPlease Enter Password: | p/3Port print server telnetd/ h/$1/ v/$2/ i/MAC $3; Uptime $4/ d/print server/
match telnet m|^\x1b\[0m\x1b\[2J\x1b\[01;28HCONEXANT SYSTEMS, INC\.\x1b\[02;19H ACCESS RUNNER ADSL CONSOLE PORT\x1b\[24;01H>>>\x1b\[24;01HLOGON PASSWORD>\x1b\[02;53H3\.\d+\x1b\[24;17H\x1b\[24;17H\x1b\[24;17H\x1b\[24;17H| p/Conexant Access Runner adsl router telnetd/ d/router/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\n\r\nWelcome on (.*)\r\n\r\n\r\nUsername: | p/Cisco Router 2621 telnetd/ i/Banner: $1/
match telnet m|^\xff\xfb\x01\xff\xfd\x18\nTelnet Service on the PrintServer\n\n\rPassword: | p|Hawking/TRENDnet Print Server telnetd| d/print server/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\n\r\n Welcome to OpenVMS \(TM\) Alpha Operating System, Version V([\d.]+)    \r\n\r\n\rUsername: | p/OpenVMS telnetd/ i/OpenVMS $1/ o/OpenVMS/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x03\xff\xfd\x18\xff\xfd\x1f\xff\xfd \xff\xfd!\x07\r\n\r\n Welcome to OpenVMS \(TM\) Alpha Operating System, Version V([-\w_.]+)  \r\n\r\n\rUsername: | p/OpenVMS telnetd/ i/OpenVMS $1/ o/OpenVMS/
match telnet m|\xff\xfb\x01\xff\xfb\x03\r\n\r\n Welcome to OpenVMS Alpha OS, Version V[\d+.]+| p/OpenVMS telnetd/ i/OpenVMS $1/ o/OpenVMS/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x01\x1b\[0;37;40m\x1b\[2J\x1b\[0;37;40m\x1b\[1m\x1b\[5;27HVertical Horizon Stack Manager\x1b\[0;37;40m\x1b\[1m\x1b\[10;26HEnterasys Networks, Incorporated| p/Enterasys Vertical Horizon Manager/ d/switch/
match telnet m|^\xff\xfd\($| p|IBM OS/390 or SNA telnetd|
match telnet m|^\xff\xfb\r\nRemotelyAnywhere Telnet Server v([\d.]+)\r\n.*\r\n\r\n([-\w_. ]+) login\r\nuser name: | p/RemotelyAnywhere telnetd/ v/$1/ i/Name $2/ o/Windows/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x03\xff\xfd\x1f\xff\xfd\x18([^\r\n]+)\r\nRemotelyAnywhere Telnet Server ([\d.]+)\r\n.*\r\n\r\n([-\w_. ]+) login\r\nuser name: |s p/RemotelyAnywhere telnetd/ v/$2/ i/$1; Name $3/ o/Windows/
match telnet m|^\r\nVxWorks login: \xff\xfb\x01$| p/VxWorks telnetd/ o/VxWorks/
match telnet m|^\xff\xfb\x01\xff\xfd\x01\xff\xfb\x03\xff\xfd\x03\xff\xfb\x01\xff\xfd\x01\xff\xfb\x03\xff\xfd\x03\r\n\r\nSelect Access Level\r\n===================\r\n1 - Read-Only\r\n2 - Installer\r\n3 - Administrator\r\n13008 >>> | p/BreezeCOM telnetd/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\nExterior router [-\w_.]+\r\nType: Cisco 2651\r\nModule: E3/T3 interface\r\n\r\n| p/Cisco 2651 router telnetd/ o/IOS/ d/router/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\n[-\w_.]+>%| p/Cisco router telnetd/ o/IOS/ d/router/
match telnet m=^\xff\xfb\x01\r\n\r\n#\r\n\| ELSA, MicroLink Cable\r\n\| Ver\. ([\d.]+) / [\d.]+ \d\d:\d\d .*\r\n\| SN\.  \d+\r\n\| Copyright \(c\) ELSA AG, Aachen \(Germany\)\r\n\r\ncm2, Connection No\.: \d+ \(LAN\) \(read-only connection\)\r\n\r\nPassword:= p/ELSA Microlink Cable modem/ v/$1/ i/read-only connection/ d/router/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n\r\npassword: $| p/Cisco LocalDirector telnetd/ d/load balancer/
match telnet m|^\xff\xfb\x01\xff\xfb\0\xff\xfd\xfb\xff\xfd\x03\x1b\[H\x1b\[2JYou have connected to a FirstClass System\. Please login\.\.\.\r\nUserID: | p/FirstClass telnetd/
match telnet m|^\xff\xfd\x1f\xff\xfd\x18\xff\xfb\x01\xff\xfb\x03\nWelcome to GoodTech Telnet Server for Windows 95/98 \(V([\d.]+)\) \(Evaluation Copy\)\n\r\n\(C\) Copyright \d+-\d+ GoodTech Systems, Inc\.\n\r\n\nLogin username: | p/GoodTech telnetd/ v/$1/ o/Windows/
match telnet m|^Please wait \.\.\. Connecting \.\.\.| p/Java Object Oriented Telnet Talker/
match telnet m|^\xff\xfe\x01\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\xff\xfd\x18Georgia SoftWorks Telnet Server for Windows NT/2000/XP/2003 Ver\. ([\d.]+)\n\rEvaluation copy, \d+ users enabled\. Expiration date is \d+/\d+/\d+\.\n\r\n\rPlease wait\.\.\.\n\rUser \d+ of \d+\n\r\n\r\n\rlogin:| p/Georgia SoftWorks telnetd/ v/$1/ i/Evaluation copy/ o/Windows/
match telnet m|^\xff\xfe\x01\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\xff\xfd\x18Georgia SoftWorks Telnet Server for Windows NT/2000/XP Version ([\d.]+)\n\rYour evaluation copy of this product expired, disconnecting\.\.\.| p/Georgia SoftWorks telnetd/ v/$1/ i/Expired trial/ o/Windows/
match telnet m|^\xff\xfe\x01\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\xff\xfd\x18Georgia SoftWorks Telnet Server for Windows NT/2000/XP/2003 Ver\. ([\d.]+)\n\rRegistered copy, \d+ users enabled\.\n\r\n\rPlease wait\.\.\.\n\rUser \d+ of \d+\n\r\n\r\n\rlogin:| p/Georgia SoftWorks telnetd/ v/$1/ i/Registered version/ o/Windows/
match telnet m|^\xff\xfe\x01\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\xff\xfd\x18Georgia SoftWorks Telnet Server for Windows NT/2000/XP/2003/Vista Ver\. ([-\w_.]+)\n\r| p/Georgia SoftWorks telnetd/ o/Windows/ v/$1/
match telnet m|^\xff\xfe\x01\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\xff\xfd\x18Georgia SoftWorks Telnet Server for Windows NT/2000 Version ([\w._-]+)\n\rRegistered copy| p/Georgia SoftWorks telnetd/ v/$1/ i/Registered version/ o/Windows/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\r\n\r\n\t\tWelcome to X330WAN-2DS1\r\n\t\tSW version ([\d.]+)\r\n\r\n\r\nLogin: | p/Avaya X330WAN-2DS1 telnetd/ v/$1/ d/router/
match telnet m|^\x1b\[0m\x1b\[2J\x1b\[01;28HCONEXANT SYSTEMS, INC\.\x1b\[02;14HATU-R ACCESS RUNNER ADSL TERMINAL\x1b\[24;01HENTER CHOICE-->| p/Conexant ATU-R ADSL router telnetd/ d/router/
match telnet m=^\xff\xfb\x01\xff\xfb\x03\r\n\r\n#\r\n\| LANCOM L-54g Wireless\r\n\|= p/LANCOM L-54g Wireless router telnetd/ d/router/
match telnet m|^\xff\xfc\x01\r\nHP JetDirect\r\n\r\nPassword: | p/HP JetDirect telnetd/ d/printer/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x01\r\n\r\nCisco Systems, Inc\. Console\r\n\r\n\r\n\r\n\r\nEnter password: | p/Cisco Catalyst switch telnetd/ d/switch/ o/IOS/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x01\r\n\r\nCisco Systems, Inc\. Console\r\n\r\n\r\n\r\r\n\r\nUsername: | p/Cisco Catalyst switch telnetd/ d/switch/ o/IOS/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n\r\nComOS - Livingston PortMaster\r\n\r\nlogin: | p/Livingston Portmaster telnetd/ d/telecom-misc/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\n\r +\*+\n\r +Welcome to DSLink 200 U/E\n\r +\*+\n\r\n\rGlobespanVirata Inc\., Software Release VIK-([\w.]+)\n\r| p/DSLink 200 adsl modem telnetd/ v/Software version $1/ d/router/
match telnet m|^\xff\xfe\x01\xff\xfd\x03\xff\xfd\x18\xff\xfd\x1f\xff\xfd\0\xff\xfb\x03\xff\xfb\x01\xff\xfb\0This copy of the Ataman TCP Remote Logon Services is registered as licensed to:\r\n\t(.*)\r\n\r\nAccount Name: | p/Ataman TCP Remote Logon Service telnetd/ i/Registered to $1/ o/Windows/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x03\xff\xfd\x1f\xff\xfd\x18Windows NT Workstation ([\d.]+) \(build \d+\) Service Pack (\d+)\r\nRemotelyAnywhere Telnet Server ([\d.]+)\r\n| p/RemotelyAnywhere telnetd/ v/$3/ i/WinNT $1 SP$2/ o/Windows/
match telnet m|^\r\nSorry, Access to Telnet is Denied\.\r\n$| p/Motorola VT1000v VOIP Adapter telnetd/ i/Access denied/ d/VoIP adapter/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\n\r\n\[ORiNOCO-AP-(\d+)[-\d]*\]> Please enter password: | p/Orinoco AP-$1 telnetd/ d/router/
match telnet m|^\xff\xfb\xfd\xff\xfb\x01\n\r\n\rFabric OS \(tm\)  Release v([\w.]+)\n\r\n\r| p/Brocade SilkWorm switch telnetd/ i/Fabric OS $1/ d/switch/
match telnet m|^\xff\xfb\x05\xff\xfd\x1f\xff\xfd\x01\xff\xfb\x03Nortel Networks CVX Access Switch\r\nlogin: | p/Nortel CVS Access switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\n\r-> \x08\x08\x08\x08        \*\*\*  EPSON Network Print Server \(([^)]+)\)  \*\*\*\n\r\n\r\x08\x08\x08\x08        \n\rPassword: | p/EPSON Network print server telnetd/ v/$1/ d/print server/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\r\n\nLantronix MSS100 Version V([\d.]+)/\d+\(\d+\)\n\r\nType HELP at the 'Local_2> ' prompt for assistance\.\n\r\n\r\n\nUsername> | p/Lantronix MSS100 serial interface telnetd/ v/$1/ d/specialized/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\r\0\r\0\r\n\x07# \0| p/Lantronix MSS100 serial interface telnetd/ d/specialized/
match telnet m|^\xff\xfb\x01OPTIBASE MGW5100 COMMAND LINE INTERFACE\r\n| p/Optibase MGW5100 TV streaming device telnetd/ d/media device/ o/VxWorks/
match telnet m|^\r\n\0Videolan Server Administration System\0\r\n\r\n\0\xff\xfb\x01\xff\xfb\x03\xff\xfe\"Login: \0| p/VideoLAN Server telnetd/ d/media device/
match telnet m=^\xff\xfb\x01\r\n\r\n#\r\n\| ELSA LANCOM DSL/I-10 Office\r\n\| Ver\. ([\d.]+) / [\d.]+\r\n\| SN\.  (\d+)\r\n= p/Elsa DSL I-10 router telnetd/ v/$1/ i/SN $2/ d/router/
match telnet m|^PC Telnetd ([\d.]+)\r\n\r\nlogin: | p/PC Telnetd/ v/$1/ o/Windows/
match telnet m|^\r\n>>> DECT@NET D&T Agent <<<\r\n\r\nlocal> | p/Philips DECT D&T Agent telnetd/
match telnet m=^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\x1b\[H\x1b\[2J\x1b\[0m\x1b\[0m\x1b\[0m\x1b\[H\x1b\[2J\x1b\[0m \+-+\+\r\n \| NuSight GEMS Console +Version v([\d.]+) \|\r\n \| Copyright \(c\) 1998-2001, NPI +\|\r\n= p/NPI Keystone switch telnetd/ v/$1/ d/switch/
match telnet m|^rsconfig: port rose not active\n\xff\xfd\"\r\nLinuxNode v([\d.]+) \(([-\w_.]+)\)\r\n\r\nlogin: | p/LinuxNode telnetd/ v/$1/ h/$2/ o/Linux/
match telnet m|^\xff\xfd\"\r\nLinuxNode v([\d.]+) \(([-\w_.]+)\)\r\n\r\nlogin: | p/LinuxNode telnetd/ v/$1/ h/$2/ o/Linux/

match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\r\n\r\nBusyBox v([-\w.]+) \(.*\) Built-in shell \(ash\)\r\nEnter 'help' for a list of built-in commands\.\r\n\r\n.*root@OpenWrt:/# |s p/Busybox telnetd/ v/$1/ i/open; OpenWrt/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\r\n\r\nBusyBox v([-\w_.]+) \([^)]+\) Built-in shell \(ash\)\r\nEnter 'help' for a list of built-in commands\.\r\n\r\n# | i/MacSense HomePod Wireless MP3 Player/ p/BusyBox telnetd/ v/$1/ d/media device/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\n\r\nBusyBox v([-\w_.]+) \([^)]+\) Built-in shell \(ash\)\r\nEnter 'help' for a list of built-in commands\.\r\n\r\n# | i/Netgear DG834G/ p/BusyBox telnetd/ v/$1/ d/router/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\n\r\nBusyBox v([-\w_.]+) \([^)]+\) Built-in shell \(ash\)\r\nEnter 'help' for a list of built-in commands\.\r\n\r\n/bin # | i/Popcorn Hour media player telnetd/ p/BusyBox telnetd/ v/$1/ d/media device/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\r\n\r\nBusyBox v([-\w_.]+) \([^)]+\) Built-in shell \(ash\)\r\nEnter 'help' for a list of built-in commands\.\r\n\r\nroot@H:/# $| p/BusyBox telnetd/ v/$1/ i/Accton VM1188T VoIP phone/ d/VoIP phone/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\n\r\nBusyBox v([-\w_.]+) \([^)]+\) built-in shell \(ash\)\r\nEnter 'help' for a list of built-in commands\.\r\n\r\nermittle die aktuelle TTY\r\ntty is \"/dev/pts/0\"\r\nConsole Ausgaben auf dieses Terminal umgelenkt\r\n# | p/BusyBox telnetd/ v/$1/ i/AVM FRITZ!Box 7150 WAP/ d/WAP/

# Fairly common so relying on release date:
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\n\r\nBusyBox v([-\w_.]+) \(2006\.02\.15-21:18\+0000\) Built-in shell \(msh\)\r\nEnter 'help' for a list of built-in commands\.\r\n\r\n# | i/DiskEdge storage telnet config/ p/BusyBox telnetd/ v/$1/ d/storage-misc/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\nRouter>| p/Cisco 806 router telnetd/ d/router/ o/IOS/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\r\n\r\nUser Access Verification\r\n\r\nPassword: | p/Cisco 2514 router telnetd/ d/router/ o/IOS/
match telnet m|^\xff\xfd\x01\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\xff\xfe\"\xff\xfc\"\x1b\[2J\x1b\[3;0H\x1b\[0mLogin Menu \x1b\[m\x1b\[4;0H\x1b\[0m_+\x1b\[m\x1b\[1;0H\x1b\[0mMCT-2114 Version ([\d.]+) \x1b\[m\x1b\[20;10H\x1b\[0m| p/MCT-2114 switch telnetd/ v/$1/ d/switch/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\nAmiNET\d+ login: | p/Amino AmiNET set-top box telnetd/ d/media device/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\nMSDOS [\d.]+ Windows [\d.]+ \([\d.]+\) \(ttyp\d\)\r\n\r\nlogin: | p/Windows for Workgroups telnetd/ o/Windows/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n\r\n\x07HP (\w+)  Ethernet SNMP Module\r\n ROM B\.([\d.]+)\r\n EEPROM A\.([\d.]+)\r\n HW B\.([\d.]+)\r\n\r\nEnter password: | p/HP AdvanceStack $1 Ethernet hub SNMP Module telnetd/ i/ROM $2; EEPROM $3; HW $4/ d/hub/
match telnet m|^USR5450 Telnet server v([\d.]+)\n\r\nPassword : | p/USR5450 access point telnetd/ v/$1/ d/router/
match telnet m|^\xff\xfb\0\xff\xfd\0\xff\xfb\x01\xff\xfb\x03\xff\xfd\x03\x1b\[1}\x1b\[0;37;40m\x1b\[2J\x1b\[1;1HLogin Name:  | p/HP Integrated Lights-Out remote configuration telnetd/ d/remote management/
match telnet m|^\xff\xfb\x01\x1b\[m\x1b\[m\x1b\[m\x1b\[m\x1b\[m\x1b\[16;35H\x1b\[1;1H\x1b\[2J\x1b\[16;35H\x1b\[1;1HLogin Screen\x1b\[8;5HCopyright \(c\) \d+-\d+ Enterasys Networks, Inc\.  All rights reserved\x1b.*RoamAbout R2\x1b|s p/Enterasys RoamAbout WAP router telnetd/ d/router/
match telnet m|^Welcome to the OfficeConnect\(TM\) LAN modem Telnet Server\n\rConnected From IpAddr/Port# \w+/\d+ To Port# \d+\n\r\nLANmodem> Password: | p/3Com OfficeConnect LAN modem telnetd/ d/router/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n\n\*+\r\n\*     Welcome to Telnet Console     \*\r\n\*+\r\n\r\nServer Name      : [^\0]+\0\0\0\0\0\0\0\0\0\r\nModel +: DP-([\d.]+)\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\r\nFirmware Version : ([\d.]+)  \0\0\0\0\r\nMAC Address      : ([\w ]+)\r\nUp Time          : ([^\r\n]+)\r\n| p/D-Link DP-$1 router telnetd/ i/Firmware $2; MAC $3; Uptime $4/ d/router/
match telnet m|^\xff\xfd\x03\xff\xfb\x03\xff\xfd\x01\xff\xfb\x01\d\d-\w+-\d+ \d\d:\d\d:\d\d %MSCM-I-NEWTERM: New TELNET connection from ([\d.]+)\r\r\nPassword:| p/Dell PowerConnect switch telnetd/ d/switch/
match telnet m|^\xff\xfd\x03\xff\xfb\x03\xff\xfd\x01\xff\xfb\x01User Name:| p/Dell PowerConnect switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\n\r\n\r             Copyright \(C\) \d+ Multi-Tech Systems, Inc\.,\n\r                      Multi-Tech Systems, Inc\.,\n\r                   2205 Woodale Drive, Mounds View,\n\r                        Minnesota 55112, USA\.\n\r\n\r                       MultiVOIP Version ([\d.]+)\n\r| p/Multicom voip telnetd/ i/MultiVOIP $1/ d/VoIP adapter/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\r\n\r\r\n\r           Welcome to the WRT54G Shell Box\r\n\r\r\n\rFirmware version: Wifi-box\.net ([\d.]+)\.wfb \d\d/\d\d/\d\d\r\n| p/Linksys WRT54G with wifi-box.net firmware telnetd/ v/$1/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\xff\xfb\x03EthernetBoard OkiLAN 8100e Ver 0([\d.]+) TELNET server\.\r\0\n\r\0\nlogin: | p/OkiLAN 8100e print server telnetd/ v/$1/ d/print server/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\r\0\n\nLantronix ETS16 Version V([\d.]+)/\d+\(\d+\)\n\r\0\nType HELP at the 'BRTR-ETS16>' prompt for assistance\.\n\r\0\nUsername> | p/Lantronix ETS16 terminal server telnetd/ v/$1/ d/terminal server/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x03TELNET session now in ESTABLISHED state\r\n\r\n(.*) login: | p/Allied Telesyn Rapier switch telnetd/ i/$1/ d/switch/
match telnet m%^\xff\xfe\x01\r\n\r\n\+=+\+\r\n\| +\[ ConnectUPS Web/SNMP Card Configuration Utility \]              \|\r\n\+=+\+\r\n\r\nEnter Password: % p|ConnectUPS Web/SNMP Card telnetd| d/power-device/
match telnet m|^\r\nWelcome to slush\.  \(Version ([\d.]+)\)\r\n\r\n\r\n\xff\xfb\x01\xff\xfb\x03([-\w_. ]+) login: | p/slush telnetd/ v/$1/ i/$2/ o/TiniOS/
match telnet m|^\xff\xfb\x01\n\r\n\rWebRamp 410i    login: $| p/WebRamp 410i ISDN router telnetd/ d/router/
match telnet m|^Please Wait\.\.\.Connection Accepted \(TelSrv ([\d.]+)\)\r\n\r\nUsername : | p/TelSrc telnetd/ v/$1/ o/Windows/
match telnet m|\xff\xfb\x01\xff\xfb\x03\r\nINTERMEC 540\+/542\+ TELNET Print Server V([\d.]+) .*\r\n\r\nINTERMEC 540\+/542\+ network login: | p|Intermec 540+/542+ print server telnetd| v/$1/ d/print server/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\x1b\[2J\x1b\[1;1HConnecting\.\.\.\.\x1b\[2J\x1b\[1;1HAdtran - TSU 120e\r\n\r\nPassword: | p/Adtran TSO 120e telnetd/ d/broadband router/
match telnet m|^\xff\xfd\x1f\xff\xfd\x18\xff\xfb\x01\xff\xfb\x03\nWelcome to GoodTech Systems Telnet Server for Windows \S+ \(Evaluation Copy\)\n\r\n\(C\) Copyright \d+-\d+ GoodTech Systems, Inc\.\n\r\n\nLogin username: | p/GoodTech Systems telnetd/ i/Evaluation copy/ o/Windows/
match telnet m|^\xff\xfd\x18\xff\xfe\"\xff\xfb\x03\xff\xfe\x01\xff\xfb\x01\xff\xfa\x18\x01\xff\xf0\xff\xfd\x1fBytefusion Telnet ([\d.]+), Copyright \d+-\d+ Bytefusion Ltd\.\n\rUnregistered Evaluation\. See www\.bytefusion\.com/telnet\.html\r\n\n\rWIN3 Login: | p/Bytefusion telnetd/ v/$1/ i/Evaluation copy/ o/Windows/
match telnet m|^Windows Telnet Server Version ([\d.]+)\r\nCopyright\(C\) Jordan Stojanovski \d+\r\n------------------------------------\r\nUser name: | p/Jordan Stojanovski Windows telnetd/ v/$1/ o/Windows/
match telnet m|^\xff\xfe\x01\xff\xfd\x03\xff\xfd\x18\xff\xfd\x1f\xff\xfd\0\xff\xfb\x03\xff\xfb\x01\xff\xfb\0This is an unregistered copy of the Ataman TCP Remote Logon Services\.\r\nThe Ataman TCP Remote Logon Services has a \d+ day evaluation period\.\r\nThis copy was installed \d+ days ago\.\r\n\r\nAccount Name: | p/Ataman telnetd/ i/Evaluation copy/ o/Windows/
match telnet m=^\xff\xfb\x01\xff\xfd\x1f\xff\xfb\x03\x1b\[1;1f\x1b\[37m +\x1b\[2;1f +\x1b\[3;1f +\x1b\[4;1f -+ +\x1b\[5;1f\|  KpyM Telnet Server v([\d.]+) +\|= p/KpyM telnetd/ v/$1/ o/Windows/
match telnet m|^\x1b\[2J\x1b\(0\x1b\[01;00Hlqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqk\x1b| p/3Com Linkswitch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\r\nD-link Corp\. Access Point login: | p/D-Link DWL access point telnetd/ d/router/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\x1b\[0m\x1b\[2J\x1b\[0m\x1b\[2J\x1b\[2;66H\x1b\[1m\x1b\[21;1H\x1b\[0m-+\x1b\[22;2H\x1b\[0mFunction:\x1b\[23;2H\x1b\[0mMessage:\x1b\[24;2H\x1b\[7mCTRL\+R = Refresh +\x1b\[8;12H\x1b\[0mIBM BladeCenter 4-Port Gb Ethernet Switch Module Console| p/IBM BladeCenter 4-Port Gb switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18    \x1bc\x1b\[2J\x1b\[1;1HTelnet\r\n\x1b\[3;1H                     CF8720 Olicom Fast Ethernet L3 Switch| p/Olicom CrossFire 8720 switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfe\x01\xff\xfd\x03\xff\xfb\x03\x1b\[0;1H\x1b\[J\x1b\[1;1H\x1b\[0;1H\x1b\[J\x1b\[1;1H\x1b\[0m =+\r\n AT-8326GB Management System Version ([\d.]+) \r\n Remote - Telnet\r\n| p/Allied Telesyn 8326GB switch telnetd/ v/$1/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\r\n                 Welcome to Quidway A8010 Expert Multiservice Access Switch\r\n| p/Huawei Quidway A8010 remote access telnetd/ d/remote management/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\x1b\[0m\x1b\[2J\x1b\[0m\x1b\[2J\x1b\[1;1H\x1b\[0m-.*Enter case-sensitive username\. No username is assigned by default\.|s p/Intel 460T Standalone switch telnetd/ d/switch/
match telnet m|^\r\nEfficient 5851 SDSL \[ATM\] Router \(5851-\d+\) v([-\d.]+) Ready\r\n\xff\xfb\x01\xff\xfb\x03\xff\xfd\x01\xff\xfe\x01Login: | p/Efficient 5851 DSL router telnetd/ v/$1/ d/router/
match telnet m|^\[TS\]\r\n$| p/Teamspeak VoIP Information telnetd/
match telnet m|^\xff\xfb\x01\r\n\r\*+\n\r\r\* Copyright \(c\) \d+ Nortel Networks, Inc\.  \*\n\r\r\* All Rights Reserved +\*\n\r\r\* Passport 8010 +\*\n\r\r\* Software Release ([\d.]+) | p/Nortel Passport 8010 router telnetd/ v/$1/ d/router/
match telnet m|^Rapture Runtime Environment v([\d.]+) -- \(c\) \d+ -- Iron Realms Entertainment\r\n| p/Rapture-based MUD telnetd/ v/$1/
match telnet m|^NPC Telnet permit one connection\.\r\n But One connection\(\) already keep alive\.\r\nGood Bye !! \r\n| p/Samsung printer telnetd/ d/printer/
match telnet m|^\n\r\n\r.*\* MWR Ver ([\d.]+) \*.*SMAUG|s p/SMAUG MUD server/ v/$1/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\x1b\[2J\x1b\[0;0H\x1b<\r\n          \x1b\[7m +\x1b\[0m +\r\n +\x1b\[7m +Welcome to Management Blade ([\d.]+) | p/BX600 Blade Chassis Manager telnetd/ v/$1/ d/remote management/
match telnet m|^\r\n\r\nWelcome to the SoundBridge Shell version ([\d.]+) Release\r\nType '\?' for help or 'help <command>' for help on <command>\.\r\n\r\nSoundBridge> | p/Roku SoundBridge telnetd/ v/$1/ d/media device/
match telnet m|^\xff\xfb\x01\r\nWelcome to NetLinx v([\d.]+) Copyright AMX Corp\. \d+-\d+\r\n>| p/AMX NetLinx telnetd/ v/$1/ d/media device/ o/VxWorks/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\n\r\n\[Dell  TM 1170 AP 2\]> Please enter password: | p/Dell TrueMobile 1170 wireless router telnetd/ d/router/
match telnet m|^\r\nSiemens \d+ T1E1 \[COMBO\] Router \(([-\d]+)\) v([\d.]+) Ready\r\n\xff\xfb\x01\xff\xfb\x03\xff\xfd\x01\xff\xfe\x01Username: | p/Siemens $1 T1E1 router/ v/$2/ d/router/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\n\r\n\r\n\rWelcome to the SIA2410R\n\r| p/Net to Net SIA2410R DSL router telnetd/ d/router/
match telnet m|^\xff\xfb\x01Welcome to the DataStage Telnet Server\.\r\0\r\nEnter user name: | p/Ascentia DataStage telnetd/
match telnet m|^\xff\xfd\x18\xff\xfb\x01\x1b\[2J\x1b\[\?7l\x1b\[4;23r\x1b\[\?6l\x1b\[1;1H\x1b\[\?25l\x1b\[1;1HCopyright \(C\) 1991-1994 Hewlett-Packard Co\.  All Rights Reserved\.| p/HP switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\nReload scheduled for .* \(in .*\)\r\nRouter>| p/Cisco 1601R router telnetd/ o/IOS/ d/router/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03Telnet access disabled\. Enable in switch CLI\r\n| p/Aruba Networks AP 61 telnetd/ d/router/
match telnet m|^\xff\xfb\x01\xff\xfd\x01\xff\xfb\x03\xff\xfd\x03\xff\xfb\x05\xff\xfd\x05PointRed Technologies, Inc\. PartNo: ([-\d]+), Version: ([\d.]+)\r\n\r\nlogin:| p/PointRed Technologies PartNo $1 telnetd/ v/$1/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\n\r\n\r +Copyright \(C\) \d+ MultiTech Software Systems Inc\.,\n\r.*MultiVoIP Version ([\d.]+)\n\r|s p/MultiTech MultiVoIP telnetd/ v/$1/ d/VoIP adapter/
match telnet m=^\xff\xfb\x01\xff\xfb\x03\r\n     ____  _  _  _            _      ____          _\r\n    / _  \|\| \|\| \|\(_\)  ___   __\| \|    \|  _ \\   __ _ \| \|_  __ _\r\n= p/Allied Data CopperJet router telnetd/ d/router/
match telnet m|^\xff\xfc\x01\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfb\x18\xff\xfd\x1f\xff\xfb\x1f\xff\xfb\"\xff\xfb\x05\r\nCLI access not allowed until the SCC is active\.\r\n\r\n| p/Checkpoint firewall telnetd/ d/firewall/
match telnet m|^\xff\xfb\x01   IP PHONE 2 V([\d.]+) | p/NG VoIP Phone 2 telnetd/ v/$1/ d/VoIP phone/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\n\r\n\r\n\r  Huawei HONET UA5000 Universal Access Unit\.\n\r  Copyright\(C\) 1998-2005 by Huawei Technologies Co\., Ltd\.\n\r\r\n>>User name:| p/Huawei HONET UA5000 Universal Access Unit telnetd/
match telnet m|^\xff\xfb\x01\r\n-> 115260:51\.665 \(nEcho\): Log: \[NON_FATAL\] Num:\[0\], Mod:\[tcpEchoBytes\], EOF\r\n$| p/Xerox Phaser 4400DX printer/ d/printer/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\xff\xfb\x03SHARP (AR-\w+) Ver ([\w._+-]+) TELNET server\.\r\0\nCopyright\([cC]\) [\d -]+,? silex technology, Inc\.\r\0\nlogin: $| p/Sharp $1 printer telnetd/ v/$2/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\xff\xfb\x03SHARP (MX-\w+) Ver ([\w._+-]+) TELNET server\.\r\0\nCopyright\(C\) [\d -]+ SHARP CORPORATION\r\0\nCopyright\(C\) [\d -]+ silex technology, Inc\.\r\0\nlogin: | p/Sharp $1 printer telnetd/ v/$2/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\xff\xfb\x03Sharp (AR-\w+) Ver ([\w._+-]+) TELNET server\.\r\0\nCopyright\(C\) [\d -]+ SHARP CORPORATION\r\0\nCopyright\(C\) [\d -]+ Japan Computer Industry Inc\.\r\0\nlogin: | p/Sharp $1 printer telnetd/ v/$2/
match telnet m|^\xff\xfb\x01AMBIT VoIP TRIO, ([\w._/]+), MAC:([0-9A-F]{12}),VOIP FLG=1\n\r\n\rInternational numbers routed to VoIP\.\n\r\n\rLogin: | p/Softbank Trio 1 WAP telnetd/ v/$1/ d/WAP/ i/MAC: $2/


# A bit general:
match telnet m|^\xff\xfb\x01\n?\r\n\r?VxWorks login: | p/VxWorks telnetd/ o/VxWorks/
match telnet m|^\xff\xfb\x01\r\n\r\nVxWorks login: | p/VxWorks telnetd/ o/VxWorks/
match telnet m|^\xff\xfb\x01\r\n([-\w_.]+) wireless  login: $| p/Conceptronic C54APT wireless router telnetd/ i/Name $1/ d/router/
match telnet m|^\xff\xfb\x01\r\n\rPassword: $| p|ZyXEL Prestige/Efficient Speedstream adsl router telnetd| d/router/
match telnet m|^\xff\xfb\x03\xff\xfb\x01password: $| p/D-Link ADSL router telnetd/ d/router/
match telnet m|^\r\n\xff\xfb\x01Enter password: $| p/SunSwitch telnetd/ d/switch/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\rLogin: $| p/Cisco 3000 series VPN Concentrator telnetd/ d/terminal server/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\w+ login: | p/PXES Linux Thin Client telnetd/ o/Linux/ d/terminal/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x01\n\rlogin: | p/Cayman Gatorbox router telnetd/ d/router/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03(\r\n)?User: | p/Aruba switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\n\(\w+\) \r\nUser: | p/Aruba switch telnetd/ d/switch/
match telnet m|^login: \xff\xfb\x01\xff\xfb\x03| p|USRobotics/Sagem router telnetd| d/router/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfb\0\xff\xfd\0login: | p/Sagem router telnetd/ d/router/
match telnet m|^\xff\xfb\x01\xff\xfb\x03Password: | p/Telindus router telnetd/ d/router/
match telnet m|^220 FTP server \(ver 1\.0\) ready\.\r\n$| i/Mitel 3300 PBX controller ftpd/ d/PBX/

match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\nBusyBox on dslmodem login: | p/Actiontec DSL router/ d/router/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\xff\xfd\x1f\xff\xfd\x18| p/BladeCenter or TANDBERG Codec telnetd/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\nlogin: | p/D-Link DSL router telnetd/ d/router/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n([-\w_.]+) login: | p|NASLite-SMB/Sveasoft Alchemy firmware telnetd| h/$1/
match telnet m|^\r\nAnother telnet session is in progress\.\r\n$| p/HP JetDirect telnetd/ d/printer/
match telnet m|^\r\nSystem unavailable\.  Please try later\.\r\n$| p/Cisco CSS telnetd/ d/load balancer/ o/IOS/
match telnet m|^\xff\xfb\x03\xff\xfa\x18\x01\xff\xf0$| p/Netgear FVS318 router telnetd/ d/router/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\r\n(FVS\w+) login: | p/Netgear $1 router telnetd/ d/router/
match telnet m|^\xff\xfb\0\xff\xfd\0\xff\xfb\x01\xff\xfd\x01\xff\xfb\x03\xff\xfd\x03Login Name:  | p/HP Remote Lights-Out Edition II telnetd/ d/remote management/
match telnet m|^\xff\xfb\x01\xff\xfe\"\r\n\*$| p/Network Systems Group router telnetd/ d/router/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\n\r\nUser Access Verification\r\n\r\nlogin:| p/Cisco 1721 router telnetd/ o/IOS/ d/router/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n Disconnecting\.\.\.\r\n\n$| p/HP LaserJet printer telnetd/ d/printer/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\x1b\[2J\x1b\[0;0H\x1b\[K\x1b\[7mTelnet configuration                          RELEASE ([\d.]+)\x1b| p/Pirelli Age UB router telnetd/ v/$1/ d/router/
match telnet m|^Telnet server disabled\r\n$| p/F5 BIG-IP load balancer telnetd/ i/telnet disabled/ d/load balancer/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n login: | p/Linksys WRT54G telnetd/ i/Sveasoft firmware/ d/WAP/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03([\w._-]+) login: | p/Busybox telnetd/ h/$1/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfb\x01\xff\xfb\x03([\w._-]+) login: | p/Busybox telnetd/ h/$1/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\(none\) login: | p/BusyBox telnetd/
match telnet m|^\xff\xfb\x01Copyright \(C\) \d+ by Compaq Computer Corp\. \r\n\rlogin: | p/Compaq 5450 switch telnetd/ d/switch/
match telnet m|^\n\r\n\rTHIS IS A MUD BASED ON\.\.\.\.\.\n\r\n\r                                ROM Version (.*)\n| p/ROM-based MUD/ v/$1/
match telnet m|^\r\n.*Based\(loosely\) on CircleMUD ([\d.]+)|s p/CircleMUD-based MUD telnetd/ v/$1/
match telnet m|^\r\n.*Based on CircleMUD ([\w._-]+),\r\n|s p/CircleMUD telnetd/ v/$1/
match telnet m|^\xff\xfb\x01\xff\xfd\x01\xff\xfb\x03\xff\xfd\x03\xff\xfb\x01\xff\xfd\x01\xff\xfb\x03\xff\xfd\x03\r\n\r\nSelect Access Level\r\n===================\r\n1 - Read-Only\r\n2 - Installer\r\n3 - Administrator\r\n| p/BreezeACCESS wireless router telnetd/ d/router/
match telnet m|^\x1b\[0;37;40m\x1b\[2J\x1b\[0;37;40m\x1b\[1m\x1b\[15;22HAT-(\w+), version ([\d.]+)\x1b| p/Allied Telesyn $1 switch telnetd/ v/$1/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfe\x01\xff\xfd\x03\xff\xfb\x03\x1b\[0;0H\x1b\[0J\x1b\[0;0H\x1b\[0J\x1b\[1;28HAT-([-\w_.]+) Login Menu\x1b\[5;18HAT-[-\w_.]+ Local Management System Version ([\d.]+) \x1b| p/Allied Telesyn $1 switch telnetd/ v/$2/ d/switch/

match telnet m|^\xff\xfd\x03\xff\xfb\x01\x1b\[2J\x1b\[1;1H\x1b\[0m\x1b\[\?3l\x1b\(0\x1b\[2;40H\x1b\(B\x1b\(0\x1b\[2;28H\x1b\(BCSX([-\w_.]+) Local Management\x1b\[0m\x1b\(0\x1b\[5;24H\x1b\(BCABLETRON Systems, Incorporated\x1b| p/Cabletron CSX$1 router telnetd/ d/router/
match telnet m|^\xff\xfb\x01\xff\xfd\x01\xff\xfb\x03\xff\xfd\x03\xff\xfb\x05\xff\xfd\x05SpeedStream Telnet Server\r\n\r\n\r\nlogin: | p/Efficient Networks Speedstream router telnetd/ d/router/
match telnet m=^\xff\xfb\x01\xff\xfb\x03\r\n\r\n#\r\n\| LANCOM 821 ADSL/ISDN\r\n\| Ver\. ([\d.]+) /= p|Lancom 821 DSL/ISDN router telnetd| v/$1/ d/router/
match telnet m|^\xff\xfb\x01\n\rno data rcvd for version string\n\rrecv version id unsuccessful\n\rSSH Session task 0x\w+: Version Exchange Failed\n\r| p/Cisco Aironet 1200 router telnetd/
match telnet m|^\xff\xfe\x01Foxconn VoIP TRIO 3C| p/Foxconn VoIP TRIO 3C telnetd/
match telnet m|^Sorry telnet connections not permitted\.\n$| p/Aruba router telnetd/ d/router/
match telnet m|^\r\nSorry, this system is engaged\.\r\n$| p/DirecWay satellite router telnetd/ d/router/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\nBusyBox on \(none\) login: | p/BusyBox telnetd/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\nBusyBox on ([-\w_.]+) login: | p/BusyBox telnetd/ h/$1/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\n\r\nBusyBox v([-\w_.]+) \(| p/BusyBox telnetd/ v/$1/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\r\n\r\nBusyBox v(.*) Built-in shell \(ash\)\r\n| p/Busybox telnetd/ v/$1/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03\(none\) login: | p/FetchTV DVR telnetd/ d/media device/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\x1b\(B\x1b\)0\x1b\[2J\x1b\[H\x1b\[m\x0f\x1b\[10;32H\x0e                 \x1b\[11;32H lq\x0f\x1b\[1mLogin\x0e\x1b\[mqqqqqqqqk\x1b\[12;32H x\x1b\[13C x\x1b\[13;32H mqqqqqqqqqqqqqqj\x1b\[12;34H| p/Adtran Atlass 500 T1 router telnetd/ d/router/
match telnet m|^\xff\xfb\x01\xff\xfd\x1fHummingbird Ltd\., Windows NT, Telnetd \((\w+) Version ([\d.]+)\)\r\n\r\nlogin: | p/Hummingbird windows telnetd/ v/$2/ h/$1/ o/Windows/
match telnet m|^\xff\xfb\x01Hummingbird Communications Ltd\., Windows NT, Telnetd Version ([\d.]+) \(([-\w_.]+)\)\r\n\r\n login: | p/Hummingbird windows telnetd/ v/$1/ h/$2/ o/Windows/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\nUser Access Verification\r\n\r\nPlease Enter Login Name: | p/Foundry Networks telnetd/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\nUser Access Verification\r\n\r\nPlease Enter Password: | p/Foundry Networks telnetd/
match telnet m|^\xff\xfb\x01\xff\xfb\x03BR-telnet@FI_Core>| p/Foundry FastIron 1500 switch telnetd/ d/switch/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\x1b\[\?3l\x1b\[2JPlease enter your user name and password!! \r\n\r\nLogin:| p/Hawking Technology print server telnetd/ d/print server/
match telnet m|^\xff\xfb\x01\r\nD-Link Access Point login: | p/D-Link Access Point telnetd/ d/router/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03.*\r\n([-\w_.]+) login: |s p/utelnetd/ h/$1/ o/Unix/
match telnet m|^\xff\xfb\x01Select access level \(read, write, administer\): | p/3Com SuperStack II Switch telnetd/ d/switch/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03Login failed\.\r\n| p/Busybox telnetd/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\(none\) login: | p/Busybox telnetd/ v/1.0/
match telnet m|^\r\nEfficient 5851 SDSL \[CM\] Router \((5851-\d+)\) v([\d.]+) Ready\r\n\xff\xfb\x01\xff\xfb\x03\xff\xfd\x01\xff\xfe\x01Login: | p/Efficient Networks $1 SDSL router telnetd/ v/$2/ d/router/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\r\n\nLantronix LPS1 Version V(\d[\w/-_+.]+)\((\d+)\)\n\r\nType HELP at the 'Local_3> ' prompt for assistance\.\n\r\nUsername> | p/Lantronix LPS1 telnetd/ v/$1/ i/Released $2/ d/print server/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\r\nTA 600R\r\n\n\n\ruser: | p/Adtran TA 600R router telnetd/ d/router/
match telnet m|^\xff\xfd\x03\xff\xfb\x03\xff\xfd\x01\xff\xfb\x01\r\n\r\r\nUser Name:$| p/Dell PowerConnect switch telnetd/ d/switch/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\xff\xfb\x03\x1b\[1;1H\x1b\[2K\x1b.*BayStack ([-\w_.]+) Main Menu\x1b|s p/BayStack $1 switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\n\r +\*+\n\r +Welcome to ([-\w_.]+)\n\r +\*+\n\r\n\rD-Link Corp\., Inc\. Software Release ([-\w_.)(/]+)\n\rCopyright \(c\) \d+-\d+ by D-Link Corp\., Inc\.\n\r\n\rlogin: | p/D-Link router telnetd/ v/$2/ i/$1/ d/router/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03# | p/AML M7100 telnetd/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\xff\xfd\x1f\r\nUsing telnet exposes your password\. Using ssh is a safer choice\.\r\n\r\nUsername: | p/Blue Coat telnetd/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\xff\xfb\x03\xff\xfb\x01\r\n\r\nPIX passwd: | p/Cisco PIX firewall telnetd/
match telnet m|^TELNET server version ([\d.]+) ready at \r\n\r\r\npassword: \xff\xfc\x01| p/ASCOM ColtSoho router telnetd/ v/$1/ d/router/
match telnet m|^\xff\xfb\x01\r\n#-+\r\n# Tasman Networks Inc\. Telnet Login\r\n#| p/Tasman Networks router telnetd/ d/router/
match telnet m|^\n\r\n\rHi! I am your Net Tamagotchi! I love you!!| p/Net Tamagotchi telnetd/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\r\n\r\n\t\t Welcome to P330\r\n\t\tSW version ([\d.]+)\r\n\r\n\r\nLogin: | p/Avaya P330 switch telnetd/ v/$1/ d/switch/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\r\n\r\n\t\tWelcome to P333R\r\n\t\tSW version ([\d.]+)\r\n\r\n\r\nLogin: | p/Avaya P333R switch telnetd/ v/$1/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfd\x01\xff\xfb\x03\xff\xfd\x03\xff\xfb\x05\xff\xfd\x05\xff\xfd\x1fSpeedStream Telnet Server\r\n\r\n\r\nlogin: | p/SpeedStream router telnetd/ d/router/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\r\n\rwelcome on your dreambox! - Kernel (\d[\w.]+) \([\d:]+\)\.\r\n\r([-\w_.]+) login: | p/Dreambox DVB telnetd/ d/media device/ i/Kernel $1/ h/$2/ o/Linux/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\nPLi dm7000 Helenite \d+ \(based on [-\w_.]+\)\r\n\rwelcome on your dreambox! - Kernel ([-\w_.]+) | p/Dreambox DVB telnetd/ d/media device/ o/Linux/ i/Kernel $1; Helenite firmware/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\r\n\r[ *\r\n]*Welcome on your dreambox! - Kernel (\d[\w.]+) | p/Dreambox DVB telnetd/ d/media device/ i/Kernel $1/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x1f\r\n\x1b\[34;1m   \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* \r\n\x1b\[34;1m| p/SAP J2EE engine telnetd/
match telnet m|^\xff\xfe\"\xff\xfb\x01          \x1b\[H\x1b\[J\x1b\[3;1HCB-1000 S/N: (\d+)\x1b\[3;56HSymbol Technologies, Inc\.\x1b\[4;1HVersion ([-\w_.]+)\x1b\[4;44HEthernet HW address ([\w:]+)\x1b\[21;1H| p/Symbol CB-1000 bridge telnetd/ v/$2/ i/SN $1; MAC $3/ d/bridge/
match telnet m|^StoneGate firewall \([\d.]+\) \n\rSG login: | p/StoneGate firewall telnetd/ d/firewall/
match telnet m|^\xff\xfb\x01\x1b\[2J\x1b\[0m\x1b\[1;1H\n\r\x1b\[2;1H\n\r\x1b\[3;1H\n\r\x1b\[4;1H\n\r\x1b\[5;1H\n\r\x1b\[6;1H\n\r\x1b\[7;1H\n\r\x1b\[8;1H\n\r\x1b\[9;1H\n\r\x1b\[10;1H\n\r\x1b\[11;1H\n\r\x1b\[12;1H\n\r\x1b\[13;1H\n\r\x1b\[14;1H\n\r\x1b\[15;1H\n\r\x1b\[16;1HEnter Ctrl-Y to begin\.\x1b\[18;3H\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\x1b\[19;3H\*\*\* Ethernet Switch 460-24T-PWR | p/Nortel 460-24T-PWR switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\x1b\[2J\x1b\[0m\x1b\[1;1H \n\r\x1b\[2;1H\n\r\x1b\[3;1H\n\r\x1b\[4;1H\n\r\x1b\[5;1H\n\r\x1b\[6;1H\n\r\x1b\[7;1H\n\r\x1b\[8;1H\n\r\x1b\[9;1H\n\r\x1b\[10;1H\n\r\x1b\[11;1H\n\r\x1b\[12;1H\n\r\x1b\[13;1H\n\r\x1b\[14;1H\n\r\x1b\[15;1H\n\r\x1b\[16;1HEnter Ctrl-Y to begin\.\x1b\[18;3H\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\x1b\[19;3H\*\*\* BayStack 420 | p/BayStack 420 switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\x1b\[2J\x1b\[0m\x1b\[1;1H \*\*\*\*\*      \*\*\*     \*     \*    \*\*\*\*\*   \*\*\*\*\*\*\*\*\*     \*\*\*| p/BayStack 470 switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\x1b\[2J\x1b\[56184256;1H\x1b\[0m\x1b\[1;1H \*\*\*\*\*      \*\*\*     \*     \*    \*\*\*\*\*   \*\*\*\*\*\*\*\*\*     \*\*\*| p/BayStack 5510 switch telnetd/ d/switch/
match telnet m|^200 Hamster Remote Control, Hamster[ -]Playground Vr\. ([\w._-]+)\r\n| p/Hamster-Playground telnetd/ v/$1/ o/Windows/
match telnet m|^200 Hamster Remote Control, Hamster[ -]Playground Vr\. [\w._-]+ \(Build ([\w._-]+)\)\r\n| p/Hamster Playground telnetd/ v/$1/ o/Windows/
match telnet m=^\xff\xfb\x01\x1b\[2J\x1b\[H\x1b\[2J\x1b\[H\x1b\[1;12H----------------------------------------------------------\x1b\[2;11H\|\x1b\[16CCisco VG248 \(= p/Cisco VG248 telnetd/ d/VoIP adapter/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\x1b\[\?25h\x1b\[2J\x1b\[0;0H\x1b<\r\nRemote Access Controller/Modular Chassis \(DRAC/MC\)\r\nCopyright \(C\) 2000-200[4457] Dell Inc\.| p|Dell DRAC/MC telnetd| d/remote management/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\xff\xfb\x03IB-21E Ver ([\d.]+) TELNET server\.\r\0\nCopyright \(C\) 2001-2003 KYOCERA CORPORATION\r\0\n| p/Kyocera IB-21E telnetd/ v/$1/ d/print server/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n\n\*+\r\n\*  Welcome to D-Link Print Server  \*\r\n\* +Telnet Console +\*\r\n\*+\r\n\r\nServer Name    :  ([\w._-]+)\0+\r\nServer Model   :  ([\w_.+-]+)\0+\r\nF/W Version    :  ([\w._-]+)  \0.\0+\r\nMAC Address    :  ([\w ]+)\r\nUptime         :  ([^\r\n]+)\r\n\nPlease Enter Password: |s p/D-Link $2 print server telnetd/ h/$1/ i/FW version $3; MAC $4; Uptime $5/ d/print server/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n\n\*+\r\n\*  Welcome to D-Link Print Server  \*\r\n\* +Telnet Console +\*\r\n\*+\r\n\r\nServer Name    :  ([\w._-]+)\0+\r\nServer Model   :  ([\w_.+-]+)\0|s p/D-Link $2 print server telnetd/ h/$1/ d/print server/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n\r\n\*+\r\n\*  Welcome to D-Link Print Server  \*\r\n\* +Telnet Console +\*\r\n\*+\r\n\r\nServer Name    :  ([\w._-]+)\0+\r\nServer Model   :  ([\w_.+-]+)\0+\r\nF/W Version    :  ([\w._-]+) *\0.\0+\r\nMAC Address    :  ([\w ]+)\r\nUptime         :  ([^\r\n]+)\r\n\n|s p/D-Link $2 print server telnetd/ d/print server/ h/$1/ i/FW version $3; MAC $4; Up $5/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n\r\n\*+\r\n\*  Welcome to D-Link Print Server  \*\r\n\* +Telnet Console +\*\r\n\*+\r\n\r\nServer Name    :  ([\w._-]+)\0+\r\nServer Model   :  ([\w._+-]+)\0+\r\nF/W Version    :  ([\w._-]+) *\0.\0+\r\nMAC Address    :  ([\w ]+)|s p/D-Link $2 print server telnetd/ d/print server/ v/$3/ i/name $1; MAC $4/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n\r\n\*+\r\n\*  Welcome to D-Link Print Server  \*\r\n\*.*\r\nServer Name    :  ([\w._-]+)\0+\r\nServer Model   :  ([\w._+-]+)\0|s p/D-Link $2 print server telnetd/ d/print server/ h/$1/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n\r\n\*+\r\n\*  Welcome to D-Link Wireless Print Server  \*\r\n\* +Telnet Console +\*\r\n\*+\r\n\r\nServer Name    :  ([\w._-]+)\0+\r\nServer Model   :  ([\w._+-]+)\0+\r\nF/W Version    :  ([\w._-]+)\0.\0+\r\nMAC Address    :  ([\w ]+)|s p/D-Link $2 wireless print server telnetd/ h/$1/ i/FW $3; MAC $4/
match telnet m|^\xff\xfe\0\xff\xfc\0\xff\xfe\x01\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\n\n\rLocal User Access Verification: \n\n\rLogin: | p/Allied Telesyn switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\n\r\n\x1b\[H\x1b\[JWelcome at ActiveFax Server\.\r\n\r\n| p/ActiveFax telnetd/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\xff\xfb\x01\xff\xfb\x03\r\n\r\nLogin: $| p/ActionTec DSL router/ d/broadband router/
match telnet m|^\xff\xfc\x01PCS-(\w+) Telnet2? Server\r\nlogin: | p/Sony PCS-$1 telnetd/ d/media device/
match telnet m|^\xff\xfb\x01\xff\xfb\x03RemoteX Telnet Server V([\d.]+)\n\r\n\rc:\\>| p/RemoteX telnetd/ v/$1/ d/game console/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03 ADSL Router\r\nLogin name: | p/BT Voyager ADSL router telnetd/ d/broadband router/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\n\r +\*+\n\r +Welcome to ZXDSL 831\n\r +\*+\n\r\n\rZTE Corporation, Software Release VIK-([-\w_.]+)\n\r| p/ZyXEL ZXDSL 831 telnetd/ v/$1/ d/broadband router/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03                        =======================\r\n                        Welcome to ZXDSL 831II\r\n                        =======================\r\nLogin:| p/ZXDSL 831II ADSL modem telnetd/ d/broadband router/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03                ===========================\r\n                  Welcome to ZXDSL  (831CII)\r\n                ===========================\r\n\r\nZTE Inc\., Software Release ZXDSL 831CIIV([\w._-]+)\r\n\r\nLogin name: | p/ZXDSL $1 ADSL modem telnetd/ v/$2/ d/broadband router/
match telnet m|^\r\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\n\r\*  HiPath (\d+) Telnet  \*\n\r| p/Siemens HiPath $1 telnetd/ d/firewall/
match telnet m%^\xff\xfe\x01\r\n\r\n\+=+\+\r\n\| +\[ MGE UPS SYSTEMS SNMP/Web agent Configuration menu \]% p/MGE UPS telnetd/ d/power-device/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03root@HD:/# | p/utelnetd/ i/**NO PASSWORD**/ o/Unix/
match telnet m|^\xff\xfb\x01\xff\xfd\x01\xff\xfe\x01\xff\xfd\x03\xff\xfb\x03\*+\r\n\r\nThis session allows you to set the TCPIP parameters for your\r\nDell Laser Printer ([\w+]+) Ethernet internal network device| p/Dell $1 printer telnetd/ d/printer/
match telnet m|^\xff\xfb\x01\xff\xfd\x01\xff\xfe\x01\xff\xfd\x03\xff\xfb\x03\*{60}\r\n\r\nThis session allows you to set the TCPIP parameters for your\r\nDell (\w+) Laser Printer Ethernet internal network device, with a hardware\r\naddress of [0-9A-F]{12} ([0-9A-F]{12}) \(MSB, Canonical\)\.\r\n| p/Dell $1 printer telnetd/ d/printer/ i/MAC $2/
match telnet m|^\*{60}\r\n\r\nThis session allows you to set the TCPIP parameters for your\r\nDell Laser Printer Printer Dell (\w+) MFP Ethernet internal network device, with a hardware\r\naddress of ([0-9A-F:]{17}) \(MSB, Canonical\)\.\r\nIt's an ethernet card\.\r\nNetwork Firmware Version is V([\w._-]+)\(\w+ MFP\) ([\d-]+)\.\r\nSystem Up Time is ([^\r\n.]+)\.\r\n\r\n| p/Dell $1 printer telnetd/ d/printer/ v/$3/ i/MAC $2; uptime $4/
match telnet m|^\xff\xfb\"\xff\xfb\x03\xff\xfb\x01\xff\xfb\0\xff\xfd\0\n\r\nWelcome to the PDP-10 simulator\r\n\n| p/PDP-10 simulator telnetd/
match telnet m|^\xff\xfb\x01\(Enable\) Password\? | p/Enterasys gated config telnetd/ d/router/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\nWelcome to Linux \(ZEM200\) for arca\r\n\rKernel ([-\w_.]+) on an arca \r\n\rZEM200 login: | p/ZEM200 biometric device config telnetd/ i/Linux $1/ o/Linux/ d/specialized/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\r\n\r\nCGX3224 Switch Manager Console\. Version: CGX([\d.]+) Bld (\d+),.*\r\n\r\nPassword:| p/COMPEX CGX3224 switch telnetd/ i/CGX $1.$2/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\x1b\[0m\x1b\[2J\x1b\[01;00H\r\n\r\0\r\n\r\0[ \t]+\r\n\r\0\r\n\r\0\r\0VersaXpress HPNA Routing Concentrator\r\n| p/Versatek VersaXpress HPNA Routing Concentrator telnetd/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\nSportster Pro ([\d.]+) Image Sagem D-BOX2 - Kernel ([-\w_.]+) | p/Sagem D-BOX2 Sportster Pro telnetd/ v/$1/ i/linux kernel $2/ o/Linux/ d/media device/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n.*Sagem D-BOX2 - Kernel ([-\w_.]+) |s p/Sagem D-BOX2 telnetd/ i/linux kernel $1/ o/Linux/ d/media device/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\0\r\n\*\*\* Lantronix Universal Device Server \*\*\*\r\n\r\0Serial Number (\d+)  MAC address ([\w:]+)\r\n\r\0Software Version V([\d.]+) \((\d+)\)\r\0\r\n\r\n\r\0Press Enter to go into Setup Mode \r\n\r\0| p/Lantronix Universal Device Server telnetd/ v/$3.$4/ i/Serial $1; MAC $2/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\0\n\*\*\* Lantronix Universal Device Server \*\*\*\r\0\nSerial Number (\d+)  MAC address ([\w:]+)\n\r\0Software version 0*([\d.]+) \((\d+)\)\r\0\n\r\0\nPress Enter to go into Setup Mode \r\0\n| p/Lantronix Universal Device Server telnetd/ v/$3.$4/ i/Serial $1; MAC $2/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03Fritz!Box web password: | p/AVM FRITZ!Box 7170 telnetd/ d/WAP/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\nFritz!Box web password: | p/AVM FRITZ!Box telnetd/ d/WAP/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\nDD-WRT v([-\w_+. ]+) Date:| p/DD-WRT telnetd/ v/$1/ d/WAP/ o/Linux/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\nDD-WRT v([^\r\n]+)\r\n| p/DD-WRT telnetd/ v/$1/ d/WAP/ o/Linux/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03DD-WRT (v\d+)[^\r\n]*\r\nRelease: ([^\r\n]+)\r\n\xff\r\ngateway login: | p/DD-WRT telnetd/ v/$2/ d/WAP/ o/Linux/ i/DD-WRT $1/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03DD-WRT (v[^\r\n]+)\r\n| p/DD-WRT telnetd/ i/DD-WRT $1/ d/WAP/ o/Linux/
match telnet m|^\xff\xfd\x18\xff\xfd \xff\xfd#\xff\xfd\x1f\xff\xfd'\xff\xfd\$$| p/Siemens HiPath PBX telnetd/ d/PBX/
match telnet m|^\xff\xfb\x01\xff\xfb\x03Welcome to Network Camera telnet daemon\r\n\r\nPassword:| p/Vivotek 3102 Camera telnetd/ d/webcam/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n\r\nU\.S\. Robotics\r\nTotal Control \(tm\) NETServer 8/16\r\n\r\nlogin: | p|USRobotics TotalControl NetServer 8/16 telnetd|
match telnet m|^\xff\xfb\x01\r\n\r\n\*\*\* ADTRAN TSU ESP \*\*\*\r\n\r\n   ENTER PASSWORD -> \xff\xfd\x03\xff\xfb\x03| p/Adtran TSU-ESP telnetd/ d/telecom-misc/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\n\rError: \r\n\rTelnet has NOT been enabled on your target VTrak 15100 system\r\n| p/VTrak 15100 telnetd/ d/storage-misc/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\r\n\nLantronix (SCS\d+) Version V([\d/().]+)\n\r\nType HELP| p/Lantronix $1 Secure Console Server telnetd/ v/$2/ d/terminal server/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n\r\nPassword :| p/Cisco 7940 VoIP Phone telnetd/ d/VoIP phone/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\(none\) login: | p/Tandberg MPS 800 telnetd/ d/media device/
match telnet m|^\xff\xfb\x03\xff\xfd\x03\xff\xfb\x01Welcome to ([-\w\s.]+)\r\nTANDBERG Codec Release ([\w.]+)| p/Tandberg MXP Video Conference appliance telnetd/ d/media device/ i/Site: $1/ v/Tandberg codec: $2/
match telnet m|^\xff\xfb\x01\xff\xfb\x01\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\n\*+\r\n\* Copyright \(c\) 1998-2006 Huawei Technologies Co\., Ltd\. All rights reserved \*\r\n\*| p/Huawei Quidway s8500 switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfb\x01\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\n\*+\r\n\*  Copyright\(c\) 1998-2007 Huawei Technologies Co\., Ltd\.  All rights reserved\.  | p/Huawei AR28-09 router telnetd/ d/router/
match telnet m|^\xff\xfb\x01\xff\xfb\x01\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\n\*+\r\n\*  Copyright\(c\) 1998-2006 Huawei Technologies Co\., Ltd\.  All rights reserved\.  \*\r\n| p/Huawei Quidway S5624P-PWR telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\r\nEnter password: | p/Alteon Networks ACEDirector switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\n\r +\*+\n\r +Welcome to P([-\w_.+]+) \n\r +\*+\n\r\n\rZyXEL Inc\., Software Release ([\w.()]+)\n\r| p/ZyXEL Prestige $1 ADSL modem telnetd/ v/$2/ d/broadband router/ 
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x03\r\n\r\n\r\nWelcome to X2301 version V\.([-\w_+. ()]+) IPSec from [\d/]+ [\d:]+\r\nsystemname is ([-\w_.]+),| p/Bintec X2301 ADSL modem telnetd/ v/$1/ i/Name $2/ d/broadband router/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x03\r\n\r\n\(([-\w_.]+)\) Enter password: | p/Ascend DSLPipe ADSL modem telnetd/ h/$1/ d/broadband router/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\n\r *\**\n\r *Welcome to Viking II\.  \n\r *\**\n\r\n\rGlobespanVirata Inc\., Software Release VIK-([-\w_.]+)\n\r| p/GlobespanVirata Viking II telnetd/ v/$1/ d/broadband router/
match telnet m|^\xff\xfb\x01\xff\xfe\x01\xff\xfd\x03\xff\xfb\x03\x1b\[1;1H\x1b\[J\x1b\[22;0H>\x1b\[1K\x1b\[999D\r\0login: | p/Asante IntraCore 35160 telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\n\r\rTelnet session\n\r\r\n\r\r\r\nCarrier Access - Adit 600\n\r\n\r[\d: /]+\n\r\n\r Login: | p/Carrier Access Adit 600 telnetd/
match telnet m|^\x1b\[2J\x1b\[1;1fATOS Telnet Server\r\n\r\nCTRL\+d to exit\n\r\n\xff\xfb\x01\xff\xfb\x03\xff\xfd\x03Init Command Line Interface\.\. \n\rBoot Version: [\d.]+\n\rBoot Date: [\d :/]+\n\rATOS Version: ([\d.]+)  \([^)]+\)\n\rATOS Date: [\d :/]+\n\rHardware: \w+\n\rProduct Code  : \d+\n\rSerial Number : (\d+)\n\rStarVoice version: ([\d.]+)\n\rStarVoice model: (\w+)\n\rLes version: [\d.]+\n\r\n\rUser name :| p/Aethra StarVoice $4 telnetd/ v/$3/ i/ATOS $1; Serial $2/ d/broadband router/
match telnet m|^\x1b\[2J\x1b\[1;1fATOS Telnet Server\r\n\r\nCTRL\+d to exit\n\r\n\xff\xfb\x01\xff\xfb\x03\xff\xfd\x03Init Command Line Interface\.\. \r\nBoot Version: [\d.]+\r\nBoot Date: [\d :/]+\r\nATOS Version: ([\d.]+)  \([^)]+\)\r\nATOS Date: [\d :/]+\r\nHardware: \w+\r\nProduct Code  : \d+\r\nSerial Number : (\d+)\r\nLAN0 MAC Address : ([A-F0-9:]+)\r\nADSL Modem SW version: [\w._-]+ *\r\nADSL Modem API version: \d+\r\nADSL Driver version: [\w._-]+\r\n([\w._-]+) release: ([\w._-]+)+\r\nHW encryption not supported\r\nVinetic fw version : [\w._-]+\r\n\r\nUser name :| p/Aethra StarVoice $4 telnetd/ v/$5/ i/ATOS $1; Serial $2; MAC $3/ d/broadband router/
match telnet m|^\xff\xfb\x01VPAD01 V([\d.]+) settings\r\nPassword:| p/E-tech VPAD01 telnetd/ v/$1/ d/VoIP adapter/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\n(NE[-\d]+) NetEngine IAD ([\d.]+) \r\nSerial num : Ethernet Address : ([-\w]+)\r\r\n\r\nPress any key to continue\.\.\.| p/Verilink NetEngine IAD $1 telnetd/ v/$2/ i/MAC $3/ d/VoIP adapter/
match telnet m|^\x1b\[0m\x1b\[2J\x1b\[01;24HHUAWEI TECHNOLOGIES,CO\.,LTD\.\x1b\[02;19H ACCESS RUNNER ADSL CONSOLE PORT\x1b| p/Huawei Access Runner ADSL telnetd/ d/broadband router/
match telnet m|^\xff\xfb\x01\xff\xfe\x01\n\r\n\r\n\r\n\n\n\n\r\t=+\n\r\t +Samsung SWL-6100AP Configuration\n\r\t| p/Samsung SWL-6100AP telnetd/ d/WAP/
match telnet m|^\r\nEfficient 5871 IDSL Router \(5871-601 / 5871-001 HW\) v([-\d.]+) Ready\r\n| p/Efficient Networks 5871 IDSL router telnetd/ v/$1/ d/broadband router/
match telnet m=^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\n\r +\*+\n\r +Welcome to [-\w_.]+\n\r +\*+\n\r\n\rD-Link (Corp|Inc)\., Software Release R([-\w_.]+)[\r\n(]= p/D-Link ADSL router telnetd/ v/$2/ d/broadband router/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\n\r\nCopyright \(c\) 2004 - 2006 3Com Corporation\. All rights reserved\.\r\n\n\r\n\r\0Username: \n\r\0Password: \n\r\0\r\n\r\nCopyright \(c\) 2004 - 2006 3Com Corporation\. All rights reserved\.\r\n\n\r\n\r\0Username: | p/3Com WX4400 WAP telnetd/ d/WAP/
match telnet m|^\xff\xfb\x01\xff\xfe\x01Connected\x1b\[K\r\n\x1b\[1;1HAironet (BR\w+) V([\d.]+) +\x1b| p/Aironet $1 telnetd/ v/$2/ d/WAP/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\0\nMAC address (\w+)\n\r\0Software version V([\d.]+) \((\d+)\) XPTEXE\r\0| p/Lantronix XPort telnetd/ v/$2 $3/ i/MAC $1/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03USR ADSL Gateway\r\nLogin: | p/USRobotics ADSL router telnetd/ d/broadband router/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\nService Processor login: | p/HP-UX GSP processor telnetd/ o/HP-UX/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfb\0\xff\xfd\0\xff\xfd\x1f\r\n.*User Access Verification\r\n\r\nUsername: |s p/Cisco telnetd/ d/router/ o/IOS/
match telnet m|^CCProxy Telnet>CCProxy Telnet Service Ready\.\r\nCCProxy Telnet>| p/CCProxy telnet configuration/ o/Windows/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03ADSL2\+ Wireless Router (\w+) \r\nSoftware Version: ([\w.]+)\r\nLogin name: | p/BT ADSL2+ $1 wireless router telnetd/ v/$2/ d/WAP/
match telnet m|^\xff\xfb\x01Symbol Access Point User/Admin password: | p/Symbol WAP telnetd/ d/WAP/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x03\xff\xfb\x05\xff\xfd\x18\xff\xfd\x1f\xff\xfd \xff\xfd!\xff\xfe\"\xff\xfc\"Username Access Verification\r\n\r\nLogin :| p/Zelax router telnetd/ d/router/
match telnet m|^\xff\xfb\x01\xff\xfb\x03Broadband Cable Device Telnet Daemon\n\r\n\rEnter user:| p|SMC8013WG cable modem/WAP telnetd| d/WAP/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\x1bmbedded Telnet Server \r\n\r\nWARNING:  Access allowed by authorized users only\.\r\n\r\n| p/WebStar DPX 2203 cable modem telnetd/ d/broadband router/
match telnet m|^\xff\xfb\x01\xff\xfd\x01\xff\xfb\x03\xff\xfd\x03\xff\xfb\x05\xff\xfd\x05Welcome to Telnet Server ([\d.]+)\r\n\x1b\[0m\x1b\[2J\x1b\[05;28HDimension Switch (ES-\w+)\x1b\[07;22H| p/ZyXEL $2 dimension switch telnetd/ v/$1/ d/switch/
match telnet m|^\r\n\r\nPassword required, but none set\r\n| p/Cisco catalyst switch telnetd/ i/no password set/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x03\xff\xfd\x18\xff\xfd\x1fWelcome to your TiVo\r\n\r\n=\[tivo:root\]-# | p/TiVo telnetd/ i/OPEN/ d/media device/
match telnet m|^\xff\xfa\x18\x01\xff\xf0\xff\xfb\x01\xff\xfb\x03AMBIT Cable Modem\r\n\r\nlogin: | p/Ambit cable modem telnetd/ d/broadband router/
match telnet m|^\xff\xfb\x01\x1b\[2J\x1b\[0m\x1b\[1;1H\x1b\[2;1H\x1b\[3;1H\x1b\[4;1H ###      ###  ###########   ##########  #############| p/Nortel Baystack 470-48t switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01AN-30 Ver\. ([\d.]+) \(c\) Copyright 2000-2002 Redline Communications Inc\.\r\n\r\nUsername:\0| p/Redline Communications AN-30 wireless bridge telnetd/ v/$1/ d/WAP/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\r\nNortel Networks Layer2-3 GbE Switch Module\.\r\n\r\n\r\nEnter password: | p/Nortel Gbe switch telnetd/ d/switch/
match telnet m|^refused in\.telnetd from [-\w_.]+ logged\n| p/tcpwrapped telnetd/ i/refused/
match telnet m|^\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r.*Broadband Satellite HN7000S VSAT|s p/Hughes HN7000S Satellite Modem telnetd/ d/router/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n\n\*+\r\n\*  Welcome to Print Server  \*\r\n\*     Telnet Console        \*\r\n\*+\r\n\r\nServer Name    :  ([\w._ -]+)\0\r\nServer Model   :  APSUSB1\0+\r\nF/W Version    :  ([\w._-]+)  \0\0\0\0\r\nMAC Address    :  ([\w ]+)\r\nUptime         :  ([^\r\n]+)\r\n| p/AirLink USB print server telnetd/ i/name $1; MAC $3; uptime $4/ d/print server/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\n\r +\*+\n\r +Welcome to SMC DSL MODEM\n\r +\*+\n\r\n\rSMC Network Inc\., Software Release ([^\r\n]+)\n\r| p/SMC DSL modem telnetd/ v/$1/ d/router/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfb\x1fError2 negotiated with client 18 and get 1 char is a a d\..*VOIP CPE firmware +VG112-D51\(S\) +V([\d.]+)|s p/VG112-D51 VoIP CPE telnetd/ v/$1/ d/VoIP adapter/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\n\r +\*+\n\r +Welcome to Viking  \n\r +\*+\n\r\n\rGlobespanVirata Inc\., Software Release ([\w/.]+)\n\r| p/Viking router telnetd/ v/$1/ d/router/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\xff\xfd\x1fWelcome to OSE Shell OSE([\d.]+)\.\r\n\$ | p/Interpeak AB embedded security device telnetd/ i/OSE $1/ d/security-misc/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\x1b\[2J\x1b\[0;0H\x1b\[1;32m                    \.-------------\.| p/stchat telnetd/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\x1b\[2J\x1b\[2;28H\x1b\[m\x1b\[1mNetopia (\w+) v([\d.]+)\x1b| p/Netgear Netopia $1 router telnetd/ v/$2/ d/router/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\n\((FSM\w+)\) \r\nUser:| p/Netgear $1 router telnetd/ d/router/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03Access DENIED\.\r\n| p/OpenWrt telnetd/ d/WAP/
match telnet m|^\r\nCP2E Control Console\r\nConnected to Host: ([-\w_.]+)\r\n| p/Creston CP2E control telnetd/ d/specialized/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\xff\xfb\x03([\w-]+) Ver ([-\w_.]+) TELNET server\.\r\0\nCopyright \(C\) [\d-]+ KYOCERA CORPORATION\r\0\nCopyright \(C\) [\d-]+ KYOCERA MITA CORPORATION\r\0\nlogin:| p/Kyocera $1 printer telnetd/ v/$2/ d/printer/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\xff\xfb\x03([\w-]+) Ver ([-\w_.]+) TELNET server\.\r\0\nCopyright\(C\)[\d-]+ KYOCERA MITA Corporation\r\0\nCopyright\(C\)[\d-]+ Revised Edition KYOCERA MITA Corporation\r\0\nAll Rights Reserved\.\r\0\nlogin: | p/Kyocera $1 printer telnetd/ v/$2/ d/printer/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\xff\xfb\x03(NS-\w+) Ver ([-\w_.]+) TELNET server\.\r\0\nCopyright \(C\) 2001-2002 KYOCERA MITA CORPORATION\r\0\nlogin: | p/Okidata $1 printer telnetd/ d/printer/ v/$1/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\xff\xfb\x03Imagistics (\w+) Ver ([\d.]+) TELNET server\.\r\0\n\r\0\nlogin: | p/Imagistics $1 printer telnetd/ v/$2/ d/printer/
match telnet m=\xff\xfb\x01\r\n\r\n#\r\n\| Siemens I-Gate LAN 2\r\n\| Ver\. ([\d.]+) / [\d.]+\r\n\| SN\.  (\w+)\r\n\|= p/Siemens I-Gate LAN 2 telnetd/ v/$1/ i/Serial $2/ d/router/
match telnet m|^\xff\xfb\x01\x1b\[1;1H\x1b\[2K\x1b\[2;1H\x1b\[2K\x1b\[3;1H\x1b\[2K\x1b\[4;1H\x1b\[2K\x1b\[5;1H\x1b\[2K\x1b\[6;.*Business Policy Switch 2000| p/Nortel Business Policy Switch 2000 telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\r\nHP ProLiant BL p-Class C-GbE2 Interconnect Switch B\r\n| p/HP ProLiant BL p-Class C-GbE2 switch telnetd/ d/switch/
match telnet m|^\x11\x11\x11\*\*[-\w_.]+\r\r\[CONNECT TCP/IP/[\d.]+/TELNET\]\r\nT-Mail v\.([^ ]+) \(C\) 1992-99 by Andy Elkin\r\n\*\*| p/T-Mail Fidonet BBS telnetd/ v/$1/ o/Windows/
match telnet m|^BeanShell ([-\w_.]+) - by Pat Niemeyer \(pat@pat\.net\)\nbsh % | p/BeanShell java scripting telnet console/ v/$1/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\xff\xfd\x1f\r\n\(Aruba800\) \r\nUser: | p/Aruba800 switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\x1b\[1;1H\x1b\[2K\x1b\[2;1H\x1b\[2K\x1b\[3;1H\x1b\[2K\x1b\[4;1H\x1b\[2K\x1b\[5;1H\x1b\[2K\x1b\[6;1H\x1b.*BayStack 420 |s p/Nortel BayStack 420 switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x03\xff\xfd\x18\xff\xfb\x01\xff\xfd\x1f\xff\xfd!\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\nUser Access Login\r\n\r\nPassword:| p/Adtran Netvanta 3200 router telnetd/ d/router/
match telnet m=^\xff\xfb\x01\xff\xfb\x03\r\n\r\n#\r\n\| ELSA LANCOM 1000 Office\r\n\| Ver\. ([-\w_.]+) / [\d.]+\r\n\| SN\.  ([\w.]+)\r\n\| Copyright \(c\) ELSA AG, Aachen\r\n\r\n([-\w_.]+), Verbindung= p/ELSA Lancom 1000 ISDN router telnetd/ v/$1/ i/Serial $2/ h/$3/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\xff\xfb\x03SHARP (MX-\w+) Ver ([-\w_.]+) TELNET server\.| p/Sharp $1 printer telnetd/ v/$2/ d/printer/
match telnet m|^\xff\xfb\x03\xff\xfd\x18\xff\xfb\x01\xff\xfd\x1f\xff\xfd!\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\n\r\nUser Access Login\r\n\r\nUsername:| p/Procurve Secure Router telnetd/ d/router/
match telnet m|^\r\nSorry, unable to access input device\.\r\n$| p/Netgear WG102 WAP telnetd/ d/WAP/ i/disabled/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\n\r +\*+\n\r +Welcome to ([-\w_.]+) *\n\r +\*+\n\r\n\rZoom Software Release Zoom (X5 GS Ver [-\w_.]+)\n\r| p/Zoom ADSL modem telnetd/ d/broadband router/ v/$2/ h/$1/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\xff\xfb\x03IB-21E Ver ([\d.]+) TELNET server\.\r\0\nCopyright \(C\) 2001 KYOCERA CORPORATION\r\0\nlogin:| p/Kyocera IB-21E printer telnetd/ v/$1/ d/printer/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\nOpenDreambox ([-\w_.]+) (dm\w+)\r\n| p/Dreambox $2 telnetd/ v/$1/ d/media device/
match telnet m|^\xff\xfb\x01\xff\xfb\x03Welcome to (DCS-\w+) telnet daemon\r\n\r\nPassword:| p/D-Link $1 webcam telnetd/ d/webcam/ 
match telnet m|^\xff\xfb\x01\r\nVoIP Phone V([-\w_.]+) settings\r\nPassword:| p/Soyo G668 VoIP phone telnetd/ v/$1/ d/VoIP phone/
match telnet m|^\xff\xfb\x01\r\nAIRAYA login: $| p/Airaya WAP config telnetd/ d/WAP/
match telnet m|^\xff\xfb\x03\xff\xfd\x03\xff\xfb\x01Welcome to VCSCDCS2\r\r\nTANDBERG Codec Release L([\d.]+)\r\r\n| p/Tandberg T150 Personal VoIP phone telnetd/ d/VoIP phone/ i/Tandberg codec $1/
match telnet m=^\d+\|Connected to foobar2000 Control Server v([\d.]+)= p/foobar2000 remote control telnetd/ v/$1/ o/Windows/
match telnet m|^\xff.\x01\0?\xff\xfd.*Welcome to ViewStation.*Password:|s p/Polycom ViewStation Video Conferencing telnetd/ d/webcam/
match telnet m|^AD6680 Gateway Software\r\n[-\w_]+  \(MAC  ([\w:]+)\)\r\n| p/Netcomm V300 VoIP adapter telnetd/ d/VoIP adapter/ i/MAC $1/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\r\n\r([\d.]+)\r\n\rLinux ([-\w_.]+) on a armv4tl \([\d:]+\)\r\n\r([-\w_.]+) login:| p/AXIS webcam telnetd/ v/$1/ i/Linux $2/ o/Linux/ d/webcam/ h/$3/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\r\nHP ProLiant BL p-Class C-GbE2 Interconnect Switch A\.\r\n| p/HP ProLiant switch telnetd/ d/switch/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03Netgear DM111 ADSL2\+ Modem \r\nSoftware Version: ([-\w_.]+)\r\nLogin name:| p/Netgear DM111 broadband router telnetd/ d/broadband router/ v/$1/
match telnet m|^\xff\xfb\x03\xff\xfd\x03\xff\xfb\x01\r\nPrecise/RTCS v([\d.]+) Telnet server\r\n\r\0\r\nService Port Manager Active\r\0\r\n<Esc> Ends Session\r\0\r\n| p/Liebert OpenComms remote management telnetd/ d/remote management/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n\r\n\*+\r\n\*  Welcome to Print Server  \*\r\n\* +Telnet Console +\*\r\n\*+\r\n\r\nServer Name    :  ([\w._-]+)\0\0\0\0\0\0\r\nServer Model   :  2U1P Print Server\0+\r\nF/W Version    :  ([\w._-]+).*\r\nMAC Address    :  ([\w ]+)| p/Xterasys 2U1P print server telnetd/ d/print server/ v/$2/ i/name $1; MAC $3/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\nScarlet One\r\nFirmware version: ([-\w_.]+)\r\nScarlet\r\n\r\nPlease login:| p/Scarlet One telnetd/ i/Firmware $1/ d/VoIP adapter/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\xff\xfd\x1f\xff\xfd\x18\r\ntelnet session telnet\d+ on /dev/ptyb\d+\r\n\r\nlogin: | p/Extreme Networks switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\r\n-> \*\*\*  EPSON Network Print Server \(([^)]+)\)  \*| p/Epson $1 print server telnetd/ d/print server/
match telnet m|^\xff\xfb\x01\xff\xfd\x1f\xff\xfb\x03\r\n.*KpyM Telnet/SSH Server - fully functional unregistered version\.\r\n|s p/KpyM telnetd/ i/Unregistered/ o/Windows/
match telnet m|^\xff\xfb\x03\xff\xfd\x03\xff\xfb\x01\r\n\r\nMMC Technology Telnet\r\nMW-3000AP   \w+\( Combo ([-\w_.]+) \)\r\n\r\n| p/MMC MW-3000AP telnetd/ d/WAP/ i/$1/
match telnet m|^\xff\xfb\x01\r\n\"D-Link Access Point - AVC\" login: | p/D-Link DWL-2100AP telnetd/ d/WAP/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\n\r.*\n\r\n\rSoftware Release R([-\w_.]+)\([^)]+\)\n\rCopyright \(c\) 2001-2003 by D-Link, Inc\.\n\r\n\rlogin: |s p/D-Link D-500G telnetd/ d/broadband router/ v/$1/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\r\nGO Networks MBW System - WLP\r\nSW Version: ([-\w_.]+)\r\n\r\nUser Name:| p/GO Networks MBW telnetd/ d/WAP/ v/$1/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n +Welcome to Media Gateway Processor\r\n +FW version ([-\w_.]+)\r\n\r\nLogin:| p/Avaya Call Manager telnetd/ i/Firmware $1/ d/PBX/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfe!\xff\xfd\x1f\xff\xfe\"\xff\xfe\x03IRRd version ([-\w_.]+) \[\w+\]\r\n\r\nUser Access Verification| p/Merit Internet Routing Registry telnet config/ v/$1/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\nWelcome to the WhatRoute TELNET Server\.\r\n| p/WhatRoute telnetd/ o/Mac OS/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\nCNU-550pro login: | p/C-motech CNU-550pro telnetd/ d/broadband router/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03picotux login: | p/Picotux telnetd/ o/Linux/ d/specialized/
match telnet m|^\xff\xfb\x03\xff\xfd\x18\xff\xfb\x01\xff\xfd\x1f\xff\xfd!\r\nCadant C3 CMTS\r\n| p/Cadant C3 Cable Modem Termination Server telnetd/ d/specialized/
match telnet m|^\r\n\(c\) Copyright 2005, Extron Electronics, IPL T S2, V([\d.]+),| p/Extron IPL T S2 telnetd/ d/media device/ v/$1/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\n.*HM410dp ADSL2\+ Router\r\n\r\nLogin:|s p/Ericsson HM410dp ADSL router telnetd/ d/broadband router/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03Dynalink ADSL2\+ Router RTA1320NZ .*\r\nSoftware Version: ([-\w_.]+)\r\n| p/Dynalink RTA1320NZ ADSL router telnetd/ d/broadband router/ v/$1/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\xff\xfb\x03NS-30G Ver ([-\w_.]+) TELNET server\.\r\0\nCopyright \(c\) \d+ KYOCERA| p/Kyocera NS-30G printer telnetd/ d/printer/ v/$1/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\nWelcome to MediaMVP!\r\n| p/Hauppauge MediaMVP telnetd/ d/media device/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x03\r\n\r\n\r\nWelcome to X4100 version V\.([-\w_.]+) Rev\. (\d+) \(Patch (\d+)\) from [\d/]+ [\d:]+\r\nsystemname is ([-\w_.]+),| p/Sun X4100 telnetd/ d/terminal server/ v/$1.$2.$3/ h/$4/
match telnet m|^\xff\xfe\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03login: $| p/Axis 2100 Network Camera telnetd/ d/webcam/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\nZyXEL Corporation Embedded Telnet Server \(c\) 2000-2003\r\n| p/ZyXEL Prestige cable modem telnetd/ d/broadband router/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\nHGW EC506 login: | p/Huawei EC506 WAP telnetd/ d/WAP/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\0\n\*\*\* Lantronix Universal Device Server \*\*\*\r\0\nSerial Number (\d+)  MAC address (\w+)\n\r\0Software version V([\w._-]+) | p/Lantronix UDS10 ethernet-serial telnetd/ i/serial $1; MAC $2/ v/$3/ d/specialized/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\*\*\* Lantronix UDS1100 Device Server \*\*\*\r\0\nMAC address (\w+)\n\r\0Software version V([\w._-]+) \((\d+)\) \r\0\nPassword :| p/Lantronix UDS1100 ethernet-serial telnetd/ i/MAC $1/ v/$2 $3/ d/specialized/
match telnet m|^\xff\xfb\x03\xff\xfd\x03\xff\xfb\0\xff\xfd\0\xff\xfb\x01\r\nMinix  (.*)\r\n\r\n([\w._-]+) login:| p/Minix telnetd/ o/Minix/ v/$1/ h/$2/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03(BCM\w+) ADSL Router\r\n| p/Broadcom $1 ADSL router telnetd/ d/broadband router/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03DSL Router\.  Welcome!\r\nLogin: | p/Broadcom BCM96345 ADSL router telnetd/ d/broadband router/
match telnet m|^\xff\xfb\x01\xff\xfb\x01\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\n\*+\r\n\*  Copyright\(c\) 2004-2006 3Com Corp\. and its licensors\.| p/3Com Superstack switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\r\n\r\nEnter password: | p/Nortel Alteon switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\n\r +\*+\n\r +Welcome  \n\r +\*+\n\r\n\rSoftware Release ([\w._]+)\n\rCopyright \(c\) 2001-2004\n\r\n\rlogin: | p/Siemens C2-010-I ADSL router telnetd/ d/broadband router/ v/$1/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03Dynalink Wireless ADSL2\+ Router (\w+) \r\nSoftware Version: ([\w._-]+)\r\nLogin name: | p/Dynalink $1 WAP telnetd/ d/WAP/ v/$2/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\r\n\r\nProduct type: Avaya (\w+) Media Gateway Release ([\w._-]+)\r\n\r\n\r\n\r\nLogin: | p/Avaya $1 media gateway telnetd/ v/$2/ d/media device/
match telnet m|^\xff\xfd\0\xff\xfd\x1fWelcome to MLDonkey ([\w._-]+)\n\x1b\[36mWelcome on mldonkey command-line\x1b| p/MLDonkey telnetd/ v/$1/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\n\r +\*+\n\r +\*   POSTEF ADSL Modem/Router ([\w._-]+) | p/POSTEF $1 ADSL router telnetd/ d/broadband router/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\xff\xfb\x03Belkin Network USB Hub Ver ([\w._-]+) TELNET server\.| p/Belkin network USB hub telnetd/ d/specialized/ v/$1/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\*+\r\n\r\* +\*\r\n\r\*   The Gemini Project   \*\r\n\r\* +\*\r\n\r\*+\r\n\r\r\n\rwelcome on your dreambox! - Kernel ([\w._-]+) | p/Dreambox media device telnetd/ i/Linux $1/ o/Linux/ d/media device/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\*+\r\n\r\* +\*\r\n\r\* +The Gemini Project v([\w. ]+) +\*\r\n\r\* +XD mod, date: ([\d.]+) +\*\r\n\r\* +!!! WITHOUT BOMB !!! +\*\r\n\r\* +\*\r\n\r\*+\r\n\r\r\n\rwelcome on your dreambox! - Kernel ([\w._-]+) | p/Dreambox media device telnetd/ i/Linux $1/ o/Linux/ d/media device/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\nPLi dm500 Garnet \d+ \(based on ([\w._-]+)\)\r\n\rwelcome on your dreambox! - Kernel ([\w._-]+) \([\d:]+\)\.\r\n\rdreambox login: | p/Dreambox 500 media device telnetd/ i/Linux kernel $2; PLi image Garnet, based on $1/ o/Linux/ d/media device/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\nPLi\xae jade dm7020si\r\n\r\r\n\rdm7020si login: | p/Dreambox 7020si media device telnetd/ i/PLi image jade/ d/media device/ o/Linux/
match telnet m|^\xff\xfb\x01\xff\xfb\x01\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\n\*+\r\n\*          All rights reserved \(1997-2004\)              \*\r\n\*      Without the owner's prior written consent,| p/Huawei Quidway Eudemon firewall telnetd/ d/firewall/ 
match telnet m|^\xff\xfb\x01\xff\xfb\x01\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\n\*+\r\n\* Copyright\(c\) 1998-2008 Huawei Technologies Co\., Ltd\.                      \*\r\n\* Without the owner's prior written consent,| p/Huaweir Quidway S8505 switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfb\x01\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\n\*+\r\n\*  Copyright\(c\) 2004-2008 3Com Corp\. and its licensors\. All rights reserved\.   \*\r\n\*  Without the owner's prior written consent,| p/3Com 4500 switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfb\x01\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\n\*+\r\n\*          All rights reserved \(1997-2006\)              \*\r\n\*      Without the owner's prior written consent, +\*\r\n| p/3Com 4500 switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfb\x01\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\n\*+\r\n\* Copyright \(c\) 2004-2009 Hangzhou H3C Tech\. Co\., Ltd\. All rights reserved\.  \*\r\n\* Without the owner's prior written consent,| p/H3C switch/ d/switch/
match telnet m|^Welcome to the DataStage Telnet Server\.\r\0\r\nEnter user name: | p/WebSphere DataStage telnetd/
match telnet m|^\xff\xfb\x01\xff\xfd\x03-?>?\r\nHi, my name is :     ([^\r\n]+)\r\nHere is what I know about myself:\r\nModel:               VSX ([\w._-]+)\r\nSerial Number:       (\w+)\r\nSoftware Version:    Release ([\w._-]+) -| p/VSX $2 telnetd/ d/telecom-misc/ i/name $1; serial $3/ v/$4/
match telnet m|^\r\nSorry, this system is engaged by a rlogin session\.\r\nHost IP address: ([\d.]+)\.\nLogin name: ([\w._-]+)\.\n| p/3Com LANplex switch telnetd/ i/in use by $2 from $1/ d/switch/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\xff\xfb\x03\xff\xfb\x01.*\r\n\r\nUser Access Verification\r\n\r\nUsername: |s p/Cisco ASA firewall telnetd/ d/firewall/
match telnet m|^Connected\r\nUse log command to LOGON\r\n$| p/IBM 2218 Link Level Converter telnetd/ d/specialized/
match telnet m|^\xff\xfb\x01\xff\xfb\x03Grandstream ([\w-]+) Command Shell\r\nPassword: | p/Grandstream $1 VoIP phone telnetd/ d/VoIP phone/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03Grandstream ([\w-]+)  V([\w.]+) Command Shell| p/Grandstream $1 VoIP router telnetd/ v/$2/ d/VoIP adapter/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03Grandstream ([\w._-]+) Command Shell Copyright [\d-]+\r\nPassword: | p/Grandstream $1 VoIP phone telnetd/ d/VoIP phone/
match telnet m|^Welcome to LDK-300 system\. Press enter\.\r\nYour address is| p/LG Aria LDK-300 PBX telnetd/ d/PBX/
match telnet m|^\d+-NENET AB Ethernet Com Card V([\w._-]+)  Built .*\r\nDebugOutput: \d+  DebugLevel: \d+\r\nHit 0-4 to change debug level, S for socket status\r\n| p/NENET AB ethernet telnet config/ v/$1/
match telnet m=^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03ADSL Router\r\nLogin (?:user|name): = p/ADSL router telnet config/ d/broadband router/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03AH4021\r\nLogin: | p/AliceBox AH4021 telnet config/ d/broadband router/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\nWelcome to Linux \(ZEM300\) for MIPS\r\n\rKernel ([\w._-]+) ([\w._-]+) on an MIPS\r\n| p/ZKSoftware ZEM300 embedded Linux telnetd/ o/Linux/ i/Kernel $1; MIPS/ h/$2/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\n\r\0SNTP Version ([\d.]+) Server ([\w._-]+)\n\r\0\r\0\nMAC address (\w+)\n\r\0Software version V[\d.]+ \(\d+\) ([\w._-]+)\r\0\nPassword :| p/Larus 54580 NTP clock telnetd/ v/$2/ i/NTP $1; MAC $3/ h/$4/
match telnet m|^uShare \(([\w._-]+)\) \(Built .*\)\nFor a list of registered commands type \"help\"\n\n> | p/GeeXboX uShare telnetd/ v/$1/
match telnet m|^SMPlayer ([\w._-]+)\r\nType help for a list of commands\r\n| p/SMPlayer telnetd/ v/$1/
match telnet m|^S: FTGate [\w._-]+ \[Build ([\w._-]+) .*\]\n\r| p/Floosietek FTgate telnetd/ v/$1/
match telnet m|^Slirp command-line ready \(type \"help\" for help\)\.\r\nSlirp> | p|Slirp PPP/SLIP-on-terminal emulator telnetd|
match telnet m|^Slirp v([\w._-]+)(?: \(BETA\))?(?: FULL_BOLT)?\n\nCopyright \(c\) 1995,1996 Danny Gasparovski and others\.\n| p|Slirp PPP/SLIP-on-terminal emulator telnetd| v/$1/
match telnet m|^Sorry, already connected\.\r\n$| p|Slirp PPP/SLIP-on-terminal emulator telnetd| i/connection in progress/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\xff\xfb\x01\xff\xfb\x03\r\nCopperJet ([\w._-]+) RouterPlus .*\r\nFirmware version: ([\w._ -]+)\r\nAllied Data Technologies\r\n\r\nPlease login: | p/Allied Data CopperJet $1 telnetd/ v/$2/ d/broadband router/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03ASUS500ROUTER login: | p/ASUS WL-500g WAP telnetd/ d/WAP/
match telnet m|^\n\rMordor MUD\n\r  Mordor v([\w._-]+)\n\rProgrammed by:\n\r  Brooke Paul, Paul Telford & John P\. Freeman\n\r| p/Mordor MUD telnetd/ v/$1/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03.*Firmware Version: ([\w._-]+)\r\n\rBuilt: .*\r\n\rOA Bay Number:  \d+ \r\n\rOA Role: .*\r\n\r([\w._-]+) login:|s p/HP BladeSystem Onboard Administrator telnetd/ i/FW $1/ h/$2/ d/remote management/
match telnet m|^\xff\xfb\x01\xff\xfb\x03Welcome to the Windows CE Telnet service on MP370\r\n\r\nPocket CMD v ([\w._-]+)\r\n\\> \n\r\n\\> \\>| p/MP370 PDA Pocket CMD telnetd/ v/$1/ d/PDA/
match telnet m|^\xff\xfb\x01\r\n3Com Access Point 7760 login: | p/3Com 7760 WAP telnetd/ d/WAP/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03 login: | p/Netgear DG834GT telnetd/ d/broadband router/
match telnet m|^\r\nSiemens 5940 T1E1 \[COMBO\] Router \(5940-001\) v([\w._-]+) Ready\r\n\xff\xfb\x01\xff\xfb\x03\xff\xfd\x01\xff\xfe\x01Username: | p/Siemens 5940 T1E1 router telnetd/ d/router/ v/$1/
match telnet m|^\r\n\*+\r\n\* +Network Services Processor                \*\r\n\*                      Version ([\w._-]+)                       \*\r\n\*                ESI \(Estech Systems, Inc\.\)| p/Estech Systems Inc Network Services Processor telnetd/ v/$1/ d/telecom-misc/
match telnet m|^\xff\xfd\x03\xff\xfb\x01\xff\xfb\x03PRICOM 3100 Ver ([\w._-]+) TELNET server\.\r\0\nCopyright \(C\) 2002-2004 silex technology, Inc\.\r\0\nlogin:| p/PRICOM 3100 print server telnetd/ v/$1/ d/print server/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\r\r\n\r\r\nWelcome to Aerohive Wireless Product\r\r\n\r\r\nlogin: | p/Aerohive WAP telnetd/ d/WAP/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\nLexmark International Telnet\r\n\r\nlogin: | p/Lexmark C500 printer telnetd/ d/printer/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03Siemens ADSL SL-2141 IS \r\nSoftware Version: ([\w._-]+)\r\n| p/Siemens ADSL SL-2141 IS telnetd/ d/broadband router/ v/$1/
match telnet m|^\xff\xfb\x03\xff\xfb\x01Alcatel-Lucent: A7510\r\nA7510_(R\d+) .*\r\n\r\n\r\nLogin: | p/Alcatel-Lucent A7510 Media Gateway telnetd/ v/$1/ d/telecom-misc/
match telnet m|^\xff\xfd\x18\xff\xfd\x1f\xff\xfd!\xff\xfd\x17\xff\xfb\x01\xff\xfb\x03\xff\xfd \xff\xfd#\r\n\r\n Welcome to OpenVMS \(TM\) VAX Operating System, Version V([\w._-]+)    \r\n\r\n\r\0Username: | p/MultiNet OpenVMS telnetd/ o/OpenVMS/ i/OpenVMS $1; VAX/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\n\r\n>>>  System ([\w._-]+) - OpenVMS Alpha V([\w._-]+)  <<<\r\n\r\n\rUsername: | p/OpenVMS telnetd/ h/$1/ o/OpenVMS/ i/OpenVMS $2; Alpha/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\n\r\n Welcome to OpenVMS \(TM\) Alpha Operating System, Version V([\w._-]+)  \r\n\r\n\rUsername: | p/OpenVMS telnetd/ o/OpenVMS/ i/OpenVMS $1; Alpha/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\r\nGbE2c Ethernet Blade Switch for HP c-Class BladeSystem\.\r\n\r\nCopyright\(C\)2003 Hewlett-Packard Development Company, L\.P\.\r\n\r\n\r\nEnter password: | p/HP GbE2c Ethernet Blade Switch telnetd/ d/switch/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\nWelcome to \r\n\r\r\n\r       ###### .*Have a good time !! ;-\)\r\n\rCyberVia login:|s p/Cybervia media center telnetd/ d/media device/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\*+\r\n\r\* +\*\r\n\r\*   The Gemini Project   \*\r\n\r\* +\*\r\n\r\*+\r\n\r\r\n\rOpenDreambox ([\w._-]+) (\w+)\r\n| p/Dreambox $1 telnetd/ i/OpenDreambox $2/ d/media device/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfb\x01\xff\xfb\x03\r\r\n\*+\r\n\r\* +\*\r\n\r\*   The Gemini Project   \*\r\n\r\* +\*\r\n\r\*+\r\n\r\r\n\rOpenDreambox ([\w._-]+) (\w+)\r\n| p/Dreambox $1 telnetd/ i/OpenDreambox $2/ d/media device/
match telnet m|^\xff\xfe\"\xff\xfb\x01\x1b\[7m\x1b\[f\x1b\[9B\x1b\[9B\x1b\[5B  ArrowKey Or AZ:Move Cursor, Enter:Select, ESC:Escape, L:Line Draw, X:Redraw   \x1b\[0m\x1b<\x1b>\x1b\[\?25l\x1b\[0m\x1b\[2J\x1b\(B\x1b\)0\x0f\x1b\[7m\x1b\[f +Areca Technology Corporation RAID Controller| p/Areca RAID-Controller telnetd/ d/storage-misc/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\x1b\[0m\x1b\[2J\x1b\[0m\x1b\[2J\x1b\[21;1H\x1b\[0m\*+\x1b\[22;1H\x1b\[0mMessage Area:\x1b\[24;1H\x1b\[7mCTRL\+R = Refresh +\x1b\[9;16H\x1b\[0mSSR22i Stackable Fast Ethernet Switch Console Management| p/Amer.com SSR22i switch telnetd/ d/switch/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03U\.S\. Robotics ADSL 4-Port Router\r\nLogin: | p/USRobotics ADSL router telnetd/ d/broadband router/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03Siemens ADSL SL2-141-I HSN2 \r\nSoftware Version: ([\w._-]+)\r\nLogin name: | p/Siemens ADSL SL2-141-I HSN2 ADSL telnetd/ d/broadband router/ v/$1/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\n\r\0\*\*\* Mitsubishi ProjectorView Server \*\*\*\r\0\nMAC address (\w+)\n\r\0Software version V([\w._-]+) \((\d+)\) MELCO\r\0\n\n\r\0Press Enter for Setup Mode \n\r\0| p/Mitsubishi Electric XD1000 ProjectorView telnetd/ v/$2 $3/ i/MAC $1/ d/media device/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03ROTAL Wireless ADSL2\+ Router RTA1025W \r\nSoftware Version: ([\w._-]+)\r\nLogin name: | p/ROTAL RTA1025W WAP telnetd/ d/WAP/ v/$1/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03 === IMPORTANT ============================\r\n  Use 'passwd' to set your login password\r\n  this will disable telnet and enable SSH\r\n.*\r\n KAMIKAZE \(bleeding edge, (r\d+)\)|s p/BusyBox telnetd/ i/no password; OpenWrt Kamikaze $1/ o/Linux/ d/WAP/
match telnet m#\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03 === IMPORTANT ============================\r\n  Use 'passwd' to set your login password\r\n  this will disable telnet and enable SSH\r\n ------------------------------------------\r\n\r\n\r\nBusyBox v(.*) built-in shell \(ash\)\r\n.*\r\n KAMIKAZE \(([^)]*)\)#s p/BusyBox telnetd/ v/$1/ i/no password; OpenWrt Kamikaze $2/ o/Linux/ d/WAP/
match telnet m#\xff\xfd\x01\xff\xfd\x1f\xff\xfb\x01\xff\xfb\x03 === IMPORTANT ============================\r\n  Use 'passwd' to set your login password\r\n  this will disable telnet and enable SSH\r\n ------------------------------------------\r\n\r\n\r\nBusyBox v(.*) built-in shell \(ash\)\r\n.*\r\n KAMIKAZE \(([^)]*)\)#s p/BusyBox telnetd/ v/$1/ i/no password; OpenWrt Kamikaze $2/ o/Linux/ d/WAP/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n === IMPORTANT ============================\r\n  Use 'passwd' to set your login password\r\n  this will disable telnet and enable SSH\r\n ------------------------------------------\r\n\r\n\r\nBusyBox v(.*) built-in shell \(ash\)\r\nEnter 'help' for a list of built-in commands\.\r\n\r\n ___        ___  ___                                                 \r\n\(  _`\\  _ /'___\)'___\)      Bifferboard mini-distribution v([\w._-]+)\r\n| p/BusyBox telnetd/ o/Linux/ v/$1/ i/Bifferboard $2/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03                        =======================\r\n                               DSL-500B       \r\n                        =======================\r\nLogin:| p/D-Link DSL-500B telnetd/ d/broadband router/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n\r\n\r\nAG 5000\r\n\r\n\r\nLogin: | p/Nomadix AG 5000 telnetd/ d/WAP/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\nWelcome to Linux \(ZEM500\) for MIPS\r\n\rKernel ([\w._-]+) \w+ on an MIPS\r\n\rZEM500 login: | p/ZKSoftware ZEM500 fingerprint reader telnetd/ d/security-misc/ i/Linux $1; MIPS/ o/Linux/
match telnet m|^\xff\xfb\x01\xff\xfe\x01Connected\r\n\n\rAironet BR500E V([\w._-]+)                Main Menu| p/Cisco Aironet BR500E telnetd/ v/$1/ d/WAP/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03login: | p/D-Link 524 or WBR-1310 WAP telnetd/ d/WAP/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03TrioLink \(ADSL IAD\)\r\nLogin: | p/Nortel-LG VoIP IAD telnetd/ d/PBX/
match telnet m|^Linux ([\w._-]+) \[INSTALL: [\d-]+\]\nLASTPATCH: [\d-:]+\n| p/Netkit-telnetd/ o/Linux/ i/Linux $1/
match telnet m|^\xff\xfb\0\xff\xfd\0\xff\xfb\x01\xff\xfd\x01\xff\xfb\x03\xff\xfd\x03\x1b\[0;37;40m\x1b\[2J\x1b\[1;1HLogin Name:  | p/HP Remote Insight Lights-Out telnetd/ d/remote management/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03Xcelerator IP \r\nLogin: | p/Vertical Xcelerator IP telnetd/ d/VoIP adapter/
match telnet m|^Console is locked by another telnet/SSH application!\n| p/Arris tm602g cable modem telnetd/ i/console in use/ d/broadband router/
match telnet m|^odec=\d+ u=\d+, p=\d+, i=\d+, max entries = \d+ \r\n\d+: IMGREQUEST: request_stats, image buffers available = \d+ \r\n\d+: MAIN: (\d+) images\(J=\d+, P=\d+, I=\d+\) stored on disk in last minute| p/Dedicated Micros Digital Sprite 2 DVR debug telnetd/ i/$1 images saved in last minute/ d/webcam/
match telnet m|^\r\nSiemens 5940 T1E1 \[COMBO\] Router \([\w._-]+\) v([\w._-]+) Ready\r\n\xff\xfb\x01\xff\xfb\x03\xff\xfd\x01\xff\xfe\x01Username: | p/Siemens 5940 T1E1 router telnetd/ d/router/ v/$1/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\n\r\nWelcome to Dinion-IP-NWC [\d.]+ from [\d.]+\r\n| p/Dinion IP NWC webcam telnetd/ d/webcam/
match telnet m|^\xff\xfb\x01\xff\xfb\x03Welcome to the Agilent PNA Network Analyzer at ([\w._-]+)\r\n\r\nSCPI> | p/Agilent PNA Network Analyzer SCPI telnetd/ d/specialized/ h/$1/
match telnet m=^\xff\xfb\x01\xff\xfb\x03\r\n\r\n#\r\n\| ELSA LANCOM DSL/([\w._-]+) Office\r\n\| Ver\. ([\w._-]+) / ([\w._-]+)\r\n\| SN\.  (\w+)\r\n\| Copyright \(c\) ELSA AG, Aachen\r\n\r\n= p|ELSA Lancom DSL/$1 Office router telnetd| d/router/ v/$2 $3/ i/Serial $4/
match telnet m|^\n\rCMI SEC\n\rProgram: +\d+\n\rMajor\.Minor\.Rel:  ([\w._-]+)\n\rMAC Address:      ([\w:]+)\n\r\n\rPress <ENTER> to go into setup mode\.| p/ADP IP Timeclock telnetd/ v/$1/ i/MAC $2/ d/specialized/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\xff\xfe\x01\xff\xfd\0\r\nser2net port \d+ device (/dev/[-\w_]+) \[\d+ \w+\] \(Debian GNU/Linux\)\r\n|s p/ser2net telnetd/ i/Debian; serial port $1/ o/Linux/
match telnet m|^Port's device already in use\n\r$| p/ser2net telnetd/ i/device in use/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfe\x01\n\rTerminal shell v1\.0\n\r\rCopyright \xa9\d+ Netopia, Inc\.  All rights reserved\.\n\r\rNetopia Model ([\w-]+) Wireless DSL Ethernet Switch\n\rRunning Netopia SOC OS version ([\d.]+ \(build \w+\))\n| p/Netopia $1 wireless ADSL router telnetd/ i/SOC OS $2/ o/SOC OS/ d/WAP/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfe\x01\n\rTerminal shell v1\.0\n\r\rCopyright \xa92008 Motorola, Inc\.  All rights reserved\.\n\r\rNetopia Model ([\d-]+)(?: AnnexA)? High-Power Wireless DSL Ethernet Managed Switch\n\rRunning Netopia SOC OS version ([\w.-]+ \(build \w+\))\n| p/Netopia $1 wireless ADSL router telnetd/ i/SOC OS $2/ o/SOC OS/ d/WAP/
# The esses spell "DSLink 260E".
match telnet m|^\xff\xfb\x01\xff\xfb\x03ssss   ssss sss     s         ss           sss   sss   sss  sssss \r\n s  s s   s  s                 s          s   s s  s  s   s  s   \r\n s  s s      s                 s          s   s s     s   s  s  \r\n s  s  ss    s     ss   ssss   s sss         s  ssss  s   s  sss  \r\n s  s    s   s      s    s  s  s s          s   s   s s   s  s   \r\n s  s     s  s      s    s  s  sss         s    s   s s   s  s    \r\n s  s s   s  s   s  s    s  s  s  s       s     s   s s   s  s   \r\nssss  ssss  ssssss sss  sss sssss ss      sssss  sss   sss  sssss\r\nLogin: $| p/Optimcom DSLink 260E ADSL router telnetd/
match telnet m|^\r\nPRO2 Control Console\r\n| p/Crestron PRO2 automation system telnetd/
match telnet m|^\r\nMC2E Control Console\r\n| p/Crestron MC2E automation system telnetd/
match telnet m|^(?:\x1b\[23;1H\r\n\r\x1b\[\?25h\x1b\[23;11H\x1b\[24;1HSession Terminated, Connect again\r\n\r\x1b\[\?25h\x1b\[24;1H)?\xff\xfd\x18\xff\xfb\x01\x1b\[2J\x1b\[\?7l\x1b\[3;23r\x1b\[\?6l\x1b\[1;1H\x1b\[\?25l\x1b\[1;1HProCurve (J\w+) Switch (\d+)\r\n\rFirmware revision [^\r\n]+\r\n| p/HP ProCurve Switch $2/ d/switch/ i/JetDirect $1/
match telnet m|^\xff\xfb\x03\xff\xfd\x03\xff\xfb\x01\r\n\r\nCache for Windows NT \(Intel\) 5\.0\.18 \(Build 6103\) [^\r\n]*\r\nNode \w+ Port: ([\w._-]+)/(\d+)\r\n\r\nUsername: | p/InterSystems Cache ftpd/ o/Windows/ h/$1/ i/port $2/
match telnet m|^\xff\xfb\x01\xff\xfd\.\r\n\r\nWelcome to the SX-2000 \(vxTarget\)\r\n\r\nlogin: \0| p/Mitel SX-2000 PBX telnetd/ d/PBX/
match telnet m|^\w{12}\r\nETHMAC ([0-9a-f:]+)\r\nWIFIMAC ([0-9a-f:]+)\r\n>| p/Roku media player telnetd/ d/media device/ i/Ethernet MAC: $1, wi-fi MAC: $2/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\nWireless AP Manager Console [^\r\n]+\r\n please enter your password: | p/Ovislink AirLive WAP telnetd/ d/WAP/
match telnet m|^\xff\xfc\x01\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfb\x18\xff\xfd\x1f\xff\xfb\x1f\xff\xfb\"\xff\xfb\x05Login:| p/VBrick 4300 video encoder telnetd/ d/media device/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\n\r\nYou are connected to configuration tool\r\nEnter the password: | i/Alvarion BreezeMAX WiMAX WAP telnetd/ d/WAP/
match telnet m%\xff\xfe\x01\r\n\r\n\+============================================================================\+\r\n\|             \[ interSeptor Configuration Utility Main Menu \]                \|\r\n\+============================================================================\+\r\n\r\nEnter Password: % p/Jacarta interSeptor environmental monitor telnetd/ d/specialized/
match telnet m|^\nThis is packet-o-matic built-([\d-]+)\nCopyright Guy Martin 2006-20\d\d\n\n\xff\xfb\x01\xff\xfb\x03\xff\xfd\x1f\xff\xfe\"pom> | p/packet-o-matic telnetd/ i/built $1/
# The ASCII art is a huge Conexant logo.
match telnet m%^\xff\xfb\x01\xff\xfb\x03\r\n                ,vvvdP9P\?\?\?\^   ,,,\r\n              vvd###P\^`\^         vvvvv v\r\n         vv#####\?\^                  \?\?\?\?####vv,\r\n      vv####\?\?     ,vvvdP\?\?\?\^  ,,,        \?\?##\^\r\n     v#####\?    ,vvd##P\?\^        #\?#v#vvv\r\n   v#####\?    v###P\^    ,vvv,        '\?#\?,\r\n  ######\?   ####\?\^ ,vd#P\?\^     `\?\?\?##\r\n  #####\?   v####  ,d##P\^           ''\r\n ######   v####  \]###L                   _   _          _                  ___\r\n #####\?   v####  \]##L                   /   / \\  \|\\ \|  \|_  \\/   /\\   \|\\ \|   \|\r\n ######    ####  \]###L                  \\_  \\_/  \| \\\|  \|_  /\\  /--\\  \| \\\|   \|\r\n% p/Zoom X6 ADSL router telnetd/ d/broadband router/
match telnet m|^\xff\xfb\x01\xff\xfd\x01\xff\xfb\x03\xff\xfd\x03\xff\xfb\x05\xff\xfd\x05\r\n\*\*\* Welcome to VTM   \*\*\*\r\n\r\n\r\n\rLogin   : | i/Stratus ftServer VTM telnetd/ d/remote management/
match telnet m|^\r\nCEN-IDOC Control Console\r\n\r\nCEN-IDOC>| p/Crestron CEN-IDOC music player connection telnetd/ d/media device/
match telnet m|^\xff\xfe\x01\xff\xfd\x03\xff\xfd\x18\xff\xfd\x1f\xff\xfb\x03\xff\xfb\x01jBASE Telnetd Server Version ([\d.]+) \n\r\r\nAccount Name: | p/jBASE telnetd/ v/$1/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfb\0\xff\xfd\x01\xff\xfd\0\r\0\n\r\0\n-----------------------------------------------------------------------------\r\0\nModel name       : NPort (\d+)\r\0\nMAC address      : ([0-9A-F:]+)\r\0\nSerial No\.       : \d+\r\0\nFirmware version : ([^\r]+)\r\0\nSystem uptime    : ([^\r]+)\r\0\n| p/Moxa NPort $1 serial-to-IP converter telnetd/ v/$3/ i/MAC $2; uptime $4/
match telnet m|^\xff\xfb\x01\r\nWelcome to Ring v([\d.]+) Copyright \(C\) AMX Corp\. 2002-2003\r\n| p/AMX NXD-CV5 Modero touch panel telnetd/ d/specialized/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03TESTING MODEL ADSL Router\r\nLogin: | p/D-Link DSL-2542B ADSL router telnetd/ d/broadband router/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\[([^]]*)\]\[([^]]*)\]\[([^]]*)\]\r\n| p/Neuf Box telnetd/ v/$2/ i/hardware $1; firmware $3/
match telnet m|^\xff\xfe\"\xff\xfb\x01\x1b<\x1b>\x1b\[\?25l\x1b\[0m\x1b\[2J\x1b\(B\x1b\)0\x0f\x1b\[7m\x1b\[f                  Areca Technology Corporation RAID Controller             | p/Areca 1280 RAID controller telnetd/ d/storage-misc/
match telnet m|^Secure Defrag Service v([\d.]+)\r\n \[\]\r\nlocal time: ([^\r\n]*)\r\n| p/Secure Defrag Service telnetd/ v/$1/ i/local time $2/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03Huawei (SmartAX \w+)\r\nLogin: | p/Huawei $1 ADSL router telnetd/ d/broadband router/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\n\r\n\r\n\r\n\*{76}\r\n\r\n +Minolta Network Configuration Utility\r\n +Minolta\r\n +Version ([\w.]+)\r\n| p/Minolta PagePro 20 printer telnetd/ v/$1/ d/printer/
match telnet m|^\xff\xfb\x01\xff\xfd\x18\xff\xfb\x03$| p/Tandem Himalaya K2000 telnetd/ o/GuardianOS/
match telnet m|^\xff\xfb\x01\xff\xfb\x03                  ZebraNet PrintServer Configuration Utility\r\n\r\n Type your password\. Press Enter when finished\.\r\n\r\n Password: | p/Zebra print server telnetd/ d/print server/
match telnet m|^\xff\xfd\x03\xff\xfe\x01\xff\xfb\x01\s+ZebraNet Internal Wired PS Configuration Utility\r\n\r\n Type your password\. Press Enter when finished\.\r\n\r\n Password: | p/Zebra print server telnetd/ d/print server/
match telnet m|^\xff\xfb\x01\n\rWelcome to TrueTime Network Interface\n\r\rUser name: | p/TrueTime GPS clock telnetd/
match telnet m|^MythFrontend Network Control\r\nType 'help' for usage information\r\n---------------------------------\r\n# | p/mythfrontend MythTV control/ d/media device/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\n\(Cisco Controller\) \r\nUser: | p/Cisco 4402 WLAN controller telnetd/ d/remote management/
match telnet m|^\x1b\[0m\r\nWelcome to (IC-\d+)!\r\n\r\n\x1b7\x1b\[\?25l\x1b\[501;501H\x1b\[6n\x1b8\x1b\[\?25h\r\x1b\[0m\x1b\[1mIC-\d+ # \x1b\[0m\x1b\[J\r\x1b\[10C| p/ICOM $1 amateur radio telnetd/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x03\x0c\x1b\[2JEnter Password: | p/InterTel IPRC VoIP management card telnetd/ d/PBX/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\r\n\r.*\xaf\xaf\xaf\xaf\xaf\r\n\r               Kernel ([\w._-]+) \(00:17:54\)\r\n\rdreambox login: |s p/Dreambox DVB telnetd/ i/Linux $1/ o/Linux/ d/media device/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\nRSC version ([\d.]+) \(([\w._-]+)\)\r\n\r\nPlease login: | p/Sun Remote System Control telnetd/ v/$1/ h/$2/ d/remote management/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x03\r\n\r\n\r\nWelcome to (R\w+) version (.*) from [\d /:]+\r\nsystemname is ([\w@_.-]+), location ([^\r\n]*)\r\n\r\n\r\nLogin: | p/Funkwerk bintec $1 router/ v/$2/ h/$3/ i/location: $4/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03FAST(\w+) ADSL Router \(Software Version:([\w._-]+)\)\r\nLogin: | p/Sagem F@st $1 ADSL router telnetd/ v/$2/ d/broadband router/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\x1b\[2J\x1b\[H\x1b\[2J\x1b\[H ------------------------------------------------------------------------------\r\r\n                                D A T A C O M\r\r\n +(DM\w+) - Minimux Router\r\r\n| p/Datacom $1 router telnetd/ d/router/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\x1b\[2J\x1b\[H\x1b\[2J\x1b\[H ------------------------------------------------------------------------------\r\r\n                                D A T A C O M\r\r\n +(DM\w+) - G\.SHDSL 2 Wire Modem Router\r\r\n| p/Datacom $1 router telnetd/ d/router/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\r\nBNT Layer 2/3 Copper Gigabit Ethernet Switch Module for IBM BladeCenter\.\r\n\r\n\r\nEnter password: | p|Nortel Layer 2/3 Gigabit Ethernet switch for IBM BladeCenter| d/switch/
# The ascii art spells "newcs".
match telnet m|^\xff\xfb\x01\xff\xfd\"\r\n#####   ####  ##   ##  ####   #####\r\n##  ## ##  ## ## # ## ##  ## ##\r\n##  ## ###### ####### ##      #####\r\n##  ## ##     ####### ##  ##      ##\r\n##  ##  #####  ## ##   ####  ######\r\n     A Butter Team Creation\r\n\r\nPassword :| p/NewCS card sharing system telnetd/
match telnet m|^sysrqd password: | p/sysrqd/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\r\n(DGFV\w+) login: | p/Netgear $1 WAP telnetd/ d/WAP/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\r\n(FVX\w+) login: | p/Netgear $1 firewall/ d/firewall/
match telnet m#^\xff\xfb\x01\xff\xfb\x03\x1b\[2J\x1b\[00H\+----------------------------------------------------------------------\+\r\0\r\n.*\| Motorola (PTP \d+) Lite Console Application +\|\r\0\r\n.*\| Software Version: ([\w._-]+) +\|\r\0\r\n\| Hardware Version: ([\w._-]+) +\|\r\0\r\n#s p/Motorola $1 WAP telnetd/ v/$2/ i/hardware version $3/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03Actiontec DSL Gateway\r\nLogin: | p/Actiontec GT704-WGB WAP telnetd/ d/WAP/
match telnet m|^\xff\xfc\x01\xff\xfb\x01\xff\xfb\x03\xff\xfe\x18\xff\xfd\x1f\xff\xfb\x1f\xff\xfb\"\xff\xfb\x05TiMOS-([\w._-]+) cpm/hops ALCATEL SR (\w+)| p/Alcatel $2 SR router telnetd/ d/router/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfb\0\xff\xfd\0QEMU ([\w._-]+) monitor - type 'help' for more information\r\n\(qemu\) | p/QEMU monitor telnetd/ v/$1/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\0\n\*\*\* TemPageR (\w+) Settings \*\*\*\r\0\nMAC address ([0-9A-F]{12})\n\r\0Software version V([^\r]*)\r\0\nPassword :| p/Avtech TemPageR $1 temperature monitor telnetd/ v/$3/ i/MAC $2/
match telnet m|^\xff\xfb\x01\xff\xfe\0\xff\xfc\0\r\0\n(SC\w+) Telnet session\r\0\n\r\0\nUsername: \xff\xf6| p/Beck IPC@CHIP $1 embedded telnetd/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\n\x1b\[1;1H\x1b\[2J\r\n\r\nObeh\xf6riga \xe4ga ej tilltr\xe4de\r\n\r\n\xf6vertr\xe4delse beivras\.\r\n\r\n\rUsername: | p/OpenVMS 8.3 telnetd/ i/Swedish/ o/OpenVMS/
match telnet m|^\n\rTA-005-FXO1-122M : CLI\n\rLogin : $| p/Open EasyChat210 VoIP phone telnetd/ d/VoIP phone/
match telnet m|^\xff\xfe\0\xff\xfc\0\xff\xfe\x01\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f$| p/HP StorageWorks tape autoloader telnetd/ d/storage-misc/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\nWelcome to (OpenPhone \w+) IP\r\n\rVersion ([\w._-]+)\r\n\r\r\n\rlast reset cause: software reset \(memory controller also reset\)\r\n\r\r\n\r([\w._-]+) login: | p/Aastra $1 telnetd/ v/$2/ h/$3/ d/VoIP phone/
match telnet m|^\xff\xfb\x01\xff\xfb\x01\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\n\*{80}\r\n\*  Copyright\(c\) 2004-2007 3Com Corp\. and its licensors\. All rights reserved\.   \*\r\n\*  Without the owner's prior written consent,                                  \*\r\n\*  no decompiling or reverse-engineering shall be allowed\.| p/3Com 5500G-EI switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfb\x01\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\n\*{80}\r\n\*  Copyright\(c\) 2004-2009 3Com Corp\. and its licensors\. All rights reserved\.   \*\r\n\*  Without the owner's prior written consent,                                  \*\r\n\*  no decompiling or reverse-engineering shall be allowed\.| p/3Com 5500-EI switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfb\x01\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\n\*{57}\r\n\*          All rights reserved \(1997-2005\)              \*\r\n\*      Without the owner's prior written consent,       \*\r\n\*no decompiling or reverse-engineering shall be allowed\.\*\r\n| p/3Com SuperStack 3 Switch 4500 or Huawei Quidway AR28-09 WAP telnetd/
match telnet m|^\xff\xfb\x01\xff\xfe\x01\n\r\n\r\n\r\n\n\n\n\r\t={51}\n\r\t       Samsung ([\w()-]+) Configuration\n\r\t={51}\n\r\n\r\tTo configure the Access Point, the password is required\.\n\r\tEnter password:| p/Samsung $1 WAP telnetd/ d/WAP/
match telnet m|^220 SB06D2F0 FTP server \(INTERFACE version ([\w._-]+)\) ready\.\n| p/Kyocera Mita KM-1530 printer telnetd/ v/$1/ d/printer/
match telnet m|^\xff\xfe\x01\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\xff\xfd\x18Georgia SoftWorks Telnet Server for Windows NT/2000/XP/2003/Vista/2008 Ver\. ([\w._-]+)\n\rEvaluation copy, \d+ users enabled\. Expiration date is ([\d/]+)\.\n\r\n\rUser \d+ of \d+\n\r\n\rlogin:| p/Georgia SoftWorks Telnet Server/ v/$1/ o/Windows/ i/expiration date $2/
match telnet m|^\xff\xfc\x01\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfb\x18\xff\xfd\x1f\xff\xfb\x1f\xff\xfb\"\xff\xfb\x05Username:| p/OneAccess ONE100A router telnetd/ d/router/ o/OneOS/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\0\nMAC address ([0-9A-F]{12})\n\r\0Software version V([\w_.\(\) -]+) \r\0\n\n\r\0Press Enter for Setup Mode \n\r\0| p/Enistic zone controller telnetd/ v/$2/ i/MAC $1/
# The ASCII art is a big "BS" seal.
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\+{79}\r\n\r\+{33}#############\+{33}\r\n\r\+{28}######           ######\+{28}\r\n\r| p/BitSwitcher firmware/ d/broadband router/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03login as: | p/D-Link DVA-G3170i telnetd/ d/broadband router/
match telnet m|^\xff\xfb\x01\xff\xfb\x03BR-telnet@(FES\w+) Router>| p/Foundry $1 switch telnetd/ d/switch/
match telnet m|^\xff\xfb\"\xff\xfb\x03\xff\xfb\x01\xff\xfb\x1f\xff\xfb\x18Login: | p/Force10 S50N switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\n\r\0\*\*\* Siemens (\w+) \*\*\*\n\r\0\r\0\nSerial Number (\d+)  MAC address ([0-9A-F]{12})\n\r\0Software version ([^\r]+)\r\0\nPassword :| p/Siemens $1 remote management telnetd/ d/remote management/ i/serial $2; MAC $3/
match telnet m|^\xff\xfc\x01\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfb\x18\xff\xfd\x1f\xff\xfb\x1f\xff\xfb\"\xff\xfb\x05PTLDOR69SH3HT4000HG6 Hatteras (\w+)\r\nLogin: | p/Hatteras $1 PBX telnetd/ d/PBX/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03                        =======================\r\n                               ([\w._-]+) +\r\n                        =======================\r\nLogin: | p/D-Link $1 ADSL router/ d/broadband router/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\n\r\nCopyright \(c\) 2005 - 2008 Enterasys, Inc\. All rights reserved\.\r\n\n\r\n\r\n\r\0Username: | p/Enterasys RBT-8200 switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\nCopperJet ([\w._-]+) Router VoATM\r\nFirmware version: ([\w._-]+)\r\nAllied Data Technologies\r\n\r\nPlease login: | p/Allied Data CopperJet $1 ADSL router telnetd/ v/$2/ d/broadband router/
match telnet m|^\r={74}\n\rTransition Networks Telnet Server\n\rSystem name: SMKG-PKGEAST-([\w._-]+)\n\rPress CTRL-D to disconnect\.\n\rEnter password: | p/Raritan $1 KVM switch telnetd/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\r\nCTRING login: | p/MicroDigital MDR-4600 DVR telnetd/ d/media device/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\n\r        Welcome to QUIDWAY ([\w._-]+) Access Server\n\r      Copyright \(c\) \d+-\d+ HUAWEI TECH CO\. LTD\.\n\r\n\rUser Name:| p/Huawei Quidway $1 switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n \*{73}\r\n  This is a private system\. \r\n  Do not attempt to login unless you are an authorized user\.  \r\n  Any authorized or unauthorized access or use may be monitored and can\r\n  result in criminal or civil prosecution under applicable law\.\r\n \*{73}\r\n\r\nMP login: | p/HP Integrated Lights-Out Advanced telnetd/ d/remote management/
match telnet m|^\xff\xfe\"\xff\xfb\x01\x1b\[f\x1b\[9C\x1b\[9C\x1b\[9C\x1b\[2C\x1b\[9B\x1b\[5B                      \x1b\[f\x1b\[9C\x1b\[9C\x1b\[9C\x1b\[2C\x1b\[9B\x1b\[6B                      \x1b\[f\x1b\[9C\x1b\[9C\x1b\[9C\x1b\[2C\x1b\[9B\x1b\[7B                      \x1b\[f\x1b\[9C\x1b\[9C\x1b\[9C\x1b\[9C\x1b\[9C\x1b\[9B\x1b\[2B  Verify Password  \x1b\[f\x1b\[9C\x1b\[9C\x1b\[9C\x1b\[9C\x1b\[9C\x1b\[9B\x1b\[4B                   \x0e\x1b\[f\x1b\[9C\x1b\[9C\x1b\[9C\x1b\[9C\x1b\[8C\x1b\[9B\x1b\[1Blqqqqqqqqqqqqqqqqqqqk\x1b| p/DNF Storage F16fz NAS device telnetd/ d/storage-misc/
match telnet m|^\xff\xfb\x03\xff\xfd\x18\xff\xfb\x01\xff\xfd\x1f\xff\xfd!Username: | p/McData switch telnetd/ d/switch/
match telnet m|^Sorry, new remote sessions are disallowed by current switch configuration\.| p/Dell PowerConnect 6248 switch telnetd/ d/switch/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\x1b\[H\x1b\[J\r\nWireless Router Manager Console , Version : ([\w._-]+)\r\nPlease enter your password : | p/Ovislink WLA-9000AP WAP telnetd/ d/WAP/ v/$1/
match telnet m|^\xff\xfb\x01\xff\xfd\x18\xff\xfb\x03\xff\xfd\x1f| p/HP Tandem NonStop telnetd/
match telnet m|^\xff\xfb\x03\xff\xfd\x18\xff\xfb\x01\xff\xfd\x1f\xff\xfd!\x1b\[2J\x1b\[H\x0fUser Access Verification \r\n\r\nWaiting on TACACS\+ server\.\.\.\r\n\nUser Access Verification\r\n\r\nUsername: | p/Adtran NetVanta 6355 VoIP gateway telnetd/ d/VoIP adapter/ i/TACACS enabled/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\*{60}\r\n\* WARNING ALERT: AUTHORIZED USERS ONLY! +\*\r\n\* +\*\r\n\* All activities conducted on this system may be monitored \*\r\n\* and recorded\. If you are not an authorized user, log off \*\r\n\* immediately\.  Illegal entry, misuse, and / or criminal   \*\r\n\* activity will be documented and prosecuted to the full   \*\r\n\* extend of the law\. +\*\r\n\*{60}\r\n\r\n\r\nPress <Enter> to accept and continue the login process\.\.\.\.\r\n| p/Foundry NetIron XMR 4000 router telnetd/ d/router/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\x1b\[2J\x1b\[0m\x1b\[1;1H\x1b\[2;1H\x1b\[3;1H\x1b\[4;1H ###      ###  ###########   ##########  ############# ########### ###\x1b\[5;1H ####     ### ############# ############ ############# ########### ###\x1b\[6;1H[ #]{70}\x1b\[7;1H[ #]{70}\x1b\[8;1H[ #]{70}\x1b\[9;1H[ #]{70}\x1b\[10;1H[ #]{70}\x1b\[11;1H[ #]{70}\x1b\[12;1H[ #]{78}\x1b\[13;1H[ #]{78}\x1b\[14;1H\x1b\[15;1H\x1b\[16;1HEnter Ctrl-Y to begin\.\x1b\[18;3H\*{38}| p/Nortel 4548 switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x03\xff\xfd\x01\xff\xfd\x1f\xff\xfb\x05| p/Netgear FSM700S switch/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\x1b\[2J\x1b\[1;1H\x1b\[1mwb-adtran-\w+       ADTRAN (TDU-\w+)\x1b\[0m\x1b\[2;1HConnecting\.\.\.\.| p/Adtran $1 PBX telnetd/ d/PBX/
# Probably more general than this --Ed.
match telnet m|^\r\n%connection closed by remote host!\0| p/HP H3C SR8808 SecBlade firewall module telnetd/ d/firewall/
match telnet m|^Sorry, telnet is not allowed on this port!$| p/Cisco 4400 wireless LAN controller telnetd/ d/remote management/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\ncli ([\w._-]+)\r\nUser Name: | p/ZyXEL G-570S WAP telnetd/ d/WAP/ v/$1/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\nBUFFALO INC\. LinkStation series HS-DHGL\(JINMU\)\r\n\rFENCHURCH login: | p/Buffalo LinkStation HS-DHCL series NAS device/ d/storage-misc/
match telnet m|^\nFelix Remote Shell Console:\r\n============================\r\n\r\n-> | p/Apache Felix remote console/
match telnet m|^\r\n\r\nBackup Server Telnet Session\r\n\r\nUser:| p/NovaNET-WEB backup server telnetd/
match telnet m|^Start Telnet Server:\r\n| p/ATmega32 Telnet-to-RS232/
match telnet m|^\xff\xfb\x01\xff\xfd\"\[game001\] remote control session\.\r\nPassword:\0$| p/Rappelz game admin telnetd/
match telnet m|^\r\nVOLKTEK Corporation\r\nSystem version: ([\w._-]+) \((built at .*?)\)\r\n\r\nUsername: | p/Volktek router telnetd/ v/$1/ d/router/
match telnet m|^\xff\xfd\x18\xff\xfb\x01\x1b\[2J\x1b\[\?7l\x1b\[3;23r\x1b\[\?6l\x1b\[1;1H\x1b\[\?25l\x1b\[1;1HProCurve J\w+ Switch ([\w-]+)\r\n\rSoftware revision ([\w._-]+)\r\n| p/HP ProCurve $1 switch telnetd/ v/$1/
match telnet m|^This is version ([\w._-]+) of the API\nSMS is enabled and HOMEAUTOMATION is enabled for you\n>> | p/Dovado 4GR WAP telnetd/ v/$1/ d/WAP/

#(insert telnet)

match telnet-proxy m|^nodnsquery/[\d.]+ is not authorized to use the telnet proxy\r\n| p/Gauntlet telnet proxy/
match telnet-proxy m|^Eingabe Servername\[:Port\] : | p/JanaServer telnet proxy/ i/German/
match telnet-proxy m|^\xff\xfb\x01\xff\xfb\x03Telnet Gateway ready=enter computer name to connect to\.\\x0d\\x0a\\xd\\xahost\[:port\]: \r\n| p/602LAN Suite telnet proxy/ o/Windows/
match telnet-proxy m|^\r\n\r\nEnter computer name to connect to\.\r\ne\.g\. \"NetCom\.com\"<CR>| p/WinProxy telnet proxy/ o/Windows/
match telnet-proxy m|^\xff\xfc\x01\xff\xfd\"ixProxy V([\d.]+), Copyright \(C\) \d+ Ixia Communications\r\nEnter target port ip address as login name \(example: 10\.0\.1\.1\)\r\nlogin:| p/Ixia ixProxy telnet proxy/
match telnet-proxy m|^\xff\xfb\x01\xff\xfb\x03Blue Coat Shell proxy\r\nShell-proxy>| p/Blue Coat Shell proxy/ o/SGOS/
match telnet-proxy m|^Welcome to kingate ([\w._-]+)-win32 telnet proxy\.\r\nPlease enter host and port\r\nexample: abc\.com 23\r\nkingate >| p/kingate telnet proxy/ v/$1/ o/Windows/

# tinc 1.0.2-2 on Linux
match tinc m|^0 \w+ 17\n| p/tinc vpn daemon/

# TIME
# This will match systems with clocks set between the
# following 2 dates:
# 0xCA000000 = Thu May 24 14:13:52 2007
# 0xD7FFFFFF = Sat Nov  1 18:57:35 2014
# Calculate this with the Python program:
# python -c 'import datetime; print datetime.datetime.fromtimestamp(0xca000000 - 2208988800).ctime()'
# Also needs updating (search for TIME):
#   UDP Help
#   TCP NULL
match time m|^[\xca-\xd7]...$|s i/32 bits/
match time m|^[\xca-\xd7]....\0\0\0$|s i/64 bits/

# Need more examples... -Doug
match timeedit m|^\0\0\0H\0\0\0\x02\x0fTimeEdit131\.| p/Evolvera TimeEdit/ v/1.3.1/

# Tiny Personal Firewall 2.0
match tinyfw m|^\x0f\0\n\0\x01\0\0\0\0\x02\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\xc0\x0ef7\xbb\x9bS\xfc\x86\xe4\x7f\x18\xb8\x97\x06 | p/Tiny Personal Firewall/ v/2.0/

# http://www.tmail.spb.ru/index-19.htm
match tmail m|^\*\*\x18B0800000000022d\r\n\x11\x11\x11\*\*EMSI_REQA77E\r\r\[CONNECT TCP/IP/[\d.]+/IFC\]\r\nT-Mail v([\w.]+)/TCP/IP/Noncommercial \(C\) 1992-99 by Andy Elkin\r\n\*\*EMSI_REQA77E\rSorry\.\. Mail only node\.\r\n| p/T-Mail/

match trackerlink m=^\d+\|\d+\|TrackerLINK Ver\. ([\d.]+)= p/TrackerLINK/ v/$1/

match trendnet-webcam m|^0301&<\x16\0\x84\xc7\x02\xe0\xe1\xb1\x008\x13\x1e\x0b\x80<\x16\0\xc7\t\x8f\x05\xc0\xf0X\0\x1c\xc2c\x01p\x1e\x0b\x80\xe3c\x01p\xdcX\0\x1c7\x8f\x05\xc0q\x0b\x80\xe3F\xc7\x02\xe0\xb8,\0\x8e\x1b\xb1\x008n\x05\xc0q\xa3\x008n\xb4\x02\xe0\xb8\xd1\x01p\xdch\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0$| p/TRENDnet TV-IP100 webcam display/ d/webcam/

# Kerio Personal Firewall 4.02 on Windows 2000, 4.0.11 on W2K SP4+ too (port 44xxx)
match keriopfservice m|^\x12\0\x03\0\x04\0\0\0\0\x02\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0| p/Kerio PF 4 Service/ i/maybe 4.0.2-11/
# Kerio PF 4.0.11 unregistered - GUI process (Port 1027-1200,44xxx? RPC?) on MS W2K SP4+
match keriopfgui m|^\x12\0\r\0\x03\0\0\0\0\x02\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\x9a\x20\xd0Z\x1e\x1b\xa3\*\xf2\xdd\xe2\(\xc3sp&\xda\xe4Yp\xdbET\xf9\x8cc\xc24\*Y\xbe\xb3\xba\xd6%\xf5\xb668\xad\xab>@D<\x01<i\x80O>\xdd>\)\xdb\x18\xf55\xd1\xba\x96\x1c\x17\x17\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\x01\0\x01| p/Kerio PF 4 GUI/ i/maybe 4.0.11/
# Kerio Personal Firewall 2.1.4 on Windows
# Tiny Personal Firewall 2.0
# Kerio Personal Firewall, Firewall engine version 2.1.5 Driver version 3.0.0 on WinXP
match tinyfw m|^\x0f\0\n\0\x01\0\0\0\0\x02\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0| p/Kerio Personal Firewall/ v/2.1.X/ i/or Tiny Personal Firewall/

match trackmania-gbx m|^\x0b\0\0\0GBXRemote 2$| p/TrackMania game GBX remote/

match venti m|^venti-02-libventi\n| p/Plan 9 venti storage system/

match visitview m|^Greetings:  The VISITview Server \$Revision: ([\w._-]+) \$ welcomes you!\n$| p/VISITview/ v/$1/

# VMware has a buch of different auth settings so this gets messy
match vmware-auth m/^220 VMware Authentication Daemon Version (\d[-.\w]+).*\r\n530 Please login with USER and PASS\.\r\n/s p/VMware Authentication Daemon/ v/$1/
match vmware-auth m/^220 VMware Authentication Daemon Version (\d[-.\w]+), ServerDaemonProtocol:(SOAP|IPC), MKSDisplayProtocol:VNC/ p/VMware Authentication Daemon/ v/$1/ i/Uses VNC, $2/

match ssl/vmware-auth m|^220 VMware Authentication Daemon Version (\d[-.\w]+): SSL Required\r\n| p/VMware Authentication Daemon/ v/$1/
match ssl/vmware-auth m|^220 VMware Authentication Daemon Version (\d[-.\w]+): SSL [rR]equired, MKSDisplayProtocol:VNC(?: ,)? \r\n| p/VMware Authentication Daemon/ v/$1/ i/Uses VNC/
match ssl/vmware-auth m/^220 VMware Authentication Daemon Version (\d[-.\w]+): SSL Required, ServerDaemonProtocol:(SOAP|IPC), MKSDisplayProtocol:VNC/ p/VMware Authentication Daemon/ v/$1/ i/Uses VNC, $2/

match vmware-aam m|^\0\0\x04\x90\x01\0\0\0\x03\x03\x01\x03@\xe4\x01\x02\0\x01\x02\0\xfe\xff\xff\xff\0\0d\0\0\x01\x02\0\xfe\xff\xff\xff\0\0d\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\x14\0\0\0\x8fd\0\0tO\xf7\t\0\0\0\0\x02\0\0\0\x01\0\0\0\x01\x02\0\0\x04\0\0\0k\x1f\0\0\0\0\0\0\x02\0\0\0\x8fc\0\0\x8cO\xf7\t\0\0\0\0\.\0\0\0\0\0\0\0| p/VMware Automated Availability Manager/

match vnc m|^RFB 003\.00(\d)\n$| p/VNC/ i/protocol 3.$1/
match vnc m|^RFB 003\.00(\d)\n\0\0\0\0\0\0\0\x1aToo many security failures$| p/VNC/ i/protocol 3.$1; Locked out/
match vnc m|^RFB 003.130\n$| p/VNC/ i/unofficial protocol 3.130/
match vnc m|^RFB 003\.88[89]\n$| p/Apple remote desktop vnc/ o/Mac OS X/
match vnc m|^RFB 000\.000\n$| p/Ultr@VNC Repeater/
match vnc m|^RFB 003\.00(\d)\n\0\0\0\0\0\0\0jServer license key is missing, invalid or has expired\.\nVisit http://www\.realvnc\.com to purchase a licence\.| p/RealVNC/ i/Unlicensed, protocol 3.$1/
match vnc m|^RFB 004\.000\n| p/RealVNC Personal/ i/protocol 4.0/
match vnc m|^RFB 003\.00(\d)\n\0\0\0\0\0\0\0:Unable to open license file: No such file or directory \(2\)| p/RealVNC Enterprise Edition/ i/protcol 3.$1/
match vnc m|^RFB 103\.006\n| p/Microsoft Virtual Server remote control/ o/Windows/
match vnc m|^ISD 001\.000\n$| p/iTALC/
match vnc m|^.{27}\x16\x20\xe4\xb0\x95\x63\x29\x78\xdb\x6e\x35\x92$|s p/Ultr@VNC/

softmatch vnc m/RFB \d\d(\d)\.\d\d\d\n/ i/protocol $1/

match vtun m|^VTUN server ver +(\d[-.\w /]+)\n\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0| p/Vtun Virtual Tunnel/ v/$1/
match vtun m|^VTUN server ver \. (\d[-.\w /]+)\n\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0| p/Vtun Virtual Tunnel/ v/$1/
match vtun m|^VTUN server ver \(.*\) (\d[-.\w /]+)\n\0\0\0\0\0\0\0\0\0\0\0\0\0\0| p/Vtun Virtual Tunnel/ v/$1/

match vhcs m|^250 OK moleSoftware VHCS2 Server Welcomes You !\r\n| p/moleSoftware virtual hosting control system/ o/Linux/

match weather m|^TrueWeather\r\n\r\n>| p/TrueWeather Desktop Weather Authority server/
# http://www.3w.net/lan/faq.html
match websense-eim m|^\x96\xfeS\xab$| p/Websense EIM/

match websm m|^\+ read portFile\n\+ head -1\n\+ find /var/websm/| p/AIX wsmserver/ o/AIX/
match websm m|^\+ read portFile\n\+ find /var/websm/data/wservers/| p/AIX wsmserver/ o/AIX/

match winshell m/^Microsoft Windows( (?:2000|XP|NT 4\.0)|) \[Version ([\d.]+)\]\r\n\(C\) Copyright 1985-20\d\d Microsoft Corp\.\r\n\r\n/ p/Microsoft Windows$1 $2 cmd.exe/ o/Windows/ i/**BACKDOOR**/
match winshell m/^Microsoft Windows \[Version ([\d.]+)\]\r\nCopyright \(c\) 20\d\d Microsoft Corporation\.  All rights reserved\.\r\n\r\n/ p/Microsoft Windows $1 cmd.exe/ o/Windows/ i/**BACKDOOR**/

# CcXstream Media Server 1.0.15 on Linux - Uses XBMSP (X-Box Media Streaming Protocol)
match xbmsp m|^XBMSP-1\.0 1\.0 CcXstream Media Server (\d[-.\w]+)\n| p/CcXstream Media Server/ v/$1/
match xbmsp m|^XBMSP-1\.0 1\.0 Media File XStream Server \n| p/Media File XStream/
match xbmsp m|^XBMSP-1\.0 1\.0 xbmsd ([\w._-]+)\n| p/xbmspd/ v/$1/
match xinetd m=^([-\w_.]+ (tcp|udp) \d{1,5}\n)+= p/xinetd service display/ o/Unix/
# XFCE Desktop Version 3.99.4 From Gentoo 1.4 Ebuild on Linux 2.4.6
match xfce-session m|^\0\x01\0.\0\0\0\0$|s p/XFCE Session Manager/
match xmail-ctrl m|^\+\d+ <[\d.]+@[\d.]+> XMail ([\d.]+) \(Linux/Ix86\) CTRL Server; .*\r\n| p/XMail CTRL Server/ v/$1/ o/Linux/
match xmail-ctrl m|^\+\d+ <[\d.]+@[\d.]+> XMail ([\d.]+) CTRL Server; .*\r\n| p/XMail CTRL Server/ v/$1/
match xmbmon m|^TEMP0 +: +[\d.]+\nTEMP1 +: +[\d.]+\nTEMP2 +: +[\d.]+\nFAN0 +: +[\d.]+\nFAN1 +: +[\d.]+\nFAN2 +: +[\d.]+\n| p/Mother Board Monitor/

# Right now once a softmatch triggers, only match lines with the same
# service name will match.  Like with the HTTP softmatch, this is somewhat
# restrictive.  If softmatch is ever updated to behave differently 
# go ahead and uncomment these (Brandon)
#softmatch xml m|^<\?xml version=\"([^\"]+)\" encoding=\"([^\"]+)\"[^>]*(?<=\?)>| i/XML version $1; encoding: $2/
#softmatch xml m|^<\?xml version=\"([^\"]+)\"[^>]*(?<=\?)>| i/XML version $1/

match xine-remote m|^([-\w_.]+) xine-ui ([\d.]+) remote server\. Nice to meet you\.\n| p/Xine-UI remote control/ v/$1/

match yiff m|^\0\0\0\n\0\x03\0\0\0\0$| p/YIFF network sound server/

match zebra m|^\r\nHello, this is zebra \(version (\d[-.\w]+)\)\.\r\nCopyright 1996-20| p/GNU Zebra routing software/ v/$1/
match zebra m|^\r\nHello, this is zebra \(version (\d[-.\w]+)\)\.\r\nCopyright 200\d| p/GNU Zebra routing software/ v/$1/
match zebra m|^Vty password is not set\.\r\n$| p/Quagga routing software/
match zebra m|^\r\nUser Access Verification\r\n\r\n\xff\xfb\x01\xff\xfb\x03\xff\xfe\"\xff\xfd\x1fPassword: | p/GNU Zebra routing software/

match zenworks m|^<AgentInfo><Version>([^<]+)</Version></AgentInfo>\0?| p/ZENworks Patch Management/ v/$1/ o/Windows/

match pcp m|^\0\0\0\x14\0\0p\0\0\0..\0\0\0\0\x02\x01\0\0|s p/SGI Performance Co-Pilot/
match pcp m|^\0\0\0\x14\0\0p\0\0\0..\xff\xff\xfc\x11\x02\x000a|s p/SGI Performance Co-Pilot/

match smtp m|^220 SPAM, we hates it.\r\n| p/Barracuda Spam firewall/

# 13720/tcp
match bprd m|^\0\0\0.EXIT[ _]STATUS \d+$|s p/Veritas Netbackup/
match bprd m|^request daemon can't accept sessions\nanother instance may already be running\.\nAddress already in use\n$| p/Veritas Netbackup/
match bprd m|^bp[-\w]+: error while loading shared libraries: libstdc\+\+-libc6\.2-2\.so\.3: cannot open shared object file: No such file or directory\n$| p/Veritas Netbackup/ i/broken/
# 13782/tcp
match bprd m|^gethostbyaddr: [\w ]+\n$| p/Veritas Netbackup/ i/refused/
match bprd m|^bpjava-msvc: error while loading shared libraries: libpam\.so\.0: cannot open shared object file: No such file or directory\n| p/Veritas Netbackup/ i/broken/

# PostCast SMTP server 2.6.0 ( http://www.postcastserver.com/ )
match smtp m|^220 PostCast SMTP server.*\r\n$| p/PostCast SMTP server/

match omapi m|^\0\0\0d\0\0\0\x18$| p/ISC (BIND|DHCPD) OMAPI/
match openvpn m|^\0\x0e@........\0\0\0\0\0\0\x0e@|s p/OpenVPN/
match openvpn m|^\0\x0e@........\0\0\0\0\0|s p/OpenVPN/
match openvpn m|^\0\*@.*\0\0\0\0\0|s p/OpenVPN/
match openvpn m|^\0<\xaa\xc5\r\^\xf7\x1b\xd1\xe1a/\xe8\x17P\x9dOb\xbb\x93\x87\xe0\xf3v\x81K\xa4!\xe6\xc7\x01\x977u5A\xd1M\x1b;\xc7\xcb\x87\xb5\x87\xf3~\xc8w\xef\xd3\x87eA\0\^\xbf\xc5\x93i\xf6\x87$| p/OpenVPN/
match openvpn-management m|^>INFO:OpenVPN Management Interface Version ([\d.]+) -- type 'help' for more info\r\n>| p/OpenVPN Management Interface/ v/$1/
match osiris m|^\x80[=+:]\x01\x03\x01\0.\0\0\0\x10\0|s p/osiris host IDS agent/

match osiris m|^\x16\x03\x01\0.\x01\0\0|s p/osiris host IDS agent/

#<\x03\x01H\|\t\xfa\x80\x1fr\x1aN\.\xa2\xa9\?\x0e~\]\xb7\x9dG\xb3\x93E9p\xb5\x01\xeb\x8f21\xde/\0\0\x14\x009\x008\x005\0\x16\0\x13\0\n\x003\x002\0/\0\x05\x02\x01\0
###############^\x16\x03\x01\0.\x01\0\0<\x03\x01I\x01\xe0\x9dn\xfd\n\x8c`\x99\xd9\x9bV}\x92\xe4\xe1\xee\xab\x184\x0f\x08\xb4\xf1\xfc\x10XF\xe9\xae\xfb\0\0\x14\x009\x008\x005\0\x16\0\x13\0\n\x003\x002\0/\0\x05\x02\x01\0
###############^\x16\x03\x01\0.\x01\0\0>\x03\x01I\x7fDY\(}\xafA1%\xe8W\x8e\x04\x8e\xeem\x1aQ\xa6k_\x978\x8a\xe4\xc5%_S\xa9K\0\0\x16\x009\x008\x005\0\x16\0\x13\0\n\0f\x003\x002\0/\0\x05\x02\x01\0

match rtsp m|^RTSP/1\.0 400 Bad Request\r\nDate: .*\r\nAllow: OPTIONS, DESCRIBE, SETUP, PLAY, PAUSE, TEARDOWN\r\n\r\n$| p/Geovision webcam rtspd/ d/webcam/

match svnserve m|^\( success \( \d \d \( (ANONYMOUS )?\) \( | p/Subversion/

match sumatra-ds m|^v7\x87\x12\0\0\0\x01........$|s p/Sumatra DS Server/

match icecream m|^[\x14-\x1f]\0\0\0$| p/icecreamd/

#commenting out - not APC, likely java-rmi - TomS - 2010.09.26
#match apc-agent m|^\xac\xed\0\x05$| p/APC PowerChute agent/ d/power-device/

match afs3-fileserver m|^load1:[\d.]+###load2:[\d.]+###load3:[\d.]+###MemTotal:(\d+) kB###MemFree:(\d+) kB| p/AFS fileserver/ i|$2/$1 kB free|

match vtp m|^220 Welcome to Video Disk Recorder \(VTP\)\r\n| p/VTP control for VDR/ d/media device/

match warcraft m|^\0\x06\xec\x01....$|s p/World of Warcraft world server/
match warcraft m|^\0\x2a\xec\x01....|s p/World of Warcraft world server/

match wingate-control m|^.\x01.[\x02\x03]\x01\d+\0$|s p/WinGate Administration/ o/Windows/
# Wingate redir: Probably not general enough
match wingate m|^\0\n\0\0\x02\0\0\0\x01\0$| p/WinGate transparent redirection/ o/Windows/
match mail-admin m|^OK0100 eXtremail V([\d.]+) release (\d+) REMote management \.\.\.\r\n| p/eXtremail remote management/ v/$1 release $2/
match ppp m|^SuSE Meta pppd \(smpppd\), Version ([\d.]+)\r\n| p/SuSE Meta pppd/ v/$1/ o/Linux/

# \xc0\x21 -> LCP
match ppp m|^\x7e\xff\x7d\x23\xc0\x21}!}!} }4}\"}&} } } } }%}&\xf4\xd1\xa2\xf6}'}\"}\(}\"\xc7}#~~\xff}#\xc0!}!}!} }4}\"}&} } } } }%}&\xf4\xd1\xa2\xf6}'}\"}\(}\"\xc7}#~~\xff}#\xc0!}!}!} }4}\"}&} } } } }%}&\xf4\xd1\xa2\xf6}'}\"}\(}\"\xc7}#~~\xff}#\xc0!}!}!} }4}\"}&} } } } }%}&\xf4\xd1\xa2\xf6}'}\"}\(}\"\xc7}#~~\xff}#\xc0!}!}!} }4}\"}&} } } } }%}&\xf4\xd1\xa2\xf6}'}\"}\(}\"\xc7}#~~\xff}#\xc0!}!}!} }4}\"}&} } } } }%}&\xf4\xd1\xa2\xf6}'}\"}\(}\"\xc7}#~~\xff}#\xc0!}!}!} }4}\"}&} } } } }%}&\xf4\xd1\xa2\xf6\x7d\x27\x7d\x22\x7d\x28\x7d\x22\xc7\x7d\x23\x7e| p/pppd/
match ppp m|^\x7e\xff\x7d\x23\xc0\x21}!}!} }4}\"}&} } } } }%}&\x81\xf4\xdb\xc0}'}\"}\(}\"\xc4\x80~~\xff}#\xc0!}!}!} }4}\"}&} } } } }%}&\x81\xf4\xdb\xc0}'}\"}\(}\"\xc4\x80\x7e| p/pppd/

match pppctl m|^PPP on ([-\w_.]+)> | p/pppctld/ h/$1/

match honeypot m|^503 Service Unavailable\r\n\r\n\0$| p/Network Flight Recorder BackOfficer Friendly honeypot/
match honeypot m|^\r\nlogin: \0$| p/Network Flight Recorder BackOfficer Friendly telnet honeypot/
match honeypot m|^\r\n[-\w_.]+ [\d.]+ - Unauthorized access \x07prohibited under penalty of law\.\r\n\r\nlogin: \xff\xfc\x01| p/Whiz Kid Technomagic Imaginary telnet honeypot/ o/Windows/
match honeypot m|^Microsoft Windows XP \[Version [\d.]+\]\n\(C\) Copyright 1985-\d+ Microsoft Corp\.\n\nC:\\>| p/honeyd cmdexe.pl/

match dlswpn m|(?<=.)IOS\x20\(tm\)\x20([-\d\w.]+).{20,30}\x20Version\x20([-\d\w.()]+),\x20|s p/Cisco $1 Router/ i/IOS $2/ o/IOS/ d/router/
match tunnelvision m|^HELLO Welcome to Tunnel Vision \(([\d.]+)\)\n| p/Tunnel Vision VPN info/ v/$1/


match domain m|^\x80\xf0\x80\x12\0\x01\0\0\0\0\0\0\x20CKAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA\0\0!\0\x01| p/Microsoft DNS/ o/Windows/

# There are two different version numbers in the signature (see captures). I
# don't know what they correspond to.
match amx-icsp m%^\x02\0\]\x02\0\0\0\0\0\0\x01\0.\0\0\0\x01\x0f\xff\x81\0\x97\0\0\0.\0\x04\0\0\0\x01\x01\+\d+x\d+\0\0\x01\|v([\d.]+)\0NI Master\0AMX Corp\.\0\x06\x0c\xc0\xa8\"D\x05'\0`\x9f....\x02\0U\x02\0\0\0\0\0\0\x01\0.\0\0\0\x01\x0f\xff\x82\0\x97\0\0\0.\0\x04\x01\0\0\x01\x01\+N/A             \x01zv[\d.]+\0vxWorks Image\0AMX Corp\.\0\0\0.\x02\0O\x02\0\0\0\0\0\0\x01\0.\0\0\0\x01\x0f\xff\x83\0\x97\0\0\0.\0\x04\x02\0\0\x01\x01\+N/A             \x01{v[\d.]+\0BootROM\0AMX Corp\.\0\0\0.\x02\0\^\x02\0\0\0\0\0\0\x01\0.\0\0\0\x01\x0f\xff\x84\0\x97\0\0\0.\0\x04\x03\0\0\x01\x01\x000000000000000000\x01\x0ev([\d.]+)\0AXLink I/F uController  \0AMX Corp\.\0\x03\0.$% p/AMX ICSP/ o/VxWorks/

match uc4 m|^\d\d\d\d\d\d\d\dUC4:global001NAT {24}\x04H(.+)\x20| p/UC4 Executor/ i/name: $1/
match uc4 m|^\d\d\d\d\d\d\d\dUC4:global001NAT {24}| p/UC4 Executor/

match wyse-devmgr m|^Invalid Command Sent:GET / HTTP/1\.0\r\n\r\n$| p/Wyse Device Manager/

# Not sure about these. It's port 9200 on some printers. On Intermec printers
# at least, port 9200 is some kind of XML printing service. The first byte
# appears to be a total length.
match xml-print m|^.\0\0\0\0(IBM Infoprint \w+)\0$|s p/$1 printer XML printing/ d/printer/
match xml-print m|^.\x2f\0\0\0(Lexmark \w+)\0|s p/$1 printer XML printing/ d/printer/

# http://www.brainz.co.kr/product/infra_05.php
match zenius-sms m|^Zenius SMS Agent V([\w. ]+) \(zagent-\w+-sparc\) 1400\r\n\0\0\0\0\0\0\0\0\0\0| p/Brainz Zenius Server Management System Agent/ v/$1/ i/SPARC/

match zeo m|^\0\0\0\x04Z(\d)0(\d)$| p/Zope Enterprise Objects service/ i/ZODB $1.$2/
match zeo m|^\0\0\0\x04Z(\d)([1-9]\d)$| p/Zope Enterprise Objects service/ i/ZODB $1.$2/

##############################NEXT PROBE##############################
Probe TCP GenericLines q|\r\n\r\n|
rarity 1
ports 21,23,35,43,79,98,110,113,119,199,214,264,449,505,510,540,587,616,628,666,731,771,782,1000,1010,1040-1043,1080,1212,1220,1248,1302,1400,1432,1467,1501,1505,1666,1687-1688,2010,2024,2600,3000,3005,3128,3310,3333,3940,4155,5000,5400,5432,5555,5570,6112,6667-6670,7144,7145,7200,7780,8000,8138,9000-9003,9801,11371,11965,13720,15000-15002,18086,19150,26214,26470,31416,30444,34012,56667

# Library as in books: http://solutions.3m.com/wps/portal/3M/en_US/library/home/resources/protocols/
match 3m-sip m|^Invalid request string: Request string is: \"\r\"$| p/Standard Interchange Prototol 2.0/ i/Integrated Library System authentication; Civica Spydus 7/

match abc m|^Feedback\nError=You need unique ID to command ABC!| p/ABC Torrent http interface/

match achat m|^ERROR\r\n$| p/AChat chat system/

match antivir m|^\0\0\x80\0$| p/drweb anti-virus/
match as-servermap m|^-\0\0\0\0$| p|IBM OS/400 as-servermapd| o|OS/400|
match access-remote-pc m|^\x99\xf3\0\0\0\0\0\0\xff\xff\xff\xff$| p/Access Remote PC/ o/Windows/

match as-sts m|^\0\0\0\0\0\0\0\x08$| p/IBM Service Tool Server AS-STS/

match authpoint m|^\[AUTHPOINT RESPONSE\]\r\nreturn_code=AUTHPOINT ERROR\r\nreturn_code_text=Error response parsed by base message object: Invalid or missing register #\r\nresponse=\r\nidentifier=\r\napproval_code=\r\n$| p/Authpoint payment processing/

match avk m|^Unknown command\r\n$| p/G Data AVK anti-virus/

match backdoor m|^Can't fork pty, bye!\n$| p/PsychoPhobia backdoor/ i/**BACKDOOR**/

match biff m|^Message received\n$| p/NotifyMail biffd/
match biff m|^Use of uninitialized value in transliteration \(tr///\) at /var/jchkmail/user-filter| p/Joe's j-chkmail biffd/
match bitdefender-ctrl m|^\(null\) 500 Internal Error\n\(null\) 500 Internal Error\n$| p/Bitdefender Remote Admin Console/ o/Windows/

match bittorrent-tracker m|^This is not a rootkit or other backdoor, it's a BitTorrent\r\nclient\. Really\.| p/Transmission bittorrent tracker/

# bnetd (PvPGN BnetD Mod version 1.5.0) on Debian GNU/Linux (sid)
match bnetd m|^BOT or Telnet Connection from \[[\d.]+\]\r\n\r\nEnter your account name and password\.\r\nSorry, there is no guest account\.\r\n\r\nUsername: | p/PvPGN BnetD Mod/ v/1.5.0/

match bnetd m|^Connection from \[[\d.]+\]\r\n\r\nEnter your account name and password\.\r\nSorry, there is no guest account\.\r\n\r\nUsername: | p/bnetd/

# bnetd server 0.4.25 on Linux
match bnetd m|^Username: $| p/bnetd open source Blizzard Battlenet server/
match bnetd m|^\r\nEnter your account name and password\.\r\n\r\nUsername:| p/bnetd open source Blizzard Battlenet server/
match boinc m|^<unrecognized/>\n\x03$| p/Boinc GUI RPC port/
match boinc m|^<error>unrecognized op</error/>\n\x03$| p/Boinc GUI RPC port/
match boinc m|^<boinc_gui_rpc_reply>\n<error>unrecognized op</error>\n</boinc_gui_rpc_reply>\n\x03| p/Boinc GUI RPC port/
match boinc m|^<boinc_gui_rpc_reply>\n<error>unrecognized op: \r\n\r</error>\n</boinc_gui_rpc_reply>\n\x03| p/Boinc GUI RPC port/
match boinc m|^<boinc_gui_rpc_reply>\n<client_version>(\d+)</client_version>\n<error>unrecognized op</error>\n</boinc_gui_rpc_reply>\n| p/Boinc GUI RPC port/ v/$1/
match boinc m|^<boinc_gui_rpc_reply>\n<client_version>(\d+)</client_version>\n<unauthorized/>\n</boinc_gui_rpc_reply>\n| p/Boinc GUI RPC port/ v/$1/
match boinc m|^<boinc_gui_rpc_reply>\n<major_version>(\d+)</major_version>\n<minor_version>(\d+)</minor_version>\n<release>(\d+)</release>| p/Boinc GUI RPC port/ v/$1.$2.$3/
match boinc m|^<boinc_gui_rpc_reply>\n<unauthorized/>\n</boinc_gui_rpc_reply>\n\x03| p/Boinc GUI RPC port/ i/Unauthorized/

match bzr m|^error\x01Generic bzr smart protocol error: bad request '\\r'\n$| p/Bazaar VCS bzr serve/

match caldav m|^HTTP/1\.1 503 Service Unavailable\r\nServer: DavMail Gateway ([\w._-]+)\r\nDAV: 1, calendar-access, calendar-schedule, calendarserver-private-events, addressbook\r\n.*Content-Length: 32\r\n\r\njava\.util\.NoSuchElementException$|s p/DavMail CalDAV http gateway/ v/$1/ d/proxy server/

match cisco-lm m|^<\?xml version=\"1\.0\" encoding=\"UTF-8\"\?><LicXmlDoc><MessageType><ParamValue>RESPONSE</ParamValue></MessageType><OperationCode><ParamValue>4923</ParamValue></OperationCode></LicXmlDoc>$| p/Cisco CallManager license manager/ v/6/

# Cisco PIX 501 running PIX IOS 6.3(1)
match ciscopsdm m|^\xc0\0\x01\0....\0\0\0\x03|s p/Cisco PIX Secure Database Manager/ d/firewall/ o/IOS/
match cisco7200sim m|^200-At least a module and a command must be specified\r\n200-At least a module and a command must be specified\r\n| p/Cisco 7200 Simulator/
match crossmatchverifier m|^Idle\r\n$| p/Cross Match Technologies Verifier fingerprint capture control port/
match clam m|^UNKNOWN COMMAND\n$| p/Clam AV/
match cmae m|^_err=refused%20by%20workers\r\n$| p/Cloudmark cmae_server antispam/
match conserver m|^ok\r\nunknown command\r\nunknown command\r\n$| p/conserver serial console daemon/ d/specialized/

match crestron-control m|^INVALID_COMMAND\r| p/TiVo DVR Crestron control server/ d/media device/

match cso m|^598:\(null\):Command not recognized\.\n| p/Columbia University QIL Gateway/ i/Qi to LDAP/

match datamaxdb m|^X01\r\nX01\r\n$| p/MailMax DataMaxDB/ o/Windows/

match desktop-central m|^Invalid FT GWADDR / START protocol\n$| p/ManageEngine Desktop Central DesktopCentralServer/ d/remote management/
match desktop-central m|^Invalid GWADDR / START protocol\n$| p/ManageEngine Desktop Central DesktopCentralServer/ d/remote management/

# HP Digital Sender Service (dss)
match hpdss m|^(53 client not logged in\.\r\n)+$| p/HP Digital Sender client/

match dusk m|^\x03Not a valid name\. This may because you left it blank or used invalid symbols\. Please try again\.\n| p/Dusk Java-based game/

match ecopy m|^e\0C\0o\0p\0y\0V\x004\x000\0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \x006\x007\0 \x004\x000\x002\0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \x000\0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \0 \x000\0F\0a\0i\0l\0e\0d\0 \0t\0o\0 \0r\0e\0t\0r\0i\0e\0v\0e\0 \0a\0 \0f\0u\0l\0l\0 \0e\0C\0o\0p\0y\0 \0T\0c\0p\0H\0e\0a\0d\0e\0r\0:\0 \0o\0n\0l\0y\0 \0\[\x004\0\]\0 \0b\0y\0t\0e\0s\0 \0r\0e\0c\0e\0i\0v\0e\0d\0!\0$| p/eCopy Agent/

# I think this type of eggdrop banner is only used when customized or such.
match eggdrop m|^\r\nNickname\.\r\nSorry, that nickname format is invalid\.\r\n$| p/Eggdrop irc bot console/
match eggdrop m|\r\nSorry, that nickname format is invalid\.\r\n$| p/Eggdrop irc bot console/
match eggdrop m|^\r\nSurnom\.\r\nSorry, that nickname format is invalid\.\r\n$| p/Eggdrop irc bot console/ i/French/

match finger m|^Gathering system data\.\.\.\nUsername Real name                      Idletime TTY Remote console location\n| p/Cfingerd/
match finger m|^Punix version ([\d./()]+) - Current Time \(since boot\) \d+:\d\d:\d\d\r\nName        pid    stat   pc       cpusec    stack    pr/sy   idle    tty\r\n| p/Lantronix ETS16 fingerd/ i/Punix $1/ d/terminal server/ o/Punix/
match finger m|^Finger online user list request denied\.\r\n| p/SLMail fingerd/ o/Windows/
match finger m|^Username Real name                      Idletime TTY Remote console location\n| p/Configurable Finger-Query Daemon/ o/Unix/
match finger m|^Login     Name       Tty      Idle  Login Time   Office     Office Phone\r\n| p/Debian fingerd/ o/Linux/
match finger m|^\r\nIntegrated port\r\nPrinter Type: Dell Laser Printer ([-\w+.]+)\r\nPrint Job Status: (.*)\r\n| p/Dell $1 laser printer fingerd/ i/Status: $2/ d/printer/
match finger m|^\r\nIntegrated port\r\nPrinter Type: Dell ([-\w+.]+) Laser Printer\r\nPrint Job Status: (.*)\r\n| p/Dell $1 laser printer fingerd/ i/Status: $2/ d/printer/
match finger m|^This is finger server\r\n\r\nPlease use username@domain format\.\r\n| p/ArGoSoft Mail fingerd/ o/Windows/
match finger m|^This is ([-\w_.]+) finger server\.\r\n\r\nPlease use username@domain format\.\r\n| p/ArGoSoft Mail fingerd/ h/$1/ o/Windows/
match finger m|^\r\nIntegrated port\r\nPrinter Type: Lexmark ([^\r\n]+)\r\n| p/Lexmark $1 printer fingerd/ d/printer/
match finger m|^finger: /var/adm/lastlog open error\nNo one logged on\r\n| p/Solaris 10 fingerd/ i/Nobody logged in/ o/Solaris/
match finger m|^finger: /var/adm/lastlog open error\nLogin       Name| p/Solaris 10 fingerd/ i/Somebody logged in/ o/Solaris/
match finger m|^\r\nUSB port \d+\r\nPrinter Type:  Photo AIO Printer (\w+)\r\nPrint Job Status: ([^\r\n]+)\r\n| p/Dell Photo AIO $1 printer fingerd/ i/Status $2/ d/printer/
match finger m|^\nDebian GNU/Linux      Copyright \(c\) 1993-1999 Software in the Public Interest\n\n                 Your site has been rejected for some reason\.\n\n         This may be caused by a missing RFC 1413 identd on your site\.\n\n| i/Debian Cfingerd/ o/Linux/
match finger m|^Debian GNU/Linux      Copyright \(C\) 1993-1999 Software in the Public Interest\n.*You haven't specified a user\.\n\n               A general listing is not provided to the public\.|s p/Debian Cfingerd/ o/Linux/
match finger m|^\r\nPrinter Type: Lexmark Optra LaserPrinter\r\n| p/Lexmark Optra LaserPrinter fingerd/ d/printer/
match finger m|^MSS485 Version V([\w._/-]+)\(([\w._-]+)\) - Time Since Boot:| p/Lantronix MSS485 serial to ethernet bridge fingerd/ v/$1 $2/ d/bridge/
match finger m|^Login     Name                Tty      Idle  Login Time   Office     Office Phone\n| p/xfingerd/

match ftp m|^220 Welcome to Stupid-FTPd server\.\r\n422 Too busy to play with you\.\r\n| p/stupid-ftpd/

match mon m|^520 invalid command\n$| p/Perl service monitoring daemon/

match mysql m|^\x10\0\0\x01\xff\x13\x04Bad handshake$| p/MySQL/

match netbackup m|^\xea\xdd\xbe\xef\0\0\0\x05\0\0\x000\0\0\x000\0\0..\0\0\0\x08\0a\0f\0f\0s\0p\0r\0n\0g\0\0\0\0\0\0\0\0$|s p/Veritas Netbackup Professional/

match nimp m|^V([\d.]+)\r\nERROR 0\r\n$| p/Linux NetworX Network ICE Management Protocol/ v/$1/ o/Linux/

# Alcatel Speedtouch ADSL Router
match ftp m|^220 Inactivity timer = \d+ seconds\. Use 'site idle <secs>' to change\.\r\n221 Goodbye \(badly formated command seen\)\.  You uploaded 0 and downloaded 0 kbytes\.\r\n221 Goodbye \(badly formated command seen\)\.  You uploaded 0 and downloaded 0 kbytes\.\r\n$| p/Alcatel Speedtouch ADSL router ftpd/ d/broadband router/
# bftpd 1.0.22 on Linux 2.4
match ftp m|^220 \r\n500 Unknown command: \"\"\r\n500 Unknown command: \"\"\r\n$| p/bftpd/
# Multitech MultiVoip 410 VoIP gateway
match ftp m|^220 Service ready\r\n500 Unsupported command\r\n$| p/Multitech MultiVoip 410 VoIP gateway ftpd/ d/VoIP adapter/
# NetportExpress PRO/100 3 port print server
match ftp m|^220 FTP server ready\.\r\n530 access denied\.\r\n| p/Intel NetportExpress print server ftpd/ d/print server/
# D-Link Print Server internal FTP daemon (Firmware version 1.38) - D-Link Print Server DP-101
match ftp m|^220 FTP server ready\.\r\n501 Command not supported\.\r\n$| p/D-Link Printer Server ftpd/ d/print server/
match ftp m|^220 ([-.\w]+) FTP server ready\.\r\n530 Please login with USER and PASS\.\r\n530 Please login with USER and PASS\.\r\n$| p/Solaris ftpd/ h/$1/ o/Solaris/
match ftp m|^220 ([-.\w]+) FTP Server ready \.\.\.\r\n530 \r  : User not logged in\. Please login with USER and PASS first\.\r\n530 \r  : User not logged in\. Please login with USER and PASS first\.\r\n$| p/Bulletproof ftp server/ o/Windows/ h/$1/
# BulletProof FTP 2.21 on Windows 2000 Server
match ftp m|^220 ftp\r\n$| p/Bulletproof ftp server/ o/Windows/
match ftp m|^220 FTP server ready\.\r\n200 NOOP command successful\.\r\n| p/Tektronix Phaser ftpd/ d/printer/
match ftp m|^220 \"Welcome to Bot FTP service\.\"\r\n331 Please specify the password\.\r\n230 Login successful\. Have fun\.\r\n| p/Unknown trojan ftpd/
match ftp m|^220 OK\n226 OK\n| p/Sasser worm minimal ftpd/ o/Windows/
# USR8022 or AirLive WT-2000R WAPs
match ftp m|^220 FTPd ([\d.]+)\r\n500 Bad command\r\n| p/Generic WAP ftpd/ v/$1/ d/WAP/
match ftp m|^220 Telindus FTP server ready\.\r\n502 Command not implemented\.\r\n502 Command not implemented\.\r\n| p/Telindus ftpd/ d/router/
match ftp m|^220 Server ready\r\n500 '\r': command not understood\.\r\n500 '\r': command not understood\.\r\n| p/Welltech Wellgate VoIP adapter ftpd/ d/VoIP adapter/
match ftp m|^220 muddleftpd \(([\d.]+)\) server ready\. Enter Username\.\r\n500 Only one command at a time\.\r\n| p/Muddleftpd/ v/$1/
match ftp m|^220 .*\r\n500 Only one command at a time\.\r\n| p/Muddleftpd/
match ftp m|^220 OK\r\n500 Syntax error, command unrecognized\.\r\n| p/NcFTPd/ i/Banner masking/
match ftp m|^220 ([\w._-]+) FTP server ready\.\r\n502 '': command not understood\.\r\n502 '': command not understood\.\r\n| p/lukemftpd/ h/$1/ o/Mac OS X/
match ftp m|^220 ([\w._-]+) FTP server ready\.\r\n500 '': command not understood\.\r\n500 '': command not understood\.\r\n| p/OpenBSD ftpd/
match ftp m|^220 FTP server ready\.\r\n500 \?\r\n500 \?\r\n| p/Kiss DP-558 PVR ftpd/ d/media device/
match ftp m|^220 ICS FTP Server ready\r\n500 '\r': command not understood\.\r\n500 '\r': command not understood\.\r\n| p/berretz.de mini-ftpd/ o/Windows/
match ftp m|^220 Welcome to pyftpd\. Happy downloading\.\r\n500 I'm gonna ignore this command\.\.\. maybe later\.\.\.\r\n| p/pyftpd/
match ftp m|^220 Ready\r\n502 Not implemented\r\n$| p/Global Cache GC-100 ftpd/ d/media device/
match ftp m|^220 FTP server ready\.\r\n530 Please login with USER and PASS\.\r\n$| p|TRENDnet/Hawking webcam ftpd| d/webcam/
match ftp m|^220 ([\w._-]+) server ready\.\r\n502 command  not implemented\.\r\n502 command  not implemented\.\r\n| p/Konica Minolta bizhub printer smtpd/ d/printer/ h/$1/
match ftp m|^220 Ftp firmware update utility\r\n500 Unknown command: \"\"\r\n500 Unknown command: \"\"\r\n| p/D-Link or USRobotics ADSL router firmware update ftpd/ d/broadband router/
match ftp m|^220 Adtec .* FTP server, ready \r\n530 Login failed, check Username/Password\.\r\n| p/Adtec broadcast video ftpd/ d/media device/
match ftp m|^220 FTP Server Ready\r\n530 Authentication required\.\r\n530 Authentication required\.\r\n| p/HP LaserJet P4014 printer ftpd/ d/printer/
match ftp m|^220 FTP server ready\.\r\n530 USER and PASS required\r\n530 USER and PASS required\r\n| p/VBrick 4300 video encoder ftpd/ d/media device/
match ftp m|^220 FTP server ready\.\r\n510 command not supported\.\r\n| p/Panasonic DP-1820E printer ftpd/ d/printer/
match ftp m|^220 ftp server ready\.\r\n500 Unknown command: \"\"\r\n500 Unknown command: \"\"\r\n| p/Linksys WRT54Gv5 WAP ftpd/ d/WAP/
match ftp m|^220 Connection established\.\r\n502  command not recognized\.\r\n502  command not recognized\.\r\n| p/Canon imageRUNNER C2880 printer ftpd/ d/printer/
match ftp m|^550 Access is denied\.\r\n550 Access is denied\.\r\n220 ProFTPD ([\w._-]+) Server \(([\w._-]+)\)| p/ProFTPD/ v/$1/ h/$2/
match ftp m|^220 UnleashX FTP ready\.\r\n503 Login with USER first\.\r\n| p/UnleashX Xbox shell ftpd/ d/game console/
match ftp m|^220 BBPS3FTP ready\r\n500 command not recognized\r\n| p/Blackbox PlayStation 3 ftpd/ d/game console/
match ftp m|^220 IronPort WSA ready\.\r\n500 Syntax error, command unrecognized\.\r\n| p/IronPort WSA firewall ftpd/ d/firewall/
match ftp m|^220 \r\n500-'\r\n500  ': command not understood\.\r\n500-'\r\n500  ': command not understood\.\r\n| p/Microsoft FTP Service/ o/Windows/
match ftp m|^220 ps2ftpd ready\.\r\n500 Not understood\.\r\n| p/ps2ftpd/ d/game console/
match ftp m|^\xff\xfb\x01\xff\xfb\x03\xff\xfc\"\r\n\r\n\n\rauthentication failed!\n\rpassword: | p/Effekta MH 6000 UPS telnetd/ d/power-device/
match ftp m|^\xff\xfc\"\xff\xfb\x01\r\nPassword: \r\nbad password\r\n| p|Campbell Scientific NL-100/105 Ethernet-to-serial bridge telnetd| d/bridge/
match ftp m|^\xff\xfb\x03\xff\xfd\x03\xff\xfb\x01\r\nUsername: \r\nPassword: \r\nAccess Denied\r\n| p/InterSystems CTELNETD/
match ftp m|^\xff\xfe\x01\xff\xfb\x01\xff\xfb\x1f\xff\xfb\x03\xff\xfd\x03\xff\xfe'\xff\xfc'\xff\xfc\"\xff\xfd\x1f\xff\xfa\x18\x01\xff\xf0\0\r\nWelcome to ([\w._-]+), please identify yourself\r\n\r\nuser:\r\r\npass:\*ReactOS Operating System \[Version ([\w._-]+)\]\r\n\(C\) Copyright [\d-]+ ReactOS Team\.\r\n\r\nC:\\ReactOS\\System32>| p/ReactOS telnetd/ v/$2/ h/$1/ i/no authentication/
match ftp m|^220-Authenticate for FTP Access\. \r\n220 \r\n500-Syntax error -- unknown command\r\n500 \r\n500-Syntax error -- unknown command\r\n500 \r\n| p/Microsoft TMG firewall ftpd/ d/firewall/

# vsftpd (Very Secure FTP Daemon) 1.0.0 on linux with custom ftpd_banner
# We'll have to see if this match is unique enough ... no, it is not enough...
# Turning match line into softmatch because it can match much more than just
# vsftpd and WU-FTPD... (Brandon)
# Adding this back as a hard match or we'll never stop getting vsftpd
# submissions. (David)
# See version 2.0.8 note under TCP Help probe.
match ftp m|^220 .*\r\n530 Please login with USER and PASS\.\r\n530 Please login with USER and PASS\.\r\n| p/vsftpd (before 2.0.8) or WU-FTPD/

match flashconnect m|^FlashCONNECT ([\d.]+) invalid message\.\n$| p/Raining Data FlashCONNECT/ v/$1/

match fw1-topology m|^Q\0\0\0$| p/Checkpoint FW-1 Topology download/ d/firewall/

match geovision-control m|^..\0\0\xff\xff\xff\xff$|s p/Geovision webcam control/ d/webcam/
match geovision-audio m|^\$\0\0\0\xd4\x17\0\0\x01\0\0\0\x05\0\0\0\x01\0\0\0\x05\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0$| p/Geovision webcam audio/ d/webcam/

# GKrellM System Monitor 2.1.15 on Linux
softmatch gkrellm m|^<error>\nBad connect string!| p/GKrellM System Monitor/

match control-gc-ports m|^unknowncommand 14\r$| p/Global Cache GC-100 config/ d/media device/

match halfd m|^{type INIT} {up \d+} {auth \d+} {name {([^}]+)}} {ip [\d.]+} {max \d+} {port (\d+)}\r\n| p/halfd Half-Life admin/ i/Name $1; HL port $2/

match hasp-lm m|^\xf2\xfa\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\xf2\0\0\0\0\0\0\0\0$| p/Aladdin NetHASP license manager/

match hpssd m|^msg=messageerror\nresult-code=5\n| p/HP Services and Status Daemon/ o/Linux/

# Ubicom embedded ( http://www.ubicom.com/home.htm )
match http m|^HTTP/1\.1 400 Bad Request\r\nCache-control: no-cache\r\nServer: Ubicom/(\d[-.\w ]+)\r\n| p/Ubicom httpd/ v/$1/
match http m|^HTTP/1\.0 400 Bad Request\r\nExpires: Mon, 1 Jan 2001 12:00:01 GMT\r\nCache-control: no-cache\r\nServer: Ubicom/([\w._-]+)\r\nContent-Length: 11\r\nConnection: close\r\n\r\nBad RequestHTTP/1\.1 500 Server Error\r\n\r\nConnection: close\r\n$| p/Ubicom httpd/ v/$1/ i/CradlePoint MBR1000 WAP http config/ d/WAP/
match http m|^<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 3\.2//EN\">\n<html>\n<head>\n<title>GoodTech Systems Telnet Server Administration Login</title>\n| p/GoodTech Systems telnet server http config/ o/Windows/
match http m|^HTTP/1\.1 400 Bad Request\r\nDate: .*\r\nConnection: close\r\nContent-Type: text/html\r\nContent-Length: 50\r\n\r\n<HTML><BODY><H1>400 Bad Request</H1></BODY></HTML>$| p/VMware Server http config/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\nContent-type: text/html; charset:UTF-8\r\n\r\n.*<TITLE>SQLite Book</TITLE>|s p/SQLite Book database frontend/

# Some web servers don't give a 'Server: ' line for the Get request, but do for this probe.
match http m|^HTTP/1\.1 400 .*\r\nServer: Microsoft-IIS/(\d[-.\w]+)\r\n| p/Microsoft IIS httpd/ v/$1/ o/Windows/
# Icecast version: 1.9+2.0alphasn
match http m|^HTTP/1\.0 401 Authentication Required\r\nWWW-Authenticate: Basic realm=\"Icecast2 Server\"\r\n\r\nYou need to authenticate\r\n| p/Icecast streaming media server/
# Network Flight Recorder v3.2 on Solaris 8 (sparc)
match http m|^HTTP/1\.0 400 Bad request\r\n\r\n$| p/Network Flight Recorder IDS/
# Cisco 350 Series 802.11 AP - THIS MATCH LINE MIGHT BE TOO GENERAL -Doug
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: thttpd/(\d[-.\w ]+)\r\n| p/thttpd/ v/$1/ d/WAP/
# OpenPGP Public Key Server 0.9.6
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: pks_www/([-\w+.]+)\r\nContent-type: text/html\r\n\r\n<HEAD><TITLE>400 Bad Request</TITLE></HEAD><BODY></BODY>\r\n| p/OpenPGP Public Key Server/ v/$1/
match http m|^HTTP/1\.1 401 Unauthorized\r\nConnection: close\r\nContent-Length: \d+\r\nContent-Type: text/html\r\nWWW-Authenticate: Basic realm=\"osiris\"\r\n| p/osiris host IDS web interface/
match http m|^HTTP/1\.1 501 Not Implemented\r\nCache-Control: no-cache, must-revalidate, max-age=0\r\nContent-Type: text/html; charset=UTF-8\r\nContent-Length: \d+\r\nConnection: close\r\n\r\n<html><body><h1>Not Implemented</h1>Whatever the heck you just requested, I can't generate\.</body></html>| p/darkstat network analyzer httpd/ o/Unix/
match http m|^\xff\xf0 400 Bad Request\r\n\r\n<HEAD><TITLE>400 Bad Request</TITLE></END>\r\n<BODY><H1>400 Bad Request</H1></BODY>| p/HP JetDirect printer embedded httpd/ d/printer/
match http m|^HTTP/1\.0 400 Bad Request\r\n.*This is a WebSEAL error message template file\.|s p/Tivoli Access Manager WebSEAL httpd/
# Keep this above the more general thttpd match lines below
match http m|^UNKNOWN 400 Bad Request\r\nServer: thttpd\r\n.*<HTML>\n\t<HEAD><TITLE>Error</TITLE><LINK REL=\"stylesheet\" TYPE=\"text/css\" HREF=\"/std\.css\">.*Your request has bad syntax or is inherently impossible to satisfy|s p/thttpd/ i/Linksys NSLU2 http config/ d/storage-misc/
match http m|^UNKNOWN 400 Bad Request\r\nServer: thttpd/([\w.]+) \w+\r\n| p/thttpd/ v/$1/
match http m|^UNKNOWN 400 Bad Request\r\nServer: \r\nContent-Type: text/html\r\n.*<H2>400 Bad Request</H2>\nYour request has bad syntax or is inherently impossible to satisfy\.\n|s p/thttpd/
match http m|^HTTP/1\.0 400 Bad Request\r\n.*<h2>400 Bad Request<h2>\n  <p>\n  Your request has bad syntax or is inherently impossible to satisfy\.\n|s p/thttpd/
match http m|^HTTP/1\.0 400 Bad Request\r\nContent-type: text/html; charset=iso-8859-1\r\nAccept-Ranges: bytes\r\nConnection: close\r\n\r\n<HTML><HEAD><TITLE>400 Bad Request</TITLE></HEAD>\n<BODY BGCOLOR=\"#cc9999\"><H2>400 Bad Request</H2>\n<HR>\nYour request has bad syntax or is inherently impossible to satisfy\.\n</BODY></HTML>\n$| p/thttpd/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: UnrealEngine UWeb Web Server Build (\d+)\r\n|s p/Unreal Tournament http admin/ v/Build $1/
match http m|^HTTP/1\.0 405 Method Not Allowed\r\nAllow: GET, HEAD\r\n\r\n405 Method Not Allowed\r\n\r\n| p|D-Link printer/webcam http config|
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: WDaemon/([\d.]+)\r\n| i/Alt-N MDaemon webmail/ p/World Client WDaemon httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\nAccept: text/html\nConnection: close\n\n<html>\n<body text=#FFFFFF bgcolor=#000000>\n<center><b><hr height=4 width=400 color=#FF0000>\n<font size=5>PunkBuster Server WebTool for ([-\w_.]+)</font>| p/PunkBuster http config/ i/Game: $1/
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: MpSconServer/([\d.]+)\r\n| p/ZebraNet print server httpd/ i/MpSconServer $1/ d/print server/
match http m|^HTTP/1\.1 \d\d\d .*var l1=\"([^"]+)\"\n.*document\.write\(\"D-Link DI-\"\+l1\)|s p/D-Link DI-$1 router http config/ d/router/
match http m|^HTTP/1\.0 400 bad http request\r\ndate: .*\r\nserver: SAP Web Application Server\r\n| p/SAP Web Application Server/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: text/html; charset=UTF-8\r\nPragma: no-cache\r\nWindow-target: _top\r\n| p/Symantec AntiVirus Scan Engine http config/
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: QTSS ([\d.]+) Admin Server/([\d.]+)\r\n| p/QTSS Admin Server httpd/ v/$2/ i/QTSS $1/
match http m|^HTTP/1\.0 400 Bad Request 2\r\nContent-Type: text/html\r\n\r\n<body><h1>HTTP/1\.0 400 Bad Request 2</h1></body>\r\n$| p/WatchGuard Firebox http config/ d/firewall/
match http m|^HTTP/1\.0 400 Bad Request\r\nContent-Type: text/html\r\n\r\n<title>400 Bad Request</title><body>400 Bad Request</body>$| p|Generic router http config| d/router/
match http m|^HTTP/1\.1 \d\d\d .*\nWWW-Authenticate: Basic realm=\"Anti-Spam SMTP Proxy \(ASSP\) Configuration\"\nContent-type: text/html\n\n<html><body><h1>Unauthorized</h1>\n</body></html>\n| p/ASSP Anti-Spam Proxy http config/
match http m|^HTTP/1\.0 400 Bad Request\r\nConnection: close\r\nServer: HttpServer/([\d.]+)\r\nDate: .*\r\nContent-Type: text/html\r\n\r\nError:<HR>\n<H1>Server Error: 400 Bad Request</H1>\r\n<P><HR><H2>URL parsing error</H2><P>| p/Cisco ONS MSPP httpd/ i/HttpServer $1/
match http m|^HTTP/1\.0 500 no query\r\n\r\n$| p/pkspxy/
match http m|^HTTP/1\.0 400 msg=Bad%20Request&rc=%00%00%03%1b\r\n| p/TimesTen httpd/
match http m|^HTTP/1\.1 400  Bad  request\r\nContent-Type: text/html; charset=ISO-8859-1\r\n\r\n<body><h1>HTTP/1\.1 400  Bad  request <h1></body>| p/XOSoft WanSync http config/ o/Windows/
match http m|^HTTP/\*\.\* 400 Bad Request\r\nDate: .*\r\nContent-Type:text/plain\r\nContent-Length:61\r\n\r\nThe received request is either NULL or invalid/wrong format\r\n| p/Kaba application server httpd/

# This lame service responds in many wierd ways - luckily always to GenericLines
match http m|^HTTP/1\.1 403 Forbidden\r\nContent-Type: text/xml\r\n\r\n<\?xml version='1\.0' encoding='UTF-8' \?><autnresponse><action>NONE</action><response>The action you attempted is forbidden by your client</response></autnresponse>| p/Veritas backup exec continuous protection httpd/
match http m|^HTTP/1\.1 403 Forbidden\nContent-Type: text/xml\n\n<ACTION>GETSTATUS</ACTION><RESPONSE>The action you attempted is forbidden by your client</RESPONSE>| p/Veritas backup exec continuous protection httpd/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: text/html\r\n\r\n\n\nCONNECTION NOT AUTHORIZED\n\n\n| p/Veritas backup exec continuous protection httpd/ i/unauthorized/
match http m|^HTTP/1\.0 200 OK\nContent-type: text/plain\n\n\nConnection refused\.\nInvalid IP Address\n| p/Veritas backup exec continuous protection httpd/ i/unauthorized/

match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-Length: \d+\r\nContent-Type: text/html\r\nConnection: close\r\nServer: Fastream IQ Web/FTP Server\r\n\r\n| p/Fastream IQ reverse http proxy/ o/Windows/
match http m|^HTTP/1\.0 -1 Internal Server Error\r\n\r\n| p/Panasonic webcam http config/ d/webcam/
match http m|^HTTP/1\.1 401 Authorization Required\nServer: JBidWatcher/([\d.]+) \(Java\)\nWWW-Authenticate: Basic realm=\"JBidWatcher\"\n| p/JBidWatcher httpd/ i/Java/ v/$1/
match http m|^HTTP/1\.0 501 R\r\nContent-Type: text/html\r\n\r\nNot Implemented| p|D-Link router/Airlink NAS http config|
match http m|^HTTP/1\.1 500 Internal server error\r\nContent-Length: 7\r\n\r\nBummah\.| p/Sendmail Mailstream Manager http config/
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: IngrianManagementConsole\r\n| p/Ingrian Management Console httpd/ d/security-misc/
match http m|^\(null\) 400 Bad Request\r\nDate: .*<title>400 Bad Request</title></head>\n<body>\n<h3>400 Bad Request</h3>\nCan't parse request\.\n</body>\n</html>\n|s p/m0n0wall http portal/ o/FreeBSD/ d/firewall/
match http m|^\(null\) 302 Found\r\nServer: \r\nDate: .*\r\nLocation: /index\.cgi\r\nContent-Type: text/html; charset=%s\r\nCache-Control: max-age=0\r\n| p|Intel/Acer/FlaconStor storage device http config| d/storage-misc/
match http m|^HTTP/1\.1 505 Server Error\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<HTML><BODY>\n<TITLE>505 Internal Server Error</TITLE><H1>Internal Server Error: Invalid request</H1>\n<BR><BR>Internal Error\.\n</BODY></HTML>\n| p/Google Desktop Search for Linux Beta httpd/ o/Linux/
match http m|^<HTML><HEAD><TITLE>400 Malformed request line</TITLE></HEAD><BODY.*http://tjws\.sourceforge\.net\">Rogatkin's JWS based on Acme\.Serve Version ([-\w_.]+), .Revision: ([-\w_.]+)|s p/TJWS httpd/ v/$2/ i/Based on Acme.Server $1/
match http m|^HTTP/1\.1 500 Internal Server Error\r\nContent-Length: \d+\r\n\r\nTraceback \(most recent call last\):\n  File \"/usr/share/deluge/plugins/WebUi/gtk_cherrypy_wsgiserver\.py\"| p/Deluge bittorrent http interface/ i/CherryPy httpd/
match http m|^HTTP/1\.0 400 Invalid Request\r\nContent-Type: text/html\r\nContent-Length: 31\r\n\r\n<title>Invalid Request</title>\n$| p/opentracker BitTorrent tracker/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: HP Web Jetadmin (\d[-.\w]+)\r\n| p/HP Web Jetadmin print server http config/ v/$1/ d/print server/
match http m|^HTTP/1\.1 404 \r\n.*<ns1:stackTrace xmlns:ns1=\"http://xml\.apache\.org/axis/\">java\.io\.IOException: Cannot handle non-GET, non-POST, non-HEAD request\n\tat org\.globus\.wsrf\.container\.ServiceThread\.parseHeaders\(ServiceThread\.java:855\)|s p/Globus Web Service httpd/
match http m|^HTTP/1\.1 511 Not Implemented\r\n\r\n$| p|SMC Barricade/Netgear http config| d/broadband router/
match http m|^HTTP/1\.1 400 Bad Request\r\n.*document\.write\(document\.nxp\.skin\.getProductName\(\)\);\n      document\.write\('Security Console :: Error</title>'\);\n|s p/Rapid7 NeXpose http config/ d/security-misc/
match http m|^HTTP/1\.1 400 Bad Request\r\n.*<link rel=\"shortcut icon\" href=\"/style/image/favicon\.ico\" type=\"image/vnd\.microsoft\.icon\"></link>\n   <script type=\"text/javascript\" src=\"/scripts/controller\.js\"></script>\n   <script type=\"text/javascript\" src=\"/scripts/sarissa\.js\"></script>|s p/Rapid7 NeXpose http config/ d/security-misc/
match http m|^HTTP/1\.1 200 OK\r\nServer: peerguardnf/([\w._-]+) \(Unix\)\r\nX-Powered-By: You need to wind it\r\n| p/Phoenix Labs PeerGuardian httpd/ v/$1/ o/Unix/
match http m|^HTTP/1\.0 500 Internal Server Error\r\n.*<h2>Error parsing HTTP header</h2><pre>\njava\.net\.ProtocolException: Cannot handle non-GET, non-POST, non-HEAD request\n\tat org\.globus\.wsrf\.container\.ServiceThread\.parseHeaders\(ServiceThread\.java:1103\)\n|s p/Globus Toolkit Java Container httpd/
match http m|^HTTP/1\.0 404 Not Found\r\nContent-Type: text/html\r\n\r\n<HTML><HEAD><TITLE>HTTP 404 File not found</TITLE></HEAD><BODY TEXT=BLACK BGCOLOR=WHITE>The requested file was not found</BODY></HTML>| p/Websense Block Message httpd/
match http m|^HTTP/1\.1 401 Unauthorized\r\nDate: .*\r\nServer: cPanel\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"cPanel WebDisk\"\r\n\r\n| p/cPanel httpd/ o/Linux/ i/unauthorized/
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: micro_httpd\r\n| p/micro_http/
match http m|^HTTP/1\.0 401 Unauthorized\r\nConnection: close\r\nContent-Type: text/html\r\nServer: SNARE\r\nWWW-Authenticate: Basic realm=\"SNARE\"\r\n\r\n.*<ADDRESS>Snare Server Remote Control facility</ADDRESS>|s p/InterSect Alliance SNARE http config/
match http m|^HTTP/1\.0 200 OK\r\nCache-Control: no-cache\r\nPragma: no-cache\r\nExpires: 0\r\ncharset: UTF8\r\nContent-Type: text/html\r\n\r\n.*<title>MONyog</title>|s p/MONyog MySQL http admin/
match http m|^HTTP/1\.1 400 Bad Request\r\nServer: ATL Server - CounterSpyAgentSoapService\r\n.*<SOAP:Envelope xmlns:SOAP=\"http://schemas\.xmlsoap\.org/soap/envelope/\">\r\n  <SOAP:Body>\r\n   <SOAP:Fault>\r\n     <faultcode>SOAP:Client</faultcode>\r\n     <faultcode>Invalid Request</faultcode>\r\n     <detail>Not a recognized HTTP Verb &amp;Empty URL &amp;Not a recognized HTTP Version \(only 1\.1 is supported\) &amp;</detail>\r\n   </SOAP:Fault>\r\n  </SOAP:Body>\r\n</SOAP:Envelope>|s p/Sunbelt Software CounterSpy Agent antimalware SOAP over HTTP/
match http m|^HTTP/1\.0 500 Internal error\r\nContent-Length: 49\r\nContent-Type: text/plain\r\n\r\nMethod not allowed \(must be POST HTTP/1\.0 or 1\.1\)$| p/SoftPerfect Bandwidth Manager httpd/
match http m|^HTTP/1\.0 501 Not Implemented\r\nServer: Dorgem/([\w._-]+)\r\n| p/Dorgem webcam server http/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 400 Bad request version \(crypto mismatch\?\)\r\nServer: ShadowBot/([\d.]+)\r\n| p/ShadowBot/ v/$1/ i/HP Opsware/
match http m|^\(null\) 400 Bad Request\r\nServer: \r\n.*<HTML>\n            <HEAD><TITLE>400 Bad Request</TITLE></HEAD>\n            <BODY BGCOLOR=\"#cc9999\" TEXT=\"#000000\" LINK=\"#2020ff\" VLINK=\"#4040cc\">\n            <H4>400 Bad Request</H4>\nCan't parse request\.\n            <HR>\n            <ADDRESS><A HREF=\"\"></A></ADDRESS>\n            </BODY>\n            </HTML>\n$|s p/Linksys SVR4000 router/ d/router/
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: Extent/([\d.]+)\r\n\r\n<HTML><HEAD>\n<TITLE>Error</TITLE>\n</HEAD>\n<BODY>\n<H2>400 Bad Request</H2></BODY>\n</HTML>\n$| p/Alepo Extent/ v/$1/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"esecsrva\"\r\n\r\n\0{829,}| p/IBM Director wmicimserver httpd/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"esecsrva\"\r\n\r\n$| p/IBM Director wmicimserver httpd/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"ANLYX2\"\r\n\r\n\0*$| p/IBM Director wmicimserver httpd/
match http m|^HTTP/1\.0 501 Document Follows\r\nContent-Type: text/html\r\nContent-Length: 106\r\n\r\n<HEAD><TITLE>501 Method Not Implemented</TITLE></HEAD>\r\n<BODY><H1>501 Method Not Implemented</H1>\r\n</BODY>$| p/HP StorageWorks AG118A tape autoloader http config/ d/storage-misc/
match http m|^UNKNOWN 400 Bad Request\r\nServer: mini_httpd/([\w._ -]+)\r\n| p/mini_httpd/ v/$1/
match http m|^HTTP/1\.0 404 Not Found\r\nContent-Type: text/html\r\n\r\n$| p/JBoss service httpd/
match http m|^HTTP/1\.0 400 Bad Request\r\n.*Server: PeopleSoft PSRENSRV/([\w._-]+)\r\n.*<I>PeopleSoft PSRENSRV/[\w._-]+ on http://([\w._-]+):\d+</I>|s p/PeopleSoft Remote Event Notification Server httpd/ v/$1/ h/$2/
match http m|^ 501 Not Implemented\r\n.*Server: HT5XX ht\r\n|s p/Grandstream HT502 VoIP router http config/ d/VoIP adapter/
match http m|^HTTP/1\.0 400 Bad Request\r\n.*Server: sw-cp-server/([\w._-]+)\r\n.*<title>400 - Bad Request</title>|s p/sw-cp-server httpd/ i/Parallels Plesk WebAdmin version/
match http m|^HTTP/1\.0 \d\d\d [\w ]+\r\nServer: GRISOFT-AVG TCP Server/(\d[-.\w]+) .*\r\n| p/Grisoft AVG TCP Server/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\n.*<title>Netflix Application</title>.*<em>Generated by version ([\w._-]+) </em>|s p/Netflix Application httpd/ v/$1/ o/iOS/
match http m|^HTTP/1\.0 501 Not Implemented\r\n.*Server: SonicWALL (SSL-VPN [\w._-]+) Web Server\.\r\n.*POST to non-script is not supported\.\n|s p/Boa httpd/ i/SonicWALL $1 http proxy/ d/proxy server/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: application/ogg\r\nicy-br:(\d+)\r\nicy-description:VirtualDJ Direct Broadcast\r\nicy-genre:\r\nicy-name:VirtualDJ\r\nicy-pub:0\r\nicy-url:http://www\.virtualdj\.com/\r\nServer: VirtualDJ\r\n\r\n| p/VirtualDJ streaming audio/
match http m|^HTTP/1\.0 200 OK\r\nServer: icecast/(\d[-.\w]+)\r\n| p|Shoutcast/Icecast streaming audio| v|$1|
match http m|^HTTP/1\.0 200 OK\r\nContent-length: 0\r\n\r\nIBM Tivoli Identity Manager - ADK Version ([\w._-]+)\r\n\r\n| p/IBM Tivoli Identity Manager httpd/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\n\r\n<html><head><title>mongodb ([\w._-]+):\d+ </title>.*<pre>db version v([\w._-]+), pdfile version ([\w._-]+)\ngit hash: ([0-9a-f]{40})\nsys info: Linux [\w._-]+ ([\w._-]+) .* BOOST_LIB_VERSION=([\d_]+)\n\ndbwritelocked:  0 \(initial\)\nuptime:    ([^\n]+)\n|s p/MongoDB http console/ h/$1/ v/$2/ i/git version $4; pdfile $3; Boost $SUBST(6,"_","."); uptime $7/ o/Linux $5/
match http m|^HTTP/1\.1 501 Not Implemented\r\nServer: sfcHttpd\r\nContent-Length: 0\r\nConnection: close\r\n\r\nHTTP/1\.1 400 Bad Request\r\nServer: sfcHttpd\r\nContent-Length: 0\r\nConnection: close\r\n\r\n| p/sfcHttpd/ i/SuperMicro IPMI Small Footprint CIM Broker/
match http m|^HTTP/1\.1 501 Not Implemented\r\nServer: sfcHttpd\r\nContent-Length: 0\r\n\r\nHTTP/1\.1 400 Bad Request\r\nServer: sfcHttpd\r\nContent-Length: 0\r\n\r\n| p/sfcHttpd/
match http m|^HTTP/1\.0 400 Bad Request\r\n.*Server: CleanMail Service ([\w._-]+)\r\n|s p/CleanMail antispam http admin/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*Server: lighttpd/([\w._-]+).*<\?xml version=\"1\.0\" encoding=\"iso-8859-1\"\?>\n<!DOCTYPE html PUBLIC \"-//W3C//DTD XHTML 1\.0 Transitional//EN\"\n         \"http://www\.w3\.org/TR/xhtml1/DTD/xhtml1-transitional\.dtd\">\n<html xmlns=\"http://www\.w3\.org/1999/xhtml\" xml:lang=\"en\" lang=\"en\">\n <head>\n  <title>\d\d\d - [\w ]+</title>|s p/lighttpd/ v/$1/
match http m|^HTTP/1\.1 405 Method Not Allowed\r\nAllow: GET,HEAD\r\nDate: .*\r\nServer: Genetic Lifeform and Distributed Open Server ([\w._-]+)\r\n| p/Hentai@Home httpd/ v/$1/

match http-proxy m|^HTTP/1\.0 400 Bad Request\r\nContent-Type: text/html\r\nPragma: no-cache\r\nConnection: close\r\nContent-Type: text/html; charset=utf-8\r\n\r\n<html><body>Invalid request<P><HR><i>This message was created by WinRoute Proxy</i></body></html>| p/WinRoute http proxy/ o/Windows/
match http-proxy m|^HTTP/1\.0 400 Bad Request\r\n.*<html><body>\t\t<i><h2>Invalid request:</h2></i><p><pre>Bad request format\.\n</pre><b>\t\t</b><p>Please, check URL\.<p>\t\t<hr>\t\tGenerated by Oops\.\t\t</body>\t\t</html>$|s p/Oops! http proxy/ d/proxy server/
match http-proxy m|^HTTP/1\.0 503 Internal error\r\nServer: awarrenhttp/([\w._]+)\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<html> <head> <title> Internal Error </title> </head> <body> <hr> <p> An internal server error occurred while processing your request\. Please contact administrator\.\n<BR> <BR> Reason: Could not relay request </p> </body> </html>$| p/awarrenhttp http proxy/ v/$1/ d/proxy server/ i/Cyberoam CR200 proxy server/

match hp-problemdiagnostics m|^<\?xml version=\"1\.0\" encoding=\"UTF-8\"\?>\n<NETPATH_PROBE version=\"([\w._-]+)\">\n\t<SOURCE device_type=\"HOST\">\n\t\t<DNS>([\w._-]+)</DNS>\n\t\t<IP_OUT>([\d.]+)</IP_OUT>\n\t</SOURCE>\n\t<DESTINATION name=\"\" arguments=\"\">\n\t\t<ERROR code=\"3\">\n\t\t\t<MESSAGE>No destination specified</MESSAGE>\n\t\t</ERROR>\n\t</DESTINATION>\n</NETPATH_PROBE>\n\n$| p/HP Problem Diagnostics/

# slident 0.0.19
match ident m|^0, 0: ERROR: UNKNOWN-ERROR\n$| p/slident/
# mlidentd 1.1 on Linux
match ident m|^0,0:ERROR:UNKNOWN-ERROR\r\n$| p/mlidentd/
# This identd might be BSD derived:
match ident m|^2 , 0 : ERROR : UNKNOWN-ERROR\r\n$|
match ident m|^0 , 0 : ERROR : UNKNOWN-ERROR\r\n$|
# FreeBSD 4.8-RC inetd internal identd
match ident m|^0 , 0 : ERROR : INVALID-PORT\r\n$| p/FreeBSD identd/ o/FreeBSD/
# pidentd-3.1a19-157
match ident m|^ : ERROR : UNKNOWN-ERROR\r\n$| p/pidentd/
match ident m|^0, 0 : ERROR : X-INVALID-REQUEST\r\n$| p/Minidentd or fakeidentd/
# http://packages.debian.org/unstable/net/ident2.html
match ident m|^0 , 0 : ERROR : INVALID-PORT\r\n0 , 0 : ERROR : INVALID-PORT\r\n$| p/Ident2/
# midentd 2.3.1 on Linux
match ident m|^0, 0 : ERROR : INVALID-PORT\r\n| p/midentd/
#midentd 2.1 on Linux 2.4.21
match ident m|^0,0 : ERROR : INVALID-PORT\r\n| p/midentd/
# authd 1.4.3 on Linux
match ident m|^0 , 0 : ERROR :INVALID-PORT\r\n| p/authd/
match ident m|^: USERID : UNIX : CacheFlow Server\r\n| p/CacheFlow identd/ o/CacheOS/
match ident m|^:USERID:OTHER:\d+-ident-is-a-completely-pointless-protocol-that-offers-no-security-or-traceability-at-all-so-take-this-and-log-it!\r\n| p/Fake identd/
match ident m|^ : USERID : UNIX : ([-\w_]+)$| p/Klient identd/ i/IRC Nick $1/
match ident m|^\r\n: ERROR : HIDDEN-USER\r\n$| p/Borderware Firewall identd/ d/firewall/
match ident m|^ : USERID : UNIX : [a-z]{4,8}\r\n$| o/Windows/
match ident m|^1 , 1 : USERID : OTHER : chuck-the-bsd-deamon\r\n$| p/widentd/
match ident m|^,  : USERID : UNIX : [^\r\n]+\r\n$| p/FTPRush FTP client identd/ o/Windows/
match ident m|^0 , 0 : ERROR : FORMAT-ERROR\r\n$| p/GTA GB-Ware firewall identd/ d/firewall/
match ident m|^,  : USERID : UNIX : ([-\w_]+)\r\n,  : USERID : UNIX : ([-\w_]+)\r\n$| p/Snak IRC client identd/

match imap m|^\* OK IMAP4 1\.0 server ready\r\n\* BAD Argument\r\n| p/Cisco VPN Concentrator 3000-series imapd/ d/terminal server/

match imond m|^ERR password required\r\nERR password required\r\n| p/imond fli4l router config/ d/router/
match imond m|^ERR administrator password required\r\nERR administrator password required\r\n$| p/imond fli4l router config/ d/router/
match imond m|^ERR\r\nERR\r\n$| p/imond fli4l router config/ d/router/

# Broken inetd configuration
# <27>Dec 19 17:37:37 inetd\[28433\]: execv /usr/openv/netbackup/bin/bpjava-msvc: No such file or directory
match inetd m|^<\d+>[A-Z][a-z][a-z] +\d+ \d+:\d+:\d+ inetd\[\d+\]: execv (/[-.\\/\w]+): (\w[\s\w.,-]+)$| p/inetd/ i/failed to exec $1: $2/

match ipmi-rmcp m|^\0\0\0\x02\t\0\0\0\x01\0\0\0\0\0\0\0\0$| p/SuperMicro IPMI RMCP/

# Diverse IRC bot
match ircbot m|^ \r\nSorry, that nickname format is invalid\.\r\r\n$| p/Diverse IRC bot/

match irc m|^:([-\w_.]+) 421 \r\n\r\n :\r\n\r\n unimplemented protocol request\r\n:[-\w_.]+ 421 \r\n\r\n :\r\n\r\n unimplemented protocol request\r\n| p/Crackalaka ircd/ h/$1/

match irc-proxy m|^\+OK \r\n-ERR XXX authorization first\r\n$| p/muh irc proxy/

match irr m|^% No search key specified\n\n| p/Merit Internet Routing Registry/

match istat m|^<\?xml version=\"1\.0\" encoding=\"UTF-8\"\?><isr athrej=\"1\"></isr>$| p/istatd server for iStat iPhone app/

match kerberos-sec m%^\x00\x00\x00.~.0.\xa0\x03\x02\x01\x05\xa1\x03\x02\x01\x1e\xa4\x11\x18\x0f(\d\d\d\d)(\d\d)(\d\d)(\d\d)(\d\d)(\d\d)Z\xa5[\x03-\x05]\x02(?:\x03...|\x02..|\x01.)\xa6\x03\x02\x01=\xa9.\x1b.([\w._-]+)\xaa%s p/MIT Kerberos/ h/$7/ i/server time: $1-$2-$3 $4:$5:$6Z/

match laserfiche m|^HLO 0 0 \. 0 71\r\nContent-type: application/vnd\.laserfiche\.lrnp\r\n\r\nLRNP/1\.1\r\n\r\nlistener\r\nEND\r\nERR 0 1 \. 71 80\r\nContent-type: application/vnd\.laserfiche\.lrnp\r\n\r\n451 0 Invalid message \(-2001\)\r\nEND\r\nMSG 0 2 \. 151 58\r\nContent-type: application/vnd\.laserfiche\.lrnp\r\n\r\nCLOSE 0\r\nEND\r\n$| p/Laserfiche document service/

match lastfm m|^ERROR: Command doesn't seem to be followed by a space followed by arguments\n$| p/Last.fm client/
match lexlm m|^.\x08\0\0|s p/Lexmark language monitor/

# Part of Linux net-snmp-5.0.6-17
match linuxconf m|^500 access denied: Check networking/linuxconf network access\r\n$| p/Linuxconf/ i/Access denied/ o/Linux/
# Linuxconf 1.26r4
match linuxconf m|^500 access denied: Check config/networking/misc/linuxconf network access\r\n<p>\r\nBy default,| p/Linuxconf/ i/Access denied/

match loglogic m|^\x02\x02$| p/LogLogic protocol/ d/security-misc/

match memcache m|^ERROR\r\nERROR\r\n$| p/memcached/

match netbios-ssn m|^\x82\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0$| p/Nepenthes fake honeypot netbios-ssn/

# Netsaint Status Daemon 2.15
match netsaint m|^Unknown command\n$| p/Netsaint Status Daemon/
match netsaint m|^ERROR No function requested from client\.| p/Nagios Statd Server/
match netsaint m|^ERROR: Unknown request number\.| p/NC_Net nagios server/

# NSClient - http://nsclient.ready2run.nl/
match nsclient m|^ERROR:Wrong password$| p/Netsaint Windows Client/
match nsclient m|^ERROR: Invalid password\.\nERROR: Invalid password\.\n$| p/NSClient++/

match omniback m|^HP OpenView OmniBack II ([-.\w]+): INET, | p/HP OpenView OmniBack/ v/$1/

match oracle-db-rmi m|^\0\0\xfa\xda\0\x02$| p/Oracle Database Lite RMI/

match paromed m|^PCS-[\w._-]+,V([\w._-]+),OK\nERROR:102: ENERROR:102: EN| p/Paromed milling machine/ v/$1/ d/specialized/

# torque, Tera-scale Open-source Resource and QUEue manager (PBS)
# http://supercluster.org/torque
# maui, http://supercluster.org/maui
match pbs-maui m|^\+2\+15\+15056\+\d+\+\d+| p|PBS/Maui Roll| i/Rocks Cluster/ d/specialized/

match peercast m|^OK2\r\nicy-caps:\d+\r\n\r\nOK\r\n$| p/Peercast/
# Mercury/32 3.32 PH Server module on Windows XP
match ph-addressbook m|^598::Command not recognized\.\r\n598::Command not recognized\.\r\n$| p|Mercury/32 PH addressbook server| o|Windows|

match pop3 m|^\+OK POP3 ([-.+\w]+) v(\d[-.\w]+) server ready\r\n| p/ipop3d/ h/$1/ v/$2/
match pop3 m|^\+OK POP3 \[([-.+\w]+)\] (\d[-.\w]+) server ready\r\n| p/ipop3d/ h/$1/ v/$2/
# iopd 2003debian0.0304182231-1
match pop3 m|^\+OK POP3 \[([-.\w]+)\] v(200[-.\w]+) server ready\r\n-ERR Null command\r\n-ERR Null command\r\n| p/ipopd/ h/$1/ v/$2/
# Solid POP3d 0.15
match pop3 m|^\+OK Solid POP3 server ready\r\n-ERR unknown command\r\n-ERR unknown command\r\n$| p/Solid POP3d/
# OS 400 V4R4M0
match pop3 m|^\+OK POP3 server ready\r\n-ERR invalid command\r\n$| p/IBM OS 400 pop3d/ o|OS/400|
# mailgate v3.5.177 on Win2K
match pop3 m|^\+OK pop server ready\r\n$| p/MailGate pop3d/ o/Windows/
match pop3 m|^\+OK POP3 server ready <[-\w]+>\r\n-ERR Invalid command\r\n$| p/SmarterMail pop3d/ o/Windows/
match pop3 m|^\+OK POP3\r\n-ERR Invalid command in current state\.\r\n| p/hMailServer pop3d/ o/Windows/
match pop3 m|^\+OK ([\w._-]+) Welcome\r\n-ERR Invalid command \(\) \(\) p1=\(\)\r\n-ERR Invalid command \(\) \(\) p1=\(\)\r\n| p/SurgeMail pop3d/ h/$1/
match pop3 m|^-ERR Invalid command\.\r\n-ERR Invalid command\.\r\n| p/cPanel Courier pop3d/
match pop3 m|^\+OK POP3 ready\r\n-ERR invalid command\r\n| p/Zimbra Collabration Suite pop3d/
match pop3 m|^\+OK DavMail POP ready at [^\r\n]*\r\n-ERR unknown command\r\n-ERR unknown command\r\n| p/DavMail pop3d/

match pop3 m|^\+OK [^\r\n]*\r\n-ERR Unknown command\.\r\n-ERR Unknown command\.\r\n| p/Dovecot pop3d/

# Perdition
match pop3-proxy m|^\+OK POP3 Ready ([-\w_.]+) \w+\r\n-ERR Null command, mate\r\n| p/Perdition pop3 proxy/ h/$1/
match pop3-proxy m|^\+OK POP3Proxy ready\r\n-ERR Unknown command\r\n-ERR Unknown command\r\n| p/Astaro firewall pop3 proxy/ d/firewall/

# Postgres 7.1.3
match postgresql m|^EInvalid packet length\0$| p/PostgreSQL DB/
# postgresql-7.2.3-5.73; linux 2.4.20-18.7 redhat 7.3
match postgresql m|^EFATAL 1:  invalid length of startup packet\n\0| p/PostgreSQL DB/
match postgresql m|^EFATAL:  ung\xfcltige L\xe4nge des Startpakets\n\0| p/PostgreSQL DB/ i/German/

match priv-print m|^\xc0\0\x12Data field missing$| p/AXIS 560 print server/ d/print server/

# Postfix qmqpd on Linux 2.4
match qmqp m|^58:Dnetstring format error while receiving QMQP packet header,$| p/Postfix qmqpd/ i/Quick Mail Queueing Protocol/

match realport m|^\xff\x17Access to unopened port.$|s p/Digi EtherLite 32 RealPort/ d/terminal server/
# Ximian Red Carpet Daemon 1.4.4 on RedHat Linux 9.0
match redcarpet m|^Status: 400 Bad Request\r\nContent-Length: 0\r\n\r\n| p/Ximian Red Carpet Daemon/

match rsa-authmgr m|^-ERR Invalid command: \r\n-ERR Invalid command: \r\n| p/RSA Authentication Manager node manager/

match s2-emerge m|^resolutions=\"4CIF\",\"2CIF\",\"CIF\",\"QCIF\"&mpeg_enabled=\"TRUE\"&jpeg_enabled=\"TRUE\"&alarms=\d+&relays=\d+&audio_in\[\]=0x3,0x0&audio_out=\[\]0x3,0x0\0{375,}| p/S2 eMerge Door Access Controller/

match sdcomm m|^ERR 27$| p/RSA SecureID Ace Server/

match seagull-lm m|^\xf1\xf8\xf2\xf6\xf3\xf3\xf0\xf0\xf3\xf8\xf7\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xe2\xf6\xf5\xf6\xf9\xc5\xf9\xc3\0\xf0\xf0\xf3\xf1\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0\xf0$| p/BlueZone Seagull license manager/ o/Windows/

match shell m|^bash: line 1: \r: command not found\nbash: line 2: \r: command not found\n| p/Bash shell/ i/**BACKDOOR**/

match smtp m|^220 ([\w._-]+) ESMTP ready\r\n500 5\.5\.1 Command unrecognized\r\n500 5\.5\.1 Command unrecognized\r\n| p/Kerio MailServer smtpd/ h/$1/
match smtp m|^220 ([\w._-]+) ESMTP I2PNet Mailservice\r\n500 5\.5\.2 Error: bad syntax\r\n500 5\.5\.2 Error: bad syntax\r\n| p/I2P smtpd/

# Hopefully obsoleted by the SOCKS probes -Doug
#match socks m|^\0\[\r\n...\0$| p/Socks4/
#match socks m|^\x05\x01\0.\0\0\0\0\0\0$| p/Socks5/

match solfe m|^\x02\0\x01\xfb\xff\xfb\xff\xff\xff\xff\xffNOSUP| p/HP PNM Solid FlowEngine/

match softros-im m|^none\r\n$| p/Softros LAN Messenger instant messaging/

match spamassassin m|^SPAMD/1\.0 76 Bad header line: \r\n| p/SpamAssassin spamd/

match stargazer m|^ERHD$| p/Stargazer Billing System/

# Giving some problems:
#match stickynote m|^\x01\0\0\0$| p/StickyNote windows freeware/ o/Windows/

match sstp m|^SSTP/([\d.]+) 400 Bad Request\r\n\r\n\0$| p/Sakura Script Transfer Protocol/ i/Protocol $1/

match smux m|^A\x01\x02$| p/Linux SNMP multiplexer/ o/Linux/

match sphereicall m|^\x01\0\0\0z\0\0\x003,DBServer,\d+,Restarts,\d+,\d+,UpTime,\d+,\d+,MediaServer| p/Sphericall DBServer MediaServer VoIP/

match telemecanique m|^220 Service ready on ([\w._-]+) system Version:([\w._:-]+) Subsystem:([\w._:-]+)\r\n500 Unsupported command\r\n| p/Telemecanique Magelis XBTGT 7340 industrial control/ d/specialized/ v/$2/ i/Subsystem $3; Name $1/

# This could go into the null probe, but the problem is that it is a prefix
# of what other routers (at least HP JetDirect printer telentd) send.
# And at least the JD sends the string below first, before it send the
# rest in other packets.  So it is best to capture this one here in
# GenericLines.
# Removed because of too many conflicts!
#match telnet m|^\xff\xfb\x03\xff\xfb\x01$| p/Nokia M1112 router telnetd/ d/router/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\nUser:\r\n\r\nUser:\r\n\r\nUser:| p/Dell PowerConnect M6220-series switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\r\nUsername:\r\r\nError: Username must be non-NULL\r\r\nUsername:\r\r\nError: Username must be non-NULL\r\r\nUsername:| p/Enterasys 1H582-25 switch telnetd/ d/switch/

match tor-control m|^514 Authentication required\.\r\n$| p/Tor control port/ i/Authentication required/

# Solaris 9
match uucp m|^login: Please enter user name: Password: $| p/Solaris uucpd/ o/Solaris/
# SunOS 4
match uucp m|^login: Password: Login incorrect\.$| p/SunOS uucpd/ o/SunOS/
match uucp m|^login: login: login: $| p/NetBSD uucpd/ o/NetBSD/
match uucp m|^login: uucpd: \d+-\d+ The user is not known\.\n| p/AIX uucpd/ o/AIX/

match ups m|^32\r $| p/Cyber Power PowerPanelPlus UPS Server/ o/Windows/

match whois m|^Process query: ''\nQuery recognized as IP(v4)?\.\nQuerying ([\w\d_.-]+):(\d+) with whois\.\n\n| p/gwhois/ i/Uses $2:$3/
match whois m|^Process query: ''\nQuery recognized as IP\.\n| p/gwhois/
match whois m|^%rwhois V-[\w:.-]+ ([-\w_.]+) \(by Network Solutions, Inc\. V-([\d.]+)\)\n| p/rwhois/ v/$2/ h/$1/
match whois m|^Query may not be an empty string\n| p/Public Interest Registry whois server/
match whois m|^WHOIS LIMIT EXCEEDED - SEE WWW\.PIR\.ORG/WHOIS FOR DETAILS\n| p/Public Interest Registry whois server/
match whois m%^ -{62}\n \| UNINET WHOIS Server {40}\|\n \| Created by i-DNS\.net\t\t\t\t\t      \|\n.* INFO: This domain name has not been registered\.\n%s p/Uninet whois/

match irr m|^%  No entries found for the selected source\(s\)\.\n$| p/Merit Internet Routing Registry whoisd/

match wincomm m|^128 System Incompatible Windows Communicator client or server version\r\n128 System Incompatible Windows Communicator client or server version\r\n| p/Windows Communicator/
match zebedee m|^\x02\x01$| p/Zebedee encrypted tunnel/

match bmc-perform-service m|^SDPACK$| p/BMC Perform Service Daemon/
# Grisoft AVG antivirus server (distributing virus database updates)

match nntp m|^200 Coruscant BBS News \(Synchronet NNTP Service v(\d[-.\w ]+)\)\r\n| p/Synchronet NNTP Service/ v/$1/

match telnet m|^\xff\xfb\x01\n\rSSH service name not present in rcvd msg\n\rSSH Session task 0x\w+: Version Exchange Failed\n\r\n\r\n\rSSH service name not present in rcvd msg\n\r| p/Cisco 350 Series AP telnetd/ d/router/
match telnet m|^\xff\xfe\"\xff\xfb\x01\xff\xfb\x03User : \r\n\r?SpeedTouch \(([-\w]+)\)\r\n\r?Password : Invalid Password\r\n\r?Closing connection\r\n| p/Alcatel SpeedTouch DSL router/ i/MAC $1/ d/router/
match telnet m|^\xff\xfe\x01\xff\xfd\x03\xff\xfd\x18\xff\xfd\x1f\xff\xfb\x03\xff\xfb\x01\r\nAccount Name: \r\nPassword: \r\nThis copy of the Ataman Telnetd Server is registered as licensed to:\r\n\t(.+)\r\n\r\nLogin failed: unknown user name, password or privilege incorrect\.\r\n| p/Ataman telnetd/ i/Registerd to $1/ o/Windows/
match telnet m|^Password:\xff\xfb\x01\n\rTry again, you polio:\n\n\rTry again, you polio:\n| p/VLC Player telnetd/
match telnet m=^\xff\xfb\x01\xff\xfb\x03\r\n\r\n\r\n +-+\r\n +\| Cyclades-PR4000: CyROS  V_([\d.]+)  \(.*\)     \|\r\n= p/Cyclades PR4000 router telnetd/ d/router/
# Billion 741GE or D-Link DSL2-300G
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\n\r\nLogin: \r\n\r\nYou must supply a username\r\n\r\nLogin: \r\n\r\nYou must supply a username\r\n\r\nLogin: | p/Billion or D-Link ADSL router telnetd/ d/router/
# Not sure if this is really a telnet service but many people reported it running on port23:
match telnet m|^\xff\xfb\x01$| p/SMC SMC2870W Wireless Ethernet Bridge/ d/bridge/
match telnet m|^\r\n\r\nThis is a FirstClass system, from Open Text Corporation\.\r\n\r\n\r\nFirstClass is an e-mail and conferencing system with a graphical user interface\.\r\n\r\n\r\nThe Command Line Interface is not available on this sy| p/FirstClass telnetd/ i/CLI disabled/
match telnet m|^\xff\xfb\x01\r\nPassword:\r\nLogged in as guest\r\n| p/Linkstar Comsat router telnetd/ d/router/
match telnet m|^\xff\xfb\x01Login: \r\nLogin: \r\nLogin: | p/Lingo VoIP config telnetd/ d/VoIP adapter/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x18\xff\xfd\x1f\r\nuser: \r\npassword: \r\n\r\nuser: | p/KIRK Wireless Server 600 telnetd/ d/VoIP adapter/
match telnet m|^\xff\xfb\x01\n\r-> \n\r-> \n\r-> | p/Coresma Phazer Docsis USB cable modem telnetd/ d/broadband router/
match telnet m|^bad password\r\n$| p/Cybersitter CLI/
match telnet m|^\xff\xfd\"\xff\xfb\x01SSE version ([\d.]+)\r\nCopyright [\d, ]+ by Motorola\r\nUsername:| p/Motorola Canopy telnetd/ i/SSE $1/ d/telecom-misc/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\n\r\n\[ORiNOCO-AP-[-\w]+\]> Please enter password: \r\nIncorrect Password\r\n\r\n\[ORiNOCO-AP-[-\w]+\]> Please enter password: \r\n| p/ORiNOCO wireless router telnetd/ d/router/
match telnet m|^\xff\xfb\x01Password\? \r\n500 Configuration error\. Disconnecting!\n| p/Tru64 UNIX gated/ o/Tru64 UNIX/
match telnet m|^\xff\xfb\x01\r\n\r\nlogin: \r\n\r\n\r\r\npassword: $| p/Welltech Wellgate VoIP adapter telnetd/ d/VoIP adapter/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\xff\xfb\x1f\xff\xfd\x18Avocent CPS-810 S/W Version ([\d.]+)\r\nUsername: \r\nPassword: \r\nInvalid Login\r\nUsername: | p/Avocent CPS-810 serial port server telnetd/ v/$1/ d/specialized/

match telnet m|^\xff\xfb\x01\xff\xfb\x03\nGestetner Maintenance Shell\.   \n\rUser access verification\.\n\rPassword:| p/Gestetner DSm622 maintenance telnetd/ d/printer/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\nNRG Maintenance Shell\.   \n\rUser access verification\.\n\rPassword:| p/NRG maintenance telnetd/ d/printer/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\nRICOH Maintenance Shell\.   \n\rUser access verification\.\n\r| p/Ricoh maintenance telnetd/ d/printer/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\nRICOH Maintenance Shell\.   ([\w:]+)\n\rUser access verification\.\n\rPassword:| p/Ricoh maintenance telnetd/ i/MAC $1/ d/print server/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\nSAVIN Maintenance Shell\.   \n\rUser access verification\.\n\r| p/SAVIN printer telnetd/ d/printer/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\nTOSHIBA Maintenance Shell\.   \n\rUser access verification\.\n\rlogin:| p/Toshiba print server telnetd/ d/print server/

match telnet m|^\r\nPress return:\*\*\*\*\r\nEnter Password:| p/IPSentry telnetd/ o/Windows/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x03\r\0\n\r\0\n\r\0\n\r\0\n- NetQue AppleTalk/NetWare/TCP/LAT Printer Server| p/EMULEX NetQue print server telnetd/ d/print server/
match telnet m|^\r\n\r\nUser Access Verification\r\n\r\nPassword: \r\nPassword: \r\nPassword: \r\n% Bad passwords\r\n| p/Cisco telnetd/ d/router/ o/IOS/
match telnet m|^\xff\xfb\x01\xff\xfe\"\xff\xfe\0\xff\xfd\x03\xff\xfd\x18\xff\xfd\x1f\r\n\r\n\r\nlogin: | p/freeSSHd telnetd/ o/Windows/
match telnet m|^\xff\xfb\x01\x1b\[7l\x1b\[\?1l\x1b\[0m\x1b\[2JUsername: \x1b\[7l\x1b| p/CyberSwitching Dualcom power device rabbit 2000 embedded telnetd/ d/power-device/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\nRead /disclaimer\.txt and have fun with yadi on your Nokia D-BOX2 - Kernel ([-\w_.]+) \(| p/Nokia D-BOX2 telnetd/ o/Linux/ i/Linux kernel $1/ d/media device/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\nPhilips D-BOX2 - Kernel ([\w._-]+) \(| p/Philips D-BOX2 telnetd/ o/Linux/ i/Linux kernel $1/ d/media device/
match telnet m|^\xff\xfb\x01\n\rLogin: \n\r\n\r\n\rLogin: \n\rLogin: | p/Nortel Extranet Contivity Secure IP Services telnetd/ d/security-misc/
match telnet m|^\xff\xfd\x01\xff\xfd\x1f\xff\xfd!\xff\xfb\x01\xff\xfb\x03\r\r\n\r\n\rlogin: \r\n\r\nLogin incorrect\r\n\r\nlogin: | p/Cisco Intrusion Prevention System telnetd/ o/IOS/ d/security-misc/
match telnet m|^ 105 Access denied\.\r\n 105 Access denied\.\r\n 105 Access denied\.\r\n 105 Access denied\.\r\n| p/ShroudBNC telnet config/
match telnet m|^User Name: \r\r\nPassword: \r\r\nRemote MAC address: | p/Airaya WAP diagnostics telnetd/ d/WAP/
match telnet m|^\xff\xfb\x01\r\nAP11G login: \r\n\r\nPassword: | p/OfficeConnect AP11G WAP telnetd/ d/WAP/
match telnet m|^\xff\xfb\x01\xff\xfb\x03Welcome to the Windows CE Telnet service on ([-\w_.]+)\r\n\r\nlogin: \n\r\nPassword:| p/Windows CE telnetd/ o/Windows/ h/$1/
match telnet m|^\xff\xfb\x01\xff\xfd\x03\xff\xfb\x03\x1b\[2J\x1b\[H \n\r\0\x1b\[H\x1b\[JPASSaPORT CS-(\d+)  SW V([-\w_.]+) , HW V([-\w_.]+)\r\n\r\n| p/RADLINX PASSaPORT CS terminal server telnetd/ i/$1 ports; SW $2; HW $3/ d/terminal server/
match telnet m|^\xff\xfb\x01\r\nlogin: \r\npassword: \r\nLogin incorrect!\r\n$| p/Netgear GS108T switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\xff\xfd\x01\xff\xfe\x01\xff\xfd\x03\xff\xfb\x03\*+\r\n\r\nThis session allows you to set the TCPIP parameters for your\r\nLexmark (\w+) Ethernet internal network device, with a hardware\r\naddress of (\w+) (\w+) | p/Lexmark $1 printer telnetd/ i/MAC $2; MAC2 $3/ d/printer/
match telnet m|^\*+\r\n\r\nThis session allows you to set the TCPIP parameters for your\r\nLexmark (\w+) Ethernet internal network device, with a hardware\r\naddress of (\w+) (\w+) | p/Lexmark $1 printer telnetd/ i/MAC $2; MAC2 $3/ d/printer/
match telnet m|^\*+\r\n\r\nThis session allows you to set the TCPIP parameters for your\r\nLexmark Optra LaserPrinter internal network device, \r\nwith a hardware address of (\w+)     (\w+)\r\n| p/Lexmark Optra LaserPrinter telnetd/ d/printer/ i/MAC $1; MAC2 $2/
match telnet m|^\xff\xfb\x01\xff\xfd\x01\xff\xfe\x01\xff\xfd\x03\xff\xfb\x03\*{60}\r\n\r\nThis session allows you to set the TCPIP parameters for your\r\nIBM Infoprint (\d+) Ethernet internal network device, with a hardware\r\naddress of((?: [0-9A-F]{12})+) \(MSB, Canonical\)\.\r\nIt's an ethernet card\.\r\n\r\n\*{60}\r\n\r\n| p/IBM Infoprint $1 printer/ i/MAC addresses:$2/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfb\x1fError2 negotiated with client \d+ and get 1 char is a a d\. \n\r\n\r\*+\n\r\*\* +\*\*\n\r\*\* IP Phone firmware +V([\w._-]+) | p/Thomson VoIP phone telnetd/ v/$1/ d/VoIP phone/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\xff\xfb\x01\xff\xfb\x03\r\nLogin: \r\r\nPassword: \r\r\n\r\r\nLogin failed\r\r\n\r\r\nLogin: | p/Siemens SANTIS WAP telnetd/ d/WAP/
match telnet m|^Password: \xff\xfb\x01\r\nWrong password\.\r\nPassword: \r\nWrong password\.\r\nPassword: | p/VLC media player telnetd/
match telnet m|^\xff\xfb\x01\xff\xfd\x01\xff\xfe\x01\xff\xfd WxGoos-(\d+) v([\w._-]+) | p/WxGoos-$1 Climate Monitor telnetd/ v/$2/ d/specialized/
match telnet m|^\xff\xfd\0\xff\xfd\x03\xff\xfb\0\xff\xfb\x03\xff\xfb\x01\x03\x04\r\nPassword: \r\n\n\rComtrol DeviceMaster RTS   ModelID: (\d+) \n\r\rNS-Link ([\w._-]+) \n\rBuilt: .*\n\rIP Addr: [\d.]+  Mask: [\d.]+ Gateway: [\d.]+ \n\rMAC Addr: ([\w ]+) \n\r\n\r\r\n\rdm> \r\nInvalid Command\r\n\rdm>| p/Comtrol DeviceMaster RTS ethernet to serial telnetd/ d/specialized/ i/Model $1; NS-Link $2; MAC $3/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\xff\xfd\x01\xff\xfd\x18\r\0\r\nPassword: \r\nPassword incorrect\r\n| p/Sun StorEdge 3511 telnetd/ d/storage-misc/
match telnet m|^\xff\xfd\x01\xff\xfd!\xff\xfb\x01\xff\xfb\x03AH4222\r\nLogin: \r\n\r\nPassword: | p/Club-Internet telnetd/ d/broadband router/
match telnet m|^\xff\xfe\x01\xff\xfb\x01\xff\xfc\"\xff\xfd\x1flogin: \r\nlogin: \r\nlogin: | p/GigaVUE-420 switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\xff\xfe\x01-> \n\r-> \n\r-> | p/ser2net telnetd/
match telnet m|^\x1b\[24;1HUsername: \x1b\[\?25h\x1b\[24;1H\x1b\[\?25h\x1b\[24;11H\x1b\[24;11H\x1b\[\?25h\x1b\[24;11H\x1b\[24;1H\r\n\r\x1b\[\?25h\x1b\[24;11H\xff\xfd\x18\xff\xfb\x01\x1b\[2J\x1b\[\?7l\x1b\[3;23r\x1b\[\?6l\x1b\[1;1H\x1b\[\?25l\x1b\[1;1HProCurve (\w+) Switch (\w+)\r\n\rSoftware revision ([\w.]+)\r\n| p/HP ProCurve Switch $2 telnetd/ v/$3/ i/JetDirect $1/
match telnet m|^\xff\xfb\x01\r\nConfiguration Login: \r\n\r\n\r\nConfiguration Login: \r\nConfiguration Login: $| p/HP E1200 storage telnetd/ d/storage-misc/
match telnet m|^\r\nEnter Password: \r\nInvalid Password\.\r\nEnter Password: \r\nInvalid Password\.\r\nEnter Password: | p/WPI Network Power Switch (remote reboot) telnetd/ d/remote management/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\nWelcome to IFBD-HE05/06 TELNET Utility\.\r\nCopyright\(C\) 2005 Star Micronics co\., Ltd\.\r\n\r\n<< Connected Device >>\r\n    Device Model: (\w+) \(STR_T-001\)\r\n    NIC Product : IFBD-HE05/06\r\n    MAC Address : ([0-9A-F:]+)\r\n\r\n\r \r\nlogin: \r\n| p/Star Micronics $1 printer telnetd/ d/printer/
match telnet m|^\xff\xfb\x01Username: \n\rPassword: \n\rUsername: | p/3Com 8760 WAP telnetd/ d/WAP/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\nLANIER Maintenance Shell\.   \n\rUser access verification\.\n\rlogin:| p/Ricoh Aficio printer telnetd/ d/printer/
match telnet m|^\xff\xfb\x01\r\nUser Name : \r\nUser Name : \r\nUser Name : | p/APC AP9630 network management telnetd/ d/power-device/
match telnet m|^\xff\xfb\x01\xff\xfb\x03\r\n\r\nWelcome to VIP-X ([\w._-]+) from [\w._-]+\r\nTLS invalid record length\r\n\r\n\r\n\r\ninvalid username\r\n\r\nTLS version 0300 not supported\r\nenter username  -> | p/Bosch VIP X1 video encoder telnetd/ d/webcam/ h/$1/

match transbase m|^\0\0\+\x04\0\0\0@TransBase Multiplexer error report:\nIllegal request| p/Transbase Database/

# MiniUPnP
match upnp m|^ 501 Not Implemented\r\n.*Server: Tomato UPnP/([\w.]+) MiniUPnPd/([\w.]+)\r\n|s p/MiniUPnP/ v/$2/ o/Linux/ i/Tomato firmware; UPnP $1/
match upnp m|^ 501 Not Implemented\r\n.*Server: (RT-\w+) UPnP/([\w.]+) MiniUPnPd/([\w.]+)\r\n|s p/MiniUPnP/ v/$3/ i/Asus $1 WAP; UPnP $2/ d/WAP/
match upnp m|^ 501 Not Implemented\r\n.*Server: DrayTek/Vigor([\w._-]+) UPnP/([\w.]+) miniupnpd/([\w.]+)\r\n|s p/MiniUPnP/ v/$3/ i/DrayTek Vigor $1 router; UPnP $2/ d/router/
match upnp m|^ 501 Not Implemented\r\n.*Server: OpenWRT/kamikaze UPnP/([\w._-]+) MiniUPnPd/([\w._-]+)\r\n|s p/MiniUPnP/ v/$2/ i/OpenWrt Kamikaze; UPnP $1/ d/WAP/ o/Linux/

# MiniDLNA
match upnp m|^HTTP/1\.1 501 Not Implemented\r\nContent-Type: text/html\r\nConnection: close\r\nContent-Length: 149\r\n\r\n<HTML><HEAD><TITLE>501 Not Implemented</TITLE></HEAD><BODY><H1>Not Implemented</H1>The HTTP Method is not implemented by this server\.</BODY></HTML>\r\n| p/MiniDLNA/
match upnp m|^HTTP/1\.1 501 Not Implemented\r\nContent-Type: text/html\r\nConnection: close\r\nContent-Length: 149\r\nServer: Fedora/([\w._-]+) DLNADOC/([\w._-]+) UPnP/([\w._-]+) MiniDLNA/([\w._-]+)\r\n| p/MiniDLNA/ v/$4/ i/Fedora $1; DLNADOC $2; UPnP $3/ o/Linux/
match upnp m|^HTTP/1\.1 501 Not Implemented\r\nContent-Type: text/html\r\nConnection: close\r\nContent-Length: 149\r\nServer: RAIDiator/([\w._-]+) DLNADOC/([\w._-]+) UPnP/([\w._-]+) MiniDLNA/([\w._-]+)\r\n| p/MiniDLNA/ v/$4/ i/RAIDiator $1; DLNADOC $2; UPnP $3/ o/Linux/

match upnp m|^HTTP/1\.1 501 Not Implemented\r\nConnection: close\r\nContent-type: text/html\r\n\r\n<HTML><HEAD><TITLE>501 Not Implemented</TITLE></HEAD><BODY><H1>Not Implemented</H1>The HTTP Method is not implemented by this server\.</BODY></HTML>\r\n$| p/MiniUPnP/
match upnp m|^ 501 Not Implemented\r\n.*Server: Linux Mips ([\w._-]+) UPnP/([\w.]+) MiniUPnPd/([\w.]+)\r\n|s p/MiniUPnP/ v/$3/ o/Linux/ i/Linux $1 (MIPS); UPnP $2/
match upnp m|^ 501 Not Implemented\r\n.*Server: SmoothWall Express/([\w._-]+) UPnP/([\w.]+) miniupnpd/([\w.]+)\r\n|s p/MiniUPnP/ v/$3/ o/Linux/ i/SmoothWall Express $1; UPnP $2/
match upnp m|^HTTP/1\.1 400 Bad Request\r\nDATE: .*\r\nConnection: Keep-Alive\r\nServer: UPnP/([\d.]+)\r\nContent-Length: 0\r\nContent-Type: text/xml; charset=\"utf-8\"\r\nEXT:\r\n\r\n$| p/UPnP/ v/$1/ d/broadband router/
match upnp m|^HTTP/1\.1 \d\d\d .*\r\nServer: *Linux/([-\w_.]+), UPnP/([-\w_.]+), TwonkyVision UPnP SDK/([-\w_.]+)\r\n|s p/TwonkyMedia UPnP/ i/Linux $1; UPnP $2; SDK $3/ o/Linux/
match upnp m|^HTTP/1\.1 400 Bad request\r\nServer: Reciva UPnP/([\w._-]+) Radio/([\w._-]+) DLNADOC/([\w._-]+)\r\nContent-length: 0\r\nConnection: close\r\n\r\n$| p/dnt IPdio radio UPnP/ v/$2/ i/UPnP $1; DLNADOC $2/ d/media device/
match upnp m|^HTTP/0\.0 400 Bad Request\r\nServer: ([\w._-]+) \d+/Service Pack (\d+), UPnP/([\d.]+), TVersity Media Server\r\n| p/TVersity Media Server UPnP/ v/$1 SP $2/ o/Windows/ i/UPnP $3/
match upnp m|^HTTP/0\.0 400 Bad Request\r\nServer: ([\w._-]+) 2/, UPnP/([\w._-]+), TVersity Media Server\r\n|s p/TVersity Media Server UPnP/ v/$1/ o/Windows/ i/UPnP $2/
match upnp m|^HTTP/1\.1 \d\d\d .*\r\nDATE: .*\r\nConnection: Keep-Alive\r\nServer: LINUX/([\d.]+) UPnP/([\d.]+) BRCM400/([\d.]+)\r\n| p|Belkin/Linksys wireless router UPnP| i/Linux $1; UPnP $2; BRCM400 $3/ d/router/ o/Linux/
match upnp m|^HTTP/1\.1 400 Bad Request\r\nServer: Symbian/([\w._-]+) UPnP/([\d.]+)\r\nContent-Length: 151\r\n\r\n<!DOCTYPE HTML PUBLIC \"-//IETF//DTD HTML 2\.0//EN\">\n<html><head>\n<title>400 Bad Request</title>\n</head><body>\n<h1>Bad Request</h1>\n<hr />\n</body></html>$| p/Nokia N85 media share/ d/phone/ i/SymbianOS $1; UPnP $2/ o/SymbianOS/

match uptime-agent m|^ERR\n$| p/up.time server monitor/

match remoting m|^\.NET\x01\0\x02\0\0\0\0\0\0\0\x02\0\x03\x01\0\x03\0\x01\x01..\0\0Server encountered an internal error\. To get more info turn on customErrors in the server's config file\.\x05\0\0\0\0| p/MS .NET Remoting services/
match remoting m|^\.NET\x01\0\x02\0\0\0\0\0\0\0\x02\0\x03\x01\0\x03\0\x01\x01..\0\0Le serveur a rencontr\xc3\xa9 une erreur interne\. Pour obtenir plus d'informations, activez customErrors dans le fichier de configuration du serveur\.\x05\0\0\0\0| p/MS .NET Remoting services/ i/French/
match remoting m|^\.NET\x01\0\x02\0\0\0\0\0\0\0\x02\0\x03\x01\0\x03\0\x01\x01..\0\0System\.Runtime\.Remoting\.RemotingException: Tcp channel protocol violation: expecting preamble\.\r\n|s p/MS .NET Remoting services/
match remoting m|^\.NET\x01\0\x02\0\0\0\0\0\0\0\x02\0\x03\x01\0\x03\0\x01\x01..\0\0System\.Runtime\.Remoting\.RemotingException: Violation de protocole de canal tcp\xc2\xa0: pr\xc3\xa9ambule attendu\.\r\n|s p/MS .NET Remoting services/ i/French/

match spy-net m%^tentarnovamente\|\r\ntentarnovamente\|\r\n% p/Spy-Net or CyberGate backdoor/ i/**BACKDOOR**/

match vnc m|^0\x82\x01\n\x02\x82\x01\x01\0| p/Ultr@VNC/ v/1.0.8.0/ o/Windows/

match bitkeeper m|^ERROR-Try help\nERROR-Try help\n$| p/Bitkeeper/
match webcache m|^HTTP/1\.0 400 Bad Request\r\nExpires: .*\r\nContent-Type: text/html\r\n\r\n<html>\n<head><title>Bad formed request or url</title>\n| p/webcache/
# Novell ZENworks for Desktops Imaging Proxy 4.01.03
# Not sure if this is netware specific (linux too?) -Doug
match zenimaging m|^\xff\xff\xfb&$| p/Novell ZENworks Imaging Proxy/

match ajp12 m|^Status: 400 Bad Request\r\nServlet-Error: Malformed data sent to JServ\r\n\r\n$| p/Apache Jserv/

match nuttcp m|^KO\nnuttcp-t: v([\d.]+): error scanning parameters\nmay be using older client version than server\n\r\nKO\n| p/nuttcp network throughput tester/ v/$1/
match backdoor m|^sh-2\.05b\$ | p/r0nin rootkit backdoor/

match websense-eim m|^\0\x0c\r\n\0\x01\0\x01\0\0\0\0$| p/Websense EIM/

match wesnoth m|^\0\0\0.\0\0\0\x1f\x02version\0\x04[\d.]+\0\0\x02mustlogin\0\x05\x01\0|s p/Battle For Wesnoth game server/ v/$1/
match wesnoth m|^\0\0\0.\0\0\0.\x1f\x8b\x08\0\0\0\0\0\0\xff\x8b\.K-\*\xce\xcc\xcf\x8b\xe5\x8a\xd6\x873\x01 \xbc\x17\x06\x15\0\0\0| p/Battle For Wesnoth game server/

match workrave m|^\0\x26\x02\0\0\x06\0.[\d.]+:\d+\0\x01\0\x11\0\x04\0\x01\0\x03\0\xaa\x02\0\0\x06\0.[\d.]+:\d+\0\x01\0\x10\0\x88\0\x03\0\x0bmicro_pause\0\x20\x4c\xa4\x86\x8e\0\0\0\xb4\0\0\0\x01\0\0\0\0\0\0\0\0L\xa4\x86\x8d\0\0\0\xb4\0\0\0\x0arest_break\0|s p/Workrave/

match wtam m|^WTAM/1\.0 401 Unrecognized Command\n\n$| p/Webtrends WTAM/

match wub-command m|^Command Shell\r\n\r\n% \r\n% | p/Wub httpd command console/

match xboxdebug m|^201- connected\r\n407- unknown command\r\n$| p/Microsoft XBox Debugging Kit/ d/game console/
match xns m|^HELLO XBOX!$| p/Relax XBOX file server/ d/game console/

match zabbix m|^ZBXD\x01\x10\0\0\0\0\0\0\0ZBX_NOTSUPPORTED| p/Zabbix Monitoring System/

match zmodem m|^\*\*\x18B0100000023be50\r\x8a\x11$| p/ZMODEM/

# Know the device, but not the service.
# Port 2000.
# match unknown m|^\x20$| p/Samsung CLX-3175FW printer/ d/printer/


##############################NEXT PROBE##############################
Probe TCP GetRequest q|GET / HTTP/1.0\r\n\r\n|
rarity 1
ports 1,70,79,80-85,88,113,139,143,280,497,505,514,515,540,554,591,620,631,783,888,898,900,901,993,995,1026,1080,1042,1214,1220,1234,1311,1314,1344,1503,1610,1611,1830,1900,2001,2002,2030,2064,2160,2306,2396,2525,2715,2869,3000,3002,3052,3128,3280,3372,3531,3689,3872,4000,4444,4567,4660,4711,5000,5427,5060,5222,5269,5280,5432,5800-5803,5900,6103,6346,6544,6600,6699,6969,7002,7007,7070,7100,7402,7776,8000-8010,8080-8085,8088,8118,8181,8443,8880-8888,9000,9001,9030,9050,9080,9090,9999,10000,10001,10005,11371,13013,13666,13722,14534,15000,17988,18264,31337,40193,50000,55555
sslports 443,4443

match ajp13 m|^AB\0\x13\x04\x01\x90\0\x0bBad Request\0\0\0AB\0\x02\x05\x01$| p/Apache Jserv/

match athinfod m|^athinfod: invalid query\.\n$| p/Athena athinfod/

# Kerio PF 4.0.11 unregistered - Service process (Port 44xxx?) on MS W2K SP4+
match keriopfservice m|^(HTTP/1\.0) 200 OK\r\nServer: Kerio Personal Firewall\r\n| p/Kerio PF 4 Service/ i/$1/

match backupexec-remote m|^\xf6\xff\xff\xff\x10\0\0\0\0\0\0\0\0\0\0\0$| p/Veritas BackupExec Remote Agent/

match backdoor m|^:[-\w_.]+ 451 GET :\r\n| p/**BACKDOOR**/ o/Windows/
match backdoor m|^<HTML>\n<HEAD>\n<TITLE>Directory /</TITLE>\n<BASE HREF=\"file:/\">\n</HEAD>\n<BODY>\n<H1>Directory listing of /</H1>| p/No-auth shell/ i/**BACKDOOR**/ o/Unix/

match bentley-projectwise m|^ACKNOSEC$| p/Bentley Systems ProjectWise/

match bittorrent m|^Nice try\.\.\.\r\n$| p/Transmission Bittorrent client/

match bluecoat-logd m|^\x03\0\0\x01$| p/Blue Coat Reporter log server/

match brio m|^com\.sqribe\.null\0java\.lang\.String\0com\.sqribe\.transformer\.TransformerException\0java\.lang\.String\0TRCP version mismatch: Current version: (\d+) Client version: unknown\0$| p/Brio 8 business intelligence tool/ v/$1/

match caldav m|^HTTP/1\.1 401 Unauthorized\r\n.*WWW-Authenticate: negotiate \r\nWWW-Authenticate: digest nonce=\"\d+\", realm=\"/Search\", algorithm=\"md5\"\r\n.*Server: Twisted/([\w._-]+) TwistedWeb/([\w._-]+)\r\n|s p/TwistedWeb httpd/ v/$2/ i/Apple iCal Server; Twisted $1/

match csta m|^<HTML>\r\n<HEAD>\r\n<TITLE>CSTA-Mono Server Home Page </TITLE>\r\n| p/Alcatel OmniPCX Enterprise/ d/PBX/

match daap m|^HTTP/1\.1 404 Not Found\r\nConnection: close\r\nDate: .*\r\nContent-Length: 24\r\n\r\nCommand not implemented\.$| p/Amarok music player DAAP/
match daap m|^HTTP/1\.1 400 Bad Request\r\nDate: .*\r\nDAAP-Server: iTunes/(\d[-.\w]+) \((.*)\)\r\n| p/Apple iTunes DAAP/ v/$1/ o/$2/
match daap m|^HTTP/1\.1 403 Forbidden\r\nDate: .*\r\nDAAP-Server: iTunes/(\d[-.\w]+) \((.*)\)\r\nContent-Type: application/x-dmap-tagged\r\nContent-Length: 0\r\n\r\n$| p/Apple iTunes DAAP/ v/$1/ o/$2/
match daap m|^HTTP/1\.1 \d\d\d .*\r\nServer: mt-daapd/([-\w.]+)\r\n|s p/mt-daapd DAAP/ v/$1/
match daap m|^HTTP/1\.0 404 Not Found\r\nDate: .*\r\nContent-Length: 0\r\n\r\n$| p/mt-daapd DAAP/
match daap m|^HTTP/1\.1 \d\d\d .*\r\nDAAP-Server: daap-sharp\r\nContent-Type: application/x-dmap-tagged\r\nContent-Length: \d+\r\n\r\ninvalid session id| p/DAAPsharp DAAP/
match daap m|^HTTP/1\.0 400 Bad Request\nServer: Hughes Technologies Embedded Server \(persistent patch\)\r\n| p/daapd/ i/Hughes embedded/

match dnet-keyproxy m|^HTTP/1\.0 302 Found\r\nLocation: http://www\.distributed\.net/\r\n\r\n$| p/Distributed.Net HTTP Keyproxy/

match drda m|^\0\x79\xd0\x02\xff\xff\0\x73\x12\x4c\0\x06\x11\x49\0\x08\0\x4e\x11S\0\xd3| p/IBM DRDA/
match drda m|^\0\x1b\xd0\x02\0\x01\0\x15\x12\x4c\0\x06\x11\x49\0\x08\0\x06\0\x0c\0\0\0\x05\x11\x4a\x03$| p/Apache Derby DRDA/

match emco-remote-screenshot m|^\x06!\x01\0\0\0\0\0\xff\xd8\xff\xe0\0\x10JFIF| p/EMCO Remote Screenshot/

# Digital UNIX 5.6
match finger m|^Login name: /         \t\t\tIn real life: \?\?\?\r\n\r\nLogin name: GET       \t\t\tIn real life: \?\?\?\r\n\r\nLogin name: HTTP/1\.0  \t\t\tIn real life: \?\?\?\r\n$| p/Digital UNIX fingerd/ o/Digital UNIX/
# Internet Rex v2.67 Beta 1a
match finger m|^No such user No such user N\n$| p/Internet Rex finger server/
# IQinVision IQeye3 security camera
match finger m|^\n Nodename:\s+(\w+)\r\n| p/IQinVision fingerd/ i/Camera/ h/$1/ d/webcam/
# FreeBSD 4.9-STABLE /usr/libexec/fingerd/
match finger m|^finger: /: no such user\r?\nfinger: GET: no such user\r?\nfinger: HTTP/1\.0: no such user\r?\n$| p/FreeBSD fingerd/ o/FreeBSD/
# Bay Networks Micro Annex Comm. Server R10.0
match finger m|^No such activity\.\r\n$| p/Bay Networks Micro Annex terminal server fingerd/ d/terminal server/
# Mercury/32 3.32 Finger Server module on Windows XP
match finger m|^GET / HTTP/1\.0 is not known at this site\.\r\n$| p|Mercury/32 fingerd| o|Windows|
# ffingerd 1.28
match finger m|^That user does not want to be fingered\.\n$| p/ffingerd/
# Finger 0.17 from debian linux (which is from Linux netkit I believe)
# OpenBSD 2.3
match finger m|^finger: GET: no such user\.\nfinger: /: no such user\.\nfinger: HTTP/1\.0: no such user\.\n$| p|BSD/Linux fingerd|
# Linux port of in.fingerd from OpenBSD network tools - started with -w to show welcome banner
match finger m|^\r\nWelcome to Linux version (\d[-.\w]+) at ([-.\w]+) !\r\n\n.*\n\r\nfinger: GET: no such user\.|s p/OpenBSD fingerd/ i/ported to Linux; $2 users logged in; Linux version $1/ h/$2/ o/Linux/
# Redhat Linux from finger-server-0.17-9 RPM
match finger m|^finger: GET: no such user.\r\nfinger: /: no such user.\r\nfinger: HTTP/1.0: no such user.\r\n$| p/Linux fingerd/ o/Linux/
# NetBSD 1.6ZA (berkeley fingerd 8.1 sibling)
match finger m|^finger: GET: no such user\nfinger: /: no such user\nfinger: HTTP/1\.0: no such user\n$| p/NetBSD fingerd/
# Solaris 9
match finger m|^Login       Name               TTY         Idle    When    Where\r\nGET                   \?\?\?\r\n/                     \?\?\?\r\nHTTP/1\.0              \?\?\?\r\n$| p/Sun Solaris fingerd/ o/Solaris/
# mlfingerd 1.1
match finger m|^Information for user 'GET\+20\+2F\+20HTTP\+2F1\.0':\r\nUnknown user\.\r\n$| p/mlfingerd/
# SGI IRIX 6.5.18f finger
match finger m|^Login name: GET       \t\t\tIn real life: \?\?\?\r\n$| p/SGI IRIX or NeXTSTEP fingerd/
# Windows fingerd
match finger m|^No such user\n$| p/Windows fingerd/ o/Windows/
match finger m|^MSS100 Version V([\d/.]+)\(\d+\) - Time Since Boot: \d+:\d\d:\d\d\r\nName        pid     stat  pc       cpusec    stack    pr/sy   idle    tty\r\n| p/Lantronix MSS100 serial interface fingerd/ v/$1/ d/specialized/
match finger m|^finger: GET / HTTP/1\.0: no such user\n| p/efingerd/ o/Unix/
match finger m|^ +-;;=\n +\.;M####\+\n| p/mIRC with ircN script fingerd/ o/Windows/
match finger m|^User not found\r\n| p/XMail fingerd/
match finger m|^EMail       : [-\w_.]+@([-\w_.]+)\r\n  Real Name : \?\?\r\n  Home Page : \?\?\r\n| p/XMail fingerd/ h/$1/
match finger m|^\r\nIntegrated port\r\nPrinter Type: IBM Infoprint (.*)\r\n| p/IBM Inforprint $1 fingerd/ d/print server/
match finger m|^Login name: HTTP/1\.0       In real life: \?\?\?\r\n| p/OpenVMS fingerd/ o/OpenVMS/
match finger m|^No information available\r\n$| p/Post.Office fingerd/
match finger m|^finger: sorry, no such user\.\n$| p/xfingerd/

match git m|^0077ERR \n  Your Git client has made an invalid request:\n  GET / HTTP/1\.0\r\n\r\n\n  Visit http://support\.github\.com for help$| p/Git/ i/GitHub/

match gnutella m|^HTTP/1\.[01] 404 Not Found\r\nServer: gtk-gnutella/(\d[-.\w]+) \(([^\)\r\n]+)\)\r\n| p/gtk-gnutella P2P client/ v/$1/ i/$2/
match gnutella m|^HTTP/1\.[01] 403 Browse Host Disabled\r\nServer: gtk-gnutella/(\d[-.\w]+) \(([^\)\r\n]+)\)\r\n| p/gtk-gnutella P2P client/ v/$1/ i/$2; browse host disabled/
match gnutella m|^HTTP/1\.[01] \d\d\d .*\r\nServer: gtk-gnutella/(\d[-\w.]+) \([-\d]+; GTK2; Linux i686\)\r\n.*sharing (\d+) files ([\d.]+ \w+) total</h3>\r\n|s p/gtk-gnutella P2P client/ v/$1/ i/Sharing $2 files, $3/ o/Linux/

# LimeWire 3.5.8 on Suse Linux 8.1
match gnutella m|^HTTP/1\.1 406 Not Acceptable\r\n(\r\n)?$| p/LimeWire Gnutella P2P client/
match gnutella m|^HTTP/1\.0 406 Not Acceptable\r\nDate: .*\r\nServer: LimeWire/([\w._-]+)\r\n| p/LimeWire Gnutella P2P client/ v/$1/
match gnutella m|^HTTP/1\.0 200\r\nServer: Mutella\r\n| p/Mutella Gnutella P2P client/
match gnutella m|^HTTP/1\.1 404 Not Found\r\nServer: giFT-Gnutella/(\d[-.\w]+)\r\n| p/GiFT P2P client gnutella module/ v/$1/
match gnutella m|^HTTP/1\.1 200 OK\r\n.*Server: Shareaza (\d\S+)|s p/Shareaza/ v/$1/
match gnutella m|^HTTP/1\.1 \d\d\d .*Server: BearShare ([\d.]+)\r\n|s p/BearShare Gnutella P2P client/ v/$1/ o/Windows/
match gnutella m|^HTTP/1\.1 \d\d\d .*Server: BearShare ([\d.]+) \(([^)]+)\)\r\n|s p/BearShare Gnutella P2P client/ v/$1/ i/$2/ o/Windows/
match gnutella m|^HTTP/1\.1 503 Web: Disabled\r\nServer: BearShare Pro ([\d.]+)\r\nContent-Length: \d+\r\n| p/BearShare Pro Gnutella P2P client/ v/$1/ i/Web disabled/ o/Windows/
match gnutella m|^HTTP/1\.1 503 Web: Disabled\r\nServer: BearShare Lite ([\d.]+)\r\nContent-Length: \d+\r\n| p/BearShare Lite Gnutella P2P client/ v/$1/ i/Web disabled/ o/Windows/
match gnutella m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: GhostWhiteCrab/([\d.]+)\r\nConnection: close\r\n\r\n| p/GhostWhiteCrab gnutella cache/ v/$1/
match gnutella m|^HTTP/1\.0 501 Not Implemented\r\nDate: .*\r\nServer: Frosty/([\w._-]+)\r\nContent-Length: 0\r\nConnection: Close\r\n\r\n| p/Frostwire P2P/ i/Frosty $1/

match gopher m|^HTTP/1\.0 200 Ok\r\nMIME-Version: 1\.0\r\nServer: GopherWEB/(\d[-.\w]+)\r\n| p/Internet Gopher Server/ i/Gopher+ protocol; GopherWeb $1/
match gopher m|^0'/GET / HTTP/1\.0' doesn't exist!\t\terror\.host\t1\r\n\.\r\n$| p/Bucktooth gopherd/
match gopher m|^3 --6 Bad Request\. \r\n\.\r\n$| p/Windows gopherd/ o/Windows/
match gopher m|^3 --6 Ung\xfcltige Anforderung\. \r\n\.\r\n$| p/Windows gopherd/ i/German/ o/Windows/
match gopher m|^3'/GET / HTTP/1\.0' does not exist \(no handler found\)\t\terror\.host\t1\r\n| p/pygopherd/
# GoFish is also a Gopher-to-HTTP gateway.
match gopher m|^HTTP/1\.0 500 Server Error\r\nServer: Server: GoFish/([\d.]+) \(Linux\)\r\n|s p/GoFish gopherd/ v/$1/ o/Linux/
match gopher-proxy m|^3That item is not currently available\.\r\n$| p/Symantec gopher proxy/

# GoverLan Remote Admin/Control (Tom Sellers)
match goverlan m|^\0\0\0\0/\x20HT| p/Goverlan Remote Administration/

match gpsd m|^GPSD,G=\?,E=\?,T=\?,T=\?,T=\?,P=\?\r\n| p/gpsd/
match gpsd-ng m|^{\"class\":\"VERSION\",\"release\":\"([\w._-]+)\",\"rev\":\"([\w._-]+)\",\"proto_major\":\d+,\"proto_minor\":\d+}\r\n$| p/GPSD-NG/ v/$1 rev $2/

match groupwise m|^\xbc\xef\x16\0\xb5\xfe\x14\0\0\0\0 \xb5x3\x06a\x05\0\0\x16\0\xbc\xef\x1a\0\xb5\xfe\x18\0\0\0\0 d\xcf2\n\0\0\0\0\0\0\0\0\x1a\0\xbc\xef\x14\0\xb5\xfe\x0e\0\x02\0\x02!\x03\x16\x7f\$r\xe7\x14\0$| p/Novell GroupWise/

match hp-logic-analyzer m|^\r\n\r0\.1/PTTH / TEG.\r\n$| p/HP 1662C logic analyzer/ d/specialized/

# Needs to go before the Apache match lines -Doug
match http-proxy m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Apache\r\n.*X-orenosp-filt:|s p/Orenosp reverse http proxy/
# Needs to go before BaseHTTP match lines.
match ovs-agent m|^HTTP/1\.0 200 OK\r\n.*Server: BaseHTTP/([\d.]+) Python/([\w.]+)\r\n.*<title>Python: OVSAgentServer Document</title>|s p/Oracle OVSAgentServer/ v/22/ i/BaseHTTP $1; Python SimpleXMLRPCServer; Python $2/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: BaseHTTP/([\d.]+) Python/([\w.]+)\r\n.*<tt>This&nbsp;server&nbsp;exports&nbsp;the&nbsp;following&nbsp;methods&nbsp;through&nbsp;the&nbsp;XML-RPC&nbsp;protocol.</tt>|s p/BaseHTTP/ v/$1/ i/Python SimpleXMLRPCServer; Python $2/

match http m|^HTTP/1\.0 \d\d\d .*\r\n(.*\r\n)?Server: MochiWeb/(\d[-.\w]+) \([-.'\w\s]+\)\r\n| p/MochiWeb Erlang HTTP library/ v/$2/
match http m|^HTTP/1\.0 200 OK\r\nServer: Apache/([\d.]+)\r\nPragma: no-cache\r\nDate: .*<title></title>\r\n.*\r\nvar my_upnp = 1;\r\n// backup log and config\r\nvar PM = \"7004ABR\";|s p/SMC Broadband router 7004ABR http config/ i/Identifies as Apache $1/ d/broadband router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nPragma: no-cache\r\nContent-type: text/html\r\nWWW-Authenticate: Basic realm=\"Login to the Router Web Configurator\"\r\n\r\n<html>\n  <head>\n  <title>401 Unauthorized</title>\n  </head>\n<body>\n\n<div align=\"center\">| p/Draytek Vigor ADSL router webadmin/ d/broadband router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: webfs/(\d[-.\w]+)\r\n| p/WebFS httpd/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nConnection: Keep-Alive\r\nContent-Type: text/html\r\nContent-Length: \d+\r\n\r\n<HTML>\n<!-- Copyright IBM Corporation, 1999 -->\n<HEAD>\n<META HTTP-EQUIV=\"Content-Type\" CONTENT=\"text/html; charset=| p/IBM switch webadmin/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: WebCam2000/(\d[-.\w]+) \(([-/.+\w]+); www\.stratoware\.com/webcam2000/\)\r\n| p/WebCam2000 httpd/ v/$1/ i/$2/
match http m|^HTTP/1\.0 404 Not Found\r\nDate: .*\r\nServer: BWS/1\.0b3\r\n\r\n| p/Corel Paradox relational database web interface/ v/9.X/ i/Embedded BWS 1.0b3/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: WebSite/(\d[-.\w]+)\r\n| p/Deerfield VisNetic WebSite Professional/ v/$1/
match http m|^HTTP/1\.0 \d\d\d\r\nServer: Statistics Server (\d[-.\w]+)\r\n| p/DeepMetrix Statistics Server/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\nDate: Tue, 07 Oct 2003 12:26:05 GMT\r\nAllow: GET, HEAD\r\nServer: Spyglass_MicroServer/(\d[-.\w]+)\r\n\r\n<html>\n\n<head>\n\n<title>.*PhaserLink| p/Tektronix Phaser printer webadmin/ i/Ebedded Spyglass MicroServer $1/ d/printer/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: 3Com/v(\d[-.\w]+)\r\n.*WWW-Authenticate:Basic realm=\"device\"\r\n|s p/3Com switch webadmin/ v/$1/
match http m|^HTTP/1\.0 401 Unauthorized\nDate: .*\nServer: Acme\.Serve/v(\d[-.\w ]+)\nConnection: close\nExpires: .*\nWWW-Authenticate: Basic realm=\"PowerChute network shutdown\"\n|s p/APC Powerchute UPS web management/ i/Embedded Acme.Serv $1/ d/power-device/
match http m|^HTTP/1\.0 401 Unauthorized\nDate: .*\nServer: Acme\.Serve/v(\d[-.\w ]+) of \w+\nConnection: close\nExpires: .*\nWWW-Authenticate: Basic realm=\"PowerChute Network Shutdown\"\n|s p/APC Powerchute UPS web management/ i/Embedded Acme.Serv $1/ d/power-device/
match http m|^HTTP/1\.0 302 Found\r\nLocation: /index\.htm\r\n\r\n| p/Alcatal Speedtouch ADSL router webadmin/ d/broadband router/
match http m|^HTTP/1\.0 404 Not Found\r\nServer: pks_www/(\d[-.\w]+)\r\n| p/OpenPGP public key server/ v/$1/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: Apache/0\.6\.5\r\nPragma: no-cache\r\nContent-type: text/html\r\nWWW-Authenticate: Basic realm=\"System Setup\"\r\n| p/BenQ AWL wireless router webadmin/ d/broadband router/
# Orinoco bg-2000 Access Point
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: Agranat-EmWeb/R([\w_]+)\r\nWWW-Authenticate: Basic realm=\"gateway\"\r\n| i/Orinoco WAP http config/ p/Agranat-EmWeb/ v/$SUBST(1,"_",".")/
# ORiNOCO AP-600
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: Virata-EmWeb/R([\w_]+)\r\nWWW-Authenticate: Basic realm=\"Access-Product\"\r\n| i/Orinoco WAP http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/
match http m|^HTTP/1\.1 200 OK\nConnection: close\nContent-type: image/gif\nPragma: no-cache\nContent-Length: 22528\n\nMZ| p/bobax.worm.c httpd/ o/Windows/

# HP Printers
match http m|^HTTP/1\.1 200 OK\r\nServer: Agranat-EmWeb/R([\d_]+)\r\nContent-Type: text/html;charset=ISO-8859-1\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n\r\n<HTML> \n<HEAD>\n<TITLE> | i/HP LaserJet http config/ p/Agranat-EmWeb/ v/$SUBST(1,"_",".")/ d/printer/
match http m|^HTTP/1\.1 200 OK\r\nServer: Virata-EmWeb/R([\d_]+)\r\nContent-Type: text/html;charset=ISO-8859-1\r\nExpires: .*\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n\r\n<!DOCTYPE html\nPUBLIC | i/HP LaserJet http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/printer/
match http m|^HTTP/1\.1 200 OK\r\nServer: Virata-EmWeb/R([\d_]+)\r\nContent-Type: text/html;charset=utf-8\r\nExpires: Thu, 01 Jan 1970 00:00:00 GMT\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n\r\n<!--  DOCTYPE tag is included to support the XHTML  -->\n<!DOCTYPE html\n   PUBLIC | i/HP LaserJet http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/printer/
match http m|^HTTP/1\.1 200 OK\r\nServer: Virata-EmWeb/R([\d_]+)\r\n-ransfer-Encoding: chunked\r\nContent-Type: text/html\r\nExpires: .*\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n\r\n\n\n<!DOCTYPE html\nPUBLIC| i/HP JetDirect http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/
match http m|^HTTP/1\.1 301 Moved Permanently\r\nServer: Virata-EmWeb/R([\d_]+)\r\nLocation: https://([\d.]+)/\r\nContent-Type: text/html\r\nContent-Length: [89][0123456789]\r\n\r\n<HEAD><TITLE>Moved</TITLE></HEAD><BODY>| i/HP LaserJet http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/printer/ h/$2/
match http m|^HTTP/1\.0 301 Resource Moved\r\nCONTENT-LENGTH: 0\r\n.*\r\nSERVER: HP-ChaiSOE/([\d.]+)\r\n|s i/HP LaserJet http config/ p/HP-ChaiSOE/ v/$1/ d/printer/
match http m|^HTTP/1\.1 301 Resource Moved\r\nCONTENT-LENGTH: 0\r\nEXPIRES: .*\r\nLocation: /hp/device/this\.LCDispatcher\r\nCACHE-CONTROL: no-cache\r\nSERVER: HP-ChaiSOE/([\d.]+)\r\n-ONNECTION: Keep-Alive\r\n\r\n| i/HP LaserJet http config/ p/HP-ChaiSOE/ v/$1/ d/printer/
match http m|^HTTP/1\.1 200 OK\r\nServer: Agranat-EmWeb/R([\d_]+)\r\nContent-Type: text/html;charset=ISO-8859-1\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n\r\n<HTML> \n<HEAD>\n<TITLE> | i/HP LaserJet http config/ p/Agranat-EmWeb/ v/$SUBST(1,"_",".")/ d/printer/
match http m|^HTTP/1\.1 200 OK\r\nServer: Virata-EmWeb/R([\d_]+)\r\n-ransfer-Encoding: chunked\r\nContent-Type: text/html\r\nExpires: .*\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n\r\n\n\n<!DOCTYPE html\nPUBLIC| i/HP JetDirect http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/printer/
match http m|^HTTP/1\.1 301 Moved Permanently\r\nServer: Virata-EmWeb/R([\d_]+)\r\nLocation: https://([\d.]+)/\r\nContent-Type: text/html\r\nContent-Length: 90\r\n\r\n<HEAD><TITLE>Moved</TITLE></HEAD><BODY>| i/HP Color LaserJet 3500 http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/printer/ h/$2/
match http m|^HTTP/1\.1 301 Moved Permanently\r\nServer: Virata-EmWeb/R([\d_]+)\r\nAccept-Ranges: none\r\nLocation: https://([\d.]+)/\r\nContent-Type: text/html\r\nContent-Length: 90\r\n\r\n| i/HP Officejet Pro L7680 http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/printer/ h/$2/
match http m|^HTTP/1\.1 200 OK\r\nServer: Virata-EmWeb/R([\d_]+)\r\n.*\n\n\n<title> HP Color LaserJet 2840  /|s i/HP Color LaserJet 2840 http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/printer/
match http m|^HTTP/1\.1 200 OK\r\nServer: Virata-EmWeb/R([\d_]+)\r\n.*<title>HP Officejet Pro (\w+)</title>\n|s i/HP OfficeJet Pro $2 http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/printer/
match http m|^HTTP/1\.1 200 OK\r\nServer: Virata-EmWeb/R([\d_]+)\r\n.*<title>HP Officejet (\w+) series</title>|s i/HP Officejet $2 http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/printer/
match http m|^HTTP/1\.1 200 OK\r\nServer: Virata-EmWeb/R([\d_]+)\r\n.*<title>HP Officejet Pro (\w+) A909g</title>|s i/HP Officejet $2 http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/printer/
match http m%^HTTP/1\.1 \d\d\d .*\r\nServer: Virata-EmWeb/R([\d_]+)\r\nContent-Type: text/html; ?charset=UTF-8\r\nExpires: .*<title>HP (Color |)LaserJet ([\w._ -]+)&nbsp;&nbsp;&nbsp;%si p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ i/HP $2LaserJet $3 printer http config/ d/printer/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Virata-EmWeb/R([\d_]+)\r\n.*<title>HP LaserJet (\w+)&nbsp;&nbsp;&nbsp;|s p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ i/HP LaserJet $2 printer http config/ d/printer/
match http m|^HTTP/1\.1 200 OK\r\nServer: Virata-EmWeb/R([\d_]+)\r\n.*<title>HP Photosmart ([\w._+-]+) series</title>|s p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ i/HP Photosmart $2 series printer http config/ d/printer/
match http m|^HTTP/1\.1 404 Not Found\r\nConnection: close\r\nServer: HP HTTP Server; HP Photosmart ([\w._+-]+) series - \w+; Serial Number: (\w+);| p/HP Photosmart $1 series printer http config/ d/printer/ i/Serial $2/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: \$ProjectRevision: ([\d.]+) \$\r\n.*<title>HP LaserJet (\w+)</title>|s p/HP LaserJet $2 printer http config/ v/$1/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: \$ProjectRevision: ([-\d.]+) \$\r\n.*<title>HP Color LaserJet 2600n</title>|s p/HP Color LaserJet 2600n http config/ v/$1/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: \$ProjectRevision: ([\d.]+) \$\r\n.*<title>HP LaserJet (\w+)(?: MFP)&nbsp;&nbsp;&nbsp;([\d.]+)</title>|s p/HP LaserJet $2 printer http config/ v/$1/ d/printer/ h/$3/

match http m|^HTTP/1\.0 200 OK\nServer: stats\.mod/(\d[-.\w]+)\n| p/Eggdrop stats.mod web statistics module/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\nServer: PPR-httpd/(\d[-.\w]+)\r\n| p/PPR print spooling daemon ppradmin/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*\r\nServer: RAC_ONE_HTTP (\d[-.\w]+)\r\n| p/Dell Embedded Remote Access card httpd/ v/$1/ d/terminal server/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\n\r\n<HTML>\r\n<HEAD>\r\n<TITLE>EpsonNet WebAssist Rev\.(\d[-.\w]+)</TITLE>| p/EpsonNet WebAssist printer configuration/ v/$1/ d/printer/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\n\r\n<HTML><HEAD><META HTTP-EQUIV=\"Content-type\" CONTENT=\"text/html; charset=iso-8859-1\">\r\n<TITLE>Lexmark ([-/.+\w]+)</TITLE>| p/Lexmark printer webadmin/ i/Lexmark $1/ d/printer/
match http m|^HTTP/1\.0 200 OK\nServer: III (\d[-.\w]+)\n| p/Innovative Interfaces Innopac httpd/ v/$1/
match http m|^HTTP/1\.0 401 Unauthorized\r\nContent-type: text/html\r\nWWW-Authenticate: Basic realm=\"CISCO_WEB\"\r\n| p/Cisco DSL router webadmin/  d/broadband router/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\n.*Server: Allegro-Software-RomPager/([\w.]+)\r\n\r\n<HTML>\n<HEAD>\n<TITLE>Cisco Systems, Inc\.</TITLE>.*Cisco IP Phone ([-\w_]+)|s p/Cisco IP Phone $2/ i/Allegro RomPager $1/ d/VoIP phone/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nRAKeepAliveHeader: \.+\r\n| p/RemotelyAnywhere remote PC management httpd/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: RemotelyAnywhere/([\d.]+)\r\n|s p/RemotelyAnywhere remote PC management httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: Ipswitch-IMail/(\d[-.\w]+)\r\n| p/Ipswitch IMail web service/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: IMail_Monitor/(\d[-.\w]+)\r\n| p/Ipswitch IMail Monitor web service/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: Ipswitch Web Calendaring /(\d[-.\w]+)\r\n| p/Ipswitch IMail Web Calendar/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nSet-Cookie:WhatsUp={[-\w]+}; path=/\r\nContent-Type: text/html\r\nServer: Ipswitch ([\d.]+)\r\n| p/Ipswitch WhatsUp httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: text/html\r\nPragma: no-cache\r\nCache-Control: no-cache\r\n\r\n<html><head><title>Authentication Form</title></head><BODY BGCOLOR=\"#000000\" TEXT=\"#00FF00\"><p><h3 align=left><font face=\"arial,helvetica\">Client Authentication Remote Service</font>| p/Check Point Firewall-1 Client Authentication httpd/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: text/html\r\nPragma: no-cache\r\nCache-Control: no-cache\r\n\r\n.*<title>\n  Authentication Form.*Client Authentication Remote \nService</font>.*FireWall-1 message: User: <p> <P>\n|s p/Check Point Firewall-1 Client Authentication httpd/
match http m|^HTTP/1\.0 200\r\nPragma: no-cache\r\nCache-Control: no-cache\r\nContent-Type: text/html\r\nContent-Length: \d+\r\n\r\n<TITLE>Error</TITLE>\n<BODY>\n<H1>Error</H1>\nFW-1 at ([-\w_.]+): Failed to connect to the WWW server\.</BODY>\r\n| p/Check Point Firewall-1 httpd/ h/$1/
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"FW-1\"\r\nContent-Type: text/html\r\nContent-Length: \d+\r\n\r\n<TITLE>Error</TITLE>\n<BODY>\n<H1>Error 401</H1>\n\nFW-1 at ([-\w_.]+):| p/Check Point Firewall-1 httpd/ h/$1/

match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: Check Point SVN foundation| p/Check Point SVN foundation httpd/ d/firewall/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: HP-UX_Apache-based_Web_Server/(\d[-.\w]+) (.*)\r\n| p/HP-UX httpd/ v/$1/ i/Apache derived; $2/ o/HP-UX/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: HP-UX_Apache-based_Web_Server\r\n| p/HP-UX httpd/ i/Apache derived/ o/HP-UX/
match http m|^HTTP/1\.1 302 Moved\r\nContent-type: text/html\r\nConnection: close\r\nLocation: /1[012]\d{8}/l\r\n\r\n<H1>Document| p/Novell NetMail ModWeb webmail/
match http m/^GIF89a\xa8\0-\0\xf7\0\0\x03\x03\x03\x83\x83\x83\xc4\xc4\xc4\xfe\x02\x02\xc9\x85c\x85|\xb5\xe2\xe2\xe2\xca\xa2\x8e\xd4RRCCC\xdeb\"\xa5\xa5\xa5\xe7\xc5/ p/Tweak XP web advertisement blocker/
# Management interface for Xerox Phaser printers. 
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\nDate: .*\r\nExpires: .*\r\nLast-Modified: .*\r\nPragma: no-cache\r\nServer: Allegro-Software-RomPager/(\d[-.\w]+)\r\n\r\n<HTML>\n<!--Copyright \(c\) Xerox Corporation | p/Xerox printer webadmin/ i/Embedded Allegro-Software-RomPager $1/ d/printer/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\nDate: .*\r\nExpires: .*\r\nLast-Modified: .*\r\nPragma: no-cache\r\nServer: Allegro-Software-RomPager/(\d[-.\w]+)\r\n\r\n<html>\n<head>\n<title>\nHome - \nPhaser (\w+)</title>\n|s p/Xerox printer webadmin/ i/Printer $2; Embedded Allegro-Software-RomPager $1/ d/printer/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"CentreWare_IS_Admin\"\r\nContent-Type: text/html\r\nServer: Allegro-Software-RomPager/([\d.]+)\r\n\r\n| p/Allegro RomPager httpd/ v/$1/ i/Xerox Phaser printer/ d/printer/
match http m|^HTTP/1\.1 \d\d\d .*\r\nContent-Type: text/html\r\nDate: .*Server: Allegro-Software-RomPager/([\d.]+)\r\n\r\n<html>\n<head>\n<title>\nAccueil - \nPhaser (\w+)</title>|s p/Xerox printer webadmin/ i/French; Printer $2; Embedded Allegro-Software-RomPager $1/ d/printer/
match http m|^HTTP/1\.0 302 Moved Temporarily\r\nserver: IronPort httpd/(\d[-.\w]+)\r\n| p/IronPort mail appliance admin websever/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\nServer: Virata-EmWeb/R(\d[-.\w]+)\r\nContent-Type: text/html\r\nExpires: .*\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n\r\n\n<html>\n<head><title>(CopperJet [-.+\w ]+)</title>| i/Allied Data CopperJet ADSL modem; $2/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/broadband router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\nServer: dhttpd/(\d[-.\w]+)\r\n| p/dhttpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Snap Appliance, Inc\./(\d[-.\w]+)\r\n| p/Snap Appliance storage system webadmin/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nPragma: no-cache\r\nContent-Type: text/html\r\n\r\n<HTML>\n<FRAMESET COLS=\"105,\*\" FRAMEBORDER=NO BORDER=0\nFRAMESPACING=0>\n<FRAME SRC=\"/side\.html\" SCROLLING=NO>\n<FRAME SRC=\"/startupdata\.html\">\n</FRAMESET>\n</HTML>\n$| p/Motorola cable modem webadmin/ d/broadband router/
match http m|^HTTP/1\.0 200 OK\nDate: .*\nServer: Intel NetportExpressPro/(\d[-.\w]+)\n| p/Intel NetportExpress Pro print server webadmin/ v/$1/ d/print server/
match http m|^HTTP/1\.0 200 Ok\r\nContent-Type: text/html; charset=\"utf-8\"\r\n\r\n<HTTP>\r\n<HEAD>\r\n  <TITLE>MythTV Status</TITLE>| p/MythTV Linux PVR webadmin/ o/Linux/

# Very specific... Will probably have to be changed when MythTV changes their CSS...
match http m|^HTTP/1\.[01] 200 .*<style type=\"text/css\" title=\"Default\" media=\"all\">\r\n  <!--\r\n  body {|s p/MythTV Linux PVR webadmin/ o/Linux/

match http m|^HTTP/1\.0 302 Found\r\nLocation: http://[-.+\w]+:32\d\d\d/\r\n\r\n$| p/Sun Solaris Management Console/ i/Apache Tomcat/ o/Solaris/
# Cyclades PR2000 Router
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"PR2000 - Login\"\r\nContent-Type: text/html\r\nServer: Allegro-Software-RomPager/ ?([\w.]+)\r\n\r\n.*</H1>This object on the Cyclades PR2000 - RomPager server is protected|s p/Cyclades PR2000 Router/ i/Allegro RomPager $1/ d/router/
# 3Com OfficeConnect 812 Router telnetd
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"OCR-([-.\w]+)\"\r\nContent-Type: text/html\r\nServer: Allegro-Software-RomPager/(\d[-.\w]+)\r\n| p/3Com OfficeConnect Router webadmin/ i/Embedded Allegro-Software-RomPager $2; OfficeConnect OCR-$1/ d/router/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"APC Management Card\"\r\nContent-Type: text/html\r\nServer: Allegro-Software-RomPager/ ?([\w.]+)\r\n\r\n| p/APC Management Web Server/ i/Allegro RomPager $1/ d/power-device/
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"PDU\"\r\nServer: Allegro-Software-RomPager/ ?([\w.]+)\r\n\r\n<HTML>\n<HEAD>\n<TITLE>Protected Object</TITLE>\n</HEAD>\n<BODY BGCOLOR=\"WHITE\">\n<H1>Protected Object</H1>\nThis object on the MasterSwitch Web Server is protected\.| p/APC masterswitch http config/ i/Allegro RomPager $1/ d/power-device/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"MasterSwitch Plus\"\r\nContent-Type: text/html\r\nServer: Allegro-Software-RomPager/ ?([\w.]+)\r\n\r\n<HTML>\n<HEAD>\n<TITLE>Protected Object</TITLE>.*This object on the APC Management Web Server is protected\.|s p/APC masterswitch http config/ i/Allegro RomPager $1/ d/power-device/
match http m|^HTTP/1\.0 200 OK\r\nPragma: no-cache\r\nContent-Type: text/html\r\n\r\n<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.0 Transitional//EN\">\n.*<META NAME=Copyright CONTENT=\"Copyright \(c\) 2003 3Com Corporation\. All Rights Reserved\.\">\n.*<META http-equiv=\"3Cnumber\" content=\"([-.\w]+)\">\n|s p/3Com OfficeConnect router webadmin/ i/3Com` $1/ d/router/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\n.*\r\nServer: Allegro-Software-RomPager/ ?([\w.]+)\r\n\r\n<!DOCTYPE HTML PUBLIC \"-//IETF//DTD HTML//EN\">\n\n<html>\n\n<head>\n<meta http-equiv=\"Content-Type\" content=\"text/html; iso-8859-1\">\n<title>Summit Management Interface</title>|s p/Summit Management Interface/ i/Allegro RomPager $1/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\n.*Server: Allegro-Software-RomPager/([\w.]+)\r\n\r\n\n<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.01 Transitional//EN\">\n<html>\n<head>\n<title>\n([^&\r\n]+)&nbsp;- Status</title>|s p/Roku Sound Bridge Web Interface/ i/Allegro RomPager $1; Name $2/ d/media device/
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"\r\n\r\n<title>401 Unauthorized</title><body><h1>401 Unauthorized</h1></body>| p/Acer Warplink Firewall Router webadmin/ d/router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: httpd\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"Sitecom WL-([-.\w]+)\"\r\n| p/Sitecom webadmin/ i/Sitecom WL-$1/ d/WAP/
match http m|^HTTP/1\.0 200 OK\r\nDate: .*\r\n\r\n<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.0 Transitional//EN\"><html><body bgcolor=\"#C0C0C0\" text=\"#000000\" vlink=\"#800080\" link=\"#0000FF\"><P><h1>TempTrax Digital Thermometer</h1>| p/SensaTronics TempTrax Digital Thermometer/ d/specialized/
match http m|^HTTP/1\.1 401 Unauthorised\r\nServer: Zeus/(\d[-.\w]+)\r\n.*WWW-Authenticate: basic realm=\"Zeus Admin Server\"\r\n|s p/Zeus httpd Admin Server/ v/$SUBST(1,"_",".")/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Zeus/(\d[-.\w]+)\r\n|s p/Zeus httpd/ v/$1/
match http m|^HTTP/1\.0 404 File not Found\r\nServer: SPiN ChatSystem/(\d[-.\w]+)\r\n| p/SPiN web chat system/ v/$1/

# IP_SHARER WEB
match http m|^HTTP/1\.0 200 Document follows\r\nServer: IP_SHARER WEB ([\w._-]+)\r\nContent-type: text/html\r\n\r\n<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.0 Transitional//EN\">\n\n<html><head><title>Setup</title>| i/Siemens SpeedStream SS2601/ p/IP_SHARER WEB/ v/$1/ d/router/
match http m|^HTTP/1\.0 200 OK\r\nServer: IP_SHARER WEB ([\w._-]+)\r\nContent-type: text/html\r\nConnection: close\r\n\r\nunknown \(([\d.]+)\) is managing this device| i/TRENDnet router http config; being managed by $2/ p/IP_SHARER WEB/ v/$1/ d/router/
match http m|^HTTP/1\.0 200 OK\r\nServer: IP_SHARER WEB ([\w._-]+)\r\n.*<meta name=\"description\" content=\"Belkin (\d+)\">|s i/Belkin $2 wifi router http config/ p/IP_SHARER WEB/ v/$1/ d/WAP/
match http m|^HTTP/1\.0 200 OK\r\nServer: IP_SHARER WEB ([\w._-]+)\r\n.*<title>Setup</title>.*type=\"text/javascript\">\nfunction loadnext\(\)|s i/TRENDnet TW100-BRV204 router http config; no admin pass/ p/IP_SHARER WEB/ v/$1/ d/router/
match http m=^HTTP/1\.0 200 OK\r\nServer: IP_SHARER WEB ([\w._-]+)\r\n.*<title>TRENDnet \| TW100-BRF114 \| Setup</title>=s i/TRENDnet TW100-BRF114 router http config/ d/router/ p/IP_SHARER WEB/ v/$1/
match http m|^HTTP/1\.0 401 Unauthorized\nServer: IP_SHARER WEB ([\w._-]+)\r\nContent-type: text/html\r\nWWW-Authenticate: Basic realm=\"NETGEAR WP([-\w+]+)\"\r\n\r\n| i/Netgear $2 WAP http config/ p/IP_SHARER WEB/ v/$1/ d/WAP/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: IP_SHARER WEB ([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"(AT-\w+)\"\r\nContent-type: text/html\r\n\r\n401 Unauthorized| i/Allied Telesyn $1 WAP http config/ p/IP_SHARER WEB/ v/$1/ d/broadband router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: IP_SHARER WEB ([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"BEFSR41W\"\r\nContent-type: text/html\r\n\r\n401 Unauthorized| i/Linksys BEFSR41W router http config/ p/IP_SHARER WEB/ v/$1/ d/router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: IP_SHARER WEB ([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"(DG[\w]+)\"\r\n| i/Netgear $2 WAP http config/ p/IP_SHARER WEB/ v/$1/ d/WAP/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: IP_SHARER WEB ([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"(FM\w+)\"\r\n| i/Netgear $2 http config/ d/broadband router/ p/IP_SHARER WEB/ v/$1/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: IP_SHARER WEB ([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"(FR[-.\w+]+)\"\r\n| i/Netgear $1 firewall router http config/ p/IP_SHARER WEB/ v/$1/ d/router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: IP_SHARER WEB ([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"NeedPassword\"\r\nContent-type: text/html\r\nConnection: close\r\n\r\n401 Unauthorized$| i/TRENDnet TW100-BRV204 router http config; admin pass set/ p/IP_SHARER WEB/ v/$1/ d/router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: IP_SHARER WEB ([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"NeedPassword\"\r\nContent-type: text/html\r\n\r\n401 Unauthorized| i|Airlink/Sitecom wireless router| p/IP_SHARER WEB/ v/$1/ d/router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: IP_SHARER WEB ([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"(NR[\w+]+)\"\r\n| i/Netgear $2 router http config/ p/IP_SHARER WEB/ v/$1/ d/router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: IP_SHARER WEB ([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"(WGPS[\w+]+)\"\r\n| i/Netgear $2 print server http config/ p/IP_SHARER WEB/ v/$1/ d/print server/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: IP_SHARER WEB ([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"WRT54GC\"\r\n| i/Linksys WRT54GC http config/ p/IP_SHARER WEB/ v/$1/ d/WAP/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: IP_SHARER WEB ([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"WYR-G54\"\r\n| i/Buffalo Airstation WYR-G54 WAP http config/ p/IP_SHARER WEB/ v/$1/ d/WAP/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: IP_SHARER WEB ([\w._-]+)\r\nContent-type: text/html\r\n\r\n<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.0 Transitional//EN\">\n<html><head>\n<meta name=\"description\" content=\"SOHO Version ([\d.]+)\">\n\n<title>Setup</title>\n| i/SpeedStream router http config; SOHO Version $2/ p/IP_SHARER WEB/ v/$1/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: IP_SHARER WEB ([\w._-]+)\r\nContent-type: text/html\r\n\r\nunknown \(.*\) is managing this device| i/SpeedStream router http config/ p/IP_SHARER WEB/ v/$1/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: IP_SHARER WEB ([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"FVS114\"\r\n| i/Netgear ProSafe FVS114 firewall http config/ p/IP_SHARER WEB/ v/$1/ d/firewall/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: IP_SHARER WEB ([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"FWG114P\"\r\n| i/Netgear FWG114P wireless firewall http config/ p/IP_SHARER WEB/ v/$1/ d/firewall/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: IP_SHARER WEB ([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"MR814v2\"\r\n| i/Netgear MR814v2 wireless router http config/ p/IP_SHARER WEB/ v/$1/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: IP_SHARER WEB ([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"(WGR614[^"]*)\"\r\n| i/Netgear $2 router http config/ p/IP_SHARER WEB/ v/$1/ d/router/

# PRINT_SERVER WEB
match http m|^HTTP/1\.0 200 Document follows\r\nServer: PRINT_SERVER WEB ([\w._-]+)\r\n.*<meta name=\"description\" content=\"([\w-]+) \d+\">\n\n<title>NetGear Print Server Setup</title>|s p/PRINT_SHARER WEB/ v/$1/ i/Netgear $2 print server http config/ d/print server/

# Netgear FR314 Firewall Router
match http m|^HTTP/1\.0 200 OK\r\nServer: NETGEAR Firewall\r\n| p/Netgear FR-series firewall router http config/ d/router/
# Netgear FVS318 Firewall/Router
match http m|^HTTP/1\.0 200 OK\r\nServer: Netgear\r\nContent-Type: text/html\r\nPragma: no-cache\r\nLast Modified: .*\r\nConnection: close\r\n\r\n.*<title>\r\t\t\tNETGEAR Router \r|s p/Netgear FVS318 router http config/ d/router/
# Netgear RP614 firmware version 4.12
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"(RP\d+)\"\r\nServer: Embedded HTTPD v(\d[-.\w]+), | p/Netgear router http config/ i/Netgear $1; Delta Networks Embedded HTTPd $2/ d/broadband router/
# CiscoSecure ACS 3.1 on Windows 2000 Server
# Cisco Secure ACS for Windows 2000
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\nContent-length: \d+\r\n\r\n<html>\r\n<head>\r\n<title>CiscoSecure ACS Login</title>| p/Cisco Secure ACS web interface/ o/Windows/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\nContent-length: \d+\r\n\r\n<html>\r\n<head>\r\n<title>CiscoSecure ACS for Windows 2000/NT Login</title>\r\n| p/Cisco Secure ACS web interface/ o/Windows/
# Pix Device Manager (PDM) version 3.01
match http m|^HTTP/1\.[01] 401 Unauthorized\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"PIX\"|s p/Cisco PIX Device Manager/ d/firewall/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: DHost/(\d[-.\w]+) HttpStk/(\d[-.\w]+)\r\n| p/Novell eDirectory DHOST httpd/ v/$1/ i/HttpStk: $2; used by iMonitor/ o/Unix/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: 3ware/(\d[-.\w]+)\r\n| p/3Ware web interface/ v/$1/ i/RAID storage/

match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Cherokee\r\n|s p/Cherokee httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Cherokee/([-.\w]+)\r\n|s p/Cherokee httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Cherokee/([-.\w]+) \(Debian GNU/Linux\)\r\n|s p/Cherokee httpd/ v/$1/ i/Debian/ o/Linux/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Cherokee/([-.\w]+) \(Ubuntu\)\r\n|s p/Cherokee httpd/ v/$1/ i/Ubuntu/ o/Linux/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Cherokee/([-.\w]+) \(openSUSE Build Service\)\r\n|s p/Cherokee httpd/ v/$1/ i/OpenSUSE/ o/Linux/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Cherokee/([-.\w]+) \(Gentoo Linux\)\r\n|s p/Cherokee httpd/ v/$1/ i/Gentoo/ o/Linux/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Cherokee/([-.\w]++) \(UNIX\)\r\n|s p/Cherokee httpd/ v/$1/ o/Unix/

match http m|^HTTP/1\.0 200 OK\r\nServer: HomeSeer\r\n| p/HomeSeer Home Control Web Interface/ o/Windows/
match http m|^HTTP/1\.0 401 \r\nWWW-Authenticate: Basic realm=\"HomeSeer\d+\"\r\n\r\n| p/HomeSeer Home Control Web Interface/ o/Windows/
# Multitech MultiVoip 410 VoIP gateway
match http m|^HTTP/1\.1 200 OK\r\nServer: RTXCweb Software (\d[-.\w]+)\r\nDate: .*\r\nContent-type: text/html\r\n\r\n<html>\r\n<head>\r\n<META HTTP-EQUIV=\"PRAGMA\" CONTENT=\"NO-CACHE\">\r\n<META HTTP-EQUIV=\"EXPIRES\" CONTENT=\"-1\">\r\n<script language = \"Javascript\">\r\nvar title_string = \" v \[Firmware - [\w ]+\]| i/Multitech MultiVoip VoIP gateway http config/ p/RTXCweb/ v/$1/ d/VoIP adapter/
# NetComm NB1300 ADSL Modem/Router
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: WindWeb/(\d[-.\w]+)\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"([-./\w ]+)\"\r\nContent-Type: text/html\r\n\r\n| p/$2 router http config/ i/runs WindWeb $1/ d/broadband router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: SimpleServer:WWW/(\d[-.\w]+)\r\n| p/AnalogX SimpleServer httpd/ v/$1/ o/Windows/
# Xitami - Try to match PHP first!
match http m|^HTTP/1\.[01] \d\d\d .*\r\nContent-Length: \d+\r\nX-Powered-By: ([-/.\w ]+)\r\nContent-Type: .*\r\nServer: Xitami\r\n| p/Xitami httpd/ i/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Xitami\r\n|s p/Xitami httpd/
match http m|^ERROR: Malformed startup string$| p/Xitami httpd admin port/
match http m|^HTTP/1\.1 500 Server Error\r\nConnection: close\r\nContent-Length: \d+\r\nDate: .*\r\nServer: Radio UserLand/(\d[.\w ]+)-([-.\w ]+)\r\n\r\n| p/Radio Userland blog server/ v/$1/ i/$2/ 
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: (prod )?[Ff]red (\d[-.\w]+) \(build (\d+)\) HTTP Servlets\r\n\r\n|s p/Freenet Fred anonymous P2P/ v/$2 build $3/
match http m|^HTTP/1\.0 200 Ok\r\nServer: diva_httpd\r\n| p/Eicon Diva ISDN card configuration server/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Resin/(\d[-.\w]+)\r\n| p/Caucho Resin JSP engine/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nMIME-Version: 1\.0\r\nServer: linuxconf/(\d[-.\w]+)\r\n| p/Linuxconf web configuration server/ v/$1/ o/Linux/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: TinyWeb/([\d.]+)\r\n|s p/Tinyweb httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nDate: .*\r\nServer: WebSitePro/(\d[-.\w]+)\r\n|s p/O'Reilly WebSite Pro/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Lucent Security Management Admin Server \r\n| p/Lucent Security Management Admin Server/ i/Lucent VPN Firewall/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: thttpd/(\d[-.+\w]+) ([\w?]+)\r\n| p/thttpd/ v/$1 $2/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: thttpd/(\d[-.+\w]+) ([\w?]+) Built-in PHP| p/thttpd/ v/$1 $2/ i/Built-in PHP/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: thttpd\r\n| p/thttpd/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nX-Powered-By: PHP/([\d.]+)\r\nServer: thttpd/([\w.]+) PHP/([\d.]+)\r\n|s p/thttpd/ v/$2/ i/PHP $1 ($3)/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: thttpd/([\w.]+) PHP/([\d.]+)\r\n| p/thttpd/ v/$1/ i/PHP $2/

match http m|^HTTP/1\.[01] .*Server: FirstClass/(\d[-.\w]+)\r\n|s p/FirstClass/ v/$1/
match http m|^HTTP/1\.1 400 Bad request\r\nServer: Citrix Web PN Server\r\n| p/Citrix Metaframe ICA Browser/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: HP-ChaiServer/(\d[-.\w]+)\r\nContent-length: 0\r\n\r\n|s p/HP JetDirect printer webadmin/ i/HP-ChaiServer $1/ d/printer/
# mldonkey-2.5-3 http port on Linux 2.4.21
match http m|^HTTP/1\.[01] 404 Not Found\r\nServer: MLdonkey\r\nConnection: close\r\nContent-Type: application/x-bittorrent\r\nContent-length: 0\r\n\r\n| p/MLDonkey multi-network P2P web interface/
match http m%^HTTP/1\.1 401 Unauthorized\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"(?:MLdonkey|P2P)\"\r\n% p/MLDonkey multi-network P2P web interface/
# Docupoint Discovery 3.0(Apache) on Windows 2000 Professional
match http m|^<html>\r<head><title>Docupoint Discovery</title>\r<META HTTP-EQUIV=\"Content-Type\" CONTENT=\"text/html; CHARSET=UTF-8\">\r| p/Docupoint Discovery search engine/
match http m|^HTTP/1\.0 200 OK\r\n.*\r\n\r\n<!DOCTYPE html PUBLIC \"-//W3C//DTD XHTML 1\.1//EN\" \"http://www\.w3\.org/TR/xhtml11/DTD/xhtml11\.dtd\">\n<html><head><title>BitTorrent download info</title>\n?</head>\n<body>\n<h3>BitTorrent download info</h3>\n<ul>\n<li><strong>tracker version:</strong> (\d[-.\w]+)</li>|s p/BitTorrent P2P tracker/ v/$1/ i/bttrack.py/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: eMule\r\n.*<title>eMule (\d[-.\w]+) |s p/eMule P2P/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: eMule\r\n.*<title>eMule Plus (\d[-.\w]+) |s p/eMule Plus P2P/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: eMule\r\n.*<title>Web Interface ([\w._-]+)</title>|s p/eMule P2P/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: eMule\r\n|s p/eMule P2P/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: embedded\r\n.*<title>eMule ([\w._-]+) \[MorphXT v([\w._-]+)\]|s p/eMule MorphXT P2P/ v|$1/$2|
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: aMule\r\n.*<title>aMule (\d[-.\w]+) - Web Control Panel</title>|s p/aMule P2P/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: aMule\r\n| p/aMule P2P/
match http m|^HTTP/1\.0 200 OK\r\nServer: Agent-ListenServer-HttpSvr/1\.0\r\n.*<ComputerName>([-.\w]+)</ComputerName><version>([\d\.]+)</version>|s p/Network Associates ePolicy Orchestrator/ i/Computername: $1 Version: $2/
# Network Associates EPO 3.0
match http m|^HTTP/1\.0 200 OK\r\nServer: Agent-ListenServer-HttpSvr/1\.0\r\n.*<ComputerName>([-.\w]+)</ComputerName>|s p/Network Associates ePolicy Orchestrator/ i/Computername: $1/
match http m|^HTTP/1\.0 403 Forbidden\r\nServer: Agent-ListenServer-HttpSvr/1\.0\r\n| p/Network Associates ePolicy Orchestrator/
match http m|^HTTP/1\.0 401 Unauthorized\r\nSPIPE-Authenticate: {[-\w]+}\r\n\r\n$| p/Network Associates ePolicy Orchestrator/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: [dD]ebut/(\d[-.\w]+)\r\n|s p|Brother/HP printer webadmin| i|Debut embedded httpd $1| d|printer|
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: kpf\r\n| p/KDE Public Fileserver/
match http m|^HTTP/1\.1 200 OK\r\nServer: Netscape-FastTrack/(\d[-.\w]+)\r\n| p/Sun Iplanet httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: dwhttpd/(\d[-.\w]+) \(([^\r\n\)]+)\)\r\nContent-type: text/html\r\n\r\n.*<TITLE>AnswerBook2: Personal Library</TITLE>\n|s p/Sun AnswerBook2 httpd/ v/$1/ i/$2/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: enCoreXpress/(\d[-.\w]+)\r\n|s p|enCoreXpress MOO| i|http://lingua.utdallas.edu/encore|
# Lispweb 2.0 Allegro Common Lisp.
match http m|^HTTP/1\.0 \d\d\d .*\nMime-Version: .*\nServer: LispWeb (\d[-.\w]+) \(acl\)\n| p/Lispweb httpd/ v/$1/
# World Client for MDaemon (www.altn.com) on Windows 2000
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: WDaemon/(\d[-.\w]+)\r\n| i/Alt-N MDaemon webmail/ p/World Client WDaemon httpd/ v/$1/ o/Windows/
# pop3proxy web interface from spambayes 1.0a5 on Linux
match http m|^HTTP/1\.1 \d\d\d .*\r\nConnection: close\r\nContent-Type: text/html\r\nDate: .*\r\n\r\n<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.01 Transitional//EN\">\r\n<html>\r\n<head>\r\n<title id=\"title\">Home</title>\r\n<meta content=\"no-cache\" http-equiv=\"Pragma\"/>\r\n<meta content=\"no-cache\" http-equiv=\"Cache\"/>\r\n| p/Spambayes pop3proxy web interface/
# Oracle XML Database - SuSe Linux 8.1 Personal, Linux 2.4.19, Oracle9i Database
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Oracle XML DB/(Oracle[\w]+ Enterprise Edition Release) (\d[-.\w]+) |s p/Oracle XML DB Enterprise Edition httpd/ v/$2/ i/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Oracle XML DB/Oracle Database\r\n|s p/Oracle XML DB Enterprise Edition httpd/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Oracle9iAS \((\d[-.\w]+)\) Containers for J2EE\r\n| p/Oracle 9iAS J2EE httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Oracle9iAS/(\d[-.\w]+) Oracle HTTP Server\r\n| p/Oracle 9iAS httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Oracle9iAS\r\n| p/Oracle 9iAS httpd/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nAllow: .*\r\nServer: Oracle9iAS-Web-Cache/(\d[-.\w]+)\r\n| p/Oracle 9iAS Web Cache/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Oracle9iAS/(\d[-.\w]+)  Lotus-Domino Oracle9iAS-Web-Cache/(\d[-.\w]+) |s p/Lotus Domino httpd/ i/Proxied by Oracle9iAS $1 Web Cache $2/
match http m|^HTTP/1\.1 401 Unauthorized.*\r\nWWW-Authenticate:.*\r\nDate:.*\r\nServer:Criston Precision Agent (\d[-_.\w]+)| p/Criston Precision Agent/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: ALT-N SecurityGateway ([0-9]+.[0-9]+.[0-9]+)| p/ALT-N SecurityGateway httpd/ v/$1/

match nimbud-netmon m|^nimbus/([\d.]+) \d+ \d+\r\nmtype| p/Nimsoft Nimbus network monitor/ v/$1/

# ntop - lots of submissions
match ntop-http m|^HTTP/1\.0 \d\d\d .*\nServer: ntop/(\d[-.\w]+) [^\r\n]*\([\w\d-]*linux[\w\d-]*\)\r?\n|s p/Ntop web interface/ v/$1/ o/Linux/
match ntop-http m|^HTTP/1\.0 \d\d\d .*\nServer: ntop/(\d[-.\w]+) \([\w\d.-]*freebsd[\w\d.-]*\)\r?\n|s p/Ntop web interface/ v/$1/ o/FreeBSD/
match ntop-http m|^HTTP/1\.0 \d\d\d .*\nServer: ntop/(\d[-.\w]+) \(([-.\w]+)\)\n|s p/Ntop web interface/ v/$1/ i/$2/
match ntop-http m|^HTTP/1\.0 \d\d\d .*\nServer: ntop/(\d[-.\w]+) \([^\)\r]+\)\r\n|s p/Ntop web interface/ v/$1/
match ntop-http m|^HTTP/1\.0 \d\d\d .*Server: ntop/([-\w_.]+)|s p/Ntop web interface/ v/$1/
match ntop-http m|^HTTP/1\.0 401 Unauthorized to access the document\nWWW-Authenticate: Basic realm=\"ntop HTTP server\"\n| p/Ntop web interface/
match ntop-http m|^HTTP/1\.0 \d\d\d .*Server: ntop/([\d.]+) SourceForge \.tgz \(([-\w_.]+)\)\r\n|s p/Ntop web interface/ v/$1 SourceForge .tgz/ i/platform $1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Apt-proxy (\d[-.\w]+)\r\n|s p/Debian Apt-proxy/ v/$1/
match http m|^HTTP/1\.0 404 NON-EXISTENT BACKEND\r\n\r\n$| p/Debian Apt-proxy/ i/Broken: no backend/
# This one is too general; I'm not including it -Doug
#match http m|^HTTP/1\.0 404 Not Found(\r\nConnection: close)?\r\n\r\n$| p/Debian Apt-proxy/

match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: mini_httpd/([\w._ /-]+)\r\n| p/mini_httpd/ v/$1/

# HP ProCurve Switch 2650 / Firmware revision H.07.32
match http m|^HTTP/1\.0 200 OK\r\nServer: eHTTP v([\w._-]+)\r\n.*<title> \n    HP ProCurve Switch ([-\w_.]+) \n|s p/eHTTP/ v/$1/ i/HP ProCurve Switch $2 http config/ d/switch/
match http m|^HTTP/1\.0 200 OK\r\nServer: eHTTP v([\w._-]+)\r\n.*<title> \n.*HP (\w+) ProCurve Switch ([-\w_.]+)\n    </title> \n|s p/eHTTP/ v/$1/ i/HP $2 ProCurve Switch $3 http config/ d/switch/
match http m|^HTTP/1\.0 200 OK\r\nServer: eHTTP v([\w._-]+)\r\n.*<title> \n.*- ProCurve (\w+) Switch ([-\w_.]+)\n    </title> \n|s p/eHTTP/ v/$1/ i/HP $2 ProCurve Switch $3 http config/ d/switch/
match http m|^HTTP/1\.0 200 OK\r\nServer: eHTTP v([\w._-]+)\r\n.*ProCurve Switch ([-\w_.]+) \(([\w]+)\)\n|s p/eHTTP/ v/$1/ i/HP ProCurve Switch $3 $2 http config/ d/switch/
match http m|^HTTP/1\.0 200 OK\r\nServer: eHTTP v([\w._-]+)\r\n.*<title>\n   \n      ProCurve Switch ([-\w_.]+) \(ProCurve (\w+)\)\n   </title>|s p/eHTTP/ v/$1/ i/HP ProCurve Switch $3 $2 http config/ d/switch/
match http m|^HTTP/1\.0 200 OK\r\nServer: eHTTP v([\w._-]+)\r\n.*<title>HP Virtual Stack</title>\n<!-- Changed by: Jon A\. LaRosa, 26-Apr-2000 -->\n|s p/eHTTP/ v/$1/ i/HP ProCurve Switch 2626 http config/ d/switch/
match http m|^HTTP/1\.0 200 OK\r\nServer: eHTTP v([\w._-]+)\r\n.*<title>\n +([\w._-]+)\n +- HP (\w+) ProCurve Switch ([\w-]+)\n   </title>|s p/eHTTP/ v/$1/ i/HP ProCurve Switch $3 $4 http config/ h/$2/
match http m|^HTTP/1\.0 200 OK\r\nServer: eHTTP v([\w._-]+)\r\n.*<title>\n   ([\w._-]+) - \n      ProCurve Switch ([\w._+/-]+) \((J\w+)\)\n   </title>|s p/eHTTP/ v/$1/ i/HP ProCurve Switch $3 http config; $4/ h/$2/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: eHTTP v(\d[\w._-]+)\r\n.*WWW-Authenticate: Basic realm=\"HP ([-.\w]+)\"\r\n\r\n|s p/eHTTP/ v/$1/ i/HP $2 http config/ d/switch/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: eHTTP v([\w._-]+)\r\n.*WWW-Authenticate: Basic realm=\"ProCurve (J\w+)\"\r\n\r\n|s p/eHTTP/ v/$1/ i/HP ProCurve Switch $2 http config/ d/switch/

match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Sun-ONE-Application-Server/(\d[-.\w]+)\r\n|s p/SunONE Application Server/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: SunONE WebServer (\d[-.\w]+)\r\n|s p/SunONE WebServer/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Sun-ONE-Web-Server/(\d[-.\w]+)\r\n|s p/SunONE WebServer/ v/$1/

match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: IBM_HTTP_Server/(\d[-.\w]+) +(Apache/)?(\d[-.\w]+) \(([^\r\n]+)\)\r\n|i p/IBM HTTP Server/ v/$1/ i/Derived from Apache $3; $4/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: IBM_HTTP_Server/(\d[-.\w]+) +(Apache/)?(\d[-.\w]+)\r\n|i p/IBM HTTP Server/ v/$1/ i/Derived from Apache $3/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: IBM_HTTP_SERVER/(\d[-.\w]+) +Apache/(\d[-.\w]+) \(Unix\) DAV/([\d.]+)\r\n| p/IBM HTTP Server/ v/$1/ i/Derived from Apache $2; DAV $3/ o/Unix/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: IBM_HTTP_SERVER/(\d[-.\w]+) +Apache/(\d[-.\w]+) \(Unix\) PHP/([\d.]+)\r\n| p/IBM HTTP Server/ v/$1/ i/Derived from Apache $2; PHP $3/ o/Unix/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: IBM_HTTP_SERVER/(\d[-.\w]+) +Apache/(\d[-.\w]+) \(Unix\) mod_jk\r\n| p/IBM HTTP Server/ v/$1/ i/Derived from Apache $2; using mod_jk/ o/Unix/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: IBM_HTTP_Server/(\d[-.\w]+) (Apache/.*)\r\n| p/IBM HTTP Server/ v/$1/ i/Derived from $2/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: IBM_HTTP_Server/(\d[-.\w]+) (Apache/.*) \(Win32\)\r\n|s p/IBM HTTP Server/ v/$1/ i/Derived from $2/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: IBM_HTTP_Server/(\d[-.\w]+) \(Win32\)\r\n|s p/IBM HTTP Server/ v/$1/ i/Derived from Apache/ o/Windows/ 
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: IBM_HTTP_Server/(\d[-.\w]+) \(Unix\)\r\n|s  p/IBM HTTP Server/ v/$1/ i/Derived from Apache/ o/Unix/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: IBM_HTTP_Server\r\n| p/IBM HTTP Server/ i/Derived from Apache/
match http m|^HTTP/1\.1 \d\d\d .*Server: IBM_HTTP_Server\r\n|s p/IBM HTTP Server/ i/Derived from Apache/


# D-Link DWL-1000AP webadmin
match http m|^HTTP/1\.0 200 OK\r\nServer: PSIWBL/(\d[-.\w]+)\r\nDate: .*Title: www\r\n\r\n<HTML>\n <HEAD>\n   <meta http-equiv=\"Refresh\" content=\"0; url=/startup/startup\.shtml\">\n </HEAD>\n <BODY>\n </BODY>\n</HTML>$|s i/D-Link http config/ p/PSIWBL/ v/$1/
# D-Link DWL-900AP+ WAP
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: Embedded HTTP Server (\d[-.\w]+) *\r\nWWW-Authenticate: Basic realm=\"(DWL-[-+.\w]+)\"\r\n| i/D-Link $2 http config/ p/Embedded HTTP Server/ v/$1/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: Embedded HTTP Server v(\d[-.\w]+)\r\nWWW-Authenticate: Basic realm=\"(DWL-[-+.\w]+)\"\r\nConnection: close\r\n\r\n| i/D-Link $2 http config/ p/Embedded HTTP Server/ v/$1/
match http m|^HTTP/1\.0 401 Unauthorized\r\n.*WWW-Authenticate: Basic realm=\"(DIR-\w+)\"\r\n|s i/D-Link $1 WAP http config/ d/WAP/
# D-Link DWL-1000AP Wireless Access Point
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: PSIWBL/(\d[-.\w]+)\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"Enter Password \(Leave User Name Empty\)\"\r\n| i/D-Link http config/ p/PSIWBL/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: WhatsUp_Gold/(\d[-.\w]+)\r\n| p/Ipswitch Whats Up Gold/ v/$1/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"(MR[-.\w]+)\"\r\nContent-Type: text/html\r\nServer: ZyXEL-RomPager/(\d[-.\w]+)\r\n\r\n| i|Netgear $1 WAP/router http config| p/ZyXEL-RomPager/ v/$2/ d/WAP/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"(R[PT][-.\w]+)\"\r\nContent-Type: text/html\r\nServer: ZyXEL-RomPager/(\d[-.\w]+)\r\n\r\n| i/Netgear $1 router http config/ p/ZyXEL-RomPager/ v/$2/ d/router/
# Netgear MR814 wireless router remote administration, Firmware 4.13 Aug 20 2003
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"(MR[-.+\w]+)\"\r\nServer: Embedded HTTPD v(\d[-.\w]+), (.*)\r\n| p/Netgear MR-series WAP http config/ i/$1; Embedded HTTPD $2, $3/ d/WAP/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"Prestige ([-.\w ]+)\"\r\nContent-Type: text/html\r\nServer: ZyXEL-RomPager/(\d[-.\w ]+)\r\n\r\n| p|ZyXEL Prestige webadmin| v|$2| i|Prestige model $1|
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"Prestige ([-.\w ]+)\"\r\nContent-Type: text/html\r\nServer: RomPager/(\d[-.\w ]+) ([-./\w]+)\r\n\r\n| p|ZyXEL Prestige webadmin| v|$2| i|Prestige model $1; $3|
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Roxen/(\d[-.\w]+)\r\n|s p/Roxen/ v/$1/
# A-link (Avaks) Hasbani Web Server on RoadRunner 44b ADSL Router
match http m|^HTTP/1\.1 403 Forbidden\r\nServer: WindWeb/(\d[-.\w]+)\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"Home Gateway\"\r\nContent-Type: text/html\r\n\r\nHasbani Web Server| p/A-link Hasbani webadmin/ i/Runs WindWeb $1 embedded httpd; Often a DSL router/ d/broadband router/
# Sambar Server V5.3 on Windows NT
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: SAMBAR ([\d.]+)\r\n| p/Sambar/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: SAMBAR\r\n| p/Sambar/
match http m|^HTTP/1\.1 .*\r\nDate: .*\r\nServer: aEGiS_nanoweb/(\d[-.\w]+) \(([^\)]+)\)\r\n| p/AEGiS Nanoweb httpd/ v/$1/ i/$2/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: WebLogic WebLogic Server (\d[-.\w]+( SP\d+)?) +\w\w\w|s p/WebLogic applications server/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: WebLogic ([\d.]+) Service Pack (\d+) [^\r\n]+\r\n|s p/WebLogic applications server/ v/$1/ i/Service Pack $2/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nDate: .*\r\nServer: WebLogic Server ([\d.]+ SP\d+) | p/WebLogic httpd/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nDate: .*<META NAME=\"GENERATOR\" CONTENT=\"WebLogic Server\">\n|s p/WebLogic httpd/
# Samba 3.0.0rc4-Debian
match http m|^HTTP/1\.0 401 Authorization Required\r\nWWW-Authenticate: Basic realm=\"SWAT\"\r\n| p/Samba SWAT administration server/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\nDate: .*\n<TITLE>Samba Web Administration Tool</TITLE>|s p/Samba SWAT administration server/
match http m|^HTTP/1\.0 \d\d\d .*\r\nConnection: close\r\nContent-Type: text/html\r\n\r\n<HTML><HEAD><TITLE>.*</TITLE></HEAD><BODY><H1>.*</H1>Samba is configured to deny access from this client\n<br>Check your \"hosts allow\" and \"hosts deny\" options in smb\.conf <p></BODY></HTML>\r\n\r\n$| p/Samba SWAT administration server/ i/Access denied/
match http m|^HTTP/1\.0 500 Server Error\r\nConnection: close\r\nContent-Type: text/html\r\n\r\n<HTML><HEAD><TITLE>500 Server Error</TITLE></HEAD><BODY><H1>500 Server Error</H1>chdir failed - the server is not configured correctly<p></BODY></HTML>\r\n\r\n| p/Samba SWAT administration server/ i/broken/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: icecast/(\d[-.\w]+)\r\n| p/Icecast streaming media server/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\n.*<html>\n<head>\n<meta http-equiv=\"Content-Type\" content=\"text/html; charset=UTF-8\">\n<title>Icecast for ([\w._-]+ \[Station\])</title>\n<link rel=\"stylesheet\" type=\"text/css\" href=\"style\.css\">|s p/Icecast streaming media server/ i/$1/
match http m|^HTTP/1\.0 \d\d\d [^\r\n]*\r\n.*<title>Icecast Streaming Media Server</title>\n|s p/Icecast streaming media server/
match http m%^HTTP/1\.1 200 OK\r\nContent-Type: (?:audio/mpeg|application/x-ogg)\r\nConnection: close\r\nPragma: no-cache\r\nCache-Control: no-cache, no-store\r\n\r\n% p/Music Player Daemon streaming media server/
match http m|^HTTP/1\.0 200 OK\r\nServer: HP-Web-Server-(\d[-.\w]+)\r\n.*<!-- framework\.ini ([A-Z]:\\[-.\w \\]+)-->|s p/HP Web Jetwebadmin/ v/$1/ i/framework.ini: $2/ o/Windows/
match http m|^HTTP/1\.0 200 OK\r\nServer: HP-Web-Server-(\d[-.\w]+)\r\n.*<!-- framework\.ini (/[\w\\/-_. ]+)-->|s p/HP Web Jetwebadmin/ v/$1/ i/framework.ini: $2/ o/Unix/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: HP Web Jetadmin (\d[-.\w]+)\r\n| p/HP Web Jetadmin print server http config/ v/$1/ d/print server/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: HP Web Jetadmin/(\d[-.\w]+) (.*)\r\n| p/HP Web Jetadmin print server http config/ v/$1/ i/$2/ d/print server/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: HP-Web-JetAdmin-(\d[-.\w]+)\r\n| p/HP Web Jetadmin print server http config/ v/$1/ d/print server/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Tomcat Web Server/(\d[-.\w ]+) \( ([^)]+) \)\r\n|s p/Apache Tomcat/ v/$1/ i/$2/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Tomcat Web Server/(\d[-.\w ]+)\r\n\r\n|s p/Apache Tomcat/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServlet-Engine: Tomcat Web Server/(\d[-.\w]+) \(([^\)]+)\)\r\n|s p/Apache Tomcat/ v/$1/ i/$2/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServlet-Engine: Tomcat Web Server/(\d[-.\w]+) \(([^\)]+)\) \(([^\)]+)\)\r\n|s p/Apache Tomcat/ v/$1/ i/$2; $3/
match 3dm-http m|^HTTP/1\.0 200 OK\r\nServer: 3ware/(\d[-.\w]+)\r\n.*<title>3ware 3DM - No remote access</title>|s p/3Ware 3DM Raid Daemon/ v/$1/ i/Access denied/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: publicfile|s p/publicfile httpd/
# http://xaxxon.slackworks.com/ehs/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Embedded HTTP Server ([\d.]+)\r\n| p/Embedded HTTP Server/ v/$1/

# APACHE
match http m|^HTTP/1\.[01].*?\r\nServer: Apache/(\d+\.\d+\.[-.\w]+) ([^\r\n]+)|s p/Apache httpd/ v/$1/ i/$2/
match http m|^HTTP/1\.[01].*Server: Apache/([\d\.\w-]+)\s*\r?\n|s p/Apache httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Apache/(\d[-.\w]+)\r\n.*X-Powered-By: ([^\r\n]+)\r\n|s p/Apache httpd/ v/$1/ i/$2/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Apache/(\d[-.\w]+)\r\n|s p/Apache httpd/ v/$1/
# apache 1.3.26-0woody3 or Apache 2.0.45
match http m|^HTTP/1\.[01] \d\d\d.*\r\nDate: .*\r\nServer: Apache\r\n| p/Apache httpd/
match http m|^HTTP/1\.[01] \d\d\d.*\r\nConnection: .*\r\nDate: .*\r\nServer: Apache\r\n| p/Apache httpd/
match http m|^HTTP/1\.[01] \d\d\d.*\r\nDate: .*\r\nServer: Apache +\(([^\r\n\)]+)\)\r\n| p/Apache httpd/ i/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Apache (\d+\.\d+\.[-.\w]+)\r\nX-Powered-By: ([^\r\n]+)\r\n| p/Apache httpd/ v/$1/ i/$2/
match http m|^HTTP/1\.[01] \d\d\d.*\r\nDate: .*\r\nServer: Apache-AdvancedExtranetServer/(\d[-.\w]+) \(Mandrake ?[Ll]inux/[-.\w]+\) (.*)\r\n| p/Apache Advanced Extranet Server httpd/ v/$1/ o/Linux/ i/$2/
match http m|^HTTP/1\.[01] \d\d\d.*\r\nDate: .*\r\nServer: Apache-AdvancedExtranetServer/(\d[-.\w]+) \(Mandrake ?[Ll]inux/[-.\w]+\)\r\n| p/Apache Advanced Extranet Server httpd/ v/$1/ o/Linux/
match http m|^HTTP/1\.[01] \d\d\d.*\r\nDate: .*\r\nServer: Apache-AdvancedExtranetServer/(\d[-.\w]+) \(Linux-Mandrake/[-.\w]+\)\r\n| p/Apache Advanced Extranet Server httpd/ v/$1/ o/Linux/
match http m|^HTTP/1\.[01] \d\d\d.*\r\nDate: .*\r\nServer: Apache-AdvancedExtranetServer/(\d[-.\w]+) \(Linux-Mandrake/[-.\w]+\) (.*)\r\n| p/Apache Advanced Extranet Server httpd/ v/$1/ i/$2/ o/Linux/
match http m|^HTTP/1\.[01] \d\d\d.*\r\nDate: .*\r\nServer: Apache-AdvancedExtranetServer/(\d[-.\w]+)\r\n| p/Apache Advanced Extranet Server httpd/ v/$1/ o/Linux/
match http m|^HTTP/1\.[01] \d\d\d.*\r\nDate: .*\r\nServer: Apache-AdvancedExtranetServer\r\n|s p/Apache Advanced Extranet Server httpd/ o/Linux/
match http m|^HTTP/1\.[01] \d\d\d.*\r\nDate: .*\r\nServer: ?(.*) Apache-AdvancedExtranetServer/(\d[-.\w]+) \(Mandrakelinux/[-.\w]+\) ?(.*)\r\n| p/Apache Advanced Extranet Server httpd/ v/$2/ i/$1 $3/ o/Linux/
match http m|^HTTP/1\.[01] \d\d\d.*\r\nDate: .*\r\nServer: Apache-AdvancedExtranetServer/(\d[-.\w]+) \(Mandriva Linux/PREFORK-([-\w_.]+)\) (.*)\r\n| p/Apache Advanced Extranet Server httpd/ v/$1/ i/Mandriva $2; $3/ o/Linux/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Apache-AdvancedExtranetServer/([\d.]+) \(Mandrakelinux/PREFORK-([-\w_.]+)\) ?([^\r\n]*)\r\n|s p/Apache Advanced Extranet Server httpd/ v/$1/ i/Mandrake $2; $3/ o/Linux/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Apache Tomcat/(\d[-.\w]+)|s p/Apache Tomcat/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d.*\r\nServer: Apache[- ]Coyote/(\d[-\d.]+)\r\n.*/Tomcat-(\d[-\d.]+)\r\n|s p|Apache Tomcat/Coyote JSP engine| v|$1| i|Tomcat $2| 
match http m|^HTTP/1\.[01] \d\d\d.*\r\nServer: Apache[- ]Coyote/(\d[-\d.]+)\r\n|s p|Apache Tomcat/Coyote JSP engine| v|$1|
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Apache/([\w._-]+) Ben-SSL/([\w._-]+) \(Unix\)\r\n|s p/Apache httpd/ v/$1/ i/Ben-SSL $1/ o/Unix/

# Place hard matched Apache banners above this line
softmatch http m|^HTTP/1\.[01] \d\d\d.*\r\nDate: .*\r\nServer: Apache ([^\r\n]+)\r\n| p/Apache httpd/ i/$1/

# Apache Stronghold
match http m|^HTTP/1\.[01] \d\d\d.*\r\nDate:.*\r\nServer: Stronghold/([-.\w]+) Apache/([-.\w]+)| p/Apache Stronghold httpd/ v/$1/ i/based on Apache $2/
softmatch http m|^HTTP/1\.[01] \d\d\d.*\r\nDate:.*\r\nServer: Stronghold| p/Apache Stronghold httpd/  i/based on Apache/


match http m|^HTTP/1\.[01] \d\d\d [^\r\n]*\r\n.*Server: nginx\r\n| p/nginx/
match http m!^HTTP/1\.[01] \d\d\d [^\r\n]*\r\n.*Server: nginx/([\d.]+)\r\n!s p/nginx/ v/$1/
match http m!^HTTP/1\.[01] \d\d\d [^\r\n]*\r\n.*Server: nginx/([\d.]+) \+ ([^\r\n]*)\r\n!s p/nginx/ v/$1/ i/$2/

# Citrix NFuse 2.0 on MS IIS 5.0
match http m|^HTTP/1\.[01].*\r\nServer: Microsoft-IIS/([-.\w]+)\r\n.*\r\nContent-Location: http://[^/]+/nfuse.htm\r\n.*\r\n---- NFuse ([-.\w]+) \(Build |s p/Citrix NFuse/ v/$2/ i/Microsoft IIS $1/ o/Windows/
match http m|^HTTP/1\.[01].*\r\nServer: Microsoft-IIS/([-.\w]+)\r\n|s p/Microsoft IIS httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 200 OK\r\nDate: .+\r\nServer: Tomcat/([-.\w]+)\r\nContent-Type: text/html\r\nContent-Length: \d+\r\nServlet-Engine: Tomcat/[-.\w]+ \(Java ([-.\w]+); SunOS ([-.\w]+) (\w+); java\.vendor=Sun Microsystems Inc\.\)\r\n| p/Solaris management console server/ i/Java $2; Tomcat $1; SunOS $3 $4/ o/SunOS/
match http m|^HTTP/1\.[01] 200 OK\r\n.*Server: CommuniGatePro/([-.\w ]+)\r\n|s p/CommuniGate Pro httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: DSS ([-.\w]+) Admin Server/([-.\w]+)|s p/DarwinStreamingServer/ v/$1/ i/Admin Server $2/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: QTSS (\d[-.\w]+) Admin Server/(\d[-.\w]+)\r\n| p/Apple QTSS Admin Server/ v/$2/ i/from QTSS $2/
match http m|^HTTP/1\.0 200 OK\r\nServer: fnord/(\d[-.\w]+)\r\n| p/Fnord httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Fnord\r\n| p/Fnord httpd/
match http m#^HTTP/1\.0 404 Not Found\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<title>Not Found</title>(?:This host is not served here\.|No such file or directory\.)$# p/Fnord httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: MiniServ/([\d.]+)\r\n|s p/MiniServ/ v/$1/ i/Webmin httpd/
match http m|^HTTP/1.1 200 OK\r\nServer: NetWare-Enterprise-Web-Server/([-.\w]+)\r\n| p/Novell NetWare enterprise web server/ v/$1/ o/NetWare/
match http m|^HTTP/1.1 302 Object Moved Temporarily\r\nServer: NetWare HTTP Stack\r\n| p/Novell NetWare HTTP Stack/ i/HTTPSTK.NLM/ o/NetWare/
match http m|^HTTP/1.1 \d\d\d [\w ]+\r\nServer: NetWare HTTP Stack\r\n| p/Novell NetWare HTTP Stack/ i/HTTPSTK.NLM/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: HTTPd-WASD/([-.\w]+) OpenVMS/(.*)\r\n| p|WASD httpd| v|$1| i|$2| o/OpenVMS/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: HTTPd-WASD/([-.\w]+) OpenVMS/(.*)\r\n| p|WASD httpd| v|$1| i|$2| o/OpenVMS/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Lotus-Domino/Release-(\d[-.\w]+)\r\n|s p/Lotus Domino httpd/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Lotus-Domino/Release-(\d[-.\w]+)\(Intl\)\r\n|s p/Lotus Domino International httpd/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Lotus-Domino/Release\r\n|s p/Lotus Domino httpd/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Lotus-Domino/(\d[-.\w]+)\r\n|s p/Lotus Domino httpd/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Lotus-Domino(/0)?\r\n|s p/Lotus Domino httpd/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Domino-Go-Webserver/([\d.]+)\r\n|s p/Lotus Domino Go httpd/ v/$1/

# G-Net BB0060 ADSL Modem (I'm not sure this is GlobespanVirata, but that is
# what the t3lnetd on this device said).
match http m|^HTTP/1.1 302 Document Follows\r\nLocation: /hag/pages/home.ssi\r\n\r\n$| p/GlobespanVirata httpd/ i/on broadband router/
match http m|^HTTP/1.0 200 OK\r\nServer:HTTP/1.0\r\n.*<title>Hewlett Packard</title>|s p/HP Jetdirect httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: EHTTP/([\d.]+)\r\nPragma:no-cache\r\nContent-Type:text/html\r\n\r\n<html> \n<head>\n<title> \n(.*) \n- HP (J\w+) ProCurve Switch (\w+)\n</title>| p/HP $3 Procurve Switch $4 http config/ i/EHTTPd $1; Name $2/ d/switch/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: EHTTP/([.\d]+)\r\nWWW-Authenticate: Basic realm=\"HP ([-.\w]+)\"\r\n| p/HP switch EHTTP admin server/ v/$1/ i/HP $2 switch/ d/switch/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Virata-EmWeb/([-.\w]+)\r\n.*\r\n\r\n\n<!--\nFile name: index\.html\n\nThis is the 'parent' file that calls the individual child frames\. \nThis is the file that is first accessed when the user types http://<ipaddress> \nin the browser toolbar\. \n\nThe UI Architecture consists of a total of 4 frames\. This file calls 3 high-level |s i/HP LaserJet printer webadmin/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/printer/
match http m|^HTTP/1\.0 \d{3} .*\r\nServer: CompaqHTTPServer/([.\w\d]+)\r\n|s p/Compaq Insight Manager HTTP server/ v/$1/
match http m|^HTTP/1\.1 401 Authorization Required\r\nWWW-Authenticate: Basic realm="Linksys ([-.A-Z\d/ ]+)"\r\n| p/Linksys router http config/ i/device model $1/ d/WAP/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: httpd\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"Dell TrueMobile ([\d.]+) Wireless Broadband Router\"\r\n| p/Dell TrueMobile $1 wireless router http config/ d/WAP/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: httpd\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"Linksys WAP54G\"\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n| p/Linksys WAP54G wireless-G router http config/ d/WAP/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: httpd\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"(WRT[-\w]+)\"\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n| p/Linksys $1 wireless-G router http config/ d/WAP/
match http m|^HTTP/1\.0 401 Unauthorized\nContent-type: text/html\r\nDate: .*\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"(WRT[^"]+)\"\r\n\r\n<HEAD><TITLE>401 Unauthorized</TITLE></HEAD>\n<BODY><H1>401 Unauthorized</H1>\n\n</BODY>\n| p/Linksys $1 wireless-G router http config/ d/WAP/
match http m|^HTTP/1\.0 401 Not Authorized\r\nServer: RapidLogic/([\d.]+)\r\nMIME-version: 1\.0\r\nPragma: no-cache\r\nContent-type: text/html\r\nWWW-Authenticate: Basic realm=\"Linksys WRT55AG\"\r\n\r\n\r\nAuthorization Required\r\n\r\n| i/Linksys WRT55AG WAP http config/ p/RapidLogic/ v/$1/ d/WAP/
match http m|^HTTP/1\.1 401 Not Authorized\r\nServer: Rapid Logic/([\d.]+)\r\n.*WWW-Authenticate: Basic realm=\"([^"]*)\"\r\n|s i/Linksys $2 WAP http config/ p/RapidLogic/ v/$1/ d/WAP/
match http m|^HTTP/1\.[01] 401 Unauthorized\r\nWWW-Authenticate: Basic realm="MET-(\w+)"\r\n| p/Linksys $1 http config/ d/router/
# Notice the spelling mistake in the HTML
match http m|^HTTP/1\.0 401 Bad Request\r\nServer: httpd\r\nDate: .*\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<HTML><HEAD><TITLE>401 Bad Request</TITLE></HEAD>\n<BODY BGCOLOR=\"#cc9999\"><H4>401 Bad Request</H4>\nCann't use wireless interface to access web\.\n</BODY></HTML>\n| p/Linksys WRT54G WAP http config/ d/WAP/ i/Wireless admin disabled/
match http m|^<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.0 Transitional//EN\">\r\n<HTML><HEAD><TITLE>Bad Request</TITLE>.*<H4>401 Bad Request</H4>Cann't use wireless interface to access web\.\";|s p/Linksys WRT54G WAP http config/ d/WAP/ i/Wireless admin disabled/
match http m|^HTTP/1\.0 200 Ok\r\nServer: httpd\r\nDate:.*\n\t\t<title>(WRT54\w+) - Info</title>|s p/DD-WRT milli_httpd/ i/Linksys $1 WAP http config/ o/Linux/ d/WAP/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: \r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"Linksys WRT300N\"\r\n| p/Linksys WRT300N WAP http config/ d/WAP/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: httpd\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"Shared Storage Drive\"\r\n| p/Maxtor Shared Storage NAS http config/ d/storage-misc/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: httpd\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"NETWORK HDD\"\r\n| p/Argosy Research HD363N Network HDD http config/ d/storage-misc/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: httpd\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"SimpleShare \(default user name is admin and password is simple\)\"\r\n| p/SimpleShare WAP http config/ d/WAP/

# This might be too general, but this is probably the most common device
# this will match. I'm leaving it -Doug
# Also matches Mapower KC31N NAS device http config.
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: httpd\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"([^"]+)\"\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n| p/Linksys wireless-G WAP http config/ i/Name $1/ d/WAP/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Insight Manager (\d)\r\n\r\n|s p/Compaq Insight Manager/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\nContent-Length: \d+\r\nConnection: close\r\nPragma: no-cache\r\nCache-Control: no-cache, no-store, must-revalidate\r\nExpires: 0\r\nContent-Type: text/html\r\n\r\n| p/GNU Httptunnel/
# Blue Coat Port 80 Security Appliance Model: Blue Coat SG400 Software Version: SGOS 2.1.6044 Software Release id: 19480 Service Pack 4
match http m|^HTTP/1\.0 301 Moved Permanently\r\nLocation: /Secure/Local/console/index\.htm\r\n\r\n$| p/Blue Coat Security Appliance HTTP admin interface/ o/SGOS/
match http m|^HTTP/1\.1 401 Authentication Required\r\nWWW-Authenticate: Basic realm=\"[\d.]+\"\r\nRefresh: 0;URL=\"/Secure/Local/console/logout\.htm\"\r\nServer: BlueCoat-Security-Appliance\r\n| p/Blue Coat SG210 http proxy config/ o/SGOS/ d/proxy server/
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: AkamaiGHost\r\n| p|AkamaiGHost| i|Akamai's HTTP Acceleration/Mirror service|
match http m|^HTTP/1\.0 \d\d\d .*\r\n.*Server: Netscape-Enterprise/([-. \w]+)\r\n|s p/Netscape Enterprise httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\n.*Server: Netscape-Enterprise/([-. \w]+)\r\n|s p/Netscape Enterprise httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r?\nDate: .*\r?\nServer: NCSA/(([\d.]+))\r?\n| p/NCSA httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Netscape-FastTrack/(\d[-.\w]+)\r\n| p/Netscape FastTrack web server/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: (Oracle[-.\w/]+) Oracle HTTP Server ([-.\w]+)|s p/Oracle HTTP Server/ v/$1/ i/$2/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Oracle HTTP Server Powered by Apache\r\n|s p/Oracle HTTP Server Powered by Apache/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Oracle HTTP Server Powered by Apache/([-.\w]+)\r\n|s p/Oracle HTTP Server Powered by Apache/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Oracle HTTP Server Powered by Apache/([-.\w]+) \(Win32\) ([^\r\n]+)\r\n|s p/Oracle HTTP Server Powered by Apache/ v/$1/ i/$2/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Oracle HTTP Server Powered by Apache/([-.\w]+) \(Unix\) ([^\r\n]+)\r\n|s p/Oracle HTTP Server Powered by Apache/ v/$1/ i/$2/ o/Unix/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: Embedded HTTP Server (\d[.\d]+)\r\nWWW-Authenticate: Basic realm=\"([-+.\w]+)\"\r\nConnection:| p/D-Link http config/ v/$1/ i/on D-Link $2/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\n.*Pragma: no-cache\r\nServer: Allegro-Software-RomPager/ ?([\w.]+)\r\n\r\n<HTML><head>\n<META HTTP-EQUIV=\"Content-Type\" CONTENT=\"text/html; charset=iso-8859-1\">\n<TITLE></TITLE></HEAD><frameset framespacing=\"0\" BORDER=\"false\" frameborder=\"0\" rows=\"90,\*\">\n  <frame NAME=\"fLogo\" scrolling=\"no\" noresize src=\"/html/Hlogo\.html\"|s p/D-Link DSL-300g or g+ http config/ i/Allegro RomPager $1/ d/broadband router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: \r\n.*WWW-Authenticate: Basic realm=\"Please enter your user name and password on DSL-([\w+]+)\"\r\n\r\n|s p/D-Link DSL-$1 http config/ d/broadband router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: \r\n.*WWW-Authenticate: Basic realm=\"DSL-([\w+]+) Admin Login\"\r\n\r\n|s p/D-Link DSL-$1 http config/ d/broadband router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"IntelEmbeddedWeb@Express460T\"\r\nContent-Type: text/html\r\nServer: Allegro-Software-RomPager/([\w.]+)\r\n| p/Intel 460T Standalone Switch/ i/Allegro RomPager $1/
# Some D-Link Switches
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\n.*Server: Allegro-Software-RomPager/ ?([\w.]+)\r\n\r\n.*DES-(\d+) Web Management|s p/D-Link DES-$2 switch http config/ i/Allegro RomPager $1/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\n.*Server: Allegro-Software-RomPager/ ?([\w.]+)\r\n\r\n.*<TITLE>.*?(DES-\d+).*?</TITLE>|s p/D-Link $2 Switch http config/ i/Allegro RomPager $1/

# iCal 3.6
match http m|^HTTP/1\.1 200 OK\r\n.*Server: Wapapi/([\w._-]+)\r\nContent-Type: text/html\r\nContent-Length: \d+\r\n\r\n<html>\r\n<head><title>iCal Tutorial:  Introduction</title></head>|s p/Wapapi/ v/$1/ i/Brown Bear iCal web calendar/

match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Virata-EmWeb/R([\w_]+)\r\nWWW-Authenticate: Basic realm=\"Administration Tools\"\r\n\r\n401 Unauthorized\r\n$| i/Netscreen administrative web server/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/firewall/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Virata-EmWeb/R([\w_]+)\r\nContent-Type: text/html\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n\r\n.*<link rel=\"SHORTCUT ICON\" href=\"/favicon\.ico\">\n\n<title>Login</title>|s i/Netscreen administrative web server/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/firewall/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*\r\nServer: Web/R([\w_]+)\r\n.*Content-Type: text/html\r\n.*\r\n\r\n<html>\n<head>\n\n<script language=\"javascript\">\n|s i/Netscreen administrative web server/ p/Web/ v/$SUBST(1,"_",".")/ d/firewall/

# Phaser860 Printer
match http m|^HTTP/1\.1 404 Not Found\r\nDate: .*\r\nAllow: GET, HEAD\r\nServer: Spyglass_MicroServer/(\d[-.\w]+)\r\nContent-Type: text/html\r\nContent-Length: \d+\r\n\r\n<HTML><HEAD><TITLE>Not Found</TITLE></HEAD>\r\n<BODY>The requested URL was not found\.</BODY></HTML>\r\n| p/Spyglass MicroServer/ v/$1/ d/printer/
# Cisco Catalyst 3500-XL switch IOS 12.0(5)XU
match http m|^HTTP/1\.0 401 Unauthorized\r\nDate: .*\r\nContent-[Tt]ype: text/html\r\nExpires: .*\r\nWWW-Authenticate: Basic realm=\"level 15 access\"\r\n| p/Cisco IOS http config/ d/switch/ o/IOS/
# Cisco 828 G.SHDSL
match http m|^HTTP/1\.0 200 OK\r\nDate: .*\r\nServer: cisco-IOS/(\d[-.\w ]+) HTTP-server/(\d[-().\w ]+)\r\n| p/Cisco IOS http config/ v/$2/ i/IOS $1/ o/IOS/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nDate: .*\r\nServer: cisco-IOS\r\n| p/Cisco IOS http config/ o/IOS/
match http m|^HTTP/1\.0 200 OK \nServer: cisco-IOS Technologies/([\w._-]+) HTTP-server\n| p/Cisco IOS http config/ o/IOS/
# Xerox Document Centre (DocuCentre) 425
match http m|^HTTP/1\.1 200 OK\r\nContent-Length: \d+\r\nContent-Type: text/html\r\nDate: .*\r\nAllow: GET, HEAD\r\nServer: Xerox_MicroServer/([-.\w]+)\r\nExpires: .*\r\nCache-Control: no-cache\r\n\r\n<HTML>\n<HEAD>\n<TITLE>([-.+ \w]+)</TITLE>| p/Xerox MicroServer httpd/ v/$1/ i/on $2/
match http m|^HTTP/1\.1 200 OK\r\nContent-Length: \d+\r\nContent-Type: text/html\r\nDate: .*\r\nAllow: GET, HEAD\r\nServer: Xerox_MicroServer/([-.\w]+)\r\n| p|Xerox MicroServer httpd| v|$1| i|usually a printer/copier|
match http m|^HTTP/1\.1 200 OK\r\n.*<!-- Copyright \(c\) \d+-\d+, Fuji Xerox Co\., Ltd\. All Rights Reserved\. -->.*<TITLE>\r\n(Document Centre \w+) - [\d.]+\r\n</TITLE>|s p/FujiXerox $1 http config/ d/printer/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\nDate: .*\r\nAllow: GET, HEAD\r\nServer: Spyglass_MicroServer/(\d[-.\w]+)\r\nLast-Modified: .*\r\nExpires: .*\r\nPragma: no-cache\r\n\r\n\n<html> \n<head>\n   <meta http-equiv=\"Content-Type\" content=\"text/html; charset=iso-8859-1\">\n   <meta name=\"keywords\" content=\"printer; embedded web server; int| p/Spyglass MicroServer/ v/$1/ i/embedded in printer/ d/printer/
match http m|^HTTP/1\.0 500 Internal Server Error\r\nServer: Cougar (\d[-.\w]+)\r\n\r\n$| p/Microsoft Windows Media Server/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: video/x-ms-asf\r\nCache-Control: max-age=0, no-cache\r\nServer: Cougar/(\d[-.\w]+)\r\n| p/Microsoft Windows Media Server/ v/$1/ o/Windows/
match http m|^HTTP/1\.[01] \d\d\d .*Server: NetApp/(\d[-.\w]+)\r\n|s p/NetApp filer httpd/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/(\d[.\d]+)\r\nMIME-version: 1\.0\r\nContent-type: text/html\r\n\r\n<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.0 Frameset//EN\"\r\n\t\t\t\"http://www\.w3\.org/TR/REC-html40/frameset\.dtd\">\r\n<HTML>\r\n<HEAD>\r\n\t<TITLE>Netopia Router Web </TITLE>| p/Netopia RapidLogic admin server/ v/$1/ d/router/
match http m|^HTTP/1\.1 200 OK\r\nServer: WebSTAR/(\d[-.()\w]+) ID/| p/WebSTAR httpd/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*\r\nServer: 4D_WebSTAR_S/([\d.]+) \(MacOS X\)\r\n| p/WebSTAR httpd/ v/$1/ o/Mac OS X/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: Agranat-EmWeb/R([\w_]+)\r\nWWW-Authenticate: Basic realm=\"accessPoint\"\r\n\r\n401 Unauthorized\r\n$| i/Orinoco AP-200 webadmin/ p/Agranat-EmWeb/ v/$SUBST(1,"_",".")/
match http m|^HTTP/1\.0 404 NO_STREAM_FOUND\r\nConnection: close\r\n\r\n$| p/Chain Cast P2P streaming service/
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: Rex/(9\.0\.0\.\d+)\r\n| p|Chain Cast support service| v|Rex/$1|
match http m|^HTTP/1\.0 401 Unauthorized\r\nDate: .*\r\nServer: Boa/(\d[-.\w]+) \(with Intersil Extensions\)\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"WG602 v2\"\r\n| i/Netgear WG602v2 wireless router http config/ p/Boa httpd/ v/$1 (with Intersil Extensions)/ d/router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nDate: .*\r\nServer: Boa/(\d[-.\w]+) \(with Intersil Extensions\)\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"LOGIN Enter Password \(default is medion, ignore username\)\"\r\n| i/Medion router http config/ p/Boa httpd/ v/$1 (with Intersil Extensions)/ d/router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nDate: .*\r\nServer: Boa/(\d[-\w_.]+) \(with Intersil Extensions\)\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"Enter Password \(Leave User Name Empty\)\"\r\n| p/CN3000 WAP http config/ i/Boa httpd $1 (with Intersil Extensions)/ d/WAP/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: Boa/([-\w_.]+)\r\nWWW-Authenticate: Basic realm=\"Broadband Router\"\r\n| p/Arescom NetDSL ADSL router http config/ i/Boa httpd $1/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: Boa/(\d[-.\w]+)\r\n| p/Boa HTTPd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: (\d[-.\w]+)\r\n.*<title>GNUMP3d |s p/GNUMP3d streaming server/ v/$1/

match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Jetty\((\d[-.\w]+)\)\r\n\r\n<html>\n  <head><title>Wildfire HTTP Binding Service</title></head>|s p/Jetty httpd/ v/$1/ i/Wildfire HTTP Bindings/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Jetty\((\d[-.\w]+)\)\r\n\r\n.*Contexts known to this server are: <ul><li><a href=\"/ninan/\">/ninan|s p/Ninan usenet downloader http interface/ i/Jetty $1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nDate: .*\r\nServer: Jetty/(\d[-.\w]+) \(([^)\r\n]+)\)?\r\n| p/Jetty httpd/ v/$1/ i/$2/
match http m|^HTTP/1\.[01] .*\r\nServer: Jetty\(([\w._-]+)\)\r\n|s p/Jetty httpd/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: MortBay-Jetty-([-\w_.]+)\r\n|s p/Jetty httpd/ v/$1/
match http m|^HTTP/1\.1 404 Not Found\r\nContent-Type: text/html\r\nContent-Length: \d+\r\n\r\n<HTML>\n<HEAD>\n<TITLE>Error 404 - Not Found</TITLE>\n<BODY>\n<H2>Error 404 - Not Found\.</H2>\nNo context on this server matched or handled this request\.| p/Jetty httpd/

match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: WebSphere Application Server/([-\w_.]+)\r\n|s p/IBM WebSphere Application Server/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: JRun Web Server/([\d.]+)\r\n|s p/JRun Web Server/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: JRun Web Server\r\n|s p/JRun Web Server/
match http m|^401 Access denied\r\nWWW-Authenticate: Negotiate \r\nContent-length: 0\r\n\r\n| p/Microsoft IIS 5.0 WebDAV/ i/access denied/ o/Windows/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: RomPager/([-.\w/ ]+)\r\n|s p/Allegro RomPager/ v/$1/ i/ZyXEL ZyWALL 2/

match http m|^HTTP/1\.0 200 OK\r\nServer: (Gordian Embedded\d\.\d)\r\n.*<title>IQeye3 (\w+):|s p/IQinVision IQeye3 httpd/ i/$1/ d/webcam/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: IDSL MailGate (\d[-.\w]+)\r\n| p/MailGate web proxy/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*<TITLE>The AXIS 200 Home|s p/AXIS 200/ d/webcam/
# A couple little easter eggs! -Doug (who else?)
match http m|^HTTP/1\.1 \d\d\d .*\nServer: Anti-Web V([\d.]+) \([\w .-]+\)\n| p/Anti-Web httpd/ v/$1/ i/Best httpd out there!/
match http m|^HTTP/1\.1 \d\d\d .*\nServer: Anti-Web HTTPD V([\d.]+) \([\w .-]+\)\n| p/Anti-Web httpd/ v/$1/ i/Best httpd out there!/
match http m|^HTTP/1\.1 400 Bad Request\r?\nServer: Antiweb/([\w._-]+)\r?\n| p/Antiweb/ v/$1/ i/Best httpd out there!/ o/Unix/
match http m|^HTTP/1\.0 200 OK\r\nServer: ArGoSoft Mail Server Pro for WinNT/2000/XP, Version [\d.]+ \(([\d.]+)\)\r\n| p/ArGoSoft Mail Server Pro httpd/ v/$1/ o/Windows/
# Lantronix ThinWeb Manager
match http m|^HTTP/1\.0 200 OK\r\nServer: Gordian Embedded([\d.]+)\r\nContent-type: text/html\r\n.*\r\n\r\n\n<HTML>\n<HEAD>\n<TITLE>Lantronix ThinWeb Manager ([\d.]+): Home</TITLE>\n|s p/Lantronix ThinWeb Manager/ v/$2/ i/Gordian Embedded $1/
match http m|^HTTP/1\.1 302 Found\r\nDate: .*\r\nLocation: /iw/webdesk/login/\r\nX-Cache: MISS from .*\r\nConnection: close\r\nContent-Type: text/html\r\n\r\n| p/Interwoven TeamSite/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*\r\nServer: OpenSA/([\d.]+) / Apache/([\d.]+) \((\w*)\) mod_ssl/([\d.]+) OpenSSL/([\d.]+)\r\n.*<LINK REL=\"SHORTCUT ICON\" HREF=\"http://([\w.-_]+)/iss\.ico\">\r\n<TITLE> System Scanner Vista Welcome Page </TITLE>\r\n|s p/ISS System Scanner Vista/ i|OpenSA/$1 Apache/$2 mod_ssl/$4 OpenSSL/$5| o/$3/ h/$6/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*\r\nServer: OpenSA/([\d.]+) / Apache/([\d.]+) \(Win32\) ([^\r\n]+)\r\n| p/OpenSA httpd/ v/$1/ i/Apache $2; $3/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: BaseHTTP/([\d.]+) Python/([\w.]+) edna/([\d.]+)\r\n| p/BaseHTTP/ v/$1/ i/Edna Streaming MP3 Server $3; Python $2/
match http m|^HTTP/1\.1 404 Path not found: /\r\nServer: BaseHTTP/([\d.]+) Python/([\w.]+)\r\n.*Content-Length: 198\r\n\r\n<head>\n<title>Error response</title>\n</head>\n<body>\n<h1>Error response</h1>\n<p>Error code 404\.\n<p>Message: Path not found: /\.\n<p>Error code explanation: 404 = Nothing matches the given URI\.\n</body>\n$|s p/BaseHTTP/ v/$1/ i/Open ERP XML-RPC/
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: Speed Touch WebServer/([\d.]+)\r\nContent-type: text/html\r\nContent-length: \d*\r\n\r\nHTTP/1\.0 400 Bad Request\r\n: Invalid or incomplete request\.\r\n\r\n| p/Alcatel Speedtouch ADSL router httpd/ v/$1/ d/router/
# Management Interface for Netscape FastTrack web server 2.01
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Netscape-Administrator/([\d.]+)\r\n| p/Netscape FastTrack Administrator/ v/$1/
# Siemens SpeedStream 2-port SS2601 Router
match http m|^HTTP/1\.1 \d\d\d .*\r\nWWW-Authenticate: Basic realm=\"InterMapper\"\r\n.*\r\nServer: InterMapper/([\d.]+)\r\n|s p/InterMapper Network Monitor httpd/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\n.*\r\nServer: ZOT-PS-13/([\d.]+)\r\n|s p/Hawking Print Server httpd/ v/$1/ d/print server/
match http m|^HTTP/1\.0 200 OK.*\r\nServer: ZOT-PS-11/([\d.]+)\r\n.*\n<head><!-- Simon Hung, Zero One Tech\. 98/8 -->\n|s p/3P print server http config/ i/ZOT-PS-11 $1/ d/print server/
match http m|^HTTP/1\.0 401 Unauthorized\r\n.*\r\nServer: (ZOT-PS-[\d]+/[\d.]+)\r\n|s p/print server http config/ v/$1/ d/print server/
match http m|^HTTP/1\.0 302 Temporarily Moved\nLocation: /winamp\?page=main\nConnection: close\nContent-type: text/html\n\n<html>\n<head>\n<title>Winamp Web Interface</title>| p/Winamp Web Interface/
match http m|^HTTP/1\.[01] \d\d\d .*Server: Lasso/([\d.]+)\r\n\r\n|s p/Lasso httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: BaseHTTP/([\d.]+) Python/([\w.]+)\r\nDate: .*<title>Roundup trackers index</title></head>\n<body><h1>Roundup trackers index</h1>|s p/BaseHTTP/ v/$1/ i/Roundup issue tracker; Python $2/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: BaseHTTP/([\d.]+) Python/([\w.]+)\r\n.*<title>Ajaxterm</title>|s p/BaseHTTPd/ v/$1/ i/Ajaxterm; Python $2/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: fwlogwatch[ /]([\d.]+) 200\d/\d\d/\d\d \(C\) Boris Wesslowski| p/fwlogwatch/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nConnection: close\r\nServer: GNUMP3d ([-\w_.]+)\r\n| p/GNUMP3d streaming server/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nConnection: close\r\nServer: ([\d.]+)\r\nContent-type: text/html; charset=utf-8\r\nSet-Cookie: theme=Tabular;path=/; expires=.*;\r\nConnection: close\r\n\r\n| p/GNUMP3d/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*\r\nServer: HTTP/x\.y\.z \(Unix\) PHP/x\.y\.z mod_ssl/x\.y\.z SSL/x\.y\.z\r\nLast-Modified: .*\r\nETag: \".*\"\r\nAccept-Ranges: bytes\r\nContent-Length: .*\r\nConnection: close\r\nContent-Type: text/html\r\n\r\n<HTML>\n<HEAD>\n<TITLE>Loading\.\.\.</TITLE>\n| p/Coldfusion httpd/ i/SSL support/ o/Unix/
match http m|^HTTP/1\.0 200 OK\r\nContent-Length: \d+\r\nContent-Type: text/html\r\nServer: SIMS/([\w.]+)\r\n\r\n<HTML>\r<HEAD>\r  <TITLE>Stalker Internet Mail Server: Setup Entrance</TITLE>\r</HEAD>\r<BODY BGCOLOR=white>\r\r<H2><TABLE WIDTH=\"100%\" BORDER=0 CELLSPACING=0 CELLPADDING=0>\r<TR>\r<TD><H3><IMG SRC=\"/Icon\.gif\" ALIGN=MIDDLE>([-\w_.]+)</H3>| p/Stalker Mail Server web config/ v/$1/ h/$2/ o/Mac OS/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Apache  -OOPS Development Organization-\r\n.*X-Powered-By: ([^\r\n]+)\r\n|s p/Apache - OOPS Devel Org/ i/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Apache  -OOPS Development Organization-\r\n|s p/Apache - OOPS Devel Org/ i/$1/
match http m|^HTTP/1\.0 200 OK\nDATE: .*\nPragma: no-cache\nServer: Delta UPSentry\n| p/Sentry Bulldog UPS httpd/
match http m|^HTTP/1\.[01] \d\d\d .*Server: Gatling/([\d.]+)\r\n|s p/Gatling httpd/ v/$1/
# PolyCom ViewStation 128
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Viavideo-Web\r\n|s p/Polycom ViewStation/ d/webcam/
match http m|^HTTP/1\.0 \d\d\d .*\nDate: .*\nMIME-version: [\d.]+\nServer: Micro-HTTP/([\d.]+)\nContent-type: text/html\n.*Copyright Tektronix, Inc\.|s p/Tektronix printer httpd/ d/printer/ i|Micro-HTTP/$1|
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: IBM HTTP Server/([\w]+)\r\n| p/IBM httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: SAlive/ ([\d.]+)\r\n|s p/Servers Alive network monitor/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type:text/html\r\nContent-Length:\d+\r\n\n\n<HTML>\n<HEAD>\n<TITLE>Not Supported</TITLE>\n</HEAD>\n<body>\n\n<H1 ALIGN=CENTER>The Command sent is not Supported</H1>\n\n\n</BODY>\n</HTML>\n\n\0\0| p/NetWare FTP stats httpd/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Abyss/([-\w.]+)-Linux AbyssLib/([\d.]+)\r\n|s p/Abyss httpd/ v/$1/ i|AbyssLib/$2| o/Linux/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Abyss/([-\w.]+) \(Win32\) AbyssLib/([\d.]+)\r\n|s p/Abyss httpd/ v/$1/ i|AbyssLib/$2| o/Windows/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Abyss/([-\w.]+)-Win32 AbyssLib/([\d.]+)\r\n|s p/Abyss httpd/ v/$1/ i|AbyssLib/$2| o/Windows/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Abyss/([-\w.]+)-MacOS X AbyssLib/([\d.]+)\r\n|s p/Abyss httpd/ v/$1/ i|AbyssLib/$2| o/Mac OS X/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Abyss/([-\w.]+)-Linux AbyssLib/([\d.]+)\r\nWWW-Authenticate: Basic Realm=\".*Abyss Web Server Console\"\r\n|s p/Aprelium Abyss httpd console/ i/Abyss $1; AbyssLib $2/ o/Linux/
match http m|^HTTP/1\.[01] \d\d\d .*Server: Abyss/([-\w.]+) \(Win32\) AbyssLib/([\d.]+)\r\nWWW-Authenticate: Basic Realm=\".*Abyss Web Server Console\"\r\n|s p/Aprelium Abyss httpd console/ i/Abyss $1; AbyssLib $2/ o/Windows/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: LseriesWeb/([\w.-]+) \(HP_UNIQUE\)\r\n| p/HP Tape Library Web Interface Software httpd/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*Server: AOLserver/([\w+.]+)\r\n|s p/AOLserver httpd/ v/$1/
match http m%^HTTP/1\.0 \d\d\d .*\r\nServer: uIP/([\d.]+) (?:http://www\.sics\.se/~adam/uip/|\(http://dunkels\.com/adam/uip/\))\r\n% p/uIP/ v/$1/
match http m|^HTTP/1\.0 401 Unauthorized\r\nContent-Type: text/html\r\nWWW-Authenticate: Basic realm=\"DI-514\"\r\n\r\n<title>401 Unauthorized</title><body><h1>401 Unauthorized</h1></body>| p/D-Link DI-514 router http config/ d/router/
match http m|^HTTP/1\.0 302 Redirect\r\nServer: GoAhead-Webs\r\nDate: .*\r\nPragma: no-cache\r\nCache-Control: no-cache\r\nContent-Type: text/html\r\nLocation: http(s?)://SwitchViewIP\.Avocent\.com/splashscreen\.asp\r\n| p/Avocent Switchview http$1 config/ d/switch/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Orion/([\d.]+)\r\n| p/Orion Java Application Server httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Agent-ListenServer-HttpSvr/([\d.]+)\r\n| p/NAI EPO Agent framework/ i/Agent ListenServer $1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nMIME-version: 1\.0\r\nServer: ZOT-PS-19/([\d.]+)\r\nWWW-Authenticate: Basic realm=\"PrnServr\"\r\nContent-Type: text/html\r\n\r\n<TITLE>AUTH</TITLE><H1>401 Unauthorized\.</H1>| p/IOGear USB Print Server/ i/ZOT-PS-19 $1/ d/print server/
match http m|^HTTP/1\.1 \d\d\d .*\r\nConnection: close\r\nDate: .*\r\nServer: RMC Webserver ([\d.]+)\r\n| p/Dell Embedded Remote Access Card/ i/RMC httpd $1/ d/remote management/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: TwistedWeb/([\w.]+)\r\n|s p/TwistedWeb httpd/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Twisted/([\d.]+) TwistedWeb/SVN-Trunk\r\n|s p/TwistedWeb httpd/ v/$1 SVN-Trunk/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Twisted/([-\w_.+]+) TwistedWeb/\[twisted\.web\d+, version ([^]]+)\]\r\n|s p/TwistedWeb httpd/ v/$2/ i/Twisted $1/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: Twisted/([\w._-]+) TwistedWeb/\[OPSI\.web\d+, version ([^]]+)\]\r\n|s p/TwistedWeb httpd/ v/$2/ i/Twisted $1/
match http m|^HTTP/1\.1 401 Unauthorized\r\nContent-Length: 141\r\nServer: Twisted/([\w._+-]+) TwistedWeb/([\w._+-]+)\r\nDAV: 1, access-control\r\nDate: .*\r\nContent-Type: text/html\r\nWWW-Authenticate: digest nonce=\"\d+\", realm=\"/Search\", algorithm=\"md5\"\r\nConnection: close\r\n\r\n<html><head><title>Unauthorized</title></head><body><h1>Unauthorized</h1><p>You are not authorized to access this resource\.</p></body></html>$| p/TwistedWeb/ v/$2/ i/Twisted $1; Mac OS X teamsserver/ o/Mac OS X/
match http m|^HTTP/1\.1 404 Not Found\r\n.*Server: Twisted/([\w._-]+) TwistedWeb/([\w._-]+)\r\n.*<meta name=\"generator\" content=\"\">\n<meta name=\"apple_required_ui_revision\" content=\"\">\n<meta name=\"apple_collab_uid\" content=\"\">\n|s p/TwistedWeb/ v/$2/ i/Twisted $1; Mac OS X teamsserver/ o/Mac OS X/
match http m|^HTTP/1\.[01].*\r\nServer: Twisted/([\.\d]+) TwistedWeb/([\.\d]+)|s p/TwistedWeb/ v/$2/ i/Twisted $1/ o/Mac OS X/
match http m|^HTTP/1\.0 \d\d\d .*\r\nConnection: close\r\nContent-Length: \d+\r\nContent-Type: text/html.*\r\n\r\n<!DOCTYPE html\nPUBLIC.*\n<title>MikroTik RouterOS Managing Webpage</title>\n|s p/MikroTik router config httpd/ d/router/
match http m|^HTTP/1\.1 \d\d\d .*Server: Azureus ([\d.]+)\r\n|s p/Azureus Bittorrent tracker httpd/ v/$1/
match http m|^HTTP/1\.1 401 BAD\r\nWWW-Authenticate: Basic realm=\"Azureus - Swing Web Interface\"\r\n\r\nAccess Denied\r\n| p/Azureus Bittorrent webui plugin/ i/Access denied/
match http m|^HTTP/0\.9 200 Document follows\r\nConnection: close\r\nMIME-Version: 1\.0\r\nContent-Type: text/html\r\nContent-Length: \d+\r\n\r\n.*<html> \r\n<head> \r\n   <title>Thomson Cable Modem Diagnostics</title>\r\n|s p/Thomson Cable Modem Web Diagnostics/ d/broadband router/
match http m|^HTTP/1\.0 200 Ok\r\nServer: micro_httpd\r\n.*<title>Thomson Cable Modem Diagnostics</title>\r\n|s p/Thomson Cable Modem Web Diagnostics/ i/micro_httpd/ d/broadband router/
match http m|^HTTP/1\.0 302 Redirect\r\nServer: GoAhead-Webs\r\nPragma: no-cache\r\nCache-Control: no-cache\r\nContent-Type: text/html\r\nLocation: https://(iDRAC-\w+)(?::443)?(?:/Applications/dellUI/login\.htm)?\r\n\r\n| p/GoAhead-Webs/ i/Dell iDRAC http config/ d/remote management/ h/$1/
match http m|^HTTP/1\.0 302 Redirect\r\nServer: GoAhead-Webs\r\nDate: .*\r\nPragma: no-cache\r\nCache-Control: no-cache\r\n| p/GoAhead-Webs embedded httpd/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*\r\nServer: FortiWeb-([\d.]+)\r\n| p/Fortinet FortiWifi 60 http config/ i/FortiWeb $1/ d/router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"Serverdoc Remote\"\r\nConnection: close\r\n\r\n\r\n| p/Serverdoc remote httpd/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\n<title>BNBT Tracker Info</title>\n|s p/BNBT Bittorrent Tracker/
match http m|^HTTP/1\.1 200 OK\r\nServer: AnomicHTTPD \(www\.anomic\.de\)\r\n| p/AnomicHTTPD/
match http m|^HTTP/1\.1 200 OK\r\nConnection: close\r\nPragma: no-cache\r\n.*\n<html lang=\"(..)\">\n<head>\n<title>POPFile |s p/POPFile web control interface/ i/Lang: $1/
match http m|^HTTP/1\.0 200 OK\r\nPragma: no-cache\r\nContent-Type: text/html\r\n\r\n\n\n\n\t\n\n\n\t\n\n\n\n\n\n<!--  -->\n\n\n\n<!-- \$R..file: i_pagestart\.shtm,v \$  -->\n<html>\n<head>\n| p/Axis 5400 print server web config/ d/print server/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\nDate: .*\r\nAllow: GET, HEAD\r\nServer: Spyglass_MicroServer/([\w.]+)\r\n\r\n<html>\n\n<head>\n\n<title>  Software de administraci&#243;n de impresora PhaserLink  </title>\n\n| p/Tektronix Phaser printer web config/ i/Spyglass embedded httpd $1/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nConnection: close\r\nServer: Microsoft-WinCE/([\d.]+)\r\n| p/ChipPC Extreme httpd/ i/WinCE $1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: DManager\r\nMIME-version: 1\.0\r\nWWW-Authenticate: Basic realm=\"surgemail| p/Surgemail webmail/ i/DNews based/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: DManager\r\n| p/DNews Web Based Manager/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: IDS-Server/([\d.]+)\r\n| p/IDS-Server httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nConnection: keep-alive\r\nContent-Type: text/HTML\r\nContent-Length: \d+\r\nServer: Indy/([\d.]+)\r\nSet-Cookie: .*\r\n\r\n<!-- header\.html -->.*TeamSpeak|s i/TeamSpeak 1.X admin httpd/ p/Indy httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nConnection: keep-alive\r\nContent-Type: text/HTML\r\nContent-Length: \d+\r\nServer: Indy/([\d.]+)\r\nSet-Cookie: .*<title>TeamSpeak 2 - Server-Administration</title>|s i/TeamSpeak 2.X admin httpd/ p/Indy httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nConnection: close\r\nContent-Type: text/plain\r\nServer: Indy/([\d.]+)\r\n\r\n| i/TiVo Home Media Option httpd/ p/Indy httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\nDate: .*\nServer: FrontPage-PWS32/([\d.]+)\n| p/FrontPage Personal Webserver/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: WindWeb/([\d.]+)\r\nConnection: close\r\nContent-Type: text/html\r\nWWW-Authenticate: Basic realm=\"Home Gateway\"\r\n\r\n<html>\r\n\r\n<head>\r\n<meta http-equiv=\"Content-Type\" content=\"text/html; charset=windows-1252\">\r\n<meta name=\"GENERATOR\" content=\"Microsoft FrontPage 4\.0\">\r\n<meta name=\"ProgId\" content=\"FrontPage\.Editor\.Document\">\r\n<title>Pirelli Smart Gate</title>\r\n\r\n| p/Pirelli Smartgate Ethernet dsl router web config/ i/WindWeb httpd $1/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*Server: TSM_HTTP/([\d.]+)\n|s p/Tivoli Storage Manager http interface/ i/TCM httpd $1/
match http m|^HTTP/1\.0 \d\d\d .*Server: ADSM_HTTP/([\d.]+)\nContent-type: text/html\n\n<HEAD>\n<TITLE>\nServer Administration\n</TITLE>\n\n<META NAME=\"IBMproduct\" CONTENT=\"ADSM\">\n<META NAME=\"IBMproductVersion\" CONTENT=\"([\d.]+)\">.*Storage Management Server for AIX|s p/Tivoli Storage Manager http interface/ v/$2/ i/ADSM httpd $1/ o/AIX/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: ADSM_HTTP/([\d.]+)\r\nContent-type: text/html\r\n\r\n<html><head><title>Server Administration</title></head><body><h1>Not Supported</h1><p>ANR4747W The web administrative interface is no longer supported\. Begin using the Integrated Solutions Console instead\.</p></body></html>| p/Tivoli Storage Manager http interface/ v/$1/ i/discontinued/
match http m|^HTTP/1\.0 \d\d\d .*Server: ADSM_HTTP/([\d.]+)\r?\n.*<TITLE>\nServer Administration\n</TITLE>.*<META NAME=\"IBMproductVersion\" CONTENT=\"([\d.]+)\">.*<TITLE>\nAdministrator Login\n</TITLE>.*Storage Management Server for Windows|s p/Tivoli Storage Manager http interface/ v/$2/ i/ADSM httpd $1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: EPSON-HTTP/([\d.]+)\r\n| p/Epson printer httpd/ v/$1/ d/printer/
match http m|^HTTP/1\.0 200 OK\r\nContent-length: \d+\r\nContent-type: text/html\r\n\r\n<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.0 Transitional//EN\" \"http://www\.w3\.org/TR/REC-html40/loose\.dtd\">\n<HTML>\n<HEAD>\n<TITLE>ADSL ROUTER Control Panel</TITLE>\n</HEAD>\n| p/Dynalink RTA DSL router http config/ d/router/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*\r\nServer: ENI-Web/R([\d_.]+)\r\nContent-Type: text/html\r\nExpires: .*\r\nLast-Modified: .*\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n\r\n<html>\n\n<head>\n<meta http-equiv=\"Content-Type\" content=\"text/html; charset=iso-8859-1\">\n<title>SpeedStream (\d+) Management Interface</title>\n</head>\n\n| p/SpeedStream $2 router http config/ i/ENI-Web httpd $1/ d/router/
match http m|^HTTP/1\.1 401 Unauthorized\r\nDate: .*\r\nServer: ENI-Web/R([\d_]+)\r\nWWW-Authenticate: Basic realm=\"standard@\d+\"\r\n\r\n401 Unauthorized\r\n| p/SpeedStream router http config/ i/ENI-Web httpd $1/ d/router/
match http m|^HTTP/1\.1 403 Forbidden \( The server denies the specified Uniform Resource Locator \(URL\)\. Contact the server administrator\.  \)\r\n| p/MS ISA httpd/ o/Windows/
match http m|^HTTP/1\.1 401 Unauthorized \( The server requires authorization to fulfill the request\. Access to the Web server is denied\. Contact the server administrator\.  \)\r\n| p/MS ISA httpd/ o/Windows/
match http m|^HTTP/1\.1 500 \( No data record is available\. For more information about this event, see ISA Server Help\.  \)\r\n| p/MS ISA httpd/ o/Windows/
match http m|^HTTP/1\.1 400 Bad Request \( The data is invalid\.  \)\r\nVia:| p/MS ISA httpd/ o/Windows/
match http m|^HTTP/1\.1 403 Forbidden \( The ISA Server denied the specified Uniform Resource Locator \(URL\)\.  \)| p/MS ISA httpd/ o/Windows/
match http m|^HTTP/1\.1 500 \(  Connection refused \)\r\n| p/MS ISA httpd/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .* \( El servidor requiere autorizaci\xf3n para satisfacer la petici\xf3n\. Acceso al servidor Web denegado\. P\xf3ngase en contacto con el administrador del servidor\.  \)| p/MS ISA httpd/ i/Spanish/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .* \( La p\xe1gina debe visualizarse en un canal seguro \(es decir, en un nivel de sockets seguro\)\. P\xf3ngase en contacto con el administrador del servidor\.  \)| p/MS ISA httpd/ i/Spanish/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .* \( El servidor deniega la direcci\xf3n URL \(Uniform Resource Locator\) especificada\. P\xf3ngase en contacto con el administrador del servidor\.  \)| p/MS ISA httpd/ i/Spanish/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<HTML><HEAD><TITLE>SMC Barricade Wireless Broadband Router</TITLE>| p/SMC Barricade WAP http config/ d/WAP/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n.*<HTML><HEAD><TITLE>SMC Barricade Broadband Router</TITLE>|s p/SMC Barricade router http config/ d/broadband router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Monkey/([\d.]+) \(Linux\)\r\n|s p/Monkey httpd/ v/$1/ o/Linux/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Monkey Server\r\n| p/Monkey httpd/
match http m|^HTTP/1\.0 \d\d\d .*\nDate: .*\nPragma: no-cache\n      Server: wr_httpd/([\d.]+)\n| p/wr_httpd embedded httpd/ v/$1/
match http m|^HTTP/1\.0 401 Authorization Required\r\nContent-length: 0\r\nWWW-Authenticate: Basic realm=\"Cayman-2E\"\r\n\r\n| p/Cayman 2E router http config/ d/router/
match http m|^HTTP/1\.0 401 Authorization Required\r\nContent-length: 0\r\nWWW-Authenticate: Basic realm=\"Cayman-DSL\"\r\n\r\n| p/Cayman DSL router http config/ d/router/
match http m|^HTTP/1\.1 400 Bad Request\r\nContent-Type: text/html\r\nDate: .*\r\nConnection: close\r\nContent-Length: \d+\r\n\r\n<h1>Bad Request \(Invalid .*\)</h1>$| p/Microsoft IIS httpd/
match http m|^HTTP/1\.0 200 OK\nMIME-version: 1\.0\nContent-type: text/html\n\n<html>\n<head><title> XTide Tide Prediction Server </title>| p/xtide Tide prediction httpd/
match http m|^HTTP/1\.1 401 Unauthorized\r\nDate: .*\r\nServer: Agranat-EmWeb/R([\d_.]+)\r\nWWW-Authenticate: Basic realm=\"User\"\r\n\r\n401 Unauthorized\r\n| i/Nortel Bay router http config/ p/Agranat-EmWeb/ v/$SUBST(1,"_",".")/
match http m|^HTTP/1\.0 200 OK\r\nCache-control: no-cache\r\nPragma: no-cache\r\n.*<title>DTA310 Web Configuration Pages</title></head>|s p/DTA310 VoIP router http config/ d/VoIP adapter/
match http m|^HTTP/1\.0 200 OK\nContent-type: text/html\nContent-length: \d+\n\n<html><head><title></title>.*<font size=\"5\"><a href=\"PrintSir\.htm\">Enter PrintSir utilities</font><|s p/Edimax Printserver httpd/ d/print server/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: FSPMS/([\d.]+) \(Win32\)|s p/F-Secure Policy Manager Server httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nWWW-Authenticate: Basic realm=\"SpeedTouch \(([-\w]+)\)\"\r\n\r\n| p/SpeedTouch DSL router http config/ i/MAC $1/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: RapidLogic/([\d.]+)\r\nMIME-version: [\d.]+\r\nContent-type: text/html\r\nDate: .*<META NAME=\"GENERATOR\" Content=\"Visual Page 2\.0 for Windows\">\r\n|s p/Brocade Silkworm Fibreswitch http config/ i/RapidLogic httpd $1/ d/switch/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Netscape-Commerce/([\d.]+)\r\n| p/Netscape-Commerce httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nWWW-Authenticate: Basic Realm=\"DSLink 200 U/E\"\r\n| p/DSLink 200 DSL router http config/ d/router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nContent-Type: text/html\r\nDate: .*\r\nServer: TUX/([\d.]+) \(Linux\)\r\n| p/TUX httpd/ v/$1/ o/Linux/
match http m|^HTTP/1\.0 200 OK\r\nPragma: no-cache\r\nExpires: .*\r\nContent-Type: text/html\r\n\r\n\n<html>\n\n  <head>\n    <meta http-equiv=\"content-type\" content=\"text/html;charset=iso-8859-1\">\n    \n    <title>Remote UI &lt;Top Page&gt; :  ; [\d ]+</title>\n| p/Canon LBP-2000 printer httpd/ d/printer/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: 2Wire-Gateway/([-\w_.]+)\r\n| p/2Wire HomePortal router http config/ i/Firmware $1/ d/router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: 2wire Gateway ([\d.]+)\r\n|s p/2Wire HomePortal http config/ v/$1/ d/broadband router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: 2wire Gateway\r\n|s p/2Wire HomePortal http config/ d/broadband router/
match http m|^HTTP/1\.0 200 OK\r\nPragma:no-cache\r\nContent-Length: \d+\r\nContent-Type: text/html\r\n\r\n<html>\n<head>\n<title>AXIS ([\d/+]+); IP address: [\d.]+</title>\n| p|AXIS $1 print server http config| d/print server/
match http m|^HTTP/1\.0 200 OK\r\nServer: Gordian Embedded([\d.]+)\r\nContent-type: text/html\r\nDate: .*\r\nLast-Modified: .*\r\nExpires: .*\r\nPragma: no-cache\r\nCache-Control: no-cache\r\n\r\n<html>\n<head>\n<title>Lantronix Web Manager</title>\n| p|Lantronix MSS/100 http config| i/Goridan embedded httpd $1/
match http m|^HTTP/1\.0 \d\d\d.*<TITLE>Lantronix Web Manager ([\d.]+) : Home</TITLE>|s p/Lantronix Web Manager/ v/$1/
match http m|^HTTP/1\.1 302 Redirected\r\nConnection: close\r\nContent-Length: 0\r\nLocation: /login\r\n\r\n$| p/Kerio MailServer http config/
match http m|^HTTP/1\.0 \d\d\d .*\r\nWWW-Authenticate: Basic realm=\"DI-(\w+)\"\r\n\r\n| p/D-Link DI-$1 http config/ d/WAP/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Embedded HTTP Server *([\d.]+)\r\nWWW-Authenticate: Basic realm=\"DI-(\w+) *\"\r\n| p/D-Link DI-$2 http config/ i/Embedded httpd $1/ d/WAP/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nWWW-Authenticate: Basic Realm=\"D-Link ([-\w_.]+) Router\"\r\n| p/D-Link $1 router http config/ d/WAP/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: Agranat-EmWeb/R([\d_]+)\r\nWWW-Authenticate: Basic realm=\"administration\"\r\n\r\n401 Unauthorized\r\n| i/Efficient Networks router http config/ p/Agranat-EmWeb/ v/$SUBST(1,"_",".")/ d/router/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<!--CAS:0003--><HTML><HEAD><SCRIPT LANGUAGE=JavaScript><!--\ndocument\.write\(\"<TITLE>\"\)\nvar l1=\"713P\"| p/D-Link DI-713P wireless access point http config/ d/WAP/
match http m|^HTTP/1\.0 200 OK\r\ncontent-type:text/html\r\n\r\n<HTML><HEAD><TITLE>WWWinamp</TITLE>| p/WWWinamp remote control httpd/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-Length: \d+\r\n.*<TITLE>Live view / - AXIS 205( Network Camera)? version ([\d.]+)</TITLE>\n|s p/AXIS 205 network camera web interface/ v/$2/ d/webcam/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: RapidLogic/([\d.]+)\r\nMIME-version: [\d.]+\r\nContent-type: text/html\r\n\r\n<html>\r\n  <title>VT1000v Status</title>| p/Motorola VT1000v VoIP Adapter http config/ i/RapidLogic httpd $1/ d/VoIP adapter/
match http m|^HTTP/1\.0 200 Okay\r\nDate: .*\r\nConnection: close\r\nContent-Type: text/html\r\nContent-Length: \d+\r\n\r\n<html>\n<head><title>home\.htm</title>| p/NetComm NS4000 network camera http interface/ d/webcam/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*\r\nContent-Type: \(null\)\r\nConnection: close\r\n\r\n([-\w_.]+)\n$| p/IRC Services http stats/ h/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Oracle Application Server Containers for J2EE\r\n| p/Oracle Application Server httpd/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Oracle Application Server Containers for J2EE 10g \(([\d.]+)\)\r\n| p/Oracle Application Server httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Oracle Application Server Containers for J2EE 10g \(([\d.]+)\) - Developer Preview\r\n| p/Oracle Application Server httpd/ v/$1/ i/Developer preview/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Oracle-Application-Server-10g/([\d.]+) Oracle-HTTP-Server\r\n| p/Oracle Application Server 10g httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Oracle-Application-Server-10g/([\d.]+) Oracle-HTTP-Server|s p/Oracle Application Server 10g httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: OracleAS-Web-Cache-10g/([\d.]+)\r\n|s p/OracleAS Web Cache 10g/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*Server: Oracle-Application-Server-10g/([\d.]+) Oracle-HTTP-Server OracleAS-Web-Cache-10g/([\d.]+) |s p/Oracle Application Server 10g httpd/ v/$1/ i/OracleAS-Web-Cache-10g $2/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Oracle Containers for J2EE\r\n.*<TITLE>Oracle Application Server 10g Release 3 \(([\d.]+)\)|s p/Oracle Application Server 10g httpd/ v/$1/ i/Oracle Containers for J2EE/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Oracle Containers for J2EE\r\n.*<title>Oracle Containers for J2EE 10g Release 3 \(([\d.]+)\)|s p/Oracle Application Server 10g httpd/ v/$1/ i/Oracle Containers for J2EE/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Oracle Containers for J2EE\r\n.*<TITLE>Welcome to Oracle Containers for J2EE 10g \(([\w._-]+)\)</TITLE>|s p/Oracle Application Server 10g httpd/ v/$1/ i/Oracle Containers for J2EE/
match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-type: text/html\r\nCache-Control: public\r\nPragma: cache\r\nExpires: .*\r\nWWW-Authenticate: Basic realm=\"Linksys WRV54G\"\r\n| p/Linksys WRV54G router http config/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\ncontent-length: \d+\r\ncontent-type: text/html\r\ndate: .*<title>MikroTik RouterOS Managing Webpage</title>|s p/MikroTik httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Embedded HTTP Server v([\d.]+)\r\n.*<body bgcolor=\"#DAE3EB\"|s p/SMC wireless router http config/ i/Embedded httpd $1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Askey Software ([\d.]+)\r\n.*<title>Scientific.A..anta WebStar Cable Modem</title>.*|si p/Scientific Atlanta WebStar cable modem http config/ d/broadband router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nConnection: close\r\nServer: XES 8830 WindWeb/([\d.]+)\r\n| p|Xerox 8830 printer/plotter httpd| i/WinWeb $1/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Embedded HTTP Server USR([\w_.]+)\r\nWWW-Authenticate: Basic realm=\"([^"]+)\"\r\nConnection: close\r\n\r\n<| p/USRobotics router http config/ i/Embedded httpd $1; Name $2/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Embedded HTTP Server ([\w_.]+)\r\nWWW-Authenticate: Basic realm=\"(USR\d+)\"\r\nConnection: close\r\n\r\n| p/$2 wireless router http config/ i/Embedded httpd $1/ d/router/
match http m|^HTTP/1\.1 401 Unauthorized \r\nServer:httpd\r\nDate: .*\r\nContent-Type:text/html\r\nWWW-Authenticate: Basic realm=\"U\.S\.Robotics\"\r\nConnection:close\r\n\r\n<HTML> <Title> 401 unAuthorized </title>                   <body> <H1> 401 unauthorized request </H1></body>                   </HTML>| p/USRobotics router http config/ d/broadband router/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: micro_httpd.*Basic realm=\"USR ADSL Gateway\"\r\n|s p/USRobotics router http config/ i/embedded micro_httpd/ d/broadband router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: WN/([\d.]+)\r\n| p/WN httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-Type: text/html\r\nWWW-Authenticate: Basic realm=\"DWL-700AP\"\r\n\r\n| p/D-Link DWL-700AP router http config/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nConnection: close\r\nServer: WindWeb/([\d.]+)\r\nDate: .*\r\nContent-Type: \r\n\r\n<html>\n<head>\n<title>DW6000 System Control Center</title>| p/Hughes DW6000 satellite router http config/ i/WindWeb httpd $1/ d/router/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\nServer: WindWeb/([\d.]+)\r\n.*WWW-Authenticate: Basic realm=\"HUGHES Terminal\"\r\n\r\n<html>\n<head>\n<title>HN7000S System Control Center</title>|s p/Hughes HN7000S satellite router http config/ i/WindWeb httpd $1/ d/router/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"DM602 \"\r\nContent-type: text/html\r\nContent-length: 0\r\n\r\n/\"\r\nContent-type: text/html\r\nContent-length: 0\r\n\r\n| p/Netgear DM602 router http config/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nWWW-Authenticate: Basic realm=\"EvoCam\"| p/EvoCam http interface/ d/webcam/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: GST ([\d.]+) .*\r\n| p/Linksys WAP11 http config/ i/Firmware $1/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nConnection: [Cc]lose\r\nServer: LANCOM ([-\w.+/]+) Office ([\w. /]+)\r\n| p|Lancom DSL/$1 router http config| v/$2/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nConnection: Close\r\nServer: LANCOM ([\w-]+) Wireless ([\w. /]+)\r\n| p/Lancom $1 wireless router http config/ v/$2/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nConnection: Close\r\nServer: LANCOM ([\w-]+) ADSL/ISDN ([\w. /]+)\r\n| p|Lancom $1 DSL/ISDN router http config| v/$2/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nConnection: Close\r\nServer: LANCOM ([\w-]+) VPN ([\w. /]+)\r\n| p/Lancom $1 VPN http config/ v/$2/ d/security-misc/
match http m|^HTTP/1\.0 403 Forbidden\r\nServer: Gordian Embedded([\d.]+)\r\n.*<HTML>\n<HEAD>\n<TITLE>Lantronix - Authentication for ([^<]+)</TITLE>\n|s p/Lantronix MSSVIA http config/ i/Gordian embedded httpd $1; Name $2/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Virata-EmWeb/R([\d_]+)\r\n.*<title>Cisco Systems, Inc\. VPN (\d+) Concentrator|s i/Cisco VPN $2 Concentrator http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/terminal server/
match http m|^HTTP/1\.1 301 Moved Permanently\r\nServer: Web Server\r\nLocation: .*\r\nContent-Type: text/html\r\nContent-Length: \d+\r\n\r\n<HEAD><TITLE>Moved</TITLE></HEAD><BODY><A HREF=\".*\">Moved</A></BODY>\r\n$| p/Cisco VPN Concentrator http config/ d/terminal server/
match http m|^HTTP/1\.1 301 Moved Permanently\r\nServer: Web Server\r\nLocation: https://[\d.]+/webvpn\.html\r\nContent-Type: text/html\r\nContent-Length: \d+\r\n\r\n<HEAD><TITLE>Moved</TITLE></HEAD><BODY><A HREF=\"https://[\d.]+/webvpn\.html\">Moved</A></BODY>\r\n| p/Cisco VPN Concentrator http config/ d/terminal server/
match http m|^HTTP/1\.1 200 OK\r\nServer: Web Server\r\n.*\n<title>Cisco Systems, Inc\. VPN (\d+) Concentrator \[VPN-EPUL\]</title>|s p/Cisco VPN $1 Concentrator http config/ d/terminal server/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: BrowseAmp\r\n| p/BrowseAmp WinAmp webcontrol plugin/ o/Windows/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\n\r\n<HTML><HEAD><META HTTP-EQUIV=\"Content-type\" CONTENT=\"text/html; charset=iso-8859-1\">\r\n<TITLE>Dell Laser Printer (\w+)</TITLE>| p/Dell Laser Printer $1 http config/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: PRINT_SERVER WEB ([\d.]+)\r\nWWW-Authenticate: Basic realm=\"NeedPassword\"\r\nContent-type: text/html\r\n| p/Netgear Mini print server http config/ i/PRINT_SERVER WEB httpd $1/ d/print server/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: PRINT_SERVER WEB ([\d.]+)\r\nContent-type: text/html\r\n\r\n<html><head><title>NETGEAR Setup</title>| p/Netgear print server http config/ i/PRINT_SERVER WEB httpd $1/ d/print server/
match http m|^HTTP/1\.0 401 Password Required\r\nWWW-Authenticate: Basic realm= StarVoice\r\nServer: GoAhead-Webs\r\n| p/Aethra Starvoice DSL router http config/ i/GoAhead httpd/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Thy/([\d.]+) Debian/[\w/]+ \([^)]+\) GnuTLS/([\d.]+) zlib/([\d.]+)\r\n| p/Thy httpd/ v/$1/ i/Debian; GnuTLS $2; zlib $3/ o/Linux/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Thy/([\d.]+) Debian \(\w+\) GnuTLS/([\d.]+) zlib/([\d.]+)\r\n| p/Thy httpd/ v/$1/ i/Debian; GnuTLS $2; zlib $3/ o/Linux/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Thy/([\d.]+) zlib/([\d.]+)\r\n| p/Thy httpd/ v/$1/ i/zlib $2/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nDate: .*\r\nServer: FileMakerPro/([\w.]+) WebCompanion/([\w.]+)\r\n| p/WebCompanion httpd $2/ i/FileMakerPro $1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: FileMakerPro/([\d.]+)\r\n|s p/FileMakerPro httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: AdSubtract ([\d.]+)\r\n| p/AdSubtract httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer:ATMEL Embedded Webserver\r\nWWW-Authenticate: Basic realm=\"Linksys WAP11\",\r\n\r\n| p/Linksys WAP11 http config/ i/ATMEL embedded httpd/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-Type: text/html\r\nWWW-Authenticate: Basic realm=\"Linksys WAP11\"\r\n\r\n| p/Linksys WAP11 http config/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: bozohttpd/(\w+)\r\n|s p/bozohttpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*Server: Null httpd ([\d.]+)\r\n|s p/Null httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\nServer: Dune/([\d.]+)\r\n| p/Dune httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Meredydd Luff's Surfboard/([\d.]+) \(UNIX/\w+\)\r\n| p/Surfboard httpd/ v/$1/ o/Unix/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: zawhttpd ([\d.]+)\r\n| p/zawhttpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\nDate: .*\nServer: NeepHttpd/([\d.]+) \(Linux\)\n| p/NeepHttpd/ v/$1/ o/Linux/
match http m|^HTTP/1\.0 401 Unauthorized\r\nConnection: close\r\nServer: WindWeb/([\d.]+)\r\nDate: .*\r\nContent-Type: text/html\r\nWWW-Authenticate: Basic realm=\"Home Gateway\"\r\n\r\nHasbani Web Server Error Report:| p/Conexant DSL router http config/ i/WindWeb httpd $1/ d/router/
match http m|^HTTP/1.0 401 Unauthorized\r\nConnection: close\r\nServer: WindWeb/([\d\.]+)\r\nDate: .*\r\nContent-Type: text/html\r\nWWW-Authenticate: Basic realm="(AG \w+)"\r\n| p/WindWeb/ v/$1/ i/Nomadix $1 router http config/ d/router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: WindWeb/([\d.]+)\r\nWWW-Authenticate: Basic realm=\"Home Gateway\"\r\nContent-Type: text/html\r\nDate: .*\r\nAge: 0\r\n\r\nHasbani Web Server Error Report:<HR>\n<H1>Server Error: 401 Unauthorized</H1>\r\n<P><HR><H2>Access denied</H2><P><P><HR><H1>/doc/index\.htm</H1><P>| p/3Com router http config/ i/WindWeb httpd $1/ d/router/
match http m|^HTTP/1\.0 403 Forbidden\r\nConnection: close\r\nServer: WindWeb/([\d.]+)\r\nDate: .*\r\nContent-Type: text/html\r\nWWW-Authenticate: Basic realm=\"Home Gateway\"\r\n\r\nHasbani Web Server Error Report:<HR>\n<H1>Server Error: 403 Forbidden</H1>\r\n<P><HR><H2>Access denied</H2><P>| p/eTec DSL router http config/ i/WindWeb httpd $1/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: AKCP Embedded Web Server\r\n.*<font color=#FFCC66>Uptime Devices</font>|s p|UptimeDevices Sensorprobe temp/humidity http config| i/AKCP embedded httpd/ d/specialized/
match http m|^HTTP/1\.[01] \d\d\d.*\r\nServer: SHS\r\n|s p/Small Home Server httpd/ o/Windows/
match http m|^HTTP/1\.0 200 OK\nContent-type: text/html\r\nDate: .*\r\nConnection: close\r\nLast-Modified: .*\r\nContent-length: \d+\r\n\r\n<html>\n<head>\n\t<title>PXES on P\d+</title>| p/PXES Linux Thin Client httpd/ o/Linux/ d/terminal/

match http m|^HTTP/1\.1 401 Access Denied Still Working\r\nWWW-Authenticate: Basic realm=.*\r\nServer: cpsrvd/([\w._-]+)\r\n|s p/cPanel httpd/ v/$1/ o/Linux/ i/unauthorized/
match http m|^HTTP/1\.1 401 Access Denied Still Working\r\nWWW-Authenticate: Basic realm=\"[^"]+\"\r\nConnection: close\r\nSet-Cookie: logintheme=cpanel;| p/cPanel httpd/ o/Linux/ i/unauthorized/
match http m|^HTTP/1\.[01] \d\d\d .*\nServer: cpaneld/([\d.]+)\n|s p/cPanel httpd/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\nServer: cpsrvd/([\d.]+)\r\n|s p/cPanel httpd/ v/$1/ o/Unix/

match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Embedded HTTP Server v([\w.]+)\r\nWWW-Authenticate: Basic realm=\"DWL-810\+\"\r\n| p/D-Link DWL-810+ WAP http config/ i/Embedded httpd $1/ d/WAP/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Embedded HTTP Server V([\w.]+)\r\nWWW-Authenticate: Basic realm=\"(DWL-[\w+-.]+)\"\r\n| p/D-Link $2 WAP http config/ i/Embedded httpd $1/ d/WAP/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: Embedded HTTP Server ([\d.]+)    \r\nWWW-Authenticate: Basic realm=\"([^"]+)\"\r\nConnection: close\r\n\r\n<HTML><HEAD><TITLE>401 Unauthorized</TITLE></HEAD>\n<BODY BGCOLOR=\"#ffffff\"><H4>401 Unauthorized</H4></BODY></HTML>\n$| p/D-Link DWL-9000+ WAP http config/ i/Embedded httpd $1; Name $2/ d/WAP/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: Embedded HTTP Server ([\w.]+)\r\nWWW-Authenticate: Basic realm=\"AP0F1D85\"\r\nConnection: close\r\n\r\n<HTML><HEAD><TITLE>401 Unauthorized</TITLE></HEAD>\n<BODY BGCOLOR=\"#ffffff\"><H4>401 Unauthorized</H4></BODY></HTML>\n| p/Topcom skyracer 544 router http config/ d/router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: Embedded HTTP Server ([\d.]+)\r\nWWW-Authenticate: Basic realm=\"([^"]+)\".*\r\n\r\n<HTML><HEAD><TITLE>401 Unauthorized</TITLE></HEAD>\n<BODY BGCOLOR=\"#ffffff\"><H4>401 Unauthorized</H4></BODY></HTML>\n|s p/D-Link DWL-624 WAP http config/ i/Embedded httpd $1; Name $2/ d/WAP/
match http m|^HTTP/1\.1 200 .*\r\nServer: Allegro-Software-RomPager/([\w._-]+)\r\n.*<title>(DWL-\w+)</title>|s p/D-Link $2 WAP http config/ d/WAP/ i/Allegro RomPager httpd $1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nMIME-Version: [\d.]+\r\nServer: CERN/([\d.]+)\r\n.*alert\(\"\\r\\nThis version of your browser cannot support the router's configuration completely\. Please refer to the router's CD-ROM for upgrade information\.\"\);|s i/Edimax BR-6004 broadband router http config/ p/CERN httpd/ v/$1/ d/broadband router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nConnection: close\r\nDate: .*\r\nCache-Control: no-cache\r\nPragma: no-cache\r\nContent-Type: text/html\r\nContent-Length: \d+\r\nServer: Web-Server/([\d.]+)\r\n\r\n<HTML>\n<FRAMESET ROWS=\"82,40,\*\"| p|NRG/Ricoh copier http config| i/Web-Server httpd $1/ d/printer/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Savant/([\d.]+)\r\n| p/Savant httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nConnection: close\r\nContent-Type: text/html; charset=iso-8859-1\r\n\r\n.*<th width=\"50%\">TiVo Web Project - TCL - v([\d.]+)&nbsp;</th><th>&nbsp;|s p/TiVo Web Project http interface/ v/$1/ d/media device/
match http m|^HTTP/1\.1 \d\d\d .*\r\nConnection: close\r\nContent-Type: text/plain\r\nContent-Length: \d+\r\nServer: TiVo Server/([\d.]+)\r\n\r\n| p/TiVo Desktop httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: WebTopia/([\w.]+) \(Unix\)\r\n| p/Archetopia WebTopia httpd/ v/$1/ o/Unix/
match http m|^HTTP/1\.1 \d\d\d .*\r\nConnection: close\r\nContent-Length: \d+\r\nContent-Type: text/html\r\n\r\n.*C<small>ISCO<font height=10 size=2> S<small>YSTEMS<br>|s p/Cisco IP Phone http config/ d/VoIP phone/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Apache/([\d.]+)\+NITI ([^\r\n]+)\r\n| p/Net Integration Modified Apache httpd/ v/$1/ i/$2/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Microsoft ASP\.NET Web Matrix Server/([\d.]+)\r\n| p/Microsoft ASP.NET Web Matrix httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-Type: text/html\r\n\r\n.*<TITLE>Lexmark Optra (\w+)</TITLE>|s p/Lexmark Optra $1 printer http config/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-Type: text/html\r\n\r\n.*<TITLE>Lexmark Optra SC (\w+)</TITLE>|s p/Lexmark Optra SC $1 printer http config/ d/printer/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: GWS/([\d.]+)\r\n|s p/Google httpd/ v/$1/ i/GWS/ o/Linux/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: GFE/([\d.]+)\r\n|s p/Google httpd/ v/$1/ i/GFE/ o/Linux/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: GWS-GRFE/([\d.]+)\r\n|s p/Google httpd/ v/$1/ i/GWS-GRFE/ o/Linux/

# These should hopefully match before the more general Ubicom line in GenericLines
match http m|^HTTP/1\.1 \d\d\d .*\r\nCache-control: no-cache\r\nServer: Ubicom/(\d[-.\w ]+)\r\nContent-Length: \d+\r\nWWW-Authenticate: Basic realm=\"Linksys WET54G\"\r\n| i/Linksys WET54G wireless bridge http config/ p/Ubicom httpd/ v/$1/ d/bridge/
match http m|^HTTP/1\.1 302 Moved Temporarily\r\nCache-control: no-cache\r\nServer: Ubicom/(\d[-.\w ]+)\r\nLocation: login\.html\r\n\r\n$| i/SMC SMC2870W Wireless bridge http config/ p/Ubicom httpd/ v/$1/ d/bridge/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Ubicom/([\d.]+)\r\n.*<title>(DI-\w+)</title>\n|s i/D-Link $2 router http config/ p/Ubicom httpd/ v/$1/ d/router/
match http m%^HTTP/1\.0 200 OK\r\nCache-control: no-cache\r\nServer: Ubicom/([\d.]+)\r\nContent-Type: text/html\r\n\r\n\xef\xbb\xbf.*<title>TRENDnet TEW-([\w ]+) Router \|\r\n\t\t Login\r\n\t</title>%s p/Ubicom httpd/ v/$1/ i/TRENDnet TEW-$2 WAP http config/ d/WAP/
match http m%^HTTP/1\.0 200 200 OK\r\n.*Server: Ubicom/([\d.]+)\r\n.*\n\t<title>D-LINK SYSTEMS, INC\. \| WIRELESS ROUTER  :\n\t\t Login\n\t</title>%s i/D-Link DIR-655 WAP http config/ p/Ubicom httpd/ v/$1/ d/WAP/
match http m%^HTTP/1\.0 200 OK\r\n.*Server: Ubicom/([\d.]+)\r\n.*<link rel=\"stylesheet\" rev=\"stylesheet\" href=\"/substyle_(DIR-\w+)\.css\" type=\"text/css\" />.*<title>D-LINK SYSTEMS, INC\. \| WIRELESS ROUTER  :\r\n         Login\r\n    </title>%s p/Ubicom httpd/ v/$1/ d/WAP/ i/D-Link $2 WAP http config/
match http m%^HTTP/1\.0 200 OK\r\n.*Server: Ubicom/([\d.]+)\r\n.*<title>D-LINK SYSTEMS, INC\. \| WIRELESS ROUTER  :\r\n         Login\r\n    </title>%s i/D-Link DIR-655 WAP http config/ p/Ubicom httpd/ v/$1/ d/WAP/
match http m%^HTTP/1\.0 200 OK\r\n.*Server: Ubicom/([\d.]+)\r\n.*<title>D-LINK SYSTEMS, INC\. \| WIRELESS ROUTER :\r\r\nLogin\r\r\n</title>%s p/Ubicom httpd/ v/$1/ i/D-Link WAP http config/ d/WAP/

match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: GoAhead-Webs\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"Default: admin/1234\"\r\n| p|Router with realtek 8181 chipset http config| i/GoAhead-Webs embedded httpd/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nCache-Control: max-age=3600\r\nContent-Type: text/html\r\n\r\n<html>\n<head>\n<META HTTP-EQUIV=\"Pragma\" CONTENT=\"no-cache\"> \n<title>Base Station Management Tool</title>\n<META HTTP-EQUIV=\"MSThemeCompatible\"| p/Microsoft Wireless Base Station http config/ d/router/
match http m|^HTTP/1\.0 302 Moved Temporarily\r\nContent-Length: 169\r\nContent-Type: text/html\r\nLocation: /Volumes/\r\n\r\n<head><title>Moved Temporarily</title></head>\r\n<body><h2>Moved Temporarily!</h2>\r\n<p>The requested resource has been temporarily movedto a new location\.\r\n</p>\r\n</body>\r\n$| p/AXIS StorPoint CD http config/ d/storage-misc/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: text/html\r\nContent-length: \d+\r\n.*<!-- \(c\) Copyright Axis Communications.*Network CD-ROM Server</h2>|s p/AXIS StorPoint CD http config/ d/storage-misc/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: PRINT_SERVER WEB ([\d.]+)\r\nContent-type: text/html\r\nWWW-Authenticate: Basic realm=\"NeedPassword\"\r\n\r\n401 Unauthorized$| p/Linksys wireless print server http config/ i/PRINT_SERVER WEB httpd $1/ d/print server/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Virata-EmWeb/R([\d_]+)\r\nContent-Type: text/html\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n\r\n.*<title>Cisco Systems, Inc\. VPN 3002 Hardware Client|s i/Cisco VPN 3002 http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/security-misc/
match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-Type: text/html; charset=iso-8859-1\r\nContent-Length: \d+\r\nServer: Boche/([\d.]+) xmmsd/([\d.]+)\r\n\r\n| p/xmmsd xmms control web server/ v/$2/ i/Boche httpd $1/ o/Unix/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: libwww-perl-daemon/([\d.]+)\r\n| p/libwww-perl-daemon httpd/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nServer: \r\nContent-Type: text/html; charset=iso-8859-1\r\nDate: .*\r\nLast-Modified: .*\r\nAccept-Ranges: bytes\r\nConnection: close\r\nContent-Length: \d+\r\n\r\n<HTML>\n<HEAD>\n  <META HTTP-EQUIV=Refresh CONTENT=\"0; URL=/cgi-bin/index\.cgi\">\n</HEAD>\n</HTML>\n\n| p/Barracuda Spam firewall http config/ d/firewall/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\n\r\n.*\r\n<title>MiniShare</title>\r\n.*<td class=\"total\" colspan=\"2\">Total: (\d+) files</td><td class=\"totalsize\">(\d+) bytes</td></tr>\r\n</table>\r\n<hr><p class=\"versioninfo\"><a href=\"http://minishare\.sourceforge\.net/\">MiniShare ([\d.]+)</a>|s p/Minishare http interface/ v/$3/ i/$1 files, $2 bytes shared/ o/Windows/
match http m|^<html>\n<head>\n<title>Touchstone Status</title>\n<META HTTP-EQUIV=\"Pragma\"| p/Arris Touchstone Cable Modem http config/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: MACOS_Personal_Websharing\r\n.*<meta name=Title content=\"([^"]+)\">|s p/Mac OS X Personal Websharing httpd/ i/Name $1/ o/Mac OS X/
# Server line is odd. Somebody's idea of a joke?
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Sinclair ZX-81 Spectrum\r\n| p/Urchin Web Statistics httpd/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: WWW File Share Pro\r\n| p/WWW File Share Pro httpd/ o/Windows/
match http m|^HTTP/1\.1 302 Redirect\r\nServer: GoAhead-Webs\r\nDate: .*\r\nPragma: no-cache\r\nCache-Control: no-cache\r\nExpires: 0\r\n<META http-equiv=\"Content-Type\" content=\"text/html; charset=ISO-8559-1\">\r\nLocation: http://\(null\)/index\.html\r\n\r\n| p/ASUS SL6000 series router http config/ d/router/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nDate: .*\r\nServer: HP Apache-based Web Server/(\d[\w.]+) \(Unix\)\r\n| p/HP Apache-based httpd/ v/$1/ o/Unix/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nDate: .*\r\nServer: HP Apache-based Web Server/(\d[\w.]+) \(Unix\) ?([^\r\n]+)\r\n| p/HP Apache-based httpd/ v/$1/ i/$2/ o/Unix/
match http m|^HTTP/1\.0 \d\d\d .*\r\nConnection:close\r\nHost:([-\w_.]+)\r\nServer:WebSVR Version ([^\r\n]+)\r\n| p/WebSVR httpd/ v/$2/ h/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Internet Firewall\r\n| p/3Com OfficeConnect Firewall http config/ d/firewall/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: Router/([\d.]+)\r\nContent-Type: text/html\r\nPragma: no-cache\r\nExpires: 0\r\nConnection: close\r\nWWW-Authenticate: Basic Realm=\"Login as admin\"\r\n\r\n| p/D-Link DI-804V VPN router http config/ i/Router httpd $1/ d/router/
match http m|^<html>\n<title>NETGEAR Web Smart Switch</title>\n<frameset rows='109,\*' framespacing=0 frameborder=no>\n <frame name=top src=top\.htm scrolling=no>\n| p/Netgear FS526T Switch http config/ d/switch/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: text/html\r\n\r\n<HTML>\r\n<HEAD>\r\n<TITLE>NETGEAR Web Smart Switch</TITLE>\r\n| p/Netgear FS726TP switch http config/ d/switch/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\n.*\n<html><head><title>NETGEAR Web Smart Switch</title>|s p/Netgear GS108T switch http config/ d/switch/
match http m|^HTTP/1\.0 200 OK\r\nPragma: no-cache\r\n.*\n<html>\n<title>NETGEAR Web Smart Switch</title>|s p/Netgear GS716T switch http config/ d/switch/
match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<!---CAS:\d+--><HTML><HEAD><TITLE>SMC Barricade Wireless Broadband Router</TITLE>| p/SMC Barricade wireless broadband router http config/ d/broadband router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: swcd/([\d.]+)\r\n| p/swcd httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: LiveStats Reporting Server\r\n.*<TITLE>DeepMetrix LiveStats ([\d.]+) - Login</TITLE>|s p/DeepMetrix LiveStats httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Embedded HTTPD v([\d.]+), \d+\(c\) Delta Networks Inc\.\r\n.*<title>NETGEAR Router</title>|s p/Netgear router http config/ i/Delta Networks Embedded HTTPD $1/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Embedded HTTPD v([\d.]+), \d+\(c\) Delta Networks Inc\.\r\n| p/Delta Networks Embedded HTTPD/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nAllow: .*\r\nServer: Spyglass_MicroServer/([\w.]+)\r\n| p/Spyglass Microserver embedded httpd/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d.*<title>Metasploit Framework Web Console v([-\w_.]+)</title>|s p/Metasploit Framework web console/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nHTTP/1\.0 200 OK\r\nServer: (\w+)\r\nConnection: close\r\nCache-Control: must-revalidate = no-cache\r\nContent-Type: text/html\r\nExpires: 0\r\nLast-Modified: 0\r\n\r\n<html><head>\r\n<title>Netgear Access Point http config</title>| p/Netgear WG602 wireless router http config/ i/$1 httpd/ d/router/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html; charset=iso-8859-1\r\nServer: Grandstream/([\d.]+)\r\n\r\n<HTML><HEAD><TITLE>Login Page</TITLE>.*<font size=4 color=\"ffffffff\">Welcome to Grandstream IP Phone</font>|s p/BudgeTone-100 VoIP phone http config/ i/Grandstream embedded httpd $1/ d/VoIP phone/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html;charset=iso-8859-1\r\nContent-Length: \d+\r\nServer: Grandstream BT200 ([\w._-]+)\r\n| p/Grandstream BT200 VoIP phone http config/ d/VoIP phone/ v/$1/
match http m|^HTTP/1\.0 200 OK\n.*<title>Grandstream Device Configuration</title>\n.*<form action=\"/cgi-bin/dologin\" method=\"post\" name=\"loginForm\">|s p/Grandstream HT502 VoIP router http config/ d/VoIP adapter/
match http m|^HTTP/1\.1 200 OK\r\n.*<title>Grandstream Device Configuration</title>\r\n.*<form action=\"dologin\.htm\" method=\"post\" name=\"loginForm\">|s p/Grandstream HT286 VoIP router http config/ d/VoIP adapter/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: Tcl-Webserver/([\d.]+) .*CRADLE VERSION ([\d.]+) CONTENTS TEMPLATE\r\n|s i/Cradle Web-Access httpd $2/ p/Tcl-Webserver/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: Tcl-Webserver/([\d.]+) .*\r\n| p/Tcl-Webserver/ v/$1/
match http m|^HTTP/1\.0 401 Authorization Required\r\n.*Server: ListManagerWeb/([\w.]+) \(based on Tcl-Webserver/([\d.]+)\)\r\n|s p/Lyris ListManagerWeb/ v/$1/ i/based on Tcl-Webserver $2/
match http m|^HTTP/1\.0 401 Unauthorized\r\nDate: .*\r\nContent-type: text/html\r\nExpires: .*\r\nWWW-Authenticate: Basic realm=\"level \d+ access\"\r\n\r\n<HEAD><TITLE>Authorization Required</TITLE></HEAD><BODY><H1>Authorization Required</H1>Browser not authentication-capable or authentication failed\.</BODY>\r\n\r\n| p/Cisco wireless router http config/ d/router/
match http m|^HTTP/1\.0 401 Unauthorized \nContent-type:text/html\nExpires: .*\nWWW-Authenticate: Basic realm=\"access\"\n\n<HEAD><TITLE>Authorization Required</TITLE></HEAD><BODY BGCOLOR=#FFFFFF><H1>Authorization Required</H1>Browser not authentication-capable or authentication failed\.</BODY>\n\n| p/Cisco Catalyst switch http config/ d/switch/ o/IOS/
match http m|^HTTP/1\.0 401 Unauthorized\r\nDate: .*\r\nContent-type: text/html\r\nExpires: .*\r\nWWW-Authenticate: Basic realm=\"access\"\r\n\r\n<HEAD><TITLE>Authorization Required</TITLE>.*Browser not authentication-capable or authentication failed|s p|Cisco switch/router http config| o/IOS/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: 4D_WebStar_(\w+)/([\d.]+)\r\n| p/4D WebStar $1/ v/$2/ o/Mac OS/
match http m|^HTTP/1\.[01] \d\d\d .*X-Got-Fish: Pike v([\d.]+ release \d+)\r\n.*Server: Caudium/([^\r\n]+)\r\n|s p/Caudium httpd/ v/$2/ i/Pike $1/
match http m|^HTTP/1\.[01] \d\d\d .*Server: Caudium/([^\r\n]+)\r\n|s p/Caudium httpd/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*Server: Caudium\r\n|s p/Caudium httpd/
match http m|^HTTP/1\.1 \d\d\d .*\r\nMIME-Version: [\d.]+\r\nServer: JC-HTTPD/([\d.]+)\r\n.*<title>(C[-+\w]+)</title>|s p/Oki Data $2 printer http config/ i/JC-HTTPD $1/ d/printer/
match http m|^HTTP/1\.1 \d\d\d .*\r\nMIME-Version: [\d.]+\r\nServer: JC-HTTPD/([\d.]+)\r\n.*<TITLE>(IB-[-+\w]+)</TITLE>|s p/Kyocera $2 printer http config/ i/JC-HTTPD $1/ d/printer/
match http m|^HTTP/1\.1 200 OK\r\nMIME-Version: 1\.0\r\nServer: JC-HTTPD/([\w._-]+)\r\n.*<title>Network USB Hub</title>|s p/JC-HTTPD/ v/$1/ i/Belkin Network USB Hub http config/
match http m|^HTTP/1\.1 200 OK\r\nMIME-Version: 1\.0\r\nServer: JC-HTTPD/([\d.]+)\r\n.*Content-Length: 748\r\n.*\r\n<frame name=topframe noresize scrolling=no src=\"\./top\.htm\">\r\n<frame name=main src=\"\./eng/start/start\.htm\">\r\n|s p/JC-HTTPD/ v/$1/ i/Kyocera FS-1030D printer http config/ d/printer/
match http m|^HTTP/1\.1 200 OK\r\nMIME-Version: 1\.0\r\nServer: JC-HTTPD/([\d.]+)\r\n.*<title>Imagistics\w+ - TOP PAGE -</title>|s p/JC-HTTPD/ v/$1/ i/Sharp Imagistics printer http config/ d/printer/
match http m|^HTTP/1\.1 200 OK\r\nMIME-Version: 1\.0\r\nServer: JC-HTTPD/([\d.]+)\r\n.*<title>Sharp(AR-\w+) - TOP PAGE -</title>|s p/JC-HTTPD/ v/$1/ i/Sharp $2 network card http config/ d/printer/
match http m|^HTTP/1\.1 400 Bad Request\r\nMIME-Version: 1\.0\r\nServer: JC-SHTTPD/([\d.]+)\r\n| p/JC-SHTTPD/ v/$1/ d/printer/ i/Sharp printer/
match http m|^HTTP/1\.0 .*\r\nDate: .*<html>\n<head>\n<title> Sun Java\(tm\) System Messenger Express </title>|s p/Sun Java System Messenger Express httpd/
match http m|^HTTP/1\.0 .*\r\nDate: .*\r\n\r\n<html>\n<head>\n<title>Login : Messenger Express</title>\n<script>\n|s p/Netscape Messenger Express httpd/
match http m|^HTTP/1\.0 200 OK\r\nDate: .*<title>Sun Java\[tm\] System Calendar Express (\d+) ([\w]+)</title>|s p/Sun Java System Calendar Express $1 httpd/ v/$2/
match http m|^HTTP/1\.0 200 OK\n\n<title>.* NDT server</title>\n| p/NDT httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: GeoHttpServer\r\n| p/GeoVision GeoHttpServer for webcams/ d/webcam/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: ATR/([\d.]+)\r\nWWW-Authenticate: Basic realm=\"ATI Switch\"\r\n| p/Allied Telesyn Rapier switch http config/ i/ATR httpd $1/ d/switch/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: ATR-HTTP-Server/([\d.]+)\r\nContent-Type: text/html\r\nWWW-Authenticate: Basic realm=\"Allied Telesyn Rapier (\w+)\"\r\n| p/Allied Telesyn Rapier $2 switch http config/ i/ATR httpd $1/ d/switch/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: UPS_Server/([\d.]+)\r\n.*\r\n<TITLE>ConnectUPS Web/SNMP Card</TITLE>|s p|Powerware ConnectUPS WEB/SNMP Card http config| i/UPS_Server httpd $1/ d/power-device/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: PortWise mVPN \(www\.portwise\.com\)\r\n|s p/PortWise mVPN httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: WYM/([\d.]+)\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"Camera Server\"\r\n| i/IP-Video embedded camera http config/ p/WYM httpd/ v/$1/ d/webcam/
match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-type: text/html\r\nContent-Length: \d+\r\n\r\n<html>\r\n\r\n<head>\r\n<title>Mercury HTTP Services</title>\r\n| p|Mercury/32 httpd| o/Windows/
# Wow! Temperature of the device! The Java version seems to be incorrect, though, so I'm excluding it
match http m|^HTTP/1\.0 200 OK\r\nDate: .*\r\nServer: Java/[\d.]+\r\nContent-type: text/html\r\nContent-length: \d+\r\n\r\n.*<TITLE>TINIWebServer</TITLE>.*Current temperature ([\d.]+) F<BR>|s p/TINIWebServer Java httpd/ i/Device temperature $1F/ o/TiniOS/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: Embedded HTTP Server ([\w. ]+)\r\nWWW-Authenticate: Basic realm=\"AP-Router\"\r\nConnection: close\r\n\r\n<HTML><HEAD><TITLE>401 Unauthorized</TITLE></HEAD>\n<BODY BGCOLOR=\"#ffffff\"><H4>401 Unauthorized</H4></BODY></HTML>\n| p/Topcom wireless router http config/ i/Embedded httpd $1/ d/router/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\nDate: .*\nThe requested URL '' was not found on the Divar\.<p>\nReturn to|s p/Bosch Divar closed circuit camera http config/ d/webcam/
match http m|^HTTP/1\.0 501 Unsupported method \('GET'\)\r\nServer: BaseHTTP/([\d.]+) Python/([\w.]+)\r\n| p/BaseHTTP/ v/$1/ i/Python SimpleXMLRPCServer; Python $2/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"Cable Modem\"\r\nContent-length: \d+\r\nContent-type: text/html\r\nConnect: Keep-Alive\r\n\r\n<html>\r\n<head><title>401 Unauthorized</title></head>\r\n<body><h1>401 Unauthorized</h1>\r\n<p>Access to this resource is denied; your client has not supplied the correct authentication\.</p></body>\r\n</html>\r\n| p|Coresma/Belkin Cable Modem httpd| d/router/
match http m|^HTTP/1\.1 200 OK\r\nServer: Virata-EmWeb/R([\d_]+)\r\n.*<!-- Begin Hiding\n         netscapeVersion =|s i/HP Deskjet 5800 http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/printer/
match http m|^HTTP/1\.1 200 OK\r\nServer: Virata-EmWeb/R([\d_]+)\r\n.*\n\n<title></title>\n\n\n\n\n<script language=\"JavaScript1\.1\">\n<!-- Begin Hiding\n netscapeVersion =|s i|HP PhotoSmart/Deskjet printer http config| p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/printer/
match http m|^HTTP/1\.0 200 OK\r\nServer: Sun_Ray_Admin_Server/([\d.]+)\r\n| p/SunRay http config/ v/$1/ o/Solaris/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: WatchGuard Firewall\r\nwww-authenticate: Digest realm=\"WatchGuard SOHO (.+) Configuration\"| p/WatchGuard SOHO $1 http config/ d/firewall/
match http m|^HTTP/1\.1 200 OK\r\nServer: WindWeb/([\d.]+)\r\nConnection: close\r\n.*\r\n<title>Cisco Web Accessible Phone Settings</title>\r\n|s p/Cisco 7935 IP Phone Conference Station http config/ i/WindWeb embedded httpd $1/ d/VoIP phone/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: \r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"NETGEAR (D\w+)\"\r\n| p/Netgear $1 router http config/ d/router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: \r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"NETGEAR (DG[-\w+]+) \"| p/Netgear $1 router http config/ d/router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: \r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"NETGEAR DG\w+  \"\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<html>\n<head>\n\n<meta name=\"description\" content=\"DG(\w+) FR \d+\">\n| p/Netgear DG$1 FR WAP http config/ i/French/ d/WAP/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: \r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"NETGEAR (\w+) *\"\r\n| p/Netgear $1 router http config/ d/broadband router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: \r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"NETGEAR (\w+) ADSL2\+ Modem\"\r\n| p/Netgear $1 ADSL router http config/ d/broadband router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: NetPort Software ([\d.]+)\r\n.*<TITLE>Connection Information</TITLE><!-- Copyright\(C\) \d+ Efficient Ne..orks -->|s p/Efficient Networks Speedstream DSL router http config/ d/router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: NetPort Software ([\d.]+)\r\n| p/NetPort embedded httpd $1/
match http m|^HTTP/1\.1 400 Bad Request\r\nContent-Type: text/html\r\nDate: .*\r\nContent-Length: \d+\r\nVia: [\d.]+ Application and Content Networking System Software ([\d.]+)\r\n| p/Cisco ACNS http cache/ v/$1/ o/IOS/
match http m|^HTTP/1\.0 \d\d\d .*<a href=\"http://www\.cisco\.com/\">Application and Content Networking (System )?Software ([\d.]+)</a>\)\n</BODY></HTML>\n|s p/Cisco ACNS httpd/ v/$2/ o/IOS/
match http m|^HTTP/1\.0 \d\d\d .*<title>VLC media player</title>\n|s p/VLC media player http interface/
match http m|^HTTP/1\.0 \d\d\d .*<a href=\"http://www\.videolan\.org/\">VLC media player ([\d.]+)[^<]+</a> \(http interface\)</h2>\n|s p/VLC media player http interface/ v/$1/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: \r\nContent-Type: text/html\r\nDate: .*\r\nLast-Modified: .*\r\nAccept-Ranges: bytes\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"WebAdmin\"\r\n\r\n<HTML>\n<HEAD><TITLE>401 Unauthorized</TITLE></HEAD>\n<BODY BGCOLOR=\"#cc9999\" TEXT=\"#000000\" LINK=\"#2020ff\" VLINK=\"#4040cc\">\n| p/ActionTec DSL http config/ d/broadband router/
match http m|^HTTP/1\.0 302 Document Follows\r\nLocation: https?:///private/welcome\.ssi\r\nConnection: close\r\n\r\n$| p|BladeCenter/IBM RSA2 http config| d/remote management/
match http m|^HTTP/1\.0 200 OK\r\nServer: \r\nContent-Type: text/html; charset=iso-8859-1\r\nDate:.*//inserted by Edward on 2004/01/07 for user pressing \"Enter\" to login if \"Username\" and \"Password\" are right|s p/D-Link DSL router http config/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: OmniHTTPd/([\d.]+)\r\n|s p/OmniHTTPd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: OmniSecure/([\w.]+)\r\n|s p/OmniSecure httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\n\r\n<HTML><HEAD><META HTTP-EQUIV=\"refresh\" CONTENT=\"0;URL=/bluedragon/nonadmin\.cfm\"></HEAD></HTML>\n\n| p/Blue Dragon Built-in httpd/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: MirandaWeb/([\d.]+)\r\n|s p/MirandaWeb http plugin for Miranda-IM/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 200 OK\r\nPragma: no-cache\r\nContent-Type: text/html\r\n\r\n.*<title>OfficeConnect Wireless 11g Cable/DSL Gateway</title>\n|s p/3Com OfficeConnect wireless router http config/ d/router/
match http m|^HTTP/1\.0 200 OK\r\nPragma: no-cache\r\nContent-Type: text/html\r\n\r\n.*<title>OfficeConnect 11Mbps Wireless Access Point</title>\n|s p/3Com OfficeConnect wireless access point http config/ d/router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Mirapoint/([-\w_.]+)\r\n| p/Mirapoint email appliance http interface/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*<title>Network Storage Link for USB 2\.0 Disks</title>\r\n\r\n|s p/Linksys NSLU2 http config/ d/storage-misc/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Unknown\r\n.*<title>NetEnforcer Manager</title>|s p/Allot NetEnforcer bandwidth management http config/ d/load balancer/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: \r\nContent-Type: text/html; charset=iso-8859-1\r\n.*<meta name=\"description\" content=\"(DG\d+)\">\r\n<title>NetGear Gateway Setup</title>|s p/Netgear $1 router http config/ d/router/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: LabVIEW/([\d.]+)\r\n| p/National Instruments LabVIEW integrated httpd/ v/$1/ d/specialized/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: [\d.]+/[\d.]+\r\n.*<link rel=\"stylesheet\" href=\"\.\./www/neronet\.css\" type=\"text/css\">|s p/NeroNET Nero Burning ROM http plugin/
match http m|^HTTP/1\.1 302 Found\r\nLocation: http://www\.cfauth\.com/\?cfru[\w=]+\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n| p/CacheFlow http cache/ o/CacheOS/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nDate: .*\r\nServer: Groove-Relay/([\d.]+)\r\n| p/Groove-Relay http service/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Askey Software ([\d.]+)\r\nDate: .*\r\nContent-type: text/html\r\n\r\n<html>\r\n\r\n<head>\r\n<title>Cable Modem Web Page</title>\r\n<meta name=\"GENERATOR\" content=\"Microsoft FrontPage 4\.0\">\r\n| p/Motorola VoIP adapter http config/ i/Askey httpd $1/ d/VoIP adapter/
match http m|^HTTP/1\.0 200 OK\r\nServer: Askey/([\d.]+)\r\nMIME-version: 1\.0\r\nContent-type: text/html\r\n\r\n.*<b>This \r\n        website is blocked by the URL filter of Wireless Router\. Please browse to another \r\n        site or go back\.</b>|s p/Siemens Gigaset SE505 WAP http config/ d/WAP/

match http m|^HTTP/1\.0 404 File Not Found\r\nContent-Type: text/html\r\n\r\n<b>The source you requested could not be found\.</b>\r\n$| p/Icecast http statistics plugin/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\n.*<title>Icecast Streaming Media Server</title>\n|s p/Icecast http statistics plugin/
match http m|^HTTP/1\.0 200 OK\r\n.*title>Security</title>.*font size=4 face=Arial>This unit is password protected</font></p><p align=center><font size=3 face=Arial>Please enter the correct password  to access the web pages</font>|s p|VoIP/POTS gateway http config| d/VoIP adapter/

match http m|^HTTP/1\.0 \d\d\d .*<title>CiscoSecure ACS Login</title>|s p/Cisco Secure ACS login/ o/IOS/
match http m|^HTTP/1\.0 \d\d\d .*<title>CiscoSecure ACS Trial Login</title>\r\n|s p/Cisco Secure ACS login/ i/Trial version/ o/IOS/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: httpd\r\n.*<title>Motorola HomeNet Product </title>|s p/Motorola broadband router http config/ d/broadband router/
match http m|^HTTP/1\.0 200 OK\nServer: Olicom/v([\d.]+)\nExpires: .*\nContent-Length: \d+\n\n<html>\r\n\r\n<head>\r\n<title>(CF\w+) Olicom Fast Ethernet L3 Switch \([\d.]+\)</title>| p/Olicom $2 switch http config/ i/Olicom httpd $1/ d/switch/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: text/html\r\nPragma: no-cache\r\nCache-Control: no-cache\r\n\r\n<html><head>\n<title>\n  Authentication Form \n</title> \n</head> \n \n<BODY BGCOLOR=\"#000000\" TEXT=\"#00FF00\"> \n\n<p> \n<h3 align=left><font face=\"arial,helvetica\">Client Authentication Remote \nService</font></h3>| p/Checkpoint firewall client authentication httpd/ d/firewall/
match http m|^HTTP/1\.0 500 Internal Server Error\r\nCONTENT-LENGTH: 42\r\n\r\nYour request cannot be properly processed\.$| p/DVR 2400 Security Camera web interface/ d/webcam/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: IBM-HTTP-Server/([\d.]+)\r\n| p/IBM httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Agranat-EmWeb/R([\d_]+)\r\nContent-Length: \d+\r\nContent-Type: text/html\r\nETag: \"[^"]+\"\r\n.*<FRAME NAME=\"logon\" SRC=\"logon\.html\" SCROLLING=\"auto\">\n</FRAMESET>\n<BODY BGCOLOR=\"#FFFFFF\">\n</BODY>\n</HTML>\n|s i/Nortel BayStack switch http config/ p/Agranat-EmWeb/ v/$SUBST(1,"_",".")/ d/switch/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: WebSnmp Server Httpd/([\d.]+)\r\n| p/Apache WebSnmp module/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\nContent-type: text/html\n.*<frame src=\"PrintServer\.htm\" name=\"PrintServer\" scrolling=\"auto\">.*<a href=\"PrintServer\.htm\">Enter PrintServer utilities</font>|s p|Gembird/Hawking/Netgear print server http config| d/print server/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: \r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"ADSL Router \(ANNEX A\)\"\r\n.*System Authentication Failed\.|s p/TRENDnet DSL router http config/ d/router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Plan9\r\n|s p/Plan 9 httpd/ o/Plan 9/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: IceWarp WebSrv/([\d.]+)\r\n| p/IceWarp webmail httpd/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: IceWarp/([\d.]+)\r\n| p/IceWarp webmail httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nConnection: close\r\nServer: WindWeb/([\d.]+)\r\nDate: .*\r\nContent-Type: \r\n\r\n<html>\n<head>\n<title>DW([\d]+) System Control Center</title>| p/Hughes DirecWay $2 satellite router http config/ i/WindWeb embedded httpd $1/ d/router/
match http m|^HTTP/1\.1 \d\d\d .*\nDate: .*\nServer: BBIagent\.Net/([\d.]+) Powered by HKSP\.COM\n| p/BBIagent.Net httpd/ v/$1/ o/Linux/
match http m|^HTTP/1\.0 200 Ok\r\nContent-Type: text/html\r\nCache-Control: no-cache\r\nExpires: 0\r\nSet-Cookie: hpRibSession=;| p/HP Remote Lights-Out Edition II http config/ d/remote management/
match http m|^HTTP/1\.1 200 Ok\r\n.*Copyright 2001,2003 Hewlett-Packard Development Company.*<title>\r\nData Frame - Browser not HTTP 1\.1 compatible\r\n</title>|s p/HP Remote Lights-Out http config/ d/remote management/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: Allegro-Software-RomPager/ ([\d.]+)\r\n\r\n<HTML><HEAD>\n<script Language=\"JavaScript\">\nfunction login\(\)\n{\ntop\.location = \"/alogin\.htm\"\n}\nfunction delay\(\)|s p/APC Masterswitch power controller http interface/ i/Allegro RomPager $1/ d/power-device/
match http m|^HTTP/1\.0 \d\d\d .*\r\nWWW-Authenticate: Basic realm=\"Masterswitch\"\r\nServer: Allegro-Software-RomPager/([\d.]+)\r\n\r\n| p/APC Masterswitch power controller http interface/ i/Allegro RomPager $1/ d/power-device/
match http m|^HTTP/1\.[01] 403 Forbidden\r\nContent-Type: text/html\r\nServer: Allegro-Software-RomPager/ *([\w._-]+)\r\n.*<H1>Notice</H1>\nSomeone is currently logged into the APC Management Web Server\.<p>|s p/APC Masterswitch power controller http interface/ i/server busy; Allegro RomPager $1/ d/power-device/
match http m|^HTTP/1\.0 401 Authorization Required\r\nWWW-Authenticate: BASIC realm=\"Administrator or User\"\r\n\r\nPassword Error\. \r\n\r\n$| p/D-Link web camera http config/ d/webcam/
match http m|^HTTP/1\.0 \d\d\d .*\nContent-Length: \d+\n.*<B>Cable Modem Description :</B>.*<P>ZyXEL Prestige (\w+), HW V([\d.]+), SW ZyNOS V([\d.]+)\(|s p/ZyXEL Prestige $1 router http config/ i/HW version $2; ZyNOS $3/ d/broadband router/ o/ZyNOS/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: micro_httpd\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"ZyXEL\"\r\n| p/ZyXEL Cable Modem http config/ d/broadband router/ i/micro_httpd/
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"(FVL[\w+]+)\"\r\nContent-type: text/html\r\n\r\n401 Unauthorized| p/Netgear $1 router http config/ d/router/

match http m|^HTTP/1\.0 200 Ok\r\nConnection: close\r\nContent-Type: text/html\r\n\r\n<HTML><FRAMESET COLS=\"23%,\*\"><FRAME NAME=\"side\" SRC=\"MENUNET\.htm\"><FRAME NAME=\"middle\" SRC=\"HOME\.htm\"></FRAMESET><NOFRAMES>Your Browser must support frames to view this page\.</NOFRAMES></HTML>$| p/OkiLan 6020e print server http config/ d/print server/
match http m|^HTTP/1\.0 \d\d\d .*Server: Web-Server/([\d.]+)\r\nContent-Type: text/html; charset=UTF-8\r\n.*<title>Web Image Monitor</title>\n|s p/Ricoh Aficio printer web image monitor/ i/Web-Server httpd $1/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*Server: Web-Server/([\d.]+)\r\nContent-Type: text/html; charset=UTF-8\r\n.*<title>websys default page</title>\n|s p/Ricoh Aficio printer web image monitor/ i/Web-Server httpd $1/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*\r\nSet-Cookie: ssnid=[^;]+; path=/;\r\nContent-Type: text/html; charset=[Uu][Tt][Ff]-8\r\nWWW-Authenticate: Basic realm=\"sapbc\"\r\n| p/SAP Business Connector/
match http m|^HTTP/1\.1 \d\d\d .*\r\nContent-Type: text/html\r\n.*<!-- Copyright \(c\) \d+-\d+, Fuji Xerox Co\., Ltd\. All Rights Reserved\. -->\r\n.*<TITLE>\r\nDocuColor (\d+) - [\d.]+\r\n</TITLE>|s p/Xerox DocuColor $1 printer http config/ d/printer/
match http m|^HTTP/1\.1 \d\d\d .*\r\nContent-Type: text/html\r\nDate: .*\r\nAllow: GET, HEAD\r\nServer: Spyglass_MicroServer/([-\w_.]+)\r\n\r\n<html>\n\n<head>\n\n<title>  PhaserLink Printer Management Software  </title>| p/Tektronix PhaserLink printer http config/ i/Spyglass httpd $1/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-Type: text/html\r\n\r\n<HTML><TITLE>Lexmark Optra ([^<]+)</TITLE>| p/Lexmark Optra $1 printer http config/ d/printer/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Rapid Logic/([\d.]+)\r\n.*<!-- Copyright &#copy; \d+-\d+ Hewlett Packard Company\. All rights reserved\. -->\r\n.*<title>hp business inkjet ([^<]+)</title>|s p/HP Business Inkjet $2 printer http config/ i/Rapid Logic httpd $1/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: OpenLink-Web-Configurator/([\d.]+)\r\n| p/OpenLink http config/ v/$1/
match http m|^HTTP/1\.0 401 Unauthorized\nServer: wr_httpd/([\d.]+) .*\nWWW-Authenticate: Basic realm=\"WebRamp \(use wradmin as the User Name\)\"\n| p/Webramp router http config/ i/wr_httpd $1/ d/router/
match http m|^HTTP/1\.1 \d\d\d .*{FONT: bold 10pt Arial,Helvetica,sans-serif; COLOR: white;}.*{FONT: 10pt Arial,Helvetica,sans-serif; COLOR: black; BORDER: Medium White None; border-collapse: collapse}.*{\tCOLOR: #b5b5e6}.*{COLOR: #b5b5e6}.*src=Gozila\.js>|s p/Linksys BEFW11S4 router http config/ d/router/
match http m|^<html>\n<title>DGS-(\w+) *(Login)?</title>\n| p/D-Link DGS-$1 Gigabit switch http config/ d/switch/
match http m|^HTTP/1\.1 401 Authorized Required\r\nWWW-Authenticate: Basic realm=\"Linksys WML(\w+)\"\r\n| p/Linksys WML$1 media device http config/ d/media device/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: CERN/([-\w.]+)\r\n|s p/CERN httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\n<TITLE>KONICA MINOLTA PageScope Light for (Di\d+)</TITLE>\r\n|s p/Konica Minolta Di$1 printer http config/ d/printer/ i/PageScope Light/
match http m|^HTTP/1\.1 \d\d\d .*\r\n<title>KONICA MINOLTA PageScope Web Connection</title>\r\n|s p/Konica Minolta PageScope Web Connection/ d/printer/
match http m|^HTTP/1\.1 \d\d\d .*\r\n<TITLE>KONICA MINOLTA PageScope Web Connection for (\w+)</TITLE>\r\n|s p/Konica Minolta $1 printer http config/ d/printer/ i/PageScope Web Connection/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nDate: .*\r\nServer: Embperl/([\w.]+) Apache/([\w.]+) \(Fedora\)\r\n| p/Apache httpd/ v/$2/ i/Embperl $1; Fedora/ o/Linux/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nDate: .*\r\nServer: Embperl/([\w.]+) Apache/([\w.]+) \(Debian GNU/Linux\) (.*)\r\n| p/Apache httpd/ v/$2/ i/Embperl $1; Debian; $3/ o/Linux/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nDate: .*\r\nServer: Embperl/([\w.]+) Apache/([\w.]+) \(Debian GNU/Linux\)\r\n| p/Apache httpd/ v/$2/ i/Embperl $1; Debian/ o/Linux/
match http m|^.*<address>Apache/([\d.]+) \([^)]+\) ?(.*) Server at ([-\w_.]+) Port \d+</address>\n</body></html>\n|si p/Apache httpd/ v/$1/ i/$2/ h/$3/
match http m|^.*<address>Apache/([\d.]+) \([^)]+\) Server at ([-\w_.]+) Port \d+</address>\n</body></html>\n|si p/Apache httpd/ v/$1/ h/$2/
match http m|^.*<address>Apache/([\d.]+) Server at ([-\w_.]+) Port \d+</address>\n</body></html>\n|si p/Apache httpd/ v/$1/ h/$2/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: SiteScope/([\d.]+) .*\r\n| p/Mercury SiteScope Application Managment httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: \r\nDate: .*\r\n\r\n<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.01 Transitional//EN\">\n<html>\n<head>\n<title>OSBRiDGE (\w+) Login Page</title>\n|s p/OSBRiDGE $1 router http config/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: SilverStream Server/([\d.]+)\r\n\r\n|s p/SilverStream Application Server httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*<title>Welcome to Squeezebox</title>|s p/Slim Devices Squeezebox http config/ d/media device/
match http m|^HTTP/1\.0 \d\d\d .*\r\nWWW-Authenticate: Basic realm=\"VPN\"\r\nContent-Type: text/html\r\nAccept-Ranges: bytes\r\nConnection: close\r\nServer: Embedded HTTP Server v([\d.]+), \d+, Magic Control Technology Inc\.\r\n\r\n| p/IOGear BOSS http config/ i/MCT Embedded httpd $1/ d/storage-misc/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nDate: .*\r\nServer: PicoWebServer\r\n| p/Newmad PicoWebServer/ i/WinCE/ d/PDA/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: tivo-httpd-1:([^\r\n]+)\r\n| p/TiVo To Go httpd/ v/$1/ d/media device/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Dahlia/([\d.]+) \([^)]+\)\r\n.*<title>Sony Library Administration Menu</title>\r\n|s p/Sony Storestation http interface/ i/Dahlia httpd $1/ d/storage-misc/
match http m|^HTTP/1\.0 200 OK\r\n.*<th width=\"50%\">TivoWebPlus Project - v([\d.]+)&nbsp;</th>|s p/TiveWebPlus Project httpd/ v/$1/ d/media device/
match http m|^HTTP/1\.0 200 OK\r\n.*<TITLE>Main Menu \[[\w._-]+\]</TITLE>.*<A title=\"Return to Main Menu\" HREF=\"/\">TivoWebPlus</A>|s p/TiveWebPlus Project httpd/ d/media device/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: WEBrick/([\d.]+) \(Ruby/([\d.]+)/([-\d]+)\)\r\n|s p/WEBrick httpd/ v/$1/ i/Ruby $2 ($3)/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: WEBrick/([\d.]+) \(Ruby/([\d.]+)/([-\d]+)\) OpenSSL/([-\w_.]+)\r\n|s p/WEBrick httpd/ v/$1/ i/Ruby $2 ($3); OpenSSL $4/
match http m|^HTTP/1\.0 \d\d\d .*<title>FRITZ!Box|s p/FRITZ!Box http config/ d/broadband router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-Length: \d+\r\nContent-Type: text/html\r\n\r\n<HTML><HEAD><TITLE>404 Not Found \(ERR_NOT_FOUND\)</TITLE></HEAD><BODY><H1>404 Not Found</H1><BR>ERR_NOT_FOUND<HR><B>AR7 Webserver</B>| p/FRITZ!Box router http config/ i/TI AR7 chip/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: WebCam2000/([\d.]+) \(Windows; http://www\.webcam2000\.info/\)\r\n| p/WebCam2000 httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 401 Login failed!\r\nServer: micro_httpd\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"WRT54GXv2\"\r\n| p/Linksys WRT54GXv2 http config/ d/broadband router/ i/micro_httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\n\r\n<HTML>\n<HEAD><TITLE>OpenWrt</TITLE>|s p/OpenWrt BusyBox httpd/ d/WAP/ o/Linux/
match http m|^HTTP/1\.0 \d\d\d .*\n\t\t<title>OpenWrt Administrative Console</title>|s p/OpenWrt BusyBox httpd/ d/WAP/ o/Linux/
match http m|^HTTP/1\.0 \d\d\d .*<meta http-equiv=\"refresh\" content=\"0; URL=/?cgi-bin/webif[\w/.]+sh\" />\n|s p/OpenWrt BusyBox httpd/ d/WAP/ o/Linux/
match http m|^HTTP/1\.0 401 Unauthorized\r\n.*WWW-Authenticate: Basic realm=\"OpenWrt\"\r\n\r\n|s p/Linksys WRT OpenWrt http config/ d/WAP/ o/Linux/
match http m|^HTTP/1\.0 401 Unauthorized\r\n.*WWW-Authenticate: Basic realm=\"WRT54GS\"\r\n|s p/Linksys WRT54GS WAP http config/ d/WAP/ o/Linux/
match http m|^HTTP/1\.0 401 Unauthorized\r\n.*WWW-Authenticate: Basic realm=\"[Tt]omato\"\r\n|s p/Linksys WRT54G WAP http config/ d/WAP/ o/Linux/ i/Tomato firmware/
match http m|^HTTP/1\.[01] 401 Unauthorized\r\n.*WWW-Authenticate: Basic realm=\"WRT(\w+)\"\r\n|s p/Tomato WAP firmware httpd/ i/Linksys WRT$1 WAP/ d/WAP/ o/Linux/
match http m|^HTTP/1\.0 401 Unauthorized\r\nDate: .*\r\nContent-Type: text/html; charset=utf-8\r\nCache-Control: no-cache, no-store, must-revalidate, private\r\nExpires: Thu, 31 Dec 1970 00:00:00 GMT\r\nPragma: no-cache\r\nWWW-Authenticate: Basic realm=\"[^"]*\"\r\nConnection: close\r\n\r\n<html><head><title>Error</title></head><body><h2>401 Unauthorized</h2> Unauthorized</body></html>$| p/Tomato WAP firmware httpd/ d/WAP/
match http m|^HTTP/1\.0 401 Unauthorized\r\n.*WWW-Authenticate: Basic realm=\"Linksys WAG(\w+) ?\"\r\n|s p/Linksys WAG$1 WAP http config/ d/WAP/ o/Linux/
match http m|^HTTP/1\.0 401 Unauthorized\r\n.*WWW-Authenticate: Basic realm=\"Linksys WRT(\w+)\"\r\n|s p/Linksys WRT$1 WAP http config/ d/WAP/ o/Linux/
match http m|^HTTP/1\.0 \d\d\d .*var path='http://www\.axis\.com/cgi-bin/prodhelp\?prod=axis_(\d+)&ver=([\d.]+)|s p/AXIS $1 print server http config/ v/$2/
match http m|^HTTP/1\.0 200 OK\r\nHTTP/1\.0 200 OK\r\nServer: ap\r\n.*<title>NetGear Remote Bridge Setup</title>|s p/Netgear ethernet Bridge http config/ d/bridge/

match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Virata-EmWeb/R([\d_]+)\r\n.*<TITLE>optiPoint ([\w .]+) Home Page</TITLE>|s i/Siemens optiPoint $2 VoIP phone http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/VoIP phone/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Virata-EmWeb/R([\d_]+)\r\n.*<TITLE>optiPoint(\d+)Entry Home Page</TITLE>|s i/Siemens optiPoint $2 entry http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/VoIP phone/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Virata-EmWeb/R([\d_]+)\r\n.*<TITLE>optiPoint(\d+)Standard Home Page</TITLE>|s i/Siemens optiPoint $2 standard http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/VoIP phone/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Virata-EmWeb/R([\d_]+)\r\n.*<TITLE>optiPoint(\d+)Advance Home Page</TITLE>|s i/Siemens optiPoint $2 advance http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/VoIP phone/

match http m|^HTTP/\d\.\d \d\d\d .*\r\nServer: Mathopd/([\w.]+)\r\n| p/Mathopd httpd/ v/$1/ o/Unix/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: ml_www/(.*)\r\n| p/ml_www WinAmp control httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 302 Redirect\r\nServer: GoAhead-Webs\r\nDate: .*\r\nPragma: no-cache\r\nCache-Control: no-cache\r\nContent-Type: text/html\r\nLocation: http://Netlinx/WebControl\.asp\r\n\r\n| p|AMX NetLinx A/V control| i/GoAhead embedded httpd/ d/media device/
match http m|^HTTP/1\.0 200 OK \r\nCache-Control: max-age=60\r\nContent-type: text/html; charset=ISO-8859-1\r\n\r\n<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.01 Frameset//EN\" >\r\n<HTML>\r\n    <HEAD><TITLE>SandvallsangFSK: (\w+)</TITLE>| p/Kirk $1 VoIP gateway http config/ d/VoIP adapter/
match http m|^HTTP/1\.1 200 OK\r\nConnection: close\r\nPragma: no-cache\r\n.*<title>POPFile Control Center</title>\n|s p/POPFile http control center/
match http m|^HTTP/1\.1 403 Forbidden \( Der Server hat den angegebenen URL \(Uniform Resource Locator\) verweigert\. Wenden Sie sich an den Serveradministrator\.  \)\r\n| p/Microsoft IIS httpd/ i/German/ o/Windows/
match http m|^HTTP/1\.1 403 Forbidden \( Der Server hat die angegebene URL verweigert\. Wenden Sie sich an den Serveradministrator\.  \)\r\n| p/Microsoft IIS httpd/ i/German/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: fhttpd/([\d.]+)\r\n| p/fhttpd/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\nContent-Type: text/html\r\nContent-Length: \d+\r\nCache-Control: no-cache\r\n\r\n<html>\r\n<head><meta charset=\"utf-8\">\r\n<title> Home </title>\r\n<script language=\"JavaScript\">\r\n<!--\r\n// the start of Cookie related function\r\nfunction getCookieVal \(offset\) {  \r\n| p/Samsung ML-2251N printer http config/ d/printer/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: Agranat-EmWeb/R([\d_]+)\r\nWWW-Authenticate: Basic realm=\"Siemens Web User Interface\"\r\n\r\n401 Unauthorized\r\n| i/Siemens router http config/ p/Agranat-EmWeb/ v/$SUBST(1,"_",".")/ d/router/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\" /\"\r\nContent-type: text/html\r\nContent-length: 0\r\n\r\n$| p|Casi-Rusco camera/Bestelco VoIP phone http config|
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: MyServer ([-\w.]+)\r\n|s p/MyServer httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Quantum Corporation\./([\d.]+)\r\n| p/Quantum backup appliance http config/ v/$1/ d/storage-misc/
match http m|^<html><head><title>ServiceRegistry</title><META HTTP-EQUIV=\"Pragma\" CONTENT=\"no-cache\"></head><basefont size=\"2\" face=\"Arial\" color=\"Black\">.*<br><h1><i>ServiceRegistry</i></h1>\r\nAvailable commands:\r\n<ul>| p/HP SAN Manager ServiceRegistry httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\nWWW-Authenticate: Basic realm=\"HP ISEE @| p/HP ISEE httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Simple java\r\n.*<title>hp OpenView storage area manager - GUI download</title>|s p/HP OpenView Storage Area Manager httpd/ i/Simple java httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Micro-Web\r\nContent-type: text/html\r\n\r\n<html>\r\n<head>\r\n<TITLE> HP StorageWorks MSL Tape Library Management Console </TITLE>\n| p/HP StorageWorks MSL Tape Library http config/ i/Micro-Web httpd/ d/storage-misc/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: RapidLogic/([\d.]+)\r\n.*<HTML>\n<HEAD>\n<TITLE>Switch Explorer</TITLE>\n|s p/Fabric switch http config/ i/RapidLogic httpd $1/ d/switch/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Mono-XSP Server/([\d.]+) Unix\r\n| p/Mono-XSP .NET httpd/ v/$1/ o/Unix/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: SimpleHTTP/([\d.]+) Python/([\d.]+)\r\n| p/Karrigell Python httpd/ i/SimpleHTTP $1; Python $2/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Cougar ([\d.]+)\r\n|s p/VideoLAN Server streaming media/ i/Cougar $1/
match http m|^HTTP/1\.0 404 Not found\r\n.*<title>Error 404</title>.*<a href=\"http://www\.videolan\.org\">VideoLAN</a>|s p/VideoLAN Server streaming media/
match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-type: text/html; charset=UTF-8\r\nCache-Control: no-cache\r\nContent-Length: \d+\r\n.* - - - - >\r?\n<  index\.html: VLC media player web interface\r?\n|s p/VLC media player http interface/
match http m|^HTTP/1\.0 \d\d\d .*<title>mikrotik routeros > administration</title>.*font-size: 9px\">mikrotik routeros ([\d.]+) administration|s p/MikroTik router http config/ i/RouterOS $1/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*<title>mikrotik routeros > administration</title>|s p/MikroTik router http config/ d/router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: thttpd-alphanetworks/([\d.]+)\r\nContent-Type: text/html\r\nDate: .*\r\nLast-Modified: .*\r\nAccept-Ranges: bytes\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"Broadband Router\"\r\n\r\n<HTML><HEAD><TITLE>401 Unauthorized</TITLE></HEAD><BODY onLoad=javascript:document\.forms\[0\]\.submit\(\);>| p/FiberLine router http config/ i/thttpd-alphanetworks $1/ d/router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: RMC Webserver ([\d.]+)\r\n.*<title>Remote Access Controller</title>|s p/Dell Remote Access Controller http interface/ v/$1/ d/remote management/
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"PROJECTOR[3]?\" \r\nContent-Type: text/html\r\n\r\n<HTML><BODY><H2>HTTP Error 401 - Unauthorized</H2><HR></BODY></HTML>| p/Panasonic Video Projector http config/ d/media device/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Footprint ([\d.]+)/FPMCP\r\n| p/Sandpiper Footprint http load balancer/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: LogMeIn Web Gateway\r\n| p/LogMeIn remote access web gateway/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: ArGoSoft Mail Server Freeware, Version [\d.]+ \(([\d.]+)\)\r\n| p/ArGoSoft Mail Server Freeware httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-Type: text/html\r\nContent-Length: \d+\r\nConnection: close\r\nServer: Fastream NETFile Web Server ([\d.]+)\r\n| p/Fastream httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 200 \(OK\) \r\nPragma: No-Cache\r\nCache-Control: no-cache\r\nDate: .*\r\nServer: HTTP Server\r\n.*Copyright \d+, \d+ Nortel Networks\.|s p/Nortel Extranet switch http config/ i/WindWeb httpd/ d/switch/
match http m|^<html>\n<title>24-Port 10/100M Fast Ethernet Web Smart Switch</title>\n<frameset rows='60,\*'.*<frame name=main src=cgi_login noresize>\n|s p/TRENDnet SMART24B switch http config/ d/switch/
match http m|^HTTP/1.0 403 Forbidden\r\nServer: SI3PHX1/([\d.]+)\r\n| p/Prolexic DDoS protected httpd/ i|SE3PHX1/$1|
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: WebServer ([\d.]+)\r\nLast-Modified: .*\r\nETag: \"[-\w]+\"\r\nAccept-Ranges: bytes\r\n| p/Cryptologic httpd/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: WebServer/([\d.]+)\r\n.*<META http-equiv=\"Refresh\" content=\"0; Url=/trane/tsws/login\.htm\" >\n  <title>redirect</title>|s p/Trane Tracer Summit building control httpd/ v/$1/ d/remote management/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: HDS Hi-Track Server/([\d.]+)\r\n| p/Hitachi Data System http config/ i/Hi-Track httpd $1/ d/storage-misc/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: WebTrends HTTP Server ([\w.]+)\r\n| p/Webtrends httpd/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: WebTrends HTTP Server \r\n| p/Webtrends httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: Desktop On-Call HTTPD V([\d.]+)\r\n| p/IBM Desktop On-Call httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: OCServer\r\nContent-Type: text/html\r\n\r\n\n\n<!-- WebConnect HTML -->| p/WebConnect http service/ i/OCServer httpd/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: ENI-Web/R([\d_]+)\r\nWWW-Authenticate: Basic realm=\"standard@3Com\"\r\n\r\n| p/Speedstream DSL router http config/ i/ENI-Web httpd $1/ d/router/
match http m|^HTTP/1\.1 200 OK\r\nConnection: Keep-Alive\r\nKeep-Alive: timeout=180\r\nContent-Type: text/html\r\nContent-Length: \d+\r\n\r\n<html>\n<head>\n<META HTTP-EQUIV=\"EXPIRES\" CONTENT=\"0\">\n<meta http-equiv=\"Pragma\" Content=\"No-cache\">\n</head>\n<body>\n<center>\n<h3><BR>Sorry, the switch is already being managed\. Concurrent management is not allowed!\n</center>\n</body></html>\n\0| p/Compex switch http config/ d/switch/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: \r\n.*\r\n\r\n<HTML>\n<HEAD>\n<TITLE>Actiontec</TITLE>\n\n|s p/Actiontec DSL router http config/ d/router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: JavaWebServer/([\d.]+) \r\nContent-Length: .*<HEAD>\n<TITLE>CentreVu Explorer II</TITLE>\n|s p/Lucent CentreVu Explorer II http config/ d/telecom-misc/
match http m|^<!-- saved from url=\(\d+\)http://internet\.e-mail -->\n<html>\n\n<head>\n<title>HTML-Konfiguration</title>\n\n| p/Deutsche Telekom wireless router http config/ i/micro_httpd/ d/router/
match http m|^HTTP/1\.1 \d\d\d .*\nWWW-Authenticate: Basic realm=\"Web Host Manager\"\nConnection: close\nServer: whostmgr/([\d.]+)\n| p/whostmgr httpd/ v/$1/
match http m|^HTTP/1\.1 403 Forbidden \( The server denied the specified Uniform Resource Locator \(URL\)\. Contact the server administrator\.  \)\r\n| p/Microsoft IIS/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: RMC Webserver ([\d.]+)\r\nLast-Modified: .*\r\nAllow: GET, HEAD\r\nContent-Length: \d+\r\nContent-Type: text/html\r\n\r\n<HTML>\r\n<HEAD>\r\n<TITLE>TopTools Remote Control</TITLE>\r\n| p/HP TopTools http control/ i/RMC httpd $1/
# HP OpenView ITO agent (probably version 7.25) on Windows, port 381
match http m|^HTTP/1\.1 \d\d\d .*\r\nserver: BBC (\d[-.\w]+); com\.hp\.openview\.Coda (\d[-.\w]+)\r\n\r\n|s i/HP OpenView ITO agent - Coda $2/ p/BBC httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nserver: BBC (\d[-.\w]+); com\.hp\.openview\.bbc\.LLB[Ss]erver (\d[-.\w]+)\r\n\r\n|s i/HP OpenView ITO agent - LLB server $2/ p/BBC httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Servertec-IWS/([\d.]+)\r\n| p/Servertec IWS Java httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: DirectUpdate/([\d.]+)\r\n| p/DirectUpdate dynamic IP updater/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: CCS/Jigsaw/([\d.]+)\r\n|s p/Commerce One httpd/ i/Java Jigaw $1/
match http m|^HTTP/1\.1 \d\d\d .*Server: VisiBroker/([\d.]+)\r\n\r\n|s p/Borland VisiBroker CORBA httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Compaq Insight Manager XE ([\d.]+)\r\n|s p/Compaq Insight Manager XE httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: ISS-PXServer/1\.0\r\n|s p/ISS-PXServer httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Jigsaw/([\w.-]+)\r\n|s p/Java Jigsaw httpd/ v/$1/
match http m|^Language received from client: .*\nSetlocale: .*\n| p/AIX Web-based System Manager/ o/AIX/
match http m|^HTTP/1\.0 \d\d\d .*\r\nConnection: close\r\nServer: gnump3d2 ([\d.]+) \([\d/]+\)\r\n| p/GNUMP3d streaming server/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: SpyBot([\d.]+)\r\n| p/SpyBot httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Virata-EmWeb/R([\d_]+)\r\nContent-Type: text/html\r\n.*\r\n\r\n<HTML>\n<HEAD><TITLE>NBX NetSet</TITLE>\n|s i/3Com SuperStack 3 NBX switch http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/switch/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: WWW-KODEKS/([\d.]+)\r\n| p/Knowledge On Demand httpd/ v/$1/ o/Unix/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Ares ([\d.]+)\r\nConnection: Keep-Alive\r\n\r\n| p/Ares Galaxy P2P httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Paws/([\d.]+)\r\n.*<title>ParaSoft LicenseServer  ([\d.]+)</title>|s i/ParaSoft LicenseServer $2/ p/Paws/ v/$1/
match http m|^HTTP/1\.1 ERROR\r\nServer: Server: Paws/([^\r\n]+)\r\nDate: \d.*\r\nExpires: .*\r\nContent-type: text/html\r\nContent-length: 2\r\n\r\n\r\n$| p/Paws/ v/$1/ i/ParaSoft Concerto software development platform/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/plain\r\n\r\nNode: \d+\n| p/DSpy D2OL statistics httpd/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nConnection: close\r\nServer: WindWeb/([\d.]+)\r\nDate: .*\r\nContent-Type: text/html\r\n\r\n<HTML>\n<HEAD>\n<TITLE>Horizon Monitor  HTML</TITLE>\n| p/Sun Tape Library http config/ i/WindWeb httpd $1/ d/storage-misc/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: monit ([\d.]+)\r\n| p/monit httpd/ v/$1/ o/Unix/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Red Carpet Daemon/([\d.]+)\r\n\r\n| p/Red Carpet httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: CL-HTTP/([\d.]+) \(LispWorks; ([\d.]+)\)\r\n| p/CL-HTTPd/ v/$1/ i/LispWorks/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: SAP-Internet-SapDb-Server/([\d.]+)\r\n| p/SAP Internet DB httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: JTALKServer\r\n| p/JTALKServer httpd/
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"HostMonitor's Web Service\"\r\n\r\n| p/HostMonitor Web Service/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: iSoft Commerce Suite Server\r\n| p/iSoft Commerce Suite httpd/
match http m|^HTTP/1\.1 \d\d\d .*\.\r\nServer: MS \.NET Remoting, MS \.NET CLR ([\d.]+)\r\n| p/MS .NET Remoting httpd/ i/.NET CLR $1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: BSE ([\d.]+)\r\n| p/Pinnacle Showcenter http config/ i/BSE httpd $1/ d/media device/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: WebMail/([\d.]+)\r\nDate: .*\r\nContent-type: text/html\r\n\r\n<!-- top\.txt -->\r\n\r\n<HTML>\r\n<HEAD>\r\n<TITLE>WebMail Server</TITLE>\r\n| p/True North Soft WebMail httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 200 \r\nContent-Type: text/html\r\n\r\n<HTML><HEAD><TITLE>MX G2000 DEDICATED FILE SERVER</TITLE>| p/Murex G2000 file server httpd/
match http m|^HTTP/1\.1 \d\d\d .*\r\nConnection: close\r\nContent-Type: text/html\r\nContent-Length: \d+\r\nExpires: \d+\r\nCache-Control: no-cache\r\nServer: Indy/([\d.]+)\r\nLocation: /prtg\.htm\r\nSet-Cookie: PRTG4SESSION=| i/Paessler PRTG Traffic Grapher httpd/ p/Indy httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nConnection: close\r\nContent-Type: text/html\r\nContent-Length: \d+\r\nExpires: \d+\r\nCache-Control: no-cache\r\nServer: Indy/([\d.]+)\r\nLocation: /allsensors\.htm\r\n\r\n<HTML><BODY><B>301 Moved Permanently</B></BODY></HTML>\r\n| i/Paessler PRTG Traffic Grapher httpd/ p/Indy httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nConnection: close\r\nContent-Type: text/html\r\nContent-Length: \d+\r\nExpires: \d+\r\nCache-Control: no-cache\r\nServer: Indy/([\d.]+)\r\nLocation: /sensorlist\.htm\r\n\r\n| i/Paessler PRTG Traffic Grapher httpd/ p/Indy httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Indy/([\d.]+)\r\nWWW-Authenticate: Basic realm=\"Please enter your login for PRTG(\d)\"\r\n|s i/Paessler PRTG SNMP $2 bandwidth monitor/ p/Indy httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 301 Moved Permanently\r\nConnection: close\r\nContent-Type: text/html\r\nContent-Length: 56\r\nExpires: 0\r\nCache-Control: no-cache\r\nServer: Indy/([\w._-]+)\r\nLocation: /login\.htm\r\n\r\n<HTML><BODY><B>301 Moved Permanently</B></BODY></HTML>\r\n| i/Paessler PRTG Traffic Grapher http config/ p/Indy httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: PRTG/([\w._-]+)\r\n|s p/Paessler PRTG Traffic Grapher httpd/ v/$1/ i/Indy httpd/ o/Windows/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: _httpd\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"\.\"\r\nContent-type: text/html\r\nConnection: close\r\n\r\n<HTML><HEAD><TITLE>401 Unauthorized</TITLE></HEAD>\n<BODY BGCOLOR=\"#cc9999\"><H4>401 Unauthorized</H4>\nAuthorization required\.\n</BODY></HTML>\n| p/Kaspersky AntiVirus http admin/ v/4.X/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Indy/([\d.]+)\r\n.*\r\n<title>Server Monitor Lite</title>\r\n|s i/Pure Networking Server Monitor Lite http interface/ p/Indy httpd/ v/$1/
match http m|^HTTP/1\.0 .*\r\nConnection: close\r\nDate: .*\r\nServer: JavaOpServer\r\n| p/JavaOp httpd/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: SmarterTools/([\d.]+)\r\n.*SmarterStats.*; Professional Edition - v\.([\d.]+) - Customer Login Page\r\n|s p/SmarterStats http interface/ v/$2/ i/SmarterTools httpd $1/
match http m|^HTTP/1\.1 403 Forbidden \( Der Server hat den angegebenen URL verweigert\. Wenden Sie sich an den Serveradministrator\.| p/Microsoft IIS httpd/ i/German/ o/Windows/
match http m|^HTTP/1\.1 403 Forbidden \( Le serveur a refus\xc3\xa9 l'URL \(Uniform Resource Locator\) sp\xc3\xa9cifi\xc3\xa9e\. Contactez l'administrateur du serveur\.| p/Microsoft IIS httpd/ i/French/ o/Windows/
match http m|^HTTP/1\.1 403 Forbidden \( El servidor deneg\xc3\xb3 la direcci\xc3\xb3n URL \(Uniform Resource Locator\) especificada\. P\xc3\xb3ngase en contacto con el administrador del servidor\.| p/Microsoft IIS httpd/ i/Spanish/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Project Engine Server\r\n| p/Project Engine Server httpd/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Indy/([\d.]+)\r\nWWW-Authenticate: Basic realm=\"NetStatus Professional\"\r\n|s i/NetStatus Professional/ p/Indy httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: McAfee-Agent-HttpSvr/([\d.]+)\r\n| p/McAfee Agent httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: HoneydHTTP/([\d.]+) Python/([\d.]+)\r\n| p/Honeyd httpd/ v/$1/ i/Python $2/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: 3ware/([\d.]+)\r\n.*<title>3ware 3DM2 - ([-\w_.]+) - Summary</title>|s p/3ware 3DM2 Serial RAID http config/ v/$1/ h/$2/ d/storage-misc/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: 3ware/([\d.]+)\r\n.*<title>3DM2 - ([-\w_.]+) - Summary</title>|s p/3ware 3DM2 Serial RAID http config/ v/$1/ h/$2/ d/storage-misc/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: unknown\r\nLocation: https://xweb-ext/__extraweb__/\r\nSet-Cookie: EXTRAWEB_REFERER=| p/Aventail SSL VPN Concentrator http config/ d/security-misc/
match http m|^HTTP/1\.1 \d\d\d .*\r\nAccept: application/vnd\.syncml\+xml, application/vnd\.syncml\+wbxml\r\nCache-Control: no-store\r\nServer: MultiSync Plugin\r\n\r\nNo such file or directory\.|s p/SyncML PIM sync server for MultiSync/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: C4D/([\d.]+)\r\n| p/Cinema 4D Renderer http interface/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\nServer: servermgrd\r\nConnection: close\r\nContent-Type: text/html\r\n.*<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 3\.2 Final//EN\"><HTML>\r\n<HEAD>\r\n<TITLE>Server Admin module list</TITLE>|s p/Apple Server Monitor http interface/ o/Mac OS X/
match http m|^HTTP/1\.1 401 Authorization Required\r\nServer: servermgrd\r\nWWW-Authenticate: Basic realm = \"Server Admin\"\r\n.*The server could not verify that you are authorized to access the requested content\.<P>\r\n<HR>\r\n</BODY></HTML>\r\n\r\n|s p/Apple Server Monitor http interface/ o/Mac OS X/
match http m|^HTTP/1\.1 401 Authorization Required\r\nServer: servermgrd\r\nSupportsXMLRPC\r\nSupportsBinaryPlist\r\nContent-Type: \xe2\x80\xa0%\xc6\x92<\r\n| p/Mac OS X Server Admin http config/ o/Mac OS X/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: BBC ([\d.]+) ; /Hewlett-Packard/OpenView/AutoDiscovery/com\.hp\.openview\.OvAgency\.OvAgencyCommand ([\d.]+)\r\n\r\n|s p/HP OpenView AutoDiscovery http interface/ v/$1/ i/BBC httpd $1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nX-Powered-By: Servlet/([\d.]+)\r\n.*Server: Sun-Java-System/Application-Server\r\n|s p/Sun Java System Application Server httpd/ i/Servlet $1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Sun-Java-System/Application-Server\r\n| p/Sun Java System Application Server httpd/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Sun-Java-System-Application-Server/([^\r\n]+)\r\n| p/Sun Java System Application Server httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Sun-Java-System-Web-Server/([\d.]+)\r\n| p/Sun Java System httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nX-Powered-By: Servlet/([\d.]+)\r\n.*Server: Sun Java System Application Server Platform Edition ([\d_.]+)\r\n|s p/Sun Java System Application Server Platform Edition httpd/ v/$2/ i/Servlet $1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nX-Powered-By: Servlet/([\w._-]+)\r\n.*Server: Sun Java System Application Server ([\w._-]+)\r\n|s p/Sun Java System Application Server httpd/ v/$2/ i/Servlet $1/
match http m|^HTTP/1\.1 200 OK\r\n.*\r\nServer: Allegro-Software-RomPager/([\d.]+)\r\n\r\n.*<title>Netopia Home Page</title>|s p/Netopia DSL router http config/ i/Allegro RomPager embedded httpd $1/ d/router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nWWW-Authenticate: Basic realm=\"Netopia-(\w+)\"\r\nContent-Type: text/html\r\nServer: Allegro-Software-RomPager/([\d.]+)\r\n\r\n| p/Netopia $1 router http config/ i/Allegro RomPager httpd $2/ d/router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nContent-Type: text/html\r\nDate: .*\r\nPragma: no-cache\r\nServer: Allegro-Software-RomPager/([\d.]+)\r\n\r\n\n<html>\n<head>\n<title>\nNetopia Router</title>\n|s p/Netopia Cayman 334x router http config/ i/Allegro RomPager httpd $1/ d/router/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html; charset=BIG5\r\nPragma: No-cache\r\nServer: ACOS HTTPD/([\d.]+)\r\nCache-Control: no-cache\r\n.*<title>Authorization Page</title>.*action=\"checkAuthorization\" target=\"_self\">\r\n|s p/Foxconn VoIP TRIO 3C http config/ i/ACOS httpd $1/ d/VoIP phone/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: AltaVista Avhttpd ([\d.]+)\r\n| p/Altavista Enterprise Search httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Servage\.net Cluster \(Enhanced Apache\) \(Unix\) (.*)\r\n| p/Servage.net enhanced Apache/ i/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\n\r\n<!-- Login\.html -->\n\n\n.*<title>Login</title>.*colors\n\ndk blue: #adc3dc\nlt blue: #d2dae3\norange: #ee7d00\nlt orange: #FDDF97\n|s p/Aruba router http config/ d/router/
match http m|^HTTP/1\.1 302 Moved Temporarily\r\nDate: .*\r\nLocation: https://securelogin\.arubanetworks\.com/| p/Aruba router secure http config/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nConnection: close\r\nAccept-Ranges: none\r\n.*<title>Citrix Administration Tool</title>| p/Citric Secure Gateway http admin/ o/Windows/
match http m|^HTTP/1\.0 301 Moved Permanently\r\nCache-Control: no-cache\r\nConnection: close\r\nAccept-Ranges: none\r\nLocation: /CitrixLogonPoint/AccessGateway/\r\n\r\n| p/Citric Secure Gateway http admin/ o/Windows/
match http m|^HTTP/1\.0 301 Moved Permanently\r\nCache-Control: no-cache\r\nConnection: close\r\nAccept-Ranges: none\r\nLocation: https://([\w._-]+)/CitrixLogonPoint/Default/\r\nContent-Length: 0\r\n\r\n$| p/Citrix Access Gateway firewall http config/ o/Windows/ h/$1/ d/firewall/
match http m|^HTTP/1\.1 \d\d\d .*\r\nContent-Type: text/html; charset=utf-8\r\nConnection: close\r\nPragma: no-cache\r\nCache-Control: no-store\r\n.*<title>Instant Virtual Extranet</title>|s p/Juniper Seca HTTPS VPN appliance/ d/security-misc/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Nucleus WebServ\r\nWWW-Authenticate: Basic realm=\"/\"\r\n.*<H1>Authorization Required</H1></BODY></HTML>\r\n|s p/Allied Telesyn 802x switch http config/ i/Nucleus httpd/ d/switch/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: RapidLogic/([\d.]+)\r\nMIME-version: 1\.0\r\nContent-type: text/html\r\n\r\n<html>\r\n<head>\r\n<title>Spectrum24 Access Point</title>\r\n\r\n| p/Symbol Spectrum24 access point http config/ i/RapidLogic httpd $1/ d/router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"VoIP Configuration Web Server\"\r\nContent-type: text/html\r\n\r\n<html>\r\n<body><h1>401 Unauthorized</h1></body></html>\r\n$| p/Welltech Wellgate VoIP adapter http config/ d/VoIP adapter/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: Thunderstone-Texis/([\d.]+)\r\n| p/Thunderstone Texis search appliance http config/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"B49G\"\r\n| p/Gigabyte B49G WAP http config/ d/WAP/
match http m|^HTTP/1\.1 200 OK\r\nServer: WoWEmu\r\n| p/WoWEmu httpd/ i/World of Warcraft emulated server/
match http m=^HTTP/1\.1 \d\d\d .*\r\nServer: InkHTTP/([\d.]+) Python/([\d.]+)\r\nDate: .*<title>Wirehog \| =s p/Wirehog http transfer interface/ i/InkHTTP $1; Python $2/
match http m|^HTTP/1\.1 \d\d\d .*\r\nContent-Length: \d+\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<HTML><HEAD><TITLE>   IP PHONE 2 V([\d.]+)         </TITLE>| p/NG VoIP Phone 2 http config/ v/$1/ d/VoIP phone/
match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-Type: text/html; charset=UTF-8\r\nContent-Length: \d+\r\nConnection: close\r\n\r\n<!DOCTYPE html.*\n<title>WikiHome</title>\n</head>\n<body>\n<div id='header'>\n<form method='get' action='/?Search'>\n<table border='0' width='100%'>\n<tr>\n<td align='left' ><strong>WikiHome</strong>  \( <a href='\?edit' title='Edit this wiki page contents\. \[alt-j\]' accesskey='j'>Edit</a> \)|s p/Didiwiki httpd/
match http m|^HTTP/1\.0 400 Wrong Port\r\nServer: ConferenceRoom/IRC\r\nConnection: Close\r\nContent-type: text/html\r\n\r\n<HTML><HEAD><TITLE>Connection to Wrong Port</TITLE></HEAD>\r\n<BODY>You have connected to an IRC server as if it were a web server</BODY>\r\n</HTML>\r\n| p/ConferenceRoom ircd/
match http m|^HTTP/1\.1 400 Bad Request\r\nServer:httpd\r\nDate: .*\r\nContent-Type:text/html\r\n\r\n<html><title>400 Bad Request </title>                         <body> <h1> Bad Request or Syntax Error/Not able to                         understand the request| p/Sagem F@st router httpd/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: NETID/([\d.]+)\r\n| p/Optivity NetID httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: WYM/([\d.]+)\r\nConnection: close\r\nContent-Type: text/html\r\nContent-Length: \d+\r\nLast-Modified: .*\r\n\r\n<HTML>\n<HEAD>\n<TITLE>IP Camera</TITLE>\n| i/Aviosys IP Camera http config/ p/WYM httpd/ v/$1/ d/webcam/
match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-Type: text/html\r\nDate: .*\r\n\r\n<H1>\w+: A WebGroup/Virtual Host to handle / has not been defined\.</H1><BR><H3>\w+: A WebGroup/Virtual Host to handle [-\w_.:/]+ has not been defined\.</H3><BR><I>IBM WebSphere Application Server</I>| p/IBM WebSphere httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-Type: text/html\r\nDate: .*\r\n\r\n<H1>\w+: Un host WebGroup/Virtual per la gestione / non \xe8 stato definito\.</H1><BR><H3>\w+: A WebGroup/Virtual Host to handle [-\w_.:/]+ has not been defined\.</H3><BR><I>IBM WebSphere Application Server</I>| p/IBM WebSphere httpd/ i/Italian/
match http m|^HTTP/1\.0 404 Not Found\r\nContent-Type: text/html\r\nDate: .*\r\n\r\n<H1>\w+: Un host WebGroup/Virtual per la gestione / non \xe8 stato definito\.</H1><BR><H3>SRVE0017W: Un host WebGroup/Virtual per la gestione / non \xe8 stato definito\.</H3><BR><I>IBM WebSphere Application Server</I>| p/IBM WebSphere httpd/ i/Italian/
match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-Type: text/html;charset=ISO-8859-1\r\n\$WSEP: \r\nContent-Language: .*\r\nServer: WebSphere Application Server/([\d.]+)\r\n| p/IBM WebSphere httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\t<title>Strongdc\+\+ webserver - Login Page</title>\t|s p/StrongDC++ httpd/
match http m|^HTTP/1\.0 200 OK\r\nServer: HellBot\r\n| p/HellBot Trojan httpd/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: ENI-Web/R([\d_]+)\r\nWWW-Authenticate: Basic realm=\"standard@Modem\"\r\n\r\n| p/Efficient SpeedStream router http config/ i/ENI-Web httpd $1/
match http m|^<html>\n<title>48-Port 10/100/1000Mbps Web-Smart Gigabit Ethernet Switch</title>\n| p/D-Link 48-Port switch http config/ d/switch/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: MailEnable-HTTP/([\d.]+)\r\n| p/MailEnable httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 200 OK\r\nConnection: close\r\nContent-Type: text/html\r\nServer: Indy/([\d.]+)\r\n\r\n<HTML><BODY><B>200 OK</B></BODY></HTML>\r\n| i/WebRoot SpySweeper http config/ p/Indy httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nConnection: Close\r\nContent-Type: text/html\r\nDate: .*\r\nLocation: login\.php\r\nServer: Kerio Embedded WebServer ([\d.]+)\r\nX-Powered-By: PHP/([\d.]+)\r\n\r\n| p/Kerio Embedded httpd/ v/$1/ i/PHP $2/ o/Windows/
match http m|^HTTP/1\.1 401 Unauthorized\r\nDate: .*\r\nServer: Agranat-EmWeb/R([\d._]+)\r\nWWW-Authenticate: Basic realm=\"read@\"\r\n\r\n401 Unauthorized\r\n| i/3Com SuperStack II Switch http config/ p/Agranat-EmWeb/ v/$SUBST(1,"_",".")/ d/switch/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: and-httpd/(\d+\.\d+\.[-.\w]+) \(Debug\)|s p/and-httpd/ v/$1/ i/Debug version/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: and-httpd/(\d+\.\d+\.[-.\w]+) ([^\r\n]+)|s p/and-httpd/ v/$1/ i/$2/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: and-httpd/(\d+\.\d+\.[-.\w]+)|s p/and-httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: and-httpd|s p/and-httpd/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: httpd\r\nDate: .*\r\nWWW-Authenticate: Basic\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<HTML><HEAD><TITLE>401 Unauthorized</TITLE></HEAD>\n<BODY BGCOLOR=\"#cc9999\"><H4>401 Unauthorized</H4>\nAuthorization required\.\n</BODY></HTML>\n| p/Linksys Wireless-G DSL router http config/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nPragma: no-cach\r\nContent-Type: text/html; charset=windows-1251\r\n\r\n<HTML>\r\n<HEAD>\r\n<TITLE>UserGate report area</TITLE>\r\n| p/UserGate http report area/ o/Windows/
match http m|^<HTML>\r\n<HEAD>\r\n<TITLE>UserGate report area</TITLE>\r\n| p/UserGate http report area/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Kerio MailServer ([\d.]+) patch (\d+)\r\n\r\n|s p/Kerio MailServer http config/ v/$1 patch $2/ o/Windows/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: VOIP\r\nWWW-Authenticate: Digest realm=\"VOIP\", nonce=\"\w+\", opaque=\"\w+\",| p/ACT VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: KHAPI/([\d.]+) \(Linux\)\r\n|s p/KHAPI httpd/ v/$1/ o/Linux/
# HP OpenView ITO agent (probably version 7.25) on Windows, port 383
# Moved from RTSPRequest because fallback can take care of it
match http m|^HTTP/1\.1 \d\d\d.*\r\nContent-Type: text/html(?:; charset=us-ascii)?\r\nServer: Microsoft-HTTPAPI/([\d.]+)\r\n| p/Microsoft HTTPAPI httpd/ v/$1/ i|SSDP/UPnP| o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Mediasurface/([\d.]+)\r\n| p/Mediasurface CMS httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: RapidLogic/([\d.]+)\r\n.*<TITLE>WireSpeed Data Gateway</TITLE>|s p/WireSpeed Data Gateway router http config/ i/RapidLogic httpd $1/ d/router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: SmarterTools/([\d.]+)\r\n.*SmarterStats|s p/SmarterTools SmarterStats httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: SmarterTools/([\d.]+)\r\n| p/SmarterTools httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*<HTML><HEAD><TITLE>Scientific-Altanta WebStar Cable Modem</TITLE>|s p/Scientific-Altanta WebStar Cable Modem http config/ d/broadband router/
# WebStar DPC2100 and EPC2100
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: micro_httpd\r\n.*<title>Scientific-Altanta WebStar Cable Modem</title>|s p/Scientific Atlanta WebStar Cable Modem http config/ i/micro_httpd/ d/broadband router/
match http m|^HTTP/1\.0 302 Redirect\r\n.*\r\nServer: GoAhead-Webs\r\nDate: .*\r\nPragma: no-cache\r\nCache-Control: no-cache\r\nContent-Type: text/html\r\nLocation: http://Device/config/log_off_page\.htm\r\n\r\n| p/Dell PowerConnect http config/ d/switch/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"Enable Mode\"\r\nContent-Type: text/html\r\nServer: Allegro-Software-RomPager/([\d.]+)\r\n\r\n<HTML><HEAD><TITLE><script>document\.location\.href='/config/AccessNotAllowedPage\.htm'| p/Dell PowerConnect http config/ d/switch/
match http m|^HTTP/1\.1 \d\d\d .*\r\n\r\n<BODY><CENTER><BR><BR><strong><font size=5 face=verdana>SRW224 24-Port 10/100 \+ 2-Port Gigabit <BR>|s p/Linksys SRW224 gigabit switch http config/ d/switch/
match http m|^HTTP/1\.1 \d\d\d .*\r\nConnection: close\r\nCache-Control: no-cache\r\nServer: SQ-WEBCAM\r\n| p/dvr1614n web-cam httpd/ d/webcam/
match http m|^HTTP/1\.0 \d\d\d .*Server: BeOS/PoorMan\r\n|s p/BeOS poorman httpd/ o/BeOS/
match http m|^HTTP/1\.0 200\r\nContent-type: text/html\r\n\r\n<HTML>\r\n<HEAD><TITLE>WJ-NT104 MAIN PAGE</TITLE></HEAD>\r\n| p/Panasonic WJ-NT104 network camera httpd/ d/webcam/
match http m|^HTTP/1\.0 \d\d\d .*Server: TwistedWeb/([\d.]+)\r\n\r\n.*<title>Punjab |s p/Punjab HTTP -> XMMP proxy/ i/TwistedWeb httpd $1/
match http m|^HTTP/1\.1 \d\d\d .*<title>I\.M\. Everywhere</title>|s p/Trillian IM Everywhere http plugin/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*Server: Grandstream/([\d.]+)\r\n\r\n|s p/Grandstream VoIP phone http config/ v/$1/ d/VoIP phone/
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"RV042\"\r\n| p/Linksys RV042 VPN router http config/ d/router/
match http m|^HTTP/1\.0 200 OK\r\nServer: Router/([\d.]+)\r\n.*<TITLE>Cable/xDSL Wireless Router</TITLE>|s p/SparkLAN WX-2211A wireless router http config/ v/$1/ d/router/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: LiteServe/([\d.]+)\r\n| p/Perception LiteServe httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: httpd-impacct/([\d.]+) ([\d/]+)\r\n| p/Zonet ZSR0104CP router http config/ v/$1/ i/Released $2/ d/router/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: YAZ/([\w._-]+)\r\n|s p/YAZ Z39.50 http interface/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: svea_httpd/([\d.]+) ([^\r\n]+)\r\n| p/svea_httpd/ v/$1/ i/Released $2/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: svea_httpd/([\d.]+)\r\n| p/svea_httpd/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Microsoft-PWS/([\d.]+)\r\n| p/Microsoft Peer Web Services httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Microsoft-PWS-95/([\d.]+)\r\n| p/Microsoft Peer Web Services 95 httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 302 Found\r\nConnection: Close\r\nLocation: /iw-cc/command/iw\.base\.show_done_page| p/Interwoven TeamSite game proxy httpd/
match http m|^HTTP/1\.0 302 Found\r\nLocation: http://xbtt\.sourceforge\.net/\r\n\r\n| p/xbtt bittorrent tracker httpd/
match http m|^HTTP/1\.1 302 Found\r\nLocation: http://([-\w_.]+)/.*<FONT face=\"Helvetica\">\n<big>Redirect \(authentication_redirect_to_virtual_host\)</big>|s p/Blue Coat http config/ h/$1/
match http m|^HTTP/1\.0 200 OK\nServer: EntropyChat ([\d.]+)\n| p/cPanel EntropyChat httpd/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\nServer: Jaguar Server Version ([\d.]+)\r\n.*<TITLE>Sybase EAServer Version ([\d.]+)\n</TITLE>|s p/Sybase EAServer httpd/ v/$2/ i/Jaguar httpd $1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: BRS-WebWeaver/([\d.]+)\r\n| p/BRS WebWeaver httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nDate: .*\r\nServer: eSoft/([\d.]+) \(Unix\)\r\n| p/eSoft emumail webmail httpd/ v/$1/ o/Unix/
match http m|^HTTP/1\.1 400 Bad Request\r\nDate: .*\r\nServer: tigershark/([\d.]+) | p/tigershark httpd/ v/$1/ o/Unix/
match http m|^HTTP/1\.1 200 Document Follows\r\n.*CONTENT=\"TANDBERG ASA \(http://www\.tandberg\.net\)\">\r\n<meta name=\"description\"\r\ncontent=\"TANDBERG is a leading global provider of videoconferencing|s p/Tandberg video conferencing http config/ d/media device/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nContent-type: text/html\r\nServer: Tandberg Television Web server\r\n| p/Tandberg Television httpd/ d/media device/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nWWW-Authenticate: Basic realm=\"([^\"]+)\"\r\n.*\r\n.*\r\nServer :Tandberg Television Web server\r\n| p/Tandberg Television httpd/ d/media device/ i/Realm: $1/
match http m|^HTTP/1\.0 200 OK\nContent-type: text/html\n\n<!-- \n#ident \"%W%\"\n# Copyright \(c\) 2\d+ SteelEye Technology Inc\. - Mountain View, CA, USA\n################### LifeKeeper| p/SteelEye LifeKeeper cluster http config/ o/Unix/
match http m|^HTTP/1\.0 \d\d\d .*Server: Ubicom/([\d.]+)\r\n.*<title>D-Link Gaming Router : Login</title>|s i/D-Link gaming router http config/ p/Ubicom httpd/ v/$1/ d/router/
match http m|^HTTP/1\.1 \d\d\d .*Server: Allegro-Software-RomPager/([\d.]+)\r\n\r\n<HTML>\n<HEAD>\n<TITLE>LANIER 5613 / LANIER Network Printer D model-Network Administration</TITLE>|s p/Lanier 5613 network printer http config/ i/Allegro RomPager httpd $1/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*\nServer: Novell-HTTP-Server/([\w.]+)\n.*<TITLE>GroupWise WebAccess</TITLE>|s p/Novell GroupWise webmail/ i/Novell httpd $1/
match http m|^HTTP/1\.0 \d\d\d .*\nDate: .*\nServer: Novell-HTTP-Server/([\w._-]+)\n| p/Novell httpd $1/
match http m|^HTTP/1\.0 400\r\nContent-Type: text/html\r\n\r\n<html><head><title>Error</title></head><body>\r\n<h2>ERROR: 400</h2>\r\nHost name unspecified\.\n<br>\r\n</body></html>\r\n$| p/Teros application firewall/ d/firewall/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Intoto ?Http ?Server..([\d.]+)\r\n|s p/Intoto httpd/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nConnection: close\r\nServer: httrack-small-server\r\n| p/httrack offline browsing httpd/ o/Windows/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: GeneWeb/([\d.]+)\r\n| p/GeneWeb httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*USEMAP=.SwitchMasthead ALT=\\\"Fast Ethernet Switch 8275-416\\|s p/IBM 8275-416 switch http config/ d/switch/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: jabberd ([\d.]+)\r\n| p/jabberd httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nConnection: close\r\nContent-Length: \d+\r\nContent-Type: text/html; charset=utf-8\r\n\r\n<html>\n\t<head>\n\t\t<title>Enigma Web Interface</title>\n\t| p/Dreambox DVB Enigma httpd/ d/media device/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: VB150\r\n.*<title>WebView Livescope</title>|s p/Canon WebView VB150 http config/ d/webcam/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: iGuard Embedded Web Server/([\w.]+) \(FPS(\d+)\) SN:([-\w]+)\r\n| p/iGuard FPS$2 FingerPrint Scanner http config/ i/iGuard embedded httpd $1; SN $3/ d/security-misc/
match http m|^HTTP/1\.0 \d\d\d .*<title>SP200X Web Configuration Pages</title>|s p/SignalSys SP200X VoIP http config/ d/VoIP adapter/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Beagle-XSP Server/([\d.]+) Unix\r\nX-Powered-By: ([^\r\n]+)\r\n| p/Beagle XSP/ v/$1/ i/$2/ o/Unix/
match http m|^HTTP/1\.0 \d\d\d .*\r\nWWW-Authenticate: Basic realm=\"Instant Internet\"\r\n\r\n| p/Nortel Instant Internet remote access httpd/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: NetworkActiv-Web-Server/([\d.]+)\r\n|s p/NetworkActiv httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: ATEN HTTP Server\(V([\d.]+)\)\r\n| p/Aten KVM http config/ i/Aten httpd $1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nWWW-authenticate: basic realm=\"Vina Technologies eLink 200\"\r\n| p/Vina Technologies eLink 200 http config/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nWWW-authenticate: basic realm=\"Vina Technologies T1 Integrator\"\r\n| p/Vina Technologies T1 Integrator http config/ d/telecom-misc/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nDate: .*\r\nServer: CPWS\r\n| p/Connectra Check Point Web Security httpd/ d/security-misc/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Agranat-EmWeb/R([-\w_.]+)\r\nWWW-Authenticate: Basic realm=\"Efficient Networks Web User Interface\"\r\n\r\n| i/Efficient Networks router http config/ p/Agranat-EmWeb/ v/$SUBST(1,"_",".")/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Niagara Web Server/([\d.]+)\r\nNiagara-Release: ([-\w_.]+)\r\n|s p/Sun Niagara httpd/ v/$1/ i/Niagara release $2/
#The following two lines are for the Tridium Niagara embedded device httpd, NOT the Sun (now Oracle) Solaris httpd - Tom
match http m|^HTTP/1\.[01] \d\d\d .*\r\nNiagara-Platform: ([^\r\n]+).*Server: Niagara Web Server/([\d.]+)\r\n|is p/Tridium Niagara httpd/ v/$2/ i/Platform: $1/ o/$1/ d/specialized/ 
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Niagara Web Server/([\d.]+)\r\n|is p/Tridium Niagara httpd/ v/$1/  d/specialized/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: The Knopflerfish HTTP Server\r\n|s p/Knopflerfish httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: HTTP\r\n.*<title>Inventel</title>|s p/Inventel router http config/ d/router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: Nanox WebServer\r\n| p/Nanox Web Digital Video Recorder http config/ d/media device/
match http m|^HTTP/1\.0 200 OK\r\nServer: NetPort Software ([\d.]+)\r\nDate:.* - VSX 7000</title>|s p/Polycom VSX 7000 video conferencer http config/ i/NetPort httpd $1/ d/webcam/
match http m|^HTTP/1\.0 200 OK\r\nServer: Firewall\r\n.*<TITLE>WatchGuard Configuration Settings</TITLE>|s p/WatchGuard Firebox Soho Firewall http config/ d/firewall/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nWWW-Authenticate: Digest  realm=\"spa user\", domain=\"/\".*<title>Sipura SPA Configuration</title>|s p/Sipura SPA VoIP http config/ d/VoIP adapter/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: ipMonitor ([\d.]+)\r\n| p/MediaHouse ipMonitor httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.[01] \d\d\d .*\nServer: Tarantella/([\d.]+)\n| p/Tarantella httpd/ v/$1/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: RealServer ([\d.]+)\r\n.*<H2>Access to RealServer 5\.0 Administration Denied</H2></HTML>\n|s p/RealServer httpd/ v/$1/ i/Access denied/
match http m|^HTTP/1\.0 \d\d\d .*<TITLE>AXIS ([\d]+) Camera Server</TITLE>|s p/AXIS $1 camera httpd/ d/webcam/
match http m|^HTTP/1\.0 \d\d\d .*<TITLE>The AXIS 200\+ Home Page</TITLE>|s p/AXIS 200+ camera httpd/ d/webcam/
match http m|^HTTP/1\.0 200 OK\r\n.*<TITLE>AXIS 2400 Video Server</TITLE>|s p/AXIS 2400 video httpd/ d/webcam/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Web Crossing/([\d.]+)\r\n|s p/Web Crossing collaboration httpd/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Kannel/([\d.]+)\r\n| p/Kannel SMS proxy httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Allegro-Software-RomPager/(\d[-.\w]+)\r\n\r\n.*<title>ExtremeWare Management Interface</title>|s p/Extreme Networks switch http config/ i/Allegro embedded httpd $1/ d/switch/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Allegro-Software-RomPager/(\d[-.\w]+)\r\n\r\n<HTML>\n<HEAD>\n<TITLE>AudioCodes\n</TITLE>|s p/AudioCodes VoIP gateway http config/ i/Allegro embedded httpd $1/ d/VoIP adapter/
match http m|^HTTP/1\.1 \d\d\d .*\r\nWWW-Authenticate: Basic realm=\"Switched Rack PDU\"\r\nContent-Type: text/html\r\nServer: Allegro-Software-RomPager/([\d.]+)\r\n\r\n| p/APC switched rack PDU http config/ i/Allegro embedded httpd $1/ d/power-device/
match http m|^HTTP/1\.1 \d\d\d .*\r\nWWW-Authenticate: Basic realm=\"IES-1000 \w+-\d+\"\r\nContent-Type: text/html\r\nServer: ZyXEL-RomPager/([\d.]+)\r\n\r\n| p/ZyXEL IES-1000 DSLAM http config/ i/ZyXEL httpd $1/ d/telecom-misc/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: DIONIS/([\d.]+)\r\n| p/DIONIS httpd/ v/$1/
match http m|^HTTP/1\.0 400 Bad-Request\nHTTP/1\.0 200 OK\r\n.*Aironet BR500E V([\d.]+)</td>|s p/Aironet BR500E wireless bridge http config/ v/$1/ d/WAP/
match http m|^HTTP/1\.0 \d\d\d .*\r\nWWW-Authenticate: Basic realm=\"4AFXS Configuration Web Server\"\r\n| p/SunComm 4AFXS VoIP gateway http config/ d/VoIP adapter/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: ATR-HTTP-Server/([\d.]+)\r\n.*WWW-Authenticate: Basic realm=\"Allied Telesyn AR410\"\r\n|s p/Allied Telesyn AR410 http config/ i/ATR httpd $1/ d/router/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Oracle_Web_Listener/([\d.]+)EnterpriseEdition\r\n|s p/Oracle Web Listener Enterprise Edition/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Oracle_Web_Listener/([\d.]+)AdvancedEdition\r\n|s p/Oracle Web Listener Advanced Edition/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Oracle_Web_listener_?([^\r\n]+)\r\n|s p/Oracle Web Listener/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: VOMwebserver v([\d.]+)\r\n|s p/VOMwebserver/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: RapidLogic/([\d.]+)\r\n.*<TITLE>Net2Phone Init Page</TITLE>|s p/Net2Phone VoIP adapter http config/ i/RapidLogic embedded httpd $1/ d/VoIP adapter/

match http m|^HTTP/1\.0 \d\d\d .*<title>IT Temperature Monitor: ([^<]+)</title>.*<TD>Model:</TD><TD width=10 rowspan=3><BR></TD><TD>([-\w_.]+)</TD><TD width=20 rowspan=3><BR></TD><TD>Firmware Version:</TD><TD width=10 rowspan=3><BR></TD><TD>([\d.]+)</TD>|s p/Sensatronics $2 remote temperature monitor httpd/ d/specialized/ i/name $1; Firmware version $3/
match http m|^HTTP/1\.0 \d\d\d .*<title>IT Temperature monitor: ([^<]+)</title>.*<TD>Model:</TD><TD width=10 rowspan=7><BR></TD><TD>([-\w_.]+)</TD>.*<TD>Firmware Version:</TD><TD>([\d.]+)</TD>|s p/Sensatronics $2 remote temperature monitor httpd/ d/specialized/ i/name $1; Firmware version $3/

match http m|^HTTP/1\.1 \d\d\d .*<font color=#FFFFFF size=5>Cisco ATA 186 \(SIP\)</font>|s p/Cisco ATA 186 SIP http config/ d/VoIP adapter/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: AKCP Embedded Web Server| p/AKCP embedded httpd/
match http m|^HTTP/1\.1 \d\d\d .*Server: Allegro-Software-RomPager/([\d.]+)\r\n.*<meta content=\"Printer with Embedded Web Server\"|s p/Xerox Phaser 4500 printer http config/ i/Allegro httpd $1/ d/printer/
match http m|^HTTP/1\.0 200 OK\r\n\r\n<HTML>\r\n<HEAD>\r\n<TITLE>JetDirect Home Page</TITLE>\r\n\r\n</HEAD>\r\n<BODY>\r\n<P>\r\nWelcome to the HP JetDirect print server!\r\n| p/HP JetDirect printer http config/ d/printer/
match http m|^HTTP/1\.0 200 OK\r\nServer: JVC/([\d.]+)\r\n.*<html>\r\n<head>\r\n.*<title>V\.Networks|s p/JVC V.Networks video httpd/ v/$1/ d/media device/
match http m|^HTTP/1\.0 401\r\nServer: JVC/([\d.]+)\r\n.*\r\n\r\n<html><body><h1>401 Unauthorized</h1></body></html>\r\n|s p/JVC V.Networks video httpd/ v/$1/ i/Authentication enabled/ d/media device/
match http m|^HTTP/1\.1 \d\d\d .*\r\nWWW-Authenticate: Digest  realm=\"pap user\".*<title>Linksys PAP2 Configuration</title>|s p/Linksys PAP2 VoIP http config/ d/VoIP adapter/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: SWS-([\d.]+)\r\n|s p/Sun WebServer/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*<title>Dominion SX32</title>|s p/Raritan Dominion SX32 http config/ d/terminal server/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Sensorsoft-Remote-Watchman-Enterprise/([\d.]+)\r\n| p/Sensorsoft Remote Watchman Enterprise/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 302 Found\r\nLocation: /cgi-bin/guestimage\.html\r\nContent-type: text/html; charset=ISO-8859-1\r\nCache-Control: no-cache\r\n\r\n.*<title>\r\nRedirect to guestimage: /cgi-bin/guestimage\.html\r\n|s p/Mobotix M10 PRISMB web cam http config/ i/embedded thttpd/ d/webcam/
match http m|^HTTP/1\.1 302 Moved Temporarily\r\nContent-Length: 0\r\nLocation: /\?[a-z\d]{7,8}\r\n| p/Urchin RSS aggregator/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Meridian Data/([\d.]+)\r\n| p/Meridian Quantum Snap! http config/ v/$1/ d/storage-misc/
match http m|^HTTP/1\.0 401 Unauthorized\r\nContent-type: text/html\r\nWWW-Authenticate: Basic realm=\"Login\"\r\n<HTML><HEAD><TITLE>401 Unauthorized</TITLE></HEAD>\n<BODY><H1>401 Unauthorized Access Attempt</H1>\nYou are not authorized to access the requested file\.</BODY></HTML>$| p/Cisco VG248 http config/ d/telecom-misc/
match http m|^HTTP/1\.0 200 Ok\r\n.*<H1>(ZBR\d+) - ZebraNet PrintServer</H1>|s p/ZebraNet $1 print server http config/ d/print server/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: GoAhead-Webs\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"Wireless Access Point\"\r\n.*\r\n<html><head><title>Document Error: Unauthorized</title></head>\r\n\t\t<body><h2>Access Error: Unauthorized</h2>\r\n\t\twhen trying to obtain <b>/</b><br><p>Access to this document requires a User ID</p></body></html>\r\n\r\n|s i/Ovislink WAP http config/ p/GoAhead-Webs httpd/ d/WAP/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: \r\n.*WWW-Authenticate: Basic realm=\"(WN-\w+)\"\r\n.*<title> Authorization warning</title>|s p/Ovislink $1 WAP http config/ d/WAP/
match http m|^HTTP/1\.0 200 OK\r\nDate: .*\r\nContent-Length: \d+\r\nContent-Type: text/html\r\nServer: HyNetOS/([\d.]+)\r\n\r\n<HTML>\r\n<HEAD>\r\n<TITLE>EverFocus EDSR Applet \(([\d.]+)\)</TITLE>| p/EverFocus webcam http config/ i/EDSR Applet $2; HyNetOS $1/ o/HyNetOS/ d/webcam/
match http m|^HTTP/1\.1 200 OK\r\nContent-Length: \d+\r\n\r\n<html>\n<head>\n<title>MoBif TA-200 Configuration</title>\n| p/MoBif TA-200 http config/ d/VoIP adapter/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\n.*Server: Allegro-Software-RomPager/([\w.]+)\r\n\r\n.*<title>PagePro 9100 / PagePro 9100</title>\n.*<a href=\"http://www\.minolta-qms\.com\">|s p/Minolta 9100 printer http config/ i/Allegro httpd $1/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-type: text/html\r\n\r\n<HTML><HEAD><TITLE>OkiLAN (\w+)</TITLE>| p/OkiData printer http config/ i/OkiLAN $1/ d/printer/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: IPCheck/([\d.]+) *\r\n\r\n|s p/IPCheck httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: Aragorn\r\nWWW-Authenticate: Basic realm=\"Please enter User name and password\"\r\n| p/Aastra 480i VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: Aragorn\r\nWWW-Authenticate: Basic realm=\"Aastra ([\w-]+)\"\r\n| p/Aastra $1 VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.1 200 Ok\r\nServer: snom embedded\r\nContent-Type: text/html\r\nCache-Control: no-cache\r\nCache-Control: no-store\r\n.*\n<TITLE>snom ([-\w_.]+)</TITLE>\n|s p/Snom $1 VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.1 403 Forbidden\r\nContent-Type: text/html\r\nCache-Control: no-cache\r\nCache-Control: no-store\r\nServer: snom embedded\r\n.*<TITLE>snom VoIP phone: Error</TITLE>|s p/Snom 300 VoIP phone http config/ d/VoIP phone/ i/secure connection required/
match http m|^HTTP/1\.1 200 Ok\r\nServer: snom embedded\r\n.*\n<html>\n<head>\n\n<title>snom 105 VoIP Phone :: Home</title>|s p/Snom 105 VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.1 401 Unauthorized\r\nDate: .*\r\nServer: Agranat-EmWeb/R([\d_]+)\r\nWWW-Authenticate: Basic realm=\"main@SP1\"\r\nContent-type: text/html\r\n {34}\r\n| i/CyberIQ HyperFlow 3 switch http config/ p/Agranat-EmWeb/ v/$SUBST(1,"_",".")/ d/switch/
match http m|^HTTP/1\.0 200 OK\r\nAllow:GET\r\nContent-Type:text/html\r\nExpires: .*\r\nContent-Length:\d+\r\n\r\n<HTML><HEAD><TITLE>Ringdale Printserver </TITLE>| p/Ringdale print server http config/ d/print server/
match http m|^HTTP/1\.0 302 Found\nLocation: /login\.ews\r\nCache-Control: no-store\nContent-Type: text/html\r\n\r\n| p/Emerald Management Suite httpd/
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"FXO Configuration Web Server\"\r\nContent-type: text/html\r\n\r\n<html>\r\n<body><h1>401 Unauthorized</h1></body></html>\r\n| p/Tandem NSK D40 http config/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: glass/([\d.]+) Python/([-\w.]+)\r\n| p/IronPort AsyncOS http config/ i/glass $1; Python $2/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html; charset=iso-8859-1\r\nPragma: No-cache\r\nServer: ACOS HTTPD/([\d.]+)\r\nCache-Control: no-cache\r\n.*\r\n\r\n<html>\r\n<head>\r\n<title>neuf telecom</title>\r\n|s p/Neuf Box router http config/ i/ACOS httpd $1/ d/router/
match http m|^HTTP/1\.0 200 OK\r\nServer: U S Software Web Server\r\n.*\n<html>\n<head>\n<title>StorageLoader</title>\n|s p/Tandberg Data StorageLoader http config/ d/storage-misc/
match http m|^HTTP/1\.0 200 OK\r\nDate: .*\r\nServer: VykTor XML WinAmp Server/([\d.]+)\r\nMIME-version: [\d.]+\r\n.*<title>Snow Crash</title>\r\n|s p/Snowcrash WinAmp http control plugin/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 200 OK\nContent-type: text/html\r\nDate: .*\n<TITLE>\nGigaset M740 AV - Experimentelles Web-Interface\n</TITLE>\n|s p/Siemens Gigaset M740 http config/ d/media device/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Spinnaker/([\d.]+)\r\n| p/Searchlight Software Spinnaker httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 401 Authorization Required\nWWW-Authenticate: Basic realm=\"HERCULES\"\n| p/Hercules mainframe emulator http config/
match http m|^HTTP/1\.1 302 Found\r\nDate: .*\r\nLocation: https://pgpuniversal_| p/PGP Universal httpd/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Oracle/([\d.]+)\r\nWWW-Authenticate: Basic realm=\"XDB\"\r\n|s p/Oracle XDB httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Oracle XML DB/Oracle Database\r\nWWW-Authenticate: Basic realm=\"XDB\"\r\n|s p/Oracle XDB httpd/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Oracle XML DB/Oracle9i Release ([^\r\n]+)\r\n|s p/Oracle XDB httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\n<meta name=\"GENERATOR\" content=\"Active WebCam ([\d.]+) \(http://www\.pysoft\.com\) \[Unregistered\]\">\r\n\r\n|s p/Active WebCam httpd/ v/$1/ i/Unregistered/ d/webcam/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: GoAhead-Webs\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"Venturi NMS\"\r\n| p/Venturi wireless accelerator http config/ i/GoAhead embedded httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\nserver: SAP Web Application Server \(([-\w_.;]+)\)\r\n|s p/SAP Web Application Server/ v/$1/
match http m|^HTTP/1\.0 401 Unauthorized\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"SIP Phone\"\r\nContent-Type: text/html\r\n\r\n<html>\r\n<head>\r\n<title>401 Unauthorized Ip Phone Access</title>\r\n| p/Tecom Co. SIP-Phone http config/ d/VoIP phone/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: SentinelProtectionServer/([\d.]+)\r\n| p/SafeNet Sentinel License Monitor httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: SentinelKeysServer/([\d.]+)\r\n.*<title>Sentinel Keys License Monitor</title>|s p/SafeNet Sentinel Keys License Monitor httpd/ v/$1/ i/Java Console/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Techno Vision Security System Ver\. ([\d.]+)\r\n| p/Techno Vision Security System http config/ v/$1/ d/webcam/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: webcamXP\r\n\r\n<html><head><title>.*</title><meta name=\"generator\" content=\"webcamXP PRO v([\d.]+)\">|s p/webcamXP PRO http config/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: webcamXP\r\n|s p/webcamXP httpd/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: webcamXP (\d+)\r\n|s p/webcamXP httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<!---CAS:0003--><HTML><HEAD><TITLE>Broadband NAT Router Web-Console</TITLE>| p/Digtus DN-11001 broadband router http config/ d/broadband router/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<!---CAS:0003--><HTML><HEAD>\n<TITLE>Wireless Broadband NAT Router Web-Console| p/Safecom SWBR 54000 WAP http config/ d/WAP/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<!---CAS:0003--><HTML><HEAD>\n<TITLE>(FBR-\w+)  Broadband NAT Router Web-Console</TITLE>| p/LevelOne FBR-$1 router http config/ d/router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Rapidsite/Apa/([\d.]+) \(Unix\) (.*)\r\n| p|Rapidsite/Apa httpd| v/$1/ i/$2/ o/Unix/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Rapidsite/Apa\r\n| p|Rapidsite/Apa httpd|
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Digest realm=\"Sip Utility Set\", nonce=| p/Avaya 4602 VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Sun-ILOM-Web-Server/([\d.]+)\r\n| p/Sun Integrated Lights-Out httpd/ v/$1/ d/remote management/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Apple Embedded Web Server/([\d.]+)\r\n| p/Apple Embedded httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: iPrism-httpd/v3 \(Unix\) ssl_enabled ossl\r\n| p/St. Bernard iPrism firewall http config/ i/ssl enabled/ o/Unix/ d/firewall/
match http m|^HTTP/1\.0 403 Forbidden\r\nServer: iPrism/v3\r\n| p/St. Bernard iPrism firewall http config/ d/firewall/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: XOS (\w+)\r\n| p/Extremeware XOS httpd/ v/$1/
match http m|^HTTP/1\.0 200 Okay\r\nConnection: close\r\nServer: BaseSwitch 801FM\r\nContent-Type: text/html\r\n\r\n<HTML>\n<HEAD><TITLE>Welcome to Transtec AG WEBServer</TITLE>| p/Transtec BaseSwitch 801FM http config/ d/switch/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Agranat-EmWeb/R([\d_]+)\r\nContent-Length: 0\r\nWWW-Authenticate: Basic realm=\"Authenticated_User@P330\"\r\n\r\n| p/Agranat-EmWeb/ v/$SUBST(1,"_",".")/ i/Avaya P330 switch http config/ d/switch/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: Systinet Server for Java/([\d.]+) \(([^)]+)\)\r\n| p/Systinet Server for Java/ v/$1/ i/$2/
match http m|^HTTP/1\.1 200 OK\r\nServer: Miralix License Server\r\n| p/Miralix license server httpd/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: EWS-NIC3/([\d.]+)\r\nConnection: close\r\nContent-Type: text/html\r\n\r\n<html>\n<head>\n<title>Dell Laser Printer ([\w+]+)</title>\n| i/Dell $2 laser printer http config/ p/EWS-NIC3/ v/$1/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: EWS-NIC4/([\d.]+)\r\nConnection: close\r\nContent-Type: text/html\r\n\r\n<html>\r\n<head>\r\n<title>\r\nDell Color Laser ([\w+]+)</title>\r\n| i/Dell $2 laser printer http config/ p/EWS-NIC4/ v/$1/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: EWS-NIC4/([\d.]+)\r\nConnection: close\r\nContent-Type: text/html\r\n\r\n<html>\r\n<head>\r\n<title>\r\nDell MFP Laser (\w+)</title>| i/Dell $2 MFP laser printer http config/ p/EWS-NIC4/ v/$1/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: EWS-NIC4/([\d.]+)\r\n.*<title>Phaser (\w+) - Phaser [\w-]+</title>|s p/EWS-NIC4/ v/$1/ i/Xerox Phaser $2 printer http config/ d/printer/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: EWS-NIC5/([\d.]+)\r\n.*<title>\r\nDell (\w+) Color Laser</title>|s p/EWS-NIC5/ v/$1/ i/Dell $1 printer http config/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: tracd/([-\w_.]+) Python/([-\w_.]+)\r\n| p/Tracd/ v/$1/ i/Python $2/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Sametime Server \(Meeting Services\) ([\d.]+)\r\n\r\n| p/IBM Lotus Sametime httpd/ v/$1/
# Not sure if this is used anywhere other than the debian
# apt caching server "approx"...
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: OCaml HTTP Daemon\r\n| p/OCaml httpd/
match http m|^HTTP/1\.0 200 OK\nContent-Type: text/plain\nContent-Length: \d+\n\nerror\nno table param specified\n| p/Ingenuity Works ATRT minidb/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Anapod Manager ([\w.]+)\r\n| p/Anapod iPod Explorer httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: IISGuard\r\n| p/Troxo IISGuard/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*<title>Smart VoIP IAD Web Configuration Pages</title>|s p/Patton SmartLink 4020 VoIP adapter http config/ d/VoIP adapter/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: DesktopAuthority/([\d.]+)\r\n|s p/ScriptLogic DesktopAuthority httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 302 Please login\.\nDate: .*\nServer: (P560\.GSI\.[\d.]+)\n| p/Gemtek P560 WAP http config/ v/$1/ d/WAP/
match http m|^HTTP/1\.0 302 Please login\.\nDate: .*\nServer: RG4000\.CMC\.([.\d]+)\n| p/RG4000 Access Control Gateway/ v/$1/ d/security-misc/
match http m|^HTTP/1\.0 200 OK\r\n\r\n<HTML>\r\r\n<BODY>\r\r\n\r\r\n<APPLET CODE=\"SimpleCamApplet2\.class\" CODEBASE=\"http://([-\w_.]+)/.*\" WIDTH=\"(\d+)\" HEIGHT=\"(\d+)\">| p/SimpleCam httpd/ i/Webcam resolution: $2x$3/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: LogMeIn/([\d.]+)\r\n|s p/LogMeIn httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: MacroMaker\r\n| p/MacroMaker httpd/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: NI Service Locator/([\d.]+) \(SLServer\)\r\n| p/National Instruments LabVIEW service locator httpd/ v/$1/
match http m|^HTTP/1\.1 406 Not Acceptable\r\nServer: Phex ([\d.]+)\r\n\r\n| p/Phex HTML-Shared File Export httpd/ v/$1/
match http m|^HTTP/1\.1 403 Browsing disabled\r\nServer: Phex ([\d.]+)\r\n\r\n$| p/Phex HTML-Shared File Export httpd/ v/$1/
match http m|^HTTP/1\.0 200 NoPhrase\r\n.*\r\n<HTML>\r\n<HEAD>\r\n<TITLE>\[JMX RI/([\d.]+)\] Agent View</TITLE>|s p/Sun Java Management Extensions Reference Installation httpd/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*\r\nLast-Modified: .*\r\nETag: \"[\w_]+\"\r\nAccept-Ranges: bytes\r\nContent-Length: 79\r\nConnection: close\r\nContent-Type: text/html\r\n\r\n<html>\n<script language=javascript>\n\ntop\.location=\"/login\";\n\n</script>\n</html>\n| p|Fortinet VPN/firewall http config| d/firewall/
match http m|^HTTP/1\.0 200 Ok\r\nServer: httpd\r\nDate: .*\r\nCache-Control: no-cache\r\nPragma: no-cache\r\nExpires: 0\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<script>\ntop\.location\.href=\"/login_en\.htm\";\n</script>\n\n| p/Siemens Gigaset SE505 WAP http config/ d/WAP/
match http m|^HTTP/1\.0 \d\d\d .*\r\nConnection: close\r\nServer: Gigaset ([^\r\n]+)\r\n| p/Siemens Gigaset $1 WAP http config/ d/WAP/
match http m|^HTTP/1\.1 \d\d\d .*\r\nConnection: Keep-Alive\r\nServer: Siemens Gigaset C450 IP\r\n| p/Siemens Gigaset C450 IP VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.1 \d\d\d .*\r\nConnection: Keep-Alive\r\nServer: Siemens Gigaset ([^\r\n]+)\r\n| p/Siemens Gigaset $1 WAP http config/ d/WAP/
match http m|^HTTP/1\.0 \d\d\d .*\r\nWWW-Authenticate: Basic realm=\"dbox\"\r\n\r\nAccess denied\.\r\n| p/Dbox2 Neutrino httpd/ d/media device/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: nhttpd/([\w._-]+) \(yhttpd_core/([\w._-]+)\)\r\n.*<title>dbox yWeb</title>|s p/dbox yWeb httpd/ d/media device/ i/nhttpd $1 based on yhttpd_core $2/
match http m|^HTTP/1\.0 \d\d\d .*<meta http-equiv=\"powerstate\" content=\"Switch Port7,0\">\n<meta http-equiv=\"powerstate\" content=\"Switch Port8,0\">\n<TITLE>ExpPowerControl</TITLE>|s p/Expert Power Control NET http config/ d/power-device/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: aidex/([\d.]+) \(Win32\)\r\n| p/aidex httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: httpd\r\n.*<!-- \r\n\(c\) 2003 Motorola, Inc\. All Rights Reserved\. \r\n-->\r\n\r\n<title>Motorola HomeNet Product WE800G</title>\r\n|s p/Motorola HomeNet WE800G http config/ d/bridge/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: httpd\r\n.*<!-- \r\n\(c\) 2003 Motorola, Inc\. All Rights Reserved\. \r\n-->\r\n\r\n<title>Motorola HomeNet Product WR850G</title>\r\n|s p/Motorola HomeNet WR850G http config/ d/broadband router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nMIME-Version: 1\.0\r\nServer: KS_HTTP/([\d.]+)\r\nLast-Modified: .*<meta http-equiv=\"Content-Type\" content=\"text/html; charset=Shift_JIS\">\r\n    <meta http-equiv=author content=\"Canon Inc\.\">\r\n|s p/Canon Pixma IP4000R printer http config/ i/KS_HTTP $1/ d/printer/
match http m|^HTTP/1\.0 200 Ok Welcome to VOC\r\nServer: Voodoo chat daemon ver perl ([^\r\n]+)\r\n| p/Voodoo chat daemon httpd/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nServer: AP HTTP Server\r\nSet-Cookie: LogIn=0\r\n.*<frame name=\"top\" src=\"/cgibin/entry\" marginwidth=\"10\" marginheight=\"10\" scrolling=\"auto\" frameborder=\"0\">\n    <frame name=\"center\" src=\"/user/images/selected/logslct\.gif|s p/Nortel Integrated Conference bridge http config/ i/AP HTTPd/ d/bridge/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Polycom SoundPoint IP Telephone HTTPd\r\n| p/Polycom SoundPoint VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: BISW_SDR\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"WebAdmin\"\r\nPragma: no-cache\r\n| p|Billion/TeleWell ADSL modem http config| d/broadband router/
match http m|^HTTP/1\.0 200 OK\r\nContent-Length: \d+\r\nContent-Type: text/html\r\n.*getElementById\(\"cTextChg\"\)\.innerHTML = \"<p>Die soeben durchgef&uuml;hrte System&uuml;berpr&uuml;fung hat ergeben,<br>\" \+\n \"dass ihr Bildschirm nicht die minimal erforderliche Aufl\xf6sung hat\.</p>|s p/T-Com Speedport W 501V WAP http config/ i/German/ d/WAP/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: David-WebBox/([\w.]+) \((\d+)\)\r\n| p/David WebBox httpd/ v/$1.$2/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: RapidLogic/([\d.]+)\r\nMIME-version: 1\.0\r\nContent-type: text/html\r\n\r\n<HTML>\r\n<HEAD>\r\n<TITLE>WireSpeed Dual Connect</TITLE>\r\n\r\n<META http-equiv=\"PRAGMA\" content=\"NO-CACHE\"></META>\r\n\r\n| p/Westell C90 ADSL router http config/ v/RapidLogic httpd $1/ d/broadband router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nMIME-Version: 1\.0\r\nDate: .*\r\nServer: PeopleSoft RENSRV/v([\d.]+)\r\n| p/Peoplesoft REN Server httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Virata-EmWeb/R([\d_]+)\r\nContent-Length: \d+\r\nContent-Type: text/html\r\nExpires: .*\r\nPragma: no-cache\r\n\r\n<HTML><HEAD><TITLE>Actiontec</TITLE>\n|s i/Actiontec R1524SU http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/broadband router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: HFS ([^\r\n]+)\r\n|s p/HttpFileServer httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: Embedded HTTP Server V([\d.]+)\r\nWWW-Authenticate: Basic realm=\"802\.11g Wireless Broadband Router\"\r\nConnection: close\r\n\r\n<HTML><HEAD><TITLE>401 Unauthorized</TITLE></HEAD>\n<BODY BGCOLOR=\"#ffffff\"><H4>401 Unauthorized</H4></BODY></HTML>\n| p/Topcom Skyr@cer WAP http config/ i/Embedded HTTPd $1/ d/WAP/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Ultraseek/([\d.]+)\r\n| p/Ultraseek httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nCache-control: no-cache\r\nContent-length: \d+\r\nContent-type: text/html\r\n\r\n<HTML>\r\n<HEAD>\r\n<TITLE>LANB Remote Upgrade Authentication</TITLE>\r\n.*<FONT face=\"Arial Black\" color=black size=5>VoIP Card Remote Upgrade</FONT>|s p/LG Electronics VoIP board http config/ d/VoIP adapter/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: CherryPy/([\w._-]+)\r\n.*Hi, this is ehcp-python background proses, under development now\.\.\.|s p/CherryPy httpd/ v/$1/ i/Easy Hosting Control Panel/
match http m|^HTTP/1\.0 200 OK\r\nServer: IVC Enterprise Video Server\r\n| p/IVC Enterprise Video Server http config/ d/webcam/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"Network Camera\"\r\nContent-Type: text/html\r\nServer: Network Camera\r\n\r\n<HTML>\n<HEAD>\n<TITLE>Protected Object</TITLE></HEAD><BODY>\n<H1>Protected Object</H1>This object is protected\.<P>\n</BODY></HTML>| p/Vivotek 3102 Camera http config/ d/webcam/
match http m|^HTTP/1\.0 \d\d\d .*<ADDRESS>Cheyenne/([\d.]+) Server at ([-\w_.]+) Port \d+</ADDRESS>\n|s p/Cheyenne httpd/ v/$1/ h/$2/
match http m|^HTTP/1\.1 \d\d\d\r\n.*\r\n\r\n<HTML>\r\n<HEAD>\r\n<title>Lantronix WEB-Manager</title>\r\n|s p/Lantronix Universal Device Server http config/
match http m|^<HTML><HEAD><META HTTP-EQUIV=refresh CONTENT=30; \n\t\turl=status\.html><TITLE>Stratasys Modeler Queue &amp; Job Status</TITLE>| p/Stratasys Modeler Queue printer http config/ d/printer/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: GoAhead-Webs\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"ATAboy2-| p/InfiniSAN ATAboy2 http config/ i/GoAhead embedded httpd/ d/storage-misc/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Micro-Web\r\nContent-type: text/html\r\n\r\n<html>\r\n<head>\r\n<P><TABLE BORDER=0 CELLPADDING=0 CELLSPACING=0 WIDTH=\"100%\">\n<TR><TD WIDTH=\"100%\" ALIGN=CENTER>\n<APPLET CODE=\"Login\.class\" WIDTH=545 HEIGHT=418\nALT=\"\[ Login applet is not available \]\">\n| p/Overland Storage Neo2000 http config/ i/Micro-Web httpd/ d/storage-misc/
match http m|^HTTP/1\.1 200\r\nContent-type: text/html\r\nConnection: close\r\nCONTENT-LENGTH: \d+\r\n\r\n<html>\r\n <head>\r\n  <title>1761-NET-ENI</title>\r\n| p/Allen Bradley 1761-NET-ENI http config/
match http m|^HTTP/1\.0 200 OK    \r\nServer: A-B WWW/([\d.]+)\r\n.*<img src=\"/images/rockcolor\.gif|s p/Rockwell Automation Ethernet Processor http config/ i/A-B WWW httpd $1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: NetPort Software ([\d.]+)\r\nDate: .*\r\nContent-type: text/html\r\n\r\n<html>\r\n<head>\r\n<meta http-equiv=\"content-type\" content=\"text/html;charset=Shift_JIS\">\r\n<title>NEC Projector LAN Control</title>\r\n| p/NEC Projector http config/ d/media device/
match http m|^HTTP/1\.0 200 ;OK\r\nServer: UPS_Server/([\d.]+)\r\nContent-Type: text/html\r\nConnection: Close\r\n\r\n<html>\n<head>\n<title>UPS Properties</title>\n| p/MGE UPS httpd/ v/$1/ d/power-device/
match http m|^HTTP/1\.1 \d\d\d .*\nContent-Length: \d+\nPragma: no-cache\nExpires: 0\nConnection: close\n\n<HTML><HEAD><TITLE>Bridgit Conferencing Server</TITLE>| p/Bridgit Conferencing httpd/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Web Server\r\n.*\n<title>Cisco Systems, Inc\. VPN 3000 Concentrator \[vpn-conc-3030\]</title>\n|s p/Cisco VPN 3000 Concentrator http config/ d/security-misc/
match http m|^HTTP/1\.1 302 Moved Temporarily\r\nDate: .*\r\nLocation: /webct/entryPageIns\.dowebct\r\n| p/WebCT httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Henry/([\d.]+)\r\nno-cache: set-cookie\r\nSet-Cookie: Customer=\"-[\d_]+\";| p/NEC Aspire WebPro http config/ i/Henry httpd $1/ d/telecom-misc/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: GoAhead-Webs\r\nDate: .*\r\nPragma: no-cache\r\nCache-Control: no-cache\r\nContent-Type: text/html\r\nP3P: CP=\"NON DSP CURa OUR NOR UNI\"\r\nLocation: http://[\d.]+/auth\.asp\r\n\r\n<html><head></head><body>\r\nMoved to this <a href=\"http://[\d.]+/auth\.asp\">location</a>\.\r\n<!-- response_code_begin ERIC_RESPONSE_OK| p|Peppercon/Paradox alarm system http config| i/GoAhead embedded httpd/ d/remote management/
match http m|^HTTP/1\.0 404 Not Found\r\nServer: TABS http server/([\d.]+)\r\nDate: .*\r\nContent-Type: text/html\r\nContent-Length: \d+\r\n\r\n<HTML>\r\n<HEAD>\r\n<TITLE> 404 File Not Found</TITLE>\r\n</HEAD>\r\n\r\n<BODY>\r\n<h2>File Not Found</h2>\r\n</BODY>\r\n</HTML>| p/Server Observer Network Monitor httpd/ i/TABS httpd $1/ o/Windows/
match http m|^HTTP/1\.1 401\r\nConnection: close\r\nContent-Type: text/plain\r\nWWW-Authenticate: Basic Realm=\"Vibe Streamer\"\r\n\r\n\r\nAccess denied| p/Vibe Streamer httpd/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*<!-- Copyright \(c\) 2000-2002, Fuji Xerox Co\., Ltd\. All Rights Reserved\. -->\r\n<HTML>\r\n<HEAD>\r\n<META HTTP-EQUIV=\"Content-Type\" CONTENT=\"text/html; charset=ISO-8859-1\">\r\n<TITLE>\r\nWorkCentre (\w+) -|s p/Xerox WorkCentre $1 http config/ d/printer/
match http m|^HTTP/1\.1 \d\d\d .*<!-- Copyright \(c\) 2000-2004, Fuji Xerox Co\., Ltd\. All Rights Reserved\. -->\r\n<HTML>\r\n<HEAD>\r\n<META http-equiv=\"Content-Type\" content=\"text/html; charset=windows-1252\">\r\n<TITLE>\r\nXerox WorkCentre (\w+) -|s p/Xerox WorkCentre $1 http config/ d/printer/
match http m|^HTTP/1\.1 \d\d\d .*<!--\s+/\*-+\*\\\s+Copyright \(c\) 2002-2006 Xerox Corporation\. All Rights Reserved\..*<title>\s*XEROX WORKCENTRE|s p/Xerox WorkCentre http config/ d/printer/
match http m|^HTTP/1\.1 404 Not Found\r\nConnection: close\r\nContent-Type: text/html\r\nContent-Length: \d+\r\n\r\n<body><h2>HTTP/1\.1 404 Not Found</h2></body>| p/VypressChat httpd/ o/Windows/
match http m|^HTTP/1\.0 200 Ok\r\nDate: .*\r\nMIME-Version: 1\.0\r\nServer: Rogatkin's JWS based on Acme\.Serve/.Revision: ([\d.]+) .\r\nLast-modified: .*\r\nContent-Range: bytes [-\d/]+\r\nAccept-Ranges: bytes\r\nContent-Type: text/html\r\nContent-Length: \d+\r\n\r\n<html>\r\n<head>\r\n<title>\r\nblank page\r\n</title>\r\n<META HTTP-EQUIV=\"Refresh\" CONTENT=\"2;URL=about:blank\">\r\n</head>\r\n<body>\r\nThere is nothing to see here, please move along!\r\n</body>\r\n</html>\r\n| p/SageTV PVR remote control httpd/ i/JWS based on Acme.Serve httpd $1/ d/media device/
match http m|^HTTP/1\.1 200 OK\r\nServer: SnapStream\r\nCache-Control: no-cache\r\nPragma: no-cache\r\nConnection: close\r\nContent-Type:text/html\r\n\r\n<html>\r\n<body>\r\n<h1>Beyond TV Web Admin Redirector</h1>| p/SnapStream Beyond TV http config/ d/media device/
match http m|^HTTP/1\.1 200 OK\r\nServer: SnapStream Web Server/([\d.]+)\r\n.*<title>\r\nBeyond TV - Web Admin Redirector\r\n</title>\r\n<meta HTTP-EQUIV=\"REFRESH\" CONTENT=\"2; URL=http://([\w_.-]+):(\d+)\">\r\n|s p/SnapStream Web Server/ v/$1/ i/Beyond TV http config; redirect to port $3/ h/$2/ d/media device/
match http m|^HTTP/1\.0 401 Unauthorized\nWWW-Authenticate: Basic realm=\"Server Manager\"\n\nYou must login to continue\n| p/ServerCP httpd/
match http m|^HTTP/1\.0 200 OK\r\ncontent-type: text/html\r\nconnection: close\r\npragma: no-cache\r\nX-Powered-By: PHP/([\d.]+)\r\nContent-type: text/html\r\n\r\n<!DOCTYPE html PUBLIC \"-//W3C//DTD XHTML 1\.0 Transitional//EN\" \"DTD/xhtml1-transitional\.dtd\">\n<html><head>\n<style type=\"text/css\"><!--\nbody {background-color: #ffffff;| p/Miranda mbot plugin/ i/PHP $1/
match http m|^HTTP/1\.0 200 OK\r\ncontent-type: text/html\r\nconnection: close\r\npragma: no-cache\r\nX-Powered-By: PHP/([\d.]+)\r\n\r\n<!DOCTYPE html PUBLIC \"-//W3C//DTD XHTML 1\.0 Transitional//EN\" \"DTD/xhtml1-transitional\.dtd\">\n<html><head>\n<style type=\"text/css\">\nbody {background-color: #ffffff;| p/Mianda mbot plugin/ i/PHP $1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Freechal P2P/([\d.]+)\r\n| p/Freechal P2P httpd/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Httpinfo olsrd plugin ([\d.]+) HTTP/1\.1\r\n| p/olsrd http info plugin/ v/$1/ o/Linux/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: audio/mpeg\r\nicy-br:([\d.]+)\r\n.*icy-name:([^\r\n]+)\r\n.*Server: Icecast ([\d.]+)\r\n\r\n|s p/Icecast streaming media server/ v/$3/ i/Name $2; Bitrate $1/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: audio/mpeg\r\nicy-br:([\d.]+)\r\n.*Server: Icecast ([\d.]+)\r\n|s p/Icecast streaming media server/ v/$2/ i/Bitrate $1/
match http m|^HTTP/1\.0 200 OK \r\nServer: Simple java\r\nDate: .*\r\nContent-length: \d+\r\nLast Modified: .*\r\nContent-type: text/html\r\n\r\n<html><head><title> RAID webConsole ([-\w_.]+)</title>| p/Intel Java RAID webConsole/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nLast-Modified: .*\n<HTML><HEAD><TITLE>Gopher</TITLE></HEAD><BODY>Welcome to Gopherspace!  You are browsing Gopher through\na Web interface right now\.|s p/pygopherd web-gopher gateway/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: DirectAdmin Daemon v([\d.]+) Registered to ([^\r\n]+)\r\n| p/DirectAdmin httpd/ v/$1/ i/Registered to $2/
match http m|^HTTP/1\.0 401 Unauthorized\r\nConnection: close\r\nContent-Type: text/html\r\nWWW-Authenticate: Basic realm=\"dreambox\"\r\n\r\n| p/Dreambox httpd/ d/media device/
match http m|^HTTP/1\.1 200 OK\r\nConnection: Keep-Alive\r\nKeep-Alive: timeout=180\r\nContent-Type: text/html\r\nContent-Length: \d+\r\n\r\n.*<H2>Wireless LAN Access Point Management</H2><br>\n    <Form method=\"POST\" action=\"act_login\">\n|s p/Compex Wifi APN NetPassage http config/ d/WAP/
match http m|^HTTP/1\.0 200 OK\r\nPragma: no-cache\r\n\r\n<HTML><HEAD><TITLE>WinRoute Pro - Web Interface</TITLE>| p/Kerio WinRoute Pro firewall http config/ o/Windows/
match http m|^HTTP/1\.0 302 Found\r\nCache-Control: no-cache\r\nConnection: Close\r\nContent-Length: 0\r\nContent-Type: application/octet-stream\r\nDate: .*\r\nLocation: /nonauth/login\.php\r\nPragma: no-cache\r\nServer: Kerio WinRoute Firewall Embedded Web Server\r\n\r\n| p/Kerio WinRoute firewall http config/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\ndate: .*\r\nserver: WebSEAL/([\d.]+) \(Build (\d+)\)\r\n| p/Tivoli Access Manager WebSEAL httpd/ v/$1 build $2/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Indy/([\d.]+)\r\n.*\r\n<GOTO href=\".*/kiss\.php\"|s i/FreeKiSS DVD player httpd/ p/Indy httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 200 Ok\r\nServer: httpd\r\n.*\n<title>SHARED STORAGE DRIVE</title>\n|s p/Maxtor Shared Storage Plus http config/ d/storage-misc/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: VCS-VideoJet-Webserver\r\n.*<title>VCS AG VideoJet 1000</title>|s p/VCS AG VideoJet 1000 http config/ d/media device/
match http m|^HTTP/1\.1 200 OK\r\nServer: VCS-VideoJet-Webserver\r\n.*<title>browser_capture</title>\r\n<script type=\"text/javascript\" for=document event=\"onkeydown\(\)\" language=\"JScript\">if\(window\.event\.keyCode==\"123\"\)|s p/VCS-VideoJet-Webserver httpd/ i/Bosch VIP X1 video encoder http config/ d/webcam/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: DVSS-HttpServer/([\d.]+)\r\n| p/DVSS Herculese DVR http config/ v/$1/ d/webcam/
match http m|^HTTP/1\.0 \d\d\d .*\r\nConnection: Close\r\nContent-Type: text/html\r\nServer: pcastd ([\d.]+)\r\n| p/Buffalo Linkstation http config/ i/pcastd $1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: BigFixHTTPServer/([\d.]+)\r\n| p/BigFix enterprise patch management httpd/ v/$1/
match http m|^HTTP/1\.0 200\r\nContent-Type:text/html\r\n\r\n<!--SELECTserver Full Page Header-->\r\n<html>\r\n\r\n<head>\r\n<title>\r\nSELECTserver: License Manager\r\n| p/Bentley SELECTserver license manager/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*X-Catalyst: ([\d.]+)\r\n\r\n|s p/Catalyst Framework httpd/ v/$1/
match http m|^HTTP/1\.0 301 moved \(redirection follows\)\r\nServer: BaseHTTP/([\d.]+) Python/([\w.]+)\r\nDate: .*\r\nContent-type: text/html\r\nLocation: http://([-\w_.:]+)/viewcvs/\r\n\r\n| i/ViewCVS http interface; Python $2/ p/BaseHTTP/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: GoAhead-Webs\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"DCM-202\"\r\n| p/D-Link DCM-202 Docsis Cable Modem http config/ i/GoAhead embedded httpd/ d/router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: micro_httpd\r\n.*\r\n<title>Belkin Wireless DSL Router</title>\r\n|s p/Belkin Wireless ADSL http config/ i/micro_httpd/ d/broadband router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nContent-Length: \d+\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<HTML><HEAD><TITLE>VPAD01 V([\d.]+) *</TITLE>| p/E-Tech VPAD01 http config/ v/$1/ d/VoIP adapter/
match http m|^HTTP/1\.0 \d\d\d .*: Quick 'n Easy Web Server\r\n|s p/Quick 'n Easy Web Server httpd/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: SentinelProtectionServer/([\d.]+)\r\n| p/SafeNet Sentinel Protection Server/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: WatchGuard Firewall\r\nwww-authenticate: Digest realm=\"WatchGuard Firebox Local User\"| p/WatchGuard Firewall http config/ d/firewall/
match http m|^HTTP/1\.1 200 OK\r\nServer: InterNiche Technologies WebServer ([\d.]+)\r\nDate: .*\r\nContent-type: text/html\r\nConnection: Close\r\n\r\n<html>\r\n<head>\r\n<title>CAN@Net II| p/InterNiche CAN@net II ethernet bridge http config/ v/$1/ d/bridge/
match http m|^HTTP/1\.1 200 OK\r\nDate:.*<title>Welcome to VMware ESX Server ([\d.]+)</title>\n\n|s p/VMware ESX Server httpd/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*document\.write\(\"<title>\" \+ ID_EE?SX_Welcome \+ \"</title>|s p/VMware ESXi Server httpd/
match http m|^HTTP/1\.1 400 Bad Request\r\nContent-Type: text/html.*\n<meta name=robots content=\"none\">\n<title>Secure&#32;Access&#32;SSL&#32;VPN</title>\n\n|s p/Juniper Networks Secure Access SSL VPN http config/ d/security-misc/
match http m|^HTTP/1\.1 400 Bad Request\r\nContent-Type: text/html.*\n<meta name=robots content=\"none\">\n<title>Sign&#32;in&#32;to&#32;begin&#32;\xf92\0\0\xa8o\xee\"\xa8o\xee\"sion&#46;</title>\n\n|s p/Juniper Networks Secure Access SSL VPN http config/ d/security-misc/
match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/([\d.]+)\r\nMIME-version: 1\.0\r\nContent-type: text/html\r\n\r\n<HTML>\n<HEAD>\n  <TITLE>WireSpeed Dual Connect</TITLE>\n\n| p/Westell WireSpeed Dual Connect ADSL router http config/ i/RapidLogic http $1/ d/router/
match http m|^HTTP/1\.1 401 Unauthorized\r\n.* This is a WebSEAL error message template file\.|s p/Tivoli Access Manager WebSEAL httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\nConnection: close\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n\r\n<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.0 Frameset//EN\">\n<html>\n\n<head>\n<title>Web Smart Switch</title>| p/3Com Baseline 2816 switch http config/ d/switch/
match http m|^HTTP/1\.0 200 OK\r\nServer: SimpleHTTP/([\d.]+) Python/([\d.]+)\r\nDate:.*<title>AmaroK playlist</title>\n\n|s p/AmaroK media player http interface/ i/SimpleHTTP $1; Python $2/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: LANDesk Management Agent/([\d.]+)\r\n| p|LANDesk/Intel Management Agent http config| v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: PowerSchool\r\n| p/PowerSchool student information system httpd/
match http m|^HTTP/1\.0 .*Server: NetWare GroupWise POA ([\d.]+)\r\n|s p/NetWare GroupWise POA httpd/ v/$1/ o/NetWare/
match http m|^HTTP/1\.1 \d\d\d .*Server: Webserver\r\n.*\n\tXerox Corporation \(R\)\n\t\(c\) Xerox Corporation 2002 - 2004\.\n|s p/Xerox WorkCentre Pro httpd/ d/printer/
match http m|^HTTP/1\.1 \d\d\d .*Server: Webserver\r\n.*\tCopyright \(c\) 2002-2006 Xerox Corporation\. All Rights Reserved\. \n\n|s p/Xerox WorkCentre Pro httpd/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Intrinsyc deviceWEB v([\d.]+)\r\n| p/Intermec CK31 http config/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Hitachi Web Server ([-\d.]+)\r\n| p/Hitachi Web Server httpd/ v/$1/
match http m|^HTTP/1\.1 .*\r\nServer: Hitachi Web Server\r\n|s p/Hitachi Web Server httpd/
match http m|^HTTP/1\.1 \d\d\d .*<address>MLDonkey/([\d.]+) at|s p/MLDonkey http interface/ v/$1/
match http m|^HTTP/1\.1 401 \r\nServer: PrintSir WEBPORT ([\d.]+)\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"Default password:1234\"\r\n\r\n401 Unauthorized - User authentication is required\.| p/Hawking HP1SU Printserver http config/ i/PrintSir WEBPORT $1; Default password 1234/ d/print server/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: GoAhead-Webs\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"(GN-\w+)\"\r\n| p/Gigabyte $1 WAP http config/ i/GoAhead embedded httpd/ d/WAP/
match http m|^HTTP/1.0 401 Unauthorized\r\n.*WWW-Authenticate: Basic realm="(GN-\w+)"|s p/Gigabyte $1 WAP http config/ d/WAP/
match http m|^HTTP/1\.0 200\r\nContent-type: text/html\r\nConnection: close\r\nCONTENT-LENGTH: \d+\r\n\r\n.*\r\n<meta http-equiv=\"refresh\" content=\"1; URL=secure/ltx_conf\.htm\">|s p/Lantronix XPort embedded ethernet http config/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: FreeBrowser/([\d.]+) \(Win32\)\r\n| p/FreeBox FreeBrowser http interface/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: GG/([\d.]+) \(Unix\) Debian GNU/Linux\r\nWWW-Authenticate: Basic realm=\"gg zone\"\r\n| p/Ruchomy Terminal Gadu-Gadu http interface/ v/$1/ i/Debian/ o/Linux/
match http m|^HTTP/1\.0 \d\d\d .*\r\nSet-Cookie: SESSIONID=-1 \r\nServer: Easy File Sharing Web Server v([\w.]+)\r\n| p/Easy File Sharing Web Server httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*<title>Welcome to the Galty client depl</title>\r\n|s p/Galty Technologies GaltyExplorer httpd/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Adaptec ASM ([\d.]+)\r\n| p|Adaptec/IBM ServeRAID Management http config| v/$1/ d/storage-misc/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: darkstat/([\d.]+)\r\n| p/darkstat network analyzer httpd/ v/$1/ o/Unix/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Rumpus\r\n| p/Rumpus httpd/ o/Mac OS X/
match http m|^HTTP/1\.1 \d\d\d .*Server: HTTPD\r\n.*\r\n<title>([\w-]+) Network Camera</title>|s p/Panasonic $1 webcam http config/ d/webcam/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Medusa/([\w.]+)\r\n.*\n<head>\n<meta name=\"Author\" content=\"DeStar, made by Holger Schurig\"|s i/Destar Asterisk PBX http config/ p/Medusa httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Medusa/([\w.]+)\r\n.*<title>Sophos Anti-Virus - Home</title>\n\n|s i/Sophos Anti-Virus Home http config/ p/Medusa httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\n.*Expires: Thu, 01 Jan 1970 00:00:00 GMT\r\n.*Server: Medusa/([\w._-]+)\r\n.*<title>Supervisor Status</title>\n  <link href=\"stylesheets/supervisor\.css\" rel=\"stylesheet\" type=\"text/css\" />|s p/Medusa httpd/ v/$1/ i/Supervisor process manager/
match http m|^HTTP/1\.0 .*\r\nDate: .*\r\nServer: WSGIServer/([\w._-]+) Python/([\w._-]+)\r\n| p/Django httpd/ i/WSGIServer $1; Python $2/
match http m|^HTTP/1\.0 401 Unauthorized\r\nDate: .*\r\nServer: Agranat-EmWeb/R([\d_]+)\r\nWWW-Authenticate: Basic realm=\"Nortel p-Class GbE2 Switch@[\d.]+\"\r\n\r\n401 Unauthorized\r\n| p/Agranat-EmWeb/ v/$SUBST(1,"_",".")/ i/Nortel p-Class GbE2 switch http config/ d/switch/
match http m|^HTTP/1\.1 200 OK\r\nConnection: Keep-Alive\r\nAccept-Ranges: bytes\r\nKeep-Alive: timeout=15, max=100\r\nContent-Type: text/html\r\nExpires: 0\r\n\r\n\n<html>\n<title>Apt-cacher version ([\d.]+)\n| p|apt-cache/apt-proxy httpd| v/$1/ o/Linux/
match http m|^HTTP/1\.0 200 Ok\nDate: .*\nContent-type: text/html\n\n<font size=\"-4\">\nIf you can read this, you are sitting too close to the monitor\.\n</font>\n| p/Unknown trojan/ i/**BACKDOOR**/ o/Windows/
match http m|^HTTP/1\.0 200 OK\r\n.*<meta http-equiv=\"refresh\" content=\"0; URL=/cgi-bin/status\.sh\" />\n\t\t<title>La Fonera</title>|s p/La Fonera WAP http config/ d/WAP/
match http m|^<html>\n<title>DES-(\w+) +(Login)?</title>\n| p/D-Link DES-$1 switch http config/ d/switch/
match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/([\d.]+)\r\n.*<title>Broadaband Voice Telephone Adapter</title>\r\n|s p/VG112-D51 VoIP CPE http config/ i/RapidLogic httpd $1/ d/VoIP adapter/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"Browser\"\r\nContent-Type: text/html\r\nServer: Allegro-Software-RomPager/([\d.]+)\r\n\r\n<HTML>\n<HEAD>\n<TITLE>Protected Object</TITLE>\n</HEAD>\n<BODY>\n<H1>Protected Object</H1>\n<br>This page requires a login to access\.<br><br>You have <b>failed to login properly</b>\.  Try again\.<P>\n\n</BODY>\n</HTML>\n| p/Kronos 4500 Clock http config/ i/Allegro httpd $1/ o/VxWorks/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWww-Authenticate: Basic REALM=\"snom\"\r\nContent-Type: text/plain\r\nContent-Length: 22\r\n\r\nUnauthorized request\r\n| p/Snom 300 VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.1 .*\r\nServer: Reactivity Gateway\r\n|s p/Reactivity XML Security Gateway/
match http m|^HTTP/1\.0 200 Ok\r\nServer: httpd\r\nDate: .*\n<title>WL700g Web Manager</title>|s p/Asus WL700gE Wireless Storage router http config/ d/WAP/
match http m|^<html>\n<title>24-Port 10/100Mbps \+ 2 Combo Copper/SFP PoE Management Switch</title>\n| p/D-Link DES-1526 switch http config/ d/switch/
match http m|^HTTP/1\.0 200 Ok\r\nServer: Embeded_httpd\r\nDate: .*\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<html>\r\n\r\n<head>\r\n<META NAME=\"GENERATOR\" Content=\"Multi-Functional Broadband NAT Router \(R([\d.]+)\)\">| p/Ambit DOCSIS router http config/ i/R$1/ d/router/
match http m|^HTTP/1\.1 200 OK\r\n.*\n<META NAME=\"GENERATOR\" Content=\"Multi-Functional Broadband NAT Router \(R([\d.]+)\)\">\n|s p|NTL/Ambit DOCSIS router http config| i/R$1/ d/router/
match http m|^HTTP/1\.0 200 OK\r\nDate: .*\r\nServer: qHTTPs\r\nMIME-version: 1\.0\r\nContent-type: text/html\r\nLast-modified: .*\r\nContent-length: \d+\r\n\r\n<html>\r\n<head>\r\n<title>JUPSMON</title>| p/Generex JAVA UPSMON http config/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\nContent-Type: text/html; charset=iso-8859-1\r\n\r\n<html>\r\n<head>\r\n<meta http-equiv=\"Content-Type\" content=\"text/html; charset=iso-8859-1\">\r\n<title>8 Port Gigabit Switch</title>\r\n| p/Longshine LCS-GS8208-A switch http config/ d/switch/
match http m|^<html>\r\n<head>\r\n<meta http-equiv=\"Content-Language\" content=\"it\">\r\n<meta http-equiv=\"Content-Type\" content=\"text/html; charset=windows-1252\">\r\n<meta http-equiv=\"Refresh\" content=\"10\">\r\n<title>UPS web page</title>\r\n| p/Netman UPS monitor http config/ d/power-device/
match http m|^HTTP/1\.1 200 Ok\r\nServer: NAE Server\r\nContent-Length: 73\r\nConnection: close\r\n\r\n<html><center><h1>NAE Server Health Check Succeeded\.</h1></center></html>| p/Ingrian i3xx health monitor httpd/ d/security-misc/
match http m|^HTTP/1\.1 302 Tempor\xe4r verschoben\r\nConnection: close\r\nContent-Type: text/html\r\nServer: Indy/([\d.]+)\r\nLocation: /Wikipedia/\r\n\r\n| i/German Wikipedia DVD browser httpd/ p/Indy httpd/ v/$1/
match http m|^HTTP/1\.0 200 Ok\r\nServer: httpd\r\n.*\n<title>HP Media Vault: [^<]*</title>|s p/HP Media Vault http config/ d/media device/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\nServer: WindWeb/([\d.]+)\r\nDate: .*\r\nContent-Type: text/html\r\n\r\n<html>\n<head>\n<title>(\w+) System Control Center</title>\n| p/Hughes $2 satellite modem http config/ i/WindWeb httpd $1/
# auther??
match http m|^HTTP/1\.0 200 OK\r\nServer: Camera Web Server/([\d.]+)\r\nAuther: Steven Wu\r\n| p|D-Link/Airlink IP webcam http config| v/$1/ d/webcam/
match http m|^HTTP/1\.0 200 OK\r\nServer: Web Server/([\d.]+)\r\nAuther: Steven Wu\r\n| p/D-Link print server http config/ v/$1/ d/print server/
match http m|^HTTP/1\.0 401 Authorization Required\r\nconnection: Close\r\ncontent-type: text/html\r\nserver: NEWS/([\w._-]+ \(Funk\)) \(Windows 2000\)\r\n| p/Juniper Steel-Belted Radius http config/ i/NEWS httpd $1; Windows 2000/ o/Windows/
match http m|^HTTP/1\.1 401 Unauthorized\r\nDate: .*\r\nWWW-Authenticate: basic realm=IRC Services\r\nContent-Type: text/html\r\nContent-Length: 14\r\n\r\nAccess denied\.| p/ircservices httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\nSet-Cookie: Ipswitch={| p/Ipswitch WhatsUp Professional httpd/ o/Windows/
match http m|^HTTP/1\.0 200 OK.*\r\n\tThis machine cannot be used for administration\.\r\n|s p/Cisco Secure ACS httpd/ i/administration disabled/ d/router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"Wusage\"\r\n| p/Wusage httpd/
match http m|^HTTP/1\.1 401 \r\nServer: PrintSir WEBPORT ([\d.]+)\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"Default password:sitecom\"\r\n\r\n| p/Sitecom print server http config/ i/Webport httpd $1; default password sitecom/ d/print server/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Sphere V([^\r\n]+)\r\n| p/Ultima online sphere httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: BlueDragon Server ([\d.]+)\r\n| p/New Atlanta BlueDragon httpd/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\nServer: WSTL CPE ([\d.]+)\r\n| p/Westell cable modem http config/ v/$1/ d/broadband router/
match http m|^HTTP/1\.1 200 OK\r\n.*\r\n<title>Welcome to VMware VirtualCenter ([\d.]+)</title>|s p/VMware VirtualCenter httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: vdradmind/([-\w_.]+)\r\n| p/vdradmin http config/ v/$1/ o/Linux/
match http m|^HTTP/1\.0 \d\d\d .*<TITLE>Actiontec MegaControl Panel</TITLE>|s p/Actiontec router http config/ d/router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nWWW-Authenticate: Basic realm=\"Sony Network Camera (SNC-\w+)\"\r\nContent-Type: text/html\r\nServer: NetEVI/([\d.]+)\r\n| p/Sony webcam $1 http config/ v/NetEVI httpd $2/ d/webcam/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: TiVo Calypso for Mac OS X\r\n| p/TiVo Calypso Desktop/ o/Mac OS X/
match http m|^HTTP/1\.1 0 \(null\)\r\nContent-Length: 0\r\n\r\n| p/Simpserver MSN encryption or DAAP from Rhythmbox httpd/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Java/([-\w_.]+) javax\.wbem\.client\.adapter\.http\.transport\.HttpServerConnection\r\n|s p/Java $1 http.transport.HttpServerConnection httpd/
match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/([\d.]+)\r\n.*\nExtend-sharp-setting-status: 0\r\n\r\n<HTML>\r\n<HEAD><META HTTP-EQUIV=\"Content-Type\" CONTENT=\"text/html; charset=iso-8859-1\">\r\n<TITLE>TOP PAGE</TITLE>\r\n|s i/Sharp Imagistics printer http config/ p/RapidLogic httpd/ v/$1/ d/printer/
match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/([\d.]+)\r\n.*Last-Modified: Mon, 1 Jan 2001 12:00:00 GMT\nExtend-sharp-setting-status: 0\r\n\r\n.*<title>(AR-\w+)</title>|s p/RapidLogic httpd/ v/$1/ d/printer/ i/Sharp $2 printer http config/
match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/([\d.]+)\r\n.*\nExtend-sharp-setting-status: 0\r\n.*<title>([A-Z][A-Z0-9-]+)</title>\n|s p/RapidLogic httpd/ v/$1/ i/Sharp $2 printer http config/ d/printer/
match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/([\d.]+)\r\n.*Last-Modified: Mon, 1 Jan 2001 12:00:00 GMT\nExtend-sharp-setting-status: 0\r\n.*<meta http-equiv=\"Expires\" content=\"Thu, 01 Dec 1994 16:00:00 GMT\">.*<title>(\w+)</title>|s p/RapidLogic httpd/ v/$1/ i/Sharp Imagistics printer/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Agranat-EmWeb/R([\d_]+)\r\nWWW-Authenticate: Basic realm=\"HP p-Class GbE2 Switch|s i/HP p-Class GbE2 switch http config/ p/Agranat-EmWeb/ v/$SUBST(1,"_",".")/ d/switch/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: HttpServer\r\nDate: .*\r\nContent-type: text/plain\r\nContent-length: \d+\r\nWWW-Authenticate: Basic realm=\"Pylon Anywhere Secure Gateway\"\r\n\r\nUnauthorized| p/Pylon Anywhere Secure Gateway http config/ d/security-misc/
match http m#^HTTP/1\.1 \d\d\d .*\t\t\t<TITLE> (?:KONICA MINOLTA|MINOLTA-QMS) magicolor (\w+ DL) </TITLE>\r\n#s p/Konica Minolta Magicolor $1 printer http config/ d/printer/
match http m|^HTTP/1\.1 401 Unauthorized\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"Authentication\"\r\n\r\n<HEAD><TITLE>Authorization Required</TITLE></HEAD><BODY><H1>Authorization Required</H1>Browser not authentication-capable or authentication failed\.</BODY>\n\n|s p/Cisco Adaptive Security Appliance http config/ d/security-misc/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Virata-EmWeb/R([\d_]+)\r\n.*\n\n  <title>HP LaserJet (\w+) Series|s i/HP LaserJet $2 Series http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/printer/

match http m|^HTTP/1\.0 200 Data follows\r\nDate: .*\r\nServer: Radia Integration Server([^\r\n]+)\r\n| p/HP Radia Integration Server httpd/ v/$1/
match http m|^HTTP/1\.0 200 Data follows\r\nDate: .*\r\nServer: HP Client Automation \(httpd-managementportal\) \r\n| p/HP Client Automation httpd/ i/management portal/
match http m|^HTTP/1\.0 200 Data follows\r\nDate: .*\r\nServer: HP Client Automation \(httpd-patchmanager\) \r\n| p/HP Client Automation httpd/ i/patch manager/
match http m|^HTTP/1\.0 200 Data follows\r\nDate: .*\r\nServer: HP Client Automation \(httpd-rps\) \r\n| p/HP Client Automation httpd/ i/rps/
match http m|^HTTP/1\.0 200 Data follows\r\nDate: .*\r\nServer: HP Client Automation \(httpd-pm\) \r\n| p/HP Client Automation httpd/ i/policy server/
match http m|^HTTP/1\.0 404 Not Found\r\nDate: .*\r\nServer: HP Client Automation Messaging Service ([\w._-]+)\r\n| p/HP Client Automation httpd/ v/$1/ i/messaging service/

match http m|^HTTP/1\.1 302 Document Follows\r\nLocation: /hag/pages/home\.ssi\r\n\r\nHTTP/1\.1 302 Document Follows\r\nLocation: /hag/pages/home\.ssi\r\n\r\nConnection: close\r\n\r\n| p/D-Link DSL-504G ADSL router http config/ d/router/
match http m|^HTTP/1\.0 302 Redirection\r\nDate: .*\r\nServer: iGuard Embedded Web Server/([-\w_.]+) \(\w+\) SN:([-\w]+)\r\nPragma: no-cache\r\nLocation: /Admins/index\.html\r\n\r\n| p/iGuard access control system http config/ v/$1/ i/Serial $2/ d/security-misc/
# Not sure if this will match all:
match http m|^HTTP/1\.0 200 OK\r\nDate: [A-Z]{3}.*</head>\n<body>\n<p>You will automatically be redirected to a secure connection in 2 seconds\.</p>\n</body>\n</html>\n|s p/HP 9000 http service/ o/HP-UX/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: LiteSpeed\r\n|s p/LiteSpeed httpd/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: LiteSpeed/([\w. ]+)\r\n|s p/LiteSpeed httpd/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*Powered By <a href='http://www\.litespeedtech\.com'>LiteSpeed Web Server</a>|s p/LiteSpeed httpd/
match http m|^HTTP/1\.0 200 Ok\r\nServer: httpd\r\n.*<script type=\"text/javascript\" src=\"lang_pack/language\.js\"></script>\n\t\t<link type=\"text/css\" rel=\"stylesheet\" href=\"style/[-\w_.]+/style\.css\" />\n\t\t<!--\[if IE\]>|s p/DD-WRT milli_httpd/ i/Linksys WRT54G http config/ d/WAP/ o/Linux/

match http m|^HTTP/1\.1 401 N/A\r\nServer: (?:TP-LINK )?Router\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"TP-LINK Wireless AP ([\w/]+)\"| p/TP-LINK $1 WAP http config/ d/WAP/
match http m|^HTTP/1\.1 401 N/A\r\nServer: TP-LINK Router\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"TP-LINK Wireless N Access Point ([\w/]+)\"\r\n| p/IP-LINK $1 WAP http config/ d/WAP/
match http m|^HTTP/1\.1 401 N/A\r\nServer: TP-LINK Router\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"TP-LINK Wireless Router ([\w/]+)\"| p/TP-LINK $1 WAP http config/ d/WAP/
match http m|^HTTP/1\.1 401 N/A\r\nServer: TP-LINK Router\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"TP-LINK Wireless N Router ([\w/]+)\"\r\n| p/TIP-LINK $1 WAP http config/ d/WAP/
match http m|^HTTP/1\.1 401 N/A\r\nServer: TP-LINK Router\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"TP-LINK Wireless Lite N Router ([\w/]+)| p/TP-LINK $1 WAP http config/ d/WAP/
match http m|^HTTP/1\.1 401 N/A\r\nServer: TP-LINK Router\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"Web Smart Switch\"| p/TP-LINK Web Smart Switch http config/ d/switch/
match http m|^HTTP/1\.1 401 N/A\r\nServer: TP-LINK Router\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"TP-LINK Wireless N Gigabit Router ([\w._-]+)\"\r\n| p/TP-LINK $1 WAP http config/
match http m|^HTTP/1\.1 401 N/A\r\nServer: Router\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"TP-LINK Wireless Router (WR[\w/]+)\"| p/TP-LINK $1 WAP http config/ d/WAP/
match http m|^HTTP/1\.1 401 N/A\r\nServer: Router\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"TP-LINK SOHO Router (R[\w/]+)\"| p/TP-LINK $1 WAP http config/ d/WAP/
match http m|^HTTP/1\.1 401 N/A\r\nServer: Router\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"TP-LINK Router (\w+)\"\r\n| p/TP-LINK $1 router http config/ d/router/
match http m|^HTTP/1\.1 401 N/A\r\nServer: Router\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"(TL-\w+)\xcf\xb5\xc1\xd0 SOHO\xbf\xed\xb4\xf8\xc2\xb7\xd3\xc9\xc6\xf7\"\r\nContent-Type: text/html\r\n\r\nWeb Server Error Report:<HR>\n<H1>Server Error: 401 N/A</H1>\r\nOperating System Error Nr:3997698: /userRpm/index\.htm <P><HR><H2>Access denied / wrong user name or password</H2><P><P><HR><H1>/userRpm/index\.htm</H1><P><HR>$| p/TP-LINK $1 router http config/ d/router/

match http m|^HTTP/1\.0 200 OK\r\nServer: Terayon/([\d.]+)\r\nContent-type: text/html\r\n\r\n<html><head><title>Cable Modem Information Center</title>| p/Terayon cable modem http config/ v/$1/ d/broadband router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Tornado/([-\w_.]+)\r\n| p/Puakma Tornado httpd/ v/$1/
match http m|^<html><head><title>Cannot find server</title></head><body>\n<br>Access to this web page is currently unavailable\.<P><HR></BODY></HTML>\n$| p/Arris cm450 cable modem http config/ d/broadband router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"RV082\"\r\n| p/Linksys RV082 VPN router http config/ d/router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: \r\n.*WWW-Authenticate: Basic realm=\"Linksys WAG54GS|s p/Linksys WAG54GS broadband router http config/ d/broadband router/
match http m|^HTTP/1\.1 \d\d\d .*href=\"images/favicon\.ico\">\n<title>NETGEAR ProSafe\x99 - Welcome to Configuration Manager Login</title>\n<!--\nCopyright \(c\) 2005-2006 TeamF1|s p/Netgear ProSafe FVS338 VPN firewall http config/ d/firewall/
match http m|^HTTP/1\.1 \d\d\d .*<link rel=\"icon\" type=\"image/ico\" href=\"images/favicon\.ico\">\n<title>NETGEAR ProSafe&#8482; - Welcome to Configuration Manager Login</title>\n<!--\nCopyright \(c\) 2005-2007 TeamF1, Inc\. \(www\.TeamF1\.com\)\nAll rights reserved\.\n-->|s p/Netgear ProSafe VPN firewall http config/ d/firewall/
match http m|^HTTP/1\.1 200 OK\r\n.*<title>NETGEAR ProSafe&#8482; - Welcome to Configuration Manager Login</title>\n<!--\nCopyright \(c\) 2005-2009 TeamF1, Inc\. \(www\.TeamF1\.com\)\nAll rights reserved\.\n-->\n|s p/Netgear ProSafe FVX538 VPN firewall http config/ d/firewall/
match http m|^HTTP/1\.0 \d\d\d .*\r\nMime-Version: 1\.0\r\nServer: Web Transaction Server For ClearPath MCP ([\d.]+)\r\n| p/Unisys ClearPath MCP http config/ v/$1/
match http m|^HTTP/1\.0 401 Access Denied\r\nWWW-Authenticate: NTLM\r\nContent-Length: 24\r\nContent-Type: text/html\r\n\r\nError: Access is Denied\.| p/Microsoft IIS httpd/ v/3.X/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: AnomicHTTPD \(www\.anomic\.de\)\r\n|s p/Anomic YaCy P2P Search Engine httpd/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: SnapStream\r\nCache-Control: no-cache\r\nPragma: no-cache\r\nConnection: close\r\nContent-Type:text/html\r\n\r\n<html>\r\n<head>\r\n<title>\r\nBeyond TV - Web Admin Redirector\r\n| p/SnapStream Media Beyond TV PVR http config/ d/media device/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: thttpd-alphanetworks/([\d.]+)\r\n.*\r\nWWW-Authenticate: Basic realm=\"(DI-\w+)\"\r\n|s p/D-Link $2 router http config/ i/thttpd-alphanetworks $1/ d/router/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: thttpd-alphanetworks/([\d.]+)\r\n.*\r\nWWW-Authenticate: Basic realm=\"BRL-04UR\"\r\n\r\n|s p/Planex BRL-04UR router http config/ i/thttpd-alphanetworks $1/ d/router/
match http m|^HTTP/1\.0 200 OK\r\nServer: M900\w*-HTTP-Server/([\d.]+)\r\nContent-Type: text/html\r\n\r\n<html><head><title>(M900\w*) AP</title>| p/Trango $2 AP http config/ v/$1/ d/broadband router/
match http m|^HTTP/1\.1 401 Unauthorised\r\nServer: ATR-HTTP-Server/([\d.]+)\r\nContent-Type: text/html\r\nWWW-Authenticate: Basic realm=\"Allied Telesyn AT-(AR\w+)\"\r\n| p/Allied Telesyn $2 router http config/ v/$1/ d/router/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nConnection: close\r\nServer: Yaws/([-\w_.]+) Yet Another Web Server\r\n| p/Yaws httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Web Server\r\n.*<IMG SRC = \"/base/images/netgear_(\w+)_banner\.gif\"|s p/Netgear $1 gigabit switch http config/ d/switch/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Centile Embedded HTTPSd server/([\d.]+)\r\n| p/Centile VoIP adapter http config/ v/$1/ d/VoIP adapter/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nConnection: close\r\nWWW-Authenticate: Digest realm=\"DUALCOM-\d+.USER\",| p/CyberSwitching Dualcom power device http config/ i/rabbit 2000 embedded/ d/power-device/
match http m|^HTTP/1\.0 \d\d\d .*Server: PWLib-HTTP-Server/([\d.]+) PWLib/([\d.]+)\r\n.*<HTML>\r\n\r\n<HEAD>\r\n<TITLE>Welcome to OpenMCU</TITLE>|s i/OpenMCU http interface; PWLib $2/ p/PWLib httpd/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: PWLib-HTTP-Server/([\w._-]+) PWLib/([\w._-]+)\r\n.*Expires: Tue, 01 Jan 1980 00:00:00 GMT\r\n.*<title>SOPHO (\w+) In-System Gateway</title>|s p/PWLib http/ v/$1/ i/Philips Sopho $3 PBX http config; PWLib $2/ d/PBX/
match http m|^HTTP/1\.1 200 Ok\r\nServer: micro_httpd\r\n.*<title>3Com - OfficeConnect ADSL Wireless 108Mbps 11g Firewall Router</title>|s p/3Com OfficeConnect ADSL WAP http config/ i/micro_httpd/ d/WAP/
match http m|^HTTP/1\.1 404 Not found\n\0$| p/nohttpd 404 responding httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: ICONAG web server \(Ver\.: ([-\w_.]+)\)\r\n| p/ICONAG building control http config/ v/$1/ d/specialized/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"Environmental Monitoring Unit\"\r\nContent-Type: text/html\r\nServer: Allegro-Software-RomPager/([\d.]+)\r\n\r\n| p/APC Environmental Monitoring Unit http config/ i/Allegro embedded httpd $1/ d/specialized/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: RapidLogic/([\d.]+)\r\nMIME-version: 1\.0\r\nContent-type: text/html\r\n\r\n<HTML>\r\n<HEAD>\r\n<TITLE>Westell VersaLink Wireless Gateway</TITLE>| p/Westell VersaLink WAP http config/ i/RapidLogic httpd $1/ d/WAP/
match http m|^HTTP/1\.1 \d\d\d\r\nContent-Length:\d+\r\nContent-Type: text/html\r\n\r\n<html><head><link rel=\"stylesheet\" type=\"text/css\" href=\"/viawarp\.css\" />| p/Nova viaWARP httpd/ o/Windows/
# Looks more general than a media device
match http m|^HTTP/1\.0 200 OK\r\nConnection: Close\r\nContent-Type: text/html\r\nServer: wizd ([^\r\n]+)\r\n| p/wizd media viewer httpd/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\nServer: XES WindWeb/([\d.]+)\r\n| p/XES Synergix printer http config/ i/Windweb httpd $1/ d/printer/
match http m|^HTTP/1\.0 200 OK\r\nPragma:no-cache\r\nContent-Length: \d+\r\nContent-Type: text/html\r\n\r\n<html>\n<head>\n<title>INTERMEC ([\d+/]+); IP| p/Intermec $1 print server http config/ d/print server/
match http m|^HTTP/1\.0 401 Unauthorized\r\nDate: .*\r\nServer: GoAhead-Webs\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"CameraServer\"\r\n| p/AirLink 101 SkyIPCam http config/ i/GoAhead httpd/ d/webcam/
match http m|^HTTP/1\.0 200 OK\r\nCache-control: no-cache\r\n.*<title>BVA8055 Web Configuration Pages</title>|s p/Leadtek BVA8055 VoIP adapter http config/ d/VoIP adapter/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: KTorrent/(\d[-\w_.]+)\r\n|s p/Ktorrent web interface/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Wildcat/v([-\w_.]+)\r\n|s p/Wildcat Interactive Net Server httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Allegro-Software-RomPager/([\d.]+)\r\n\r\n<HTML>\n<HEAD>\n<TITLE>NRG (\w+) .*Network Printer D Model-Network Administration</TITLE>.*<FONT SIZE=\+2>Unit Serial Number (\w+)</FONT>|s p/NRG $2 printer http config/ i/Allegro http $1; Serial $3/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Ethernut ([^\r\n]+)\r\n| p/Ethernut demo httpd/ v/$1/ o|Nut/OS|
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Mongrel ([\d.]+)\r\n|s p/Mongrel httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Micro-Web\r\nContent-type: text/html\r\n\r\n<html>\r\n<head>\r\n<FORM ACTION=/LoginPostData\.fn METHOD=POST>\r\n<INPUT TYPE=HIDDEN NAME=BrowserId VALUE=\w+>\r\n<TABLE ALIGN=CENTER BORDER=3 CELLPADDING=8 CELLSPACING=1 WIDTH=600 BGCOLOR=\"#C0C0C0\">\r\n<TR><TH COLSPAN=1><BIG><BIG>Login to the Remote Management Interface</BIG></BIG>| i/HP MSL5000 storage http config/ p/Micro-Web httpd/ d/storage-misc/
match http m|^HTTP/1\.0 \d\d\d .*Server: WindWeb/([\d.]+)\r\n.*\"/js/branding_utils\.js\"></script>\r\n<script language=\"JavaScript\"><!--\nvar iPortIndex = 0; \nvar iProtocol = 0; \nvar serialPort = 1|s i/HP MSL5000 storage config/ p/WindWeb httpd/ v/$1/ d/storage-misc/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: WindWeb/([\d.]+)\r\n.*\"/js/branding_utils\.js\"></script>\r\n\r\n<script language=\"JavaScript\"><!--\nvar ConfigDirty = 1\nvar routerMode = 1\nvar modularRouter = 0\nvar szFCHostName = \"none\"\n|s p/WindWeb httpd/ v/$1/ i/HP E1200 storage config/ d/storage-misc/
match http m|^HTTP/1\.1 401 Unauthorized\r\nDate: .*\r\nServer: Agranat-EmWeb/R([\d_]+)\r\nWWW-Authenticate: Basic realm=\"read@\"\r\n\r\n<META HTTP-EQUIV=refresh CONTENT=0;URL=/util/401\.html>| i/3com Corebuilder switch http config/ p/Agranat-EmWeb/ v/$SUBST(1,"_",".")/ d/switch/
match http m|^HTTP/1\.1 401 Unauthorized\nDATE: .*\nWWW-Authenticate: Basic realm=\"Delta UPS Web\"\nServer: Delta UPSentry\n| p/Belkin Bulldog UPS Monitor http config/ d/power-device/
match http m|^HTTP/1\.0 \d\d\d .*<h3>BitTorrent download info</h3>\n<ul>\n<li><strong>tracker version:</strong> ([-\w_.]+) \(BitTornado\)</li>|s p/BitTornado tracker/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: ChatSpace/([\d.]+)\r\n| p/Akiva ChatSpace httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\n<title>EMC Connectrix Management</title>|s p/EMC Connectrix http config/
match http m|^HTTP/1\.0 404 Not Found\r\nConnection: close\r\nContent-type: text/html\r\n\r\n<html>404 Not Found \(Error 3\)<BR></html>$| p/ESET NOD32 windows anti-virus http config/ o/Windows/
match http m|^HTTP/1\.0 200 Document follows\nContent-Type: text/html\nContent-length: \d+\n\n<html>\n<head>\n<title>BeanShell Remote Session</title>\n| p/BeanShell java scripting http console/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: IntellipoolHTTPD/([\d.]+)\r\n|s p/Intellipool Network Monitor http config/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: MX4J-HTTPD/([\d.]+)\r\n.*<title>CruiseControl - Agent View</title>\n|s i/JMX CruiseControl http config/ p/MX4J/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*/cgi-bin/prodhelp\?prod=axis_540\+/542\+&ver=([\d.]+)&|s p|AXIS 540+/542+ print server http config| v/$1/ d/print server/
match http m|^HTTP/1\.1 400 Bad Request\r\nDate: .*\r\nRIPT-Server: iTunesLib/([-\w_.]+) \(Mac OS X\)\r\n| p/Apple TV http config/ i/iTunesLib $1/ d/media device/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Vistabox\r\n| p/Convision Vistabox security camera http config/ d/webcam/
match http m|^HTTP/1\.0 200 Document follows\r\nServer: ISOCOR web500gw ([\d.]+)\r\n| p/Eudora Worldmail http config/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 200 Reply from server\r\nServer: MERCUR Messaging 2005\r\n| p/Atrium's MERCUR Webmail httpd/ o/Windows/
match http m|^HTTP/1\.0 200 Document follows\r\nDate: .*\r\nServer: Proofpoint/([\d.]+)\r\n| p/Proofpoint email security http config/ v/$1/ d/security-misc/
match http m|^HTTP/1\.1 200 OK\r\nConnection: close\r\nCache-Control: no-cache\r\nContent-Type: text/html; charset=utf-8\r\n\r\n<html><head><title>IVM Answering Attendant</title>| p/IVM Answering Attendant httpd/ o/Windows/
match http m|^HTTP/1\.0 302 Found\r\nContent-Length: 0\r\nConnection: Close\r\nContent-Type: text/html\r\nLocation: /search\?site=[-\w_.]+&client=[-\w_.]+&| p/GoogleMini Search Appliance httpd/
match http m|^HTTP/1\.0 200 OK\r\n.*\n\n<title>Remote UI &lt;Top Page&gt; : iR2000 ;|s p/Canon imageRUNNER 2000 printer http config/ d/printer/
match http m|^HTTP/1\.0 200 OK\r\nX-Powered-By: PHP/([-\w_.]+)\r\n.*\n<title>(N\d+ - N\d+)</title>\n.*// Share Explorer\n|s p/Hammer $2 myshare http config/ i/PHP $1/ d/storage-misc/
match http m|^HTTP/1\.0 200 Ok\r\nServer: httpd\r\n.*<!--- Vendor:LINKSYS\nModelName:DD-WRT\n.*\nRF SSID:([^\r\n]+)\n|s p/DD-WRT milli_httpd/ i/Linksys WAP http config; SSID $1/ d/WAP/
match http m|^HTTP/1\.0 200 OK \r\n.*<title>: innovaphone (\w+)</title>|s p/Innovaphone $1 VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.0 200 OK \r\n.*<title>NAT: innovaphone (\w+)</title>|s p/Innovaphone $1 VoIP phone http config/ d/VoIP phone/
match http m|^<!DOCTYPE HTML PUBLIC \"-//IETF//DTD HTML 2\.0//EN\">\n<html><head>\n<title>400 Bad Request</title>\n</head><body>\n<h1>Bad Request</h1>\n<p>Your browser sent a request that this server could not understand\.<br />\nReason: You're speaking plain HTTP to an SSL-enabled server port\.<br />\n.*<address>Apache/([\w._-]+) (.*) Server at ([\w._*-]+) Port \d+</address>|s p/Apache httpd/ v/$1/ i/$2; SSL-only mode/ h/$3/
match http m|^<!DOCTYPE HTML PUBLIC \"-//IETF//DTD HTML 2\.0//EN\">\n<html><head>\n<title>400 Bad Request</title>\n</head><body>\n<h1>Bad Request</h1>\n<p>Your browser sent a request that this server could not understand\.<br />\nReason: You're speaking plain HTTP to an SSL-enabled server port\.| p/Apache httpd/ i/SSL-only mode/
match http m|^HTTP/1\.1 302 Moved Temporarily\r\nDate: .*\r\nExpires: Thu, 01 Jan 1970 00:00:00 GMT\r\nSet-Cookie: SSLX_SSESHID=\w+;Path=/;Secure\r\nLocation: https://[\d.]+/showHome\.do\r\n| p/SSL Explorer browser-based VPN httpd/ i/halfd Half-Life server management/
match http m|^HTTP/1\.1 302 Moved Temporarily\r\nDate: .*\r\nContent-Type: text/html\r\nExpires: .*\r\nSet-Cookie: SSLX_SSESHID=| p/SSL Explorer browser-based VPN httpd/
match http m|^HTTP/1\.1 302 Moved Temporarily\r\nDate: .*\r\nExpires: Thu, 01 Jan 1970 00:00:00 GMT\r\nSet-Cookie: SSLX_SSESHID=| p/SSL Explorer browser-based VPN httpd/
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"Gigabit Web Smart Switch\"\r\n\r\n| p/Justec gigabit ethernet switch http config/ d/switch/ i/micro_httpd/
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: Rex/([-\w_.]+)\r\nCache-Control: no-cache\r\nPragma: no-cache\r\nPragma: client-id=| p/Rex media encoder http config/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: alevtd/([\d.]+)\r\n| p/alevtd for videotext pages httpd/ v/$1/
match http m|^HTTP/1\.0 200 200 OK\r\nCache-control: max-age=300\r\nServer: Ubicom/([\d.]+)\r\n.*<title>Wireless Bridge : Login</title>|s i/Senao WAP http config/ d/WAP/ p/Ubicom httpd/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nDate: .*\r\nConnection: Close\r\nServer: Synchronet BBS for Win32  Version ([-\w_.]+)\r\n.*<h1 id=\"siteName\">([^<]+)</h1>|s p/Synchronet BBS httpd/ o/Windows/ v/$1/ i/BBS name $2/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: DCS-3220G\r\n|s p/D-Link DCS-3220G webcam http config/ d/webcam/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*\r\nServer: Slinger/([-\w_.]+)\r\n| p/Panasonic DVR slinger http config/ v/$1/ d/media device/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\nDate: .*Server: lighttpd/([\d.]+)\r\n\r\n\n<html>\n<head>\n<title>Shared Storage Manager</title>\n\n|s p/Western Digital My Book http config/ i/lighttpd $1/ d/storage-misc/ o/Linux/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: mini_httpd/([-\w_.]+)/astlinux (\w+)\r\nDate: .*\r\nCache-Control: no-cache,no-store\r\nWWW-Authenticate: Basic realm=\"\.\"\r\n| p/Pointca PBX http config/ i/mini_httpd $1; astlinux $2/ o/Linux/ d/PBX/
match http m|^HTTP/1\.1  200 OK\r\n.*<p:DeviceName>D-Link (DIR-[-\w_.+]+)</p:DeviceName>.*<p:FirmwareVersion>([^<]+)</p:FirmwareVersion>|s p/D-Link $1 WAP http config/ d/WAP/ i/FW $2/
match http m|^HTTP/1\.1 403 Forbidden\r\nDate: .*\r\nServer: RoamAbout Switch Manager Services ([^\r\n]+)\r\nContent-length: 0\r\n\r\n| p/Enterasys RoamAbout Switch Manager http config/ v/$1/
match http m|^HTTP/1\.1 200 .*Server: Virata-EmWeb/R([-\w_.]+)\r\n.*<title>NBX NetSet</title>\n<META NAME=\"robots\" CONTENT=\"noindex,noarchive,nofollow\">\n<!-- \(c\) Copyright, 3Com Corporation or its subsidiaries|s i/3Com NBX NetSet VoIP adapter http config/ d/VoIP adapter/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/
match http m|^HTTP/1\.1 200 .*Server: Virata-EmWeb/R([-\w_.]+)\r\n.*<title> HP Color LaserJet ([-\w_.]+)|s i/HP Color LaserJet http config/ d/printer/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/
match http m|^<!DOCTYPE HTML PUBLIC \"-//IETF//DTD HTML//EN\">\n<html>\n  <head>\n    <title>404 Entity Not Found</title>\n.*The requested file or stream was not found on this server\.|s p/Icecast streaming media server/
match http m|^HTTP/1\.0 403 too few slashes in URI /\r\nContent-[tT]ype: text/html\r\n\r\n| p|apt-cache/apt-proxy httpd| o/Linux/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: CosminexusComponentContainer\r\n|s p/Cosminexus httpd/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: GoAhead-Webs\r\n.*<!-- response_code_begin ERIC_RESPONSE_OK|s p|Supermicro IPMI/Paradox Alarm http config| d/remote management/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: text/html\r\n\r\n<html><head><title>GC-100 Network Adapter</title>| p/Global Cache GC-100 http config/ d/media device/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: JAGeX/([-\w_.]+)\r\n|s p/JAGeX Java gaming httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: \r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"BSkyB (\w+) \"\r\n| p/BSkyB $1 http config/ d/broadband router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: \r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"WBR-(\w+)\"\r\n| p/LevelOne WBR-$1 http config/ d/broadband router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: \r\n.*<meta name=\"description\" content=\"DG(\w+) \d+\">\n|s p/Netgear DG$1 http config/ d/broadband router/
match http m|^HTTP/1\.1 \d\d\d .*\r\nconnection: Keep-Alive\r\ncontent-length:.*<script src=\"all/kernel/public/lib/rc/js/system/currentVersion\.xjs\?command=WSTGetVersion\" type=\"text/javascript\"></script>|s p/Samsung SyncThru http config/ d/remote management/
# Samsung CLX-3175FW
match http m|^HTTP/1\.0 200 OK\r\n.*<title>SyncThru Web Service</title>\r\n\r\n<meta http-equiv=\"Content-Type\" content=\"text/html; charset=utf-8\">\r\n\r\n<script src=\"js/cookieCode\.js\"></script>\r\n\r\n<script language=\"JavaScript\" type=\"text/javascript\">\r\n\t<!--\r\n\t\t// GLOBAL VARIABLES\r\n\t\tvar wirelessEnabled \t= \(\"Installed\"\)\.toUpperCase\(\);\r\n\t\tvar fontDIMMInstalled\t= \(\"Invisible\"\)\.toUpperCase\(\);\r\n\t\tvar faxInstalled\t\t= \(\"Installed\"\)\.toUpperCase\(\);//GXI_FAX_INSTALL\r\n\t\tvar psInstalled\t\t\t= \(\"Invisible\"\)\.toUpperCase\(\);\r\n\t\tvar s2eInstalled \t\t= \(\"Installed\"\)\.toUpperCase\(\);\r\n\t\tvar s2fInstalled \t\t\t= \"Invisible\";\r\n\t\tvar s2sInstalled \t\t\t= \"Invisible\";\r\n\t\t\r\n\t\t// display additional page\r\n\t\tvar\tparallelPortOption\t= 0;\r\n\t\tvar\tusbPortOption\t\t= 300;\r\n\r\n\t\tvar COPYRIGHT = \t\t\t\"Copyrights &#169; 1995-2008 SAMSUNG\. All rights reserved|s p/Samsung CLX-3175FW printer http config/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*<title>LaCie EdMini NAS</title>|s p/Lacie BigDisk NAS http config/ d/storage-misc/
match http m|^HTTP/1\.1 200 OK\r\nServer: Virata-EmWeb/R([\d_]+)\r\n.*<title>HP Color LaserJet (\w+)|s p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ i/HP Color LaserJet $2 http config/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: BarracudaHTTP ([\d.]+)\r\n| p/BarracudaHTTP/ i/Barracuda Networks Load Balancer http config/ v/$1/ d/load balancer/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: BarracudaHTTP ([\d.]+)\r\n| p/BarracudaHTTP/ i/Barracuda Networks Spam & Virus Firewall 300 http config/ v/$1/ d/firewall/
match http m|^HTTP/1\.0 \d\d\d .*Server: WindWeb/([\d.]+)\r\n.*WWW-Authenticate: Basic realm=\"i\.LON\"\r\n|s p/i.LON 100e2 Internet Server http config/ i/WindWeb $1/ d/remote management/
match http m|^HTTP/1\.0 401 Authorization Required\r\nWWW-Authenticate: BASIC realm=\"Administrator or User\"\r\n\r\nPassword Error\. $| p/D-Link DCS-900 webcam http config/ d/webcam/
match http m|^HTTP/1\.1 \d\d\d .*Server: Yaws/([-\w_.]+) Yet Another Web Server\r\n.*Set-Cookie: SMSESSION=logout; .*Set-Cookie: nortelxnetid=logout;|s p/Nortel VPN Gateway http config/ i/YAWS httpd $1/ d/security-misc/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: SAP Internet Graphics Server\r\n|s p/SAP Internet Graphics Server httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\nserver: SAP Message Server, release (\d+)|s p/SAP Message Server httpd/ v/release $1/
match http m|^HTTP/1\.0 \d\d\d .*\r\n\r\n<html>\n<script language=JavaScript>\nfunction show\(\)\n{\n\tform1\.submit\(\);\n}\n</script>\n<body onload=\"show\(\);\">\n<form name=form1 action=\"/cgi-bin/webconfig\?page=first&action=check\">\n</form>\n</body>\n</html>\n|s p/D-Link DHP-540 VoIP Phone http config/ d/VoIP phone/
match http m|^HTTP/1\.0 200 OK\r\nServer: ScanAlert\r\n| p/ScanAlert Hacker Safe scanner httpd/ d/security-misc/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: ATR-HTTP-Server/([\d.]+)\r\nContent-Type: text/html\r\nWWW-Authenticate: Basic realm=\"Allied Telesyn AT-8748XL\"\r\n| p/Allied Telesyn AT-8748XL switch http config/ d/switch/ i/ATR httpd $1/
match http m|^HTTP/1\.0 \d\d\d .*WWW-Authenticate: Basic realm=\"Linksys WAP51AB\"\r\n|s p/Linksys WAP51AB http config/ d/WAP/
match http m|^HTTP/1\.1 \d\d\d .*Server: Virata-EmWeb/R([\d_]+)\r\nLocation: http://ns5gt/redirect\.html\r\n|s p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ i/Netscreen NS5GT firewall http config/ d/firewall/
match http m|^HTTP/1\.1 \d\d\d .*Server: Virata-EmWeb/R([\d_]+)\r\nLocation: http://[\d.]+/redirect\.html\r\n|s p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ i/Juniper SSG5 or SSG140 firewall http config/ d/firewall/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Allegro-Software-RomPager/([\d.]+)\r\n\r\n<HTML>\n<HEAD>\n<TITLE>Cisco Systems, Inc\.</TITLE>.*Cisco Systems, Inc\. IP Phone CP-7940G \(|s p/Cisco CP-7940G VoIP phone http config/ d/VoIP phone/ i/Allegro httpd $1/
match http m|^HTTP/1\.0 200 OK\r\nServer: SysMaster Web Server/([\d.]+)\r\nContent-Length: \d+\r\nConnection: close\r\nContent-type: text/html;\r\n\r\n<script>\nif\(document\.all\)\n\tlocation=\"app_ie\.htm\";\nelse\n\tlocation=\"app_mz\.htm\";\n</script>| i/Tornado M10 media center http config/ p/SysMaster httpd/ v/$1/ d/media device/
match http m|^HTTP/1\.0 401 Authorization Required\r\nWWW-Authenticate: Basic realm=\"Linksys-CIT400\"\r\n| p/Linksys CIT400 VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.0 200 OK\r\nAllow: GET, POST, OPTIONS\r\nServer: EDA HTTP LISTENER/([\d.]+)\r\n.*<form name=\"form\" action=\"webconsole\" method=\"POST\" >|s p/WebFOCUS httpd/ i/EDA httpd $1/
# Netgear WG302v1 or Linksys WRT54G v8
match http m|^HTTP/1\.0 301 Moved Premanently\r\nLocation: https://[\d.]+/\r\nContent-type: text/html\r\n\r\n<html><head><title>Access Denied</title></head><body><h1>You must use SSL based http\(HTTPS\) server\.</h1></body></html>$| p/Netgear or Linksys WAP http config/ d/WAP/
match http m|^HTTP/1\.0 301 Moved Permanently\r\nLocation: https:///\r\nContent-type: text/html\r\n\r\n<html><head><title>Access Denied</title></head><body><h1>You must use SSL based http\(HTTPS\) server\.</h1></body></html>$| p/ZyXEL ZyWALL SSL 10 SSL-VPN appliance http config/ d/firewall/
match http m|^HTTP/1\.0 200 OK\r\nServer: ARGUS/([\d.]+)\r\n.*\r\n<TITLE>Intel Wireless Gateway</TITLE>|s p/Intel Wireless Gateway http config/ d/WAP/ i/ARGUS httpd $1/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: \r\n.*WWW-Authenticate: Basic realm=\"Conceptronic C54APRA2\+\"\r\n\r\n|s p/Conceptronic C54APRA2+ WAP http config/ d/WAP/
match http m|^HTTP/1\.0 401 Unauthorized\n.*\r\nWWW-Authenticate: Basic realm=\"AirStation\"\r\n|s p/Buffalo AirStation http config/ d/WAP/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: Indy/([\d.]+)\r\n.*<img src=\"Webimages/RaidenMAILD\.jpg\" border=\"0\" id=\"raidenLogo\">|s i/RaidenMAIL http config/ p/Indy httpd/ v/$1/
match http m|^HTTP/1\.1 200 Document follows\r\nServer: ELOG HTTP ([-\w_.]+)\r\n| p/ELOG blog httpd/ v/$1/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Digest realm=\"iRMC@.*<title>RemoteView&reg; iRMC Web Server</title>|s p/iRMC RemoteView httpd/ d/remote management/
match http m|^HTTP/1\.1 \d\d\d .*:: Welcome to ZyXEL (P-\w+) \(([-\w_.]+)\) ::\.|s p/ZyXEL $1 broadband router http config/ d/broadband router/ h/$2/
match http m|^HTTP/1\.1 200 OK\r\nServer: Web Server\r\n.*<title>Dell OpenManage Switch Administrator</title>|s p/Dell OpenManage switch http config/ d/switch/
match http m|^HTTP/1\.0 \d\d\d .*<SCRIPT language=JavaScript>\r\n\tvar PIN_change_attempted = false;\r\n\tvar Login_failed = false;\r\n\tvar password_label = \"\";\r\n</SCRIPT>\r\n<!--\r\nNote: the opening and closing HTML tags are deliberately omitted from\r\nthis file\.|s p/Citrix Access Gateway httpd/ o/Windows/
match http m|^HTTP/1\.1 200 OK\r\nServer: Micro Focus DSD ([-\w_.]+)\r\n| p/Micro Focus Directory Server httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\nServer: SCO I2O Dialogue Daemon ([-\w_.]+) \n|s p/SCO I2O Dialogue Daemon httpd/ v/$1/
match http m|^HTTP/1\.1 404 OK\r\nServer: Lotus Expeditor Web Container/([-\w_.]+)\r\n| p/Lotus Notes Expeditor httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Cpanel::Httpd like Apache\r\n.*\r\nWWW-Authenticate: Basic realm=\"cPanel WebDisk\"\r\n\r\n|s p/cPanel WebDisk httpd/ o/Linux/

match http m|^HTTP/1\.0 302 FOUND\r\nServer: PasteWSGIServer/([-\w_.]+) Python/([-\w_.]+)\r\nDate: .*location: /login/login\r\npragma: no-cache\r\ncache-control: no-cache\r\nset-cookie:  hellahella=|s p/PasteWSGIServer/ v/$1/ i/HellaHella httpd; Python $2/
match http m|^HTTP/1\.0 200 OK\r\nServer: PasteWSGIServer/([-\w_.]+) Python/([-\w_.]+)\r\n.*<title>Welcome to Pylons!</title>|s p/PasteWSGIServer/ v/$1/ i/Pylons web framework; Python $2/
match http m|^HTTP/1\.0 200 OK\r\nServer: PasteWSGIServer/([-\w_.]+) Python/([-\w_.]+)\r\n.*<div id=\"loggerheadCont\">|s p/PasteWSGIServer/ v/$1/ i/Bazaar loggerhead httpd; Python $2/

match http m|^HTTP/1\.1 200 OK\r\n.*Server: NessusWWW\r\n.*Content-Length: 5955\r\n.*ETag: \"e6f27b4d0bc325a6ddf5125b5f86e585\"\r\n.*<!-- saved from url=\(0016\)http://localhost -->\n<html lang=\"en\">\n\n<!-- \nSmart developers always View Source\. \n\nThis application was built using Adobe Flex.*<title>Nessus</title>|s p/NessusWWW/ i/Nessus vulnerability scanner http UI/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: NessusWWW\r\n.*Content-Length: 6518\r\n.*ETag: \"186071cd1807c2c4b2d058d0aad65e63\"\r\n.*<!-- saved from url=\(0016\)http://localhost -->\n<html lang=\"en\">\n\n<!-- \nSmart developers always View Source\. \n\nThis application was built using Adobe Flex.*<title>Nessus</title>|s p/NessusWWW/ i/Nessus vulnerability scanner http UI/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: NessusWWW\r\n.*Content-Length: 6518\r\n.*<!-- saved from url=\(0016\)http://localhost -->\n<html lang=\"en\">\n\n<!-- \nSmart developers always View Source\. \n\nThis application was built using Adobe Flex.*<title>Nessus</title>|s p/NessusWWW/ i/Nessus vulnerability scanner http UI/ v/4.2.2 - 4.49RC1/

# CAMEO-httpd
match http m=^HTTP/1\.0 200 Ok\r\nServer: CAMEO-httpd\r\n.*<title>D-LINK CORPORATION \| WIRELESS AP \| LOGIN</title>=s i/D-Link DAP-1150 WAP http config/ d/WAP/ p/CAMEO httpd/
match http m=^HTTP/1\.0 200 Ok\r\nServer: CAMEO-httpd\r\n.*\n<title>D-LINK SYSTEMS, INC \| WIRELESS AP \| LOGIN</title>=s i/D-Link DAP-1160 WAP http config/ d/WAP/ p/CAMEO httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: CAMEO-httpd\r\n.*WWW-Authenticate: Basic realm=\"DWL-G700AP Login\"\r\n|s i/D-Link DWL-G700AP http config/ d/WAP/ p/CAMEO httpd/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: CAMEO-httpd\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"802\.11g WLAN Login\"\r\n| i/TRENDnet WAP http config/ p/CAMEO httpd/ d/WAP/


match http m|^HTTP/1\.0 302 Object Moved\r\nServer: Cisco AWARE ([-\w_.]+)\r\n| p/Cisco ASA firewall http config/ d/firewall/ i/Cisco AWARE $1/ o/IOS/
match http m|^HTTP/1\.0 200 OK\r\n.*<title>Remote Buddy by IOSPIRIT</title>|s p/IOSPIRIT Remote Buddy http config/ o/Mac OS X/
match http m|^HTTP/1\.1 302 Moved Temporarily\r\nServer: Asterisk/[\w_]+-([-\w_.]+) \(| p/Asterisk http config/ v/$1/
match http m|^HTTP/1\.1 501 Not Implemented\r\nCIMError: Only POST and M-POST are implemented\r\n\r\n$| p/OpenPegasus CIMServer/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*\r\nServer: \r\n.*ACTION=\"/cgi-bin/cgi_authenticate\">\n<P ALIGN=\"left\"><B><FONT SIZE=\"5\" face=\"Tahoma\">User Firewall Authentication|s p/WatchGuard Firebox http config/ d/firewall/
match http m|^HTTP/1\.1 200 OK\r\n.*<TITLE>Divar Web Client</TITLE>|s p/Bosch Divar Security Systems http config/ d/security-misc/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: ISOS/([-\w_.]+) UPnP/([\d.]+) Conexant-EmWeb/R([\d_]+)\r\n| p/Conexant-EmWeb/ v/$SUBST(3,"_",".")/ i/ISOS $1; UPnP $2/ d/broadband router/
match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/([-\w_.]+)\r\nMIME-version: 1\.0\r\nPragma: no-cache\r\nContent-type: text/html\r\n\r\n<script language=\"javascript\">\n<!--\ntop\.location\.href=\"duplicate\.htm\";//-->\n</script>\n\r\n$| p/3Com OfficeConnect WAP http config/ d/WAP/
match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/([\w._-]+)\r\nMIME-version: 1\.0\r\n.*<title>802\.11g AP setup page</title>.*function doLogin\(\)\n{\nvar f=document\.submit_form ;\t\nf\.submit_login_password\.value;|s p/3Com OfficeConnect WAP http config/ i/RapidLogic httpd $1/ d/WAP/
match http m|^HTTP/1\.0 200 Ok\rServer: httpd\r.*\t\r\r<TITLE>3Com - OfficeConnect Wireless Cable/DSL Router</TITLE>|s p/3Com OfficeConnect WAP http config/ d/WAP/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: text/html\n\n<html>\n<head>\n<meta name=\"description\" content=\"Belkin ([-\w_.+]+)\">\n| p/Belkin $1 WAP http config/ d/WAP/
match http m|^HTTP/1\.0 200 OK\r\nCache-control: no-cache\r\nServer: Ubicom/([\w._-]+)\r\n.*<title>D-Link Print Server - Server Information</title>|s i/D-Link print server http config/ d/print server/ p/Ubicom httpd/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nCache-control: no-cache\r\nServer: Ubicom/([\w._-]+)\r\n.*href=\"/substyle_DIR-(6\d+)\.css\"|s i/D-Link DIR-$2 WAP http config/ d/WAP/ p/Ubicom httpd/ v/$1/
match http m|^HTTP/1\.0 200 200 OK\r\nServer: Ubicom/([\w._-]+)\r\n.*<!--@TEMPLATE:build/cooker/webgen/cooker_nonav_template\.html@-->|s i/D-Link DIR-625 WAP http config/ d/WAP/ p/Ubicom httpd/ v/$1/
match http m|^HTTP/1\.0 200 200 .*\r\nServer: Ubicom/([\w._-]+)\r\n.*<link rel=\"stylesheet\" rev=\"stylesheet\" href=\"/substyle_DIR-625\.css\"|s i/D-Link DIR-625 WAP http config/ d/WAP/ p/Ubicom httpd/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*\r\nServer: ActiveGrid/([-\w_.]+)\r\n| p/ActiveGrid httpd/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nServer: ISS-HttpMod/([-\w_.]+)\r\n| p/Intelligent Security Systems webcam httpd/ d/webcam/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nDate: .*\r\nServer: Hiawatha v([-\w_.]+)\r\n| p/Hiawatha httpd/ v/$1/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: \r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"Linksys RVS4000\n \"| p/Linksys RVS4000 security router http config/ d/broadband router/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*\r\nServer: httpdevil/([-\w_.]+)\r\n| p/httpdevil/
match http m|^HTTP/1\.0 200 OK\r\nServer: ADSM_HTTP/([-\w_.]+)\r\nContent-type: text/html\n\n<HEAD>\n<TITLE>\nServer Administration\n</TITLE>.*<META NAME=\"IBMproductVersion\" CONTENT=\"([\d.]+)\">|s p/IBM AIX Storage Management http config/ d/storage-misc/ o/AIX/ v/$1/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: Conexant-EmWeb/R([\d_]+)\r\n.*WWW-Authenticate: Basic realm=\"Connecting to router\".*\(C\) Copyright \w+ Allied Telesis|s i/Allied Telesis broadband router http config/ p/Conexant-EmWeb/ v/$SUBST(1,"_",".")/ d/broadband router/
match http m|^HTTP/1\.[01] \d\d\d .*\nServer: TIB/Rendezvous ([-\w_.]+)\n|s p/TIB Rendezvous http config/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Snug/([-\w_.]+)\r\n|s p/Snug httpd/ o/Windows/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: NetPort Software ([\d.]+)\r\n.*\n<title>([-\w_.]+) - VSX 8000</title>|s p/Polycom VSX 8000 http config/ d/webcam/ i/NetPort httpd $1/ h/$2/
match http m|^HTTP/1\.0 \d\d\d .*Server: Grandstream GXP2000 ([-\w_.]+)\r\n\r\n|s p/Grandstream GXP2000 http config/ d/VoIP adapter/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: D-Link Internet Camera\r\n.*<title>(DCS-\w+)</title>|s p/D-Link $1 webcam http config/ d/webcam/
match http m|^HTTP/1\.0 200 Ok\r\nServer: micro_httpd\r\n.*var isRouter\t='1' \? '1' : '0';\r\nvar\tisPS\t\t='' \? '' : '0';\r\nvar isAPmode\r\nif\('vlan1' =='' .. '1'=='0'\)\r\n\tisAPmode='1';\r\nelse\tisAPmode='0';\r\nvar bssid = '([\w:]+)';|s p/Belkin WAP http config/ d/WAP/ i/micro_httpd; BSSID $1/
match http m|^HTTP/1\.0 200 OK\n.*Server: SWILL/([-\w_.]+)\n|s p/SWILL httpd/ v/$1/
match http m|^HTTP/1\.1 .*<p:Type>GatewayWithWiFi</p:Type><p:DeviceName>D-Link DGL-4300</p:DeviceName>|s p/D-Link DGL-4300 WAP http config/ d/WAP/
match http m|^HTTP/1\.1 200 OK.*\r\nServer: IPL T S2/([-\w_.]+)\r\n|s p/Exton IPL T S2 http config/ d/media device/ v/$1/
match http m|^HTTP/1\.0 200 Ok\r\nServer: \r\n.*<title>RWO-CPE-PLUS-G Login Page</title>|s p/Demarc RWO WAP http config/ d/WAP/ i/mini_httpd/
match http m|^HTTP/1\.1 200 OK.*\r\nServer: Web Server\r\n.*<TITLE>Netgear System Login</TITLE>.*<IMG SRC = \"/base/images/Netgear_fsm(\w+)_banner\.gif\"|s p/Netgear FSM$1 switch http config/ d/switch/
match http m|^HTTP/1\.1 200 OK.*\r\nServer: Web Server\r\n.*<TITLE>NetGear FSM7352S</TITLE>|s p/Netgear FSM7352S switch http config/ d/switch/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: FM Web Publishing\r\n|s p/FileMaker Web Publishing httpd/
match http m|^HTTP/1\.1 \d\d\d Snakelet output follows\r\nServer: Snakelets/([-\w_.]+) Python/([-\w_.]+)\r\n| p/Snakelets httpd/ i/Python $2/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: PRINT_SERVER WEB ([\d.]+)\r\nContent-type: text/html\r\nWWW-Authenticate: Basic realm=\"NETGEAR PS121v2\"\r\n| p/Netgear PS121v2 print server http config/ d/print server/ i/PRINT_SERVER WEB httpd $1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDocuCentre Color (\d+) -|s p/Fuji Xerox DocuCentre Color $1 http config/ d/printer/
match http m|^HTTP/1\.1 \d\d\d .*Fuji Xerox Co\..*\r\n<TITLE>B6300 -|s p/Fuji Xerox B6300 printer http config/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*Server: Boa/([-\w_.]+) \(with Intersil Extensions\)\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"CONNECT2AIR AP-600RP-USB LOGIN Enter Password \(default is connect\)\"\r\n|s p/Fujitsu Siemens CONNECT2AIR AP-600RP-USB WAP http config/ d/WAP/ i/Boa httpd $1; default passwd "connect"/
match http m|^HTTP/1\.1 200 OK\r\nConnection: close\r\nServer: NetworkScanner WebServer Ver([\d.]+)\r\nCache-Control: no-cache\r\nContent-Type: TEXT/HTML\r\n\r\n<HTML>\r\n<HEAD>\r\n<TITLE>NS-30G</TITLE>| p/Kyocera NS-30G printer http config/ d/printer/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\n.*<title>Colloquy</title>|s p/Colloquy IRC web gateway/ o/Mac OS X/
match http m|^HTTP/1\.1 \d\d\d .*content=\"VMware Server is virtual infrastructure software.*\n\n<title>VMware Server ([-\w_.]+)</title>|s p/VMware Server http config/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Allegro-Software-RomPager/([-\w_.]+)\r\n.*<font color=\"#FFFFFF\" size=\"4\">Cisco Systems, Inc\. IP Phone CP-7960 \(|s p/Cisco CP-7960 VoIP phone http config/ d/VoIP phone/ i/Allegro RomPager httpd $1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: InterMapper/([-\w_.]+)\r\n|s p/Dartware InterMapper httpd/ v/$1/
match http m|^HTTP/1\.0 401 Authenticate\nWWW-Authenticate: Basic realm=\"P4Web\"\n| p/Perforce P4Web httpd/
match http m|^HTTP/1\.1 200\r\n.*<!--SELECTserver Full Page Header-->\r\n<html>\r\n\r\n<head>\r\n<title>\r\nSELECTserver: License Manager\r\n</title>|s p/SELECTserver license manager httpd/
match http m|^HTTP/1\.0 200 Document follows\r\nDate: .*\r\nServer: WebminServer\r\n| p/WebminServer httpd/
match http m|^HTTP/1\.1 200 OK.*\* Zimbra Collaboration Suite Web Client\n|s p/Zimbra http config/
match http m|^HTTP/1\.1 302 Found\r\n.*\r\nLocation: https://[\d.:]+/zimbraAdmin\r\n|s p/Zimbra admin http config/
match http m|^HTTP/1\.1 \d\d\d .*\r\nWWW-Authenticate: Basic realm=\"CANOPY ([-\w]+)\"\r\n|s p/Motorola Canopy WAP http config/ d/WAP/ i/MAC $1/
match http m|^HTTP/1\.0 200 Document follows\nMIME-Version: 1\.0\nServer: Java Cell Server\n.*<title>dCache service</title>|s p/dCache httpd/ i/Distributed Storage Node/ d/storage-misc/
match http m|^HTTP/1\.0 200 OK\r\nDate:.*\r\nServer: HighPoint Raidman WebServer/([-.\w\d]+)\r\nAccept-Ranges: bytes\r\n| p/HighPoint Raidman web config http/ v/$1/ d/storage-misc/
match http m|^HTTP/1\.1 404 Not Found\r\nconnection: close\r\ncontent-type: text/html\r\ndate: .*\r\nserver: Ruckus/([.\d]+)\r\n\r\n| p/Ruckus Media Player/ v/$1/ o/Windows/
#Novell Groupwise HTTP services
match http m|^HTTP/1\.0 \d\d\d .*\r\n(?:Date: .*\r\n)?Server: GroupWise MTA ([-_.\d\w\(\) ]+)\r\n| p/Novell GroupWise MTA httpd/ v/$1/ o/Unix/
match http m|^HTTP/1\.0 \d\d\d .*\r\n(?:Date: .*\r\n)?Server: GroupWise POA ([-_.\d\w\(\) ]+)\r\n| p/Novell GroupWise POA httpd/ v/$1/ i/Post Office Agent/ o/Unix/
match http m|^HTTP/1\.0 \d\d\d .*\r\n(?:Date: .*\r\n)?Server: GroupWise GWIA ([-_.\d\w\(\) ]+)\r\n| p/Novell GroupWise GWIA httpd/ v/$1/ i/GroupWise Internet Agent/ o/Unix/
match http m|^HTTP/1\.0 \d\d\d .*\r\n(?:Date: .*\r\n)?Server: Messenger-MA ([-_.\d\w\(\) ]+)\r\n| p/Novell Messenger httpd/ v/$1/ i/Messenger Agent/ o/Unix/
match http m|^HTTP/1\.0 200 .*\r\nDate: .*\r\nContent-Length: .*\r\nContent-Type: .*\r\n\r\n<html>\r\n<head>\r\n<title>Novell Messenger Download</title>| p/Novell Messenger download httpd/ o/Unix/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Hunchentoot ([\w._-]+)\r\n|s p/Hunchentoot httpd/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: AllegroServe/([\w._-]+)\r\n|s p/Franz Allegroserve httpd/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Hop\r\n|s p/HOP httpd/
match http m|^HTTP/1\.1 200 OK\r\nServer: minituner\r\n| p|BMC/Marimba Management http config|
match http m|^HTTP/1\.1 200 Channel Listing\r\nServer: Marimba-Transmitter/([.\d]+)\r\n| p|BMC/Marimba Transmitter| v/$1/
match http m|^HTTP/1\.0 500 Internal Server Error\r\nContent-type: text/html; charset=UTF-8\r\n\r\n<html><META HTTP-EQUIV=\"Content-Type\" CONTENT=\"text/html; charset=UTF-8\"><body>\r\nInternal Server Error</body>\r\n</html>\r\n| p|BMC/Marimba Management http config| i|Error Condition|
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"tuner\"\r\n| p|BMC/Marimba Management http config|
match http m|^HTTP/1\.0 200 OK\r\nServer: Henry/\d\.\d\r\n|s p/NEC Electra Elite IPK II WebPro/
match http m|^HTTP/1\.0 200 OK\r\n.*\r\nServer: WebZerver/V([\w._-]+)\r\n.*<title>\nAxonix\nSuperCD - cdserver\n  </title>|s p/Axonix SuperCD http config/ i/WebZerver $1/ d/media device/
match http m|^HTTP/1\.0 200 OK\r\nDate: .*\r\nMIME-version: 1\.0\r\nServer: ZOT-PS-19/([\w._-]+)\r\n.*<title>Index</title>|s p/IOGear GPSU01 print server http config/ d/print server/ i/ZOT-PS-19 $1/
match http m|^<html>\n<title>DES-2108 +</title>| p/D-Link DES-2108 switch http config/ d/switch/
match http m|^HTTP/1\.1 \d\d\d .*<title>MD Evol Web</title>|s p/Ericsson MD Evolution PBX http config/ d/PBX/
match http m|^HTTP/1\.0 200 OK\r\nServer: NetPort Software ([\w._-]+)\r\nDate: .*\r\nContent-type: text/html\r\n\r\n<html>\r\n<head>\r\n<title>On Board Remote Management</title>| p/Dell PowerVault 124T http config/ i/NetPort httpd $1/ d/storage-misc/
match http m|^HTTP/1\.0 200 OK\nContent-type: text/html\nServer: AV-TECH (AV\w+) Video Web Server\n| p|Gadspot/AV-TECH $1 webcam http config| d/webcam/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Minix httpd ([\w._-]+)\r\n| p/Minix httpd/ v/$1/ o/Minix/
match http m|^HTTP/1\.1 200 Ok\r\nServer: micro_httpd\r\n.*<title>ADSL Router</title>\r\n\r\n\r\n<script language=\"javascript\">\r\n<!--\r\nvar ModemVer='(DSL-[\w._+-]+)';|s p/D-Link $1 http config/ d/broadband router/
match http m|^HTTP/1\.0 200 OK\r\n.*<TITLE>HTML-Konfiguration</TITLE>\n<SCRIPT language=\"JavaScript\" src=\"/cgi-bin/webcm\?getpage=\.\./html/js_top\.txt\"|s p/T-Com Speedport W 501V http config/ i/German/ d/broadband router/
match http m|^HTTP/1\.0 200 OK\r\n.*Mime-Version: 1\.0\r\n.*<TITLE>HTML-Konfiguration</TITLE>\n<SCRIPT type=\"text/javascript\" src=\"/html/dom\.js\">|s p/T-Com Speedport W 101V http config/ i/German/ d/WAP/
match http m|^HTTP/1\.0 200 OK\r\nServer: Apache\r\n.*<TITLE>HTML-Konfiguration</TITLE>.*prodname=\"Speedport_W_(\w+)_Typ_B\";|s p/T-Com Speedport W $1 http config/ i/German/ d/broadband router/
match http m|^HTTP/1\.0 200 OK\r\nServer: Apache\r\n.*<title>HTML-Konfiguration</title>.*<style type=\"text/css\">\r\n#startseite|s p/T-Com Speedport W 700 http config/ i/German/ d/broadband router/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\nCache-Control: must-revalidate, no-store\r\nConnection: close\r\n\r\n<html>\n<style>\ntable\.stat th, table\.stat td {\n  font-family:\tVerdana, Geneva, sans-serif;\n  font-size : 11px;\n  color: blue;\n  border: 0px solid;\n  white-space: nowrap;\n}\n| p/Linksys SPA942 VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.1 200 OK\r\nMIME-Version: 1\.0\r\nServer: OKIDATA-HTTPD/([\w._-]+)\r\n.*<title>([^<]+)</title>|s p/Oki $2 printer http config/ d/printer/ i/OKIDATA httpd $1/
match http m|^HTTP/1\.0 200 OK\r\nServer: NetPort Software ([\w._-]+)\r\n.*<title>([^-<\r\n]+) - VSX 8000</title>\n<link rel=\"stylesheet\" href=\"sabrestyle\.css\"|s p/Polycom VSX 8000 http config/ d/webcam/ i/$2; NetPort httpd $1/
match http m|^HTTP/1\.0 200 OK\r\nServer: NetPort Software ([\w._-]+)\r\n.*<meta http-equiv=\"Content-Type\" content=\"text/html; charset=utf-8\">\n    <meta http-equiv=\"no-cache\">\n    <link rel=\"stylesheet\" href=\"sabre\.css\"|s p/Polycom VSX 8000 http config/ d/webcam/ i/NetPort httpd $1/
match http m|^HTTP/1\.0 303 Redirecting\r\nServer: httpd/[\d.]+ Python/([\d.]+)\r\n.*Cache-Control: no-store,no-cache,must-revalidate,max-age=0,post-check=0,pre-check=0\r\n.*<title>: Redirecting\n</title>\n<meta http-equiv=\"Refresh\" content=\"0; URL=http://([\w._-]+):\d+/login\"|s p/IronPort Mailflow http config/ d/specialized/ i/Python $1/ h/$2/
match http m|^<html><head><title>Task Manager Server Report</title></head>| p/Dolbey Fusion Focus Task Manager httpd/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: XGATE-Webs\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"NB(\w+) Wireless Router\"\r\n| p/NetComm NB$1 WAP http config/ d/WAP/ i/XGATE-Webs/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: XGATE-Webs\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"XG6546p2 Wireless Router\"\r\n| p/XAVi XG6546p Wireless Gateway/ d/WAP/ i/XGATE-Webs/
match http m%^HTTP/1\.0 200 Ok\r\nServer: micro_httpd\r\n.*\r\nvar isRouter\t='1' \? '1' : '0';\r\nvar\tisPS\t\t='' \? '' : '0';\r\nvar isAPmode\r\nif\('[\w-]*' =='' \|\| '1'=='0'\)\r\n\tisAPmode='1';\r\nelse\tisAPmode='0';\r\nvar bssid = '([\w:]+)';%s p/Belkin WAP http config/ d/WAP/ i/micro_httpd; BSSID $1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nConnection: Close\r\nDate: .*\r\nServer: Eye-Fi Agent/([\w._-]+) \(Windows| p/Eye-Fi Manager httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: micro_httpd\r\nCache-Control: no-cache\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"U\.S\. Robotics ADSL Gateway\"\r\n| p/USRobotics ADSL router http config/ d/broadband router/ i/micro_httpd/
match http m|^HTTP/1\.0 401 Unauthorized\n.*\r\nWWW-Authenticate: Basic realm=\"3Com AirProtect Sentry\"\r\n|s p/3Com AirProtect Sentry http config/ d/security-misc/
match http m|^HTTP/1\.1 200 OK\r\nServer: WindWeb/([\w._-]+)\r\n.*<SCRIPT LANGUAGE=\"JavaScript\">\r\n<!--\r\n  function change_Time\(\) {\r\n    window\.location = '\./cgi/mts_login\.cgi'\r\n|s p/Iwatsu ADIX PBX http config/ d/PBX/ i/WindWeb httpd $1/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\nServer: WindWeb/([\w._-]+)\r\n.*<title>TrueTime - NTS-200 Web Interface -|s p/TrueTime NTS-200 http config/ d/specialized/ i/WindWeb httpd $1/
match http m|^HTTP/1\.1 302 Found\r\nConnection: Keep-Alive\r\nServer: \r\n.*<!-- this page must have 520 bytes or more, ie is a wonderfull program -->.*<html>\r\n<head>\r\n<title>302-Found</title>\r\n<meta http-equiv=\"Content-Type\" content=\"text/html; charset=utf-8\">\r\n</head>\r\n<body>\r\n<h1>302-Found</h1>\r\n<a href='/login\.html\?id=\d+'>/login\.html</a>|s p|Siemens Gigaset PBX/TARGA DIP VoIP phone http config|
match http m|^HTTP/1\.1 302 Found\r\nConnection: Close\r\nServer: \r\n.*<!-- this page must have 520 bytes or more, ie is a wonderfull program -->.*<html>\r\n<head>\r\n<title>302-Found</title>\r\n<meta http-equiv=\"Content-Type\" content=\"text/html; charset=utf-8\">\r\n</head>\r\n<body>\r\n<h1>302-Found</h1>\r\n<a href='/login\.html\?id=\d+'>/login\.html</a>|s p/Siemens Gigaset A580 or S450 VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.0 200 OK\r\nServer: SimpleHTTP/([\d.]+) Python/([\d.]+)\r\n.*<HTML>\n<TITLE>WifiZoo v([\w._-]+) - Control Panel</TITLE>|s p/WifiZoo http control panel/ i/SimpleHTTP $1; Python $2/ v/$3/
match http m|^HTTP/1\.1 200 OK\r\n.*\n\n\t\t<title>PGP Universal - Page Not Found</title>\n|s p/PGP Universal httpd/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nDate: .*\r\nServer: PWS/([\w._-]+)\r\n| p/PWS httpd/ v/$1/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: micro_httpd\r\nCache-Control: no-cache\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"Wireless ADSL2\+ Router\"\r\n| p/Dynalink RTA1025W WAP http config/ d/WAP/ i/micro_httpd/
match http m|^HTTP/1\.1 401 \r\nServer: GoAhead-Webs\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"AirMagnet SmartEdge Sensor\"\r\n| p/AirMagnet SmartEdge Sensor http config/ d/specialized/ i/GoAhead httpd/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: http\r\n.*\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"Login to Vigor 3300\"\r\n\r\n|s p/DrayTek Vigor 3300 router http config/ d/router/
match http m|^HTTP/1\.0 200 OK\r\n.*<link rel=\"stylesheet\" type=\"text/css\" href=\"/musicpal_ie6\.css\" />\r\n<!\[endif\]-->\r\n<title>Freecom MusicPal</title>|s p/Freedom MusicPal/ d/media device/
match http m|^HTTP/1\.1 200 Document follows\r\nConnection: Close\r\nServer: Micro-Web\r\n.*<title>Oasis Semiconductor, Inc\.</title>.*<b>Welcome to a live demo of the TCP/IP network stack running Micro-Web!</b>.*\r\nSystem Up Time:  ([^\r\n<]+)\r\n.*\r\nMAC Address:\r\n([\w:]+)\r\n|s p/Oasis Micro-Web http demo/ i/Uptime $1; MAC $2/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\n\r\n<html><head><title>VDR Channel Listing</title>| p/VDR Streamdev plugin httpd/ d/media device/
match http m|^HTTP/1\.1 200 .*\r\nServer: Agranat-EmWeb/R([\d_]+)\r\n.*<SCRIPT LANGUAGE=JavaScript>\nvar helpUrl = \"\";\n//Ip we are coming from\nvar ip=document\.domain;\n\n|s i/Avaya G350 Media Gateway http config/ d/media device/ p/Agranat-EmWeb/ v/$SUBST(1,"_",".")/
match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/([\w._-]+)\r\nMIME-version: [\d.]+\r\n.*md5\(document\.logonForm\.username\.value \+ \":\" \+ document\.logonForm\.password\.value \+ \":\" \+ \"\w+\"\);  // sets the hidden field value to whatever md5 returns\.\r\n|s i/Thomson ST2030 VoIP phone http config/ d/VoIP phone/ p/RapidLogic/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nDate: .*\r\nServer: BCReport/([\w._-]+)\r\n| p/Blue Coat Reporter httpd/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: Blue Coat Reporter\r\n.*<title>Blue Coat Reporter ([\d.]+)</title>|s p/Blue Coat Reporter httpd/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nDate: .*\r\nX-Powered-By: ASP\.NET\r\n| p/Microsoft IIS httpd/ o/Windows/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<!---CAS:\d+--><HTML><HEAD><TITLE>U\.S\. Robotics Broadband Router Configuration</TITLE>| p/USRobotics ADSL router http config/ d/broadband router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: WYM/([\w._-]+)\r\n.*<META NAME=\"Author\" CONTENT=\"ChenXiaohui\">\r\n<meta http-equiv='Relfresh' content='5' />|s i/Gadspot NC1000-L10 webcam http config/ d/webcam/ p/WYM httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: WYM/([\w._-]+)\r\n.*<TITLE>Video Server \(V([\w._-]+)\)</TITLE>\n<META NAME=\"Author\" CONTENT=\"ChenXiaohui\">\n<!-- Get Server or DVR-->|s i/Gadspot Video Server $2 httpd/ d/media device/ p/WYM httpd/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\n\r\n<HTML>\r\n<HEAD>\r\n<TITLE>TallyGenicom Intelliprint (\w+)</TITLE>\r\n| p/TallyGenicom Intelliprint $1 http config/ d/printer/
match http m|^HTTP/1\.0 \d\d\d .*\r\n<META HTTP-EQUIV=\"Content-Style-Type\" content=\"text/css\">\r\n<TITLE>[^\r\n<]+ WJ-HD220 [^\r\n<]+</TITLE>|s p/Panasonic WJ-HD220 http config/ d/media device/
match http m|^HTTP/1\.1 \d\d\d .*<title>([\w-]+) Network Camera</title>|s p/Panasonic $1 webcam http config/ d/webcam/
match http m|^HTTP/1\.0 200 OK\r\n.*<TITLE>Network Camera</TITLE>.*<META HTTP-EQUIV=\"Refresh\" CONTENT=\"1;URL=CgiStart\">|s p/Panasonic BB-HCM331 Network Camera http config/ d/webcam/
match http m|^HTTP/1\.1 302 Object Moved\r\nServer: NS_([\w._-]+)\r\nLocation: http://([\w._-]+)/wts\r\n| p/Windows Terminal Server httpd/ i/NS httpd $1/ o/Windows/ h/$2/
match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/([\w._-]+)\r\n.*<TITLE>ProLine</TITLE>.*setTimeout\( \"window\.location\.href = 'homeSumBS\.htm'\", 100 \) ;   // 0\.1 second delay\r\n</script>|s p/ProLine ADSL router http config/ d/broadband router/ i/RapidLogic httpd $1/
match http m|^<HTML><HEAD><TITLE>Error</TITLE></HEAD><BODY><H1>Error</H1>Bad request or resource not found\.</BODY></HTML>\0$| p/Panasonic DP-1820E printer http config/ d/printer/
match http m|^HTTP/1\.0 200 OK\r\nServer: Contiki/([\w._-]+) http://www\.sics\.se/~adam/contiki/\r\n| p/Contiki httpd/ v/$1/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: GoAhead-Webs\r\n.*WWW-Authenticate: Basic realm=\"Wireless Router \(username: admin\)\"\r\n.*<body background=/menu-images/config_bg\.gif>|s p/ZyXEL P-330W WAP http config/ i/GoAhead httpd/ d/WAP/
match http m|^HTTP/1\.1 200 OK\r\nServer: InterNiche Technologies WebServer ([\w._-]+)\r\n.*<title>Welcome to Canopy</title>\r\n</head>\r\n\r\n<body>\r\n<p>\r\nPress <a href=\"http:index\.htm\?mac_esn=(\w+)\">Here</a>|s p/Motorola Canopy WAP http config/ d/WAP/ i/Interniche httpd $1; MAC $2/
match http m|^HTTP/1\.1 200 OK\r\nCache-Control: no-cache\r\nConnection: close\r\nContent-Type: text/html\r\n.*<title>Canopy Home Page</title>\r\n.*<frame name=\"leftFrame\" noresize src=\"smleft\.html\">\r\n|s p/Motorola Canopy WAP http config/ d/WAP/
match http m|^HTTP/1\.1 200 Ok\r\nServer: micro_httpd\r\n.*cfeVersion = '1\.0\.37-0\.7';\nif \(cfeVersion\.charAt\(9\) == '7'\)\n   document\.writeln\(\"<title>Tecom AH4222</title>\"\);\nelse\n   document\.writeln\(\"<title>Tecom AH4021</title>|s p/Tecom AH4222 router http config/ d/broadband router/ i/micro_httpd/
match http m|^HTTP/1\.1 200 Ok\r\nServer: micro_httpd\r\n.*cfeVersion = '1\.0\.37-0\..';\nif \(cfeVersion\.charAt\(9\) == '7'\)\n   document\.writeln\(\"<title>Tecom AH4222</title>\"\);\nelse\n   document\.writeln\(\"<title>Tecom AH4021</title>|s p/Tecom AH4021 router http config/ d/broadband router/ i/micro_httpd/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: \r\n.*WWW-Authenticate: Basic realm=\"Please enter your user name and password on C54APRA\"\r\n|s p/Conceptronic C54APRA WAP http config/ d/WAP/
match http m|^HTTP/1\.1 200 Ok\r\nContent-Type: text/html\r\nCache-Control: no-cache\r\nSet-Cookie: SessId=.*HREF=\"/theme/main\.css\".*TD\.calMonth SPAN\n|s p/Floosietek FTgate webmail httpd/
match http m|^HTTP/1\.1 200 OK\r\nContent-Length: \d+\r\nContent-Type: text/html;\r\n.*<TITLE>Aastra ([\w._+-]+)</TITLE>|s p/Aastra $1 VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.0 200 OK\r\n.*<img src=\"images/chumby_logo\.png\">.*<font size=10>Welcome to Chumby</font>|s p/Chumby chumbhttpd/ d/media device/
match http m|^HTTP/1\.1 200 OK\n.*<resolved count='\d+' ommitted='\d+' chumbhowld_ver='([\w._-]+)'>|s p/Chumby chumbhowld/ v/$1/ d/media device/
match http m|^HTTP/1\.1 200 OK\r \nContent-type: text/xml\r\n.*<resolved count='\d+' ommitted='\d+' chumbhowld_ver='([\w._-]+)'>\n</resolved>\r\n|s p/Chumby One chumbhowld/ v/$1/ d/media device/
match http m|^HTTP/1\.1 200 OK\r \nContent-type: text/xml\r\n.*<resolved count='\d+' ommitted='\d+' chumbhowld_ver='([\w._-]+)'>\n<resolve interface='\d+' name='([\w._-]+)' type='_http\._tcp\.'|s p/Chumby One chumbhowld/ v/$1/ h/$2/ d/media device/
match http m|^HTTP/1\.0 200 OK\r\nConnection: Close\r\nContent-Type: text/html; charset=UTF-8\r\n\r\n<html>\r\n.*if \(window != top\) {\r\n\t\t\t\t\t\t// Load page in the top frame\.\r\n\t|s p/Dell OpenManage httpd/ d/remote management/
match http m|^HTTP/1\.1 401 Authorization Required\r\nWWW-Authenticate: Basic realm=\"Linksys BEFSR41v3\"\r\n| p/Linksys BEFSR41v3 http config/ d/broadband router/
match http m|^HTTP/1\.1 200 OK\r\n.*<title>ZyWALL ([\w._+-]+)</title>|s p/ZyXEL ZyWALL $1 http config/ d/security-misc/
match http m|^HTTP/1\.1 200 OK\r\nContent-length: \d+\r\nExpires: -1\r\nContent-type: application/sxp\r\nPragma: no-cache\r\nCache-control: no-cache\r\n\r\n\(ls \)| p/Xen http config/ o/Linux/
match http m|^HTTP/1\.1 401 Authorization Required\r\nWWW-Authenticate: Basic realm=\"NB5580\"\r\n| p/Netcomm NB5580 http config/ d/broadband router/
match http m|^HTTP/1\.0 302 Found\nServer: Alpha_webserv\nDate: .*\r\nContent-Type: text/html\nAccept-Ranges: bytes\nLocation: /public/login\.htm\nX-Pad: avoid browser bug\n\n| p/D-Link DIR-100 http config/ d/broadband router/
match http m|^HTTP/1\.1 200 .*\r\nServer: Allegro-Software-RomPager/([\w._-]+)\r\n.*<font color=\"#FFFFFF\" size=\"4\">Cisco Systems, Inc\. IP Phone (CP-\w+) \( (\w+) \)|s p/Cisco $2 VoIP phone http config/ d/VoIP phone/ i/Allegro RomPager httpd $1; Serial $2/
match http m|^HTTP/1\.0 200 .*\r\nServer: Allegro-Software-RomPager/([\w._-]+)\r\n\r\n<HTML>\n<HEAD>\n<TITLE>NetBotz Network Monitoring Appliance -  </TITLE>|s p/NetBotz network monitor http config/ d/security-misc/ i/Allegro RomPager httpd $1/
match http m|^HTTP/1\.1 302 Redirect\r\nServer: GoAhead-Webs\r\nDate: .*\r\nConnection: close\r\nPragma: no-cache\r\nCache-Control: no-cache\r\nContent-Type: text/html\r\nLocation: http://Device/config/log_off_page\.htm\r\n|s i/LinkSys SLM2024 or SRW2008 switch http config/ d/switch/ p/GoAhead-Webs httpd/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*\r\nServer: WebtoB/([\w._-]+)\r\n| p/TmaxSoft WebtoB httpd/ v/$1/
match http m|^HTTP/1\.0 200 .*<head><meta http-equiv=\"refresh\" content=\"0; URL=cgi-bin/webif/info\.awx\" /><title>Webif&sup2; Administration Console</title>|s p/X-WRT Webif WAP http config/ d/WAP/
match http m|^HTTP/1\.1 200 OK\r\n.*<TITLE>\r\nWorkCentre (\d+) - [\d.]+\r\n</TITLE>|s p/Fuji-Xerox WorkCentre $1 printer http config/ d/printer/
match http m|^HTTP/1\.0 200 OK\r\n.*<title>VoIP ATA400 \(4FXS\) Web Configuration Pages</title>|s p/4FXS ATA400 VoIP adapter http config/ d/VoIP adapter/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: \r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"Linksys (WAG\w+)\n\"\r\n| p/Linksys $1 WAP http config/ d/WAP/
match http m|^HTTP/1\.[01] 200 .*Server: iPhone lighttpd\r\n|s p/iPhone lighttpd/ o/Mac OS X/
match http m|^HTTP/1\.1 200 .*\r\nServer: Allegro-Software-RomPager/([\w._-]+)\r\n.*<A HREF=\"/nic/printerstat\"><IMG SRC=\"/nic/Images/but3\.jpg\"|s p/Kyocera 7035 printer http config/ i/Allegro RomPager $1/ d/printer/
match http m|^HTTP/1\.1 200 OK\r\nSet-Cookie: ALEX_.*\r\nServer: Alexandrie\d+ \(by GBConcept\)\r\n|s p/GBConcept Alexandrie httpd/
match http m|^HTTP/1\.0 200 OK\r\nServer: XmskSvr\r\nContent-Type: text/plain\r\nContent-Length: \d+\r\n\r\nX-MSK http Server ([\w._-]+) | p/Xensoft X-MSK httpd/ v/$1/
match http m|^HTTP/1\.1 200 .*\r\nServer: Allegro-Software-RomPager/([\w._-]+)\r\n.*<TITLE>RICOH FAX (\w+) / RICOH Network Printer|s p/Richoh $2 printer http config/ d/printer/ i/Allegro RomPager httpd $1/
match http m|^HTTP/1\.[01] 401 Unauthorized.*\r\nWWW-Authenticate: Basic [rR]ealm=\"DSL-(\w+)\"|s p/D-Link $1 DSL router http config/ d/broadband router/
match http m|^HTTP/1\.1 200 .*<title>Apt-cacher version ([\w._-]+): Daemon mode</title>|s p/Apt-cacher httpd/ v/$1/
match http m|^HTTP/1\.1 404 .*<title>Not Found, APT Reconfiguration required</title>|s p/Apt-cacher-ng httpd/ i/misconfigured/
match http m|^HTTP/1\.0 200 OK\r\nServer: inets/develop\r\n.*{\"couchdb\": \"Welcome\", \"version\": \"([\w._-]+)\"}\n|s p/CouchDB REST httpd/ v/$1/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: micro_httpd\r\nCache-Control: no-cache\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"DSL Router\"\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<HTML><HEAD><TITLE>401 Unauthorized</TITLE></HEAD>\n<BODY BGCOLOR=\"#cc9999\"><H4>401 Unauthorized</H4>\nAuthorization required\.\n| p/micro_httpd/ d/broadband router/
match http m|^HTTP/1\.0 200 .*\r\n\r\n\r\n<HTML><HEAD><TITLE>Lankacom RouterOS Managing Webpage</TITLE>|s p/Lankacom router http config/ d/router/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: Comanche/([\w._-]+) \(unix\) \r\n|s p/Comanche smalltalk httpd/ v/$1/ o/Unix/
match http m|^HTTP/1\.1 400 Bad Request\r\nConnection: close\r\n\r\n.*<br>Ability FTP Server ([\w._-]+) by Code-Crafters<br>|s p/Code-Crafters Ability ftp http interface/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 401 Unauthorized\r\nDate: .*\r\nServer: WYM/([\w._-]+)\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"Welcome to IPCam !\"\r\n| i/Grandtec wifi webcam http config/ p/WYM httpd/ v/$1/ d/webcam/
match http m|^HTTP/1\.0 404 Error 404 : Domain Not Found.*\r\nServer: MMM BosServer/([\w._-]+)\r\n|s p/MMM BosServer httpd/ v/$1/
match http m|^HTTP/1\.0 200 CREATED\r\nDate: .*\r\nExpires: .*\r\nServer: WhatsUp_Gold/([\w._-]+)\r\n| p/WhatsUp Gold httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 200 OK\r\nServer: SNARE/([\w._-]+)\r\nMIME-version: [\d.]+\r\nContent-type: text/html\r\n\r\n<HTML><head><title>InterSect Alliance - Information Technology Security</title>| p/InterSect Alliance SNARE httpd/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nServer: SimpleHTTP/([\w._-]+) Python/([\w._-]+)\r\n.*<title>NPAD Diagnostics|s p/NPAD Diagnostics httpd/ i/SimpleHTTP $1; Python $2/
match http m|^HTTP/1\.1 401 Unathorized\r\nWWW-Authenticate: BASIC realm=\"PY Software Active WebCam\"\r\n| p/PY Software Active webcam httpd/ d/webcam/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: \r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"Linksys WAG200G \"\r\n| p/Linksys WAG200G http config/ d/WAP/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Digest realm=\"Thomson_cwmp_([\w._-]+)\", nonce=| p/Thomson TR-69 http config/ v/$1/ d/broadband router/
match http m|^HTTP/1\.0 200 OK\r\nServer: sks_www/([\w._-]+)\r\n| p/SKS OpenPGP Key Server httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nCOMMERCE-SERVER-SOFTWARE: Microsoft Commerce Server 2002, Enterprise Edition\r\n| p/Microsoft Commerce Server 2002 httpd/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\n<title>EpsonNet WebManager</title>|s p/EpsonNet WebManager httpd/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nContent-Length: \d+\r\nContent-Type: text/html\r\nServer: SilverStream Server/([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"Novell exteNd Application Server\"\r\n| p/Novell exteNd Application Server httpd/ i/SilverStream httpd $1/
match http m|^HTTP/1\.0 \d\d\d .*<title>EvoCam</title>\n</head>\n\n<body bgcolor=\"e3e3e3\">\n<center>\n<applet archive=\"evocam\.jar\" code=\"com\.evological\.evocam\.class\"|s p/Evological Evocam http config/ o/Mac OS X/
match http m|^HTTP/1\.0 200\r\n.*<font size=\"1\" face=\"Verdana\" color=\"#FF3300\">UDS10/100/IAP\r\nVersion ([\w._-]+)&nbsp;|s p/Lantronix UDS10 ethernet-serial http config/ v/$1/ d/specialized/
match http m|^HTTP/1\.1 200 OK\r\nServer: TriActive MicroAgent \(([\w._-]+)\)\r\n| p/TriActive MicroAgent httpd/ v/$1/
match http m|^HTTP/1\.0 302 Found\r\nLocation: /login\.app\r\nContent-Lenght: 0\r\n\r\n$| p/NetXMS httpd/
match http m|^HTTP/1\.1 200 OK\r\nCONTENT-LANGUAGE:\r\nCONTENT-LENGTH: 0\r\nCONTENT-TPYE: text/xml\r\nDATE: .*\n\r\n\r\n\(null\)| p/Syabas Popcorn Hour http config/ d/media device/
match http m|^HTTP/1\.0 404 Not Found\r\nDate: .*\r\nServer: RadiaMessagingService/([\w._-]+)\r\n| p/HP SIM NVDKIT.exe http config/ i/RadiaMessagingService $1/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: Virata-EmWeb/R([\d_]+)\r\n.*<hr noshade size=\"3\" width=\"100%\">\n<p class=\"alert\">\nYou need to supply a valid user name and password\.\n|s i/Allied Data CopperJet http config/ d/broadband router/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/
match http m|^HTTP/1\.0 302 Moved Temporarily\r\nDate: .*\r\nServer: SMSSMTPHTTP\r\n| p/Symantec smtp mail security http config/ o/Windows/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: MediabolicMWEB/([\w._-]+)\r\n|s p/Mediabolic http config/ v/$1/ d/storage-misc/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Ubicom/([\w._-]+)\r\n.*<title>SMC StreamEngine Router : Login</title>|s i/SMC StreamEngine router http config/ p/Ubicom httpd/ v/$1/ d/router/
match http m|^HTTP/1\.1 200 OK\r\nServer: d-Box network\r\n\r\n| p/Dreambox streaming audio httpd/ d/media device/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\nContent-Type: text/html\r\nContent-Length: \d+\r\nDate: .*\r\nServer: jtvchat\r\n\r\n<html>\n<head><title>Justin\.tv chat servers</title>| p/justin.tv chat server httpd/
match http m|^HTTP/1\.0 200 OK\r\n.*\r\n<TITLE>bric_web_gui</TITLE>\r\n</HEAD>\r\n<BODY bgcolor=\"#555577\">\r\n<!-- URL's used in the movie-->\r\n<!-- text used in the movie-->|s p/Comrex Access BRIC http config/ d/telecom-misc/
match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/([\w._-]+)\r\n.*<!-- saved from url=\(\d+\)http://internet\.e-mail -->.* \r\n<link href=\"miniAP\.css\"|s p/3Com 7760 WAP http config/ d/WAP/ i/RapidLogic httpd $1/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*\r\nServer: I\.T\. Watchdogs, Inc\. Embedded Web Server \(v([\w._-]+)\)\r\n| p/I.T. Watchdogs Embedded httpd/ v/$1/ d/specialized/
match http m|^HTTP/1\.0 200 \r\nServer: A-B WWW/([\w._-]+)\r\n.*<title>1763-([^<]+)</title>\r\n|s p/MicroLogix 1763-$2 logic controller http config/ i/A-B WWW $1/ d/specialized/
match http m|^HTTP/1\.0 200 OK\r\nPragma:no-cache\r\n.*<title>IBM NPS 540\+/542\+; IP address:|s p|IBM NPS 540+/542+ print server http config| d/print server/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: UltiDev Cassini/([\w._-]+)\r\n| p/UltiDev Cassini httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 200 .*\r\nServer: Swiftbase Ltd\. Embedded Web Server \(v([\w._-]+)\)\r\n.*<TITLE>Swift-CM2</TITLE>|s p/Swiftbase Ltd. Climate Monitor http config/ v/$1/ d/specialized/
match http m|^HTTP/1\.1 200 .*\r\nServer: Allegro-Software-RomPager/([\w._-]+)\r\n.*<title>\nLexmark C500</title>|s p/Lexmark C500 printer http config/ i/Allegro RomPager httpd $1/ d/printer/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: micro_httpd\r\n.*WWW-Authenticate: Basic realm=\"Siemens ADSL SL2-141\"\r\n|s p/Siemens SL2-141 ADSL router http config/ d/broadband router/ i/micro_httpd/
match http m|^HTTP/1\.0 200 Document follows\r\nServer: PRINT_SERVER WEB ([\w._-]+)\r\n.*<title>Print Server Setup</title>.*name=\"main\" src=\"ps_stat\.htm\"|s p/LevelOne FPS-3001TXU print server http config/ d/print server/ i/PRINT_SERVER WEB httpd $1/
match http m|^HTTP/1\.0 401 Not Authorized\r\nServer: RapidLogic/([\w._-]+)\r\nMIME-version: 1\.0\r\nContent-type: text/html\r\nWWW-Authenticate: Basic realm=\"Modem Secure\"\r\n| p/Westell Wirespeed DSL modem http config/ d/broadband router/ i/RapidLogic httpd $1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: NT40\r\n.*<title>NT([\w._-]+) - Multiprotocol chat tool</title></head><body><BR><BR><center><b>NT4\.0 Network</b><br><br>Server: (\S+) - \(([\w._-]+)\)<br>Local users connected: (\d+) // Connected to \d+ servers</center><br>Service uptime: ([\d:]+)<br>|s p/NT4.0 Multiprotocol Chat httpd/ v/$1/ i/Name $2; Users $4; Uptime $5/ h/$3/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: http server\r\nDate: .*\r\nCache-Control: no-cache,no-store\r\nWWW-Authenticate: Basic realm=\"Citadel\"\r\n| p/Atera Networks Citadel firewall http config/ d/firewall/
match http m|^HTTP/1\.0 200 .*\r\nServer: IST OIS\r\n.*<title>Phone&nbsp;Station&nbsp;Information</title>|s p/AllWorx 9212 VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.0 401 Unauthorized\r\nDate: .*\r\nServer: Agranat-EmWeb/R([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"GbE2c Ethernet Blade Switch for HP c-Class BladeSystem\"\r\n\r\n401 Unauthorized\r\n| i/HP GbE2c Ethernet Blade Switch http config/ d/switch/ p/Agranat-EmWeb/ v/$SUBST(1,"_",".")/
match http m|^HTTP/1\.1 200 Okay\r\n.*\r\nServer: PLT Scheme\r\n|s p/PLT Scheme httpd/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Swazoo ([\w._-]+) Smalltalk Web Server\r\n| p/Swazoo Smalltalk httpd/ v/$1/
match http m|^HTTP/1\.1 401 OK\r\nContent-Length: 0\r\nConnection: Keep-Alive\r\nWWW-Authenticate: Basic realm=\"/\"\r\nContent-Type: text/html\r\nCache-Control: no-cache\r\nEXT: UCoS, UPnP/1\.0, UDI/1\.0\r\n| p/Universal Devices Insteon home automation http config/ d/specialized/
match http m|^HTTP/1\.1 200 OK\r\n.*Set-Cookie: AUTHKEY=\r\n.*<TITLE>Welcome to Mailtraq WebMail</TITLE>|s p/Mailtraq WebMail httpd/ o/Windows/
match http m|^HTTP/1\.0 200 OK\r\nServer: TopLayer/([\w._-]+)\r\n.*ALT=\"Welcome to the AppSwitch\"|s p|Top Layer Networks AppSafe/AppSwitch IDS http config| v/$1/
match http m|^HTTP/1\.0 200 .*\r\nServer: Mbedthis-AppWeb/([\w._-]+)\r\n.*<title>BT Home Hub manager - Home</title>|s i/BT Home Hub http config/ d/broadband router/ p/Mbedthis-AppWeb/ v/$1/
match http m|^HTTP/1\.1 200 .*\r\nServer: MoxaHttp/([\w._-]+)\r\n.*<TITLE>NPort Web Console</TITLE>|s i/Moxa NPort serial to IP http config/ p/MoxaHttp/ v/$1/ d/specialized/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: MoxaHttp/([\w._-]+)\r\n|s i/Moxa embedded httpd/ p/MoxaHttp/ v/$1/ d/specialized/
match http m|^HTTP/1\.1 200 OK\r\nConnection: close\r\nCache-Control: no-store\r\nContent-Length: \d+\r\nContent-Type: text/html\r\n\r\n<html>\n<style>a{text-decoration:none}</style>\n<body vlink=black bgcolor=\"#99ccff\">\n<center>\n<h1>Invalid Access</h1>\n</center>\n</p></body>\n</html>\n\n\n| p/Cisco ATA186 VoIP adapter http config/ d/VoIP adapter/
match http m|^HTTP/1\.0 200 OK\r\nServer: http server ([\w._-]+)\r\nContent-type: text/html; charset=\(null\)\r\n.*<script>location\.href=\"http://\"\+location\.hostname\+\":\"\+8080\+\"/\";</script></head></html>\n$|s p/QNAP TS-109 NAS http config/ d/storage-misc/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nServer: http server ([\w._-]+)\r\n.*<title>NAS</title>\n<script language=\"JavaScript\">\n\nfunction setCookie\(name, value, expires\)\n|s p/QNAP TS-109-II NAS http config/ d/storage-misc/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nServer: http server ([\w._-]+)\r\n.*<script>\npr=\(document\.location\.protocol == 'https:'\) \? 'https' : 'http';\npt=\(location\.port == ''\) \? '' : ':' \+ location\.port;\nredirect_suffix = \"/redirect\.html\?count=\"\+Math\.random\(\);|s p/QNAP TS-239 or TS-509 NAS http config/ d/storage-misc/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nServer: http server ([\w._-]+)\r\n.*Content-length: 553\r\n.*{\nlocation\.href=pr\+\"://\"\+location\.hostname\+pt\+redirect_suffix;\n}\nelse\t//could be ipv6 addr\n|s p/QNAP TS-219P NAS http config/ d/storage-misc/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nServer: http server ([\w._-]+)\r\n.*Content-length: 291\r\n.*if\(location\.hostname\.indexOf\(':'\) == -1\){location\.href='http://'\+location\.hostname\+':'\+8080\+'/';\n}|s p/QNAP TS-659 NAS http config/ d/storage-misc/ v/$1/
match http m|^HTTP/1\.0 404 no application for: /\r\nServer: HttpServer\r\n\r\n$| p/Galleon TiVo Application Port http config/ d/media device/
match http m|^HTTP/1\.0 404 File not found\r\nServer: HttpServer\r\n\r\n$| p/Galleon TiVo Publishing Port http config/ d/media device/
match http m|^HTTP/1\.1 302 Redirect\r\nServer: GoAhead-Webs\r\nDate: .*\r\nConnection: close\r\nPragma: no-cache\r\nCache-Control: no-cache\r\nContent-Type: text/html\r\nLocation: http://\(null\)/config/log_off_page\.htm\r\n\r\n| p/Dell PowerConnect Gigabit switch http config/ d/switch/ i/GoAhead-Webs httpd/
match http m|^HTTP/1\.0 301 Moved Permanently\r\nContent-Length: 0\r\nConnection: close\r\nLocation: /main/main\.html\r\nServer: debut/([\w._-]+)\r\n\r\n| p/Brother MFC-8860DN printer http config/ d/printer/ i/debut httpd $1/
match http m|^HTTP/1\.1 302 Moved Temporarily\r\nDate: .*\r\nServer: Avocent DSView ([\w._/-]+)\r\nLocation: https://([\w._-]+)/dsview/\r\nConnection: close\r\n\r\n| p/Avocent DSView remote management httpd/ v/$1/ h/$2/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: RAID HTTPServer/([\w._-]+)\r\n| p/Sun StorEdge 3511 http config/ v/$1/ d/storage-misc/
match http m|^HTTP/1\.0 401 NG\r\nWWW-Authenticate: Basic realm=\"AirLive W([\w._-]+)\"\r\n\r\n<!--CAS:0003-->Unauthorized| p/AirLive W$1 WAP http config/ d/WAP/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\n.*<title>Samsung Printer Status</title>.*var contentURI = \"/general/printerDetails\.htm\"|s p/Samsung printer http config/ d/printer/
match http m|^HTTP/1\.0 200 OK\r\nCache-control: no-cache\r\nServer: Ubicom/([\w._-]+)\r\n.*<title>NETGEAR WNHDE111 |s i/Netgear WNHDE111 WAP http config/ p/Ubicom httpd/ v/$1/ d/WAP/
match http m|^HTTP/1\.0 200 .*\r\nServer: Server\r\n.*<title>[nN]euf ?box -&nbsp;Accueil</title>|s p/SFR Neuf Box DSL modem http config/ d/broadband router/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: Axigen-Webmail\r\n|s p/Axigen webmail httpd/ o/Unix/
match http m|^HTTP/1\.0 200 .*\r\nServer: Allegro-Software-RomPager/([\w._-]+)\r\n\r\n<HTML><HEAD>\n<META NAME=\"GENERATOR\" CONTENT=\"Microsoft FrontPage 3\.0\">\n<TITLE></TITLE>.*<frame NAME=\"fInfo\" scrolling=\"no\" noresize src=\"/html/Hlogin\.html\"|s p/Amer.com SSR22i switch http config/ d/switch/ i/Allegro RomPager httpd $1/
match http m|^HTTP/1\.1 301 Moved Permanently\r\nDate: .*\r\nServer: eSoft\r\nX-Powered-By: PHP/([\w._-]+)\r\nLocation: https://ThreatWall/\r\n| p/eSoft ThreatWall IPS http config/ i/PHP $1/ d/security-misc/
match http m|^HTTP/1\.0 200 OK\r\nServer: NetPort Software ([\w._-]+)\r\nDate: .*\r\nContent-type: text/html\r\n\r\n<html>\n<head>\n<title>(.*) - VSX 7000A</title>| p/Polycom VSX 7000A http config/ d/webcam/ i/NetPort httpd $1; name $2/
match http m|^HTTP/1\.1 301 Moved Permanently\r\nServer: Virata-EmWeb/R([\w._-]+)\r\nLocation: https://[\w._-]+/\+webvpn\+/index\.html\r\n| i/Cisco WebVPN http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/security-misc/
match http m|^HTTP/1\.0 200 OK\r\nServer: dtHTTPd/([\w._-]+)\r\nContent-Type: text/html\r\nContent-Length: \d+\r\nConnection: close\r\n\r\n<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.0 Transitional//EN\"><HTML><HEAD><TITLE>UX-D1200SE</TITLE>| p/Sharp Broadband UX-D1200SE Fax http config/ d/printer/ i/dtHTTPd $1/
match http m|^HTTP/1\.1 200 OK\r\nServer: Conexant-EmWeb/R([\w._-]+) SIPGT/([\w._-]+)\r\n.*<title>Login page</title>.*<img src=\"images/ixlogga\.gif\"|s i/Intertex IX68 WAP http config; SIPGT $2/ d/WAP/ p/Conexant-EmWeb/ v/$SUBST(1,"_",".")/
match http m|^HTTP/1\.0 404 Not Found\r\nContent-Length: \d+\r\nContent-Type: text/html\r\n\r\n.*<title>NOTE: The requested URL could not be retrieved</title>.*background-image: url\(/html/de/images/bg_ramp\.jpg\);\r\n|s p/AVM FRITZ!Box WAP http config/ d/WAP/
match http m|^HTTP/1\.0 404 Not Found\r\nContent-Length: \d+\r\nContent-Type: text/html\r\n\r\n.*<title>Note: The requested URL could not be retrieved\.</title>.*background-image: url\(\.\./\.\./de/images/bg_ramp\.jpg\);\n|s p/AVM FRITZ!Box WLAN 7270 WAP http config/ d/WAP/
match http m|^HTTP/1\.0 401 Unauthorized\r\nContent-Length: \d+\r\nContent-Type: text/html.*\r\nPragma: no-cache\r\nServer: Webserver\r\nWWW-Authenticate: Basic realm=\"HTTPS Access\"\r\n\r\n<HTML><HEAD><TITLE>401 Unauthorized \(ERR_ACCESS_DENIED\)</TITLE></HEAD><BODY><H1>401 Unauthorized</H1><BR>ERR_ACCESS_DENIED<HR><B>Webserver</B>| p/AVM FRITZ!Box WAP http config/ d/WAP/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: lighttpd[/ ]([\d.]+)( \([^)]+\))?\r\n|si p/lighttpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: lighttpd|si p/lighttpd/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: micro_httpd\r\nCache-Control: no-cache\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"U\.S\. Robotics ADSL Router\"\r\n| p/USRobotics USR9107A ADSL http config/ d/broadband router/ i/micro_httpd/
match http m|^HTTP/1\.0 200 Ok\r\nServer: httpd\r\nDate: .*<SCRIPT language=Javascript src=\"language_us\.js\"></SCRIPT>\n<SCRIPT>assign_var\(\);</SCRIPT>\n<SCRIPT language=JavaScript src=\"showMenu\.js\"></SCRIPT>\n<SCRIPT>\n\tvar helpItem \t='indexa';|s p/Belkin N1 F5D8231-4 WAP http config/ d/WAP/
match http m|^<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.01 Transitional//EN\" \"http://www\.w3\.org/TR/1999/REC-html401-19991224/loose\.dtd\">\n<HTML>\n<HEAD>\n<TITLE>Mac OS X Personal Web Sharing</TITLE>.*<H1>Your website here\.</H1>|s p/REALbasic 2008 example httpd/
match http m|^HTTP/1\.1 200\r\n.*<TITLE>ProjectorView Control System</TITLE>.*CODE=com\.mitsubishi\.x500u\.X500UApplet\.class\r\n|s p/Mitsubishi Projector XD1000 http config/ d/media device/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: micro_httpd\r\nCache-Control: no-cache\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"Wireless Router\"\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<HTML><HEAD><TITLE>401 Unauthorized</TITLE></HEAD>\n<BODY BGCOLOR=\"#cc9999\"><H4>401 Unauthorized</H4>\nAuthorization required\.\n| p/Asus wl-600g WAP http config/ d/WAP/
match http m|^HTTP/1\.0 301 Moved Permanently\r\nCache-Control: no-cache\r\nConnection: close\r\nPragma: no-cache\r\nLocation: /TopAccess/default\.htm\r\nServer: TOSHIBA TEC CORPORATION\r\n| p/Toshiba Tec printer http config/ d/printer/
match http m|^HTTP/1\.0 303 See Other\r\nLocation: http://[\w._-]+:8080\r\n\0 .*\rContent-Length: 0\r\n\r\n| p|Toshiba e-STUDIO 233 copier/printer/fax http config| d/printer/
match http m|^HTTP/1\.0 200 OK\r\nServer: InterNiche Technologies WebServer ([\w._-]+)\r\n| p/InterNiche Technologies httpd/ v/$1/
match http m|^HTTP/1\.1 302 Redirect\r\nServer: GoAhead-Webs\r\nPragma: no-cache\r\nCache-Control: no-cache\r\nContent-Type: text/html\r\nLocation: http://[\w._-]+/index\.asp\r\n\r\n<html><head></head><body>\r\n\t\tThis document has moved to a new| p/GoAhead-Webs/ i/Dell PowerConnect 3024 switch http config/ d/switch/
match http m|^HTTP/1\.0 302 Redirect\r\nServer: GoAhead-Webs\r\nDate: .*\r\nConnection: Close\r\nPragma: no-cache\r\nCache-Control: no-cache\r\nContent-Type: text/html\r\nLocation: http://\xee{64}/index\.html\r\n\r\n<html><head></head><body>\r\n\t\tThis document has moved to a new| p/GoAhead-Webs/ i/Allen-Bradley ControlLogix 1769-L35E automation controller http config/ d/specialized/
match http m|^HTTP/1\.1 200 OK\n\n<html>\n<head>\n<title>Touchstone Status</title>| p/Arris Touchstone cable modem http config/ d/broadband router/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: micro_httpd\r\nCache-Control: no-cache\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"ROTAL Wireless ADSL2\+ Router\"\r\n| p|ROTAL/Dynalink WAP http config| d/WAP/ i/micro_httpd/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*\r\nServer: Oversee Webserver v([\w._-]+)\r\n| p/Oversee httpd/ v/$1/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: GlobalSCAPE-Secure Server/([\w._-]+)\r\n| p/GlobalSCAPE CuteFTP secure httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: GlobalSCAPE-EFTServer/([\w._-]+)\r\n| p/GlobalSCAPE EFTServer httpd/ v/$1/
match http m|^<html>\n\n<head>\n<title>HTML-Konfiguration</title>\n\n<SCRIPT language=\"JavaScript\">\n<!--\n\n\nfunction rahmen\(but,high\)| p|Targa WR500/Speedport WV500V WAP http config| i/Bitswitcher firmware/ d/WAP/
match http m|^\[ menu  \]   - Control packet filtering\r\n5 - Logs            \[ menu  \]   - Alarm and log control\r\n6HTTP/1\.0 200 OK\r\n.*<font color=\"#ffffff\">Aironet BR500E V([\w._-]+)</td>|s p/Aironet BR500E WAP http config/ d/WAP/ v/$1/
match http m|^HTTP/1\.1 401 Authorization Required\r\nDate: .*\r\nServer: mini-http/([\w._-]+) \(unix\)\r\nConnection: close\r\nContent-Type: text/html\r\nWWW-Authenticate: Basic realm=user\r\n\r\n<!DOCTYPE HTML PUBLIC \"-//IETF//DTD HTML 2\.0//EN\">| p/Kemp 2500 load balancer http config/ d/load balancer/ o/Unix/ i/mini-http $1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: \"Pi3Web/([\w._-]+)\"\r\n|s p/Pi3Web httpd/ v/$1/
match http m|^HTTP/1\.0 401 Authorization Required\r\nWWW-Authenticate: Basic realm=\"VoIP841\"\r\n.*\r\nServer: simple httpd ([\w._-]+)\r\n|s i/Philips DECT VoIP841 http config/ p/simple httpd/ v/$1/ d/VoIP phone/
match http m|^HTTP/1\.0 401 Authorization Required\r\nWWW-Authenticate: Basic realm=\"SPH200D\"\r\n.*\r\nServer: simple httpd ([\w._-]+)\r\n|s p/simple httpd/ v/$1/ i/Netgear SPH200D http config/ d/VoIP phone/
match http m|^HTTP/1\.1 403 Forbidden\r\nServer: Mediasite Web Server/([\w._-]+)\r\nDate: .*\r\nContent-Length: \d+\r\nHttpConnection: Close\r\n| p/SonicFoundry MediaSite httpd/ v/$1/ d/media device/
match http m|^HTTP/1\.0 200 .*\r\nServer: Mbedthis-Appweb/([\w._-]+)\r\n.*\r\nX-Powered-By: PHP/([\w._-]+)\r\n.*<title>([\w._-]+) : Log In - Juniper Networks Web Management</title>|s p/Mbedthis-Appweb/ v/$1/ i/Juniper router http config; PHP $2; name $3/ d/router/
match http m|^HTTP/1\.1 302 Redirect\r\nServer: GoAhead-Webs\r\n.*Location: https://Device/config/log_off_page\.htm\r\n|s p/Linksys SRW2024 switch http config/ d/switch/ i/GoAhead httpd/
match http m|^HTTP/1\.1 401 Unauthorized\r\nContent-Type: text/html\r\nConnection: close\r\n(?:Pragma: no-cache\r\n)?WWW-Authenticate: Basic realm=\"Netcam\"\r\nContent-Length: 17\r\n\r\n401 Unauthorized\n$| p/Airlink 101 or TRENDnet TVIP-422w webcam http config/ d/webcam/
match http m|^HTTP/1\.1 503 Service Unavailable\r\nServer: NS([\w._-]+)\r\nContent-Length:\d+\r\n| p/Citrix Netscalers httpd/ d/load balancer/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\nDate: .*\r\nLast-Modified: .*\r\nContent-Language: en\r\nContent-Length: \d+\r\nServer: Wireless Network Camera\r\n\r\n<html>\r\n<frameset rows=\"2000,0\" border=\"0\" frameborder=\"no\" framespacing=\"0\">| p/LevelOne WCS-2030 webcam http config/ d/webcam/
match http m|^HTTP/1\.0 200 .*\r\nServer: wg_httpd/([\w._-]+)\(based Boa/([\w._-]+)\)\r\n.*<title>WebEye Index Page</title>\n<meta name=\"generator\" content=\"WebGateInc\">|s p/WebGateInc WebEye webcam http config/ i/wg_httpd $1 based on Boa $2/ d/webcam/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Nano HTTPD library\r\n|s p/Ferhat Ayaz's Nano httpd/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: Transmission\r\nWWW-Authenticate: Basic realm=\"Transmission\"\r\n| p/Transmission BitTorrent management httpd/ i/unauthorized/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: Transmission\r\nContent-Type: text/html; charset=ISO-8859-1\r\n| p/Transmission BitTorrent management httpd/ i/unauthorized/
match http m|^HTTP/1\.0 403 Forbidden\r\nServer: Transmission\r\nContent-Type: text/html; charset=ISO-8859-1\r\n| p/Transmission BitTorrent management httpd/ i/unauthorized/
match http m|^HTTP/1\.0 301 Moved Permanently\r\nServer: Transmission\r\nLocation: /transmission/web/\r\nContent-Type: text/html; charset=ISO-8859-1\r\n\r\n| p/Transmission BitTorrent management httpd/
match http m|^HTTP/1\.0 301 Moved Permanently\r\nServer: Transmission\r\nLocation: http://\(null\)/transmission/web/\r\nContent-Type: text/html; charset=ISO-8859-1\r\n\r\n| p/Transmission BitTorrent management httpd/
match http m|^HTTP/1\.1 200 .*<meta http-equiv=\"Refresh\" content=\"2; url=/transmission/web/\">\r\n.*<p>redirecting to <a href=\"/transmission/web\">/transmission/web/</a></p>|s p/Transmission BitTorrent management httpd/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: GoAhead-Webs\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"WebAdmin\"\r\n.*<p>Access to this document requires a User ID</p>|s p/TeleWell TW-EA510 ADSL router http config/ d/broadband router/ i/GoAhead httpd/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Enigma2 WebInterface Server ([\w._-]+) \r\n|s p/Enigma2 Dreambox http config/ d/media device/ v/$1/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: DPH-140\r\nWWW-Authenticate: Digest realm=\"DPH-140\"| p/D-Link DPH-140 VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"Topfield PVR Web Server\"\r\n\r\n| p/Topfield HDPVR satellite decoder http config/ d/media device/
match http m|^HTTP/1\.1 200 OK\r\nAccept-Ranges: bytes\r\nContent-Type: text/html\r\n\r\n.*<font size=\+3>WAGO-Ethernet TCP/IP PFC</font>.*<td>Firmware revision</td>\n\n<td>([^<]+)</td>.*<td>Hardware address</td>\n\n<td>(\w+)</td>|s p/Wago ethernet controller http config/ v/$1/ i/MAC $2/
match http m|^HTTP/1\.0 200 OK\r\nServer: vxTri's Versatile Smart Server \(TVSS\) V ([\w._-]+)\r\nSet-Cookie: Intoto=.*<title> Login Screen </title>|s p/Adtran Netvanta 2100 VPN Gateway http config/ d/security-misc/ i/vxTri's Versatile Smart Server httpd $1/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: Hauppauge's DVB EPG Webserver v([\w._-]+)\r\n| p/Hauppauge DVB EPG http config/ v/$1/ d/media device/
match http m|^HTTP/1\.0 200 .*\r\nServer: HCW_DVB_EPG_SERVER_([\w._-]+)\r\n.*<title>Hauppauge EPG</title>\r\n|s p/Hauppauge DVB EPG http config/ v/$SUBST(1,"_",".")/ d/media device/
match http m|^HTTP/1\.0 200 Ok.*<IMG SRC=\"compaq\.gif\" ALT=\"COMPAQ\"><BR>\r\n<H3>Remote Insight Lights-Out Edition<BR></H3>|s p|HP/Compaq Integrated Lights-Out http config| d/remote management/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\nContent-Type: text/html\r\nContent-Length: \d+\r\nCache-Control: no-cache\r\n\r\n<html>\n<head>\n<title> Home </title>\n<script src=\"script/cookieCode\.js\"></script>\n<script language=\"JavaScript\">\n<!--\nfunction SetDefLanguage\(\)\n| p/Xerox Phaser 3500 http config/ d/printer/
match http m|^HTTP/1\.0 200 OK\r\nCache-control: no-cache\r\nServer: Ubicom/([\w._-]+)\r\n.*<title>WGA600N Wireless Gaming Adapter  :\r\n\t\t Login\r\n\t</title>|s i/Linksys WGA600N WAP http config/ d/WAP/ p/Ubicom httpd/ v/$1/
match http m|^HTTP/1\.0 200 .*\r\nExpires: -1\r\n.*<title>NetGear GS(\w+)</title>|s p/NetGear GS$1 switch http config/ d/switch/
match http m|^HTTP/1\.1 400 Error in MIME message\r\n$| p/Wyse Winterm 1200 LE terminal http config/ d/terminal/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: Web Server\r\n.*WWW-Authenticate: Basic realm=\"WebAdmin\"\r\n.*<p class=\"alert\">Web configuration is protected\.</p>\n\n<p><a href=\"Javascript:history\.go\(-1\)\">|s p/D-Link DSL2-300G http config/ d/broadband router/
match http m|^HTTP/1\.0 200 .*<title>BPA430 Web Configuration Pages</title></head><script LANGUAGE=\"JavaScript\" src=\"menu\.js\">|s p/Packet8 BPA430 VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.0 200 Document follows\r\nServer: ADH-Web\r\n.*<meta name=\"author\" content=\"Dedicated Micros \(info@dmicros\.com\)\">\r\n|s p/Dedicated Micros Digital Sprite 2 DVR http config/ i/ADH-Web httpd/ d/media device/
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"FR114W\"\r\nContent-type: text/html\r\n\r\n401 Unauthorized| p/NetGear FR114W WAP http config/ d/WAP/
match http m|^HTTP/1\.0 200 .*\r\nServer: Mbedthis-Appweb/([\w._-]+)\r\n.*<title>Openstage IP Phone User</title>.*<meta name='author' content='Siemens AG,|s i/Siemens Openstage VoIP phone http config/ d/VoIP phone/ p/Mbedthis-Appweb/ v/$1/
match http m|^HTTP/1\.1 404 Not Found\r\nServer: Splunkd\r\n| p/Splunkd httpd/
match http m|^HTTP/1\.0 200 OK\r\n.*<!-- General javascripts -->.*var path='http://www\.axis\.com/cgi-bin/prodhelp\?prod=axis_([\w._-]+)&ver=([\w._-]+)&|s p/AXIS $1 print server http config/ v/$2/ d/print server/
match http m|^HTTP/1\.1 401 Unauthorized\r\nConnection: close\r\nContent-Type: text/html\r\nContent-Length: \d+\r\nServer: Indy/([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"KutinSoft Reboot Service\"\r\n| i/KutinSoft reboot service http config/ o/Windows/ p/Indy httpd/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\n.*VMware Server provides a virtual machine platform, which can be managed by VMware VirtualCenter Server\.\">\r\n\r\n<title>VMware Server 2</title>|s p/VMware Server http config/ v/2/
match http m|^HTTP/1\.1 200 OK\r\n.*document\.write\(\"<title>\" \+ ID_VC_Welcome \+ \"</title>\"\);.*<meta name=\"description\" content=\"VMware VirtualCenter|s p/VMware Server http config/
match http m|^HTTP/1\.0 200 Ok\r\nServer: UI-WebServer V([\w._-]+)\r\n| p/UI-View Automatic Packet Reporting System httpd/ o/Windows/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n.*<!--- Page\(\d+\)=\[Login\] --->.*<TITLE>Verizon</TITLE>|s p/Verizon FIOS Actiontec http config/ d/broadband router/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: text/html\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n.*<!--- Page\(\d+\)=\[\] --->.*<TITLE>Management Console</TITLE>|s p/USRobotics USR8200 firewall http config/ d/firewall/
match http m|^HTTP/1\.1 200 OK\r\nServer: Synacast Media Server/([\w._-]+)\r\nConnection: close\r\n\r\n| p/Synacast Media Server http config/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nServer: DCLK-HttpSvr\r\n| p/DoubleClick advertising httpd/
match http m|^HTTP/1\.1 200 OK\r\nContent-type: text/html\r\nServer: Mono-HTTPAPI/([\w._-]+)\r\n.*<H1>Ooops!</H1><P>The page you requested has been obsconded with by knomes\. Find hippos quick!</P>|s i/OpenSimulator httpd/ p/Mono-HTTPAPI/ v/$1/
match http m|^HTTP/1\.0 404 NotFound\r\nContent-type: text/html\r\n.*Server: Tiny WebServer\r\n.*<H1>Ooops!</H1><P>The page you requested has been obsconded with by knomes\. Find hippos quick!</P><P>If you are trying to log-in, your link parameters should have: &quot;-loginpage http:///\?method=login -loginuri http:///&quot; in your link </P></BODY></HTML>|s i/OpenSimulator httpd/ p/Tiny WebServer/
match http m|^HTTP/1\.0 200 OK\r\nDate: .*\r\nServer: NetGate \r\nConnection: close\r\nContent-Type: text/html\r\n| p/AT&T NetGate VPN http config/ d/security-misc/
match http m|^HTTP/1\.1 401 Unauthorized\r\nConnection: close\r\nContent-Type: text/html\r\nContent-Length: \d+\r\nServer: Indy/([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"Atis Web-Server Autentica| i/Atis Surveillance camera http config/ d/webcam/ p/Indy httpd/ v/$1/
match http m|^HTTP/1\.0 200 KDH1_STC_OK\r\nServer: KDH/([\w_.-]+) \(([\w:]+)\)\r\n.*<title>IBM Tivoli Monitoring Service Index</title>|s p/IBM Tivoli Monitoring http config/ i/KDH httpd $1 $2/ d/remote management/
match http m|^HTTP/1\.0 401 Unauthorized\r\nMIME-Version: [\d.]+\r\nServer: SNMP Research DR-Web Agent/([\w._-]+)\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"DR-Web\"\r\n| p/SNMP Research DR-Web http config/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nServer: Winstone Servlet Engine v([\w._-]+)\r\nX-Hudson: ([\w._-]+)\r\nX-Hudson-CLI-Port: (\d+)\r\n.*X-Powered-By: Servlet/([\w._-]+) \(Winstone/[\w._-]+\)\r\n|s p/Winstone Servlet Engine/ v/$1/ i/Hudson $2; Servlet $4; CLI port $3/
match http m|^HTTP/1\.0 200(?: OK)?\r\nServer: Winstone Servlet Engine v([\w._-]+)\r\n| p/Winstone Servlet Engine/ v/$1/
match http m|^HTTP/1\.0 401 Unauthorized\r\nDate: .*\r\nContent-Length: \d+\r\nContent-Type: text/html\r\nServer: SilverStream Server/([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"SilverStream\"\r\n| p/Silverstream web application management httpd/ v/$1/
match http m|^HTTP/1\.0 200 .*\r\nServer: Allegro-Software-RomPager/([\w._-]+)\r\n.*<TITLE>SONY NSP-100 Main Page</TITLE>|s p/Sony NSP-100 network player http config/ d/media device/ i/Allegro RomPager httpd $1/
match http m|^HTTP/1\.0 302 Not Found\r\nConnection: close\r\nLocation: /user/login\r\nAccept-Ranges: none\r\nServer: Sockso\r\n\r\n$| p/Sockso personal music player httpd/
match http m|^HTTP/1\.1 302 Not Found\r\nConnection: close\r\nLocation: /user/login\r\nServer: Sockso\r\n\r\n| p/Sockso personal music player httpd/
match http m|^HTTP/1\.1 303 See Other\r\nContent-Type: text/html\r\nContent-Length: 0\r\nLocation: https://[\d.]+:443/webvpn\.html\r\nSet-Cookie: webvpncontext=| p/Cisco WebVPN http config/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\nExpires: -1\r\n Cache-Control: no-cache\r\n.*<title>Contivity VPN Client</title>|s p/Contivity VPN Client httpd/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\n.*<title>RemoteView</title>.*<frame name=\"menu\" src=\"Menu_main\.htm\" target=\"parent\.work\"|s p/Kguard Security DVR http config/ d/webcam/
match http m|^HTTP/1\.0 200 OK\r\n.*<title>LaCie Network Space NAS</title>.*<meta http-equiv=\"refresh\" content=\"0;url=/cgi-bin/public/login\">|s p/LaCie Network Space NAS http config/ d/storage-misc/
match http m|^HTTP/1\.0 200 OK\r\nServer: Development/([\w._-]+) Python/([\w._-]+)\r\n| p/Google App Engine httpd/ v/$1/ i/Python $2/
match http m|^HTTP/1\.0 200 OK\r\nServer: Development/([\w._-]+)\r\n| p/Google App Engine httpd/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: text/html\r\n\r\n<html><head><title>APC Back-UPS HS 500\(BackUPS500\0\)</title>| p/APC Back-UPS HS 500 http config/ d/power-device/
match http m|^HTTP/1\.1 500 Internal Server Error\r\nConnection: close\r\nContent-Type: text/plain\r\nContent-Length: 16\r\n\r\nEAccessViolation$| p/TiVo Desktop Server http config/ o/Windows/
match http m|^HTTP/1\.0 401 Not Authorized\r\nServer: RapidLogic/([\w._-]+)\r\nMIME-version: 1\.0\r\nContent-type: text/html\r\nWWW-Authenticate: Basic realm=\"Secure Realm\"\r\n\r\n\r\nAuthorization Required\r\n\r\n$| i/3Com OfficeConnect WAP http config/ d/WAP/ p/RapidLogic/ v/$1/
match http m|^HTTP/1\.0 401 Not Authorized\r\nServer: RapidLogic/([\w._-]+)\r\nMIME-version: 1\.0\r\nPragma: no-cache\r\nContent-type: text/html\r\nWWW-Authenticate: Basic realm=\"Secure Realm\"\r\n\r\n\r\nAuthorization Required\r\n\r\n$| p/RapidLogic/ v/$1/ i/Linksys WAP55AG WAP http config/ d/WAP/
match http m|^HTTP/1\.1 400 Bad Request\r\nConnection: close\r\n\r\n.*<br>Ability Mail Server ([\w._-]+) by Code-Crafters<br>|s p/Ability Mail Server http config/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 200 OK\r\nContent-Length: \d+\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<html><head><title>Available Databases - Banshee DAAP Browser</title>| p/Banshee DAAP browser httpd/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: FlashCom/([\w._-]+)\r\n.*<html><head><title>Wowza Media Server ([^<]*)</title></head>|s p/FlashCom/ v/$1/ i/Wowza Media Server $2 http config/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: FlashCom/([\w._-]+)\r\n.*<\?xml version=\"1\.0\" encoding=\"utf-8\"\?>\n<result>\n\t<level>error</level>\n\t<code>NetConnection\.Connect\.Rejected</code>|s p/FlashCom/ v/$1/ i/Adobe Flash Media Server/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\nContent-Length: \d+Content-Type: text/html\r\n\r\n\r\n<html><body>This site is running <a href='http://www\.TeamViewer\.com'>TeamViewer</a>\.</body></html>\r\n| p/TeamViewer httpd/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\nContent-Length: \d+\r\nContent-Type: text/html\r\n\r\n<html><body>This site is running <a href='http://www\.TeamViewer\.com'>TeamViewer</a>\.</body></html>\r\n| p/TeamViewer httpd/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\nContent-Type: text/html\r\nContent-Length: 98\r\n\r\n<html><body>This site is running <a href='http://www\.TeamViewer\.com'>TeamViewer</a>\.</body></html>| p/TeamViewer httpd/
match http m|^HTTP/1\.0 200 OK\r\nCache-control: no-cache\r\nContent-Type: application/octet-stream\r\nConnection: close\r\nHTTP/1\.0 200 OK\r\nConnection: close\r\nContent-Length: 181\r\nContent-Type: text/html\r\n\r\n<html><body>This site is running <a href='http://www\.TeamViewer\.com'>TeamViewer</a>\.| p/TeamViewer httpd/
match http m|^HTTP/1\.1 \d\d\d .*\r\nContent-Type: text/html\r\n\r\n.*<p>Not a recognized search path\.</p>\n<hr />\n<p><i>MWSearch on localhost</i></p>\n</body>\n</html>\r\n|s p/MediaWiki Lucene powered search httpd/
match http m|^HTTP/1\.0 500 Internal Server Error\r\nDate: \r\nServer: \r\nContent-Length: \d+ \r\nContent-Type: text/html\r\n\r\n.*<title>Error Page 500</title>|s p/ESET NOD32 anti-virus update httpd/ o/Windows/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/xml; charset=utf-8: \r\n.*<VendorName>D-Link Systems</VendorName><ModelDescription>Xtreme N GIGABIT Router</ModelDescription><ModelName>DIR-([^<]+)</ModelName><FirmwareVersion>([^<]+)</FirmwareVersion>|s p/D-Link Xtreme $1 WAP http config/ d/WAP/ i/Firmware $2/
match http m|^HTTP/1\.0 200 OK\r\n.*<meta http-equiv=\"refresh\" content=\"0; URL=/cgi-bin/luci\" />\n</head>.*href=\"/cgi-bin/luci\">LuCI - Lua Configuration Interface</a>|s p/LuCI Lua http config/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: LuCIttpd/([\d.]+)\r\n| p/LuCIttpd/ v/$1/ d/WAP/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: LuCId-HTTPd/([\d.]+)\r\n| p/LuCId-HTTPd/ v/$1/
match http m|^HTTP/1\.0 401 Not Authorised\r\nServer: Majestic-12 WebServer v([\w._-]+)\r\n| p/Majestic-12 httpd/ v/$1/
match http m|^HTTP/1\.0 405 Method not allowed: Method not allowed by server: GET\r\nDate: .*\r\nCache-Control: no-cache\r\nServer: openwbem/([\w._-]+) \(CIMOM\)\r\n| p/Openwbem CIMOM httpd/ v/$1/
match http m|^HTTP/1\.1 401 Unauthorized\r\nContent-Type: text/html\r\nWWW-Authenticate: Basic realm=\"Network Monitor\"\r\nConnection: close\r\n\r\n<html><body><font size=\"2\"><b>You could not be authenticated by the GFI N\.S\.M\. web server\.| p/GFI Network Service Monitor http config/
match http m|^HTTP/1\.1 \d\d\d .*\r\n.*X-Powered-By: Servlet/([\w._-]+)\r\nServer: GlassFish/v([\w._-]+)\r\n| p/Sun GlassFish/ v/$2/ i/Servlet $1/
match http m|^HTTP/1\.1 \d\d\d .*\r\n.*X-Powered-By: Servlet/([\w._-]+)\r\nServer: GlassFish v([\w._-]+)\r\n| p/Sun GlassFish/ v/$2/ i/Servlet $1/
match http m|^HTTP/1\.1 \d\d\d .*\r\n.*X-Powered-By: Servlet/([\w._-]+)\r\nServer: GlassFish Server Open Source Edition ([\w._-]+)\r\n|s p/Sun GlassFish Open Source Edition/ v/$2/ i/Servlet $1/
match http m|^HTTP/1\.1 \d\d\d .*\r\n.*Server: GlassFish Server Open Source Edition ([\w._-]+)\r\nX-Powered-By: Servlet/([\w._-]+)\r\n|s p/Sun GlassFish Open Source Edition/ v/$1/ i/Servlet $2/
match http m|^HTTP/1\.1 \d\d\d .*\r\n.*X-Powered-By: Servlet/([\d.]+)\r\nServer: Sun GlassFish Enterprise Server v([\d.]+)\r\n.*X-Powered-By: JSF/([\d.]+)\r\n|s p/Sun GlassFish/ v/$2/ i/Servlet $1; JSF $3/
match http m|^HTTP/1\.1 \d\d\d .*\r\n.*X-Powered-By: Servlet/([\d.]+)\r\nServer: Sun GlassFish Enterprise Server v([\d.]+)\r\n|s p/Sun GlassFish/ v/$2/ i/Servlet $1/
match http m|^HTTP/1\.1 \d\d\d .*\r\n.*X-Powered-By: Servlet/([\d.]+)\r\nServer: Sun GlassFish Communications Server ([\d.]+)\r\n|s p/Sun GlassFish Communications Server/ v/$2/ i/Servlet $1/
match http m|^HTTP/1\.1 \d\d\d .*\r\n.*Server: Sun GlassFish Enterprise Server v([\d.]+)\r\nX-Powered-By: Servlet/([\d.]+)\r\n|s p/Sun GlassFish/ v/$1/ i/Servlet $2/
match http m|^HTTP/1\.1 \d\d\d .*\r\n.*Server: Sun GlassFish Enterprise Server v([\d.]+)\r\n|s p/Sun GlassFish/ v/$1/
match http m|^HTTP/1\.[01] 200 OK\r\n.*Server: IndigoWebServer/([\w_.-]+)\r\n|s p/Perceptive Automation Indigo http config/ v/$1/ d/specialized/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: llink-daemon/([\w._-]+) \(build (\d+)\)\r\n| p/llink media streamer httpd/ v/$1 build $2/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: text/html\r\n\r\n<html xmlns:o=\"urn:schemas-microsoft-com:office:office\"\r\n.*<title>Now SMS</title>|s p/Now SMS http config/ o/Windows/
match http m|^HTTP/1\.1 200 Ok\r\n.*<title>\r\nData Frame - Browser not HTTP 1\.1 compatible\r\n</title>.*Your browser must support HTTP 1\.1 to view iLO web pages\.|s p/HP Integrated Lights-Out http config/ d/remote management/
match http m|^HTTP/1\.0 200 Okay\r\nServer: Optenet CCOTTA ([\w._-]+)\r\nContent-Type: text/html\r\n\r\n<html><head><title>Optenet CCOTTA Status</title>| p/Optenet Mailsecure CCOTTA http config/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\nConnection: close\r\nCache-Control: no-cache\r\nContent-Type: text/html; charset=utf-8\r\n\r\n<html><head><title>Axon</title>| p/Axon VoIP Exchange virtual PBX httpd/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: OctoWebSvr/COM\r\n|s p/SLWebMail Supervisor http config/
match http m|^HTTP/1\.1 200 OK\r\n.*<meta name=\"COPYRIGHT\" content=\"&copy; \d+ Cisco Systems\. All Rights Reserved\.\">.*<title>ACE 4710 DM - Login</title>|s p/Cisco Application Control Engine 4710 DM http config/ d/load balancer/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: ODS/([\w._-]+)\r\n| p|Apple ODS DVD/CD Sharing Agent httpd| v/$1/
match http m|^HTTP/1\.1 404 Not Found\r\nServer: ODS/([\w._-]+)\r\n| p|Apple ODS DVD/CD Sharing Agent httpd| v/$1/
match http m|^HTTP/1\.1 302 Found\r\nDate: .*\r\nServer: CompaqHTTPServer/([\d.]+) HP System Management Homepage/([\d.]+) httpd/([\w.+]+)\r\n| p/CompaqHTTPServer/ v/$1/ i/HP System Management $2; httpd $3/
match http m|^HTTP/1\.1 401 N/A\r\nServer: Router\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"PENTAGRAM Cerberus ([^"]*)\"\r\n| p/Pentagram Cerberus $1 WAP http config/ d/WAP/
match http m|^HTTP/1\.0 302 Document Follows\r\nLocation: http:///index\.html\r\nConnection: close\r\n\r\n| p/Crestron PRO2 automation system web server/ o/2-Series/ d/specialized/
match http m|^HTTP/1\.1 200 Document Follows\r\n.*<META content=\"text/html; charset=windows-1252\" http-equiv=Content-Type>\n<meta NAME=\"AUTHOR\" CONTENT=\"TANDBERG ASA \(http://www\.tandberg\.net\)\">\n|s p/Tandberg 2500 video conferencing http config/ d/webcam/
match http m|^HTTP/1\.0 401 Unauthorized\r\nPragma: no-cache\r\nWWW-Authenticate: Digest realm=\"[^"]*\", domain=\"/\", nonce=\"[0-9a-f]{10}\", algorithm=\"MD5\", qop=\"auth\"\r\nWWW-Authenticate: Basic realm=\"rut-nort-vc02\"\r\nContent-Type: text/html\r\nContent-Length: 236\r\n\r\n| p/Tandberg 3000 MXP video conferencing http config/ d/webcam/
match http m|^HTTP/1\.0 200 Ok\r\nContent-Type: text/html\r\nServer: httpd\r\n.*<title>Router - Info</title>\n\n|s p/DD-WRT milli_httpd/ o/Linux/ d/WAP/
match http m|^HTTP/1\.1 200 OK\r\n.*<title>BitTorrent Download Manager</title>\r\n|s p/BitTorrent Download Manager httpd/
match http m|^HTTP/1\.0 302 Redirect\r\nServer: GoAhead-Webs\r\n.*Location: https?://vxtarget/esm_loginMain\.htm\r\n\r\n|s p/GoAhead-Webs/ i/Mitel 3300 PBX controller/ d/PBX/
match http m|^HTTP/1\.1 302 Redirect\r\nServer: GoAhead-Webs\r\n.*Location: https?://3100icp/esm_loginMain\.asp\r\n\r\n|s p/GoAhead-Webs/ i/Mitel 3100 PBX controller/ d/PBX/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: Grandstream (\w+) ([\d.]+)\r\n|s p/Grandstream $1 http config/ v/$2/
match http m|^HTTP/1\.0 401 Login failed!\r\nServer: micro_httpd\r\n.*WWW-Authenticate: Basic realm=\"WRT54GX4\"\r\n|s p/micro_httpd/ i/WRT54GX4 WAP config/ d/WAP/
match http m|^HTTP/1\.1 302 Found\r\n.*Server: SAP J2EE Engine/([\d.]+)\r\n|s p/SAP J2EE Engine httpd/ v/$1/ i/SAP NetWeaver/
match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/([\d.]+)\r\n.*<TITLE>Versalink</TITLE>.*\"window\.location\.href = 'homeSumBS\.htm'\"|s p/RapidLogic/ v/$1/ i/Westell Versalink model C90-327W30-06 WAP http config/ d/WAP/
match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/([\d.]+)\r\n.*<TITLE>VBrick Integrated Web Server \(IWS\) Login</TITLE>|s p/RapidLogic/ v/$1/ i/VBrick 4300 video encoder http config/ d/media device/
match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/([\d.]+)\r\nMIME-version: 1\.0\r\nPragma: no-cache\r\nContent-type: text/html\r\n\r\n<script language=\"javascript\">\n<!--\ntop\.location\.href=\"default\.htm\";//-->\n</script>\n\r\n$| p/RapidLogic/ v/$1/ i/3Com 3CRWE454G75 WAP http config/ d/WAP/
match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/([\d.]+)\r\nMIME-version: 1\.0\r\nContent-type: text/html\r\n\r\n<html><head><meta http-equiv='Content-Type' content='text/html; charset=iso8859-1'><META http-equiv=Refresh content=\"0; URL=https://[\d.]+/\"></head><body bgcolor=#FFFFFF></body></html>\r\n$| p/RapidLogic/ v/$1/ i/Netgear WAG102 WAP http config/ d/WAP/
match http m|^HTTP/1\.0 302 Moved Temporarily\r\nServer: RapidLogic/([\d.]+)\r\nMIME-version: 1\.0\r\nContent-type: text/html; charset=UTF-8\r\nPragma: no-cache\r\nCache-Control: no-cache\r\nLocation: /main\.html\r\n\r\n\r\n$| p/RapidLogic/ v/$1/ i/Sharp MX-2700N printer/ d/printer/
match http m|^HTTP/1\.1 404 Not Found\r\nConnection: close\r\nServer: ZING-(\d+/[\d.]+) \([0-9a-f]{32}; [\w-]+\) ([^\r\n]*)\r\n\r\n$| p/ZING httpd/ v/$1/ i/SanDisk Sansa Connect MP3 player; $2/ d/media device/
match http m|^HTTP/1\.0 503 Service Unavailable\r\nContent-Type: text/html\r\nContent-Length: 169\r\n\r\n<html><head><title>503 Service Unavailable</title></head><body><h1>503 Service Unavailable</h1><p>The service is not available\. Please try again later\.</p></body></html>$| p/Alcatel-Lucent OmniPCX PBX httpd/ d/PBX/
match http m|^HTTP/1\.0 301 Moved Permanently \r\nContent-Type: text/html\r\nDate: .*\r\nLocation: /fusionreactor/\r\n\r\nRedirecting, please wait\.$| p/FusionReactor web server monitor/
match http m|^HTTP/1\.0 401 Authorization Required\r\nServer: wgt_http ([\d.]+)\r\nWWW-Authenticate: Basic realm=\"Anlage\"\r\nConnection: close\r\n$| p/wgt_http/ v/$1/ i/Eumex 704PC ADSL router/ d/broadband router/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: Alvarion-Webs\r\nDate: THU JAN 01 01:04:22 1970\r\nWWW-Authenticate: Basic realm=\"Alvarion\"\r\n.*<html><head><title>Document Error: Unauthorized</title></head>\r\n\t\t<body><h2>Access Error: Unauthorized</h2>\r\n\t\t<p>Access to this document requires a User ID</p></body></html>\r\n\r\n$|s p/Alvarion-Webs/ i/Alvarion BreezeMAX WiMAX WAP http config/ d/WAP/
match http m|^HTTP/1\.0 400 Bad Request\r\nPragma: no-cache\r\nContent-type: text/html\r\n\r\n<html>\n  <head>\n  <title>400 Bad Request !!!</title>| p/DrayTek Vigor 2800-series ADSL router httpd/ d/broadband router/
match http m|^HTTP/1\.0 200 ;OK\r\nServer: \?\?\?\?\?\?\?\?\?\?\?\?\?\?\r\nContent-Type: text/html\r\nConnection: Close\r\n\r\n<HTML>\n<TITLE>Jacarta interSeptor\n</TITLE>| p/Jacarta interSeptor environmental monitor http/ d/specialized/
match http m|^HTTP/1\.0 302 Document Follows\r\nLocation: http:///index\.htm\r\nConnection: close\r\n\r\n| p/Dell PowerVault TL4000 http config/ d/storage-misc/
match http m|^HTTP/1\.0 302 Found\r\nConnection: close\r\nCache-Control: no-cache\r\nPragma: no-cache\r\nExpires: -1\r\nLocation: https?://[\d.]+/login\.htm\r\n\r\n.*Click <a href=\"https?://[\d.]+/login\.htm\">Here</a> to proceed\.\n|s p/3Com Baseline Switch 2948-SFP Plus web config/ d/switch/
match http m|^HTTP/1\.0 401 Unauthorized\.\r\nWWW-Authenticate: Basic realm=\"GAI-Tronics\"\r\nContent-Type: text/html\r\n\r\n<HTML><HEAD><TITLE>401 Unauthorized\.</TITLE>\r\n</HEAD><BODY>\r\n<H1>401 Unauthorized</H1>The requested URL / requires authorization\.<P>\r\n<HR>\r\n</BODY></HTML>\r\n$| p/GAI-Tronics Commander VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.1 404 Not Found\r\nContent-Length: 0\r\nServer: HBHTTP POGOPLUG - ([\d.]+) - Linux\r\nDate: .*\r\n\r\n$| p/HBHTTP/ i/Pogoplug NAS device/ o/Linux/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\nDate: .*\r\nExpires: Thu, 26 Oct 1995 00:00:00 GMT\r\n.*Server: Allegro-Software-RomPager/([\d.]+)\r\n.*<title>Emerson Network Power IntelliSlot Web/(\d+) Card</title>|s p/Allegro RomPager/ v/$1/ i|Emerson Network Power IntelliSlot Web/$2 card| d/power-device/
match http m|^HTTP/1\.1 301 Moved Permanently\r\nDate: .*\r\nLocation: https://e([\w.]+)/?\r\nConnection: close\r\nContent-Length: 0\r\n\r\n|s p/VMware Server 2 http config/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\nServer: WindWeb/([\d.]+)\r\nDate: .*\r\nContent-Type: text/html\r\nWWW-Authenticate: Basic realm=\"HP\"\r\n.*<script language=\"JavaScript\" src=\"/js/module_utils\.js\"></script>\r\n<script language=\"JavaScript\" src=\"/js/branding_utils\.js\">|s p/WindWeb httpd/ v/$1/ i/HP E1200 storage http config/ d/storage-misc/
match http m|^HTTP/1\.0 200 OK\nServer: Dave Solin's Web Daemon v\. ([\d.]+)\n.*window\.location = '/servlets/com\.marimba\.servlets\.TunerAdmin';\r\n|s p/Dave Solin's Web Daemon/ v/$1/ i/BMC HTTP service/
# Date in fingerprint was "\xd0\xa4\xaf\*\$\x99@".
match http m|^HTTP/1\.0 200 Output Follows\nServer: Apache Embedded Server\nDate: .......\n.*<title>NewCS Management Console\.\.</title>|s p/NewCS satellite card sharing system http config/ d/media device/
match http m|^HTTP/1\.0 200 Output Follows\nServer: Apache Embedded Server\nDate: \nConnection: close\nContent-Type: text/html\n\n<html>\r\n<head>\r\n<title>NewCS Management Console\.\.</title>|s p/NewCS satellite card sharing system http config/ d/media device/
match http m|^HTTP/1\.1 200 OK\r\n.*<TITLE>CCcam info pages</TITLE><BODY><H2>Welcome to CCcam ([\d.]+) server </H2>|s p/CCcam card sharing system http config/
match http m|^HTTP/1\.1 401 Authorization Required\r\nWWW-Authenticate: Basic realm=\"CCcam Server\"\r\n.*<TITLE>CCcam info pages</TITLE>|s p/CCcam card sharing system http config/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: MacHTTP/([\d.]+)\r\n|s p/MacHTTP/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*\r\nServer: Wub ([\d.]+)\r\ncontent-type: text/html; charset=utf-8\r\ncache-control: no-store, no-cache, must-revalidate, max-age=0, post-check=0, pre-check=0\r\nexpires: Sun, 01 Jul 2005 00:00:00 GMT\r\n| p/Wub/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\n.*<TITLE></TITLE>\r\n.*<meta http-equiv=\"refresh\" content=\"0; URL=/wcd/js_error\.xml\">\r\n|s p/Konica Minolta PageScope Web Connection httpd/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: sw-cp-server/([\d.]+)\r\n.*<script language=\"javascript\" type=\"text/javascript\" src=\"/javascript/common\.js\?plesk_version=([\w.-]+)\"/>|s p/sw-cp-server httpd/ v/$1/ i/Parallels Plesk WebAdmin version $2/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: sw-cp-server\r\n.*<script language=\"javascript\" type=\"text/javascript\" src=\"/javascript/common\.js\?plesk_version=([\w._-]+)\"/>|s p/sw-cp-server httpd/ i/Parallels Plesk WebAdmin version $1/
match http m|^HTTP/1\.0 500 Internal Server Error\r\nConnection: close\r\nX-UA-Compatible: IE=EmulateIE7\r\n.*P3P: CP=\"NON COR CURa ADMa OUR NOR UNI COM NAV STA\"\r\n.*Server: sw-cp-server\r\n|s p/sw-cp-server httpd/ i/Parallels Plesk WebAdmin/
match http m|^HTTP/1\.0 200 OK\r\n.*<title>Web-Thermograph</title>\r\n|s p/W&T Web-Thermograph http config/ i|firmware 1.50/1.30| o/specialized/
match http m|^HTTP/1\.0 200 OK\r\n.*<title>Web-Thermograph NTC, 10/100BT, 12-24V</title>\r\n|s p/W&T Web-Thermograph NTC http config/ i|firmware 1.53| o/specialized/
match http m|^HTTP/1\.1 200 OK\r\nStatus:200 OK\r\n.*Server: RMC Webserver ([\d.]+)\r\n.*<TITLE>VTM</TITLE>|s p/RMC Webserver/ v/$1/ i/Stratus ftServer VTM/ d/remote management/
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Digest realm=\"ActiontecBHR\"| p/Actiontec TR069 remote access/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: RemoteSupportManager/([\d.]+)\r\n.*<title>Remote Support Manager</title>|s p/RemoteSupportManager/ v/$1/ i/n-able remote management/
match http m|^HTTP/1\.1 200 OK\r\n.*location\.href=\"DE1100u\.html\";\r\n|s p/Ricoh Aficio MP C4000 http config/ d/printer/
match http m|^HTTP/1\.1 302 Found\r\n.*Server: Vernier/([\d.]+)\r\n.*Location: https://[\d.]+:447/\r\n|s p/Vernier Networks Access Manager http config/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: text/html\n\n<html>\r\n<head>\r\n<title></title>\r\n<meta http-equiv=\"Content-Type\" content=\"text/html; charset=windows-1252\">\r\n<style type=\"text/css\">\r\n<!--\r\n\.leftLink {|s p/Belkin F5D76324 WAP http config/ d/WAP/
match http m|^HTTP/1\.1  200 OK\r\nConnection: close\r\nContent-Type: text/xml; charset=utf-8\r\n\r\n.*<p:ModelDescription>SMC ([\w-]+)</p:ModelDescription>.*<p:FirmwareVersion>([\d., ]+)</p:FirmwareVersion>| p/SMC $1 WAP http config/ i/firmware version $2/
match http m|^HTTP/1\.1 200 OK\nContent-type: text/html; charset=utf-8\r\nServer: WebCit ([\d.]+) / Citadel ([\d.]+)\n| p/WebCit/ v/$1/ i/Citadel $2/
match http m|^HTTP/1\.1 200 OK\nContent-type: text/html; charset=utf-8\r\nServer: WebCit v([\d.]+) / \n| p/WebCit/ v/$1/ i/Citadel/
match http m|^HTTP/1\.0 200 OK\r\nConnection: Close\r\nDate: .*\r\nServer: HTTP/1\.1 compliant\r\n.*<!--\n \*\n \* File: index\.html\n \*\n \* Rajat Hingad rhingad@cisco\.com\n \*\n \* Copyright \(c\) 2001, 2002, 2003, 2004 by Cisco Systems, Inc\.\n \* All rights reserved\.\n \*\n \* This file calls the idm\.jnlp of the PDM\.\n \*\n \*-->\n\n<html>\n<head>\n <meta http-equiv=\"Refresh\" content=\"1; URL=idm/index\.html\">\n</head>\n$|s p/Cisco IPS Device Manager (IDM)/ d/security-misc/
match http m|^HTTP/1\.0  401 Unauthorized \r\nContent-type: text/html \r\nWWW-Authenticate: Basic realm=\"ULTAMUS RAID manager\"\r\n\r\n| p/Overland Storage Ultamus RAID manager/ d/storage-misc/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: text/html\r\n\r\n.*background:url\(data:image/gif;base64,R0lGODdhAQAeAIQeAJub/5yc/6Cf/6Oj/6am/6qq/66u/7Gx/7S0/7i4/7u8/7\+//8LD/8bG/8nK/83N/9HQ/9TU/9fX/9va/97e/\+Lh/\+Xl/\+no/\+3t//Dw//Pz//b3//v7//7\+/////////ywAAAAAAQAeAAAFGCAQCANRGAeSKAvTOA8USRNVWReWaRvXhQA7\)|s p/streamdev VDR plugin/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: Tntnet/([\d.]+)\r\n.*Set-Cookie: tntnet\.=\"[0-9a-f]+\"; Path=\"/\"; Version=\"1\"\r\n\r\n.*<title>VDR-Live - Anmelden</title>|s p/Tntnet/ v/$1/ i/LIVE VDR http config/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: Conexant-EmWeb/R([\d_]+)\r\n| p/Conexant-EmWeb/ v/$SUBST(1,"_",".")/
match http m|^HTTP/1\.0 200 OK\r\nExpires: 0\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<html>\n<title>Login</title>\n.*<font class=tdBigTitle>Connect to 192\.168\.0\.200</font>\n|s p/D-Link DGS-1224T switch http config/ d/switch/
match http m|^HTTP/1\.1 200 OK\r\n.*<meta name=\"Author\" content=\"FireBrick Ltd\">\n<meta name=\"Description\" content=\"FireBrick (\d+) Control pages\">|s p/FireBrick $1 firewall http config/ d/firewall/
match http m|^HTTP/1\.1 200 OK\r\n.*Date: Wed, 31 Dec 1969 15:00:00 GMT\r\n.*Last-Modified: Wed, 31 Dec 1969 15:00:00 GMT\r\n.*<title>PROJECTOR NETWORK SETTINGS</title>.*<!--\nvar mac=\"([0-9A-F]{12})\";\n.*var vMdl=\"(\w+)_Series\";\nvar vVer=\"([\d.]+)\";|s p/NEC $2 series projector http config/ d/media device/ i/firmware version $3; MAC $1/
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: EdgePrism/([\d.]+)\r\n.*Connection: close\r\n\r\n\n\n|s p/EdgePrism/ v/$1/ i/Limelight Networks Content Delivery Network/
match http m|^HTTP/1\.1 200 Ok\r\nServer: micro_httpd\r\n.*<TITLE>DSL-(\w+)</TITLE>.*var hostname = \"([\w_.-]+)\";\r\nvar FWTmp = \"(V[\w.]+)\"\.split\(\"_\"\);|s p/micro_httpd/ i/D-Link DSL-$1 ADSL router http config; firmware $3/ d/broadband router/ h/$2/
match http m|^HTTP/1\.0 200 OK\r\ndate: .*\r\ncontent-type: text/html\r\nconnection: close\r\nserver: Lenel Embedded Web Server/([\d.]+)\r\n\r\n| p/Lenel Embedded Web Server/ v/$1/ i/OnGuard 2008 security system management/ d/security-misc/
match http m|^HTTP/1\.1 200 Document follows\r\nConnection: Close\r\nServer: Micro-Web\r\nContent-type: text/html\r\nLast-modified: .*\r\nContent-length: 476\r\n\r\n$| p/Micro-Web/ i|Symantec Firewall/VPN 200| d/firewall/
match http m|^HTTP/1\.0 401 Unauthorized\r\n.*Server: \r\n.*WWW-Authenticate: Basic realm=\"System\"\r\n.*<HTML><HEAD><TITLE>401 Unauthorized</TITLE></HEAD>\n<BODY><H1>401 Unauthorized</H1>\nYour client does not have permission to get URL / from this server\.\n</BODY></HTML>\n$|s p/Edgewater Networks Edgemarc 4562 VoIP gateway web config/ d/VoIP adapter/
match http m|^HTTP/1\.1 401 Unauthorized\r\n.*WWW-Authenticate: Basic realm=\"server\r\n.*<HTML><HEAD><TITLE>401 Unauthorized</TITLE></HEAD>\n<BODY><H1>401 Unauthorized</H1>\nYour client does not have permission to get URL / from this server\.\n</BODY></HTML>\n$|s p/DVR Systems webcam http interface/ d/webcam/
match http m|^HTTP/1\.1 204 No Content\nServer: PRS\nDate: .*\n\n$| p/Alcatel-Lucent OmniTouch Unified Communication VoIP gateway/ d/PBX/
match http m|^<html>\n<title>USRobotics 10/100/1000 Mbps 48-Port Smart Switch Login</title>.*<td>&nbsp; System Name\n<td>&nbsp; ([\w-]+)\n.*<td>&nbsp; Location Name\n<td>&nbsp; ([\w -]+)\n|s p/USRobotics USR997748 switch http config/ h/$1/ i/location: $2/
match http m|^HTTP/1\.1 401 Authorization Required\nDate: .*\r\nWWW-Authenticate: Basic realm=\"AddPac\"\nContent-Length: 72\n\n<HTML><BODY>You must be authenticated to use this service</BODY></HTML>\n$| p/AddPac AP200B VoIP gateway http config/ d/VoIP adapter/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: NAShttpd\r\n.*WWW-Authenticate: Basic realm=\"Default ([\w._-]+:[\w._-]+)\"\r\n|s p/NAShttpd/ i/default login: $1/
match http m|^HTTP/1\.0 200 OK\r\nDate: .*\r\nServer: Embedded HTTP Server\.\r\n.*<meta http-equiv=\"refresh\" content=\"0; URL=/scgi-bin/index\.htm\">|s p/Embedded HTTP Server/ i/Netgear ProSafe FVS336G firewall http config/ d/firewall/
match http m|^HTTP/1\.0 200 OK\r\nDate: .*\r\nServer: Embedded HTTP Server\.\r\n.*<meta http-equiv=\"refresh\" content=\"0; URL=/cgi-bin/welcome\.cgi\">|s p/Embedded HTTP Server/ i/Linksys RVL200 VPN router http config/ d/router/
match http m|^HTTP/1\.1 200 OK\r\n.*if \(needToConfirm\) {\r\n return \"Leaving this page will end the remote help session\";\r\n} else {\r\nneedToConfirm = true;\r\n}\r\n}\r\n</script>|s p/SimpleHelp remote desktop httpd/
match http m|^HTTP/1\.0 302 Object Moved\r\n.*Location: /\+CSCOE\+/logon\.html\r\nSet-Cookie: tg=; expires=Thu, 01 Jan 1970 22:00:00 GMT; path=/; secure\r\n|s p/Cisco ASA firewall http config/ d/firewall/
match http m|^HTTP/1\.0 302 Moved Temporarily\r\n.*Server: Mbedthis-Appweb/([\d.]+)\r\n.*Set-Cookie: _appwebSessionId_=|s p/Mbedthis-Appweb/ v/$1/ i/Iomega StorCenter ix2 NAS device/ d/storage-misc/
match http m|^HTTP/1\.0 302 Moved Temporarily\r\nContent-Type: text/html\r\nLocation: /EnterpriseController\r\n| p/GoogleMini search appliance httpd/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: micro_httpd\r\n.*WWW-Authenticate: Basic realm=\"Huawei SmartAX (\w+)\"\r\n|s p/micro_httpd/ i/Huawei SmartAX $1 ADSL router http config/ d/broadband router/
match http m|^HTTP/1\.0 200 OK Content-type: text/html\r\n\r\n.*<H2>57066 Minolta Network Configuration Sheet 1 of 2\n\n</H2>.*Serial Number: *(\d+)\n.*Ethernet Address: *([0-9A-F.]+).*F/W Version: *([\w.]+ \(\w+\)).*Print Server Name: *([\w_.-]+)|s p/Minolta PagePro 20 printer http config/ d/printer/ i/serial number: $1, MAC: $2, firmware $3/ h/$4/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"(DCS-\w+)\"\r\n.*Server: WIC-2300\r\n|s p/D-Link $1 webcam http config/ d/webcam/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"(DCS-\w+)\"\r\n.*Server: DCS-\w+\r\n|s p/D-Link $1 webcam http config/ d/webcam/
match http m|^HTTP/1\.0 401 Authorization Required\r\nWWW-Authenticate: BASIC realm=(DCS-\w+)\r\n\r\nPassword Error\. $| p/D-Link $1 webcam http config/ d/webcam/
match http m|^HTTP/1\.0 400 bad url /\r\nServer: TinyHTTPProxy/([\d.]+) ([^\r\n]+)\r\n| p/TinyHTTPProxy/ v/$1/ i/$2/
match http m|^HTTP/1\.1 400 Bad Request\r\nContent-Type: text/html; charset=utf-8\r\nConnection: close\r\nPragma: no-cache\r\nCache-Control: no-store\r\nExpires: -1\r\n.*<script src=\"/dana-na/css/ds\.js\"></script>|s p/Juniper SA2000 or SA4000 VPN gateway http config/ d/proxy server/
match http m|^HTTP/1\.0 200 OK\r\nConnection: Close\r\nContent-Type: text/html\r\nDate: Tue, 28 Jul 2009 12:43:48 GMT\r\n\r\n<html xml:lang=\"en\" xmlns=\"http://www\.w3\.org/1999/xhtml\">\r\n<head>\r\n<meta http-equiv=\"Content-Type\" content=\"text/html; charset=utf-8\" />\r\n<title>FMS : Freenet Message System</title>| p/Freenet Message System web client/
match http m|^HTTP/1\.1 400 Bad Request\r\n.*Server: Profense\r\n|s p/Profense web application firewall/ d/firewall/
match http m|^HTTP/1\.0 200 Ok\r\nServer: NET-DK/([\d.]+)\r\n.*<title>Touchstone Status</title>|s p/NET-DK/ v/$1/ i/Arris Touchstone TM702B VoIP modem/ d/VoIP adapter/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: MediaBox HTTPd Server/([\d.]+) \(Unix\)\r\n|s p/MediaBox HTTPd Server/ v/$1/ o/Unix/
match http m|^HTTP/1\.1 200 OK\r\nServer: cab/([\d.]+) \(([^)]+)\)\r\n.*<TITLE>cab AdminApplet</TITLE>|s p/cab/ v/$1/ i/AdminApplet $2/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\n\r\n<head><meta http-equiv=\"content-type\" content=\"text/html; charset=utf-8\" /><title>Everything</title>| p/voidtools Everything search engine httpd/ o/Windows/
match http m|^HTTP/1\.1 200 OK\r\n.*Set-Cookie: sessionId=.*<HTML>\n<HEAD>\n\n<TITLE>Cisco Systems Login</TITLE>\n|s p/Cisco 4400 wireless LAN controller httpd/ d/remote management/
match http m|^HTTP/1\.0 200 OK\r\n.*<title>:: ThinStation ::</title>.*<h2>Thinstation ([\w._-]+) on ([\w._-]+) :: Main page</h2>|s p/ThinStation http admin/ v/$1/ o/Linux/ h/$2/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: \r\n.*WWW-Authenticate: Basic realm=\"ADSL Router \(ANNEX B\)\"\r\n.*<meta HTTP-EQUIV=\"Expires\" CONTENT=\"Mon, 06 Jan 1990 00:00:01 GMT\">.*<meta name=\"description\" content=\"806GA M 2073\">|s p/Allnet ALL0277DSL ADSL router http config/ d/broadband router/
match http m|^HTTP/1\.1 301 Moved Permanently\r\nDate: .*\r\nLocation: https://([\w._-]+)/\r\nConnection: close\r\nContent-Type: text/html\r\nContent-Length: 56\r\n\r\n<HTML><BODY><H1>301 Moved Permanently</H1></BODY></HTML>$| p/VMware ESXi 4.0 Server httpd/ h/$1/
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"PCS-1 Web Control\"\r\n.*Server: Allegro-Software-RomPager/([\d.]+)\r\n|s p/Allegro RomPager/ v/$1/ i/Sony PCS-1 video conferencing http config/ d/webcam/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: Ubicom/([\d.]+)\r\n.*<title>D-Link Gaming Router :\r\n\t\t Login\r\n\t</title>|s p/Ubicom/ v/$1/ i/D-Link DGL-4500 WAP http config/ d/WAP/
match http m|^HTTP/1\.1 307 Temporary Redirect\r\nConnection: keep-alive,close\r\n.*Location: http://([\w._-]+)/servlet/StartServlet\r\nServer: PEWG/([\d.]+)\r\n|s p/PEWG/ v/$2/ h/$1/ i/OCE print server/ d/print server/
match http m|^HTTP/1\.1 401 Authorization Required\r\n.*www-authenticate:Basic realm=\"(\w+)v(\d+)POE \(([0-9A-F]{12})\)\"\r\n|s p/InterTel $1 VoIP phone http config/ i/firmware $2; MAC $3/ d/VoIP phone/
match http m|^HTTP/1\.1 401 Authorization Required\r\n.*www-authenticate:Basic realm=\"(\d+)i \(([0-9A-F]{12})\)\"\r\n|s p/InterTel $1 VoIP phone http config/ i/MAC $2/
match http m|^HTTP/1\.1 401 Authorization Required\r\n.*www-authenticate:Basic realm=\"IP Resource Card \(IPRC\)\(id=[0-9A-F]+\)\"\r\n|s p/InterTel IPRC VoIP management card/ d/PBX/
match http m|^HTTP/1\.1 200 OK\r\n.*<title>Ethernetov\xfd teplom\xecr TME od Papouch s\.r\.o\.</title>|s p/Papouch TME Ethernet thermometer http interface/
match http m|^HTTP/1\.1 200 OK\r\nServer: SMC Internet Update Manager\r\nConnection: Keep-Alive\r\nContent-Type: text\r\nDate: .*\r\nContent-Length: 61\r\n\r\n<HTML>Avira Internet Update Manager ist betriebsbereit</HTML>$| p/Avira SMC Internet Update Manager/
match http m|^HTTP/1\.1 301 Moved Permanently\r\nDate: .*\r\nLocation: https://([\w._-]+)/\r\nConnection: close\r\nContent-Length: 0\r\n\r\n$| p/VMware ESX 3.5 Server httpd/ h/$1/
match http m|^HTTP/1\.0 200 Ok\r\nServer: httpd\r\n.*<SCRIPT language=Javascript src=\"language_us\.js\"></SCRIPT>.*<SCRIPT>assign_var\(\);</SCRIPT>.*<SCRIPT language=JavaScript src=\"showMenu\.js\"></SCRIPT>.*<SCRIPT>|s p/DD-WRT milli_httpd/ i/Belkin F5D8235-4 WAP http config/ d/WAP/
match http m|^HTTP/1\.1 200 OK\r\n.*<title>MiFi(\d+) Mobile Hotspot</title><meta name=description content=Sprint020>|s p/Novatel MiFi $1 WAP http config/ d/WAP/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: fec/([\w._-]+) \(([^)]+)\)\r\n.*<TITLE>Funkwerk (\w+)-TTextil - Home Page</TITLE>|s p/fec/ v/$1/ i/Funkwerk bintec $3 router; $2/ d/router/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\nServer: fec/([\w._-]+) \(([^)]+)\)\r\n.*Content-Length: 162\r\n.*<title> Configuration </title>\n</head>\n<body onload=\"location\.href='/esi/787100/esi\.cgi\?page=status-index\.xml';\">|s p/fec/ v/$1/ i/Funkwerk bintec R232B router; $2/ d/router/
match http m|^HTTP/1\.1 200 OK\r\n.*Connection: keep-Alive\r\n.*<meta name=description content=VZ018>|s p/Verizon MiFi 2200 E7C5 WAP http config/ d/WAP/
match http m|^HTTP/1\.1 200 OK\n.*<TITLE>IOGEAR MF Print Server</TITLE>|s p/IOGear GMFPSU22W6 print server http config/ d/print server/
match http m|^HTTP/1\.0 401 Unauthorized\r\n.*Server: httpd\r\n.*WWW-Authenticate: Basic realm=\"DD-WRT\"\r\n|s p/DD-WRT milli_httpd/
match http m|^HTTP/1\.0 302 Look here\r\nLocation: /rom/default\.html\r\nContent-Length: 0\r\n\r\n$| p/Intermec P4i label printer http config/ d/printer/
match http m|^HTTP/1\.1 200 OK\r\nConnection: close\r\nDate: .*\d\r\nServer: quark-([\w._-]+)\r\n| p/quark/ v/$1/
match http m|^HTTP/1\.0 302 Redirect\r\nServer: GoAhead-Webs\r\n.*Location: http://([\w._-]+)/login\.asp\r\n|s p/GoAhead-Webs/ i/Sonitrol building access control system http config/ h/$1/
match http m|^HTTP/1\.1 400 Bad Request\r\n.*<P>Your request can't be recognized by Tvants Broadcast Server\. Please visit <A href=\"http://www\.tvants\.com/\">www\.tvants\.com</A> for more information\.</P>|s p/Tvants Broadcast Server httpd/ d/media device/
match http m|^HTTP/1\.0 404 Not Found\r\nSERVER: corega ([\w-]+)\r\nCONTENT-LENGTH: 48\r\nCONTENT-TYPE: text/html\r\n\r\n<html><body><h1>404 Not Found</h1></body></html>$| p/Corega $1 router http config/ d/router/
match http m|^HTTP/1\.0 200 Failed to find service name in request URI and no default service available\r\n.*x-trapeze-fault-response: y\r\n.*Server: Trapeze-Srv/([\d.]+)\r\n.*<SOAP-ENV:Fault rowsetMode=\"struct\" xmlns=\"http://www\.trapezegroup\.com/\"><faultcode tcftype='10'>SOAP-ENV:Client</faultcode><faultstring tcftype='10'>Failed to find service name in request URI and no default service available</faultstring><detail tcftype='10'></detail></SOAP-ENV:Fault>|s p/Trapeze-Srv/ v/$1/ i/Trapeze Mobile Data Terminal SOAP over HTTP/
match http m|^HTTP/1\.0 401 Default login not authorized to perform this action\r\n.*WWW-Authenticate: Basic realm=\"/INOVAS/NovusDFM-trunk-[\w-]+/Config/([\w_.-]+)\"\r\n.*Server: Trapeze-Srv/([\d.]+)\r\n|s p/Trapeze-Srv/ v/$2/ h/$1/ i/Trapeze NOVUS http config/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: Trapeze-Srv/([\d.]+)\r\n.*<TITLE>Trapeze Service Shell response</TITLE>|s p/Trapeze-Srv/ v/$1/ i/Trapeze Service Shell/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: Trapeze-Srv/([\d.]+)\r\n|s p/Trapeze-Srv/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\n.*server: httpd\.js\r\n.*<title>Songbird WebRemote</title>|s p/httpd.js/ i/Songbird WebRemote/
match http m|^HTTP/1\.0 302 Temporary moved\r\nContent-Length: 0\r\nCache-Control: no-cache\r\nPragma: no-cache\r\nConnection: Close\r\nDate: .*\r\nLocation: https:///\r\n\r\n| p/Cisco ASA firewall http config/ d/firewall/
match http m|^HTTP/1\.0 200 OK\r\nServer: Baby Web Server\r\n| p/Baby Web Server/ o/Windows/
# BAIDA by Yandex (yandex.ru).
match http m|^HTTP/1\.1 \d\d\d [^\r\n]*\r\n.*Server: BAIDA/([\w._-]+)\r\n|s p/BAIDA/ v/$1/
match http m|^HTTP/1\.0 401 Unauthorized\r\n.*Server: httpd\r\n.*WWW-Authenticate: Basic realm=\"([^"]+)\"\r\n|s p/DD-WRT milli_httpd/ h/$1/
match http m|^HTTP/1\.0 200 OK\r\n.*<!--- Page\(\d+\)=\[Line Settings\] --->.*<TITLE>Console Alice Access Gateway</TITLE>|s p/Alice Gate 2 WAP http config/ d/WAP/
match http m|^HTTP/1\.0 200 OK\r\n.*Set-Cookie: alice_cookie_session_id=\d+; path=/;\r\n.*<!--- Page\(\d+\)=\[Modem Alice\] --->.*<TITLE>Alice Gate VOIP 2 plus Wi-Fi - Modem Alice</TITLE>|s p/Alice Gate VoIP 2 WAP http config/ d/WAP/
match http m|^HTTP/1\.0 200 OK\r\n.*Set-Cookie: alice_cookie_session_id=\d+; path=/;\r\n.*<!--- Page\(9001\)=\[Stato Modem\] --->.*<TITLE>Alice Gate VOIP 2 plus Wi-Fi - Stato Modem</TITLE>|s p/Alice Gate VoIP 2 WAP http config/ d/WAP/
match http m|^HTTP/1\.0 401 Unauthorized\r\nPragma: no-cache\r\n.*WWW-Authenticate: Basic realm=\"Demo9\"\r\nContent-Type: text/html\r\nContent-Length: 236\r\n\r\n|s p/Tandberg codec T150 http config/ d/VoIP phone/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: OTDAV/([\d.]+)\r\n.*Www-Authenticate: Digest realm=\"Olive Toast WebDAVServer\"|s p/Olive Toast WebDAVServer/ v/$1/ i/OTDAV; iPhone/ d/phone/
match http m|^HTTP/1\.0 302 Moved\r\nServer: HASP LM/([\w._-]+)\r\nDate: .*\r\nLocation: /_int_/index\.html\r\nContent-type: text/html\r\nContent-length: 106\r\n| p/Aladdin HASP license manager/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 403 Forbidden\r\nServer: HASP LM/([\d.]+)\r\nDate: .*\r\nContent-type: text/html\r\nContent-length: 137\r\n\r\n<title>403 Forbidden</title>\n<h1>403 Forbidden</h1>\nAccess to this resource has been denied to you\.\n<p>Please contact the administrator\.\n$| p/Aladdin HASP license manager/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 400 Bad Request\nDate: .*\nServer: HASP Server/([\d.]+) \(MSWin32\)\nContent-Length: 95\nConnection: close\nContent-Type: text/html\n\n<HTML><HEAD><TITLE>400 Bad Request</TITLE></HEAD><BODY><H2>400 - Bad Request</H2></BODY></HTML>$| p/Aladdin HASP license manager/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: Mbedthis-Appweb/([\d.]+)\r\nDate: .*\r\nConnection: close\r\nContent-Type: text/html\r\nContent-length: 130\r\n\r\n<HTML><HEAD><TITLE>Document Error: Bad Request</TITLE></HEAD>\r\n<BODY><H2>Access Error: 400 -- Bad Request</H2>\r\n</BODY></HTML>\r\n\r\n$| p/Mbedthis-Appweb/ v/$1/ i/Dell iDRAC6 http config/ d/remote management/
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: httpd\r\nDate: .*\r\nConnection: close\r\nContent-Type: text/html\r\nContent-length: 130\r\n\r\n<HTML><HEAD><TITLE>Document Error: Bad Request</TITLE></HEAD>\r\n<BODY><H2>Access Error: 400 -- Bad Request</H2>\r\n</BODY></HTML>\r\n\r\n$| p/Mbedthis-Appweb/ i/Dell iDRAC6 http config/ d/remote management/
match http m|^HTTP/1\.0 301 Moved Permanently\r\n.*Server: Mbedthis-Appweb/([\d.]+)\r\n.*Location: https://:443/start\.html\r\n\r\n$|s p/Mbedthis-Appweb/ v/$1/ i/Dell iDRAC6 http config/ d/remote management/
match http m|^HTTP/1\.1 200 Ok\r\nServer: micro_httpd\r\n.*<TITLE>Verizon</TITLE>.*<SCRIPT>\nfunction fnGo\(\)|s p/micro_httpd/ i/Actiontec GT704-WGB ADSL WAP http config/ d/WAP/
match http m|^HTTP/1\.0 200 Ok\r\nServer: micro_httpd\r\n.*<title>Linksys Cable Modem : Status : Modem</title>|s p/micro_httpd/ i/Linksys BEFCMU10 cable modem http config/ d/broadband router/
match http m|^HTTP/1\.1 401 Unauthorized\r\nContent-type: text/html\r\nWWW-Authenticate: Basic realm=\"Netgear\"\r\nConnection: close\r\nPragma: no-cache\r\n\r\n<html><head><title>401 Unauthorized</title>.*<form name=\"RgAuthentication\" action=\"/goform/RgAuthentication\" method=\"POST\">|s p/Netgear CVG834G cable modem http config/ d/broadband router/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: text/html\r\nConnection: close\r\n\r\n.*<title>Hollis</title>.*<td id=b>Indoor</td><td id=c bgcolor=green>([\d.]+)</td><td id=b>&deg;F</td></tr><tr><td id=b>Indoor Set Temp\.</td><td id=c><input type=text name=setTemp size=10 maxlength=10 value=([\d.]+)></td><td id=b>&deg;F&nbsp;<input type=submit name=7 value=\"Apply\"></td></tr><tr><td id=b>Outdoor temp</td><td id=c bgcolor=green>([\d.]+)</td><td id=b>&deg;F</td></tr></table></form></body></html>$| p/ControlByWeb httpd/ i/Temperature (F): indoor $1 (set to $2), outdoor $3/ d/specialized/
match http m|^HTTP/1\.0 200 OK\r\n.*Expires: Thu, 26 Oct 1995 00:00:00 GMT\r\n.*Server: IPC@CHIP\r\n.*<TITLE>IPC@CHIP&reg; Main Page</TITLE>|s p/Beck IPC@CHIP embedded httpd/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: Z-World Rabbit\r\n.*<TITLE>EC3 332 \(Rev\. (\d+)\) Web Configuration and Monitoring</TITLE>|s p/Emerson EC3 332 coldroom controller rev. $1 http config/ d/specialized/
match http m|^HTTP/1\.0 200 OK\r\nServer: http server/everfocus\r\n.*<meta http-equiv=\"refresh\" content=\"0;url=/login\.html\?1600&1\">|s p/Everfocus webcam http config/ d/webcam/
match http m|^HTTP/1\.1 200 OK\r\nServer: Netwave IP Camera\r\n| p/Netwave IP camera http config/ d/webcam/
match http m|^HTTP/1\.1 200 OK\r\n.*<TITLE>&nbsp; &nbsp; &nbsp; ETHM-1 &nbsp; &nbsp; &nbsp; </TITLE>|s p/Satel ETHM-1 alarm control unit/ d/specialized/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: KM-MFP-http/(V[\d.]+)\r\n.*document\.write\('<title>Kyocera Command Center</title>'\);|s p/KM-MFP-http/ v/$1/ i/Kyocera FS-C5300DN or FS-1350DN printer http config/ d/printer/
match http m|^HTTP/1\.0 200 OK\r\n.*Last-Modified: Thu, 01 Jan 1970 00:00:00 GMT\r\n.*Server: dcs-lig-httpd\r\n|s p/D-Link DCS-2121 webcam http config/ d/webcam/
match http m|^HTTP/1\.0 200 OK\r\n.*Date: \d\d\d\d-\d\d-\d\d [^\r\n]*\r\n.*Server: IWeb/([\d.]+)\r\n.*<title>VisionWEB</title>.*<meta name=\"AUTHOR\" content=\"Insignis Technologies\" />.*<meta name=\"DESCRIPTION\" content=\"Linearis VisionWEB\. Cieffe srl, manufactures and markets CCTV digital video recorders and Remote Surveillance products for the security market\" />|s p/IWeb/ v/$1/ i/March Networks VisionWEB webcam http config/ d/webcam/
match http m|^HTTP/1\.1 401 Not Authorized\r\nWWW-Authenticate: Basic realm=\"Communicator Jablotron (\w+)\"\r\n\r\n| p/Jablotron $1 alarm http control/ d/security-misc/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"(ES-\w+) at [^"]*\"\r\n.*Server: Allegro-Software-RomPager/([\w.]+)\r\n|s p/Allegro RomPager/ v/$2/ i/ZyXEL $1 switch http config/ d/switch/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: uhttpd/([\d.]+).*WWW-Authenticate: Basic realm=\"NETGEAR (\w+)\"\r\n|s p/uhttpd/ v/$1/ i/Netgear $2 WAP http config/ d/WAP/
match http m|^HTTP/1\.0 200 HTTP OK\r\nServer: Serv-U/([\d.]+)\r\n| p/Serv-U httpd/ v/$1/
match http m|^HTTP/1\.1 302 Redirection\r\nServer: BlueIris-HTTP/([\d.]+)\r\n| p/BlueIris/ v/$1/
match http m|^HTTP/1\.1 401 Unauthorized\r\n.*WWW-Authenticate: basic realm=\"Protected area\"\r\n.*<title>401 Unauthorized</title>\n.*<!-- Padding: \n        #############################################\n|s p/Breach ModSecurity Apache monitor httpd/
match http m|^HTTP/1\.1 200 OK\r\n.*Set-Cookie: CSPSESSIONID=\d+; path=/;\r\nCACHE-CONTROL: no-cache\r\nCONNECTION: Close\r\n.*<!-- Copyright \(c\) 2002 InterSystems Inc\. ALL RIGHTS RESERVED\. -->.*<b>CSP Error</b>|s p/InterSystems Cache Objects httpd/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: application/octet-stream\r\nCache-Control: no-cache\r\n\r\nOggS| p/VLC media streaming httpd/ i/Ogg/
match http m|^HTTP/1\.0 404 Not Found\r\nConnection: close\r\nContent-Type: text/html; charset=utf-8\r\nContent-Length: 334\r\n\r\n<\?xml version='1\.0'\?>\n<!DOCTYPE html PUBLIC \"-//W3C//DTD XHTML 1\.0 Transitional//EN\" \"http://www\.w3\.org/TR/xhtml1/DTD/xhtml1-transitional\.dtd\">\n<html xmlns=\"http://www\.w3\.org/1999/xhtml\" xml:lang=\"en\" lang=\"en\"><head><meta http-equiv=\"Content-Type\" content=\"text/html; charset=utf-8\"/></head><body><h1>404 Not Found</h1></body></html>$| p/ejabberd http admin/
match http m|^HTTP/1\.0 404 Not Found\r\nConnection: close\r\nContent-Type: text/html; charset=utf-8\r\nContent-Length: 330\r\n\r\n<\?xml version='1\.0'\?>\n<!DOCTYPE html PUBLIC \"-//W3C//DTD XHTML 1\.0 Transitional//EN\" \"http://www\.w3\.org/TR/xhtml1/DTD/xhtml1-transitional\.dtd\">\n<html xmlns='http://www\.w3\.org/1999/xhtml' xml:lang='en' lang='en'><head><meta http-equiv='Content-Type' content='text/html; charset=utf-8'/></head><body><h1>Not found</h1></body></html>$| p/ejabberd http admin/
match http m|^HTTP/1\.1 404 Not Found\r\nServer: Asterisk/([\w._-]+)\r\n| p/Asterisk/ v/$1/ d/PBX/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: SMART Web Server\r\n.*<title>SMART Technologies Connected SMART Interactive Products</title>.*SMART Room: ([\w_.-]+)</H2>|s p/SMART Web Server/ i/SMART Board whiteboard http config/ h/$1/
match http m|^HTTP/1\.1 302 Moved Temporarily\r\n.*Server: Firefly Media Server/([^\r\n]+)\r\n|s p/Firefly Media Server http config/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: AvatronHTTP \(com\.avatron\.AirSharing,([\d.]+)\)\r\n|s p/AvatronHTTP/ v/$1/ i/Air Sharing app/ o/iPhoneOS/ d/phone/
# https://git.torproject.org/checkout/tor/master/doc/spec/dir-spec.txt
match http m|^HTTP/1\.0 503 Directory unavailable\r\n\r\n| p/Tor directory/
# DirPortFrontPage set in torrc.
match http m|^HTTP/1\.0 200 OK\r\nDate: .*\r\nContent-Type: text/html\r\nContent-Encoding: identity\r\nContent-Length: \d+\r\nExpires: .*\r\n\r\n| p/Tor directory/
match http m|^HTTP/1\.1 401 Unauthorized\r\n.*Server: Zarafa iCal Gateway ([^\r\n]+)\r\n|s p/Zarafa iCal Gateway httpd/ v/$1/
match http m|^HTTP/1\.1 302 Moved Temporarily\r\nLocation: https?://([\w._-]+):(\d+)/symantec\.html\r\nContent-Length: 0\r\n| p/Symantec Endpoint Protection httpd/ i|redirect to port $2| h/$1/
match http m|^HTTP/1\.0 200 OK\r\nServer: UOS\r\n.*<title>3Com Log On</title>|s p/3Com X5 Unified Security Platform IPS http config/ d/security-misc/
match http m|^HTTP/1\.0 200 OK\r\nServer: UOS\r\n.*<title>TippingPoint Log On</title>\r\n<meta http-equiv=\"Cache-Control\" content=\"no-store\" />.*<!--\r\n////////////////////////////////////////////\r\n// Copyright TippingPoint 2002, 2003, 2004 and 2005\r\n|s p/HP TippingPoint 110 or 1200E IPS http config/ d/firewall/
match http m|^HTTP/1\.0 200 OK\r\nServer: UOS\r\n.*<title>TippingPoint Log On</title>\n<meta http-equiv=\"Cache-Control\" content=\"no-store\" />.*<!--\n////////////////////////////////////////////\n// Copyright TippingPoint 2002, 2003, 2004 and 2005\n|s p/HP TippingPoint 1200E or 5000E IPS http config/ d/firewall/
match http m|^HTTP/1\.0 200 OK\r\nServer: SpaceMon/([\d.]+)\r\n.*<TITLE>SpaceMon</TITLE>.*SpaceMon Administrator: ([^<]*)<BR>|s p/IPWorx SpaceMon storage monitor httpd/ v/$1/ o/Windows/ i/administrator: $2/
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: CloudFront\r\n| p/CloudFront httpd/
match http m|^HTTP/1\.0 401 Unauthorized\r\n.*WWW-Authenticate: Basic realm=\"Freetz \(([\w._-]+):([\w._-]+)\)\"\r\n.*<HTML><HEAD><TITLE>401 Unauthorized</TITLE></HEAD>\n<BODY><H1>401 Unauthorized</H1>\n\n</BODY></HTML>\n|s p/Busybox httpd/ i/Freetz firmware for AVM FRITZ!Box; login $1:$2/ d/WAP/
match http m|^HTTP/1\.0 401 Unauthorized\r\nContent-type: text/html\r\nAccept-Ranges: bytes\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"GeneralUser/Administrator\"\r\n\r\n<HTML><HEAD><TITLE>401 Unauthorized</TITLE></HEAD>\n<BODY BGCOLOR=\"#cc9999\"><H2>401 Unauthorized</H2>\n<HR>\nAuthorization required for the URL '/'\.\n</BODY></HTML>\n$| p/thttpd/ d/webcam/ i/Panasonic BB-HCM511A Network camera http config/
match http m|^HTTP/1\.0 200 Document follows\r\n.*Server: Unknown\r\n.*<TITLE> Guardian Digital WebTool Login </TITLE>|s p/EnGuarde Linux Guardian Digital Webtool http admin/ o/Linux/
match http m|^HTTP/1\.1 200 OK\r\nServer: Apache\r\nContent-Type: text/html\r\nContent-Length: 3587\r\nConnection: close\r\n\r\n\n<html>\n<head>\n<!-- \n     Copyright \(C\) 2005-2006 Aviv Raff \(with minor modifications by HDM for the MSF module\)\n     From: http://aviv\.raffon\.net/2005/12/11/MozillaUnderestimateVulnerabilityYetAgainPlusOldVulnerabilityNewExploit\.aspx\n     Greets: SkyLined, The Insider and shutdown \n-->| p|Metasploit multi/browser/mozilla_compareto exploit|
match http m|^HTTP1\.1 200 OK\r\nServer: WIBU-SYSTEMS HTTP Server/ Version ([^\r\n]*)\r\n| p/WIBU-SYSTEMS HTTP Server/ v/$1/ i/CodeMeter copy prevention dongle http config/ d/specialized/
match http m|^HTTP/1\.1 401 Unauthorized\r\n.*Server: AppleIDiskServer-([\w._-]+)\r\n.*WWW-Authenticate: Basic realm=\"([\w._-]+)\"\r\n|s p/Apple iDisk Server/ v/$1/ h/$2/ i/online storage access/
match http m|^HTTP/1\.1 401 Unauthorized\n.*Server: ASSP/([^\r\n]+)\n|s p/ASSP (Anti-Spam SMTP Proxy) httpd/ v/$1/
match http m|^HTTP/1\.0 302 Found\r\n.*Location: https://([\w._-]+)/[^\r\n]*\r\n.*<TITLE>Novell iChain</TITLE>|s p/Novell iChain http admin/ o/NetWare/ h/$1/
match http m|^HTTP/1\.0 200 OK\r\n.*Connection: Keep-Alive\r\nKeep-Alive: timeout=5, max=100\r\n.*<HTML>\r\n<HEAD>\r\n<TITLE></TITLE>\r\n<SCRIPT ID=clientEventHandlersJS LANGUAGE=javascript>\r\n<!--\r\nfunction loadpasswd\(\)\r\n{\r\n\ttop\.location = \"index\.htm\"\r\n}\r\nsetTimeout\(\"loadpasswd\(\)\",1\);\r\n//-->\r\n</SCRIPT>\r\n</HEAD>\r\n<BODY>\r\n</BODY>\r\n</HTML>\r\n$|s p/GoldStar iPECS 50B PBX http config/ d/PBX/
match http m|^HTTP/1\.1 200 OK\r\nExpires: Thu, 01 Jan 1970 00:00:00 GMT\r\nSet-Cookie: JSESSIONID=[0-9A-F]+; Path=/; Secure\r\n.*<title>VMware View Portal</title>|s p/VMware View Manager httpd/
match http m|^HTTP/1\.1 403 Forbidden\r\nServer: Norman Security/([\d.]+)\r\nContent-Type: text/html\r\nConnection: Close\r\nContent-Length: 90\r\n\r\n<html><title>Norman Security Error</title><body><br><h2>403 - Forbidden</h2></body></html>$| p/Norman Security Endpoint Protection httpd/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: Norman Security/([\d.]+)\r\n.*<html><title>Norman Security Error</title><body><br><h2>401 - Unauthorized</h2></body></html>$|s p/Norman Security Endpoint Protection httpd/
match http m|^HTTP/1\.1 200 OK\r\n.*<!-- \$Header: index\.html 115\.2 2003/03/18 21:32:39 hfux ship \$ -->.*<TITLE>Oracle Applications Rapid Install</TITLE>|s p/Oracle Rapid Install httpd/
match http m|^HTTP/1\.1 200 OK\r\n.*<script language=\"JavaScript\" src=\"\./en/welcomeRes\.js\"> type=\"text/javascript\">.*<meta name=\"description\" content=\"VMware Converter\">|s p/VMware vCenter Converter 4 httpd/
match http m|^HTTP/1\.1 200 OK\r\nContent-Length: 273\r\nContent-Type: text/html\r\n\r\n<HTML><HEAD><TITLE>Root Index</TITLE></HEAD><BODY><UL><LI><A HREF=\"/ccm-notify\">/ccm-notify</A></LI>\r\n<LI><A HREF=\"/ccm-proxy\">/ccm-proxy</A></LI>\r\n<LI><A HREF=\"/ccm-update\">/ccm-update</A></LI>\r\n<LI><A HREF=\"/config_public/\">/config_public/</A></LI>\r\n</UL></BODY></HTML>\r\n$| p/RSA SecurID 2.0 RADIUS http config/ o/security-misc/
match http m|^HTTP/1\.1 400 Bad Request\r\n.*Server: LapLink ([\d.]+)\r\n|s p/Laplink file transfer httpd/ v/$1/
match http m|^HTTP/1\.0 200 OK\nContent-type: text/html\n\n<HTML>\n<HEAD>\n<TITLE>[\w._-]+ - Hallo!</TITLE>| p/Xrelayd SSL engine httpd/ o/Linux/ i/OpenWrt/
match http m|^HTTP/1\.0 200 OK\r\nServer: jToolkitHTTP/([\w._-]+) Python/([\d.]+)\r\n| p/jToolkit web framework httpd/ v/$1/ i/Python $2/
match http m|^HTTP/1\.0 200 Document follows\r\n.*Server: PureMessage Web Server\r\n|s p/Sophos PureMessage spam filter http interface/
match http m|^HTTP/1\.0 200 OK\r\nServer: iCanWebServer/([\d.]+)\r\n.*<TITLE>Network Camera Viewer</TITLE>|s p/iCanWebServer/ v/$1/ d/webcam/
match http m|^HTTP/1\.1 302 Found\r\nContent-Length: 0\r\nLocation: https://([\w._-]+):(\d+)/zimbra/\r\n\r\n| p/Zimbra http config/ h/$1/ i/redirect to https on port $2/
match http m|^HTTP/1\.0 400 String index out of range: -1\r\nContent-Type: text/html\r\n\r\n$| p/Bluecat Networks Proteus IPAM or Enterasys Dragon IDS http config/ o/Linux/
match http m|^HTTP/1\.1 302 Found\r\ncontent-type: text/html;charset=utf8\r\ncache-control: no-cache\r\ncontent-length: 0\r\nlast-modified: .*\r\ndate: .*\r\nconnection: close\r\nlocation: /login\?continue=%2f\r\n\r\n$| p/Alterator remote management httpd/ o/Linux/
match http m|^HTTP/1\.0 403 Forbidden\r\n.*\r\nServer: Alfred/([\d.]+)\r\n|s p/Alfred RenderMan control httpd/ v/$1/
match http m|^HTTP/1\.0 200 Ok\r\n.*Server: AXIS ThinWizard/v([\d.]+)\r\n|s p/AXIS ThinWizard printer management httpd/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\nServer: <xxxx>\r\nContent-Length: 1057\r\n.*<TITLE>Bad Browser</TITLE>|s p/Siemens HG 1500 router http config/
match http m|^HTTP/1\.1 403 Forbidden\r\n.*Server: Allegro-Software-RomPager/([\d.]+)\r\n.*Correct authorization is required for this area\. Either your browser does not perform authorization, or your authorization has failed\. RomPager server by Digest Access Authentication, which is not supported by your browser\.<P>\nReturn to <A HREF=\"\">last page</A><P>\n\n</BODY>\n</HTML>\n$|s p/AudioCodes Mediant 200 VoIP gateway http config/ d/VoIP adapter/
match http m|^HTTP/1\.1 200 OK\r\nServer: WHC chatroom\r\n| p/Fifi chat server http interface/
match http m|^HTTP/1\.0 200 OK\r\nServer: Xunlei Http Server/([\d.]+)\r\n| p/Xunlei BitTorrent http interface/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\n.*<\?xml version=\"1\.0\" encoding=\"utf-8\"\?>\n<!DOCTYPE html PUBLIC \"-//W3C//DTD XHTML 1\.0 Transitional//EN\" \"http://www\.w3\.org/TR/xhtml1/DTD/xhtml1-transitional\.dtd\">\n<html xmlns=\"http://www\.w3\.org/1999/xhtml\" xmlns:v=\"urn:schemas-microsoft-com:vml\" xml:lang=\"en\" lang=\"en\">\n  <head>\n    <!--\n    ShellInABox - Make command line applications available as AJAX web applications\n|s p/ShellInABox httpd/
match http m|^HTTP/1\.1 400 Bad Request\r\nConnection: close\r\nDate: .*\r\nServer: Java/([-\d_.]+) javax\.wbem\.client\.adapter\.http\.transport\.HttpServerConnection\r\nContent-Length: 0\r\n\r\n| p/Solaris WBEM web management httpd/ i/Java $1/ o/Solaris/
match http m|^HTTP/1\.1 200 OK\r\n.*<TITLE>MGI ZOOM Image Server</TITLE>.*Version: ([^\n]*)\n\t\tBuild: (\d+)<build/><BR>\n|s p/Zoom Image Server httpd/ v/$1 build $2/
match http m|^HTTP/1\.0 200 OK\r\nServer: upshttpd/([\d.]+)\r\n| p/upshttpd/ v/$1/ i/Effekta UPS http config/ d/power-device/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: ZNC ZNC ([\d.]+) - by prozac@rottenboy\.com\r\n| p/ZNC IRC bouncer http config/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: (ZNC )?ZNC ([-\w_.+]+) (by prozac )?- http://znc\.sourceforge\.net\r\n| p/ZNC IRC bounce http config/ v/$2/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: ZNC ([\w_.+-]+) - http://znc\.sourceforge\.net\r\n| p/ZNC IRC bouncer httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: ZNC - http://znc\.sourceforge\.net\r\n| p/ZNC IRC bouncer httpd/ v/0.090 - 0.096/
match http m|^HTTP/1\.0 404 <no description>\r\nDate: .*\r\nServer: XMLD HTTPServer/([\d.]+)\r\n\r\n$| p/XMLD HTTPServer/ v/$1/ i/Citrix XML Service/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: Mono\.WebServer2/([\w._-]+) Unix\r\nX-AspNet-Version: ([\d.]+)\r\n|s p/Mono.WebServer2/ v/$1/ o/Unix/ i/MonoDoc httpd; ASP.NET $2/
match http m|^HTTP/1\.1 401 Unauthorized\r\n.*WWW-Authenticate: Basic realm=\"Cayman-([\w]+)\"\r\n.*Server: Allegro-Software-RomPager/([\d.]+)\r\n| p/Allegro RomPager/ v/$2/ i/Cayman $1 DSL router/ d/broadband router/
match http m|^HTTP/1\.1 200 OK\r\n.*Expires: Thu, 26 Oct 1995 00:00:00 GMT\r\n.*Server: Allegro-Software-RomPager/([\w._-]+)\r\n.*<PRE>\*{60}<BR>\* WARNING ALERT: AUTHORIZED USERS ONLY! +\*<BR>\* +\*<BR>\* All activities conducted on this system may be monitored \*<BR>|s p/Allegro RomPager/ v/$1/ i/NetIron XMR 4000 router http config/ d/router/
match http m|^HTTP/1\.0 401 Unauthorized\r\n.*Server: 2NAS_LIGHT\r\n|s p/2NAS_LIGHT/
match http m|^HTTP/1\.1 400 Bad Request\r\nServer: sfcHttpd\r\nContent-Length: 0\r\n\r\n$| p/sfcHttpd/ i/VMware Studio VAMI CIM broker/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: BLOBJ\.httpd\r\n.*<meta name='generator' content='BLOBJ WE ([\d.]+)'>|s p/BLOBJ.httpd/ i/BLOBJ Web Edition $1/
match http m|^HTTP/1\.1 401 Unauthorized\r\n.*Server: THEO\+Server/([\d.]+)\r\n.*WWW-Authenticate: Basic realm=\"THEOS Web-based Maintenance\"\r\n|s p/THEO+Server/ v/$1/ o/THEOS/ i/THEOS Corona http config/
match http m|^HTTP/1\.0 200 OK\r\nServer: CouchDB/([\w._-]+) \(Erlang ([^)]*)\)\r\n| p/CouchDB httpd/ v/$1/ i/Erlang $2/
match http m|^HTTP/1\.0 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"administrator\"\r\nServer: CouchDB/([\w._-]+) \(Erlang ([^)]*)\)\r\n| p/CouchDB httpd/ v/$1/ i/Erlang $2; unauthorized/
match http m|^HTTP/1\.1 401 Unauthorized\r\n.*Server: Httpd-Webs\r\n.*WWW-Authenticate: Basic realm=\"Linksys (WR[\w+]+) ver\. (\d+)\"\r\n|s p/Linksys $1v$2 WAP http config/ d/WAP/
match http m|^HTTP/1\.1 204 No Content\r\nConnection: close\r\nServer: AChat\r\n\r\n| p/AChat chat system httpd/
match http m|^HTTP/1\.0 200\r\n.*<title>AVTECH Software, Inc\. - TemPageR (\w+) - Real-Time Temperature Monitor For IT &amp; Facilities Environment Monitoring</title>|s p/Avtech TemPageR $1 temperature monitor httpd/
match http m|^HTTP/1\.0 403 Access denied\.  Please consult the http-access directive in the User's Guide for more information\.\r\nContent-Type: text/html\r\n\r\n<html><body>Access denied\.  Please consult the http-access directive in the User's Guide for more information\.</body></html>\r\n$| p/Port25 PowerMTA mail gateway http admin/
match http m|^HTTP/1\.1 302 Found\r\nLocation: https?:///logon\.htm\r\nContent-Length: 0\r\nServer: Intel\(R\) Active Management Technology ([\w._-]+)\r\n\r\n$| p/Intel AMT http admin/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: text/html\r\nPragma: no-cache\r\nCache-Control: no-cache\r\n\r\n<html>\n<head>\n<meta http-equiv=\"Content-type\" content=\"text/html; charset=iso-8859-1\">\n<title>Client Authentication</title>| p|Check Point VPN-1/UTM NGX R70 firewall http admin| d/firewall/
match http m|^HTTP/1\.0 404 Not Found\r\nDate: .*\r\nContent-Type: text/html\r\nConnection: close\r\nContent-Length: 82\r\n\r\n<HEAD><TITLE>404 Not Found</TITLE></HEAD><BODY>unknown uri in pks request</BODY>\r\n$| p/Seahorse http keyserver/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/xml; charset=utf-8: \r\nConnection: close\r\n\r\n.*<ModelName>([^<]*)</ModelName><FirmwareVersion>([^>]*)</FirmwareVersion>|s p/D-Link $1 WAP Home Network Administration Protocol (SOAP over HTTP)/ v/$2/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: KM_HTTP-Server/([\d.]+)\r\n.*<title>Kyocera Command Center</title>|s p/KM_HTTP-Server/ v/$1/ i/Kyocera 4050 printer http config/
match http m|^HTTP/1\.0 200 OK\r\nServer: Apache/0\.6\.5\r\n.*<title>Web Server . Gigaset (\S+) WLAN dsl</title>|s p/Siemens Gigaset $1 WAP http config/ d/WAP/
match http m|^HTTP/1\.0 302 Found\r\nServer: Apache/0\.6\.5\r\n.*Location: /relink_web\.stm|s p/Siemens Gigaset WAP http config/ d/WAP/
match http m|^HTTP/1\.0 200 OK\r\nServer: Apache/0\.6\.5\r\n.*src="top\.stm\?pn1=ho3\.gif&pn2=ad1\.gif"|s p/Philips SNB5600 WAP http config/ d/WAP/
match http m|^HTTP/1\.0 200 OK\r\nServer: Apache/0\.6\.5\r\n.*var PM="BBR-4MG";\n|s p/SMC7908VoWBRA ADSL router http config/ d/broadband router/ 
match http m!^HTTP/1\.[01] 302 .+(Location|LOCATION): .+/UE/welcome_login\.html!s p/Allegro RomPager/ i/Siemens Gigaset SX762 WAP http config/ d/WAP/
match http m|^HTTP/1\.[01] \d\d\d .*\r\n.*<title>Welcome to eDR400--login</title>|s p/EverFocus PowerPlex eDR400 security camera http config/ d/webcam/
match http m|^HTTP/1\.[01] 401 Unauthorized\r\nWWW-Authenticate: Basic realm="NETGEAR (WNR\w+)"\r\n| p/Netgear $1 WAP http config/ d/WAP/
match http m|^HTTP/1\.[01] 302 Redirect\r\nSet-Cookie: CrushAuth=| p/CrushFTP httpd/
match http m|^HTTP/1\.[01] 401 Unauthorized\r\nWWW-Authenticate: Basic realm="(WGR\w+)"\r\n| p/Netgear $1 WAP http config/ d/WAP/
match http m|^HTTP/1\.1 401 Unauthorized\r\n.*Server: NetIXServer \(([\d\.]+)\)\r\n| p/NetIXServer http admin/ v/$1/
match http m|^HTTP/1\.1 401 Unauthorized\nWWW-Authenticate: Digest realm="i3micro VRG", nonce="\d+", qop="auth", algorithm=MD5| p/i3micro VRG VoIP adapter http config/ d/VoIP adapter/
match http m|^HTTP/1\.0 302 Found\r\nLocation: /control/userimage.html\r\n| p/Mobotix Camera http config/ d/webcam/
match http m|^HTTP/1.0 401 Unauthorized\r\nDate: .*\r\nConnection: close\r\nServer: Microsoft-WinCE/5.0\r\nSet-Cookie: .*\r\nWWW-Authenticate: Basic Realm="Kesseltronics"| p/Kesseltronics car wash tunnel http config/ d/specialized/ o/Windows/
match http m|^HTTP/1.0 200\r\nContent-type: text/html\r\nConnection: close\r\nContent-Length: \d+\r\n\r\n<html>\r\n<head><title>BARIX Instreamer| p/Barix Instreamer audio encoder http config/ d/media device/ 
match http m|^HTTP/1.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm="PortServer (TS \w+)"| p/Digi Portserver $1 terminal server http config/ d/terminal server/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: Mbedthis-Appweb/([\w.-]+)\r\n.*\r\n\r\n\n<HTML>\n<HEAD>\n  <META HTTP-EQUIV=\"Refresh\" CONTENT=\"0; URL=/esp/login\.esp\">\n</HEAD>\n<BODY>\n</BODY>\n</HTML>\n\n$|s p/Mbedthis-Appweb/ v/$1/ i/PA-4050 firewall http config/ d/firewall/
match http m|^HTTP/1\.0 400 Bad Request\r\nContent-Type: text/html\r\n\r\n<HTML><HEAD><TITLE>Bad Request</TITLE></HEAD><BODY><h3>Error: Bad HTTP Request</h3></BODY></HTML>$| p/ZoneAlarm Z100G firewall http config/ d/firewall/
match http m|^HTTP/1\.1 200 OK\r\n.*Server:  \r\n.*\r\n\r\n<html>\n<head>\n<title>ZyWALL ([\w -]+)</title>\n|s p/ZyXEL ZyWALL $1 firewall http config/ d/firewall/
match http m|^HTTP/1\.0 401 Unauthorized\r\nServer: ALPHA-WebServer/([\w.]+)\r\n| p/ALPHA-WebServer/ v/$1/
# EqualLogic PeerStorage PS100E iSCSI storage array running firmware v4.1.4.
match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/([\w.]+)\r\n.*<title>vmgrp1 Group Manager</title>\n|s p/RapidLogic/ v/$1/ i/EqualLogic PeerStorage PS100E NAS device/ d/storage-misc/
# EqualLogic PeerStorage PS100E iSCSI storage array running firmware 2.3.6.
match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/([\w.]+)\r\n.*<title>nwkgrp2 Group Manager</title>\n|s p/RapidLogic/ v/$1/ i/EqualLogic PeerStorage PS100E NAS device/ d/storage-misc/
match http m|^HTTP/1\.0 404 Not Found\r\nServer: Content Gateway Manager ([\w._-]+)\r\n| p/Websense Content Gateway Manager http config/ v/$1/
match http m|^HTTP/1\.0 302 Moved Temporarily\r\n.*Set-Cookie: rg_cookie_session_id=\d+; path=/; expires=Fri, 01 Jan 2038 00:00:00 GMT\r\n.*Location: http://[\w._-]+:(\d+)/index\.cgi\?active%5fpage=9069&req%5fmode=0&strip%5fpage%5ftop=0\r\n|s p/Pirelli DRG A125G WAP http config/ d/WAP/ i/redirect to port $1/
match http m|^HTTP/1\.1 200 OK\r\nConnection: close\r\nServer: jDownloader HTTP Server\r\nContent-Type: text/html\r\nContent-Length: 0\r\n\r\n$| p/jDownloader httpd/
match http m|^HTTP/1\.1 200 OK\r\nConnection: close\r\nServer: jDownloader HTTP Server\r\nContent-Type: text/html\r\nContent-Length: 46\r\n\r\nJDRemoteControl - Malformed Request\. use /help$| p/jDownloader httpd/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"JDownloader\"\r\n\r\n$| p/jDownloader httpd/ i/unauthorized/
match http m|^HTTP/1\.0 200 OK\r\nServer: lwIP/([\w._-]+) \(http://www\.sics\.se/~adam/lwip/\)\r\n.*<title>Stellaris&reg; ([\w._-]+) Evaluation Kit</title>|s p/lwIP/ v/$1/ i/Stellaris $2 microcontroller/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\nCache-Control: no-cache\r\nPragma: no-cache\r\nExpires: .*\r\nDate: .*\r\nAccept-Ranges: bytes\r\nConnection: close\r\n\r\n<!--- Page\(\d+\)=\[Ouverture de session\] ---><HTML><HEAD><SCRIPT language=\"Javascript\"><!--\n/\*\n \* A JavaScript implementation of the RSA Data Security, Inc\. MD5 Message\n \* Digest Algorithm, as defined in RFC 1321\.\n \* Version 2\.1 Copyright \(C\) Paul Johnston 1999 - 2002\.\n \* Other contributors: Greg Holt, Andrew Kepert, Ydnar, Lostinet\n \* Distributed under the BSD License\n \* See http://pajhome\.org\.uk/crypt/md5 for more info\.\n \*/\n\n| p/Sagem Livebox WAP http config/ d/WAP/
match http m|^HTTP/1\.0 200 OK\r\n.*<title>Livebox</title>\n\t\t<meta http-equiv=\"content-type\" content=\"text/html; charset=UTF-8\">\n\t\t<meta http-equiv=\"Content-language\" content=\"fr\">\n\t\t<meta name=\"author\" content=\"Nicolas VIVIEN\">\n\t\t<meta name=\"Copyright\" content=\"SAGEM COMMUNICATIONS\">|s p/Sagem Livebox WAP http config/ d/WAP/
match http m|^HTTP/1\.1 301 Moved Permanently\r\nDate: .*\r\nConnection: close\r\nLocation: index\.htm\r\nServer: WMI (V[\w._-]+)\r\n\r\n$| p/WMI/ v/$1/ i/3Com 5500G-EI switch http config/ d/switch/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: W3MFC/([\w._-]+)\r\nAllow: GET, POST, HEAD\r\n.*<TITLE>Lan2net Statistics</TITLE>|s p/W3Mfc/ v/$1/ i/Lan2net firewall http config/ d/firewall/
match http m|^HTTP/1\.0 200 OK\r\n.*Content-Type: text/html;charset=utf-8\r\n.*Mime-Version: 1\.0\r\n.*<title>FRITZ!WLAN Repeater</title>|s p|FRITZ!WLAN Repeater N/G http config| d/WAP/
match http m|^HTTP/1\.1 200 OK\r\n.*Content-Type: text/html; Charset=UTF-8\r\nConnection: close\r\n\r\n<!DOCTYPE html PUBLIC \"-//W3C//DTD HTML 4\.01 Transitional//EN\">\r\n<html><head><title>(.*) - foobar2000</title>|s p/foobar2000 media player httpd/ i/now playing: $1/
match http m|^HTTP/1\.1 301 Redirection\r\nServer: Cegid-WEB-Access-Server/([\w._-]+)\r\n| p/Cegid-WEB-Access-Server/ v/$1/
match http m|^HTTP/1\.1 200 Ok\r\nServer: micro_httpd\r\n.*<html xmlns=\"http://www\.w3\.org/1999/xhtml\" xml:lang=\"it\" lang=\"it\">\n<head>\n\t<title>Vodafone</title>|s p/micro_httpd/ i/Vodafone Station WAP http config/
match http m%^<html>\n<head>\n<title>TRENDnet \| (TEG-\w+) \| Login</title>% p/TRENDnet $1 switch http config/ d/switch/
match http m|^HTTP/1\.1 200 OK\r\nServer: Web Server\r\n.*top\.location\.href = \"/hp_login\.html\";\r\n</script>\r\n\r\n\r\n<BODY style=\"text-align: center\" onload=\"document\.forms\[0\]\.login\.focus\(\);CheckError\(\)\">\r\n<FORM METHOD=\"POST\" ACTION=\"/hp_login\.html\">|s p/HP Procurve 1810G switch http config/ d/switch/
match http m|^HTTP/1\.0 302\r\nLocation: /Portal0000\.htm\r\n.*<HTML><HEAD><TITLE>Error</TITLE></HEAD>\r\n<BODY><CENTER><H2>/<BR><BR>302 : MOVED TEMPORARILY</H2></CENTER></BODY></HTML>$|s p/Siemens SIMATIC S7-300 PLC controller httpd/ d/specialized/
match http m|^HTTP/1\.0 401 Unauthorized\r\nContent-Type: text/html\r\nWWW-Authenticate: Basic realm=\"Web Management\"\r\n\r\n<html><title>401 Unauthorized</title><body>401 Unauthorized</body></html>$| p/Foundry EdgeIron switch http config/ d/switch/
match http m|^HTTP/1\.1 404 Not Found\r\nConnection: Close\r\nContent-Type: text/html\r\n\r\nThe specified URL cannot be found<!--(?:0123456789){50}01234-->\r\n| p/Barracuda Web Application Firewall/ d/firewall/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\nContent-Type: text/html\r\nSet-Cookie: DLILPC=\"\"; Version=1; Max-Age=0; Path=/\r\n\r\n.*<title>Power Controller </title>\n \n<script language=\"javascript\" src=\"/md5\.js\"></script>|s p/Digital Loggers Web Power Switch II http config/ d/power-device/
match http m|^HTTP/1\.1 403 Directory Listing Denied\r\nContent-Type: text/plain\r\nContent-Length: 12\r\n\r\nError: 403\r\n$| p/HP Dream Screen media player http config/ d/media device/
match http m|^HTTP/1\.0 200 OK\r\nX-Powered-By: PHP/([\w._-]+)\r\n.*<title>Seagate NAS - ([\w._-]+)</title>\n<link rel=\"stylesheet\" type=\"text/css\" href=\"/admin/layout_design\.css\" />\n|s p/Seagate Black Armor 440 NAS http config/ h/$2/ i/PHP $1/
match http m|^HTTP/1\.0 200 OK\r\nX-Powered-By: PHP/([\w._-]+)\r\n.*<title>My Book World Edition - ([\w._-]+)</title>\n.*<!-- Framework CSS -->\n<link rel=\"stylesheet\" href=\"/blueprint/screen\.css\" type=\"text/css\" media=\"screen, projection\">|s p/Western Digital My Book http config/ h/$2/ i/PHP $1/ d/storage-misc/
match http m|^HTTP/1\.1 302 Found\r\n.*Location: https://([\w._-]+)/site-web/home\.seam\r\n|s p/Seam web framework/ h/$1/
match http m|^HTTP/1\.0 200 OK\r\n.*<TITLE>Print server homepage</TITLE></HEAD>\n<FRAMESET COLS=\"200,\*\" BORDER=0 FRAMEBORDER=0>\n<FRAME SRC=\"/links_en\.html\">\n|s p/Citizen CLP-521 or Kyocera Mita KM-1530 printer http config/ d/printer/
match http m|^HTTP/1\.1 404 Not Found\r\nContent-Length: 19\r\nContent-Type: text/html\r\n\r\n 404 Page Not Found$| p/Kyocera Mita FS-1350DN printer http config/ d/printer/
match http m|^HTTP/1\.0 401 Unauthorized\r\n.*WWW-Authenticate: Basic realm=\"GeneralUser/Administrator\"\r\n\r\n<HTML><HEAD><TITLE>401 Unauthorized</TITLE></HEAD>\n<BODY BGCOLOR=\"#cc9999\"><H2>401 Unauthorized</H2>\n<HR>\nAuthorization required for the requested URL\.\n</BODY></HTML>\n|s p/thttpd/ i/Panasonic BB-HCM511 IP camera http config/
match http m|^HTTP/1\.1 307 Redirect\r\nLocation: https?://[^\r\n]*\r\nContent-Length: 0\r\n\r\n$| p/Apache httpd/ v/2.0.X/
match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/([\w._-]+)\r\n.*<title>OneAccess WCF</title>|s p/RapidLogic/ v/$1/ i/OneAccess ONE100A router http config/ d/router/ o/OneOS/
match http m|^HTTP/1\.1 200\r\n.*<meta http-equiv=\"refresh\" content=\"10;url=\"><link rel=\"stylesheet\" type=\"text/css\" href=\"/viawarp\.css\" />|s p/Nova viaWARP httpd/ o/Windows/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: Apache ([\w._-]+) in ([^\r\n]+)\r\n|s p/Apache Tomcat $1/ i/in $2/
match http m|^HTTP/1\.0 401 Unauthorized\r\nContent-type: text/html\r\nAccept-Ranges: bytes\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"PLC Adaptor\"\r\n\r\n| p/Panasonic PLC Adaptor Ethernet-to-mains bridge http config/ d/bridge/
match http m|^<html><head>\n<title>501 Method Not Implemented</title>\n</head><body>\n<h1>Method Not Implemented</h1>\n</body></html>\n$| p/kissdx media player control httpd/
match http m|^HTTP/1\.1 200 OK\r\nServer: yawcam/([\w._-]+)\r\nContent-Length:\d+\r\nMime-Type: text/html\r\nContent-Type: text/html\r\n\r\n| p/Yawcam webcam viewer httpd/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: ACS ([\w._-]+)\r\n|s p/Cisco ACS httpd/ v/$1/
match http m|^HTTP/1\.0 401 Unauthorized\r\n.*Server: WYM/([\w._-]+)\r\n.*WWW-Authenticate: Basic realm=\"Rovio\"\r\n|s p/WYM httpd/ v/$1/ i/Wowwee Rovio webcam/ d/webcam/
match http m|^HTTP/1\.1 \d\d\d .*\r\n.*Server: Kerio Connect ([^\r\n]+)\r\n|s p/Kerio Connect webmail httpd/ v/$1/
match http m|^HTTP/1\.0 500 Internal server error\nServer: M3 Business Engine ([^\r\n]+)\nConnection: close\nContent-Type: text/html; charset=UTF-8\nCache-Control: no-cache\nPragma: no-cache\nExpires: 0\nContent-Type: text/html\n\n<HTML><HEAD>\n<TITLE>500 Internal server error</TITLE>\n</HEAD><BODY>\n<H2>500 Internal server error</H2>\n<HR>\n<ADDRESS><A HREF=\"http://null/\">M3 Business Engine ServerView</A></ADDRESS>\n</BODY></HTML>\n$| p/M3 Business Engine ServerView httpd/ v/$1/
match http m|^HTTP/1\.0 200 ok\r\nContent-type: text/plain\r\n\r\nError accessing ''\r\n$| p/OpenSSL s_server -WWW httpd/
match http m|^HTTP/1\.0 200 ok\r\nContent-type: text/html\r\n\r\n<HTML><BODY BGCOLOR=\"#ffffff\">\n<pre>\n\n(.*) \nCiphers supported in s_server binary\n| p/OpenSSL s_server -www httpd/ i/command line: $1/
match http m|^HTTP/1\.1 302 Moved Temporarily\r\n.*Server: go1984\r\n.*Location: http://([\w._-]+):\d+/([\w._-]+)/Default/index\.htm\r\n\r\n|s p/go1984 httpd/ d/webcam/ h/$1/ i/session ID $2/
match http m|^HTTP/1\.1 200 OK\r\n.*Connection: close\r\nContent-Type: text/html\r\n.*<html lang=\"en\">.*<script type=\"text/javascript\" src=\"\./en/welcomeRes\.js\"> type=\"text/javascript\"></script>.*<script type=\"text/javascript\">document\.write\(\"<title>\" \+ ID_VC_Welcome \+ \"</title>\"\);</script>.*<meta name=\"description\" content=\"VMware vSphere|s p/VMware vSphere http config/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\nAccept-Ranges: none\r\n.*<SCRIPT language=JavaScript>\r\n\tvar PIN_change_attempted = false;\r\n\tvar Login_failed = false;\r\n\tvar password_label = \"\";\r\n</SCRIPT>\r\n<!--\rNote: the opening and closing HTML tags are deliberately omitted from\rthis file\.|s p/Citrix Access Gateway http login/
match http m|^HTTP/1\.1 200 OK\r\nCONTENT-ENCODING: gzip\r\n.*SERVER: Linux/([\w._-]+) Motorola/([\w._-]+)\r\n|s p/Moto Phone Portal/ v/$2/ o/Linux/ i/Linux $1/ d/phone/
match http m|^HTTP/1\.1 200 OK\r\nContent-type: text/html\r\nCache-Control: no-cache\r\n\r\n.*<b>Welcome to PLANET ([\w-]+) Web Management</b>|s p/Planet $1 switch http config/ d/switch/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: GoAhead-Webs\r\n.*Basic realm=\"(P-[\w -]+) \(username: ([\w._-]+)\)\"\r\n|s p/GoAhead-Webs/ i/ZyXEL $1 WAP http config; username: $2/ d/WAP/
match http m|^HTTP/1\.0 403 Forbidden\r\nServer: Mbedthis-Appweb/([\w._-]+)\r\n.*<H2>Access Error: 403 -- Forbidden</H2>|s p/Mbedthis-Appweb/ v/$1/ i/J-Web http config/ o/JUNOS/ d/router/
match http m|^HTTP/1\.1 200 OK\r\nServer: WindRiver-WebServer/([\w._-]+)\r\nConnection: close\r\nContent-Type: text/html\r\n\r\n.*<!-- \(c\) Copyrighted Materials, 2006\. -->.*<script language=\"JavaScript\" src=\"js_utility_JW410R19_____________\.js\"></script>|s p/WindRiver-WebServer/ v/$1/ i/Fujitsu-Siemens FibreCAT SX80 NAS device http config/ d/storage-misc/
match http m|^HTTP/1\.1 200 OK\r\nServer: WindRiver-WebServer/([\w._-]+)\r\nConnection: close\r\nContent-Type: text/html\r\n\r\n.*<!-- \(c\) Copyrighted Materials, 2006\. -->.*<script language=\"JavaScript\" src=\"js_utility_JW420R45_____________\.js\"></script>.*<title>HP StorageWorks MSA Storage Management Utility</title>|s p/HP StorageWorks MSA http config/ d/storage-misc/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: MarratechPortal/([\w._-]+) \(Java ([\w._-]+); Windows ([^)]+)\) build/(\d+)\r\n|s p/Marratech Portal/ v/$1 build $4/ i/Java $2; Windows $3/ o/Windows/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: BBVS\r\nContent-type: text/plain\r\n.*WWW-Authenticate: Basic realm=\"SecuritySpy Web Server\"\r\n\r\n401 Unauthorized\r\n$|s p/SecuritySpy webcam viewer httpd/ o/Mac OS X/
match http m|^HTTP/1\.1 200 OK\r\nConnection: close\r\nContent-Type: text/html\r\nExpires:0\r\npragma:no-cache\r\n\r\n<meta http-equiv=\"refresh\" content=\"0;url=Footprints\.html\">\r\n\r\n\r\n\r\n$| p/TED 5000 power use monitor/ d/power-device/
# http://java423.vicp.net:8652/infoserver.central/data/syshbk/collections/TECHNICALINSTRUCTION/1-61-208775-1.html
match http m|^HTTP/1\.0 400 Malformed Header in \r\nContent-Type: text/html\r\n\r\n$| p/Sun ScApp bytecode transfer httpd/
match http m|^HTTP/1\.1 200 OK\r\n\r\n<html><head><title>File Share</title></head><body><a href=\"/folder/0\">Public</a><br/></body></html>$| p/File Share httpd/ d/phone/ i/Android mobile phone/ o/Linux/
match http m|^HTTP/1\.1 200 OK\r\nConnection: close\r\n.*<title>VoIP Gateway</title>.*<frame name=\"contents\" target=\"main\" src=\"otgw\.cgi\?PAGE=USER\" scrolling=\"auto\" noresize>|s p/D-Link DVS-4088S or DVS-5088S VoIP gateway http config/ d/VoIP adapter/
match http m|^HTTP/1\.0 200 OK\r\nServer: BEJY V([\w._-]+)  HTTP ([\w._-]+) \r\n| p/BEJY httpd/ v/$2/ i/BEJY $1/
match http m|^HTTP/1\.0 404 Not Found\r\nServer: Xfire\r\nConnection: close\r\n\r\n\r\n$| p/Xfire httpd/
match http m|^HTTP/1\.0 302 Found\r\nLocation: http://guide\.opendns\.com/\?url=\r\nContent-type: text/html\r\nContent-Length: 0\r\nConnection: close\r\nDate: .*\r\nServer: OpenDNS Guide\r\n\r\n$| p/OpenDNS Guide/
match http m|^HTTP/1\.0 200 OK\r\nCache-Control: no-cache\r\nConnection: close\r\nContent-Language: en\r\n.*Content-Location: /default\.html\r\n.*ExpertAssist/([\w._-]+)\r\nSet-Cookie: RASID=\w+; path=/\r\n\r\n <html> <head> <title>ExpertAssist</title>|s p/ExpertAssist/ v/$1/ i/ScriptLogic Remote Desktop/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n\r\n<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.01 Frameset//EN\">\r\n<!-- Copyright \(c\) 2000-2002, Fuji Xerox Co\., Ltd\. All Rights Reserved\. -->\r\n<HTML>\r\n<HEAD>\r\n<META HTTP-EQUIV=\"Content-Type\" CONTENT=\"text/html; charset=ISO-8859-1\">\r\n<TITLE>\r\n(DocuPrint [\w._-]+) - ([\w._-]+)\r\n</TITLE>| p/Fuji Xerox $1 printer http config/ d/printer/ h/$2/
match http m|^HTTP/1\.1 502 Bad Gateway\r\nContent-Type: text/html\r\nContent-Length: 487\r\n\r\n<html>\n<head>\n<meta http-equiv=\"Content-Type\" content=\"text/html; charset=utf-8\">\n<title>\nContent Server Message\n</title>\n</head>\n<body>\nNetwork message format error\. Unable to parse browser environment or content item\. Unable to parse properties\. Name-value pairs are missing an '='\.\n<!---\nStatusCode=-1\nStatusMessage=Network message format error\. Unable to parse browser environment or content item\. Unable to parse properties\. Name-value pairs are missing an '='\.\n---!>\n</body></html>$| p/Oracle Universal Content Management httpd/
match http m|^HTTP/1\.0 400 Bad Request\r\nContent-Length: 0\r\n\r\n$| p/IDentifier NameTracer Pro httpd/
match http m|^HTTP/1\.1 200 OK\r\nContent-Length: 155\r\nConnection: close\r\n.*<title><FortiClient Download Portal</title>|s p/FortiClient firewall http config/ d/firewall/
match http m|^HTTP/1\.1 200 OK\r\nServer: Agranat-EmWeb/R([\d_]+)\r\nContent-Type: text/html\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n\r\n<HTML> \n<HEAD>\n<TITLE> ([\w._-]+)  \n</TITLE>\n\n<SCRIPT TYPE = \"text/javascript\">\n netscapeVersion = navigator\.appVersion\.substring\(0,4\);\n ieVersion = navigator\.appVersion\.substring\(17,25\);\n| p/Agranat-EmWeb/ v/$SUBST(1,"_",".")/ i/HP Designjet 800ps printer http config/ d/printer/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*\r\nServer: BarracudaServer\.com \(Posix\)\r\n| p/Barracuda Embedded Web Server/
match http m|^HTTP/1\.1 302 Found\r\nCache-Control: no-cache\r\nConnection: Close\r\nContent-Length: 0\r\nContent-Type: application/octet-stream\r\nDate: .*\r\nLocation: /main\.php\r\nPragma: no-cache\r\nServer: Kerio WinRoute Firewall Embedded Web Server\r\n\r\n$| p/Kerio WinRoute firewall http config/ d/firewall/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: MicroWeb/([\w._-]+)\r\n.*<html>\n<head><title>WebAlert Login Page</title></head>\n<script LANGUAGE=\"JavaScript\">\n<!--\nfunction check\(\)\n{\n\t  if\(\(document\.frmLogin\.txtUserName\.value\.length<3\)|s p/MicroWeb/ v/$1/ i/Walchem WebAlert remote monitoring/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: NSMXwui \(Juniper\)\r\n.*<title>Network and Security Manager - Download UI Client</title>|s p/NSMXwui/ i/Juniper Network and Security Manager http config/ d/firewall/
match http m|^HTTP/1\.1 200 OK\r \nContent-type: text/html\r\n.*<html xmlns=\"http://www\.w3\.org/1999/xhtml\" xml:lang=\"en\" lang=\"en\">\n<head>\n<meta http-equiv=\"Content-Type\" content=\"text/html; charset=iso-8859-1\" />\n<title>Chumby FM Radio</title>|s p/Chumby One FM radio http interface/ d/media device/
match http m|^HTTP/1\.0 301 File moved Permanently\nLocation: /cgi-bin/menu/TCP/IP Settings/\r\nDate: Mon, 23 Sep 1996 16:00:00 GMT\r\nExpires: Thu, 01 Dec 1994 16:00:00 GMT\r\nPragma: no-cache\r\nSet-Cookie: Login=DELETED; path=/;\r\n\r\n| p/Intermac scanner http config/ d/specialized/
match http m|^HTTP/1\.0 200 OK\r\nCache-Control: no-cache, must-revalidate\r\n.*<TITLE>MusicMagic Server</TITLE>.*<td>Total songs</td><td align=right>([\d,]+)</td>|s p/MusicMagic Mixer http control/ i/$1 total songs/
match http m|^HTTP/1\.1 401 BAD\r\nWWW-Authenticate: Basic realm=\"Vuze - Vuze Web Remote\"\r\n\r\nAccess Denied\r\n$| p/Vuze BitTorrent remote http admin/
match http m|^HTTP/1\.0 405 Method Not Allowed\r\nContent-Type: text/html\r\nCache-Control: public\r\nPragma: cache\r\n.*Last-Modified: Thu, 01 Jan 1970 00:00:00 GMT\r\nAccept-Ranges: bytes\r\nConnection: close\r\n|s p/ActionTec TR-069 remote access/
match http m|^HTTP/1\.0 405 Method Not Allowed\r\nContent-Type: text/html\r\nCache-Control: public\r\nPragma: cache\r\n.*<html>\n<head>\n  <title>405 Method Not Allowed</title>\n</head>\n<body bgcolor=\"ffffff\">\n  <h2>405 Method Not Allowed<h2>\n  <p>\n  \n</body>\n</html>\n$|s p/ActionTec TR-069 remote access/
match http m|^HTTP/1\.1 200 OK\r\nConnection: close\r\nContent-Length: 0\r\n\r\n$| p/TR-069 remote access/
match http m|^HTTP/1\.1 202 Accepted\r\nContent-Type: text/html;charset=UTF-8\r\n.*<!DOCTYPE html PUBLIC \"-//W3C//DTD XHTML 1\.0 Strict//EN\" \"http://www\.w3\.org/TR/xhtml1/DTD/xhtml1-strict\.dtd\">\r\n<html xmlns=\"http://www\.w3\.org/1999/xhtml\" xml:lang=\"en\" lang=\"en\">\r\n<head>\r\n<meta http-equiv=\"Content-Type\" content=\"text/html; charset=UTF-8\" />\r\n<title>GlassFish Administration Console - Installation in Progress\.\.\.</title>|s p/Sun GlassFish Administration Console/ i/installation in progress/
match http m|^<html>\r\n<META HTTP-EQUIV=\"Refresh\" CONTENT=\"10\">\r\n<head>\r\n<title>([\w\d.-]+) LanSafe: ([\w\d\s]+)</title>\r\n| p/LanSafe Status@aGlance/ i/Server: $1, Status: $2/ 
match http m|^HTTP/1\.[01] \d\d\d.*Server: IdeaWebServer/([\w._-]+)\r\n.*X-Powered-By: ([^\r\n]+)\r\n|s p/IdeaWebServer httpd/ v/$1/ i/$2/
match http m|^HTTP/1\.[01] \d\d\d.*Server: IdeaWebServer/([\w._-]+)\r\n|s p/IdeaWebServer httpd/ v/$1/
match http m|^HTTP/1\.1 302 OK\r\nDate: \w\w\w \d\d, \d\d:\d\d:\d\d\.\d\d\d\r\nServer: TreeNeWS/([\w._-]+)\r\nMime-Version: 1\.0\r\nLocation: https://index\.html\r\nContent-Length: 67\r\nContent-Type: text/html\r\n\r\n<HTML><HEAD><TITLE>Redirect</TITLE></HEAD>\n<BODY></BODY></HTML>\r\r\n\n$| p/TreeNeWS httpd/ v/$1/ i/Enterasys RBT-8200 switch http config/ d/switch/
match http m|^HTTP/1\.1 200 OK\r\nDate: \w\w\w \d\d, \d\d:\d\d:\d\d\.\d\d\d\r\nServer: TreeNeWS/([\w._-]+)\r\nMime-Version: 1\.0\r\nContent-Length: 1419\r\nContent-Type: text/html\r\nCache-Control: no-cache\r\n\r\n.*<title>Webview</title>|s p/TreeNeWS httpd/ v/$1/ i/Enterasys RBT-8200 switch http config/ d/switch/
match http m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: CANON HTTP Server\r\nContent-Type: text/html\r\n| p/Canon printer web interface/
match http m|^HTTP/1\.1 200 OK\r\nConnection: close\r\nDate: Sat, 01 Jan 2000 00:37:25 GMT\r\nLast-Modified: Sat, 01 Jan 2000 00:01:28 GMT\r\nContent-Type: text/html\r\nContent-Length: 635\r\n.*<title>VoIP Gateway</title>|s p/D-Link DVG-2032S VoIP gateway http config/ d/VoIP adapter/
match http m|^HTTP/1\.0 301 Moved Permanently\r\n.*Server: httpd\r\nContent-type: text/html\r\nETag: \"232c8e4-74d-0\"\r\nContent-length: 0\r\nConnection: close\r\nLocation: https://:443/start\.html\r\n\r\n|s p/Dell Remote Access Controller 6 http interface/ d/remote management/
match http m|^HTTP/1\.0 302 Found\r\nCache-Control: no-cache\r\nConnection: Close\r\nContent-Length: 0\r\nContent-Type: application/octet-stream\r\n.*Location: /nonauth/login\.php\r\nPragma: no-cache\r\nServer: Kerio Clientless SSL-VPN\r\n\r\n|s p/Kerio Clientless SSL-VPN/
match http m|^HTTP/1\.1 200 OK\r\n.*Last-Modified: Tue, 03 Oct 2006 19:21:12 GMT\r\nETag: \"85f_52_4522b828\"\r\n.*Content-Length: 82\r\n.*location=\"/remote/index\";\n\n</script>\n</html>\n\0{605}$|s p/Fortinet FortiGate-5001 SSL VPN remote http login/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"View Home & Status Web Pages\"\r\n.*Server: Allegro-Software-RomPager/([\w._-]+)\r\n|s p/Allegro RomPager/ v/$1/ d/printer/ i/Xerox Phaser 8560DN printer http config/
match http m|^HTTP/1\.1 302 Found\r\nLocation: https://[\d.]+/home\.html\r\nContent-Length: 0\r\nServer: Allegro-Software-RomPager/([\w._-]+)\r\n\r\n$| p/Allegro RomPager/ v/$1/ d/printer/ i/Xerox Phaser 8560DN printer http config/
match http m|^HTTP/1\.1 200 OK\r\n.*<title>XenServer ([\w._-]+)</title>|s p/Citrix Xen Simple HTTP Server/ i/XenServer $1/
match http m|^HTTP/1\.0 200 OK\r\n.*ETag: \"-127477461\"\r\n.*Server: none\r\n.*<title>Fireware XTM User Authentication</title>|s p/WatchGuard FireBox XTM firewall http config/ d/firewall/
match http m|^HTTP/1\.1 401 Unauthorized\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"uTorrent\"\r\n\r\n| p/uTorrent WebUI/ o/Windows/
match http m|^HTTP/1\.1 300 ERROR\r\nConnection: keep-alive\r\nContent-Length: 15\r\nContent-Type: text/html\r\n\r\ninvalid request$| p/uTorrent WebUI/ o/Windows/
# uTorrent 2.0.2
match http m|^HTTP/1\.1 400 ERROR\r\nConnection: keep-alive\r\nContent-Length: 15\r\nContent-Type: text/html\r\n\r\ninvalid request$| p/uTorrent WebUI/ o/Windows/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: WYM/([\w._-]+)\r\n.*Content-Length: 1029\r\nLast-Modified: Tue, 19 May 2009 02:17:02 GMT\r\n\r\n\xef\xbb\xbf<html>\r\n<head>\r\n<title>NVS</title>|s p/WYM httpd/ v/$1/ i/A+V Link NVS-4000 surveillance system http config/ d/webcam/
match http m|^HTTP/1\.1 200 OK\r\nLast-Modified: Mon, 07 Apr  2009  04:00:00 GMT\r\nContent-Type: TEXT/HTML\r\nDate: \w\w\w, \d\d \w\w\w  \d\d\d\d  \d\d:\d\d:\d\d GMT00:00 GMT\r\nServer: ICOM ([\w._-]+)    from SBS\r\nMIME-Version: 1\.0\r\nServer: ICOM [\w._-]+    from SBS\r\nConnection: close\r\nContent-Length:             861\r\n\r\n<HTML>\r\n<HEAD>\r\n<TITLE>UltraQuest Index HTML</TITLE>| p/ICOM httpd/ v/$1/ i/UltraQuest mainframe reporting/ o|OS/390|
match http m|^HTTP/1\.0 404 Not Found\r\nContent-type: text/html\r\nDate: Sat, 31 Dec 2005 23:02:28 GMT\r\nConnection: close\r\n\r\n<HEAD><TITLE>404 Not Found</TITLE></HEAD>\n<BODY><H1>404 Not Found</H1>\nThe requested URL was not found on this server\.\n</BODY>\n$| p/BusyBox httpd/ o/Linux/ i/Sphairon Turbolink IAD ADSL modem http config/
match http m|^HTTP/1\.1 302\r\nLocation: /login\.vibe\r\n\r\n$| p/VibeStreamer streaming media httpd/
match http m|^\r\n\r\n\r\n\r\n\r\n\r\n<\?xml version=\"1\.0\" encoding=\"ISO-8859-1\"\?>\r\n<!DOCTYPE html PUBLIC \"-//W3C//DTD XHTML 1\.0 Strict//EN\"\r\n  \"http://www\.w3\.org/TR/xhtml1/DTD/xhtml1-strict\.dtd\">\r\n\r\n\r\n\r\n<html>\r\n<head>\r\n<title>RealSecure SiteProtector</title>.*<meta name=\"copyright\"\r\n\t\tcontent=\"This web site, its design, copy, scripts and artwork,\r\n\t\tare copyright 2006 by Internet Security Systems, Inc\.\r\n|s p/Apache httpd/ v/2.0.63/ i/ISS SiteProtector 2.0/
match http m|^<!DOCTYPE HTML PUBLIC \"-//IETF//DTD HTML 2\.0//EN\">\n<html><head>\n<title>302 Found</title>\n</head><body>\n<h1>Found</h1>\n<p>The document has moved <a href=\"/red2301\.html\?RedirectUrl=/\">here</a>\.</p>\n<p>Additionally, a 302 Found\nerror was encountered while trying to use an ErrorDocument to handle the request\.</p>\n</body></html>\n$| p/HP System Management httpd/
match http m|^HTTP/1\.0 200 OK\nContent-type: text/html\r\n.*<title>DVR WebViewer</title>\r\n<meta http-equiv=\"Content-Type\" content=\"text/html; charset=euc-kr\">\r\n.*<OBJECT\r\n\t  classid=\"clsid:EE479A40-C128-40DD-93DA-000556AF9607\"\r\n\t  codebase=\"CtrWeb\.cab#version=1,1,1,1\"\r\n\t  width=(\d+)\r\n\t  height=(\d+)\r\n\t  align=center\r\n\t  hspace=0\r\n\t  vspace=0\r\n>\r\n<param name=\"CmdPort\" value=\"(\d+)\">\r\n<param name=\"StreamPort\" value=\"(\d+)\">|s p/MicroDigital MDR-4600 DVR httpd/ d/media device/ i/Resolution $1x$2; CmdPort $3; StreamPort $4/
match http m|^HTTP/1\.0 200 OK\r\nServer: Senturion/([\w._-]+)\r\n.*<title>Sensatronics: Senturion ([\w._-]+)</title><script language=\"javascript\" src=\"/gen\.js\">|s p/Sensatronics Senturion $2 environmental sensor httpd/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\n.*<!-- saved from url=\(0022\)http://internet\.e-mail -->\r\n<html>\r\n<head>\r\n<title>WebCam</title>\r\n</head>\r\n<body link=\"#505050\" bgcolor=\"#505050\" vlink=\"#505050\" alink=\"#505050\" topmargin=\"3\">|s p/AverMedia WebCamX httpd/ d/webcam/
match http m|^HTTP/1\.0 401 Unauthorized\r\nDate: .*\r\nConnection: close\r\nContent-Type: text/html\r\nWWW-Authenticate: Basic realm=\"User\"\r\nContent-length: 192\r\n\r\n<HTML><HEAD>\n<TITLE>Authentication Error: Access Denied, Authorization required\.</TITLE>\n</HEAD>\r\n<BODY><H2>Authentication Error: Access Denied, Authorization required\.</H2></BODY>\n</HTML>\r\n\r\n| p/Yello Strom Sparzaehler electricity meter httpd/
match http m|^HTTP/1\.0 200 OK\r\nDate: .*\r\nCache-Control: no-cache\r\nContent-type: text/html\r\nETag: \"19c-a4-4ab218f6\"\r\nContent-length: 164\r\n| p/Yello Strom Sparzaehler electricity meter httpd/
match http m|^HTTP/1\.1 200 OK\r\n.*<meta http-equiv=\"Content-Type\" content=\"text/html; charset=Shift_JIS\">\r\n\r\n<html>\r\n<head>\r\n<title>Network</title>\r\n</head>\r\n<noscript>Make sure JavaScript is ON\.</noscript>.*<frame src=\"dmy\.htm\" name=\"m\">|s p/Sanyo PLC-XU300 projector http config/ d/media device/
match http m|^HTTP/1\.0 302 Moved Temporarily\r\nPragma: no-cache\r\nLocation: https://[\w._-]+/\r\n.*<TITLE>Redirect Notification</TITLE>.*<P>Please click <a href=\"https://[\w._-]+/\">here</a> to go to the correct location\.|s p/Tandberg Border Controller VoIP proxy/ d/proxy server/ o/Linux 2.6/
match http m|^HTTP/1\.1 200 Document follows\r\n.*Connection: Close\r\nServer: Micro-Web\r\n.*<!-- \*\* THIS FILE CONTAINS NO REALTIME DATA \*\* -->.*<title>   LocalSite - ARC Plus Web Interface</title>|s p/Micro-Web httpd/ i/Burk ARC Plus remote management http interface/ d/remote management/
match http m|^HTTP/1\.1 302 \(Found\)\r\nConnection: close\r\nLocation: .*\r\nServer: Oversee Turing v([\w._-]+)\r\n|s p/Oversee Turing httpd/ v/$1/ i/domain parking/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: Java PseudoHttpd/([\w._-]+)\r\n.*<title>CSP Status</title>|s p/Java PseudoHttpd/ v/$1/ i/Card Server Proxy (CSP) http config/
match http m|^HTTP/1\.1 200 OK\r\n.*<title>XBMC</title> \n<link type=\"text/css\" rel=\"stylesheet\" href=\"basic\.css\">\n</head>\n<body>\n<h1>XBMC Webinterface</h1>|s p/XBMC http interface/ d/media device/
match http m|^HTTP/1\.1 200 OK\r\n.*<title>XBMC</title>\r\n\t\t<meta http-equiv=\"Content-Language\" content=\"EN\" />.*<!-- <link rel=\"search\" href=\"/provider\.xml\" type=\"application/opensearchdescription\+xml\" title=\"XBMC Library\" /> -->|s p/XMBC http interface/ d/media device/
match http m|^HTTP/1\.0 301 Moved Permanently\r\nLocation:http://([\w._-]+)/index\.htm\r\nContent-Type: text/plain\r\nContent-Length:2.\r\n\r\nhttp://([\w._-]+)/index\.htm$| p/Lanier IS100e image scanner httpd config/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: text/html\r\n\r\n.*<TITLE>Start</TITLE>\n</HEAD>\n<FRAMESET border=0 frameSpacing=0 rows=30,8,\* frameBorder=0>\n<FRAME name=bar src=\"CgiTagMenu\?page=Top&Language=0\" scrolling=no NORESIZE>\n<FRAME name=hrbar src=\"BarFoot\.html\" scrolling=no NORESIZE>|s p/thttpd/ i/Panasonic Network Camera http config/
match http m|^HTTP/1\.0 200 OK\r\n.*Last-Modified: Thu, 01 Jan 1970 00:00:00 GMT\r\n.*\xef\xbb\xbf<html>\r\n<head>\r\n.*<META NAME=\"Expired\" CONTENT=\"01-jan-1900 00:00:00\" />\r\n.*<title>NAS</title>.*<title></title>|s p/BusyBox httpd/ i/Hitachi SimpleNET NAS http config/ d/storage-misc/ o/Linux/
match http m|^HTTP/1\.1 200 OK\r\n.*<TITLE>(PA168S) V([\w._-]+) +</TITLE>.*<script>function sf\(\){document\.f\.auth\.focus\(\);}</script>.*<FONT size=5>Willkommen zur Administration des Telefons</FONT>|s p/Atcom AT-320 VoIP phone http config/ v/$2/ i/PalmMicro $1 chipset/
match http m|^HTTP/1\.1 200 OK\r\n.*Expires: Thu, 01 Jan 1970 00:00:00 GMT\r\n.*<TITLE>Dashboard</TITLE>.*<META name='copyright' content='Copyright 2003-2010, Red Condor, Inc\.'>|s p/Red Condor antispam appliance http config/ d/proxy server/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Digest realm=\"([\d.]+)\",  qop=\"auth\", nonce=\"[0-9a-f]+\"\r\n.*<title>BMC HTTP Server</title>\r\n.*<img src=\"ilo2_rgb2\.jpg\" class=\"mainlogo\" alt=\"\">|s p/HP Integrated Lights-Out http config/ d/remote management/
match http m|^HTTP/1\.0 300 Multiple Choices\r\nServer: Rockpile Web Server\r\nDate: Sun, 00 Jan 1900 00:00:00 GMT\r\nConnection: close\r\nLocation: http://[\w._-]+/localmenus\.cgi\?func=604\r\nContent-type: text/html\r\n\r\n.*HTTP/1\.0 404 Not Found\r\nServer: Rockpile Web Server\r\nDate: Sun, 00 Jan 1900 00:00:00 GMT\r\n|s p/Rockpile httpd/ i/Cisco 7937 VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"CentreWare Internet Services\"\r\n.*<!-- Copyright \(c\) 2000-2003, Fuji Xerox Co\., Ltd\. All Rights Reserved\. -->\r\n<HTML>\r\n<HEAD>\r\n<TITLE>FAILED</TITLE>\r\n<META http-equiv=\"Content-Type\" content=\"text/html; charset=windows-1252\">|s p/FujiXerox ApeosPort-IV C4470 http config/ d/printer/
match http m|^HTTP/1\.1 404 Not Found\r\n.*Server: iTP Secure WebServer/([\w._-]+)\r\nMIME-version: 1\.0\r\nContent-type: text/html\r\nConnection: close\r\n\r\n<TITLE>Not Found</TITLE><H1>Not Found</H1>\n The requested object was not found on this server\.$|s p/iTP Secure WebServer/ v/$1/ i/HP Tandem NonStop/
match http m|^HTTP/1\.1 302 Moved Temporarily\r\n.*Server: iTP WebServer with NSJSP/([\w._-]+) \(HTTP/1\.1 Connector\)\r\nLocation: http://([\w._-]+):\d+/index\.html\r\n|s p/iTP WebServer with NSJSP/ v/$1/ h/$2/ i/HP Tandem NonStop/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: Indy/([\w._-]+)\r\n.*<title>GregHSRWLib - RemObjects SDK for \.NET v([\w._-]+)</title>|s p/Indy httpd/ v/$1/ i/.NET $2; Acer Registration Service; greghsrw.exe/
match http m|^HTTP/1\.1 200 OK\r\nETag: W/\"[\d-]+\"\r\n.*Server: null\r\n.*<title>HP - Data Center Fabric Manager</title>|s p/HP Data Center Fabric Manager http config/
match http m|^HTTP/1\.1 200 OK\r\nETag: W/\"[\d-]+\"\r\n.*Server: censhare hyena/([\w._-]+)\r\n|s p/censhare hyena httpd/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\nETag: W/\"[\d-]+\"\r\n.*Server: Undefined\r\n.*<META HTTP-EQUIV=\"refresh\" CONTENT=\"0;URL=/core/orionSplashScreen\.do\">|s p/McAfee ePolicy Orchestrator http interface/
match http m|^HTTP/1\.1 401 \r\nDate: Sat, 21 Dec 1996 12:00:00 GMT\r\nWWW-Authenticate: Basic realm=\"Default password:1234\"\r\n\r\n401 Unauthorized - User authentication is required\.$| p/Edimax PS-1206P print server/ d/print server/
match http m|^HTTP/1\.1 301 Moved Permanently\r\n.*Server: Noelios-Restlet-Engine/([\w._-]+)\r\nLocation: http://([\w._-]+)/index\.html\r\nVary: Accept-Charset,Accept-Encoding,Accept-Language,Accept,User-Agent\r\nContent-Length: 0\r\nConnection: close\r\nContent-Type: text/plain\r\n\r\n$|s p/Sonatype Nexus Maven Repository Manager httpd/
match http m|^HTTP/1\.0 501 Not Implemented\r\nServer: SimpleHTTP/([\w._-]+) Python/([\w._-]+)\r\n.*Content-Type: text/html\r\nConnection: close\r\n\r\n<head>\n<title>Error response</title>\n</head>\n<body>\n<h1>Error response</h1>\n<p>Error code 501\.\n<p>Message: Not Implemented\.\n<p>Error code explanation: 501 = Server does not support this operation\.\n</body>\n$|s p/SimpleHTTPServer/ v/$1/ i/rPath Appliance Platform Agent; Python $2/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: CMSHTTPD/([\w._-]+) z_VM/([\w._-]+) ([^\r\n]+)\r\n|s p/CMSHTTPD/ v/$1/ i|z/VM $2; $3| o|z/VM|
match http m|^HTTP/1\.0 200 OK\nServer: Cardax Embedded Interface\n.*<H1>CardaxFT Controller #  (\d+)  \(ETS\)</H1>.*<br>Version: v([\w._/-]+) BootMon-([\w._-]+)</body>\n$|s p/Cardax FT security system http interface/ v/$2/ i/Controller #$1; BootMon $3/ d/security-misc/
match http m|^HTTP/1\.0 302 Moved Temporarily\r\nAllow: GET,POST,HEAD\r\nMIME-Version: 1\.0\r\nServer: (MA\w+) Server ([\w._-]+)\r\nLocation: http://0\.0\.0\.0\r\n\r\n$| p/Huawei $1 WAP http config/ v/$2/
match http m|^HTTP/1\.0 200 OK\r\nServer: ZyXEL SSLVPN Server v([\w._-]+)\r\n.*<title>ZyWALL SSL(\d+)</title>|s p/ZyXEL ZyWALL SSL $2 SSL-VPN applicance http config/ v/$2/ d/firewall/
match http m|^HTTP/1\.1 200 OK\r\n.*Server:  \r\n.*<title>ZyWALL ([^<]+)</title>|s p/ZyXEL ZyWALL $1 firewall http config/ d/firewall/
match http m|^HTTP/1\.0 200 OK\r\nExpires: 0\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<html>\n<title>Login</title>\n<link rel=stylesheet href=\"login\.css\" type=\"text/css\" />\n<script src=\"form\.js\" type=\"text/javascript\"></script>| p/D-Link DGS-1200T-series switch http config/ d/switch/
match http m|^HTTP/1\.1 505 HTTP Version not supported\r\nContent-Length: 0\r\nDate: .*\r\nAccept-Ranges: bytes\r\n\r\n$| p/Virtual Mic http synchronization/ d/media device/ o/iPhone OS/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"Remote-Motion CCD Network Camera\"\r\nContent-Type: text/html\r\nServer: Vivotek Network Camera\r\n\r\n<HTML>\n<HEAD>\n<TITLE>Protected Object</TITLE></HEAD><BODY>\n<H1>Protected Object</H1>This object on the server is protected\.<P>\n</BODY></HTML>$| p/Vivotek Network Camera http config/ d/webcam/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: Web Server\r\n.*<TITLE>NetGear ([\w._-]+)</TITLE>|s p/Netgear $1 switch http config/ d/switch/
match http m|^HTTP/1\.0 200 OK\r\nPragma: no-cache\r\n.*<TITLE>Management</TITLE>.*<METArem http_equiv=\"Refresh\" content=\"0; URL=index\.ssi\">\n\n</HEAD>\n<FRAMESET border=0 frameSpacing=0 rows=48,\* frameBorder=no>|s p/Tandberg MXP video conferencing http config/ d/webcam/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: HyNetOS/([\w._-]+)\r\n.*<title>(CS\d+) SNMP/Web Adapter</title>|s p/Effekta MH 6000 UPS http config/ i|$2 SNMP/Web adapter; HyNetOS $1| o/HyNetOS/ d/power-device/
match http m|^HTTP/1\.1 200 OK\r\nX-Cocoon-Version: ([\w._-]+)\r\nExpires: Thu, 01 Jan 1970 00:00:00 GMT\r\n.*<title>F-Secure Policy Manager Web Reporting</title>|s p/F-Secure Policy Manager http interface/ i/Apache Cocoon $1/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: ShellHTTPD/([\w._-]+)\r\n.*<title>Dachstein LEAF Firewall</title>|s p/ShellHTTPD/ v/$1/ i/Dachstein LEAF firewall/ o/Linux 2.2/ d/firewall/
match http m|^HTTP/1\.0 401 Unauthorized\r\nDate: Thu, 01 Jan 1970 00:00:00 GMT\r\nnServer: avtech/([\w._-]+)\.\.Expires: 0\r\nPragma:  no-cache\r\nCache-Control:  no-cache\r\nConnection: close\r\nContent-type: text/html;charset=ISO-8859-1\r\nWWW-Authenticate: Basic realm=server\r\nContent-Length: 163\r\n| p/avtech httpd/ v/$1/ i/Postef-8840 ADSL router/ d/broadband router/
match http m|^HTTP/1\.0 200 Script output follows\r\nServer: shinGETsu/([\w._-]+) \(Saku/([\w._-]+)\) Python/([\w._-]+)\r\n| p/Saku/ v/$2/ i/client for shinGETsu $1 BBS; Python $3/
match http m|^HTTP/1\.1 503 HTTP is not licensed\.<p>To set up this filer, use <a href=/api>/api</a> \.\r\nServer: Data ONTAP/([\w._-]+)\r\n| p/NetApp http vFiler/ o/Data ONTAP $1/
match http m|^HTTP/1\.1 503 HTTP is not licensed\.<p>To administer this filer, use <a href=/na_admin/>/na_admin/</a> \.\r\nServer: NetApp//([\w._-]+)\r\n| p/NetApp http vFiler/ o/Data ONTAP $1/
match http m|^HTTP/1\.0 401 Unauthorized\r\nDate: .*\r\nCache-Control: no-cache,no-store\r\nWWW-Authenticate: Basic realm=\"\.\"\r\nContent-Type: text/html; charset=%s\r\nConnection: close\r\n\r\n<html>\n<head><title>401 Unauthorized</title></head>\n<body>\n<h3>401 Unauthorized</h3>\nAuthorization required\.\n</body>\n</html>\n| p/m0n0wall FreeBSD firewall web interface/ o/FreeBSD/ d/firewall/
match http m|^HTTP/1\.0 401 Unauthorized\r\nDate: .*\r\nCache-Control: no-cache,no-store\r\nWWW-Authenticate: Basic realm=\"\.\"\r\nContent-Type: text/html; charset=%s\r\nConnection: close\r\n\r\n<html>\n<head><title>401 Unauthorized</title></head>\n<body>\n<h3>401 Unauthorized</h3>\nAuthorization required\. HuaCheng Technologies\n</body>\n</html>\n| p/HuaCheng firewall http config/ d/firewall/
match http m|^HTTP/1\.0 501 Not Implemented\r\nDate: .*\r\nCache-Control: no-cache,no-store\r\nContent-Type: text/html; charset=%s\r\nConnection: close\r\n\r\n<html>\n<head><title>501 Not Implemented</title></head>\n<body>\n<h3>501 Not Implemented</h3>\nThat method is not implemented\.\n</body>\n</html>\n$| p/Western Digital My Book http config/ d/storage-misc/
match http m|^HTTP/1\.1 200 OK\r\nServer: Axeda Agent Web Server/([\w._-]+)\r\n.*Last-Modified: 1200004200\r\n.*<title>IM_v8_Data </title>\r\n</head>\r\n<body bgcolor=\"ffffff\">\r\n<center>\r\n<DIV style=\"position:absolute; top:6; left:6; width:(\d+); height:(\d+); z-layer:1;\" >\r\n<applet codebase=\"/aagweb/classes\" code=aglance\.jag\.AAGApplet|s p/Axeda remote management http interface/ v/$1/ d/remote management/ i/Resolutino $2x$3/
match http m|^HTTP/1\.1 200 OK\r\nConnection: close\r\nContent-Type: text/html\r\nContent-Encoding: gzip\r\nCache-Control: max-age=600\r\n\r\n\x1f\x8b\x08\0\0\0\0\0| p/BenQ projector/ d/media device/ i/Crestron RoomView/
match http m|^HTTP/1\.1 302 Moved Temporarily\r\nLocation: https://([\w._-]+):\d+/symantec\.jsp\r\nContent-Length: 0\r\nDate: .*\r\nConnection: close\r\nServer: Hidden\r\n\r\n$| p/Symantec Endpoint Protection Manager http config/ d/firewall/ h/$1/
match http m|^HTTP/1\.1 302 Found\r\nDate: .*\r\nServer:  \r\nLocation: https://[\d.]+:(\d+)/redirect\.cgi\?arip=\r\n.*<address>  Server at ([\w._-]+) Port \d+</address>|s p/ZyXEL ZyWALL USG 200 firewall http config/ h/$2/ i/redirect to port $1/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\n.*<script src=\"\./message/message\.js\"></script>\n\t<script src=\"\./buffalo\.js\"></script>\n\t\n\t<script src=\"\./btsdk\.js\"></script>\n\t<script src=\"\./btuicommon\.js\"></script>|s p/Buffalo NAS BitTorrent download manager http interface/ d/storage-misc/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: text/html\r\nContent-Encoding: gzip\r\nCache-Control: max-age=600, must-revalidate\r\n\r\n\x1f\x8b\x08\0\0\0\0\0\0\0| p/Modtronix SBC65EC Web Server/
match http m|^HTTP/1\.0 301\r\n.*Server: OKWS/([\w._-]+)\r\n|s p/OKWS httpd/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: text/html\r\n\r\n.*<TITLE>PowerDownTop</TITLE>\n<SCRIPT Language=\"JavaScript\">\n<!--\ntop\.location = \"CgiPowerDownReset\?Language=0\";\n// -->\n</SCRIPT>\n</HEAD>\n<BODY></BODY></HTML>$|s p/thttpd/ i/Panasonic IP camera http viewer/ d/webcam/
match http m|^HTTP/1\.0 200 OK\r\nServer: ZK Web Server\r\nPragma: no-cache\r\nCache-control: no-cache\r\n.*<script language=JavaScript type='text/javascript'>self\.location\.href='/csl/login'</script>|s p/ZK Web Server/ i/ZKSoftware ZEM500 fingerprint reader; MIPS/ d/security-misc/ o/Linux/
match http m|^HTTP/1\.0 404 Not Found\r\nContent-Length: 69\r\nContent-Type: text/html; charset=UTF-8\r\nServer: TornadoServer/([\w._-]+)\r\n\r\n<html><title>404: Not Found</title><body>404: Not Found</body></html>$| p/Tornado httpd/ v/$1/
match http m|^HTTP/1\.1 301 0\w\w\w, \d\d \w\w\w \d\d\d\d \d\d:\d\d:\d\d GMT\r\nServer: Agranat-EmWeb/R([\d_]+)\r\nLocation: https://[\d.]+/web/content/index\.html\r\n| p/Agranat-EmWeb/ v/$SUBST(1,"_",".")/ i/Alcatel 7800 switch http config/ d/switch/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: Mbedthis-Appweb/([\w._-]+)\r\nCache-Control: no-cache, must-revalidate\r\nContent-type: text/html\r\nETag: \"[0-9a-f-]+\"\r\n.*X-Powered-By: PHP/([\w._-]+)\r\nExpires: Mon, 26 Jul 1997 05:00:00 GMT\r\n.*<title>Log In - Juniper Web Device Manager</title>|s p/Mbedthis-AppWeb/ v/$1/ i/Juniper SRX-240H UTM firewall http config; PHP $2/ o/JUNOS/ d/firewall/
match http m|^HTTP/1\.0 403 Not Authorized\r\nContent-Type: text/html\r\nContent-Length: 379\r\n\r\n<\?xml version=\"1\.0\" encoding=\"US-ASCII\"\?>.*<p>Will not send listings for this directory\.</p>\r\n</body>\r\n</html>\r\n|s p/Ashd httpd/
match http m|^HTTP/1\.1 200\r\nContent-type: text/html\r\nConnection: close\r\nCONTENT-LENGTH: \d+\r\n.*<meta http-equiv=\"Content-Type\" content=\"text/html; charset=windows-1252\">\r\n<meta name=\"GENERATOR\" content=\"Microsoft FrontPage 4\.0\">.*<title>Phoenix PowerAgent GP</title>|s p/Phoenix PowerAgent GP power monitor http interface/ d/power-device/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\nConnection: close\r\n\r\n<!---CAS:0003--><HTML><HEAD>\n<TITLE> Broadband NAT Router Web-Console           </TITLE>|s p/D-Link DGE-530T network adapter http config/
match http m|^HTTP/1\.0 200 OK\r\nAccept-Ranges: none\r\nConnection: close\r\nContent-Encoding: identity\r\nContent-Length: 4240\r\nContent-Type: text/html; charset=ISO-8859-1\r\n.*Server: IST OIS\r\n.*<title>Allworx Hosted Web Site</title>|s p/Allworx 6x VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.0 401 Unauthorized\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"ACEswitch@[\d.]+\"\r\n\r\n401 Unauthorized\r\n$| p/Alteon 2424-SSL load balancer http config/ d/load balancer/
match http m|^HTTP/1\.0 302 Found\r\nConnection: Close\r\nLocation: /search\?site=default_collection&client=default_frontend&output=xml_no_dtd&proxystylesheet=default_frontend&proxycustom=<HOME/>\r\nContent-Type: text/html\r\nContent-Length: 0\r\n\r\n$| p/Google Mini search appliance httpd/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: Apache/x\.x\.x \(Unix\) mod_ssl/x\.x\.x OpenSSL/([\w._-]+)\r\n.*<title> FASTORA Filer Storage Manager </title>.*classid=\"clsid:adb880a6-d8ff-11cf-9377-00aa003b7a11\">|s p/Apache httpd/ o/FreeBSD/ i/Fastora NAS T2 NAS device; OpenSSL $1/ d/storage-misc/
match http m|^HTTP/1\.1 400 Bad Request\r\nDate: .*\r\nCache-Control: private\r\nServer: IPOffice/([\w._()-]+)\r\nContent-Type: text/plain\r\nContent-Length: 13\r\n\r\nParsing error$| p/Avaya IP Office VoIP PBX httpd/ d/PBX/
match http m|^HTTP/1\.0 404 Not Found\r\nConnection: close\r\nServer: SimpleHTTPtutorial v([\w._-]+)\r\n\r\n$| p/SimpleHTTPtutorial httpd/ v/$1/
match http m|^HTTP/1\.0 200 OK\n.*Server: uClinux-httpd ([\w._-]+)\nExpires: 0\n\n.*<title>DxClient NetViewer</title>.*<OBJECT\r\n\tclassid=\"clsid:EF34051A-402A-4ABE-AA20-04E1B4422BD9\"\r\n\tcodebase=\"DxClient_NetViewer\.cab#version=([\d,]+)\"\r\n|s p/uClinux-httpd/ v/$1/ o/Linux/ i/DxClient NetViewer DVR viewer $SUBST(2,",",".")/
match http m|^HTTP/1\.0 302 Moved Temporarily\r\nDate: .*\r\nServer: Mbedthis-Appweb/([\w._-]+)\r\nContent-length: 0\r\nConnection: close\r\nLocation: http://http/tohttps\.jsp\r\n\r\n$| p/Mbedthis-Appweb/ v/$1/ i/Ruckus WAP http config/ d/WAP/
match http m|^HTTP/1\.0 302 Moved Temporarily\r\nDate: .*\r\nServer: Mbedthis-Appweb/([\w._-]+)\r\nCache-Control: no-cache\r\nETag: \"1b8056-34-531868\"\r\nContent-length: 0\r\nConnection: close\r\nLocation: https://https/admin/login\.jsp\r\n\r\n$| p/Mbedthis-Appweb/ v/$1/ i/Ruckus WAP http config/ d/WAP/
match http m|^HTTP/1\.1 200 OK\r\n.*Last-Modified: Mon, 13 Mar 2006 11:22:33 \+1300\r\n.*<title>Welcome</title>.*<script language=\"JavaScript\" type=\"text/JavaScript\">\r<!--\rfunction MM_preloadImages\(\) { //v3\.0\r|s p/FirstClass Internet Access Server httpd/
match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/([\w._-]+)\r\nMIME-version: 1\.0\r\nContent-type: text/html\r\nSet-Cookie: auth=\w+; path=/\r\n\r\n\xef\xbb\xbf.*<title>Logon</title>.*if \(window\.focus\) self\.focus\(\);|s p/RapidLogic httpd/ v/$1/ i/Unita VoIP phone http config/ d/VoIP phone/
match http m|^HTTP/1\.1 400 Bad Request\r\nContent-Type: text/html\r\nContent-Length: 2\r\nCache-Control: no-cache\r\nPragma: no-cache\r\nConnection: Close\r\n\r\n5\0$| p/Matrix42 remote control httpd/ d/remote management/
match http m|^HTTP/1\.0 200 OK\r\nConnection: close\r\nProxy-Connection: close\r\nContent-Type: text/html\r\nCache-Control: private\r\nExpires: 0\r\n\r\n<html><head><title></title></head><frameset cols=\"100%\"><frame src=\"http://[\d.]+:\d+/joikuspot-accept\">| p/JoikuSpot 3G tethering http interface/ d/phone/
match http m|^HTTP/1\.1 200 OK\r\nServer: Virata-EmWeb/R([\d_]+)\r\nContent-Type: text/html\r\nCache-Control: max-age=0\r\nExpires: -1\r\n\r\n<!-- \n  Copyright \(c\) 2004-2006 by Cisco Systems, Inc\.\n  All rights reserved\.\n -->.*<title>Cisco Systems, Inc\. Easy VPN Network Access</title>|s i/Cisco ASA firewall http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/firewall/
match http m|^HTTP/1\.1 200 Ok\r\nDate: .*\r\nServer: ebHTTPD ([\w._-]+)\r\n| p/ebHTTPD/ v/$1/
match http m|^HTTP/1\.0 404 not found \(/\)\r\n.*Server: Tntnet/([\w._-]+)\r\n|s p/Tntnet httpd/ v/$1/
match http m|^HTTP/1\.1 401 Authorization Required\r\n.*Server: SecureTransport/([\w._-]+)\r\n.*WWW-Authenticate: Basic realm=\"FileDriveWWW\"\r\n|s p/Axway SecureTransport httpd/ v/$1/
match http m|^HTTP/1\.0 404 Not Found\r\nContent-Length: 69\r\nContent-Type: text/html; charset=UTF-8\r\nServer: CycloneServer/([\w._-]+)\r\n\r\n<html><title>404: Not Found</title><body>404: Not Found</body></html>$| p/CycloneServer httpd/ v/$1/
match http m|^HTTP/1\.1 400 Bad request\n.*<!DOCTYPE HTML PUBLIC \"-//IETF//DTD HTML 2\.0//EN\">\n<html><head>\n<title>400 Header 'Host' is missing\.</title>|s p/Kerio MailServer http config/
match http m|^HTTP/1\.1 200 OK\r\n.*<!DOCTYPE html PUBLIC \"-//W3C//DTD XHTML 1\.0 Strict//EN\" \"http://www\.w3\.org/TR/xhtml1/DTD/xhtml1-strict\.dtd\">\n<html>\n<script language=\"JavaScript\" type=\"text/javascript\">\n  if \(top\.location != self\.location\).*<title>Authentication Required</title>|s p/D-Link DFL-800 firewall http config/ d/firewall/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: TSEWS\r\n.*<title>TechniSat WebTools</title>.*<meta name='copyright'           content='TechniSat Digital\(r\) 2006-2009\(c\)'>|s p/TechniSat Digicorder HD S2 satellite receiver http interface/ d/media device/
match http m|^HTTP/1\.1 505 HTTP Version not supported\r\n.*Server: Good\.iWare WebDAV Server for iPhone\r\n.*If you have any questions, please contact <a href=\"mailto:support@goodreader\.net\">support@goodreader\.net</a>|s p/Good.iWare WebDAV Server/ o/iOS/ d/phone/ i/GoodReader PDF reader/
match http m|^HTTP/1\.0 200 OK\r\nServer: Polycom-GAB\r\nContent-type: text/html\r\nPragma: no-cache\r\n\r\n$| p/Polycom CMA Global Address Book (GAB) httpd/
match http m|^HTTP/1\.0 200 \r\n.*Server: AURA\r\n.*<TITLE>ServerView RAID Manager</TITLE>|s p/Fujitsu Siemens ServerView RAID Manager http interface/
match http m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\nContent-Length: 227\r\n\r\n<html> <head> <title>D-Link VoIP Router</title>| p/D-Link DVG-5112S VoIP adapter/ d/VoIP adapter/
match http m|^HTTP/1\.0 503 Service Unavailable\r\nContent-Type: text/html\r\nContent-Length: 53\r\nExpires: now\r\nPragma: no-cache\r\nCache-control: no-cache,no-store\r\n\r\nThe service is not available\. Please try again later\.$| p/Pound http proxy/ d/proxy server/
match http m|^HTTP/1\.0 501 Method Not Implemented\r\nContent-Length: 0\r\n\r\n$| p/Zotero httpd/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: Schleifenbauer SPbus gateway\r\n.*<!-- seinclude basicpagehead\.txt -->\r\n|s p/Schleifenbauer SPbus gateway http config/ d/power-device/
match http m|^HTTP/1\.1 200 OK\r\nServer: ExtremeZ-IP/([\w._-]+)\r\n.*<title>ExtremeZ-IP HTTP Service</title>|s p/ExtremeZ-IP httpd/ v/$1/
match http m|^HTTP/1\.0 302 FOUND\r\nContent-Type: text/html; charset=utf-8\r\nLocation: http://[\w._-]+:\d+/login\?next=%2F\r\n.*Server: Werkzeug/([\w._-]+) Python/([\w._-]+)\r\n|s p/Werkzeug httpd/ v/$1/ i/Flask web framework; Python $2/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html; charset=utf-8\r\nVary: Cookie, User-Agent, Accept-Language\r\nConnection: close\r\nServer: MoinMoin ([\w._-]+) release Python/([\w._-]+)\r\n| p/MoinMoin wiki standalone httpd/ v/$1/ i/Python $2/
match http m|^HTTP/1\.1 401 Unauthorized\r\nConnection: close\r\nContent-Type: text/html\r\nContent-Length: 77\r\nServer: Indy/([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"Delta Server Management Interface\"\r\n| p/Indy httpd/ v/$1/ i/Avaya IP Office Delta Server/ d/PBX/
match http m|^HTTP/1\.1 200 OK\r\n.*<!--\r\n#\r\n# If you have a 'split' directory installation, with configuration\r\n# files in ~/\.i2p \(Linux\) or %APPDATA%\\I2P \(Windows\), be sure to\r\n# edit the file in the configuration directory, NOT the install directory\.\r\n#\r\n--><title>I2P Anonymous Webserver</title>|s p/I2P anonymous httpd/
match http m|^HTTP/1\.1 401 Unauthorized\r\nServer: Sun-Java-System-Web-Proxy-Server/([\w._-]+)\r\n.*WWW-authenticate: basic realm=\"Web Proxy Server Administration\"\r\n|s p/Sun Java System Web Proxy http admin/ v/$1/
match http m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Basic realm=\"Admin\"\r\nContent-Length: 0\r\n\r\n$| p/Juniper Steel-Belted Radius http config/ o/Windows/
match http m|^HTTP/1\.1 200 OK\r\nServer: PageR Enterprise/([\w._-]+)\r\nContent-Type: text/html\r\nCache-Control: no-cache, no-store, must-revalidate \r\n\r\n| p/Avtech PageR Enterprise http interface/
match http m|^HTTP/1\.0 200 OK\r\nContent-type: text/html\r\nConnection: close\r\n\r\n<html><head><link rel=stylesheet type=text/css href=indexStyle\.css><title>Healy LDS Temperature #1</title>.*Sensor 1</td>.*>([\w.]*)</td>.*&deg;([CF])</td>.*Sensor 2</td>.*>([\w.]*)</td>.*&deg;([CF])</td>.*Sensor 3</td>.*>([\w.]*)</td>.*&deg;([CF])</td>.*Sensor 4</td>.*>([\w.]*)</td>.*&deg;([CF])</td>| p/Xytronics X-DAQ-2R1-4T-I temperature sensor http interface/ i/temperatures: $1 $2, $3 $4, $5 $6, $7 $8/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: FitNesse-v([\w._-]+)\r\n|s p/FitNesse httpd/ v/$1/
match http m|^HTTP/1\.1 302 Moved Temporarily\r\n.*Location: https?://([\w._-]+)/esa\r\n.*Server: Clearwell\r\n\r\n|s p/Clearwell httpd/ h/$1/
match http m|^HTTP/1\.1 302 Found\r\nLocation: http:///logon\.htm\r\nContent-Length: 0\r\nServer: Intel\(R\) Con\. Management Engine ([\w._-]+)\r\n\r\n$| p/Intel Con. Management Engine httpd/ v/$1/
match http m|^HTTP/1\.1 401 Authorization Required\r\n.*Server: mpd web server\r\n|s p/mpd web server/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: BitMeterOS ([\w._-]+) Web Server\r\n|s p/BitMeter OS bandwidth monitor httpd/ v/$1/
match http m|^HTTP/1\.0 302 Found\r\nMIME-Version: 1\.0\r\nAccept-Ranges: bytes\r\nServer: NaviServer/([\w._-]+)\r\nDate: .*\r\nLocation: http://filemaker\.local:\d+/login\r\n| p/NaviServer httpd/ v/$1/ i/FileMaker Server/
match http m|^HTTP/1\.0 200 OK\r\nServer: Lightstreamer/([\w._ -]+) \(Lightstreamer Push Server - www\.lightstreamer\.com\) Moderato edition\r\nContent-Type: text/html\r\nExpires: Thu, 1 Jan 1970 00:00:00 GMT\r\n| p/Lightstreamer httpd/ v/$1/
match http m|^HTTP/1\.1 404 Not Found\r\nContent-type: text/html\r\nConnection: close\r\nDate: .*\r\n\r\n<HTML><HEAD><TITLE>Error 404</TITLE></HEAD><BODY><H1>Error 404</H1><P>Not Found</P></BODY></HTML>$| p/Ingrian Security Encryption http config/ d/security-misc/
match http m|^HTTP/1\.0 302 Found\r\n.*Location: http://([\w._-]+):\d+/status/hostgroup\r\nContent-Length: 113\r\nContent-Type: text/html; charset=utf-8\r\nExpires: Thu, 01 Jan 1970 00:00:00 GMT\r\nStatus: 302\r\n\r\n<html><body><p>This item has moved <a href=\"http://[\w._-]+:\d+/status/hostgroup\">here</a>\.</p></body></html>|s p/OpsView remote management/ h/$1/
match http m|^HTTP/1\.1 200 OK\r\nDate: .*\r\nServer: KM-httpd/([\w._-]+)\r\n| p/Kyocera FS-3900DN printer http config/ v/$1/ d/printer/
match http m|^HTTP/1\.1 401 Unauthorized\r\nConnection: close\r\nContent-Length: 0\r\nServer: DMRND/([\w._-]+)\r\n\r\n| p/DMRND httpd/ v/$1/ i/Samsung TV/ d/media device/
match http m|^HTTP/1\.0 404 Not Found\r\ncontent-length : 90\r\ncontent-type : text/html\r\n\r\n<html>\n<pre><html><h2>404 Not Found</h2>The server could not locate the resource you requested</html>\0</pre>\n</html>$| p/McAfee virus scanner http admin/ d/security-misc/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: iroffer-dinoex/([\w._-]+)\r\n|s p/iroffer-dinoex httpd/ v/$1/
match http m|^HTTP/1\.0 200 Ok\r\r\nContent-type: text/html\r\r\n\r\r\n<h1>BAD REQUEST: HACK DETECT</h1>\r\n\r\nCHAT\.PHP\.SPB\.RU - Chat software \(c\) Dmitry Borodin - http://php\.spb\.ru/chat/\r\n| p/chat.php.spb.ru chat server httpd/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: TMeter\r\n.*<Copyright>Copyright \(c\) \d+-\d+ Alexey Kazakovsky</Copyright>.*<Version>([\w._ -]+)</Version>|s p/TMeter traffic meter httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 400 Bad Request\r\nContent-Type: text/html; charset=utf-8\r\nServer: Mono-HTTPAPI/([\w._-]+)\r\nDate: .*\r\nContent-Length: 35\r\nConnection: close\r\n\r\n<h1>Bad Request \(Invalid host\)</h1>$| p/Mono-HTTPAPI/ v/$1/ i/Beagle desktop search/
match http m|^HTTP/1\.1 404 Not Found\r\nServer: Asterisk/\r\n| p/Digium Asterix GUI httpd/ d/PBX/
match http m|^HTTP/1\.0 401 Unauthorized\r\nContent-Length: 91\r\nContent-Type: text/html\r\nX-Plex-Protocol: 1\.0\r\n\r\n<html><head><title>Unauthorized</title></head><body><h1>401 Unauthorized</h1></body></html>$| p/Plex Media Center httpd/ o/Mac OS X/
match http m|^HTTP/1\.0 302 Moved Temporarily\r\n.*Server: zope\.server\.http \(zope\.server\.http\)\r\n.*\r\nLocation: http://([\w._-]+):\d+/calendar\r\n|s p/Zope httpd/ i/SchoolTool calendar/
match http m|^HTTP/1\.1 302 Found\r\nLocation: https://[\d.]+:\d+/home\.html\r\nContent-Length: 0\r\nServer: Allegro-Software-RomPager/([\w._-]+)\r\n\r\n$| p/Allegro RomPager/ v/$1/ i/Xerox Phaser 8560DN printer/ d/printer/
match http m|^HTTP/1\.0 200 Ok\r\ncontent-length: \d+\r\ncontent-type: text/html\r\n\r\n<\?xml version=\"1\.0\" encoding=\"utf-8\"\?>.*<meta content=\"SOGo Web Interface\" name=\"description\" />.*<meta content=\"@[\w._-]+ ([\w._-]+)\" name=\"build\" />|s p/SOGo groupware httpd/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\n.*ETag: \"\d+\"\r\nContent-Type: text/html\r\nContent-Length: 79\r\nAccept-Ranges: bytes\r\nCache-Control: private\r\n\r\n<html><head><META http-equiv=\"refresh\" content=\"0;URL=(\w\w-\w\w)\.htm\"></head></html>|s p/Milestone XProtect video surveillance http interface/ i/$1/ d/webcam/
match http m|^HTTP/1\.1 302 Moved Temporarily\r\nDate: .*\r\nServer: Zild/([\w._-]+)\r\nContent-Type: text/plain\r\nLocation: https?://([\w._-]+):\d+/index\.csp\r\nConnection: close\r\n\r\n$| p/Zild httpd/ v/$1/ i|M/Monit network monitor|
match http m|^HTTP/1\.0 200 OK\r\nServer: private\r\nCache-Control: no-cache,no-store,max-age=0\r\npragma: no-cache\r\nContent-Type: application/octet-stream\r\nContent-Length: 101376\r\nAccept-Ranges: bytes\r\nDate: .*\r\nLast-Modified: .*\r\nExpires: .*\r\nConnection: close\r\n\r\nMZP\0\x02\0\0\0\x04\0\x0f\0\xff\xff\0\0\xb8| p/Neeris worm httpd/ o/Windows/
match http m|^HTTP/1\.0 404 Not Found\r\nServer: AdaptiveServerAnywhere/([\w._-]+)\r\n| p/Sybase Adaptive Server Anywhere httpd/ v/$1/
match http m|^HTTP/1\.1 401 Authorization Required\r\nConnection: close\r\nDate: .*\r\nServer: Simple-DNS-Plus/([\w._-]+)\r\nCa DNS Plus\"\r\nContent-Type: text/plain; charset=utf-8\r\nContent-Length: 36\r\n\r\n\*Error 401 Authorization Required\*\r\n$| p/Simple DNS Plus httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: AVGADMINSERVER-\w+ \d+ BUILD=(\d+) LOC=\d+ LIC=[\w-]+\r\n.*<h1>AVG Admin Server ([\w._-]+)</h1>|s p/AVG Administration Console httpd/ v/$2/
match http m|^HTTP/1\.0 200 OK\r\nDate: [A-Z]{3}, \d\d [A-Z]{3} \d\d\d\d \d\d:\d\d:\d\d GMT\r\n.*<TITLE>HP Web Console on ([\w._-]+)</TITLE>|s p/HP Guardian Service Processor httpd/ o/HP-UX/ h/$1/
match http m|^HTTP/1\.0 200 OK\r\nDate: \w\w, \d\d \w\w\w \d\d\d\d \d\d:\d\d:\d\d GMT\r\nServer: Texis-Monitor/([\w._-]+)\r\n| p/Thunderstone Texis-monitor httpd/ v/$1/
match http m|^HTTP/1\.1 302 Moved Temporarily\r\ndate: .*This is a WebSEAL error message template file\.|s p/IBM WebSEAL httpd/
match http m|^HTTP/1\.1 200 OK\r\nDate: .* GMT Standard Time\r\nLast-Modified: .* GMT Standard Time\r\nEtag: \"[0-9a-f.]+\"\r\nContent-Type: text/html\r\nContent-Length: 7\r\nConnection: close\r\nAccept-Ranges: bytes\r\n\r\nwelcome$| p/Mongoose httpd/
match http m|^HTTP/1\.0 200 cyberoam authentication response\r\nServer: awarrenhttp/([\w._-]+)\r\n| p/awarrenhttp httpd/ v/$1/ d/proxy server/ i/Cyberoam CR200 SSL VPN/
match http m|^HTTP/1\.1 301 Moved Permanently\r\nDate: .* UTC\r\nConnection: close\r\nLocation: /admin/public/index\.html\r\n\r\n$| p/Cisco ASA 5510 firewall http config/ d/firewall/
match http m|^HTTP/1\.0 302 Moved Temporarily\r\nDate: .*\r\nServer: Mbedthis-Appweb/([\w._-]+)\r\nContent-length: 0\r\nConnection: close\r\nLocation: http://([\w._-]+):\d+/index\.html\r\n\r\n$| p/Mbedthis-Appweb/ v/$1/ h/$2/ i/Iomega StorCenter sohoclient/ o/Windows/
match http m|^HTTP/2\.0 302 Found\r\nServer: SmarterTools/([\w._-]+)\r\n.*X-AspNet-Version: ([\w._-]+)\r\n.*Location: /Login\.aspx\r\n|s p/SmarterTools httpd/ v/$1/ i/ASP.NET $2/ o/Windows/
match http m|^HTTP/1\.1 200 OK\r\n.*Set-Cookie: _sonar_session=[\w+%-]+; path=/; HttpOnly\r\n|s p/Sonar code quality management httpd/
match http m|^HTTP/1\.1 200 OK\r\nContent-Length: 0\r\nContent-Type: text/html\r\nConnection: close\r\nServer: OpenEJB/\?\?\? \(unknown os\)\r\n\r\n$| p/OpenEJB httpd/
match http m|^HTTP/1\.0 302 Found\r\n.*Location: /index\.ds\r\n.*Server: DrWebAV-DeskServer/(REL-500-[\w._-]+) Linux/i686 Lua/([\w._-]+) OpenSSL/([\w._-]+)\r\n\r\n$|s p/Dr. Web AV-Desk httpd/ v/$1/ o/Linux/ i/i686; Lua $2; OpenSSL $3/
match http m|^HTTP/1\.0 200 OK\r\n.*Expires: Thu, 01 Jan 1970 00:00:00 GMT\r\n.*Server: vdradmind/([\w._-]+)\r\n|s p/VDR-Admin httpd/ v/$1/
match http m|^HTTP/1\.1 302 Found\r\nDate: .*\r\nServer: unknown\r\nLocation: https?://([\w._-]+)/workplace/access/home\r\n| p/SonicWALL SSL-VPN http proxy auth/ h/$1/

#(insert http)


# Maybe too generic?
match http m|^HTTP/1\.0 302 Found\r\nLocation: /html/en/index\.html\r\n\r\n$| p/peercast.org/
match http m|^HTTP/1\.0 404 Not found\r\n\r\n<HEAD><TITLE>File Not Found</TITLE></HEAD>\n<BODY><H1>File Not Found</H1></BODY>\n$| p/Bacula http config/
match http m|^HTTP/1\.[01] 302 Found\r\nConnection: Close\r\nContent-Length: 0\r\nContent-type: text/html\r\nDate: .*\r\nLocation: .*/login\.php\r\n\r\n| p/Kerio MailServer http config/ o/Windows/
match http m|^HTTP/1\.0 401 Authorization Required\r\nWWW-Authenticate: BASIC realm=\"Admin\"\r\n\r\nPassword Error\.\r\n\r\n$| p/D-Link DP-301P+ print server http config/ d/print server/
match http m|^HTTP/1\.0 401 Unauthorized\nContent-type: text/html\r\nDate: .*\r\nConnection: close\r\nWWW-Authenticate: Basic realm=\"Web Server Authentication\"\r\n\r\n<HEAD><TITLE>401 Unauthorized</TITLE></HEAD>\n<BODY><H1>401 Unauthorized</H1>\n\n</BODY>\n$| p/Accton VM1188T VoIP phone http config/ d/VoIP phone/
# Seen for OpenPegasus, VMware ESX CIM server, Microsoft SCX CIM Server.
match http m|^HTTP/1\.1 501 Not Implemented\r\n\r\n$| p/Web-Based Enterprise Management CIM serverOpenPegasus WBEM httpd/ o/Linux/
match http m|^HTTP/1\.1 302 Found\r\nLocation: http://[\d.]+:8080/\r\nContent-Length: 0\r\n\r\n$| p/Red Condor antispam appliance http config/ d/proxy server/

# This one can cause false results!
# Found a better one and put it in FourOhFour
#match http m|^HTTP/1\.0 404 Not Found\r\nConnection: close\r\n\r\n$| p/apt-proxy httpd/

# Fairly general:
#match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: micro_httpd\r\n| p/micro_httpd/
#match http m|^HTTP/1\.0 200 OK\r\nServer: RapidLogic/([\d.]+)\r\n| p/RapidLogic/ v/$1/
# http://svn.dd-wrt.com:8000/dd-wrt/browser/src/router/httpd/httpd.c
match http m|^HTTP/1\.0 200 Ok\r\n.*Server: httpd\r\n|s p/DD-WRT milli_httpd/ o/Linux/ d/WAP/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: GoAhead-Webs\r\n| p/GoAhead-Webs httpd/
match http m|^HTTP/1\.0 200 OK\r\nServer: SimpleHTTP/([\d.]+) Python/([\d.]+)\r\n| p/SimpleHTTPServer/ v/$1/ i/Python $2/
match http m|^HTTP/1\.0 \d\d\d .*\r\n.*Server: Mbedthis-App[Ww]eb/([\d.]+)\r\n|s p/Mbedthis-Appweb/ v/$1/
match http m|^HTTP/1\.0 302 moved temporarily\r\n.*Server: Tntnet/([\w._-]+)\r\n|s p/Tntnet/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: PasteWSGIServer/([-\w_.]+) Python/([-\w_.]+)\r\n| p/PasteWSGIServer/ v/$1/ i/Python $2/
match http m|^HTTP/1\.1 200 OK\r\nServer: Quickserve/([\w._-]+)\r\n| p/Quickserve httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d [^\r\n]*\r\n.*Server: Allegro-Software-RomPager/([\d.]+)\r\n|s p/Allegro RomPager/ v/$1/
match http m|^HTTP/1\.[01] 200 OK\r\n.*Server: BaseHTTP/([\d.]+) Python/([\w.]+)\r\n|s p/BaseHTTP/ v/$1/ i/Python $2/
match http m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\nConnection: Keep-Alive\r\nServer: FlashCom/([\w._-]+)\r\nCache-Control: no-cache\r\nContent-Length: 0\r\n\r\n$| p/FlashCom httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d [^\r\n]*\r\n.*Server: thin ([\w._-]+) codename ([\w\s]+)\r\n|s p/Thin/ v/$1/ i/codename $2/
match http m|^HTTP/1\.0 \d\d\d .*\r\n.*Server: WYM/([\d\.]+)\r\n|s p/WYM httpd/ v/$1/
match http m|^HTTP/1\.0 200 Ok\r\nServer: NET-DK/([\d.]+)\r\n| p/NET-DK/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\n.*Server: Virata-EmWeb/R([\d_]+)\r\n|s p/Virata-EmWeb/ v/$SUBST(1,"_",".")/
match http m|^HTTP/1\.0 404 File Not Found\r\nContent-Type: text/html\r\n\r\n<b>The file you requested could not be found</b>\r\n$| p/Icecast streaming media server/
match http m|^HTTP/1\.1 \d\d\d .*\r\n.*Server: Mono-HTTPAPI/([\w._-]+)\r\n|s p/Mono-HTTPAPI/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*<a href=\"http://jetty\.mortbay\.org/?\">Powered by Jetty://</a>|s p/Jetty httpd/
match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: CherryPy/([\w._-]+)\r\n|s p/CherryPy httpd/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*Server: CherryPy/([\w._-]+) ([^\r\n]+)\r\n|s p/CherryPy httpd/ v/$1/ i/$2/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: NetBox Version ([\w._-]+ Build \d+)\r\n| p/NetBox httpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: OmikronHTTPOrigin/([\w._-]+)\r\n| p/OmikronHTTPOrigin httpd/ v/$1/
match http m|^HTTP/1\.[01] \d\d\d .*\r\n.*Server: Zope/\((?:Zope )?([\d\w][^\,\)]+),?\s*([^\)]+)\)\S*\s+([^\r]+)\r\n|s p/Zope httpd/ v/$1/ i/$2; $3/
match http m|^HTTP/1\.[01] \d\d\d .*\r\n.*Server: zope\.server\.http \(zope\.server\.http\)\r\n|s p/Zope httpd/
match http m|^HTTP/1\.[01] \d\d\d .*\r\n.*Server: zope\.server\.http \(HTTP\)\r\n|s p/Zope httpd/
match http m|^HTTP/1\.[01] \d\d\d .*\r\n.*X-Powered-By: Zope \(www\.zope\.org\), Python \(www\.python\.org\)\r\n|s p/Zope httpd/
# src/connections.c
match http m|^HTTP/1\.0 \d\d\d .*Server: lighttpd/([\w._-]+).*<\?xml version=\"1\.0\" encoding=\"iso-8859-1\"\?>\n<!DOCTYPE html PUBLIC \"-//W3C//DTD XHTML 1\.0 Transitional//EN\"\n         \"http://www\.w3\.org/TR/xhtml1/DTD/xhtml1-transitional\.dtd\">\n<html xmlns=\"http://www\.w3\.org/1999/xhtml\" xml:lang=\"en\" lang=\"en\">\n <head>\n  <title>\d\d\d - [\w ]+</title>|s p/lighttpd/ v/$1/
match http m|^HTTP/1\.0 \d\d\d .*<\?xml version=\"1\.0\" encoding=\"iso-8859-1\"\?>\n<!DOCTYPE html PUBLIC \"-//W3C//DTD XHTML 1\.0 Transitional//EN\"\n         \"http://www\.w3\.org/TR/xhtml1/DTD/xhtml1-transitional\.dtd\">\n<html xmlns=\"http://www\.w3\.org/1999/xhtml\" xml:lang=\"en\" lang=\"en\">\n <head>\n  <title>\d\d\d - [\w ]+</title>|s p/lighttpd/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Optenet Web Server\r\n| p/Optenet httpd/
match http m|^HTTP/1\.0 200 OK\n.*Server: uClinux-httpd ([\w._-]+)\n|s p/uClinux-httpd/ v/$1/ o/Linux/



# No more HTTP softmatch because many services that I don't think are
# best classified 'http' use http-like semantics (for example UPnP,
# some https servers, etc).  Maybe I should make softmatch allow
# future services that start with the service name, and relable all of
# those.  Shrug.  For now it is gone.
# softmatch http m|^HTTP/1.[01] \d\d\d|

# OCSP malformedRequest response status (1).
match http-ocsp m|^HTTP/1\.0 200 OK\r\nContent-type: application/ocsp-response\r\nContent-Transfer-Encoding: Binary\r\nContent-Length: 5\r\n\r\n0\x03\n\x01\x01$| p/OCSP over HTTP/

match http-proxy m|^HTTP/1\.1 401 Unauthorized\r\nConnection: closed\r\nContent-Length: \d+\r\nWWW-Authenticate: Basic realm=\"WebWasher configuration\"\r\n| p/WebWasher filtering proxy/ o/Windows/
match http-proxy m|^HTTP/1\.0 400 Bad Request\r\n.*<html><head><title>WebWasher - Error 400: Bad Request</title>|s p/WebWasher filtering proxy/ o/Windows/
match http-proxy m|^HTTP/1\.1 400 Bad Request\r\n.*<title>Webwasher - Notification</title>\r\n|s p/WebWasher filtering proxy/ o/Windows/
match http-proxy m|^HTTP/1\.0 400 Ung\xfcltige Anforderung\r\nConnection: Close\r\nContent-type: text/html\r\nPragma: no-cache\r\n\r\n<html><head><title>WebWasher - Fehler 400: Ung\xfcltige Anforderung</title>| p/WebWasher filtering proxy/ i/German/ o/Windows/

# MiddleMan filtering proxy server v1.5.2
# Middleman 1.8.3
match http-proxy m|^HTTP/1\.1 404 Not Found\r\nContent-Type: text/html\r\nContent-Length: 463\r\nConnection: close\r\nProxy-Connection: close\r\n\r\n<html><head><title>File not found</title></head><!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.01 Transitional//EN\">\n<body text=\"#000000\" bgcolor=\"#99AABB\"| p/Middleman filtering web proxy/
match http-proxy m|^HTTP/1\.0 \d\d\d .*\r\nServer: WWWOFFLE/(\d[-.\w]+)\r\n| p/WWWOFFLE caching webproxy/ v/$1/
match http-proxy m|^HTTP/1\.[01] 400 Host Not Found.*\r\n\r\n<html><head><title>The Proxomitron Reveals\.\.\.</title>|s p/Proxomitron universal web filter/ o/Windows/
match http-proxy m|^HTTP/1\.0 400 Bad Request\r\nDate: .*\r\n\r\n<html><body>.*<font color=\"#FF0000\">Proxy</font><font color=\"#0000FF\">\+</font> (\d[-.\w]+) \(Build #(\d+)\), Date: |s p/Fortech Proxy+ http admin/ v/$1 Build $2/ o/Windows/
match http-proxy m|^HTTP/1\.0 403 Forbidden\r\nDate: .*\r\n\r\n<html><body>.*</b> Registration key allows only ([\d]+) simultaneous users\..*>Proxy</font><font color=\"#0000FF\">\+</font> ([\d.]+) \(Build #(\d+)\),|s p/Fortech Proxy+ http admin/ v/$2 Build $3/ i/$1 concurrent users allowed/ o/Windows/
match http-proxy m|^HTTP/1\.0 \d\d\d .*\r\nServer: Jana-Server/(\d[-.\w]+)\r\n| p/JanaServer http proxy/ v/$1/ o/Windows/
match http-proxy m|^HTTP/1\.0 400 Bad Request\nContent-Type: text/html\n\n<HTML><HEAD><TITLE>DansGuardian - | p/DansGuardian HTTP proxy/
match http-proxy m|^HTTP/1\.0 400 Bad Request\r\nServer: FreeProxy/(\d[-.\w]+)\r\n| p/FreeProxy/ v/$1/
# EZproxy for Linux 2.2d GA (2003-09-01) - http://www.usefulutilities.com
match http-proxy m|HTTP/1\.[01] \d\d\d .*\r\nServer: EZproxy\r\n|s p/EZproxy web proxy/
# http://bfilter.sourceforge.net/
match http-proxy m|^HTTP/1\.0 400 Bad Request\r\n.*\r\n\r\n<!DOCTYPE html PUBLIC \"-//W3C//DTD HTML 4\.01 Transitional//EN\">\r\n<html>\r\n<head>\r\n  <title>BFilter Error</title>|s p/Bfilter proxy/
match http-proxy m|^HTTP/1\.0 501 Not Implemented\r\n.*<STRONG>\nUnsupported Request Protocol\n</STRONG>\n</UL>\n<P>\nBFilter does not support all request methods for all access protocols\.\n|s p/Bfilter proxy/
match http-proxy m|^HTTP/1\.0 \d\d\d .*\r\nServer: tinyproxy/(\d[-.\w]+)\r\n| p/Tinyproxy/ v/$1/
# MS ISA Server 2000 enterprise edition on windows 2000 advanced server
match http-proxy m|^HTTP/1\.1 502 Proxy Error \( The Uniform Resource Locator \(URL\) does not use a recognized protocol\. Either the protocol is not supported or the request was not typed correctly\. Confirm that a valid protocol is in use \(for example, HTTP for a Web request\)\.| p/Microsoft ISA Server http proxy/ o/Windows/
match http-proxy m|^HTTP/1\.1 502 Proxy Error \( L'URL \(Uniform Resource Locator\) n'utilise pas de protocole reconnu\. Soit le protocole n'est pas pris en charge, soit la demande n'a pas \xe9t\xe9 tap\xe9e correctement\.| p/Microsoft ISA Server Web Proxy/ i/French/ o/Windows/
match http-proxy m|^HTTP/1\.1 407 Proxy Authentication Required \( The ISA Server requires authorization to fulfill the request\. Access to the Web Proxy service is denied\.  \)\r\n| p/Microsoft ISA Server Web Proxy/ i/Proxy auth required/ o/Windows/
match http-proxy m|^HTTP/1\.1 407 Proxy Authentication Required \( El servidor ISA requiere autorizaci\xc3\xb3n para completar la petici\xc3\xb3n\. Acceso denegado al servicio de proxy web\.  \)\r\n| p/Microsoft ISA Server Web Proxy/ i/Spanish; Proxy auth required/ o/Windows/
match http-proxy m|^IsException=TRUE\r\nExceptionMsg=| p/Microsoft ISA Server Web Proxy/ o/Windows/
# Privoxy 3.0.0 Filtering Web Proxy - http://www.privoxy.org
match http-proxy m|^HTTP/1\.0 400 Invalid header received from browser\r\n\r\n$| p|Junkbuster/Privoxy webproxy|
match http-proxy m|^HTTP/1\.0 400 Invalid header received from browser\n\n| p/Junkbuster webproxy/
match http-proxy m|^HTTP/1\.0 400 Invalid header received from client\r\nProxy-Agent: Privoxy ([\w._-]+)\r\n| p/Privoxy http proxy/ v/$1/
match http-proxy m|^HTTP/1\.0 \d\d\d .*Server: NetCache \(NetApp/(\d[-.\w]+)\)\r\n|s p/NetApp NetCache http proxy/ v/$1/
# Not sure if the [-\w_.]+ is a hostname, it was netcache02
match http-proxy m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nContent-Length: \d+\r\nContent-Type: text/html\r\nServer: NetCache appliance \(NetApp/([-\w_.]+)\)\r\n| p/NetApp NetCache http proxy/ v/$1/
match http-proxy m|^HTTP/1\.0 \d\d\d .*Via: 1\.1 [-\w_.]+ \(NetCache NetApp/(\d[-.\w]+)\)\r\n\r\n<h1>Bad Request \(Invalid Hostname\)</h1>|s p/NetApp NetCache http proxy/ v/$1/
# Squid 2.5.STABLE3 on NetBSD 1.6ZA
match http-proxy m|^HTTP/1\.0 \d\d\d .*\r\nServer: [sS]quid/([-.\w+]+)\r\n|s p/Squid webproxy/ v/$1/
match http-proxy m|^HTTP/1\.0 \d\d\d .*\r\nServer: [sS]quid\r\n|s p/Squid webproxy/
# Blue Coat Port 80 Security Appliance  Model: Blue Coat SG400 Software Version: SGOS 2.1.6044 Software Release id: 19480 Service Pack 4
match http-proxy m|^HTTP/1\.1 504 Gateway Time-out\r\nConnection: close\r\nCache-Control: no-cache\r\nPragma: no-cache\r\nContent-Length: 2976\r\nContent-Type: text/html\r\n\r\n<DIV class=Section1> \n\t\t<P class=MsoNormal| p/Blue Coat Security Appliance http proxy/ o/SGOS/
match http-proxy m|^HTTP/1\.0 \d\d\d .*\r\nServer: MS-MFC-HttpSvr/([\w._-]+)\r\n| p/Microsoft Foundation Class httpd/ v/$1/ o/Windows/
match http-proxy m|^HTTP/1\.0 400 Cache Detected Error\r\nDate: .*\r\nContent-Type: text/html\r\nVia: 1\.0 ([-.\w]+) \(NetCache NetApp/([-.\w]+)\)\r\n\r\n| p/NetApp NetCache http proxy/ h/$1/ v/$2/
# Novell BorderManager HTTP-Proxy
match http-proxy m|^HTTP/1\.0 \d\d\d .*\r\nContent-Length: \d+\r\n\r\n.*<title>BorderManager Information Alert</title>|s p/Novell BorderManager HTTP-Proxy/
match http-proxy m|^HTTP/1\.0 400 Bad Request\r\nContent-type: text/html\r\n\r\n<html><head><title>InterScan Error</title></head>\r\n<body><h2>InterScan Error</h2>\r\nInterScan HTTP Version ([-\w_.]+) \$Date:| p/InterScan InterScan VirusWall/ v/$1/
# iPlanet-Web-Proxy-Server 3.6
match http-proxy m|^HTTP/1\.1 \d\d\d .*\r\nServer: IBM-PROXY-WTE-US/([\d.]+)\r\n| p/IBM-PROXY-WTE-US web proxy/ v/$1/
match http-proxy m|^HTTP/1\.1 \d\d\d .*Server: IBM-PROXY-FW/([\d.]+)\r\n|s p/IBM-PROXY-FW http proxy/ v/$1/
match http-proxy m|^<HTML><BODY bgColor=#FFFFFF link=#0000CC text=#000000 vLink=#CCCC88><TITLE>An error has occurred\.\.\.</TITLE><CENTER><TABLE width=600 border=0 cellpadding=2 cellspacing=1><TR bgcolor=#FFFFFF vAlign=top><TD width=\"90%\" colspan=2 bgcolor=#707888>| p/AnalogX web proxy/ i/misconfigured/
match http-proxy m|^HTTP/1\.0 \d\d\d .*\r\nContent-type: text/html\r\nContent-length: \d+\r\nWWW-authenticate: Basic realm=\"\(Password Only\) NAV for MS Exchange\"\r\n\r\n| p/NAV for MS Exchange/
match http-proxy m|^HTTP/1\.0 200 \nServer: VisualPulse \(tm\) ([\w.]+)\n| p/VisualPulse http proxy/ v/$1/
match http-proxy m|^HTTP/1\.0 302 Moved\r\nDate: .*\r\nServer: DeleGate/([\d.]+)\r\n| p/DeleGate proxy/ v/$1/
match http-proxy m|^HTTP/1\.0 302 Moved\r\nDate: .*\r\nServer: DeleGate| p/DeleGate proxy/
match http-proxy m|^HTTP/1\.0 200 OK\r\nProxy-agent: Netscape-Proxy/([\d.]+)\r\n| p/Netscape-proxy/ v/$1/
match http-proxy m|^HTTP/1\.0 504 Gateway Timeout\r\nContent-Type: text/html\r\nPragma: no-cache\r\n\r\n<H4><font COLOR=\"#FF0000\">Error parsing http request : </font></H2><p><pre>GET / / HTTP/1\.0\r\n\r\n</pre>| p/WinProxy http proxy/ o/Windows/
match http-proxy m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nContent-Length: \d+\r\nContent-Type: text/html\r\nServer: NetCache appliance \(NetApp/([\d.]+)\)\r\n\r\n| p/Network Appliance NetCache http proxy/ v/$1/ d/proxy server/
match http-proxy m|^HTTP/1\.0  500 \r\nProxy-agent: MultiCertify PROXY/([\d.]+)\r\n| p/MultiCertify http proxy/ v/$1/ o/Windows/
match http-proxy m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: HTTP::Proxy/([\d.]+)\r\n| p/Perl HTTP::Proxy/ v/$1/
match http-proxy m|^HTTP/1\.1 407 Proxy Authentication Required\r\nProxy-Authenticate: NTLM\r\nProxy-Authenticate: BASIC realm=\"DOMBUD\"\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n| p/CacheFlow http proxy/ o/CacheOS/
# Might match WinProxy as well? -Doug
match http-proxy m|^HTTP/1\.1 404 Not found\r\nConnection: close\r\nCache-Control: no-cache\r\nPragma: no-cache\r\nContent-Type: text/html\r\nContent-Length: 48\r\n\r\n<html><body>HTTP/1\.1 404 Not found</body></html>$| p/HTTHost TCP over HTTP tunneling proxy/
match http-proxy m|^HTTP/1\.0 401 Unauthorized\r\nServer: Telkonet Communications\r\n| p/Telkonet Communications http proxy/
match http-proxy m|^HTTP/1\.0 400 Bad Request\r\n.*X-Squid-Error: ERR_INVALID_|s p/Squid http proxy/
match http-proxy m|^HTTP/1\.0 503 Service Unavailable\r\n.*X-Squid-Error: ERR_CONNECT_FAIL 111\r\n|s p/Squid http proxy/
match http-proxy m|^HTTP/1\.0 403 Access Forbidden\r\nContent-Type: text/html\r\n\r\n<HTML><HEAD><TITLE>407 Proxy Authentication Required</TITLE></HEAD><BODY><H1>Proxy Authentication Required</H1><H4>Unable to complete request<P>Access denied due to authentication failure\.</H4><HR></BODY></HTML>\n\n\0| p/CA eTrust SCM http proxy/
match http-proxy m|^HTTP/1\.1 \d\d\d .*\r\nServer: FreeProxy/([\d.]+)\r\n| p/FreeProxy http proxy/ v/$1/ o/Windows/
match http-proxy m|^HTTP/1\.1 403 Forbidden\r\nContent-Type: text/html\r\nContent-Length: \d+\r\nCache-Control: no-cache\r\nPragma: no-cache\r\nConnection: Close\r\n\r\n<html><head><meta http-equiv=\"Content-Type\" content=\"text/html; charset=utf-8\"><TITLE>La solution mat\xc3\xa9rielle-logicielle WebShield&reg;| p/WebShield http proxy/ i/French/ o/Windows/
match http-proxy m|^HTTP/1\.1 403 Forbidden\r\nServer: Eplicator/([\d.]+)\r\n| p/Eplicator http proxy/ v/$1/
match http-proxy m|^AdsGone Blocked HTML Ad$| p/AdsGone http proxy/ o/Windows/
match http-proxy m|^<font face=verdana size=1>AdsGone (\d+)  Blocked HTML Ad</font>$| p/AdsGone $1 http proxy/ o/Windows/
match http-proxy m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nContent-Type: text/html\r\nPragma: no-cache\r\n\r\n<html>\n<head>\n<title>Proxy\+ WWW Admin interface</title>\n\n| p/Fortech Proxy+ http admin/ o/Windows/
match http-proxy m|^HTTP/1\.1 \d\d\d .*\r\nCache-Control: no-cache\r\nPragma: no-cache\r\nContent-Type: text/html.*\r\nProxy-Connection: close\r\nConnection: close\r\nContent-Length: \d+\r\n\r\n<HTML><HEAD>\n<TITLE>Access Denied</TITLE>\n</HEAD>.*\n<big>Access Denied \(policy_denied\)</big>\n|s p/BlueCoat SG-400 http proxy/ d/proxy server/
match http-proxy m|^HTTP/1\.1 \d\d\d .*\r\nCache-Control: no-cache\r\nPragma: no-cache\r\nContent-Type: text/html.*\r\nProxy-Connection: close\r\nConnection: close\r\nContent-Length: \d+\r\n\r\n<HTML><HEAD>\n<TITLE>Request Error</TITLE>\n</HEAD>.*\n<big>Request Error \(invalid_request\)</big>\n|s p/BlueCoat http proxy/
match http-proxy m|^HTTP/1\.0 \d\d\d .*\r\nServer: BlueCoat-Security-Appliance\r\n|s p/BlueCoat http proxy/ d/proxy server/
match http-proxy m|^HTTP/1\.1 302 Found\r\nServer: BlueCoat-Security-Appliance\r\nConnection: close\r\nLocation: /proxyclient/\r\n\r\n$| p/BlueCoat ProxyClient http interface/ d/proxy server/
match http-proxy m|^HTTP/1\.0 \d\d\d .*\r\nProxy-agent: BlueCoat-WinProxy\r\n| p/BlueCoat WinProxy http proxy/ o/Windows/ d/proxy server/
match http-proxy m|^HTTP/1\.0 \d\d\d .*\r\nServer: Sawmill/([-\w_.]+)\r\n|s p/BlueCoat Sawmill http proxy config/ v/$1/
match http-proxy m|^HTTP/1\.0 \d\d\d .*\r\nProxy-agent: BlueCoat-ProxyAV\r\n| p/BlueCoat ProxyAV appliance http proxy/ d/proxy server/
match http-proxy m|^HTTP/1\.0 \d\d\d .*\r\nPragma: no-cach\r\nContent-Type: text/html; charset=windows-1251\r\n\r\n| p/UserGate http proxy/ o/Windows/
match http-proxy m|^HTTP/1\.1 \d\d\d .*\r\nServer: Simple, Secure Web Server ([\d.]+)\r\n|s p/Symantec firewall http proxy/ i/Simple, Secure Web Server $1/ d/firewall/
match http-proxy m|^HTTP/1\.0 \d\d\d .*\r\nContent-Length: \d+\r\n.*<B>KEN! Proxy</B>|s p/AVM KEN! http proxy/
match http-proxy m|^HTTP/1\.0 400 Bad request\r\nContent-Type: text/html\r\nPragma: no-cache\r\n\r\n<H4><font COLOR=\"#FF0000\">Error parsing http request : </font></H2><p><pre>GET / / HTTP/1\.0\r\n\r\n</pre>| p/Kerio WinRoute Pro http proxy/ o/Windows/
match http-proxy m|^HTTP/1\.0 200 OK\r\n.*This request is not allowed\n\n\n by One1Stream Fastlane Acceleration Server\.,  Accelerating Server ([\d.]+)</font></p></body></html>|s p/One1Stream Fastlane accelerating http proxy/ v/$1/
match http-proxy m|^HTTP/1\.0 404 Proxy Error\r\nContent-type: text/html\r\nPragma: no-cache\r\nCache-control: no-cache\r\nContent-length: \d+\r\n\r\n<!DOCTYPE HTML PUBLIC \"-//IETF//DTD HTML 2\.0//EN\">\r\n<html><head><title>Proxy Error</title></head>\r\n<body><h1>Proxy Error</h1>\r\nThe proxy server could not handle this request\.\r\n<p>\r\n<b>bad file or wrong URL</b>\r\n</body></html>\r\n| p/Software602 602LAN Suite http proxy/ o/Windows/
match http-proxy m|^HTTP/1\.0 \d\d\d .*\r\nProxy-agent: Ositis-WinProxy\r\n| p/Ositis-WinProxy http proxy/ o/Windows/
match http-proxy m|^<Html><Body><H1> Unauthorized \.\.\.</H1></Body></Html>$| p/CCProxy http proxy/ o/Windows/
match http-proxy m|^<pre>\r\nIP Address: [\d.]+\r\nMAC Address: \r\nServer Time: .*\r\nAuth result: Invalid user\.\r\n</pre>| p/CCProxy http proxy/ o/Windows/
match http-proxy m|^HTTP/1\.0 401 Unauthorized\r\nServer: CCProxy\r\nWWW-Authenticate: Basic realm=\"CCProxy Authorization\"\r\n| p/CCProxy http proxy/ o/Windows/ i/unauthorized/
match http-proxy m|^HTTP/1\.0 407 Unauthorized\r\nServer: CCProxy\r\nProxy-Authenticate: Basic realm=\"CCProxy Authorization\"\r\n| p/CCProxy http proxy/ o/Windows/ i/unauthorized/
match http-proxy m|^HTTP/1\.[01] \d\d\d .*\r\nServer: WebMarshal Proxy\r\n|s p/WebMarshal http proxy/ o/Windows/
match http-proxy m|^HTTP/1\.0 400 Bad Request\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n.*<br>Protocol:http\n<br>Host: [N]ULL\n<br>Path:/\n<tr>|s p/Oops! http proxy/
match http-proxy m|^HTTP/1\.0 504 Gateway Timeout\. Or not in cache\r\n\r\n| p/Oops! http proxy/
match http-proxy m|^HTTP/1\.0 407 Proxy Authentication Required\r\nProxy-Authenticate: Basic realm=\"oops\"\r\n| p/Oops! http proxy/ i/Authentication Required/
match http-proxy m|^HTTP/1\.1 \d\d\d .*\r\nServer: Polipo\r\n|s p/Polipo http proxy/
match http-proxy m|^HTTP/1\.1 503 ERROR\nConnection: close\nContent-Type: text/html; charset=iso-8859-1\n\n<html>\n<head>\n<title>Error: Unable to resolve IP</title>| p/ffproxy http proxy/
match http-proxy m|^HTTP/1\.1 200 OK\r\ndate: .*\r\nconnection: close\r\n\r\n<html><body><pre><h1>Index of /</h1>\n<b>Name {53}Size {6}Last modified</b>\n\n| p/HTTP Replicator proxy/
match http-proxy m|^HTTP/1\.0 \d\d\d .*\r\nServer: BestHop ([\d.]+)\r\n|s p/BestHop CacheFly http proxy/ v/$1/
match http-proxy m|^HTTP/1\.0 407 Authentication failed\r\nConnection: close\r\nProxy-Connection: close\r\nProxy-Authenticate: Basic realm=\"HTTP proxy\"\r\n| p/Astaro Security http proxy/
match http-proxy m|^HTTP/1\.0 503 Service unavailable\r\n\r\n\r\n<html>\r\n<head>\r\n<title>Connect server failed</title>\r\n</head>\r\n<body >\r\n<h3>503 Can not connect server</h3>\r\nezProxy meets some difficulties to connect this WWW server\.| p/ezProxy http proxy/ o/Windows/
match http-proxy m|^HTTP/1\.1 403 Forbidden\r\nDate: .*\r\nServer: Mystery WebServer\r\nConnection: close\r\nContent-Type: text/html; charset=iso-8859-1\r\n\r\n<!DOCTYPE HTML PUBLIC \"-//IETF//DTD HTML 2\.0//EN\">\n<HTML><HEAD>\n<TITLE>403 Forbidden</TITLE>\n</HEAD><BODY>\n<H1>Forbidden</H1>\nYou don't have permission to access /\non this server\.<P>\n<HR>\n<ADDRESS>Mystery WebServer/([\d.]+) Server at ([-\w_.]+) Port \d+</ADDRESS>\n| p/Espion Interceptor http proxy/ v/$1/ h/$2/
match http-proxy m|^HTTP/1\.1 400 Bad Request .*Server: Traffic inspector HTTP/FTP[/ ]Proxy server \(([\w._-]+)\)\r\n|s p/Traffic Inspector http proxy/ v/$1/ o/Windows/
match http-proxy m|^HTTP/1\.0 200 OK\r\nCache-Control: no-store\r\nPragma: no-cache\r\nCache-Control: no-cache\r\nX-Bypass-Cache: Application and Content Networking System Software ([\d.]+)\r\n| p/Cisco ACNS outbound proxying/ v/$1/ i/**PROXIED**/

match http-proxy m|^<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.01 Transitional//EN\" \"http://www\.w3\.org/TR/html4/loose\.dtd\">.*ERROR: The requested URL could not be retrieved|s p/Squid http proxy/
match http-proxy m|^<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.01 Transitional//EN\" \"http://www\.w3\.org/TR/html4/loose\.dtd\">.*El URL solicitado no se ha podido conseguir|s p/Squid http proxy/ i/Spanish/
match http-proxy m|^<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.01 Transitional//EN\" \"http://www\.w3\.org/TR/html4/loose\.dtd\">.*A URL solicitada n&atilde;o pode ser recuperada|s p/Squid http proxy/ i/Portugese/
match http-proxy m|^<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.01 Transitional//EN\" \"http://www\.w3\.org/TR/html4/loose\.dtd\">.*La URL richiesta non pu&ograve; essere recuperata</TITLE>|s p/Squid http proxy/ i/Italian/
match http-proxy m|^<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.01 Transitional//EN\" \"http://www\.w3\.org/TR/html4/loose\.dtd\">.*L'URL demand&eacute;e n'a pu &ecirc;tre charg&eacute;e|s p/Squid http proxy/ i/French/
match http-proxy m|^<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 4\.01 Transitional//EN\" \"http://www\.w3\.org/TR/html4/loose\.dtd\">.*FEHLER: Der angeforderte URL konnte nicht geholt werden|s p/Squid http proxy/ i/German/

match http-proxy m|^HTTP/1\.1 \d\d\d .*\r\nServer: FSAV4IGW\r\n.*<html><head><title>F-Secure Internet Gatekeeper Welcome Page</title>|s p/F-Secure Internet Gatekeeper httpd/
match http-proxy m|^HTTP/1\.[01] \d\d\d .*\r\nServer: twproxy/([-\w_.]+)\r\n| p/ThunderWeb twproxy/ v/$1/
match http-proxy m|^HTTP/1\.0 302 Redirect\r\nPragma: no-cache\r\nCache-Control: no-cache\r\nContent-Length: 0\r\nConnection: close\r\nLocation: http://[-\w_.]+:\d+/nohost\r\n\r\n| p/Kerio WinRoute http proxy/ o/Windows/
match http-proxy m|^HTTP/1\.0 407 Proxy Authentication Required.*\r\nServer: HandyCache\r\n| p/HandyCache http caching proxy/ i/Russian/ o/Windows/
match http-proxy m|^HTTP/1\.0 \d\d\d .*Server: CF/v([\d.]+)\r\n.*X-Cache: MISS from CacheFORCE\r\n|s p/CacheForce http proxy/ v/$1/
match http-proxy m|^HTTP/1\.0 302 Found\r\nSet-Cookie:.*<TITLE>Novell Proxy</TITLE></HEAD><BODY><b><p>HTTP request is being redirected to HTTPS\.</b></BODY></HTML>\r\n|s p/Novell iChain http proxy/ o/NetWare/
match http-proxy m|^HTTP/1\.0 400 Bad Request\r\nServer: micro_proxy\r\n.*<ADDRESS><A HREF=\"http://www\.acme\.com/software/micro_proxy/\">micro_proxy</A>|s p/acme.com micro_proxy http proxy/
match http-proxy m|^HTTP/1\.0 403 Forbidden\r\n.*<br><b>Access denied due to Proxy\+'s Security settings!</b>|s p/Fortech Proxy+ http admin/ o/Windows/
match http-proxy m|^HTTP/1\.0 200 OK\r\nServer: URL Gateway ([-\w_.]+)\r\n| p/URL Gateway http proxy/ v/$1/ o/Windows/
match http-proxy m|^HTTP/1\.[01] \d\d\d .*Server: SonicWALL SSL-VPN Web Server\.?\r\n|s p/SonicWALL SSL-VPN http proxy/
match http-proxy m|^HTTP/1\.0 504 Web Acceleration Client Error \(400\.3\) - Missing Host Field in Request Header\r\nContent-type: text/html\r\nContent-length: \d+\r\n\r\n| p/HughesNet Web Acceleration http proxy/
match http-proxy m|^HTTP/1\.0 407 Proxy Authentication Required\r\nProxy-Authenticate: Basic realm=.*<h3>Access to requested resource disallowed by administrator or you need valid username/password to use this resource|s p/3Proxy http proxy/
match http-proxy m|^HTTP/1\.1 400 Malformed Request\r\nServer: WinGate ([\d.]+) \(Build (\d+)\)\r\n| p/WinGate httpd/ v/$1 build $2/ o/Windows/
match http-proxy m|^HTTP/1\.0 \d\d\d.*server: CoralWebPrx/([-\w_.]+) \(See http://coralcdn\.org/\)\r\n|s p/Coral Content Distribution Network http proxy/ v/$1/
match http-proxy m|^HTTP/1\.0 400 Bad Request\r\nContent-Type: text/html\r\n\r\nYou are trying to use a node of the CoDeeN CDN Network\.| p/CoDeeN Content Distribution Network http proxy/
match http-proxy m|^HTTP/1\.0 403 Request error by HAVP\r\n.*<title>Yoggie - Unknown Request</title>|s p/HAVP anti-virus web proxy/ i/Yoggie httpd/
match http-proxy m|^HTTP/1\.0 403 Request error by HAVP\r\n| p/HAVP anti-virus web proxy/
match http-proxy m|^HTTP/1\.1 407\r\nProxy-Authenticate: Basic realm=\"Proxy\"\r\nContent-Type: text/plain\r\n\r\nAccess denyed| p/Small HTTP Server http proxy/
match http-proxy m|^HTTP/1\.0 407 Proxy Authentication required\r\nDate: .*\r\nContent-Type: text/html\r\nProxy-Authenticate: Basic realm=\"Proxy\+ HTTP Proxy service\"\r\n| p/Proxy+ http proxy/ o/Windows/
match http-proxy m|^HTTP/1\.1 503 Freenet is starting up\r\n| p/Freenet FProxy/
match http-proxy m|^HTTP/1\.1 \d\d\d .*\r\nCache-Control: max-age=0, must-revalidate, no-cache, no-store, post-check=0, pre-check=0\r\n.*<title>Freenet FProxy Homepage|s p/Freenet FProxy/
match http-proxy m%^HTTP/1\.1 200 OK\r\nConnection: close\r\n.*<title>Browse Freenet \(Node id\|([\w._-]+)\) - Freenet</title>%s p/Freenet FProxy/ i/node id $1/
match http-proxy m|^HTTP/1\.1 200 OK\r\nConnection: close\r\n.*<title>Browse Freenet \(([\w._-]+)\) - Freenet</title>|s p/Freenet FProxy/ i/node id $1/
match http-proxy m|^HTTP/1\.[01] .*\r\nServer: Mikrotik HttpProxy\r\n|s p/Mikrotik http proxy/
match http-proxy m|^HTTP/1\.0 500 Internal Server Error\r\nCache-control: no-cache\r\nContent-type: text/html\r\n\r\n<HTML><HEAD><TITLE>SpoonProxy V([\w._-]+) Error</TITLE>| p/Pi-Soft SpoonProxy http proxy/ v/$1/ o/Windows/
match http-proxy m|^HTTP/1\.[01] \d\d\d .*\r\nServer: approx/([\w._~+-]+) Ocamlnet/([\w._-]+)\r\n|s p/Approx http proxy/ v/$1/ i/Ocamlnet $2/
match http-proxy m|^HTTP/1\.1 401 Unauthorized\nWWW-Authenticate: Basic realm=\"Anti-Spam SMTP Proxy \(ASSP\) Configuration\"\nContent-type: text/html\nServer: ASSP/([\w._-]+)\(?\)?\n| p/Anti-Spam SMTP Proxy http config/ v/$1/
match http-proxy m|^HTTP/1\.0 \d\d\d .*<b>Bad request format\.\n\t\t</b><p>Please, check URL\.<p>\t\t<hr>\t\tGenerated by <a href=\"http://www\.kingate\.net\"> kingate\(([\w._-]+)-win32\)</a>\.</body></html>\0\0|s p/kingate http proxy/ v/$1/ o/Windows/
match http-proxy m|^\njava\.net\.UnknownHostException: /\r\n\tat java\.net\.PlainSocketImpl\.connect\(Unknown Source\)\r\n| p/Apache JMeter http proxy/
match http-proxy m|^\r\n\r\njava\.net\.UnknownHostException: /\n\tat java\.net\.AbstractPlainSocketImpl\.connect\(AbstractPlainSocketImpl\.java:158\)\n| p/Apache JMeter http proxy/
match http-proxy m|^HTTP/1\.1 403 Bad Protocol\r\n.*<H1>I2P ERROR: NON-HTTP PROTOCOL</H1>The request uses a bad protocol\. The I2P HTTP Proxy supports http:// requests ONLY\. Other protocols such as https:// and ftp:// are not allowed\.<BR>|s p/I2P http proxy/
match http-proxy m|^HTTP/1\.1 405 Bad Method\r\n.*<H1>I2P ERROR: METHOD NOT ALLOWED</H1>The request uses a bad protocol\. The Connect Proxy supports CONNECT requests ONLY\. Other methods such as GET are not allowed - Maybe you wanted the HTTP Proxy\?\.<BR>|s p/I2P https proxy/
match http-proxy m|^HTTP/1\.0 502 Bad Gateway\r\nProxy-Connection: close\r\nContent-type: text/html; charset=us-ascii\r\n\r\n<html><head><title>502 Bad Gateway</title></head>\r\n<body><h2>502 Bad Gateway</h2><h3>Host Not Found or connection failed</h3></body></html>\r\n| p/3proxy http proxy/
match http-proxy m|^HTTP/1\.0 407 Proxy Authentication Required\r\nProxy-Authenticate: NTLM\r\nProxy-Authenticate: basic realm=\"proxy\"\r\nProxy-Connection: close\r\n.*<h2>407 Proxy Authentication Required</h2><h3>Access to requested resource disallowed by administrator or you need valid username/password to use this resource</h3>|s p/3proxy http proxy/ i|authentication required|
match http-proxy m|^HTTP/1\.0 404 Object not found\r\n.*<title>MIMEsweeper for Web :: ACCESS DENIED</title>|s p/Clearswift MIMEsweeper for web http proxy/ d/proxy server/
match http-proxy m|^HTTP/1\.1 200 .*<title>Web Filter Block Override</title>.*/XX/YY/ZZ/logo_fguard_wf\.gif|s p/Fortinet FortiGuard http proxy/ d/firewall/
match http-proxy m|^HTTP/1\.1 400 Bad Request\r\nServer: ziproxy\r\n.*\(ziproxy/([\w._-]+)\)</ADDRESS>|s p/ziproxy http proxy/ v/$1/
match http-proxy m|^HTTP/1\.1 400 Bad Request\r\nServer: ziproxy\r\n| p/ziproxy http proxy/
match http-proxy m|^HTTP/1\.0 400 Bad Request\r\n\r\n\0{872}$| p/Ncat http proxy/ v/0.2/ i/before Nmap 4.85BETA1/
match http-proxy m|^HTTP/1\.0 400 Bad Request\r\n\r\n$| p/Ncat http proxy/ i/Nmap 4.85BETA1 or later/
match http-proxy m|^HTTP/1\.1 404 Not found\r\nConnection: close\r\n.*<title>Proxy error: 404 Not found\.</title>\n.*<hr>Generated .* by Polipo on <em>([\w_.-]+):\d+</em>\.\n|s p/Polipo/ h/$1/
match http-proxy m|^HTTP/1\.1 401 Server authentication required\r\nConnection: close\r\n.*<title>Proxy error: 401 Server authentication required\.</title>.*<hr>Generated .*? by Polipo on <em>([\w._-]+):\d+</em>\.|s p/Polipo/ h/$1/
match http-proxy m|^HTTP/1\.0 500 Direct HTTP requests not allowed\nContent-type: text/html\n\n<font face=\"Bitstream Vera Sans Mono,Andale Mono,Lucida Console\">\nThe proxy is unable to process your request\.\n<h1><font color=red><b>Direct HTTP requests not allowed\.</b></font></h1>\n$| p/ratproxy/
match http-proxy m|^HTTP/1\.0 400 Bad Request\r\ncontent-type: text/html\r\n\r\n<h1>400</h1>\n<p>koHttpInspector: Could not understand the query: '/'</p>\n<hr>\n<address>Komodo Http Inspector, Port \d+</address>\n$| p/Komodo HTTP Inspector proxy/
match http-proxy m|^HTTP/1\.1 404 Not Found\r\nContent-Type: text/html\r\nContent-Length: \d+\r\nCache-Control: no-cache\r\nConnection: close\r\nProxy-Connection: close\r\n\r\n<style type=\"text/css\">\nbody{ font-family: Tahoma, Arial, sans-serif, Helvetica, Verdana; font-size: 11px; color: #000000; background-color: #FFFFFF; margin: 2 }\n| p/SafeSquid http proxy/
match http-proxy m|^HTTP/1\.0 302 Found\r\nServer: Distributed-Net-Proxy/([\d.]+)\r\nLocation: http://www\.distributed\.net/\r\n\r\n$| p/distributed.net personal key proxy httpd/ v/$1/
match http-proxy m|^HTTP/1\.0 200 OK\r\nServer: LastFMProxy/([\w.]+)\r\n| p/LastFMProxy HTTP-to-last.fm proxy/ v/$1/
match http-proxy m|^HTTP/1\.0 403 Forbidden\r\n.*<TITLE>\r\nFEHLER: Der Zugriff auf die angeforderte URL war nicht erfolgreich\r\n</TITLE>.*<B>KEN! DSL Proxy</B>|s p/AVM KEN! DSL http proxy/
match http-proxy m|^HTTP/1\.0 404 Not Found\r\n.*<title>HINWEIS: Der Zugriff auf die angeforderte URL war nicht erfolgreich</title>|s p/AVM FRITZ!Box Fon WAP http proxy/ d/WAP/
match http-proxy m|^HTTP/1\.0 404 Not Found\r\n.*<title>HINWEIS: Die Internetnutzung ist gesperrt\.</title>|s p/AVM FRITZ!Box Fon WLAN 7100-series http proxy/ d/WAP/
match http-proxy m|^HTTP/1\.0 407 Proxy access denied\r\nProxy-Authenticate: NTLM\r\nProxy-Connection: keep-alive\r\nContent-Length: 0\r\n\r\n$| p/ScanSafe http proxy/
match http-proxy m|^HTTP/1\.0 400 Bad Request\r\n.*Server: BaseHTTP/([\d.]+) Python/([\w._-]+)\r\n.*<head>\n<title>Error response</title>\n</head>\n<body>\n<h1>Error response</h1>\n<p>Error code 400\.\n<p>Message: Bad Request\.\n<p>Error code explanation: 400 = Bad request syntax or unsupported method\.\n</body>\n$|s p/BaseHTTP/ v/$1/ i/GAppProxy Google App Engine proxy; Python $2/
# Etisalat - United Arab Emirates telecom company.
match http-proxy m|^HTTP/1\.1 501 Not Implemented\r\n.*<title>This site is blocked</title>.*<img border=\"0\" src=\"http://([\w._-]+)/images-ip/ipblocked\.jpg\" \nuseMap=#links2 border=0>.*<area title=\"\" shape=RECT alt=\"\" coords=\"494, 20, 580, 105\" href=\"http://www\.etisalat\.ae\">|s p/Etisalat censorship http proxy/ i/site blocked/ h/$1/
match http-proxy m|^HTTP/1\.1 403 Forbidden\r\n.*<title>This site is blocked</title>.*<img border=\"0\" src=\"http://([\w._-]+)/images-ip/siteblocked\.jpg\" useMap=#links border=0>.*<area title=\"\" shape=RECT alt=\"\" coords=\"154, 449, 254, 463\" href=\"http://www\.etisalat\.ae/proxy\">|s p/Etisalat censorship http proxy/ i/site blocked/ h/$1/
match http-proxy m|^HTTP/1\.0 404 GlimmerBlocked\r\n| p/GlimmerBlocker http proxy/
match http-proxy m|^HTTP/1\.1 400 Bad Request \(Malformed HTTP request\)\r\n.*<HTML><TITLE>Vital Security Proxy Error</TITLE>|s p/Finjan Vital Security http proxy/
match http-proxy m|^HTTP/1\.0 400 Bad Request\r\nConnection: Close\r\n\r\n<HTML><HEAD>\n<TITLE>ERROR: The requested URL could not be retrieved</TITLE>\n</HEAD><BODY>\n<H2>The requested URL could not be retrieved</H2>\n<HR>\n<P>\nWhile trying to retrieve the URL:\n| p/Websense http proxy/
match http-proxy m|^HTTP/1\.0 \d\d\d .*\r\n.*Via: HTTP/1\.1 ([\w._-]+) \(Websense_Content_Gateway/([\w._-]+) \[c s f \]\)\r\n|s p/Websense Content Gateway http proxy/ v/$2/ h/$1/
match http-proxy m|^HTTP/1\.0 504 Gateway Timeout\r\nContent-Length: 237\r\n.*<p>The proxy server did not receive a timely response\nfrom the upstream server\.</p>|s p/Fortinet FortiGate-110c http proxy/ d/firewall/
match http-proxy m|^HTTP/1\.0 302 Moved Temporarily\r\nContent-length: 22\r\nConnection: close\r\nSet-Cookie: sslvpn-authck-orig-url=/; path=/\r\nSet-Cookie: sslvpn-authck-realm-name=Our Users; path=/\r\nLocation: /_formauth/login\.html\r\nContent-Type: text/plain\r\n\r\n302 Moved Temporarily\n$| p/Phion HTTPS VPN gateway/ d/proxy server/
match http-proxy m|^HTTP/1\.0 503 Service Unavailable\r\nCache-Control: no-cache\r\nConnection: close\r\nContent-Type: text/html\r\n\r\n<html><body><h1>503 Service Unavailable</h1>\nNo server is available to handle this request\.\n</body></html>\n$| p/Haproxy http proxy/ d/load balancer/
match http-proxy m|^HTTP/1\.0 200 OK\r\nCache-Control: no-cache\r\nConnection: close\r\nContent-Type: text/html\r\n\r\n<html><head><title>Statistics Report for HAProxy</title>| p/Haproxy http proxy/ d/load balancer/
match http-proxy m|^HTTP/1\.0 400\r\nContent-Type: text/html\r\n\r\n<html><head><title>Error</title></head><body>\r\n<h2>ERROR: 400</h2>\r\n<br>\r\n</body></html>\r\n$| p/Citrix Application Firewall/ d/firewall/
match http-proxy m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html; charset=utf-8\r\nContent-Length: 3366\r\nPragma: no-cache\r\n\r\n.*<style>\r\n\r\nh1, p, a, body {font-family: Arial;}\r\n\r\nh2\r\n{\r\n\ttext-align: center; \r\n\tfont: bold 20px Verdana, sans-serif; \r\n\tcolor: #00F; \r\n}|s p/Integard filtering http proxy management interface/ d/proxy server/
match http-proxy m|^HTTP/1\.0 502 Bad gateway\r\n\r\nBurp proxy error: invalid client request received: first line of request did not contain an absolute URL - try enabling invisible proxy support\r\n$| p/Burp Suite Pro http proxy/
match http-proxy m|^HTTP/1\.1 401 Unauthorized\r\nServer: RabbIT proxy version ([\w._-]+)\r\nContent-type: text/html; charset=utf-8\r\nCache-Control: no-cache\r\nPragma: no-cache\r\nDate: .*\r\nWWW-Authenticate: Basic realm=\"([\w._-]+):\d+\"\r\n| p/RabbIT http proxy/ v/$1/ h/$2/
match http-proxy m|^HTTP/1\.1 403 Forbidden\r\nServer: Lusca/([\w._-]+)\r\n| p/Lusca http proxy/ v/$1/
match http-proxy m|^HTTP/1\.0 403 Access Denied\r\nConnection: close\r\n\r\n<html>The request you issued is not authorized for GoogleSharing\.\n| p/GoogleSharing http proxy/
match http-proxy m|^HTTP/1\.0 503\r\nServer: Charles\r\n| p/Charles http proxy/

match imap-proxy m|^\* OK IMAP4 ready\r\nGET BAD invalid command\r\n| p/nginx imap proxy/

match magent m|^Agent Ready\.\.\.\r\n| p/MicroWorld mwagent.exe/ o/Windows/
match magent m|^Agent Ready\.\.\.\r\nGET / HTTP/1\.0\r\n\r\nGET 501 command not implemented ERROR\r\n| p/MicroWorld mwagent.exe/ o/Windows/
match escan-console m|^Agent Ready v([\w._]+)+\.\.\.\r\nGET / HTTP/1\.0 501 command not implemented ERROR\r\n 501 command not implemented ERROR\r\n| p/MicroWorld mwagent.exe/ v/$1/ o/Windows/ i/eScan antivirus management console/

match mas-financial m|^409 Invalid Protocol PVXAS/1\.0\r\n| p/MAS200 Financial System/ o/Windows/
match mas-financial m|^The Host cannot run the specified program\.$| p/MAS200 Financial System/ o/Windows/

match mrtgext-nlm m|^-1\n-1\n-1\n$| p/Novell NetWare MRTGEXT NLM Statistics/ o/NetWare/

match msn m|^{?Syntax Error : GET / HTTP/1\.0}? error\r\n$| p/amsn/
match msn m|^{?Erreur de syntaxe : GET / HTTP/1\.0}? error\r\n$| p/amsn/ i/French/
match msn m|^{? ?Erro de sintaxe : GET / HTTP/1\.0}? error\r\n$| p/amsn/ i/Portugese/
match msn m|^{?Errore di sintassi : GET / HTTP/1\.0}? error\r\n$| p/amsn/ i/Italian/

match icap m|^ICAP/1\.0 501 Method not implemented.*\r\nServer: IronNet/([\d.]+)\r\n\r\n|s p/IronNet Compliance Application/ v/$1/
match icap m|^ICAP/1\.0 501 Method not implemented.*\r\nService: ProxyAV AV scanner ([^\r\n]+)\r\n|s p/Blue Coat ProxyAV/ v/$1/
match icap m|^ICAP/1\.0 501 Other\r\nServer: Traffic Spicer ([\d.]+)\r\n| p/Traffic Spicer ICAP Server/ v/$1/


# gidentd 0.4.5 on Linux 2.4.X
match ident m|^0, 0 : ERROR : INVALID-PORT\r\n$| p/gidentd/
match ident m|^GET / HTTP/1\.0 : USERID : UNIX : ([-.\w]+)\r\n : USERID : UNIX : [-.\w]+\r\n| p/Nullidentd/ i/Claimed user: $1/
match ident m|^GET / HTTP/1\.0 : USERID : UNIX : ([-.\w]+)\r\n$| p/Liedentd/ i/Claimed user: $1/
# pidentd 2.81
match ident m|^0 , 0 : ERROR : X-INVALID-REQUEST\r\n$| p/pidentd/
# pidentd 3.1a25 on Linux 2.4.20 (SuSE 8.2)
match ident m|^GET : ERROR : UNKNOWN-ERROR\r\n$| p/pidentd/
match ident m|^0, 0 : ERROR : INVALID-AUTH-REQ-INFO : CAPABILITY=USER-INTERACTION : AUTH-MECH=KEBEROS_V4\r\n$| p/Stanford PC-leland identd/
# fair-identd-20000201
# pidentd-2.8.5-3
match ident m|^0 , 0 : ERROR : UNKNOWN-ERROR\r\n$| p/pidentd/ i/could be fair-identd/
# identd 1.1 on Linux 2.4.21
# linux-identd 1.2 - http://www.fukt.bth.se/~per/identd
match ident m|^GET / HTTP/1\.0 : ERROR : INVALID-PORT\r\n : ERROR : INVALID-PORT\r\n$| p/Linux-identd/ o/Linux/
# HP-UX ident
match ident m|^0 , 0 : ERROR : INVALID-PORT\r\n| p/HP-UX identd/ o/HP-UX/
match ident m|^GET / HTTP/1\.0 : USERID : UNIX : [^\r\n]+\r\n| p/KVIrc fake identd/

# uw-imap 2003debian0.0304182231-1
match imap m|^\* OK \[CAPABILITY IMAP4REV1 X-NETSCAPE LOGIN-REFERRALS STARTTLS LOGINDISABLED\] \[[-.\w]+\] IMAP4rev1 (200[-.\w]+) at .*\r\nGET BAD Command unrecognized/login please: /\r\n\* BAD Null command\r\n| p/UW imapd/
match imap m|^\* OK \[[-.+\w]+\] IMAP4rev1 v1(\d[-.\w]+) server ready\r\n| p/UW imapd/ v/1$1/
match imap m|^\* OK ([-.+\w]+) IMAP4rev1 v1(\d[-.\w]+) server ready\r\n| p/UW imapd/ h/$1/ v/1$2/
# gnu/mailutils imap4d 0.3.2 on Linux
match imap m|^\* OK IMAP4rev1\r\nGET BAD  Invalid command\r\n\* BAD  Null command\r\n$| p/GNU Mailutils imapd/
# Cyrus IMAP 2.1.14
match ssl/imap m|^\* BYE Fatal error: tls_start_servertls\(\) failed\r\n$| p/Cyrus imapd/
match imap m|^\* OK ([-\w_.]+)\r\nGET BAD Error in IMAP command received by server\.\r\n\* BAD Error in IMAP command received by server\.\r\n| p/Dovecot imapd/ h/$1/
match imap m|^\* OK .*\r\nGET BAD Error in IMAP command received by server\.\r\n\* BAD Error in IMAP command received by server\.\r\n| p/Dovecot imapd/
# Too general -- also matches Cyrus imapd 2.3.9.
# match imap m|^\* OK .*\r\nGET BAD Please login first\r\n| p/Dovecot imapd/ i/auth required/
match imap m|^\* OK IMAP4 IMAP4rev1 Server\r\nGET BAD Unrecognised Command\r\n| p/Floosietek FTgate imapd/
match imap m|^\* OK IMAP4r1 server \[([-\w_.]+)\] ready\r\nGET BAD Protocol Error: \"Unidentifiable command specified\"\.\r\n\* BAD Protocol Error: \"Tag not found in command\"\.\r\n| p/Microsoft Exchange imapd/ h/$1/ i/Version masked/ o/Windows/
match imap m|^\* OK IMAP4rev1 server ready at \d\d/\d\d/\d\d \d?\d:\d\d:\d\d\r\nGET BAD UNKNOWN Command\r\n\r\n BAD UNKNOWN Command\r\n| p/MailEnable imapd/ o/Windows/
match imap m|^\* OK IMAP4rev1 server ready\r\nGET BAD Unknown command '/'\r\n BAD Unknown command ''\r\n| p/Kerio imapd/
match imap m|^\* OK Gimap ready for requests from [\d\.]+ ([\w\d]+)| p/Google Gmail imapd/ i/$1/
match imap m|^\* OK .*IMAP4rev1 Server Completed\r\nGET BAD Protocol Error: Invalid IMAP command specified\r\n| p/Cisco imapd/
# embyte
match imap m|^\* OK  MailSite IMAP4 Server ([-.\w]+) ready| p/MailSite imapd/ v/$1/
match imap m|^\* OK ([\w._-]+) Welcome \(cimap\)\r\nGET BAD Invalid command \(/\)\r\n\* BAD - command line Insufficient tokens \(\)\r\n| p/SurgeMail imapd/ h/$1/
match imap m|^GET NO Error in IMAP command received by server\.\r\n| p/cPanel Courier imapd/
match imap m|^\* OK IMAPrev1\r\nGET BAD Unknown or NULL command\r\n BAD NULL COMMAND\r\n| p/hMailServer imapd/ o/Windows/

# Server: CUPS/1.1
match ipp m|^HTTP/1\.0 \d\d\d .*<TITLE>Home - CUPS ([\d.]+)</TITLE>.*SUMMARY=\"Common UNIX Printing System|s p/CUPS/ v/$1/
match ipp m|^HTTP/1\.0 \d\d\d .*\r\nServer: CUPS/([-\w_.]+)|s p/CUPS/ v/$1/
match ipp m|^lpd \[@[-.\w]+\]: Host name for your address \([:.\d]+\) is not known\n$| p/CUPS/
match ipp m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nServer: EPSON-IPP/([\d.]+)\r\nContent-Type: application/ipp\r\nContent-Length: \d+\r\n\r\n| p/Epson ippd/ v/$1/ d/print server/
match ipp m|^HTTP/1\.0 404 Not Found\r\nCache-Control: no-cache\r\nDate: .*\r\nPragma: no-cache\r\nContent-Type: text/html\r\nContent-Length: 91\r\nServer: Web-Server/([\d.]+)\r\n\r\n<HTML><HEAD><TITLE>404 Not Found</TITLE></HEAD>\n<BODY><H1>404 Not Found</H1></BODY></HTML>\0| p/NRG copier or Ricoh Aficio/ i/Embedded Web-Server $1/ d/printer/
match ipp m|^HTTP/1\.1 404 Not Found\r\nConnection: close\r\nContent-Type: text/html\r\nContent-Length: 89\r\nServer: Web-Server/([\d.]+)\r\n\r\n<html><head><title>404 Not Found</title></head><body><h1>404 Not Found</h1></body></html>$| p/NRG copier or Ricoh Aficio printer/ i/Embedded Web-Server $1/ d/printer/
match ipp m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: CANON HTTP Server Ver(\d[-.\w ]+)\r\n| p/Canon printer web interface/ v/$1/
match ipp m|^HTTP/1\.1 \d\d\d .*\r\nDate: .*\r\nServer: Canon Http Server (\d[-.\w ]+)\r\n| p/Canon printer web interface/ v/$1/
match ipp m|^HTTP/1\.0 200 OK\r\nContent-Type: text/html\r\n\r\n<HTML><HEAD><META HTTP-EQUIV=\"Content-type\" CONTENT=\"text/html; charset=iso-8859-1\">\r\n<TITLE>IBM Infoprint Color (\d+)</TITLE>| p/IBM Infoprint Color $1 ippd/ d/printer/
match ipp m|^HTTP/1\.0 200 OK\r\nDate: .*\r\nMIME-version: 1\.0\r\nServer: ZOT-PS-17/([\d.]+)\r\nLast-Modified: .*\r\nExpires: .*\r\nPragma: no-cache\r\nContent-Type: text/html\r\nContent-Length: \d+\r\n\r\n| p|Longshine/TRENDnet USB Print Server| i/ZOT-PS-17 $1 httpd/ d/print server/
match ipp m|^HTTP/1\.1 301 Moved Permanently\r\nServer: Virata-EmWeb/R([\w_]+)\r\nLocation: https://[\d.]+/\r\nContent-Type: text/html\r\nContent-Length: 90\r\n\r\nMoved\r\n| i/HP Laserjet 4200 TN http config/ p/Virata-EmWeb/ v/$SUBST(1,"_",".")/ d/printer/
match ipp m|^HTTP/1\.0 \d\d\d .*\r\nContent-Type: text/html\r\n\r\n<HTML><HEAD><META HTTP-EQUIV=\"Content-type\" CONTENT=\"text/html; charset=iso-8859-1\">\r\n<TITLE>Dell Laser Printer 1700n</TITLE>| p/Dell Laser Printer 1700n ippd/ d/printer/
match ipp m|^HTTP/1\.0 \d\d\d .*<TITLE>Common UNIX Printing System</TITLE>.*HREF=\"http://www\.easysw\.com\" ALT=\"Easy Software Products Home Page\">\n|s p/Easy Software Products CUPS/
match ipp m|^<HEAD><TITLE>Not Found</TITLE></HEAD><BODY><H1><B>Not Found</B></H1><P>The requested URL \"\"was not found on this server\.</BODY>\r\n| p/Epson 980N Printer/ d/printer/
match ipp m|^HTTP/1\.0 400 Bad Request\r\nConnection: close\r\nContent-Type: text/html\r\n\r\nContent-Length: \d+\r\nCache-Control: no-cache\r\n\r\n<!DOCTYPE HTML PUBLIC \"-//W3C//DTD HTML 3\.2//EN\">\n<HTML>\n<HEAD>\n<TITLE>Invalid Request</TITLE>\n</HEAD>\n\n<BODY BGCOLOR=\"#FFFFFF\" TEXT=\"#000000\">\n<CENTER>\n<FONT SIZE=\"\+2\" COLOR=\"#FFFFFF\" ALIGN=\"Center\">\n</FONT>\n<B>Invalid Request\. Some Error</B>\n</BODY>\n\n</HTML>\n\n| p/Xerox Phaser 3500/ d/printer/
match ipp m|^HTTP/1\.0 200 OK\r\n.*\r\nServer: ZOT-PS-(\d+)/([\d.]+)\r\n|s p/ZOT-PS-$1 print server/ v/$2/ d/print server/
match ipp m|^HTTP/1\.0 404 Not found\r\n\r\n404 Not found$| p/Xerox WorkCentre IPP/ d/printer/
match ipp m|^HTTP/1\.0 404 Not Found\r\nDate: .*\r\nContent-Language: C\r\nUpgrade: TLS/1\.0,HTTP/1\.1\r\nConnection: close\r\nContent-Type: text/html\r\nContent-Length: 138\r\n\r\n<HTML><HEAD><TITLE>404 Not Found</TITLE></HEAD><BODY><H1>Not Found</H1>The requested resource was not found on this server\.</BODY></HTML>\n| p/Thecus N5200 IPP/ d/storage-misc/
match ipp m|^HTTP/1\.1 200 OK\r\nPragma: no-cache\r\nConnection: close\r\nContent-Type: text/html\r\n\r\n<HTML><HEAD><META HTTP-EQUIV=\"REFRESH\" CONTENT=\"0; URL=http://([\d.]+)/\"></HEAD><BODY><P>For more printserver info please open the <A HREF=\"http://([\d.]+)/\">([\d.]+)</A> home page</BODY></HTML>$| p/Kyocera Mita KM-1530 IPP/ d/printer/

match irc m|^:Default-Chat-Community 421 \* GET :Unknown command\r\n| p/Microsoft Exchange 2000 Server Chat Service/ o/Windows/
match irc m|^:([-\w_.]+) 451  :You have not registered your connection\r\n$| p/Wircsrv/ o/Windows/ h/$1/

match ingrian-xml m|^<GenericError><Success>false</Success><FatalError>101</FatalError><ErrorString>Could not parse client request</ErrorString></GenericError>| p/Ingrian NAE XML daemon/ d/security-misc/

# Jabber 1.4.2
match jabber m|^<stream:stream xmlns:stream='http://etherx\.jabber\.org/streams' version='([\d.]+)'>| p/Jabber instant messaging server/ i/Protocol $1/
match jabber m|^<stream:stream version='([\d.]+)' from='[\w._-]+' xmlns:stream='http://etherx\.jabber\.org/streams'>| p/Jabber instant messaging server/ i/Protocol $1/

match jabber m|^<\?xml version='1\.0'\?><stream:stream xmlns='jabber:client' xmlns:stream='http://etherx\.jabber\.org/streams' id='none' from='([\w._-]+)' version='([\d.]+)'>| p/ejabberd/ h/$1/ i/Protocol $2/
match jabber m|^<\?xml version='1\.0'\?><stream:stream xmlns='jabber:client' xmlns:stream='http://etherx\.jabber\.org/streams' id='\d+' from='([\w._-]+)' version='([\d.]+)'>| p/ejabberd/ h/$1/ i/Protocol $2/
match jabber m|^<\?xml version='1\.0'\?><stream:stream xmlns:stream='http://etherx\.jabber\.org/streams' xmlns='jabber:server' xmlns:db='jabber:server:dialback'| p/ejabberd/
match jabber m|^<\?xml version='1\.0'\?><stream:stream xmlns:stream='http://etherx\.jabber\.org/streams' xmlns='jabber:component:accept' id='none' from='([-\w_.]+)'><stream:error><xml-not-well-formed xmlns='urn:ietf:params:xml:ns:xmpp-streams'/></stream:error></stream:stream>| p/jit-transport jabber-ICQ transport/ h/$1/
match jabber m|^<stream:error>Invalid XML</stream:error>$| p/Jabber instant messaging server/
match jabber m|^<stream:error>Invalid XML</stream:error></stream:stream>$| p/Jabber instant messaging server/
match jabber m|^<stream:error><invalid-xml xmlns='urn:ietf:params:xml:ns:xmpp-streams'/><text xmlns='urn:ietf:params:xml:ns:xmpp-streams' xml:lang='en'>Invalid XML</text></stream:error>| p/jabberd instant messaging server/
match jabber m|^<\?xml version=\"1\.0\"\?><stream:stream id=\"none\" from=\"([\w._-]+)\" xmlns=\"jabber:client\" xmlns:stream=\"http://etherx\.jabber\.org/streams\" version=\"1\.0\"><stream:error><xml-not-well-formed xmlns=\"urn:ietf:params:xml:ns:xmpp-streams\"/></stream:error></stream:stream>$| p/Facebook Chat XMPP/
match jabber m|^<\?xml version='1\.0'\?><stream:stream id='' xmlns:stream='http://etherx\.jabber\.org/streams' version='1\.0' xmlns='jabber:server'><stream:error><xml-not-well-formed xmlns='urn:ietf:params:xml:ns:xmpp-streams'/></stream:error></stream:stream>$| p/Prosody Jabber server/
match jabber m|^<\?xml version='1\.0'\?><stream:stream id='' xmlns:stream='http://etherx\.jabber\.org/streams' version='1\.0' xmlns='jabber:client'><stream:error><xml-not-well-formed xmlns='urn:ietf:params:xml:ns:xmpp-streams'/></stream:error></stream:stream>$| p/Prosody Jabber client/

match james-admin m|^JAMES Remote Administration Tool ([\d.]+)\nPlease enter your login and password\nLogin id:\n| p/JAMES Remote Admin/ v/$1/

match jicp m|^d\x08\x1c\0\0\0Uncorrect JICP data type: 71$| p/Jade Inter Container Protocol/

match jxta m|^JXTAHELLO tcp://[\d.]+:\d+ tcp://[\d.]+:\d+ | p/JXTA P2P Collaboration daemon/

match kazaa-http m|^HTTP/1\.1 \d\d\d .*\r\nServer: giFT-FastTrack ([\d.]+)\r\nX-Kazaa-Username: giFTed\r\nX-Kazaa-Network: ([-.\w]+)\r\n| p/giFTed FastTrack P2P client/ v/$1/ i/network: $2/
match kazaa-http m|^HTTP/1\.1 \d\d\d .*\r\nServer: giFT-FastTrack ([\d.]+)\r\nX-Kazaa-Username: www\.k-lite\.com\.br\r\nX-Kazaa-Network: ([-.\w]+)\r\n| p/K-Lite FastTrack P2P client/ v/$1/ i/network: $2/

match kazaa-http m|^HTTP/1\.0 404 Not Found\r?\nX-Kazaa-Username: (\S+)\r\nX-Kazaa-Network: ([-.\w]+)\r\n| p/KaZaA P2P client/ i/username: $1; network: $2/
match kazaa-http m|^HTTP/1\.[01] 404 Not Found\r?\nServer: giFT-FastTrack ([\d.]+)\r\nX-Kazaa-Username: (\S+)\r\nX-Kazaa-Network: ([-.\w]+)\r\n| p/KaZaA P2P client/ v/$1/ i/username: $2; network: $3/

match kazaa-peerpoint m|^HTTP/1\.0 404 Not Found\n\r\n$| p/KaZaA P2P client Peer Point Manager/

match kerberos-sec m|^\0\0\0.~\x81.0\x81..\x03\x02\x01\x05.\x03\x02\x01\x1e.\x11\x18\x0f|s p/Mac OS X kerberos-sec/ o/Mac OS X/

match lcdproc m|^huh\? Invalid command \"GET\"\n| p/LCDProc screen interface daemon/

match listserv m|^The file name you specified is invalid\. LISTSERV files have names like\r\n\"BOARD\.MINUTES\" or \"XYZ-L LOG9303\" \(without the quotes\)\.\r\n| p/LISTSERV Administration service/

match megafillers m|^400 Unknown command\.\.\. Are you surprised\?\r\n$| p/MegaFillers game server/

match moneyworks m|^This is MoneyWorks; Server is on Windows\n$| p/MoneyWorks accounting software/ o/Windows/

match mosmig m|^GET \0\0\0\0TP/1\.0\r\n$| p/OpenMosix Process Migration Service/ o/Linux/

# Wrongly matches SSL in some cases
# match msdtc m|^...\0..$|s p/Microsoft Distributed Transaction Coordinator/ o/Windows/
match msdtc m|^..\x0a\0x\x01$|s p/Microsoft Distributed Transaction Coordinator/ o/Windows/
match msdtc m|^ERROR\n$|s p/Microsoft Distributed Transaction Coordinator/ i/error/ o/Windows/

# MLDonkey 2.5
match napster m|^1INVALID REQUEST$| p/MLDonkey multi-network P2P client/
match napster m|^1$| p/WinMX or Lopster Napster P2P client/
match bittorrent-tracker m|^HTTP/1\.1 404 Not Found\r\nServer: MLdonkey\r\nConnection: close\r\nContent-Type: application/x-bittorrent\r\nContentlength: 0\r\n\r\n| p/MLDonkey multi-network P2P client/
match bittorrent-tracker m|^HTTP/1\.1 200 OK\r\nServer: MLdonkey\r\n| p/MLDonkey P2P client http config/

match netbios-ssn m/^\x83\0\0\x01\x82|\x8f$/
match netwareip m|^\xfb\xff\xfe\xff\xfb\xff\xfe\xff\xfb\xff\xfe\xff$| p|Novell NetWare/IP| o|NetWare|

match ntrip m|^SOURCETABLE 200 OK\r\nServer: NTRIP Caster ([\w._-]+)/([\w._-]+)\r\nContent-Type: text/plain\r\n| p/Ntrip Caster/ v/$1/ i/protocol $2/

match giop m|^GIOP\x01\0\x01\x06\0\0\0\0$| p/omniORB omniNames/ i/Corba naming service/

match oem-agent m|^HTTP/1\.1 \d\d\d .*\r\nConnection: Close\r\nX-ORCL-EMSV: ([\d.]+)\r\n|s p/Oracle Enterprise Manager Agent httpd/ v/$1/

match opinionsquare m|^HTTP/1\.0 505 HTTP Version not supported\r\n\r\n$| p/OpinionSquare application/

# Oracle MTS Recovery Service 9.2.0.1 on Windows 2000 Professional
match oracle-mts m|^HTTP/1\.0 200 OK\r\nContent-length: 7\r\n\r\nunknown$| p/Oracle MTS Recovery Service/
# Windows 2003
match oracle-mts m|^HTTP/1\.0 400 Bad Request\r\nContent-length: 15\r\nContent-type: text/html\r\n\r\n400 Bad Request$| p/Oracle MTS Recovery Service/

match oracle-vs m|^\(err \(type xen\.xend\.XendError\.XendError\) \(value 'Invalid operation: GET'\)\)\n$| p/Oracle Virtual Service Agent/ i/Xen/
match oracle-vs m|^\(err \(type \"<class 'xen\.xend\.XendError\.XendError'>\"\) \(value 'Invalid operation: GET'\)\)\n$| p/Oracle Virtual Service Agent/ i/Xen/

match ormi m|^\xe3\r\n\r\n\0\x01\0.\0vInvalid protocol verification, illegal ORMI request or request performed with an incompatible version of this protocol|s p/Oracle Remote Method Invocation/
match ormi m|^\xe3\r\n\r\n\0\x01\0\x03\x0b\0vInvalid protocol verification, illegal ORMI request or request performed with an incompatible version of this protocol| p/Oracle Remote Method Invocation/

match ssl/pop3 m|^-ERR \[SYS/PERM\] Fatal error: tls_start_servertls\(\) failed\r\n$| p/Cyrus pop3sd/
match ssl/pop3 m|^-ERR Fatal error: pop3s: required OpenSSL options not present\r\n| p/Cyrus pop3sd/
# Postgresql-server-7.3.2-3
match postgresql m|^EFATAL:  invalid length of startup packet\n\0$| p/PostgreSQL/
match postgrey m|^action=dunno\n\n$| p/Postfix Greylist Daemon/
match powerchute m|^server=&type=0&id=&count=1&oid=[\d.]+&value=&error=4\n| p/APC Powerchute/ d/power-device/

match retrospect m|^\0\xca\0\0\0\0\0\x04\0\0\0\0$| p/Dantz Retrospect/ v/6.0/
match rfidquery m|^Error 0 parse error\n\nError 0 parse error\n\nError 0 parse error\n\nError 0 parse error\n\nError 0 parse error\n\nError 0 parse error\n\nError 0 parse error\n\n$| p/Mercury3 RFID Query protocol/
match rtsp m|^RTSP/1.0 400 Bad Request\r\nServer: DSS/([-.\w]+) \[(v\d+)]-(\w+)\r\n| p/DarwinStreamingServer/ v/$1/ i/$2 on $3/
match rtsp m|^RTSP/1\.0 400 Bad Request\r\nServer: QTSS/([\d.]+ \[v\d+\]-Win32)\r\nCseq: \r\n| p/Apple QuickTime Streaming Server/ v/$1/ o/Windows/
match rtsp m|^RTSP/1\.0 400 Bad Request\r\nServer: QTSS/([\d.]+ \[\d+\]-Linux)\r\nCseq: \r\n| p/Apple QuickTime Streaming Server/ v/$1/ o/Linux/
match rtsp m|^RTSP/1\.0 400 Bad Request\r\nServer: QTSS/([\d.]+) \(Build/([\d.]+); Platform/MacOSX; ([^)]*); \)\r\n| p/Apple QuickTime Streaming Server/ v/$1 build $2/ i/$3/ o/Mac OS X/
match rtsp m|^RTSP/1\.0 400 Bad Request\r\nServer: QTSS/([\d.]+) \(Build/([\d.]+); Platform/MacOSX\)\r\n| p/Apple QuickTime Streaming Server/ v/$1 build $2/ o/Mac OS X/
match rtsp m|^RTSP/1\.0 400 Bad Request\r\nServer: QTSS/v([\d.]+)\r\nCseq: \r\nConnection: Close\r\n\r\n| p/Apple QuickTime Streaming Server/ v/$1/

match rtsp m|^RTSP/1\.0 505 Protocol Version Not Supported\r\nDate: .*\r\nServer: WMServer/(\d[-.\w]+)\r\n\r\n$| p/Microsoft Windows Media Server/ v/$1/ o/Windows/
match rtsp m|^RTSP/1\.0 505 RTSP Version not supported\r\nCseq: \d+\r\nServer: fbxrtspd/([\d.]+) Freebox minimal RTSP server\r\n\r\n| p/Freebox minimal rtspd/ v/$1/ d/media device/
match rtsp m|^RTSP/1\.0 400 Bad Request\r\nCseq: \d+\r\nServer: fbxrtspd/([\w._-]+) Freebox RTSP server\r\n| p/Freebox rtspd/ v/$1/ d/media device/
match rtsp m|^RTSP/1\.0 400 Bad Request\r\nDate: .*\r\nAllow: OPTIONS, DESCRIBE, SETUP, TEARDOWN, PLAY, PAUSE, STATS\r\n\r\n| p/MediaPortal TV-Server rtspd/ d/media device/
match rtsp m|^HTTP/1\.0 401 Unauthorized\r\nConnection: close\r\nContent-Type: text/html; charset=ISO-8859-1\r\nWWW-Authenticate: Basic realm=\"server\r\nContent-Length: 166\r\n| p/Avtech MPEG4 DVR control rtspd/

match sassafras m|^/0 0 ([-\w_.]+)\r\n/0 0 HUH\r\n| p/Sassafras Key Server/ h/$1/

match seti-proxy m|^HTTP/1\.0 200 OK\r\nServer: SetiQueue/(\d+)\r\n| p/SetiQueue SETI@Home proxy/
match shell m|^\x01INTERnet ACP Error  Status = %SYSTEM-F-TOOMUCHDATA\r\n\0$| p/OpenVMS shelld/ o/OpenVMS/

# SHOUTcast Distributed Network Audio: www.shoutcast.com
match shoutcast m|^ICY 200 OK\r\n.*SHOUTcast Distributed Network Audio Server/Linux.v([\d.]+).*icy-name:(.*?)\r\n|s p/SHOUTcast server/ v/$1/ i/Name: $2/ o/Linux/
match shoutcast m|^ICY 200 OK\r\n.*SHOUTcast Distributed Network Audio Server/win32.v([\d.]+).*icy-name:(.*?)\r\n|s p/SHOUTcast server/ v/$1/ i/Name: $2/ o/Windows/
match shoutcast m|^ICY 200 OK\r\n.*SHOUTcast Distributed Network Audio Server/SolarisSparc.v([\d.]+).*icy-name:(.*?)\r\n|s p/SHOUTcast server/ v/$1/ i/Name: $2/ o/Solaris/
match shoutcast m|^ICY 200 OK\r\n.*SHOUTcast Distributed Network Audio Server/FreeBSD.v([\d.]+).*icy-name:(.*?)\r\n|s p/SHOUTcast server/ v/$1/ i/Name: $2/ o/FreeBSD/
match shoutcast m|^ICY 200 OK\r\n.*SHOUTcast Distributed Network Audio Server/posix.v([\d.]+).*icy-name:(.*?)\r\n|s p/SHOUTcast server/ v/$1/ i/Name: $2/ o/Unix/
match shoutcast m|^ICY 200 OK\r\n.*SHOUTcast Distributed Network Audio Server/MacOS_X.v([\d.]+).*icy-name:(.*?)\r\n|s p/SHOUTcast server/ v/$1/ i/Name: $2/ o/Mac OS X/
match shoutcast m|^ICY 401 Service Unavailable\r\n.*SHOUTcast Distributed Network Audio Server/UNIX OS-3 v([\d.]+)| p/SHOUTcast server/ v/$1/ o/Unix/

match shoutcast m|^ICY 200 OK\r\n.*SHOUTcast Distributed Network Audio Server/Linux.v([\d.]+)|s p/SHOUTcast server/ v/$1/ o/Linux/
match shoutcast m|^ICY 200 OK\r\n.*SHOUTcast Distributed Network Audio Server/win32.v([\d.]+)|s p/SHOUTcast server/ v/$1/ o/Windows/
match shoutcast m|^ICY 200 OK\r\n.*SHOUTcast Distributed Network Audio Server/SolarisSparc.v([\d.]+)|s p/SHOUTcast server/ v/$1/ o/Solaris/
match shoutcast m|^ICY 200 OK\r\n.*SHOUTcast Distributed Network Audio Server/FreeBSD.v([\d.]+)|s p/SHOUTcast server/ v/$1/ o/FreeBSD/
match shoutcast m|^ICY 200 OK\r\n.*SHOUTcast Distributed Network Audio Server/posix.v([\d.]+)|s p/SHOUTcast server/ v/$1/ o/Unix/

match shoutcast m|^ICY \d\d\d .*SHOUTcast Distributed Network Audio Server/Linux.v([\d.]+)|s p/SHOUTcast server/ v/$1/ o/Linux/
match shoutcast m|^ICY \d\d\d .*SHOUTcast Distributed Network Audio Server/win32.v([\d.]+)|s p/SHOUTcast server/ v/$1/ o/Windows/
match shoutcast m|^ICY \d\d\d .*SHOUTcast Distributed Network Audio Server/SolarisSparc.v([\d.]+)|s p/SHOUTcast server/ v/$1/ o/Solaris/
match shoutcast m|^ICY \d\d\d .*SHOUTcast Distributed Network Audio Server/FreeBSD.v([\d.]+)|s p/SHOUTcast server/ v/$1/ o/FreeBSD/
match shoutcast m|^ICY \d\d\d .*SHOUTcast Distributed Network Audio Server/posix.v([\d.]+)|s p/SHOUTcast server/ v/$1/ o/Unix/

match shoutcast-publishing m|^invalid password\r\n$| p/SHOUTcast publishing port/

match sip m|^SIP/2\.0 400 Illegal request line\r\nFrom: <sip:missing>\r\nTo: <sip:missing>;tag=badrequest\r\nUser-Agent: AVM FRITZ!Box Fon WLAN ([\d.]+) ([^\r\n]+)\r\n| p/AVM FRITZ!Box WLAN $1/ v/$2/ d/VoIP adapter/
match sip m|^SIP/2\.0 400 Illegal request line\r\nFrom: <sip:missing>\r\nTo: <sip:missing>;tag=badrequest\r\nUser-Agent: AVM FRITZ!Box Fon (\w+) \(UI\) ([^\r\n]+)\r\n| p/AVM FRITZ!Box $1/ v/$2/ d/VoIP adapter/
match sip m|^SIP/2\.0 400 Illegal request line\r\nFrom: <sip:missing>\r\nTo: <sip:missing>;tag=badrequest\r\nUser-Agent: AVM FRITZ!Box Fon ([^\r\n]+)\r\n|s p/AVM FRITZ!Box/ v/$1/ d/VoIP adapter/
match sip m|^SIP/2\.0 400 Illegal request line\r\nFrom: <sip:missing>\r\nTo: <sip:missing>;tag=badrequest\r\nUser-Agent: AVM FRITZ!Box WLAN ([\d.]+) ([^\r\n]+)\r\n| p/AVM FRITZ!Box WLAN $1/ v/$2/ d/VoIP adapter/
match sip m|^SIP/2\.0 400 Illegal request line\r\nFrom: <sip:missing>\r\nTo: <sip:missing>;tag=badrequest\r\nUser-Agent: AVM FRITZ!Fon ([\w_-]+) ([^\r\n]+)\r\n| p/AVM FRITZ!Fon $1/ v/$2/ d/VoIP adapter/
match sip m|^SIP/2\.0 400 Illegal request line\r\nFrom: <sip:missing>\r\nTo: <sip:missing>;tag=badrequest\r\nUser-Agent: AVM Speedport (W \w+) ([^\r\n]+)\r\n| p/Speedport $1/ v/$2/ d/VoIP adapter/
match sip m|^SIP/2\.0 400 Illegal request line\r\nFrom: <sip:missing>\r\nTo: <sip:missing>;tag=badrequest\r\nUser-Agent: AVM Sinus (W \w+) ([^\r\n]+)\r\n| p/AVM Sinus $1/ v/$2/ d/VoIP adapter/
match sip m|^SIP/2\.0 400 Illegal request line\r\nFrom: <sip:missing>\r\nTo: <sip:missing>;tag=badrequest\r\nUser-Agent: Speedport (W \w+) ([^\r\n]+)\r\n| p/T-Com Speedport $1/ v/$2/ d/VoIP adapter/

match slimp3 m|^GET %2[Ff] HTTP%2[Ff]1\.0\n$| p|SliMP3 MP3 player| i|http://www.slimdevices.com|

match soap m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Digest realm=\"gSOAP_Web_Service\",.*Server: gSOAP/([\d.]+)\r\n.*<SOAP-ENV:Fault><faultcode>Client</faultcode><faultstring>HTTP Error: 401 Unauthorized</faultstring></SOAP-ENV:Fault>|s p/Sagem F@st 3464 WAP soap/ d/WAP/
match soap m|^HTTP/1\.1 401 Unauthorized\r\nWWW-Authenticate: Digest realm=\"realtek\.com\.tw\", qop=\"auth\", nonce=\"[0-9a-f]+\", opaque=\"[0-9a-f]+\"\r\nServer: gSOAP/([\w._-]+)\r\n| p/gSOAP soap/ v/$1/
match soap m|^HTTP/1\.1 \d\d\d .*\r\nServer: gSOAP/([\d.]+)\r\n|s p/gSOAP soap/ v/$1/
match soap m|^HTTP/1\.1 200 OK\r\nServer: SCS\r\nContent-Type: text/html; charset=utf-8\r\n.*<h2 style=\"color:darkcyan\">ServerView Remote Connector - Provider V([\w._-]+)</h2>|s p/Fujitsu ServerView Remote Connector soap/ v/$1/
match soap m|^HTTP/1\.0 500 Internal Server Error\r\nServer: gSOAP/([\w._-]+)\r\n.* xmlns:gmmiws=\"https://([\w._-]+):\d+/glsinternal\.wsdl\" .*<faultstring>HTTP GET method not implemented</faultstring>|s p/gSOAP soap/ v/$1/ h/$2/ i/Good Messaging Server gddomsyncsrv/
match soap m|^HTTP/1\.0 500 Internal Server Error\r\nServer: gSOAP/([\w._-]+)\r\n.* xmlns:pushws=\"https://([\w._-]+):\d+/pushws\">.*<faultstring>HTTP GET method not implemented</faultstring>|s p/gSOAP soap/ v/$1/ h/$2/ i/Good Messaging Server gdpushproc/

# spamd 2.20-1woody
match spamassassin m|^SPAMD/1\.0 76 Bad header line: GET / HTTP/1\.0\r\r?\n| p/SpamAssassin spamd/

# TLS 1.0 Alert (0x21), Fatal (0x02), Unexpected message (0x0a)
match ssl m|^\x15\x03\x01\0\x02\x02\x0a$| p/TLS/ v/1.0/

match http m|^HTTP/1\.1 405 Method Not Allowed\r\nDate:0000-01-01T18:54:43\r\nContent-Type: application/soap\+xml; charset=\"utf-8\"\r\n\r\n$| p/Samsung CLX-3175FW printer SOAP over HTTP/ d/printer/

match speech m|^ER\nLP\n#<SUBR\(6\) />\nft_StUfF_keyOK\nER\n$| p/Festival Speech Synthesis System/

match sphinx-search m|^\x01\0\0\0\0\x01\0\0\0\0\0 \0\0\0\x1cunknown command \(code=\d+\)| p/Sphinx Search daemon/

# No idea if this is general enough
match sopcast m|^HTTP/1\.0 200 OK\r\n\r\n0&\xb2u\x8ef\xcf\x11\xa6\xd9\0| p/SopCast P2P/

match tcpmux m|^-Service not available\r\n$|

match telnet m|^\xff\xfb\x01\xff\xfe\"\n\r\tNetDSL Copyright by ARESCOM 2003\n\r\n\r\n\rUsername:GET / HTTP/1\.0\r\n\n\rPassword:\r\n\n\rUsername:| p/ARESCOM NetDSL 1000 router/ d/router/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\xff\xfbi\r\n\tWelcome to Magicunix's TCP Server\.\r\n\r\n\r\nLogin: P/1\.0\r\nPassword: \r\nLogin incorrect\r\nLogin: | p/MagicUnix telnetd/
match telnet m|^\xff\xfb\x03\xff\xfb\x01\r\n\r\n\x07HP ([\w+]+) AdvanceStack 10BT Switching Hub Management Module\r\n| p/HP $1 switch telnetd/ d/switch/
match telnet m|^\xff\xfb\x01\r\n-> GET / HTTP/1\.0\r\nGET / HTTP/1\.0\r\nundefined symbol: GET\r\n-> \r\n-> | p/Konica Minolta Magicolor 2300 DL printer telnetd/ d/printer/
match telnet m|^\xff\xfe\x01Login to server\. \r\nUsername: ET / HTTP/1\.0\r\nPassword: \r\nLogin to server\. \r\nUsername:| p/EFCMService telnetd/ o/Windows/
match telnet m|^\xff\xfc\"\xff\xfb\x03\xff\xfb\x01\r\n\r\nWelcome to  C A N O P Y  CMM Micro\.\r\n\r\nPress Enter to Continue\.\.\.\r\n\r\nLogin: \r\nPassword: | p/Motorola Canopy cluster management module telnetd/ o/eCos/
match telnet m|^\xff\xfb\x01\xff\xfb\x03telnet@CER(\w+)>GET / HTTP/1\.0\r\nInvalid input -> GET / HTTP/1\.0\r\nType \? for a list\r\n| p/NetIron CER $1 switch telnetd/ d/switch/
match telnet m|^BAD_COMMAND\n| p/Lotus Domino Console/

# The Onion Router
match tor-socks m|^HTTP/1\.0 501 Tor is not an HTTP Proxy\r\n| p/Tor SOCKS Proxy/
match tor-info m|^HTTP/1\.0 \d\d\d .*\r\nContent-Encoding: identity\r\n.*signed-directory\npublished .*\nrecommended-software|s p/Tor nodes info httpd/
match tor-info m|^HTTP/1\.0 503 Directory busy, try again later\r\n\r\n$| p/Tor nodes info httpd/

match utsessiond m|^ERR/InvalidCommand\n$| p/Sun Ray utsessiond/
match utsvc m|^protocolErrorInf error=Missing\\040hw\\040string\\040from\\040:\\040null\.\\040Check\\040hardware state=disconnected\n| p/Sun Ray utsvcd/

match upnp m|^HTTP/1\.[01] 200 OK\r\n.*Server: Linux-([\w_.-]+), UPnP/([\d.]+), PMS/([\d.]+)\r\n|s p/PS3 Media Server UPnP/ v/$3/ i/Linux $1; UPnP $2/ d/media device/ o/Linux/
match upnp m|^HTTP/1\.[01] 200 OK\r\n.*Server: Windows_XP-([\w_.-]+), UPnP/([\d.]+), PMS/([\d.]+)\r\n|s p/PS3 Media Server UPnP/ v/$3/ i/Windows XP $1; UPnP $2/ d/media device/ o/Windows/
match upnp m|^HTTP/1\.[01] 200 OK\r\n.*Server: Mac_OS_X-x86_64-([\w_.-]+), UPnP/([\d.]+), PMS/([\d.]+)\r\n|s p/PS3 Media Server UPnP/ v/$3/ i/Mac OS X $1; UPnP $2/ d/media device/ o/Mac OS X/

match upnp m|^HTTP/1\.0 200 .*\r\n.*Server: Linux/([\w_.-]+), UPnP/([\w_.-]+), Free UPnP Entertainment Service/ReadyNAS\r\n|s p/FUPPES UPnP media server/ i/Linux $1; UPnP $2/ o/Linux/
match upnp m|^HTTP/1\.0 200 OK\r\n.*Server: Linux/([\w_.-]+), UPnP/([\w_.-]+), Free UPnP Entertainment Service/([^\r\n]+)\r\n| p/FUPPES UPnP media server/ v/$3/ i/Linux $1; UPnP $2/ o/Linux/
match upnp m|^HTTP/1\.0 200 OK\r\n.*Server: FreeBSD/([\w_.-]+), UPnP/([\w_.-]+), Free UPnP Entertainment Service/([^\r\n]+)\r\n| p/FUPPES UPnP media server/ v/$3/ i/FreeBSD $1; UPnP $2/ o/FreeBSD/

match upnp m|^HTTP/1\.1 500 Internal Server Error\r\nSERVER: ipOS/([\d.]+) UPnP/([\d.]+) ipUPnP/([\d.]+)\r\n| p/D-Link WAP dynamic DNS UPnP/ i|ipOS $1; UPnP $2; ipUPnP $3| d/WAP/
match upnp m|^HTTP/1\.1 400 Bad Request\r\nSERVER: ipOS/([\d.]+) UPnP/([\d.]+) ipGENADevice/([\d.]+)\r\n| p/D-Link DGL-4300 gaming router UPnP/ i|ipOS $1; UPnP $2; ipGENADevice $3| d/broadband router/
match upnp m|^HTTP/1\.0 404 Not Found\r\nSERVER: ipos/([\d.]+) UPnP/([\d.]+) (TL-\w+)/([\w._-]+)\r\n| p/TP-LINK $3 WAP UPnP/ v/$4/ i|ipos $1; UPnP $2| d/WAP/

match upnp m|^HTTP/1\.0 \d\d\d .*\r\nSERVER: Linux/([\w._-]+), UPnP/([\d.]+), Portable SDK for UPnP devices/([\w._~-]+)\r\n| p/Portable SDK for UPnP devices/ v/$3/ i/Linux $1; UPnP $2/ o/Linux/
match upnp m|^HTTP/1\.0 \d\d\d .*\r\nSERVER: Linux/([\w._-]+) UPnP/([\d.]+) DLNADOC/([\d.]+) Portable SDK for UPnP devices/([\w._~-]+)\r\n| p/Portable SDK for UPnP devices/ v/$4/ i/Linux $1; DLNADOC $3; UPnP $2/ o/Linux/

match upnp m|^HTTP/1\.[01] \d\d\d .*\r\nSERVER: Linux/([-\w_.]+), UPnP/([\d.]+), Intel SDK for UPnP devices ?/([\w._~-]+)\r\n| p/Intel UPnP reference SDK/ v/$3/ i/Linux $1; UPnP $2/ o/Linux/
match upnp m|^HTTP/1\.[01] \d\d\d .*\r\nSERVER: Linux, UPnP/([\d.]+), Intel SDK for UPnP devices ?/([\w._~-]+)\r\n| p/Intel UPnP reference SDK/ v/$2/ i/UPnP $1/ o/Linux/
match upnp m|^HTTP/1\.[01] \d\d\d .*\r\nSERVER: Darwin/([\w._-]+), UPnP/([\w._-]+), Portable SDK for UPnP devices/([\w._-]+)\r\n| p/Intel UPnP reference SDK/ v/$3/ i/Mac OS X $1; UPnP $2/ o/Mac OS X/

match upnp m|^HTTP/1\.[01] \d\d\d .*\r\nCONTENT-TYPE: text/xml\r\nContent-Length: .*<modelName>Xbox 360</modelName>.*<serialNumber>(\w+)</serialNumber>|s p/XBox 360 XML UPnP/ i/Serial number $1/ d/game console/
match upnp m|^HTTP/1.1 400 Bad Request\r\n\r\n$| p/Microsoft Windows UPnP/ o/Windows/
match upnp m|^HTTP/1\.0 \d\d\d .*\r\nDate: .*\r\nConnection: close\r\nServer: Microsoft-Windows-NT/(\d[-.\w]+) UPnP/(\d[-.\w]+) UPnP-Device-Host/(\d[-.\w]+)\r\n| p/Microsoft Windows UPnP/ v/$2/ i/UPnP Device Host: $3/ o/Windows NT $1/
match upnp m|^HTTP/1\.1 200 .*\r\nSERVER: Linux/([\w._-]+), UPnP/([\d.]+), MediaTomb/([\w._-]+)\r\n|s p/MediaTomb UPnP/ v/$3/ i/Linux $1; UPnP $2/ o/Linux/
match upnp m|^HTTP/1\.1 200 .*\r\nSERVER: Darwin/([\w._-]+), UPnP/([\d.]+), MediaTomb/([\w._-]+)\r\n|s p/MediaTomb UPnP/ v/$3/ i/Darwin $1; UPnP $2/ o/Mac OS X/
match upnp m|^HTTP/1\.1 200 OK\r\n.*SERVER: FreeBSD/([\w._-]+), UPnP/([\d.]+), MediaTomb/([\w._-]+)\r\n|s p/MediaTomb UPnP/ v/$3/ i/FreeBSD $1; UPnP $2/ o/FreeBSD/
match upnp m|^HTTP/1\.1 \d\d\d .*\r\nServer: *Linux/([-\w_.]+), UPnP/([-\w_.]+), TwonkyVision UPnP SDK/([-\w_.]+)\r\n|s p/TwonkyMedia UPnP/ i/Linux $1; UPnP $2; SDK $3/ o/Linux/
match upnp m%^HTTP/1\.1 \d\d\d .*\r\n.*Server: *Linux/([\w._-]+), UPnP/([\w._-]+), pvConnect UPnP SDK/([\w._-]+)\r\n.*<title>(?:TwonkyMedia|TwonkyMedia server media browser|TwonkyVision Configuration)</title>%s p/TwonkyMedia UPnP/ i/Linux $1; UPnP $2; pvConnect SDK $3/ o/Linux/
match upnp m|^HTTP/1\.1 \d\d\d .*\r\n.*Server: *Linux/([\w._-]+), UPnP/([\w._-]+), pvConnect UPnP SDK/([\w._-]+)\r\n.*<title>MediaServer Restriced Access</title>|s p/TwonkyMedia UPnP/ i/Iomega Home Media NAS device; Linux $1; UPnP $2; pvConnect SDK $3/ o/Linux/
match upnp m|^HTTP/1\.1 \d\d\d .*\r\nWWW-Authenticate: Basic realm=\"([\w._-]+)\"\nEXT:\r\nServer: *Linux/([\w._-]+), UPnP/([\w._-]+), pvConnect UPnP SDK/([\w._-]+)\r\n|s p/TwonkyMedia UPnP/ h/$1/ i/Linux $2; UPnP $3; pvConnect SDK $4/ o/Linux/
match upnp m|^HTTP/1\.1 \d\d\d .*\r\nContent-Type:  text/xml; charset=\"UTF-8\"\r\nServer: Orb Media Server, WINDOWS, UPnP/([\w._-]+), Intel MicroStack/([\w._-]+)\r\n| p/Orb Media Server UPnP/ o/Windows/ i/UPnP $1; Intel MicroStack $2/
match upnp m|^HTTP/1\.0 \d\d\d .*\r\nServer: OpenWRT/kamikaze UPnP/([\w._-]+) miniupnpd/([\w._-]+)\r\n|s p/MiniUPnP/ v/$2/ i/OpenWrt Kamikaze; UPnP $1/ o/Linux/ d/broadband router/
match upnp m|^HTTP/1\.0 200 OK\r\n.*Server: Linux,([\w._-]+),UPnP/([\w._-]+),Coherence UPnP framework,([\w._-]+)\r\n|s p/Coherence UPnP framework/ v/$3/ o/Linux/ i/Linux $2; UPnP $2/
match upnp m|^HTTP/1\.[01] 404 Not Found\r\n.*Server: Netgem/([\d.]+) \(NeufboxTV UPnPServer\)\r\n|s p/Netgem UPnP/ v/$1/ i/Neuf Box TV/ d/media device/
match upnp m|^HTTP/1\.1 200 OK\r\n.*Server: WINDOWS, UPnP/([\d.]+), Intel MicroStack/([\d.]+)\r\n.*<dlna:X_DLNADOC xmlns:dlna=\"urn:schemas-dlna-org:device-1-0\">(DMS-[\d.]+)</dlna:X_DLNADOC>.*<friendlyName>([\w._-]+): MediaServer</friendlyName>.*<manufacturer>Wistron</manufacturer>.*<modelDescription>WiDMS</modelDescription>|s p/Intel MicroStack UPnP/ v/$2/ o/Windows/ i/Wistron Digital Media Server $3; UPnP $1/ h/$4/
match upnp m|^HTTP/1\.1 400 Bad Request\r\nServer: Linux, UPnP/([\d.]+), (DIR-[\w+]+) Ver ([\d.]+)\r\n| p/D-Link $2 WAP UPnP/ v/$3/ o/Linux/ i/UPnP $1/
match upnp m|^HTTP/1\.0 404 Not Found\r\nSERVER: FAST Router (\w+) Router, UPnP/([\w.]+)\r\n| p/FAST $1 router UPnP $2/ d/router/
match upnp m|^HTTP/1\.0 200 OK\r\nCONTENT-TYPE: text/xml\r\nCONTENT-LENGTH: 0\r\n.*SERVER: Linux/([\w._-]+)_mvl21-malta-mips_fp_le UPnP/([\w._-]+) myigd/([\w._-]+)\r\n|s p/myigd/ v/$3/ o/Linux/ d/WAP/ i/Linksys WAG354G router; MontaVista Linux $1; UPnP $2/
match upnp m|^HTTP/1\.1 404 Bad Request\r\nCONTENT-LENGTH: 0\r\nCONTENT-TYPE: text/html\r\n\r\n$| p/SuperMicro IPMI UPnP/
match upnp m|^HTTP/1\.1 404 Not Found\r\nDate: .*\r\nServer: Unknown/0\.0 UPnP/([\d.]+) Virata-EmWeb/([-.\w]+)\r\n| i/ReplayTV UPnP; UPnP $1/ p/Virata-EmWeb/ v/$SUBST(2,"_",".")/
match upnp m|^HTTP/1\.1 200 OK\r\nContent-Type: text/html\r\n.*Server: RomPager/([\w.]+) UPnP/([\w.]+)\r\n\r\n\n<html><head>.*<title>ZyXEL Prestige Router</title>|s i/ZyXEL Prestige router UPnP; UPnP $2/ p/Allegro RomPager/ v/$1/ d/router/
match upnp m|^HTTP/1\.1 \d\d\d .*\r\nServer: NT/([\d.]+) UPnP/([\d.]+)\r\nDate: .*\r\nContent-type: text/html\r\n\r\n<html>\r\n<head>\r\n<title>HotBrick Load Balancer ([-\w_.]+)</title>\r\n| p/HotBrick Load Balancer $3 UPnP/ i/NT httpd $1; UPnP $2/ d/load balancer/
match upnp m|^HTTP/1\.1 \d\d\d .*\r\nServer: NT/([\d.]+) UPnP/([\d.]+)\r\nDate: .*\r\nContent-type: text/html\r\n\r\n<html>\r\n<head>\r\n<title>HotBrick Firewall VPN ([-\w_./]+)</title>| p/HotBrick Firewall VPN $3 UPnP/ i/NT httpd $1; UPnP $2/ d/firewall/
match upnp m|^HTTP/1\.1 200 OK\r\nServer: Unknown/[\d.]+ UPnP/([\d.]+) Virata-EmWeb/R([\d_]+)\r\nContent-Length: .*\r\n\r\n<HTML><HEAD><TITLE>Actiontec</TITLE>\n|s p/Virata-EmWeb/ v/$SUBST(2,"_",".")/ i/ActionTec DSL UPnP; UPnP $1/ d/broadband router/
match upnp m|^HTTP/1\.1 \d\d\d .*\r\nServer: Unknown/[\d.]+ UPnP/([\d.]+) GlobespanVirata-EmWeb/R([\d_]+)\r\nContent-Type: text/html\r\nExpires: .*\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n\r\n<html>\n<head>\n<title>ADSL VPN Firewall Router</title>| i/Billion 741GE ADSL router UPnP; UPnP $1/ p/Virata-EmWeb/ v/$SUBST(2,"_",".")/ d/router/
match upnp m|^HTTP/1\.1 \d\d\d .*\r\nServer: Unknown/[\d.]+ UPnP/([\d.]+) Virata-EmWeb/R([\d_]+)\r\nContent-Type: text/html\r\nExpires: .*\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n\r\n\n<html>\n<head>\n<title>ADSL Configuration Page\n</title>| p/Virata-EmWeb/ v/$SUBST(2,"_",".")/ i/Telewell 715 DSL router UPnP; UPnP $1/ d/router/
match upnp m|^HTTP/1\.1 \d\d\d .*\r\nDATE: .*\r\nConnection: Keep-Alive\r\nServer: LINUX/([\d.]+) UPnP/([\d.]+) BRCM400/([\d.]+)\r\n| p|Belkin/Linksys wireless router UPnP| i/Linux $1; UPnP $2; BRCM400 $3/ d/router/
match upnp m|^HTTP/1\.1 \d\d\d .*\r\nServer: Unknown/[\d.]+ UPnP/([\d.]+) GlobespanVirata-EmWeb/R([\d_]+)\r\nContent-Type: text/html\r\n.*<title>CopperJet ([-\w+/.]+) Router VoATM</title>|s i/CopperJet $3 VoATM router UPnP; UPnP $1/ p/Virata-EmWeb/ v/$SUBST(2,"_",".")/ d/router/
match upnp m|^HTTP/1\.1 200 OK\r\nServer: Unknown/[\d.]+ UPnP/([\d.]+) GlobespanVirata-EmWeb/R([\d_]+)\r\nContent-Type: text/html\r\n.*<head>\n<title>Wireless ADSL VPN Firewall Router</title>\n|s i/Billion BIPAC-743GE V1 ADSL WAP UPnP; UPnP $1/ p/GlobespanVirata-EmWeb/ v/$SUBST(2,"_",".")/ d/WAP/
match upnp m|^HTTP/1\.1 301 Moved Permanently\r\nServer: Nucleus/([\d.]+) UPnP/([\d.]+) Virata-EmWeb/R([\d_]+)\r\nLocation: http://[\d.]+/hag/pages/home\.htm\r\n| i|Huawei/Intracom ADSL router UPnP; Virata-EmWeb $SUBST(3,"_","."); UPnP $2| p/Nucleus/ v/$1/ d/broadband router/
match upnp m|^HTTP/1\.1 \d\d\d .*\r\nServer: Unknown/0\.0 UPnP/([\d.]+) GlobespanVirata-EmWeb/R([\d_]+)\r\nContent-Type: text/html\r\nExpires: .*\r\nCache-Control: no-cache\r\nPragma: no-cache\r\n\r\n<html>\n<head>\n<title>ADSL -modem/firewall/switch/WLAN -AP</title>\n| i/Telewell TW-EA2000 ADSL modem UPnP; UPnP $1/ p/GlobespanVirata-EmWeb/ v/$SUBST(2,"_",".")/ d/WAP/
match upnp m|^HTTP/1\.1 \d\d\d .*Server: Unknown/0\.0 UPnP/([\d.]+) Conexant-EmWeb/R([\d_]+)\r\n.*<TITLE>Siemens ([\w._ -]+) Router</TITLE>|s p/Conexant-EmWeb/ v/$SUBST(2,"_",".")/ d/router/ i/Siemens $3 router UPnP; UPnP $1/
match upnp m|^HTTP/1\.1 200 OK\r\n.*Server: Unknown/0\.0 UPnP/([\d.]+) Conexant-EmWeb/R([\d_]+)\r\n.*<TITLE>Zoom - USB Endpoint</TITLE>.*<TITLE>Zoom DSL Modem Web-Console</TITLE>|s p/Conexant-EmWeb/ v/$SUBST(2,"_",".")/ i/Zoom A6 ADSL modem UPnP; UPnP $1/ d/broadband router/
match upnp m|^HTTP/1\.1 401 Unauthorized\r\nServer: Unknown/0\.0 UPnP/([\d.]+) GlobespanVirata-EmWeb/R([\d_]+)\r\nContent-Type: text/html\r\nExpires: .*\r\nCache-Control: no-cache\r\nPragma: no-cache\r\nWWW-Authenticate: Basic realm=\"WebAdmin\"\r\n\r\n\n\n<html>\n<head>\n\n<link rel=\"stylesheet\" type=\"text/css\" href=\"/styles/default\.css\">\n\n<title>Authentication failed</title>\n\n</head>\n<body bgcolor=\"#ffffff\" link=\"#3300cc\" alink=\"#ff0000\" vlink=\"#990066\">\n\n| i/Xavi 7768r WAP UPnP; UPnP $1/ p/GlobespanVirata-EmWeb/ v/$(SUBST(2,"_",".")/ d/WAP/
match upnp m|^HTTP/1\.1 \d\d\d .*\r\nServer: Unknown/0\.0 UPnP/([\d.]+) Web Server\r\n.*<title>MT882 ADSL Router</title>|s p/Huawei SmartAX MT882 ADSL router UPnP/ i/UPnP $1/ d/broadband router/
match upnp m|^HTTP/1\.1 \d\d\d .*\r\nServer: Nucleus/([-\w_.]+) UPnP/([\d.]+) Virata-EmWeb/R([\d_]+)\r\nWWW-Authenticate: Basic realm=\"MT882\"\r\n| i/Huawei SmartAX MT882 ADSL router UPnP; Virata httpd $SUBST(3,"_","."); UPnP $2/ d/broadband router/ p/Nucleus/ v/$1/
match upnp m|^HTTP/1\.1 \d\d\d .*\r\nServer: Nucleus/([\d.]+) UPnP/([\d.]+) Virata-EmWeb/R([\d_]+)\r\nWWW-Authenticate: Basic realm=\"Viking\"\r\n\r\n401 Unauthorized\r\n| i/Viking router UPnP; Virata-EmWeb httpd $SUBST(3,"_","."); UPnP $2/ p/Nucleus/ v/$1/ d/router/
match upnp m|^HTTP/1\.1 200 OK\r\nServer: Unknown/0\.0 UPnP/([\d.]+) Conexant-EmWeb/R([\d_]+)\r\nContent-Type: text/html\r\nExpires: .*<title>VoIP/802\.11g ADSL2\+ Firewall Router</title>\n|s i|Billion ADSL/WAP/VoIP router UPnP; UPnP $1| p/Conexant-EmWeb/ v/$SUBST(2,"_",".")/ d/router/
match upnp m|^HTTP/1\.1 200 OK\r\n.*Server: Unknown/0\.0 UPnP/([\d.]+) Conexant-EmWeb/R([\d_]+)\r\n.*<TITLE>Zoom - USB Endpoint</TITLE>.*<TITLE>Zoom DSL Modem Web-Console</TITLE>|s p/Conexant-EmWeb/ v/$SUBST(2,"_",".")/ i/Zoom A6 ADSL modem UPnP; UPnP $1/ d/broadband router/
match upnp m|^HTTP/1\.1 200 OK\r\nServer: Unknown/0\.0 UPnP/([\d.]+) Conexant-EmWeb/R([\d_]+)\r\nContent-Type: text/html\r\nExpires: .*<head>\n<title>Huawei xDSL\r\n</title>|s i|Huawei ADSL/WAP/VoIP router UPnP; UPnP $1| p|Conexant-EmWeb| v|$SUBST(2,"_",".")| d/router/
match upnp m|^HTTP/1\.1 200 OK\r\n.*Server: Unknown/0\.0 UPnP/([\d.]+) Conexant-EmWeb/R([\d_]+)\r\n.*<title>VoIP/802\.11g ADSL2\+ Firewall Router</title>|s p/Conexant-EmWeb/ v/$SUBST(2,"_",".")/ i/Billion 800VGT ADSL router UPnP; UPnP $1/ d/broadband router/
match upnp m|^HTTP/1\.1 \d\d\d .*\r\nServer: Unknown/0\.0 UPnP/([\d.]+) Virata-EmWeb/R([\d_]+)\r\n.*<title>Wireless ADSL Router Control Panel</title>|s i/Eminent EM4104 WAP UPnP; UPnP $1/ p/Virata-EmWeb/ v/$SUBST(2,"_",".")/ d/WAP/
match upnp m|^HTTP/1\.1 200 OK\r\nServer: ISOS/([-\w_.]+) UPnP/([\d.]+) Conexant-EmWeb/R([\d_]+)\r\n.*<title>Scarlet One</title>|s p/ISOS/ v/$1/ i/Scarlet One UPnP; Conexant-EmWeb $SUBST(3,"_","."); UPnP $2/ d/VoIP adapter/
match upnp m|^HTTP/1\.1 404 Not Found\r\nCONTENT-LENGTH: 48\r\nDATE: Sun, 09 Mar 2008 14:51:08 GMT\r\nSERVER: Linux/6\.0 UPnP/1\.0 Intel UPnP/0\.9\r\n\r\n<html><body><h1>404 Not Found</h1></body></html>$| p/Linksys WVC54GC webcam UPnP/ d/webcam/
match upnp m|^HTTP/1\.1 200 OK\r\nServer: Unknown/0\.0 UPnP/([\w._-]+) GlobespanVirata-EmWeb/R([\w._-]+)\r\n.*<title>JetSpeed 500 i</title>|s i/Intracom JetSpeed 500i UPnP; UPnP $1/ d/broadband router/ p/GlobespanVirata-EmWeb/ v/$SUBST(2,"_",".")/
match upnp m|^HTTP/1\.1 401 Unauthorized\r\nServer: Nucleus/([\w._-]+) UPnP/([\w._-]+) Virata-EmWeb/R([\w._-]+)\r\nWWW-Authenticate: Basic realm=\"MT880\"\r\n\r\n\r\n| p/Nucleus/ v/$1/ i/Huawei SmartAX MT880 DSL modem UPnP; Virata-EmWeb $SUBST(3,"_","."); UPnP $2/ d/broadband router/
match upnp m|^HTTP/1\.1 400 Bad Request\r\nServer: Linux, UPnP/([\d.]+), (AR\w+) Ver ([\d.]+)\r\n| p/Airlink 101 $2 WAP UPnP/ v/$3/ o/Linux/ i/UPnP $1/
match upnp m|^HTTP/1\.1 200 OK\r\n.*SERVER: EPSON_Linux UPnP/([\d.]+) Epson UPnP SDK/([\d.]+)\r\n.*<title>WorkForce ([\w+]+)</title>|s p/Epson WorkForce $3 printer UPnP/ d/printer/ i/UPnP $1; Epson UPnP SDK $2/
match upnp m|^HTTP/1\.1 401 Unauthorized\r\nServer: Unknown/0\.0 UPnP/([\d.]+) Conexant-EmWeb/R([\d_]+)\r\nContent-Type: text/html\r\nExpires: Thu, 01 Jan 1970 00:00:00 GMT\r\n.*WWW-Authenticate: Basic realm=\"WebAdmin\"\r\n|s p/Conexant-EmWeb/ v/$SUBST(2,"_",".")/ i/Billion 740- or 7400-series ADSL router UPnP; UPnP $1/ d/WAP/
match upnp m|^HTTP/1\.1 \d\d\d.*Server: Unknown/0\.0 UPnP/([\d.]+) Conexant-EmWeb/R([\d_]+)\r\n|s p/Conexant-EmWeb/ v/$SUBST(2,"_",".")/ i/UPnP $1/

# UUCP 1.06.2 on Linux 2.4.X
# Taylor UUCP 1.06.2 on Slackware
match uucp m|^login: Password:$| p/Taylor uucpd/
match uucp m|^login: Login incorrect\.$| p/Solaris uucpd/

# Veritas Netbackup client v.3.4
# Veritas Netbackup 4.5 Java listener
match netbackup m|^1000      2\n43\nunexpected message received\n$| p/Veritas Netbackup java listener/
# Veritas Backup Exec 9.0 on Windows
match ndmp m|^\x80\0\0\$\0\0\0\x01....\0\0\0\0\0\0\x05\x02\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\x03\0\0\0\0|s p/Veritas Backup Exec ndmp/ v/9.0/

# Possibly a different version? -Doug
match backupexec m|^\x80\0\0\$\0\0\0\x01....\0\0\0\0\0\0\x05\x02\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\x02\0\0\0\0|s p/Veritas Backup Exec/

match vnc-http m|^HTTP/1\.1 200 OK\r\nServer: RealVNC/(\d[-.\w]+)\r\n.*<APPLET CODE="?vncviewer/VNCViewer\.class"? ARCHIVE="?vncviewer\.jar"?\r?\n *WIDTH="?(\d+)"? HEIGHT="?(\d+)"?>\r?\n<PARAM name=\"port\" value=\"(\d+)\">\r?\n</APPLET>|si p/RealVNC/ v/$1/ i/Resolution $2x$3; VNC TCP port: $4/
# Sometimes extra HTTP crap pushes the extra info out of the header we capture:
match vnc-http m|^HTTP/1\.1 200 OK\r\nServer: RealVNC/(\d[-.\w]+)\r\n| p/RealVNC/ v/$1/
match vnc-http m|^HTTP/1\.1 200 OK\r\nServer: RealVNC-x0vncserver/([\w._ ()-]+)\r\n.*<applet code=\"vncviewer/VNCViewer\.class\" archive=\"vncviewer\.jar\"\n        width=\"(\d+)\" height=\"(\d+)\">\n<param name=\"port\" value=\"(\d+)\">|s p/RealVNC x0vncserver/ v/$1/ i/Resolution $2x$3; VNC TCP port $4/

match vnc-http m|^HTTP/1\.1 200 OK\r\nServer: VNC Server Enterprise Edition/([\w._-]+) \(r(\d+)\)\r\n.*<applet code=\"vncviewer/VNCViewer\.class\" archive=\"vncviewer\.jar\"\r\n        width=\"(\d+)\" height=\"(\d+)\">\r\n<param name=\"port\" value=\"(\d+)\">|s p/VNC Server Enterprise Edition httpd/ v/$1 r$2/ i/Resolution $3x$4; VNC port $5/
match vnc-http m|^HTTP/1\.1 200 OK\r\nServer: VNC Server Personal Edition/([\w._-]+) \(r(\d+)\)\r\n.*<applet code=\"vncviewer/VNCViewer\.class\" archive=\"vncviewer\.jar\"\r\n        width=\"(\d+)\" height=\"(\d+)\">\r\n<param name=\"port\" value=\"(\d+)\">|s p/VNC Server Personal Edition httpd/ v/$1 r$2/ i/Resolution $3x$4; VNC port $5/

# RealVNC Unknown Version
match vnc-http m|^HTTP/1\.0 200 OK\n\n<HTML><TITLE>VNC desktop</TITLE>\n<APPLET CODE=vncviewer\.class ARCHIVE=vncviewer\.jar WIDTH=(\d+) HEIGHT=(\d+)>\n<param name=PORT value=(\d+)></APPLET></HTML>\n| p/RealVNC/ i/Resolution $1x$2; VNC TCP port: $3/

# TightVNC Server version 1.2.2 HTTP on Windows 2000 SP2
match vnc-http m|^HTTP/1\.0 200 OK\n\n<HTML><TITLE>TightVNC desktop \[([-.\w]+)\]</TITLE>\n<APPLET CODE=vncviewer\.class ARCHIVE=vncviewer\.jar WIDTH=(\d+) HEIGHT=(\d+)>\n<param name=PORT value=(\d+)>| p/TightVNC/ v/1.2.2/ i/Resolution $2x$3; VNC TCP port: $4/ h/$1/
# Tightvnc-1.2.3
match vnc-http m|^HTTP/1\.0 404 Not found\n\n<HEAD><TITLE>File Not Found</TITLE></HEAD>\n<BODY><H1>File Not Found</H1></BODY>\n$| p/TightVNC/
# Tightvnc 1.2.3
match vnc-http m|^HTTP/1\.0 200 OK\n\n<HTML><TITLE>TightVNC desktop \[([-.\w]+)\]</TITLE>\n<APPLET CODE=VncViewer\.class ARCHIVE=VncViewer\.jar WIDTH=(\d+) HEIGHT=(\d+)>\n<param name=PORT value=(\d+)>| p/TightVNC/ v/1.2.3/ i/User: $1; Resolution $2x$3; VNC TCP port: $4/
# TightVNC 1.2.6
match vnc-http m|^HTTP/1\.0 200 OK\n\n<HTML>\n  <HEAD><TITLE>TightVNC desktop \[[-.\w]+\]| p/TightVNC/
# TightVNC 1.2.8
match vnc-http m|^HTTP/1\.0 200 OK[\r\n]*.*<!-- \n     index\.vnc - default HTML page for TightVNC Java viewer applet, to be\n     used with Xvnc\. On any file ending in \.vnc, the HTTP server embedded in\n     Xvnc will substitute the following variables when preceded by a dollar:\n     USER, DESKTOP, DISPLAY, APPLETWIDTH, APPLETHEIGHT, WIDTH, HEIGHT, PORT,\n.*<TITLE>\n(\w+)'s X desktop.*<APPLET CODE=VncViewer\.class ARCHIVE=VncViewer\.jar\n        WIDTH=(\d+) HEIGHT=(\d+)>\n<param name=PORT value=(\d+)>\n\n</APPLET>|s p/TightVNC/ v/1.2.8/ i/User: $1; Resolution $2x$3; VNC TCP port: $4/
# TightVNC 1.2.8 - I guess it gets cut off sometimes?
match vnc-http m|^HTTP/1\.0 200 OK[\r\n]*.*<!-- \n     index\.vnc - default HTML page for TightVNC Java viewer applet, to be\n     used with Xvnc\. On any file ending in \.vnc, the HTTP server embedded in\n     Xvnc will substitute the following variables when preceded by a dollar:\n     USER, DESKTOP, DISPLAY, APPLETWIDTH, APPLETHEIGHT, WIDTH, HEIGHT, PORT,\n| p/TightVNC/ v/1.2.8/
# TightVNC 1.2.9
match vnc-http m|^HTTP/1\.0 200 OK\n.*<HTML><HEAD><TITLE>Remote Desktop</TITLE></HEAD>\n<BODY>\n<APPLET CODE=VncViewer\.class ARCHIVE=VncViewer\.jar WIDTH=(\d+) HEIGHT=(\d+)>\n\t<param name=PORT value=(\d+)>\n</APPLET>\n</BODY></HTML>\n|s p/TightVNC/ v/1.2.9/ i/Resolution $1x$2; VNC TCP port $3/
# NetWare VNCServer
match vnc-http m|^HTTP/1\.0 200 OK\n.*<!-- \r\n     index\.vnc - default HTML page for TightVNC Java viewer applet, to be.*<TITLE>\r\n([\d\w]+) - NetWare VNCServer desktop.*<APPLET CODE=VncViewer\.class ARCHIVE=VncViewer\.jar\r\n *WIDTH=(\d+) HEIGHT=(\d+)>\r\n<param name=PORT value=(\d+)>|s p/NetWare VNC Desktop/ i/User: $1; Resolution $2x$3; VNC TCP port: $4/
# WinVNC 3.3.7 Build Mar 5 2003
match vnc-http m|^HTTP/1\.0 200 OK\r\n\r\n<HTML><TITLE>VNC desktop \[([-.\w]+)\]</TITLE>\n<APPLET CODE=vncviewer\.class ARCHIVE=vncviewer\.jar WIDTH=(\d+) HEIGHT=(\d+)>\n<param name=PORT value=(\d+)| p/WinVNC/ v/3.3.7/ i/Server: $1; Resolution $2x$3; VNC TCP port: $4/
# WinVNC 3.3.3
# Tight VNC 1.5.2
match vnc-http m|^HTTP/1\.0 200 OK\n\n<HTML><TITLE>VNC desktop \[([-.\w]+)\]</TITLE>\n<APPLET CODE=vncviewer\.class ARCHIVE=vncviewer\.jar WIDTH=(\d+) HEIGHT=(\d+)>\n<param name=PORT value=(\d+)></APPLET></HTML>\n$| p/WinVNC/ i/Server: $1; Resolution $2x$3; VNC TCP port: $4; May be standard or TightVNC/
# Ultr@VNC Win32 v1.0.9 - HTTP
match vnc-http m|^HTTP/1\.0 200 OK\n\n<HTML>\n  <HEAD><TITLE>Ultr@VNC Desktop \[[-. \w]+\] ------- Ultr@VNC Home Page is  http://ultravnc\.sf\.net -------</TITLE></HEAD>\n  <BODY>\n  <SPAN style='position: absolute; top:0px;left:0px'>\n    <APPLET CODE=VncViewer\.class ARCHIVE=VncViewer\.jar WIDTH=(\d+) HEIGHT=(\d+)>\n      <PARAM NAME=PORT VALUE=(\d+)>\n      <PARAM NAME=ENCODING VALUE=Tight>\n    </APPLET>  </SPAN>\n  </BODY>\n| p/Ultr@VNC/ i/Resolution $1x$2; VNC TCP port: $3/
match vnc-http m|^HTTP/1\.0 200 OK\n\n<HTML>\n  <HEAD><TITLE> \[([-. \w]+)\] </TITLE></HEAD>\n  <BODY>\n  <SPAN style='position: absolute; top:0px;left:0px'>\n    <APPLET CODE=VncViewer\.class ARCHIVE=VncViewer\.jar WIDTH=(\d+) HEIGHT=(\d+)>\n      <PARAM NAME=PORT VALUE=(\d+)>\n      <PARAM NAME=ENCODING VALUE=Tight>\n    </APPLET>  </SPAN>\n  </BODY>\n</HTML>\n| p/Ultr@VNC/ i/Name $1; Resolution $2x$3; VNC TCP port: $4/
match vnc-http m|^HTTP/1\.0 200 OK\n\n<HTML>\n  <HEAD><TITLE> \[([-. \w]+)\] </TITLE></HEAD>\n  <BODY>\n  <SPAN style='position: absolute; top:0px;left:0px'>\n<OBJECT \n    ID='VncViewer'\n.*WIDTH = (\d+) HEIGHT = (\d+) >.*<PARAM NAME = PORT VALUE=(\d+)>|s p/Ultr@VNC/ i/Name $1; Resolution $2x$3; VNC TCP port: $4/
# VNC to java display applet over http. Final AT&T release
match vnc-http m|^HTTP/1\.0 200 .*<!-- index\.vnc - default html page for Java VNC viewer applet.*<TITLE>\n([\w._-]+)'s .*<APPLET CODE=vncviewer\.class ARCHIVE=vncviewer\.jar.*WIDTH=(\d+).*HEIGHT=(\d+).*name=PORT value=(\d+)|s p/AT&T VNC/ i/User $1; Resolution $2x$3; VNC TCP port $4/
match vnc-http m|^HTTP/1\.0 200 OK\r\n.*<!-- index\.vnc - default html page for Java VNC viewer applet\..*<TITLE>\n\?'s Android desktop \(([\w._-]+):1\)\n</TITLE>\n<APPLET CODE=VncViewer\.class ARCHIVE=VncViewer\.jar\n        WIDTH=(\d+) HEIGHT=(\d+)>\n<param name=PORT value=(\d+)>.*Further help: <BR>\n<A href=\"http://onaips\.blogspot\.com/\">oNaiPs Blog</A><BR>\n<A href=\"http://www\.tightvnc\.com/\">www\.TightVNC\.com</A>\n</HTML>\n$|s p/Android VNC Server/ h/$1/ i/Resolution $2x$3; VNC TCP port $4/
# KDE Built-in VNC Server
match vnc-http m|^HTTP/1\.0 200 OK\n.*<HTML><HEAD><TITLE>(.*)'s desktop</TITLE></HEAD>\n<BODY>\n<APPLET CODE=(?:vncviewer/)?[vV][nN][cC][vV]iewer\.class ARCHIVE=[vV]nc[vV]iewer\.jar WIDTH=(\d+) HEIGHT=(\d+)>\n\t<param name=PORT value=(\d+)>\n</APPLET>\n</BODY></HTML>\n|s p/KDE Built-in VNC/ i/User $1; Resolution $2x$3; VNC TCP port: $4/
match vnc-http m|^HTTP/1\.0 200 OK\n\n.*<TITLE>eSVNC Desktop \[([\w._-]+)\]</TITLE>.*<APPLET CODE=VncViewer\.class ARCHIVE=VncViewer\.jar WIDTH=(\d+) HEIGHT=(\d+)>.*<PARAM NAME=PORT VALUE=(\d+)>|s p/eSVNC/ h/$1/ i/Resolution $2x$3; VNC TCP port $4/
match vnc-http m|^HTTP/1\.0 200 OK\r\n.*<TITLE>\n([\w._-]+)'s [\w._:-]+ desktop \([\w._:-]+\)\n</TITLE>\n<APPLET CODE=VncViewer\.class ARCHIVE=VncViewer\.jar\n        WIDTH=(\d+) HEIGHT=(\d+)>\n<param name=PORT value=(\d+)>\n<param name=\"Open New Window\" value=yes>\n</APPLET>\n<BR>\n<A href=\"http://www\.tightvnc\.com/\">|s p/X11VNC/ i/User $1; Resolution $2x$3; VNC TCP port: $4/
match vnc-http m|^HTTP/1\.0 200 OK\r\n.*<TITLE>TightVNC desktop \[([\w._-]+)\]</TITLE>.*<APPLET ARCHIVE=\"VncViewer\.jar\" CODE=VncViewer WIDTH=1 HEIGHT=1>\n      <PARAM NAME=\"PORT\" VALUE=\"(\d+)\">\n      <PARAM NAME=\"Open new window\" VALUE=\"YES\">\n\n    </APPLET><BR>\n    <A HREF=\"http://www\.tightvnc\.com/\">|s p/TightVNC/ i/User $1; VNC TCP port: $2/
match vnc-http m|^HTTP/1\.0 200 OK\n\n<HTML>\n<TITLE>VNC desktop \[[\d.]+\]</TITLE>\n<APPLET CODE=vncviewer\.class ARCHIVE=vncviewer\.jar WIDTH=(\d+) HEIGHT=(\d+)>\n<param name=PORT value=(\d+)>\n</APPLET>\n</HTML>\n| p/Wyse Winterm 1200 LE terminal/ i/Resolution $1x$2; VNC TCP port $3/ d/terminal/

match xml-rpc m|^HTTP/1\.0 400 Bad Request\r\nServer: Apache XML-RPC (\d[-.\w ]+)\r\n\r\nMethod GET not implemented \(try POST\)$| p/Apache XML-RPC/ v/$1/
match xml-rpc m|^HTTP/1\.1 200 OK\r\n.*Server: XMLRPC_ABYSS/Xmlrpc-c ([\w._-]+)\r\n|s p/ABYSS httpd/ i/Xmlrpc-c $1/

# Kerio MailServer
match http m|^HTTP/1\.[01] 302 Redirected\r\nConnection: close\r\nContent-Length: 0\r\nLocation: /login\r\n\r\n$| p/Kerio MailServer Webmail/
match http m|^HTTP/1\.[01] .*\r\nServer: Kerio MailServer ([\d.]+)\r\n.*X-Powered-By: PHP/([\d.]+)\r\n|s p/Kerio MailServer Webmail/ v/$1/ i/PHP $2/
match http m|^HTTP/1\.[01] .*\r\nServer: Kerio MailServer ([\d.]+)\r\n|s p/Kerio MailServer Webmail/ v/$1/
match http m|^HTTP/1\.1 302 Found\r\nConnection: Close\r\nContent-Length: 0\r\n.*Location: https:///([\w._-]+)/login\.php\r\nServer: Kerio MailServer ([^\r\n]+)\r\n\r\n$|s p/Kerio MailServer/ v/$2/ h/$1/

match http m|^HTTP/1\.0\x20250\x20Ok\r\n.*<title>PowerMTA monitoring</title>|s p/Port25 PowerMTA web monitor/
# Dell OpenManage Version 3.5.0 on MS Windows 2000 server / PowerEdge 6400/700
match http m|^HTTP/1\.1 200 OK\r\nConnection: Close\r\nContent-Type: text/html; charset=UTF-8\r\n\r\n<html>\r\n    <head>\r\n        <script language=\"javascript\">\r\n\t\t\t\t\tif| p/Dell Openmanage Server Administrator/ i/PowerEdge/
# OpenManage version 5.2; these have to match on Javascript which kinda sucks...
match http m|^HTTP/1\.0 200 OK\r\nConnection: Close\r\nContent-Type: text/html; charset=UTF-8\r\n\r\n<html>.*QueryString\.keys\[QueryString\.keys\.length\] = argname;|s p/Dell OpenManage httpd/ o/Windows/
match http m|HTTP/1\.0 200 OK\r\nConnection: Close\r\nContent-Type: text/html; charset=UTF-8\r\n\r\n<html>.*for \(var i = 0; i < QueryString\.keys\.length; i\+\+\) {\n|s p/Dell OpenManage httpd/ o/Windows/
# ASPI server (www.aspi.cz) on Solaris 6666/tcp
match aspi m|^HTTP/1\.0 404 Not Found\r\nDate: .*\r\nServer: ByllSoftware Gurda/([\d.]+)\r\n| p/ASPI server/ v/$1/ o/Solaris/
match sunscreen-adm m|^\x01\0\0\0\0\0\0\0T\x03\0\0\0\0\0\x01\x1e\0\0\0\0\0\0;\0\0\0\0\0\0\0\0Error: incompatible with administration server \(version (\d[-.\w ]*)\)\nc\0\0\0\0\0\0\0\0\0\0\x01\0\0\0\0$| p/SunScreen Remote Administration server/ v/$1/

# PopChartServer
match http m|^HTTP/1\.0 200 OK\r\n.*Server: PopChartServer ([\d.]+)\r\n|s p/PopChart Pro/ v/$1/
match http m|^HTTP/1\.0 200 OK\r\n.*Server: CordaServer \(PopChartServer compatible\) ([\d.]+)\r\n|s p/CordaServer/ v/$1/

match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: WebSTAR/([\d.]+) ID/\d+\r\n|s p/WebSTAR/ v/$1/

match honeypot m|^HTTP/1\.0 401 Unauthorized\r\n\r\n<BODY><HTML><H1>401 - Authorization Failed</H1></HTML></BODY>\0| p/Network Flight Recorder BackOfficer Friendly http honeypot/

# Maybe too specific?
match hpilo-virtual-media m|^#\0\x04\0$| p/HP Integrated Lights-Out Virtual Media/

match remoting m|^\.NET\x01\0\x02\0\0\0\0\0\0\0\x02\0\x03\x01\0\x03\0\x01\x01..\0\0Server encountered an internal error\. To get more info turn on customErrors in the server's config file\.\x05\0\0\0\0|s p/MS .NET Remoting services/
match remoting m|^\.NET\x01\0\x02\0\0\0\0\0\0\0\x02\0\x03\x01\0\x03\0\x01\x01..\0\0System\.Runtime\.Remoting\.RemotingException: Tcp channel protocol violation: expecting preamble\.\r\n|s p/MS .NET Remoting services/

match webdav m|^HTTP/1\.0 302 Found\r\nConnection: Close\r\nDate: .*\r\nLocation: /ui/core/index\.html\r\n\r\n$| p/Tonido WebDAV/

match whois m|^Process query: 'GET  HTTP1\.0'\n\n\nNo lookup service available for your query 'GET  HTTP1\.0'\.\ngwhois remarks: If this is a valid domainname or handle, please file a bug report\.\n\n\n\n\n-- \n  To resolve one of the above handles:   OTOH offical handles should be recognised directly\.\n  Please report errors or misfits via the debian bug tracking system\.\n$| p/gwhois/

# Also callbook?
match winbox m|^\x01\0\0\0\x02\0\0| p/MikroTik WinBox management console/

match xmpp m|^</stream:stream>$| p/Wildfire XMPP Client/

match printer m|^An lpd test connection was completed successfully\r\n|s p/Lexmark lpd service/ d/printer/
match printer m|^Invalid protocol request \(71\): GGET / HTTP/1\.0\r\n\n$| p/Sun Solaris lpd/

# Know the device, but not the service. Port 515.
# match unknown m|^\x02| p/Conceptronics CPSERVU print server/ d/print server/


##############################NEXT PROBE##############################
Probe TCP HTTPOptions q|OPTIONS / HTTP/1.0\r\n\r\n|
rarity 4
ports 80-85,2301,443,631,641,3128,5232,6000,8080,8888,9999,10000,10031,37435,49400
fallback GetRequest

match apollo-server m=^0000000001(?:3C|C0)0000$= p/Apollo Server database access/

match caldav m|^HTTP/1\.1 200 OK\r\nServer: DavMail Gateway ([\w._-]+)\r\nDAV: 1, calendar-access, calendar-schedule, calendarserver-private-events, addressbook\r\n| p/DavMail CalDAV http gateway/ v/$1/ d/proxy server/

# IRIX 6.5.18f Distributed GL Daemon dgld
match dgld m|^OPTI$| p/IRIX Distributed GL Daemon/ o/IRIX/
# Webmaster Conferenceroom 1.8.9.1 IRC Server
match irc m|(^:[-.\w]+) 421 \* OPTIONS :Unknown command\r\n| p/Webmaster Conferenceroom IRC server/ h/$1/

# Seems sometimes CUPS doesn't respond to GET
match ipp m|^HTTP/1\.0 \d\d\d .*\r\nServer: CUPS/([-\w_.]+)|s p/CUPS/ v/$1/

#  cgi-httpd from shttpd-0.53 on FreeBSD
match http m|^HTTP/1\.0 501 method not implemented\r\nServer: cgi-httpd\r\n| p/shttpd cgi-httpd/

match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: WebSphere Application Server/(.+)\r\n| p/IBM WebSphere Application Server/ v/$1/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: Oracle HTTP Server Powered by Apache\r\n|s p/Oracle HTTP Server Powered by Apache/
match http m|^HTTP/1\.1 \d\d\d .*\r\nServer: webfs/(\d[-.\w]+)\r\n| p/WebFS httpd/ v/$1/

match http m|^HTTP/1\.1 \d\d\d .*Server: Microsoft-IIS/([\d.]+)\r\n|s p/Microsoft IIS httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.1 503 Service Unavailable\r\nContent-Type: text/html\r\nDate: .*\r\nConnection: close\r\nContent-Length: 28\r\n\r\n<h1>Service Unavailable</h1>| p/Microsoft IIS httpd/ o/Windows/

# A whole bunch of these.. All on win32
match http m|^HTTP/1\.0 510 Not Extended\r\nDate: .*\r\nServer: CompaqHTTPServer/([\d.]+)\r\n| p/Compaq Diagnostics httpd/ i/CompaqHTTPServer $1/
# HP Linux System Management, PSP 7.30 on Linux 2.4
match http m|^HTTP/1\.1 302 Found\r\nDate: .*\r\nServer: CompaqHTTPServer/([\d.]+) HP System Management Homepage/([\d.]+)\r\n| p/HP Proliant System Management/ v/$2/ i/CompaqHTTPServer $1/
match http m|^HTTP/1\.0 400 Ungueltige Anfrage\r\nServer: Web Sharing\r\n| p/Mac OS Personal Web Sharing/ i/German/ o/Mac OS/
match http m|^HTTP/1\.1 405 Method Not Allowed\r\nContent-Type:text/html\r\n\r\n<HTML><HEAD><TITLE>Remote Insight</TITLE></HEAD><BODY>\r\n<H1>Request Error</H1>\r\nHTTP/1\.1 405 Method Not Allowed\r\n</BODY></HTML>\r\n| p|HP/Compaq Integrated Lights-Out http config| d/remote management/
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: Web Sharing\r\nContent-type: text/html\r\n\r\n<HTML><TITLE>400 Bad Request</TITLE>The URL you requested could not be understood by the server\.  Do not include double slashes or colon characters in the URL\.</HTML>\r\n\r\n| p/Apple Personal Websharing httpd/ o/Mac OS/
match http m|^Command Not Reconized\r\n$| p/Microsiga httpd/
match http m|^HTTP/1\.0 405 Method Not Allowed\r\nAllow: GET, HEAD, POST, PUT\r\n\r\n$| p/Lexmark printer http config/ d/printer/
match http m|^HTTP/1\.0 405-metode ikke tillatt\r\nTillatt: GET, HEAD, POST, PUT\r\n\r\n$| p/Lexmark printer http config/ i/Norwegian/ d/printer/
match http m|^HTTP/1\.1 500 \( Die Anforderung wurde vom HTTP-Filter zur\xc3\xbcckgewiesen\. Wenden Sie sich an den ISA Server-Administrator\.  \)\r\n| p/Microsoft ISA server httpd/ i/German/ o/Windows/
match http m|^HTTP/1\.0 \d\d\d .*\nServer: GemtekBalticHTTPD/(.*)\n| p/Gemtek Systems GemtekBalticHTTPD/ v/$1/
match http m|^HTTP/1\.0 401 Authorization Required\r\nWWW-Authenticate: Basic realm=\"TiVo-web\"\r\nConnection: close\r\n\r\n| p/TiVoWebPlus Project httpd/ d/media device/
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: ELMO Web Server\r\n.*<TITLE>HV-([\w+/-]+)</TITLE>\r\n|s p/ELMO $1 Visual Presenter http config/ d/media device/
match http m|^HTTP/1\.0 501 Not Implemented\r\nServer: HTTPD/[\d.]+\r\n.*<a href=\"/\">Return to Web Management</a>.*<A HREF=\"http://www\.juniper\.net/support/\">HTTPD release ([-\w_.]+) built by|s p/Juniper router http config/ i/HTTPD $1/ d/router/
match http m|^HTTP/1\.1 404 Not found\r\nServer: BadBlue/([\d.]+)\r\n| p/BadBlue httpd/ v/$1/ o/Windows/
match http m|^HTTP/1\.0 501 Not Implemented\r\nServer: httpd/1\.00\r\nCache-Control: no-cache\r\nExpires: 0\r\nContent-Type: text/html\r\n\r\n<HTML><HEAD><TITLE>501 Not Implemented</TITLE></HEAD>\n<BODY><H2>501 Not Implemented</H2>\nThe requested method 'OPTIONS' is not implemented by this server\.\n<HR>\n<I>httpd/1\.00</I></BODY></HTML>\n$| p|Packeteer PacketShaper 4500/ISP httpd|
match http m|^HTTP/1\.0 \d\d\d .*\r\nServer: SkyX HTTPS ([^\r\n]+)\r\n| p/Packeteer SkyX Accellerator/ v/$1/
match http m|^HTTP/1\.0 501 Not Implemented\r\nDate: .*<H1>501 Not Implemented</H1>\nPOST to non-script is not supported in Boa\.\n</BODY></HTML>\n|s p/Boa httpd/
match http m|^HTTP/1\.1 200 OK\r\n.*Server: Oracle-Application-Server-11g\r\nAllow: GET,HEAD,POST,OPTIONS\r\nContent-Length: 0\r\n|s p/Oracle Application Server 11g httpd/

# HP JetDirect Card in a LaserJet printer
match http m|^HTTP/1\.1 501 Unknown or unimplemented http action\r\nMIME-Version: 1\.0\r\nServer: HP-ChaiServer/([\d.]+)\r\nContent-length: \d+\r\nContent-Type: text/html\r\n\r\n<TITLE>Request Not Implemented</TITLE><P><B>Cannot process request, not implemented at server\.</B></P><P>Unknown or unimplemented http action| p/HP JetDirect Card in a LaserJet printer/ i/HP-ChaiServer Embedded VM $1/ d/printer/
match http m|^HTTP/1\.0 501 Not Implemented\r\nServer: Waveplus HTTPD\r\n|s p/Waveplus HTTPD/ i/Thomson TG508 DSL router/ d/broadband router/

# Zero One Technology ( http://www.01tech.com/ ) print servers embedded HTTP service
match http m|^HTTP/1\.\d\x20200\x20OK\r\nDate:\x20.*\r\nMIME-version:\x201\.\d\r\nServer:\x20ZOT-PS-(\d+)/(\d[-.\w]+)\r\n| p/Zero One Technology print server model $1 HTTP server/ v/$2/ d/print server/
match http m|^HTTP/1\.0 501 Not Implemented\r\nDate: .*\r\nMIME-version: 1\.0\r\nServer: ZOT-PS-19/8\.2\.0016\r\nContent-Type: text/html\r\n\r\n<TITLE>ERROR</TITLE><H1>501 Not Implemented</H1>Method \"OPTIONS\" is not supported\.| p/IOGear GPSU01 USB print server http config/ i/ZOT-PS-19 httpd 8.2.0016/ d/print server/

match http m|^HTTP/1\.[01] \d\d\d .*\r\nServer: micro_httpd\r\n| p/micro_httpd/
# github.com/xen-org/xen-api-libs.git
match http m|^HTTP/1\.0 500 Internal Error\r\nConnection: close\r\nCache-Control: no-cache, no-store\r\n\r\n<html><body><h1>Internal Server Error</h1>Failure\(&quot;No handler table for HTTP method Unknown OPTIONS&quot;\)</body></html>$| p/Citrix Xen Simple HTTP Server/
match http m|^HTTP/1\.1 302 Found\r\nDate: \w\w\w \w\w\w \d\d \d\d:\d\d:\d\d \d\d\d\d\n GMT\r\nServer: VCS-VideoJet-Webserver\r\nLocation: http://[\w._-]+/xampp/\r\nKeep-Alive: timeout=5, max=100\r\nConnection: Keep-Alive\r\n\r\n|s p/VCS-VideoJet-Webserver httpd/ i/Bosch VIP X1 video encoder http config/ d/webcam/
match http m|^HTTP/1\.0 501 Not Implemented\r\nServer: mini_httpd ([^\r\n]+)\r\n.*Cache-Control: no-cache,no-store\r\nContent-Type: text/html; charset=%s\r\nConnection: close\r\n|s p/mini_httpd/ v/$1/
match http m|^HTTP/1\.1 400 Bad Request\r\nServer: keyreporter/([\w._-]+)\r\nConnection: Close\r\nContent-Type: text/plain\r\nContent-Length: 20\r\n.*URL is malformatted\n$|s p/Sassafras KeyReporter http interface/ v/$1/
match http m|^HTTP/1\.1 403 Forbidden\r\n.*Content-Type: text/html;charset=[\w._-]+\r\nContent-Language: ([\w._-]+)\r\n.*Server: Hidden\r\n\r\n<html><head><title>Apache Tomcat/([\w._-]+) - Error report</title>|s p/Symantec Endpoint Protection Manager http config/ d/firewall/ i/Apache Tomcat $2; $1/
match http m|^HTTP/1\.1 403 Forbidden\r\n.*Content-Type: text/html;charset=[\w._-]+\r\n.*Server: Hidden\r\n\r\n<html><head><title>Apache Tomcat/([\w._-]+) - Error report</title>|s p/Symantec Endpoint Protection Manager http config/ d/firewall/ i/Apache Tomcat $1/
match http m|^HTTP/1\.1 400 Bad Request\r\nDate: .*\r\nConnection: close\r\nContent-Type: text/html\r\nContent-Length: 50\r\n\r\n<HTML><BODY><H1>400 Bad Request</H1></BODY></HTML>$| p/VMware Server http config/
match http m|^HTTP/1\.1 200 OK\r\n.*X-Runtime: 2\r\n.*<title>Metasploit Framework Web Console ([\w._-]+)</title>\n|s p/Metasploit Framework web console/ v/$1/
match http m|^HTTP/1\.1 400 Bad Request\r\nContent-Type: text/plain\r\nContent-Length: 59\r\nConnection: close\r\n\r\nError 400: Bad Request\nCannot parse HTTP request: \[OPTIONS\]$| p/Mongoose httpd/

match kmldonkey m|^HTTP/1\.1 400 Bad Request\r\nServer: KMLDonkey/(\d\S+)| p/KMLDonkey/ v/$1/

# webmin version 1.090 on Mandrake 8.2 - not sure why it's not picked up by the getreq probe
match http m|^HTTP/1\.0 400 Bad Request\r\nServer: MiniServ/([\d.]+)\r\n.*\r\n<h1>Error - Bad Request</h1>\n|s i/Webmin httpd/ p/MiniServ/ v/$1/
match http m|^HTTP/1\.1 400 Page not found\r\nServer: GoAhead-Webs\r\nDate: .*\r\nPragma: no-cache\r\nCache-Control: no-cache\r\nContent-Type: text/html\r\n\r\n<html><head><title>Document Error: Page not found</title></head>| i/WAP http config/ p/GoAhead httpd/ d/WAP/

match http m|^HTTP/1\.0 200 Ok\r\nCseq: 0\r\nServer: VLC Server\r\nPublic: DESCRIBE, SETUP, TEARDOWN, PLAY, PAUSE\r\nContent-Length: 0\r\n\r\n| p/VLC HTTP streamer/

match http m|^ 200 OK\r\nConnection: close\r\nContent-Type: text/html\r\n.*<B>The request is not Implemented\.</B>|s p/Dell 1815dn printer http config/ d/printer/
match http m|^HTTP/1\.0 404 Not Found\r\nConnection: close\r\n\r\n<html><head><title>404 Not Found</title></head>\r\n<body><h1>Not Found</h1>The requested URL / was not found on this server\.<p>\r\n</body></html>\r\n$| p/Mono XSP httpd/
match http m|^HTTP/1\.1 302 Found\r\nLocation: http:///home\.htm\r\nContent-Length: 0\r\nWebServer:\r\n\r\n$| p/APC SmartUPS http config/ d/power-device/
match http m|^HTTP/1\.0 400\r\nContent-Type: text/html\r\n\r\n<hr><pre><font size=\+2><b>\nError\. Unsupported method\.\n</b></font>| p/Small Home Server httpd/ o/Windows/
match http m|^HTTP/1\.0 400 Bad Request\r\nContent-Length: \d+\r\nContent-Type: text/html\r\n\r\n<HTML><HEAD><TITLE>400 Bad Request \(ERR_INVALID_REQ\)</TITLE></HEAD><BODY><H1>400 Bad Request</H1><BR>ERR_INVALID_REQ<HR><B>AR7 Webserver</B>| p/AR7 embedded httpd/
match http m|^HTTP/1\.0 400 Bad Request\r\nContent-Length: \d+\r\nContent-Type: text/html\r\n\r\n<HTML><HEAD><TITLE>400 Bad Request \(ERR_INVALID_REQ\)</TITLE></HEAD><BODY><H1>400 Bad Request</H1><BR>ERR_INVALID_REQ<HR><B>Webserver</B>| p/AVM FRITZ!Box WLAN 7170 WAP http config/ d/WAP/
match http m|^HTTP/1\.1 404 Not Found\r\nServer: Cisco AWARE ([\w._-]+)\r\n| p/Cisco ASA AWARE http config/ d/firewall/ v/$1/
match http m|^HTTP/1\.1 200 OK\r\nPragma: no-cache\r\nx-responding-server: ([\w._-]+)\r\nX-dmUser: (.*)\r\nMS-Author-Via: DAV\r\n| p/CrushFTP DAV httpd/ h/$1/ i/User $2/
match http m|^HTTP/1\.1 302 Moved Temporarily\r\nLocation: /login\r\n\r\n$| p/Bizanga IMP Email http config/
match http m|^HTTP/1\.0 501 Not Implemented\t\r\nContent-Type: text/html\r\n\r\n<HTML><HEAD><TITLE>Not Implemented</TITLE></HEAD><BODY><h3>Error: HTTP Method Not Implemented</h3></BODY></HTML>$| p/Check Point UTM-1 Edge X firewall or Zonealarm Z100G WAP http config/
match http m|^HTTP/1\.1 405 Method Not Allowed\r\nServer: Cassini/([\w._-]+)\r\n.*X-AspNet-Version: ([\w._-]+)\r\n.*<title>Runtime Error</title>\r\n        <style>\r\n         body {font-fam