# Nmap OS Fingerprinting 2nd Generation DB. -*- mode: fundamental; -*-
# $Id: nmap-os-db 24476 2011-06-29 04:47:02Z david $ 
#
# Contributions to this database are welcome.  If Nmap obtains a new
# fingerprint (and test conditions are favorable), it will print out a
# URL you can use to submit the fingerprint.  If Nmap guesses wrong,
# please see http://nmap.org/submit/ .
#
# By submitting fingerprints you are transfering any and all copyright
# interest in the data to Insecure.Com LLC so it can modified,
# incorporated into Nmap, relicensed, etc.
#
# This collection of fingerprint data is (C) 1996-2010 by Insecure.Com
# LLC.  It is distributed under the Nmap Open Source license as
# provided in the COPYING file of the source distribution or at
# http://nmap.org/data/COPYING .  Note that this license
# requires you to license your own work under a compatable open source
# license.  If you wish to embed Nmap technology into proprietary
# software, we sell alternative licenses (contact sales@insecure.com).
# Dozens of software vendors already license Nmap technology such as
# host discovery, port scanning, OS detection, and version detection.
# For more details, see http://nmap.org/book/man-legal.html
#
# For a complete description of Nmap OS detection and the format of
# fingerprints in this file, see http://nmap.org/book/osdetect.html.

# This first element provides the number of points every fingerprint
# test is worth.  Tests like TTL or Don't fragment are worth less
# (individually) because there are so many of them and the values are
# often correlated with each other.  Meanwhile, elements such as TS
# (TCP timestamp) which are only used once, get more points.  Points
# are used when there are no perfect matches to determine which OS
# fingerprint matches a target machine most closely.
MatchPoints
SEQ(SP=25%GCD=75%ISR=25%TI=100%CI=50%II=100%SS=80%TS=100)
OPS(O1=20%O2=20%O3=20%O4=20%O5=20%O6=20)
WIN(W1=15%W2=15%W3=15%W4=15%W5=15%W6=15)
ECN(R=100%DF=20%T=15%TG=15%W=15%O=15%CC=100%Q=20)
T1(R=100%DF=20%T=15%TG=15%S=20%A=20%F=30%RD=20%Q=20)
T2(R=80%DF=20%T=15%TG=15%W=25%S=20%A=20%F=30%O=10%RD=20%Q=20)
T3(R=80%DF=20%T=15%TG=15%W=25%S=20%A=20%F=30%O=10%RD=20%Q=20)
T4(R=100%DF=20%T=15%TG=15%W=25%S=20%A=20%F=30%O=10%RD=20%Q=20)
T5(R=100%DF=20%T=15%TG=15%W=25%S=20%A=20%F=30%O=10%RD=20%Q=20)
T6(R=100%DF=20%T=15%TG=15%W=25%S=20%A=20%F=30%O=10%RD=20%Q=20)
T7(R=80%DF=20%T=15%TG=15%W=25%S=20%A=20%F=30%O=10%RD=20%Q=20)
U1(R=50%DF=20%T=15%TG=15%IPL=100%UN=100%RIPL=100%RID=100%RIPCK=100%RUCK=100%RUD=100)
IE(R=50%DFI=40%T=15%TG=15%CD=100)

# 4-port GSM-SIP gateway PORTech MV-374
# 2FXS VoIP gateway K-3288W
Fingerprint 2FXS K-3288W or PORTech MV-374 GSM-SIP VoIP gateway
Class 2FXS | embedded || VoIP adapter
Class PORTech | embedded || VoIP adapter
SEQ(SP=0-5%GCD=61A8|C350|124F8|186A0|1E848%ISR=8A-94%TI=I%II=RI%SS=O%TS=U)
OPS(O1=M5B4|WANM5B4T10S%O2=M578|M578W0ST10L%O3=M280|T10NNW5NM280%O4=M5B4|ST10WAL%O5=M218|M218ST10WAL%O6=M109|M109ST10)
WIN(W1=0|3180%W2=0|3180%W3=0|3180%W4=0|3180%W5=0|3180%W6=0|3180)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=WANM5B4SNN%CC=N%Q=R)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O|Z%A=S+%F=AR|AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# 2wire 1701HG Gateway 3.17.5
Fingerprint 2Wire 1701HG wireless ADSL modem
Class 2Wire | embedded || WAP
SEQ(SP=7E-9A%GCD=1-6%ISR=9E-A8%TI=I%TS=A)
OPS(O1=M5ACNNSW0NNNT11%O2=M578NNSW0NNNT11%O3=M280W0NNNT11%O4=M218NNSW0NNNT11%O5=M218NNSW0NNNT11%O6=M109NNSNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=8000%O=M5ACNNSW0N%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=E44A4E43%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=EA6C967D%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# 1701HG Gateway, Software Version: 3.17.5
# 2Wire 2700HG
# 2 Wire RG2701HG-00
# 2Wire 2701HG-B
# 2700HG-B 2Wire gateway
# 2Wire, Inc. 3800HGV-B Software Version        6.1.9.24-enh.tm
Fingerprint 2Wire 1701HG, 2700HG, 2700HG-B, 2701HG-B, RG2701HG, or 3800HGV-B wireless ADSL modem
Class 2Wire | embedded || WAP
SEQ(SP=5A-A0%GCD=1-6%ISR=98-A9%TI=I%TS=A)
OPS(O1=M5B4NNSW0NNNT11%O2=M578NNSW0NNNT11%O3=M280W0NNNT11%O4=M218NNSW0NNNT11%O5=M218NNSW0NNNT11%O6=M109NNSNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=8000%O=M5B4NNSW0N%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=E44A4E43%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=EA6C967D%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Version 6.0 (Build 6002: Service Pack 2)
# 2Wire 2701HG-B Gateway running version 5.29.47
Fingerprint 2Wire 2700HG-B wireless ADSL modem
Class 2Wire | embedded || WAP
SEQ(SP=7C-AA%GCD=1-6%ISR=94-9E%TI=I%TS=A)
OPS(O1=M5B4NNSW0NNNT11%O2=M578NNSW0NNNT11%O3=M280W0NNNT11%O4=M218NNSW0NNNT11%O5=M218NNSW0NNNT11%O6=M109NNSNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=8000%O=M5B4NNSW0N%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=N)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# 2wire 2701 HG router
Fingerprint 2Wire 2701HG wireless ADSL modem
Class 2Wire | embedded || WAP
SEQ(SP=6D-C3%GCD=1-6%ISR=96-A0%TI=I%CI=I%TS=E)
OPS(O1=M5B4NNSW0NNNT11%O2=M578NNSW0NNNT11%O3=M280W0NNNT11%O4=M218NNSW0NNNT11%O5=M218NNSW0NNNT11%O6=M109NNSNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=8000%O=M5B4NNSW0N%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=E44A4E43%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=EA6C967D%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# 2wire router/WAP/DSL-modem is model# 2701HG-B
Fingerprint 2Wire 2701HG-B wireless ADSL modem
Class 2Wire | embedded || WAP
SEQ(SP=84-DA%GCD=1-6%ISR=95-CD%TI=I|RD%II=I%SS=S%TS=A)
OPS(O1=M5B4NNSW0NNNT11%O2=M578NNSW0NNNT11%O3=M280W0NNNT11%O4=M218NNSW0NNNT11%O5=M218NNSW0NNNT11%O6=M109NNSNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=8000%O=M5B4NNSW0N%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=E44A4E43%Q=)
T3(R=Y%DF=Y%T=FA-104%TG=FF%W=8000%S=O%A=S+%F=AS%O=M109NNSW0NNNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=E44A4E43%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=EA6C967D%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=EA6C967D%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# 2Wire 2701HG-B Gateway AT&T DSL Wireless Access Point
Fingerprint 2Wire 2701HG-B wireless ADSL modem
Class 2Wire | embedded || WAP
SEQ(SP=62-9E%GCD=1-6%ISR=99-A3%TI=I%CI=I%TS=A)
OPS(O1=M5B4NNSW0NNNT11%O2=M578NNSW0NNNT11%O3=M280W0NNNT11%O4=M5B4NNSW0NNNT11%O5=M218NNSW0NNNT11%O6=M109NNSNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=8000%O=M5B4NNSW0N%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=E44A4E43%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=EA6C967D%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# 2-Wire 2701HG-G Gateway Software:  5.29.133.27
Fingerprint 2Wire 2701HG-G wireless ADSL modem
Class 2Wire | embedded || WAP
SEQ(SP=7B-85%GCD=1-6%ISR=95-9F%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NNSW0NNNT11%O2=M578NNSW0NNNT11%O3=M280W0NNNT11%O4=M218NNSW0NNNT11%O5=M218NNSW0NNNT11%O6=M109NNSNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=8000%O=M5B4NNSW0N%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=FA-104%TG=FF%W=8000%S=O%A=S+%F=AS%O=M109NNSW0NNNT11%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=N)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# 2wire wireless Broadband router version 3.5.55
# 2wire 1000SW Shasta 3.5.12
Fingerprint 2Wire Shasta wireless broadband router
Class 2Wire | embedded || WAP
SEQ(SP=76-A2%GCD=1-6%ISR=A0-AD%TI=I%TS=7)
OPS(O1=M5B4NNSW0NNNT11%O2=M578NNSW0NNNT11%O3=M280W0NNNT11%O4=M218NNSW0NNNT11%O5=M218NNSW0NNNT11%O6=M109NNSNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=8000%O=M5B4NNSW0N%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=E44A4E43%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=EA6C967D%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# 3com OfficeConnect 812 ADSL Router
Fingerprint 3com OfficeConnect 812 ADSL router
Class 3Com | embedded || broadband router
SEQ(SP=0-63%GCD=61A8|C350|124F8|186A0|1E848%ISR=8A-B0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=U)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=U)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=|U)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# 3Com X5 Unified Security Platform 3CRTPX5-U-96 with TOS Version X3.1. 1.2109
Fingerprint 3Com X5 Unified Security Platform firewall
Class 3Com | embedded || firewall
SEQ(II=I%TS=3)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3A-44%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3F%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3A-44%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=N%T=3A-44%TG=40%CD=Z)

# 3Com OfficeConnect 3CR858-91 Software version V1.13-168 (Mar 21 2008 11:57:49)
Fingerprint 3Com OfficeConnect 3CR858-91 router
Class 3Com | embedded || router
SEQ(SP=0-5%GCD=B|16|21|2C|37%ISR=30-3A%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=1770%W2=1770%W3=1770%W4=1770%W5=1770%W6=1770)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1770%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N|S%T=3B-45%TG=40%CD=Z)

# 3Com Switch 4200G 24-Port Software Version 3Com OS V3.01.00s56
# Quadway s5600 series, VRP software, Version 3.10, Release 1510P02
Fingerprint 3Com 4200G or Huawei Quidway S5600 switch
Class 3Com | embedded || switch
Class Huawei | VRP | 3.X | switch
SEQ(SP=FB-107%GCD=1-6%ISR=100-110%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1FC4%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Huawei S3928P-EI switch VRP software, Version 3.10
# 3Com Switch 4210 26-Port Software Version 3Com OS V3.01.01s56, Bootrom Version is 4.01
# Quidway S5624F, VRP software, Version 3.10, Release 1510P02
Fingerprint 3Com 4210, or Huawei Quidway S3928P-EI or S5624F switch (VRP 3.10)
Class 3Com | embedded || switch
Class Huawei | VRP | 3.X | switch
SEQ(SP=FF-109%GCD=1-6%ISR=105-111%TI=I%II=I%SS=S%TS=U)
OPS(O1=M200%O2=M200%O3=M200%O4=M200%O5=M200%O6=M200)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=100%TG=FF%W=2000%O=M200%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=100%TG=FF%W=1FC4%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=100%TG=FF%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# 3com 4500G P.O.E switch
Fingerprint 3Com 4500G switch
Class 3Com | embedded || switch
SEQ(SP=C1-CD%GCD=1-6%ISR=CD-D9%TI=I%CI=I%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1FC4%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(R=N)

# 3Com Switch 5500-EI 28-Port Software Version 3Com OS V3.03.02s168ep05
# 3Com SuperStack 4 Switch 5500G-EI 24-Port Software Version 3Com OS V3.02.04s56
Fingerprint 3Com 5500-EI switch
Class 3Com | embedded || switch
SEQ(SP=FC-106%GCD=1-6%ISR=100-10F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M200%O2=M200%O3=M200%O4=M200%O5=M200%O6=M200)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2000%O=M200%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# 3Com 8810 with 3Com 3C17508 360GB Fabric. SW Version: 3.01.31r. Also known as: Huawei Quidway S8500.
Fingerprint 3Com 8810 switch
Class 3Com | embedded || switch
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=RI%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=100%TG=FF%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=100%TG=FF%W=1FC4%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=100%TG=FF%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# 3Com Baseline Switch 2226-SFP Plus / 3CBLSF26
Fingerprint 3Com Baseline Switch 2226-SFP Plus
Class 3Com | embedded || switch
SEQ(SP=8C-96%GCD=1-6%ISR=92-9C%TI=I%II=RI%SS=O|S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=3908%W2=3908%W3=3908%W4=3908%W5=3908%W6=3908)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3908%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=3908%S=O%A=S+%F=AS%O=M5B4NW0NNT11NNLLLLLLLLLL|M5B4NW0NNT11W2DW2DNNLLLL%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Baseline Switch 2250-SFP Plus
Fingerprint 3Com Baseline Switch 2250-SFP Plus
Class 3Com | embedded || switch
SEQ(SP=90-A0%GCD=1-6%ISR=97-A1%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5A8NW0NNT11%O2=M5A8NW0NNT11%O3=M5A8NW0NNT11%O4=M5A8NW0NNT11%O5=M5A8NW0NNT11%O6=M5A8NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=43E0%W5=4180%W6=403D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=403D%S=O%A=S+%F=AS%O=M5A8NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=3401%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Baseline Switch 2924-SFP Plus
Fingerprint 3Com Baseline Switch 2924-SFP Plus
Class 3Com | embedded || switch
SEQ(SP=FD-10D%GCD=1-6%ISR=FA-112%TI=RD%CI=RD|RI%II=RI%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=100%W2=100%W3=100%W4=100%W5=100%W6=100)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=100%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=100%S=O%A=S+%F=AS%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Motorola Surfboard SB5101 Cable Modem
# SB5101 help page says: Software Version: SB5101-2.4.1.6-SCM02-NOSH; Hardware Version: 1
# Scientific Atlanta WebSTAR EPX2203 cable modem, v2.0.2r1152-050419epx2203-v202r1152-050419c-eu-5.bin
# Baseline Switch 2948-SFP Plus
# FreeBSD 4.4-RELEASE FreeBSD 4.4-RELEASE #0: Tue Sep 18 11:57:08 PDT 2001 i386
# Tandberg 3000 MXP Video Conference System, Firmware Tandberg Release F7.0
# Allworx 24x PBX
# Tandberg Edge 95MXP
# Gigavue 2404 Gigamon Lawful interception/monitoring device
# VxWorks? --Ed.
Fingerprint 3Com Baseline Switch 2948-SFP Plus; Allworx 24x PBX; Motorola SURFboard SB5101 or Scientific Atlanta WebSTAR EPX2203 cable modem; or Tandberg MXP video conferencing system
Class 3Com | embedded || switch
Class Allworx | embedded || PBX
Class Motorola | embedded || broadband router
Class Scientific Atlanta | embedded || broadband router
Class Tandberg | embedded || webcam
SEQ(SP=BE-108%GCD=1-6%ISR=E8-110%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4074%W5=4180%W6=403D)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=403D%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# 3Com SuperStack 3 Switch 3300
Fingerprint 3Com SuperStack 3 Switch 3300
Class 3Com | embedded || switch
SEQ(SP=0-5%GCD=0%ISR=0-5%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=5493%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Switch 3300TM, Software Version: 2.69, Boot PROM Version: 1.00
# Switch 3300SM 3C16987A
Fingerprint 3Com SuperStack 3 Switch 3300 TM
Class 3Com | embedded || switch
SEQ(SP=0%GCD=0%ISR=0%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M59C%O2=M59C%O3=M59C%O4=M59C%O5=M59C%O6=M59C)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M59C%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M59C%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=>0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

#  Device type: switch.   Running: 3Com embedded.
# OS details: 3Com Superstack 3, 3300XM switch , Boot PROM Version:  1.00, Software Version:  2.69, Hardware Version:  0
Fingerprint 3Com SuperStack 3 Switch 3300 XM
Class 3Com | embedded || switch
SEQ(SP=0%GCD=1-6%ISR=0%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M59C%O2=M59C%O3=M59C%O4=M59C%O5=M59C%O6=M59C)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M59C%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M59C%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=>0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# 3300 XM 24 Port
Fingerprint 3Com SuperStack 3 Switch 3300 XM
Class 3Com | embedded || switch
SEQ(SP=0-5%GCD=0%ISR=0-5%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=BABA%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# 3Com SuperStack 3, Operational Version: 3.04, Boot Version: 2.03
# SuperStack Switch 4200
# 3Com SuperStack 3 Switch 4400 SE
Fingerprint 3Com SuperStack 3 Switch 3300 XM, 4200, or 4400 SE
Class 3Com | embedded || switch
SEQ(SP=1E-6A%GCD=1-6%ISR=4B-55%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=BABA%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# 3Com 3870 Switch 3CR17451-91
Fingerprint 3Com SuperStack 3 Switch 3870
Class 3Com | embedded || switch
SEQ(SP=88-92%GCD=1-6%ISR=90-9A%TI=I%CI=I%II=RI%SS=O)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# 3Com SuperStack 3 4226T, Hardware Version: 01.01.00, Software Version: 3.00, Boot Version: 1.00
# 3Com Super Stack Switch 4200
# 3Com SuperStack 3, Hardware Version: 04.01.01, Boot Version: 2.03
# 3COM 3C17302A switch
# 3Com SuperStack 3, Operational Version: 3.00
Fingerprint 3Com SuperStack 3 Switch 4200 or 4226T
Class 3Com | embedded || switch
SEQ(SP=2E-50%GCD=1-8|5C|B8|114|170|1CC%ISR=4A-54%TI=I%II=I%SS=S%TS=U)
OPS(O1=M598%O2=M598%O3=M598%O4=M598%O5=M598%O6=M598)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M598%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M598%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=BABA%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# 3Com Super Stack 4300 48x100Mbit Switch w. Firmware Version  V1.12 and Hardware Version 4.0
# Samsung ML-2571N printer, Main Firmware Version: OS 1.01.01.18 05-03-2007, Network Firmware Version: V4.02.05(ML-2571N) 04-25-2007
# Xerox Phaser 3125/N network printer
# Samsung 6555N Scanner/Printer/Copier
# Dell Remote Access Controller in a Dell Power Edge 2650, 3.12 (Build 04.26)
# VxWorks? -- Ed.
Fingerprint 3Com SuperStack 3 Switch 4300, Dell PowerEdge 2650 remote access controller, Samsung ML-2571N or 6555N printer, or Xerox Phaser 3125N printer
Class 3Com | embedded || switch
Class Dell | embedded || remote management
Class Samsung | embedded || printer
Class Xerox | embedded || printer
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=96-A0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# 3Com SuperStack3 4400 switch
Fingerprint 3Com SuperStack 3 Switch 4400
Class 3Com | embedded || switch
SEQ(SP=0-8D%GCD=1-6|8|58|B0|108|160|1B8%ISR=48-52%TI=I%II=I%SS=S%TS=U)
OPS(O1=M594%O2=M594%O3=M594%O4=M594%O5=M594%O6=M594)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M594%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M594%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=BABA%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# 3Com SuperStack 3 Switch 4400 SE
Fingerprint 3Com SuperStack 3 Switch 4400 SE
Class 3Com | embedded || switch
SEQ(SP=0-5%ISR=0-5%GCD=0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M594%O2=M594%O3=M594%O4=M594%O5=M594%O6=M594)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M594%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M594%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=BABA%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# 3Com SuperStack 3 Switch 4400 SE
Fingerprint 3Com SuperStack 3 Switch 4400 SE
Class 3Com | embedded || switch
SEQ(SP=45-4F%GCD=1-6%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=BABA%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# 3Com 5500G-EI 48 Port
# super stack 3 4500  50 port managed switch
Fingerprint 3Com SuperStack 3 Switch 4500
Class 3Com | embedded || switch
SEQ(SP=FB-10D%GCD=1-6%ISR=107-111%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=100%TG=FF%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=100%TG=FF%W=1FC4%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=100%TG=FF%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# 3Com SuperStack 3 Switch 4500 Software Version 3Com OS V3.01.00s168
Fingerprint 3Com SuperStack 3 Switch 4500
Class 3Com | embedded || switch
SEQ(SP=B-1B%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=96-A0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FB-105%TG=FF%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FB-105%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FB-105%TG=FF%W=1FC4%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FB-105%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FB-105%TG=FF%CD=S)

# 3Com SuperStack 3 Switch 4500 PWR 26-Port, Software Version:  3.01.00s56op01, Bootrom Version:  1.01, Hardware Version:  00.00.00
# Huawei Quidway 18-32 ADSL Router, Versatile Routing Platform Software VRP(R) software, Version 3.30, Release 002
Fingerprint 3Com SuperStack 3 Switch 4500 or Huawei Quidway AR 18-32 ADSL router
Class 3Com | embedded || switch
Class Huawei | VRP | 3.X | broadband router
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=100%TG=FF%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=100%TG=FF%W=1FC4%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=100%TG=FF%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# 3Com SuperStack II Switch 3300
Fingerprint 3Com SuperStack II Switch 3300
Class 3Com | embedded || switch
SEQ(SP=0-5%GCD=0%ISR=0-5%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=99DF%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# 3Com SuperStack II Switch 3900-36 version 3.0.1
# 3com SuperStack II Switch 3900-36 (rev CA) firmware version: 3.0.5-7
Fingerprint 3Com SuperStack II Switch 3900-36
Class 3Com | embedded || switch
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# 3com SuperStack Switch 4200 (PN 3C17302), Software Version 02.10, Hardware Version 02.07.00, Boot Version 1.02
Fingerprint 3Com SuperStack Switch 4200
Class 3Com | embedded || switch
SEQ(SP=0-5%GCD=1-6%ISR=0-5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M598%O2=M598%O3=M598%O4=M598%O5=M598%O6=M598)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M598%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M598%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=BABA%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# 3Com Switch 4200, Software Version: 02.03
Fingerprint 3Com Switch 4200
Class 3Com | embedded || switch
SEQ(SP=0-5%GCD=0%ISR=0-5%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M598%O2=M598%O3=M598%O4=M598%O5=M598%O6=M598)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M598%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M598%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=BABA%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# 3CRWDR100A-72, Software version 2.06T13 (Apr 25 2007 17:06:30), Boot loader version 0.67.3, ADSL modem version 07.00.04.00A
Fingerprint 3Com OfficeConnect 3CRWDR100A-72 wireless ADSL modem
Class 3Com | embedded || WAP
SEQ(SP=0-5%GCD=A|14|1E|28|32%ISR=30-3A%TI=I|RD%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=1770%W2=1770%W3=1770%W4=1770%W5=1770%W6=1770)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1770%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N|Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N|S%T=3B-45%TG=40%CD=Z)

# 3Com OfficeConnect Wireless 11g Cable/DSL Router (3CRWE554G72T/3CRWE554G72TU), Version 2.01.05
Fingerprint 3Com OfficeConnect 3CRWE554G72T wireless broadband router
Class 3Com | embedded || WAP
SEQ(SP=8F-99%GCD=1-6%ISR=94-9E%TI=I|RD%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2238%W2=20D0%W3=2080%W4=2000%W5=2180%W6=2017)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2238%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# 3Com 3CRWER100-75 firmware 1.3
Fingerprint 3Com OfficeConnect 3CRWER100-75 wireless broadband router
Class 3Com | embedded || WAP
SEQ(SP=C7-D1%GCD=1-6%ISR=D0-DA%TI=Z%II=I%TS=7)
OPS(O1=M5ACST11%O2=M5ACST11%O3=M5ACNNT11%O4=M5ACST11%O5=M5ACST11%O6=M5ACST11)
WIN(W1=1680%W2=1680%W3=1680%W4=1680%W5=1680%W6=1680)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16B0%O=M5ACNNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1680%S=O%A=S+%F=AS%O=M5ACST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# 3com OfficeConnect wirless router 3CRWER100-75 firmware 1.2.0
Fingerprint 3Com OfficeConnect 3CRWER100-75 wireless router
Class 3Com | embedded || WAP
SEQ(SP=B1-BB%GCD=1-6%ISR=C4-CE%TI=Z%II=I%TS=7)
OPS(O1=M5B4ST11%O2=M5B4ST11%O3=M5B4NNT11%O4=M5B4ST11%O5=M5B4ST11%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# 3Com Wireless LAN Switch (3Com WX1200).
Fingerprint 3Com WX1200 Wireless LAN Switch
Class 3Com | embedded || WAP
SEQ(SP=C7-D1%GCD=2|4|6|8|A%ISR=DA-E4%TI=Z%CI=Z%II=Z%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=2DA0%W2=2DA0%W3=2DA0%W4=2DA0%W5=2DA0%W6=2DA0)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2DA0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=A%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=Z)

# Enterasys Wireless Switch RBT-8400, 7.0.9.8 REL
# 3Com WX2200 running firmware 7.0.5.6.0
Fingerprint 3Com WX2200 or Enterasys RBT-8400 WAP
Class 3Com | embedded || WAP
Class Enterasys | embedded || WAP
SEQ(SP=C4-D0%GCD=1-6%ISR=DC-E6%TI=Z%CI=Z%II=Z%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=2DA0%W2=2DA0%W3=2DA0%W4=2DA0%W5=2DA0%W6=2DA0)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2DA0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A+%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=Z)

# Philips SNB6500 wireless router - Runtime Code Version V1.09 (Dec 6 2005 14:30:34)
# 3Com OfficeConnect ADSL Wireless 11g Firewall Router, 3Com code 3CRWDR100A-72, software version 2.06
# Sinus 154 DSL Basic 3 router (German Telekom)
# SMCWEBT-G, access point with SMC firmware V1.07.2 (English, 09/18/2006)
# SMCWBR14-G2
# 3Com OfficeConnect ADSL router, wireless 54Mbit
Fingerprint Wireless broadband router (3Com OfficeConnect 3CRWDR100A-72, Philips SNB6500, Sinus 154, SMC SMCWEBT-G, or SMC SMCWBR14-G2)
Class 3Com | embedded || WAP
Class Philips | embedded || WAP
Class Sinus | embedded || WAP
Class SMC | embedded || WAP
SEQ(SP=0-1F%GCD=1-6|A|14|1E|28|32|3C%ISR=30-3A%TI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=1770%W2=1770%W3=1770%W4=1770%W5=1770%W6=1770)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1770%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1770%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N|Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N|O|S|Y%T=3B-45%TG=40%CD=Z)

# 3Com NBX 100. VxWorks: http://www.3com.com/products/en_US/detail.jsp?tab=features&pathtype=purchase&sku=WEBBNGNBX100COMSYS
Fingerprint 3Com NBX 100 VoIP gateway (VxWorks)
Class 3Com | VxWorks || VoIP adapter
SEQ(SP=13-1D%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5C2NW0NNT11%O2=M5C2NW0NNT11%O3=M5C2NW0NNT11%O4=M5C2NW0NNT11%O5=M5C2NW0NNT11%O6=M5C2NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5C2NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# MS347S : see http://www.a-tecsubsystem.com/websys/atec/web/products.jsp?prodId=1191910612953
# Mapower KC 31N, usb/nas diskbox
Fingerprint A-Tec MS347S or Mapower KC31N NAS device
Class A-Tec | embedded || storage-misc
Class Mapower | embedded || storage-misc
SEQ(SP=0-19%GCD=1-6%ISR=57-63%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=8000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=1B-25%TG=20%W=8000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=1B-25%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=1B-25%TG=20%CD=S)

# Sun RSC Version 2.2.3, bootmon 2.0.0
# aastra 480i
Fingerprint Aastra 480i IP Phone or Sun Remote System Control (RSC)
Class Aastra | embedded || VoIP phone
Class Sun | embedded || remote management
SEQ(CI=I%II=I)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=N)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# TOSHIBA e-STUDIO 3510c
# TOSHIBA e-STUDIO351c
# Toshiba e-Studio 520 copier, Firmware Version T390SY0U321, Main ROM Version 390M-14, Scanner ROM Version 390S-05
# Aastra ip phone 57i Revision 0, Firmware Version 2.3.0.82
# e-STUDIO 520 and an e-STUDIO 850
# TOSHIBA e-STUDIO281c multifunction printer
# Ethernet Routing Switch 4548GT-PWR    HW:06       FW:5.2.0.3   SW:v5.3.1.001 BN:01 (c) Nortel Networks
# VxWorks? -- Ed.
Fingerprint Aastra 57i IP phone; Nortel 4548GT switch; or Toshiba e-STUDIO 281c, 351c, 3510c, 520, or 850 printer
Class Aastra | embedded || VoIP phone
Class Nortel | embedded || printer
Class Toshiba | embedded || printer
SEQ(SP=FF-10B%GCD=1-6%ISR=FF-10F%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# AirPort Express, firmware 6.3
# Aastra 6731i Revision 0, Firmware Version 2.5.0.82
Fingerprint Aastra 6731i VoIP phone or Apple AirPort Express WAP
Class Aastra | embedded || VoIP phone
Class Apple | embedded || WAP
SEQ(CI=I%II=I)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=N)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Aastra Dialog 4425 VoIP Phone, firmware RK7
Fingerprint Aastra Dialog 4425 IP phone
Class Aastra | embedded || VoIP phone
SEQ(SP=FF-109%GCD=1-6%ISR=107-111%TI=I%CI=I%II=I%SS=S%TS=9)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Aastra/DeTeWe RFP L32 IP Poe DECT Basis Station. Software is Open Mobility Manager 1.1.4.
Fingerprint Aastra RFP L32 IP DECT WAP
Class Aastra | embedded || WAP
SEQ(SP=C2-CC%GCD=1-6%ISR=C8-D2%TI=Z%II=I%TS=8)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Aceex BR41 Broadband Router Firmware Version 2.2f
Fingerprint Aceex BR41 broadband router
Class Aceex | embedded || broadband router
SEQ(SP=0-35%GCD=1-6|B|16|21|2C|37|42%ISR=30-3A%TI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=800%W2=800%W3=800%W4=800%W5=800%W6=800)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=800%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=800%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# ACME Packet SBC Net-Net 4250 Firmware: SC6.2.0 MR-3
Fingerprint Acme Packet Net-Net 4250 VoIP session border controller
Class Acme Packet | embedded || firewall
SEQ(SP=FD-109%GCD=1-6%ISR=108-112%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5ACNW1NNT11%O2=M5ACNW1NNT11%O3=M5ACNW1NNT11%O4=M5ACNW1NNT11%O5=M5ACNW1NNT11%O6=M5ACNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5ACNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5ACNW1NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Acorp-W422G, wireless ADSL router.
# Linux 2.4.17_mvl21-malta-mips_fp_le (root@home1.homework) (gcc version 2.95.3 20010315 (release/MontaVista)) #1 Sat Sep 8 00:03:33 MSD 2007, Acorp-W400G ADSL and Wi-Fi router,
Fingerprint Acorp W400G or W422G wireless ADSL modem (MontaVista embedded Linux 2.4.17)
Class Acorp | embedded || WAP
SEQ(SP=C2-CC%GCD=1-6%ISR=C7-D1%TI=Z%II=I%TS=7)
OPS(O1=M5B4ST11%O2=M5B4ST11%O3=M5B4NNT11%O4=M5B4ST11%O5=M5B4ST11%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# This is a GT701, which is issued by QWEST.
Fingerprint Actiontec GT701 DSL modem
Class Actiontec | embedded || broadband router
SEQ(SP=C8-D2%GCD=1-6%ISR=CC-D6%TI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Actiontec Wireless Cable/DSL Router Model: R3010UW Firmware version: 1.0.10.0.76-R3010UW
Fingerprint Actiontec R3010UW wireless broadband router
Class Actiontec | embedded || WAP
SEQ(SP=71-87%GCD=1-6%ISR=75-8F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M109|M5A0%O2=M109|M578%O3=M109|M280%O4=M109|M280%O5=M109|M218%O6=M109)
WIN(W1=1194%W2=1194%W3=1194%W4=1194%W5=1194%W6=1194)
ECN(R=Y%DF=N%T=96-A0%TG=FF%W=1194%O=M109%CC=N%Q=)
T1(R=Y%DF=N%T=96-A0%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=96-A0%TG=FF%W=1194%S=A%A=Z%F=R%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=96-A0%TG=FF%W=1194%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=96-A0%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=96-A0%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=96-A0%TG=FF%W=0%S=Z%A=Z%F=R%O=%RD=0%Q=)
U1(DF=N%T=96-A0%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=96-A0%TG=FF%CD=S)

# Adaptec Model: 4000 series, Software: 3.1.603 (US), Hardware: 2.2.1, BIOS: 2.4.437
Fingerprint Adaptec RAID 4000 I/O controller
Class Adaptec | embedded || storage-misc
SEQ(SP=0-17%GCD=3200|6400|9600|C800|FA00|12C00%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2238%W2=2238%W3=2238%W4=2238%W5=2238%W6=2238)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2238%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=2238%S=O%A=O%F=A|AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=2238%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# "Snap! Server" model 100
Fingerprint Adaptec Snap Server 100 NAS device
Class Adaptec | embedded || storage-misc
SEQ(SP=C-16%GCD=3200|6400|9600|C800|FA00%ISR=96-A0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2238%W2=2238%W3=2238%W4=2238%W5=2238%W6=2238)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=2238%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=1B-25%TG=20%W=2238%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=2238%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Snap Appliance Snap Server 1100
Fingerprint Adaptec Snap Server 100 NAS device
Class Adaptec | embedded || storage-misc
SEQ(SP=D-17%GCD=3200|6400|9600|C800|FA00%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2238%W2=2238%W3=2238%W4=2238%W5=2238%W6=2238)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2238%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=2238%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=2238%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# ADIC Scalar 1000 tape library remote management unit, firmware 161A.00005
Fingerprint ADIC Scalar 1000 tape library remote management unit
Class ADIC | embedded || storage-misc
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%II=I%TS=U)
OPS(O1=M200NW0%O2=M200NW0%O3=M200NW0%O4=M200NW0%O5=M200NW0%O6=M200)
WIN(W1=578%W2=578%W3=578%W4=578%W5=578%W6=578)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=578%O=M200NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=578%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=578%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Adtran NetVanta 1224R; ADTRAN, Inc. OS version 13.14.00
Fingerprint Adtran NetVanta 1224R router
Class Adtran | embedded || router
SEQ(SP=D2-DC%GCD=1-6%ISR=DF-E9%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=DAC%W2=DAC%W3=DAC%W4=DAC%W5=DAC%W6=DAC)
ECN(R=N)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=Z)

# NetVanta 3200 Firmware Version  10.01.00.E Part Number  1202860L1
# ADTRAN Total Access 908, Second Generation. ! ADTRAN, Inc. OS version A2.04.00.E ! Boot ROM version 14.04.00
Fingerprint Adtran NetVanta 3200 or Total Access 908 ADSL router
Class Adtran | embedded || router
SEQ(SP=E1-F1%GCD=1-6%ISR=E4-F8%TI=I|RD%II=I%SS=O|S%TS=U)
OPS(O1=%O2=%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=DAC%W2=DAC%W3=DAC%W4=DAC%W5=DAC%W6=DAC)
ECN(R=N)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=Z)

# Adtran Total Access 624
Fingerprint Adtran Total Access 624 router
Class Adtran | embedded || router
SEQ(SP=0-5%GCD=388|710|A98|E20|11A8%ISR=64-6E%TI=I%II=I%SS=S%TS=U)
OPS(O1=M3F1%O2=M3F1%O3=M3EE%O4=M5B4%O5=M3EE%O6=M3ED)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=9E-A8|C6-E1%TG=FF%W=1000%O=M3F1%CC=N%Q=)
T1(R=Y%DF=N%T=83-8D|C5-D9|DD-E7%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=A7-B9|CE-DE|E1-EB%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=86-90|B0-BA|C5-CF|DA-E4|EA-F4%TG=FF%W=1000%S=O%A=S+%F=AS%O=M3ED%RD=0%Q=)
T4(R=Y%DF=N%T=9D-A7|C5-E0|E9-F3%TG=FF%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=85-8F|AF-B9|C4-CE|D9-E3|E9-F3%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=9C-A6|C4-DF|E8-F2%TG=FF%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=A1-B5|C3-CD|D8-E2|E8-F2%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=Z)

# Adtran MX2800 M13 Mux (ds1's in ds3), Code Version = 3.42A, Boot Version = 2.10A
Fingerprint Adtran MX2800 multiplexer
Class Adtran | embedded || specialized
SEQ(SP=2D-9F%GCD=FA|1F4|2EE|3E8|4E2%ISR=8A-B4%TI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1000%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1000%S=O%A=O|S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Platform: HiveAP320_n, HiveOS 3.4r1 release
Fingerprint Aerohive HiveAP 320 WAP (HiveOS 3.4)
Class Aerohive | embedded || WAP
SEQ(SP=C7-D1%GCD=1-6%ISR=CB-D5%TI=I%CI=Z%II=I%SS=S%TS=A)
OPS(O1=M5B4ST11NW2%O2=M5B4ST11NW2%O3=M5B4NNT11NW2%O4=M5B4ST11NW2%O5=M5B4ST11NW2%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW2%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW2%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# AGFA DryStar 5500 Printer
Fingerprint Agfa DryStar 5500 printer
Class Agfa | embedded || printer
SEQ(SP=0-15%GCD=3200|6400|9600|C800|FA00%ISR=8B-95%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=2238%W2=2238%W3=2238%W4=2238%W5=2238%W6=2238)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2238%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2238%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=Z)

# This is an Airaya brand microwave radio (AI108-4958-O) which has an http and a telnet interface. https://secure.airaya.com/proddetail.asp?prod=AI108-4958-O-300
Fingerprint Airaya AI108-4958-O-300 wireless Ethernet bridge
Class Airaya | embedded || bridge
SEQ(SP=13-1D%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# This is an Airlink 101 1 port USB 2.0 Multi-functional Printer Server, Model APS MFP210 (www.airlink101.com).
Fingerprint Airlink101 APS MFP210 multi-functional print server
Class Airlink101 | embedded || print server
SEQ(SP=C-16%GCD=3000|6000|9000|C000|F000%ISR=AB-B5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=5B4%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=1B-25%TG=20%W=5B4%S=O%A=O%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=1B-25%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=1B-25%TG=20%CD=S)

# AirMagnet SmartEdge Sensor, SW Version: 8.0.0-11510
Fingerprint AirMagnet SmartEdge wireless sensor
Class AirMagnet | embedded || specialized
SEQ(SP=C3-CD%GCD=1-6%ISR=C9-D3%TI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=5A8%W2=5A8%W3=5A8%W4=5A8%W5=5A8%W6=5A8)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=5B4%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=5A8%S=O%A=S+%F=AS%O=M5B4ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# D-Link DI-624 wireless router rev. C, firmware 2.76 (24 Aug 2006)
# D-Link DI-524 WAP Firmware 1.21
# D-Link DI-604, firmware 3.52
# airnet awr014g
# D-Link Wbr-2310, Hardware Version: A1, Firmware Version: 1.01
# Trendnet TEW 432brp, H/W B2.1R
# TrendNet TEW-452BRP, Copyright (c) 1996-2001 Express Logic Inc. * ThreadX JADE/Green Hills Version G4.0.4.0
Fingerprint WAP: Airnet AWR014G; D-Link DI-524, DI-604, DI-624, or WBR-2310; or TRENDnet TEW-432BRP or TEW-452BRP (ThreadX)
Class Airnet | ThreadX || WAP
Class D-Link | ThreadX || WAP
Class TRENDnet | ThreadX || WAP
SEQ(SP=B-15%GCD=FA7F|1F4FE|2EF7D|3E9FC|4E47B|5DEFA%ISR=96-A0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B0%O2=M5B0%O3=M5B0%O4=M5B0%O5=M5B0%O6=M5B0)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=7F%TG=80%W=2000%O=M5B0%CC=N%Q=)
T1(R=Y%DF=N%T=7F%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7F%TG=80%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=7F%TG=80%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7F%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7F%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7F%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7F%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7F%TG=80%CD=S)

# AirSpan ProST WiMAX CPE (Outdoor Version)
Fingerprint AirSpan ProST WiMAX access point
Class AirSpan | embedded || WAP
SEQ(II=I)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3A-44%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3A-44%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3A-44%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3A-44%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3A-44%TG=40%CD=S)

# AKCP sensorProbe2, www.AKCP.com. Firmware SP2388, dated 090608
Fingerprint AKCP sensorProbe2 remote sensor device
Class AKCP | embedded || specialized
SEQ(SP=0-5%GCD=1388|2710|3A98|4E20|61A8%ISR=78-82%TI=I%II=I%SS=S%TS=U)
OPS(O1=M3F4%O2=M3F4%O3=M3F4%O4=M3F4%O5=M3F4%O6=M3F4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=2000%O=M3F4%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=2000%S=A%A=S+%F=AS%O=M3F4%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=7B-85%TG=80%W=2000%S=A%A=S%F=AR%O=M3F4%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=2000%S=A%A=S%F=AR%O=M3F4%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=2000%S=A%A=S+%F=AR%O=M3F4%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=7B-85%TG=80%CD=Z)

# Alcatel Speedtouch 510 ADSL router
Fingerprint Alcatel SpeedTouch 510 DSL modem
Class Alcatel | embedded || broadband router
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=1)
OPS(O1=M200NW0NNT11%O2=M200NW0NNT11%O3=M200NW0NNT11%O4=M200NW0NNT11%O5=M200NW0NNT11%O6=M200NNT11)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M200NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=391F%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Alcatel SpeedTouch Pro ADSL Modem (Firmware: Khdsaa3.270  (1003194))
Fingerprint Alcatel SpeedTouch Pro ADSL Modem
Class Alcatel | embedded || broadband router
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=96-A0%TI=I%II=I%SS=S%TS=1)
OPS(O1=M200NW0NNT11%O2=M200NW0NNT11%O3=M200NW0NNT11%O4=M200NW0NNT11%O5=M200NW0NNT11%O6=M200NNT11)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M200NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Alcatel PBX 4400 running (Chorus MiX V.3.2 r4.1.5 COMP-386)
Fingerprint Alcatel 4400 PBX (Chorus MiX V.3.2 r4.1.5 COMP-386)
Class Alcatel | embedded || PBX
SEQ(SP=94-9E%GCD=1-6%ISR=95-9F%TI=I|RD%II=I%SS=S%TS=U)
OPS(O1=|M5B4%O2=|M5B4%O3=|M5B4%O4=|M5B4%O5=|M5B4%O6=|M5B4)
WIN(W1=111C%W2=1068%W3=1180%W4=1000%W5=10C0%W6=1090)
ECN(R=Y%DF=Y%T=41%TG=40%W=111C%O=|M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=41%TG=40%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=41%TG=40%W=1090%S=O%A=O|S+%F=A|AS%O=|M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=41%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Enterasys Vertical Horizon VH-2402S2
# Alcatel OmniStack 6024 switch
# Dell Laser MFP 1815dn
Fingerprint Alcatel OmniStack 6024 or Enterasys Vertical Horizon VH-2402S2 switch, or Dell 1815dn printer
Class Alcatel | embedded || switch
Class Enterasys | embedded || switch
Class Dell | embedded || printer
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Alcatel 4035 IP Phone
Fingerprint Alcatel 4035 VoIP phone
Class Alcatel | embedded || VoIP phone
SEQ(SP=F4-106%GCD=1-6%ISR=FE-108%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B0%O2=M5B0%O3=M5B0%O4=M5B0%O5=M5B0%O6=M5B0)
WIN(W1=3E80%W2=3E80%W3=3E80%W4=3E80%W5=3E80%W6=3E80)
ECN(R=Y%DF=N%T=19-23%TG=20%W=3E80%O=M5B0%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=ARF%O=%RD=0%Q=)
T3(R=Y%DF=N%T=19-23%TG=20%W=3E80%S=O%A=S+%F=AS%O=M5B0%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=RF%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=ARF%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=RF%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=ARF%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=19-23%TG=20%CD=S)

# Alcatel OmniPCX A4400, Chorus pbx1 MiX V.3.2 r4.1.5 COMP-386
Fingerprint Alcatel-Lucent OmniPCX Enterprise A4400 PBX
Class Alcatel-Lucent | embedded || PBX
SEQ(SP=92-9C%GCD=1-6%ISR=96-A6%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=111C%W2=1068%W3=1180%W4=1000%W5=10C0%W6=1090)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1090%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Alcatel-Lucent OmniPCX Enterprise
# OmniPCX Enterprise R8.0.1-g1.503-12-a-nl-c80s1 (Linux 2.4.17-ll-dhs3)
Fingerprint Alcatel-Lucent OmniPCX Enterprise PBX (Linux 2.4.17)
Class Alcatel-Lucent | Linux | 2.4.17 | PBX
SEQ(SP=C5-D3%GCD=1-6%ISR=CC-D6%TI=Z%II=I%TS=U)
OPS(O1=M5B4NNSNW0%O2=M5B4NNSNW0%O3=M5B4NW0%O4=M5B4NNSNW0%O5=M5B4NNSNW0%O6=M5B4NNS)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%S=O%A=S+%F=AS%O=M5B4NNSNW0%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Sirio by Alice, voip telephone used by Telecom Italia
Fingerprint Sirio by Alice VoIP phone
Class Alice | embedded || VoIP phone
SEQ(SP=C3-CD%GCD=1-6%ISR=CB-D5%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4ST11NW1%O2=M5B4ST11NW1%O3=M5B4NNT11NW1%O4=M5B4ST11NW1%O5=M5B4ST11NW1%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW1%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW1%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Allen-Bradley 1756-ENBT card in ControlLogix 5000-series PLC
Fingerprint Allen-Bradley 1756 ControlLogix programmable automation controller
Class Allen-Bradley | embedded || specialized
SEQ(SP=15-1F%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=9B-A5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Belkin F5D7632-4 v1000UK, firmware AR.0.01.08UK (Oct 27 2004 01:03:29)
# Intracom Jetspeed 500i ADSL router
# Iskratel Proteus 932 VDSL Modem, Firmware version: 1.66.31
# Allied Data Technologies CopperJet 816-2P Router VoATM, Software Version: 6.02 SR4
# Iskratel Sinope568+
Fingerprint Broadband router (Allied Data CopperJet 816-2P, Belkin F5D7632-4, Intracom Jetspeed 500i, or Iskratel Sinope568 or Proteus932)
Class Allied Data | embedded || broadband router
Class Belkin | embedded || WAP
Class Intracom | embedded || broadband router
Class Iskratel | embedded || broadband router
SEQ(SP=6F-87%GCD=1-6%ISR=71-8D%TI=I%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=4000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=7B-85%TG=80%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=Z%F=R%O=%RD=0%Q=)
U1(DF=N%T=96-A0%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# AlliedWare OS version 54291-05
Fingerprint Allied Telesis AlliedWare version 54291-05
Class Allied Telesis | AlliedWare || router
SEQ(SP=F7-107%GCD=1-6%ISR=F9-115%TI=I%II=RI%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M280%O4=M400%O5=M218%O6=M109)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=400%O=M400%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=400%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=Z)

# Linksys Switch SRW2048 (Firmware 1.2.1)
# Linksys SRW2024 24-port 10/100/1000 Gigabit Switch, Hardware Version: 00.03.11, Boot Version:  1.0.1, Firmware Version:  1.2.1
# Linksys SRW-224G4-EU
# Allied Telesyn Switch 8000S 48Ports
# Dell PowerConnect 3448
# Dell Blade chassis switch module: Powerconnect 5316M
# PowerConnect 5324, Software Version 2.0.0.40, Boot Version 1.0.2.02
# TP-LINK TL-SL3428 switch
# DELL POWECONNECT 2824 Switch
Fingerprint Allied Telesis AT-8000S; Dell PowerConnect 2824, 3448, 5316M, or 5324; Linksys SFE2000P, SRW2024, SRW2048, or SRW224G4; or TP-Link TL-SL3428 switch
Class Allied Telesis | embedded || switch
Class Dell | embedded || switch
Class Linksys | embedded || switch
Class TP-Link | embedded || switch
SEQ(SP=F4-10A%GCD=1-6%ISR=FA-10E%TI=RD%CI=RD%II=RI%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=200%W2=200%W3=200%W4=200%W5=200%W6=200)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=200%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=200%S=O%A=S+%F=AS%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Allied Telesis AT-9000/24 Gigabit Ethernet Switch, Runtime Image: Version 1.1.0.28
# AT-FS750/16 Fast Ethernet WebSmart Switch,  Version AT-S80 V2.3.1 [1.1.1.92], Boot Loader: Version 1.00.07
Fingerprint Allied Telesis AT-9000/24 or AT-FS750/16 switch
Class Allied Telesis | embedded || switch
SEQ(SP=0-5%GCD=0%ISR=0-5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0|B90|7271|B11B%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Allied Telesis AT-9000/24, Software Release AT-S84 1.1.1
Fingerprint Allied Telesis AT-9000/24 switch
Class Allied Telesis | embedded || switch
SEQ(SP=0-5%GCD=0%ISR=0-5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2000%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=0|2000%S=A|O%A=O|S+%F=AS|APR%O=|M218%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0|4212|8433|AE74%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Allied Telesyn CentreCOM AR300L v1 Access Router
Fingerprint Allied Telesyn AT-AR300L CentreCOM router
Class Allied Telesyn | AlliedWare || router
SEQ(SP=EF-113%GCD=1-6%ISR=F2-11C%TI=I%II=RI%SS=S%TS=U)
OPS(O1=M3EC%O2=M3EC%O3=M3EC%O4=M3EC%O5=M3EC%O6=M3EC)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=400%O=M3EC%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=400%S=O%A=O|S+%F=A|AS%O=|M3EC%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=Z)

# AT-AR410 router
Fingerprint Allied Telesyn AT-AR410 router
Class Allied Telesyn | AlliedWare || router
SEQ(SP=F3-107%GCD=1-6%ISR=F8-114%TI=I|RD%II=RI%SS=O%TS=U)
OPS(O1=M109%O2=M109%O3=M109%O4=M109%O5=M109%O6=M109)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=400%O=|M109%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0|400%S=O|Z%A=O|S+%F=AR|AS%O=|M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=Z)

# Allied Telesyn AT-AR750s
Fingerprint Allied Telesyn AT-AR750s router
Class Allied Telesyn | AlliedWare || router
SEQ(SP=FA-106%GCD=1-6%ISR=101-10D%TI=I%II=RI%SS=O%TS=U)
OPS(O1=M400%O2=M400%O3=M280%O4=M400%O5=M218%O6=M109)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=400%O=M400%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=400%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=Z)

# Allied Telesyn 8326GB switch
Fingerprint Allied Telesyn 8326GB switch
Class Allied Telesyn | embedded || switch
SEQ(SP=0-5%GCD=1-6%ISR=0-5%TI=I%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A|O%A=O|S%F=APR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A|O%A=O|S+%F=APR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A|O%A=O|S%F=APR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A|O%A=O|S%F=APR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=106B|119F|1AFE|568B|FCB7%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# AlliedTelesyn AT-8326GB Switch. It has embedded "AT-S41 Switch OS" V 1.1.6 with boot loader 1.01L
# AT - 8326GB Fast Ethernet Switch
# Allied Telesyn AT-8326GB switch.
# AT-8350GB switch, management system version 1.1.8
Fingerprint Allied Telesyn AT-8326GB or AT8350GB switch.
Class Allied Telesyn | embedded || switch
SEQ(SP=0-5%GCD=0%ISR=0-5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Allied Telesyn AT-8350GB Management System Version 1.1.6
Fingerprint Allied Telesyn AT-8350GB switch
Class Allied Telesyn | embedded || switch
SEQ(SP=0-5%GCD=0%ISR=0-5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=237|1001|57D1|5A0E|E806%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Allied Telesyn AT-9006SX/SC Ethernet Switch, AT-S26 Ethernet Switch Software: Version 1.0.3 000517
Fingerprint Allied Telesyn AT-9006SX/SC switch
Class Allied Telesyn | embedded || switch
SEQ(SP=13-B5%GCD=FA|1F4|2EE|3E8|4E2%ISR=8A-B0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Allied Telesyn switch AT-9448Ts/XP (ATS63), firmware v2.1.0
Fingerprint Allied Telesyn AT-9448Ts/XP switch
Class Allied Telesyn | embedded || switch
SEQ(SP=F3-109%GCD=1-6%ISR=FE-114%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=3E80%W2=3E80%W3=3E80%W4=3E80%W5=3E80%W6=3E80)
ECN(R=Y%DF=N%T=7C-86%TG=80%W=3E80%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=7C-86%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=7C-86%TG=80%W=0%S=A%A=Z%F=RF%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7C-86%TG=80%W=0%S=Z%A=S+%F=ARF%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7C-86%TG=80%W=0%S=A%A=Z%F=RF%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=7C-86%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7C-86%TG=80%CD=S)

# D-Link Model:DES-3226L
# Allied Telesyn AT-GS950/8 switch.
Fingerprint Allied Telesyn AT-GS950 or D-Link DES-3226L switch
Class Allied Telesyn | embedded || switch
Class D-Link | embedded || switch
SEQ(SP=0-DA%GCD=1-6|80|100|180|200|280|C581|18B02|25083|31604|3DB85%ISR=93-A5%TI=I%II=RI%SS=O%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=2000%S=O%A=S+%F=AS%O=M5B4NW0NNT11NNLLLLLLLLLL%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=0|128%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=19-23%TG=20%CD=S)

# Allied Telesyn AT-GS950/24 Gigabit Ethernet Switch with Firmware Version 1.0.0.26
Fingerprint Allied Telesyn AT-GS950/24 Gigabit Ethernet Switch
Class Allied Telesyn | embedded || switch
SEQ(SP=0-5%GCD=1-6%ISR=0-5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=2C5E%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Allied Telesyn Rapier 24i
Fingerprint Allied Telesyn Rapier 24i switch
Class Allied Telesyn | embedded || switch
SEQ(SP=F9-103%GCD=1-6%ISR=FC-106%TI=I%CI=I%II=RI%SS=O%TS=U)
OPS(O1=M109%O2=M109%O3=M109%O4=M109%O5=M109%O6=M109)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=400%O=M109%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=400%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=Z)

# Allied Telesyn Rapier G6 Switch Version 2.7.3
Fingerprint Allied Telesyn Rapier G6 switch
Class Allied Telesyn | embedded || switch
SEQ(SP=FC-108%GCD=1-6%ISR=FD-10B%TI=I%II=RI%SS=S%TS=U)
OPS(O1=M109%O2=M109%O3=M109%O4=M109%O5=M109%O6=M109)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=400%O=M109%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=Z)

# Cisco MDS 9216i SAN Switch OS version 3.1(3)
# Webcam Allnet 2210
Fingerprint Allnet 2210 webcam or Cisco MDS 9216i switch
Class Allnet | embedded || webcam
Class Cisco | embedded || switch
SEQ(SP=B4-C9%GCD=1-6%ISR=BE-CC%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Allworx 9212 phone
Fingerprint Allworx 9212 VoIP phone
Class Allworx | embedded || VoIP phone
SEQ(SP=EC-FC%GCD=1-6%ISR=F4-100%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5BCNW0NNT11%O2=M5BCNW0NNT11%O3=M5BCNW0NNT11%O4=M5BCNW0NNT11%O5=M5BCNW0NNT11%O6=M5BCNNT11)
WIN(W1=4380%W2=4110%W3=423C%W4=4074%W5=4180%W6=403D)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4410%O=M5BCNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=403D%S=O%A=S+%F=AS%O=M5BCNW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Alvarion BreezeACCESS II  Association Unit Official Release Version - 4.5.17
Fingerprint Alvarion BreezeACCESS II broadband wireless access system 4.5.17
Class Alvarion | embedded || WAP
SEQ(SP=47-51%GCD=1-6%ISR=65-6F%TI=I%II=I%SS=O|S%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=5DC%W2=5DC%W3=5DC%W4=5DC%W5=5DC%W6=5DC)
ECN(R=N)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=5DC%S=O%A=O|S+%F=AS%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=6B33|AD02|D0C3%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Alvarion BreezeMax CPE Si E 2.3 WiMAX Access Point
Fingerprint Alvarion CPE-Si-E-2.3 BreezeMAX WiMAX WAP
Class Alvarion | embedded || WAP
SEQ(SP=96-A0%GCD=1-6%ISR=9B-A5%TI=I%TS=1)
OPS(O1=M5D8NW1NNT11%O2=M5D8NW1NNT11%O3=M5D8NW1NNT11%O4=M5D8NW1NNT11%O5=M5D8NW1NNT11%O6=M5D8NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5D8NW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=O%F=AS%O=M5D8NW1NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(R=N)

# AMBIT DOCSIS 2.0 Cable Modem :: Boot Code Version : 2.1.5 / Software Version : 5.11.1130 / Hardware version 4.7
# Xerox Phaser 6350DT Network Printer
# OS: 5.78; Engine 3.1.0;
Fingerprint Ambit DOCSIS 2.0 cable modem, or Xerox Phaser 6250N or 6350DT printer
Class Ambit | embedded || broadband router
Class Xerox | embedded || printer
SEQ(SP=E-52%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=98-C4%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# AmigaOS 3.1 and EASYNET 0.172 (2009) TCP/IP stack
# AmigaOS GENESiS/AmiTCP TCP/IP stack v45.7
Fingerprint AmigaOS 3.1
Class Amiga | AmigaOS | 3.X | general purpose
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=96-A0%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1C84%W2=1B58%W3=1E00%W4=2000%W5=1F68%W6=1F0E)
ECN(R=Y%DF=N%T=37-41%TG=40%W=1C84%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=37-41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=37-41%TG=40%W=1F0E%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=37-41%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=37-41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=37-41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=37-41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Amiga OS 3.9 BB2 68060 Mediator 1200
# BB2 is BoingBag 2, something like a service pack?
Fingerprint AmigaOS 3.9 BB2
Class Amiga | AmigaOS | 3.X | general purpose
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1C84%W2=1B58%W3=1E00%W4=2000%W5=1F68%W6=1F0E)
ECN(R=Y%DF=N%T=3C%TG=40%W=1C84%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Anue X/GEM controller version v3.3.1
Fingerprint Anue X/GEM ethernet network simulator
Class Anue | embedded || specialized
SEQ(SP=0-96%GCD=1-6%ISR=0-8D%TI=I%II=I%SS=O|S%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=3C%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=R%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=0%S=O%A=S+%F=AS%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=R%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3C%TG=40%CD=S)

# APC Metered Rack PDU AP7851 running aos_270
Fingerprint APC AP7851 power distribution unit (AOS 2.7.0)
Class APC | AOS | 2.X | power-device
SEQ(SP=8-1D%GCD=1E848|3D090|5B8D8|7A120|98968%ISR=9C-A6%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=10F8%W2=1044%W3=112C%W4=10F8%W5=1060%W6=10CD)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=111C%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=10CD%S=O%A=S+%F=AS%O=M109NW0NNSNNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Model Number: AP7920, Type: APC OS, Version: 270, Hardware Revision: B2, Date: 10/12/2005
Fingerprint APC AP7920 rack PDU (AOS 2.7.0)
Class APC | AOS | 2.X | power-device
SEQ(SP=C-16%GCD=1E848|3D090|5B8D8|7A120|98968%ISR=9F-A9%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=111C%W2=1068%W3=1180%W4=111C%W5=10C0%W6=1090)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Model Number:   AP9606, AOS v2.5.4, aos254.bin
# APC PN: AP9606, Web/SNMP Management Card AOS   v3.2.6.b, Smart-UPS & Matrix-UPS APP v3.2.6.a
Fingerprint APC AP9606 Network Management Card (AOS 2.5.4 - 3.2.6)
Class APC | AOS | 2.X | power-device
SEQ(SP=E2-EC%GCD=1-6%ISR=DE-E8%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=640%W2=640%W3=640%W4=640%W5=640%W6=640)
ECN(R=Y%DF=N%T=78%TG=80%W=640%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=78%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=78%TG=80|FF%W=640%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=78%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=78%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=78%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=78%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=78%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=AB52|D22B%RUD=G)
IE(DFI=N%T=78%TG=80%CD=Z)

# APC Environmental Manager model APC9340 v3.5.6, with embedded Network Management Card AOS v3.5.7
Fingerprint APC 9340 Network Management Card (AOS 3.5.7)
Class APC | AOS | 3.X | power-device
SEQ(SP=DE-E8%GCD=1-6%ISR=E6-F0%TI=RI%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=|M109NNSNNT11)
WIN(W1=10F8%W2=1044%W3=112C%W4=10F8%W5=1060%W6=0|10CD)
ECN(R=Y%DF=N%T=41%TG=40%W=0|111C%O=|M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# APC AP79xx metered rack power distribution unit (AOS 3.x)
# AOS v3.6.1
Fingerprint APC AP7900-series power distribution unit (AOS 3.x)
Class APC | AOS | 3.X | power-device
SEQ(SP=E9-FB%GCD=1-6%ISR=E6-F2%TI=RI%CI=RI%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=10F8%W2=1044%W3=112C%W4=10F8%W5=1060%W6=10CD)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=111C%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# APC PDU - AP7930, Version: v3.3.4
Fingerprint APC AP7930 power distribution unit (AOS 3.3.4)
Class APC | AOS | 3.X | power-device
SEQ(SP=73-B7%GCD=1-6%ISR=DE-E8%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=10F8%W2=1044%W3=112C%W4=10F8%W5=1060%W6=10CD)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=111C%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# American Power Conversion Network Management Card AOS v3.3.1
# APC PN: AP9619, Network Management Card AOS v3.6.1, Smart-UPS & Matrix-UPS APP v3.5.8
# APC UPS Network Management Card, AOS v 3.3.4
# APC UPS Network Management Card, AOS v3.5.5
# Rack PDU AP7920 v3.5.8, AOS v3.5.9
Fingerprint APC AP9619 Network Management Card (AOS 3.3.1 - 3.6.1)
Class APC | AOS | 3.X | power-device
SEQ(SP=DE-104%GCD=1-6%ISR=E3-FE%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=10F8%W2=1044%W3=112C%W4=10F8%W5=1060%W6=10CD)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=111C%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# APC Network Management Card AOS v3.5.5 
# APC aos v3.3.4, Date: 01/05/2007
Fingerprint APC Network Management Card (AOS 3.3.4 - 3.3.5)
Class APC | AOS | 3.X | power-device
SEQ(SP=F4-104%GCD=1-6%ISR=EF-FD%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=10F8%W2=1044%W3=112C%W4=10F8%W5=1060%W6=10CD)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=111C%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Network Management Card AOS v3.5.7, Rack PDU APP v3.5.6
Fingerprint APC Network Management Card (AOS 3.5.7)
Class APC | AOS | 3.X | power-device
SEQ(SP=5E-B8%GCD=1-6%ISR=DD-E7%TI=RI%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=10F8%W2=1044%W3=112C%W4=10F8%W5=1060%W6=10CD)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=111C%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# APC AOS Version 5.1.1
Fingerprint APC AOS 5.1.1
Class APC | AOS || power-device
SEQ(R=N)
OPS(O1=M5B4NNSNNT11%O2=M578NNSNNT11%O3=M280NNT11%O4=M5B4NNSNNT11%O5=M218NNSNNT11%O6=M109NNSNNT11)
WIN(W1=10F8%W2=1044%W3=112C%W4=10F8%W5=1060%W6=10CD)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=111C%O=M5B4NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# aos303.bin APC Masterswitch
Fingerprint APC MasterSwitch power distribution unit (AOS 3.0.3)
Class APC | AOS || power-device
SEQ(SP=CA-D4%GCD=1-6%ISR=D5-DF%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=640%W2=640%W3=640%W4=640%W5=640%W6=640)
ECN(R=Y%DF=N%T=70%TG=80%W=640%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=70%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=70%TG=80%W=640%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=70%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=70%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=70%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=70%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=70%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=96A9%RUD=G)
IE(DFI=N%T=70%TG=80%CD=Z)

# APC NetBotz 200 Rack Monitor (NBRK0200)
Fingerprint APC NetBotz 200 rack monitor
Class APC | embedded || power-device
SEQ(SP=5F-A9%GCD=1-6%ISR=DD-E7%CI=RD|RI%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=10F8%W2=1044%W3=112C%W4=10F8%W5=1060%W6=10CD)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=111C%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# APC Smart-UPS 3000 RM, APC AOS ftpd  2.6.4  on APC AP9617 network management card
Fingerprint APC Smart-UPS 3000 RM UPS
Class APC | embedded || power-device
SEQ(CI=I%II=I)
OPS(O1=M5B4NW0NNSNNT11%O2=%O3=%O4=%O5=%O6=)
WIN(W1=10F8%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# APC Smart-UPS RT 8000 RM XL 8kVA With Link3 network management card.
Fingerprint APC Smart-UPS RT 8000 RM XL UPS
Class APC | embedded || power-device
SEQ(SP=EE-F8%GCD=1-6%ISR=EE-F8%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=10F8%W2=1044%W3=112C%W4=10F8%W5=1060%W6=10CD)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=111C%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# APC Environmental Monitoring Unit, model AP9319
# APC Smart-UPS 1000 RM, Firmware 157.4.I, Network Management Card
# APC Environmental Monitoring Unit
Fingerprint APC AP9319 Environmental Monitoring Unit or Smart-UPS 1000 RM UPS
Class APC | embedded || specialized
Class APC | embedded || power-device
SEQ(SP=C-16%GCD=1E848|3D090|5B8D8|7A120|98968%ISR=9F-A9%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=|M5B4NW0NNSNNT11%O5=|M218NW0NNSNNT11%O6=|M109NNSNNT11)
WIN(W1=10F8%W2=1044%W3=112C%W4=0|10F8%W5=0|1060%W6=0|10CD)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=111C%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=10CD%S=O%A=S+%F=AS%O=M109NW0NNSNNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# A/UX 3.0.2 SVR2 mc68030
# A/UX 3.1.1 SVR2 mc68040
# Apple's A/UX 3.0.1, PING okay, ftp/telnet/uucp: no answer
Fingerprint Apple A/UX 3.0.1 - 3.1.1 SVR2
Class Apple | A/UX | 3.X | general purpose
SEQ(SP=0-15%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=96-A0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=1000%W2=1000%W3=F00%W4=1000%W5=EA8%W6=F87)
ECN(R=Y%DF=N%T=19-23%TG=20%W=1000%O=M400%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=F87%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Apple A/UX 3.1.1 SVR2 mc68040
Fingerprint Apple A/UX 3.1.1 SVR2
Class Apple | A/UX | 3.X | general purpose
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=1000%W2=1000%W3=F00%W4=1000%W5=EA8%W6=F87)
ECN(R=Y%DF=N%T=19-23%TG=20%W=1000%O=M400%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Apple Airport Extreme Dual Band firmware version 7.4.2 (Probably NetBSD --Ed.)
Fingerprint Apple Airport Extreme WAP
Class Apple | embedded || general purpose
SEQ(SP=CD-DB%GCD=1-6%ISR=D9-E3%TI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT01SNN%O2=M5B4NW0NNT01SNN%O3=M5B4NW0NNT01%O4=M5B4NW0NNT01SNN%O5=M5B4NW0NNT01SNN%O6=M5B4NNT01SNN)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M5B4NW0SNN%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Apple Time Capsule, firmware 7.3.1
# Apple Airport Extreme
# Linux 2.6.25.18-0.2-default #1 SMP 2008-10-21 16:30:26 +0200 x86_64 x86_64 x86_64 GNU/Linux
Fingerprint Apple AirPort Extreme WAP or Time Capsule NAS device (NetBSD)
Class Apple | embedded || storage-misc
Class Apple | embedded || WAP
SEQ(SP=CC-D8%GCD=1-6%ISR=D7-E1%TI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT01SNN%O2=M5B4NW0NNT01SNN%O3=M5B4NW0NNT01%O4=M5B4NW0NNT01SNN%O5=M5B4NW0NNT01SNN%O6=M5B4NNT01SNN)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M5B4NW0SNN%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=8000%S=O%A=S+%F=AS%O=M5B4NW0NNT01SNN%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Apple TimeCapsule 500Gb.
Fingerprint Apple Time Capsule NAS device
Class Apple | embedded || storage-misc
SEQ(CI=I%II=I)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=N)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Airport Express with firmware 6.3.
Fingerprint Apple AirPort Express WAP
Class Apple | embedded || WAP
SEQ(SP=CD-DB%GCD=1-6%ISR=D8-E2%TI=I%CI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW1NNT01SNN%O2=M5B4NW1NNT01SNN%O3=M5B4NW1NNT01%O4=M5B4NW1NNT01SNN%O5=M5B4NW1NNT01SNN%O6=M5B4NNT01SNN)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SNN%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT01SNN%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Apple Airport Express (with Airtunes), using firmware version 6.3.
Fingerprint Apple AirPort Express WAP v6.3
Class Apple | embedded || WAP
SEQ(SP=FC-106%GCD=1-6%ISR=105-10F%TI=I%II=I%SS=S%TS=6)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# AirPort Extreme (802.11n)
Fingerprint Apple AirPort Extreme WAP
Class Apple | embedded || WAP
SEQ(SP=CE-D8%GCD=1-6%ISR=D7-E1%TI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT01SNN%O2=M5B4NW0NNT01SNN%O3=M5B4NW0NNT01%O4=M5B4NW0NNT01SNN%O5=M5B4NW0NNT01SNN%O6=M5B4NNT01SNN)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M5B4NW0SNN%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Apple Airport Extreme (Simultaneous Dual-Band II) router running version 7.5.1 (75100.14) of the operating system.
Fingerprint Apple AirPort Extreme WAP
Class Apple | embedded || WAP
SEQ(SP=EF-F9%GCD=1-6%ISR=FA-104%TI=RD%CI=I%II=I%TS=3|6)
OPS(O1=M5B4NW3NNT11SLL%O2=M5B4NW3NNT11SLL%O3=M5B4NW3NNT11%O4=M5B4NW3NNT11SLL%O5=M5B4NW3NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Apple Airport Extreme Base station, Firmware 7.3.2
Fingerprint Apple AirPort Extreme WAP v7.3.2
Class Apple | embedded || WAP
SEQ(SP=D7-E1%GCD=1-6%ISR=D7-E1%TI=I%TS=0)
OPS(R=N)
WIN(R=N)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M5B4NW0SNN%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=6C21|A22F|B234|B840|C32A%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Darwin 9.0.0b5 Darwin Kernel Version 9.0.0b5: Fri Aug 17 17:24:24 PDT 2007; root:xnu-1182~1/RELEASE_I386 i386
# Darwin 9.0.0 Darwin Kernel Version 9.0.0: Tue Oct  9 21:35:55 PDT 2007; root:xnu-1228~1/RELEASE_I386 i386
# Darwin 9.1.0 Darwin Kernel Version 9.1.0: Wed Oct 31 17:48:21 PDT 2007; root:xnu-1228.0.2~1/RELEASE_PPC Power Macintosh
# Darwin 9.1.0 Darwin Kernel Version 9.1.0: Wed Oct 31 17:46:22 PDT 2007; root:xnu-1228.0.2~1/RELEASE_I386 i386
# Darwin 9.0.0 Darwin Kernel Version 9.0.0: Tue Oct  9 21:37:58 PDT 2007; root:xnu-1228~1/RELEASE_PPC Power Macintosh
# Darwin Kernel Version 9.2.0:  Tue Feb 5 16:13:22 PST 2008; root:xnu-1228.3.13~1/RELEASE_I386 i386, Mac OS X Version 10.5.2 (LEOPARD)
# Darwin 9.2.2 Darwin Kernel Version 9.2.2: Tue Mar 4 21:17:34 PST 2008; root:xnu-1228..31~1/RELEASE_I386 i386
# Darwin 9.3.0 Darwin Kernel Version 9.3.0: Fri May 23 00:49:16 PDT 2008; root:xnu-1228.5.18~1/RELEASE_I386 i386
# Darwin 9.4.0 Darwin Kernel Version 9.4.0: Mon Jun  9 19:36:17 PDT 2008; root:xnu-1228.5.20~1/RELEASE_PPC Power Macintosh
# Darwin 9.5.0 Darwin Kernel Version 9.5.0: Wed Sep  3 11:29:43 PDT 2008; root:xnu-1228.7.58~1/RELEASE_I386 i386
# Darwin 9.6.0 Darwin Kernel Version 9.6.0: Mon Nov 24 17:39:01 PST 2008; root:xnu-1228.9.59~1/RELEASE_PPC Power Macintosh
# Darwin 9.7.1 Darwin Kernel Version 9.7.1: Thu Apr 23 13:52:18 PDT 2009; root:xnu-1228.14.1~1/RELEASE_I386 i386
# Darwin 9.8.0 Darwin Kernel Version 9.8.0: Wed Jul 15 16:57:01 PDT 2009; root:xnu-1228.15.4~1/RELEASE_PPC Power Macintosh powerpc
# Darwin 10.0.0 Darwin Kernel Version 10.0.0: Fri Jul 31 22:47:34 PDT 2009; root:xnu-1456.1.25~1/RELEASE_I386 i386
# Darwin 10.2.0 Darwin Kernel Version 10.2.0: Tue Nov  3 10:37:10 PST 2009; root:xnu-1486.2.11~1/RELEASE_I386 i386
# jailbroken iphone ios4
# iPhone OS 4.02 (8A400 )
# Apple iPhone 3GS phone running Apple iOS 4.0.1 (8A306),
# Apple iPhone 4 16GB running Apple iOS 4.1 public release
Fingerprint Apple Mac OS X 10.5 - 10.6.3 (Leopard - Snow Leopard) or iOS 4.0 - 4.1 (Darwin 9.0.0b5 - 10.2.0)
Class Apple | iOS | 4.X | general purpose
Class Apple | Mac OS X | 10.6.X | general purpose
Class Apple | Mac OS X | 10.6.X | general purpose
SEQ(SP=EA-10C%GCD=1-6%ISR=F8-10E%TI=RD%CI=RD|RI%II=RI%TS=3|4)
OPS(O1=M5B4NW1NNT11SLL|M5B4NW2NNT11SLL|M5B4NW3NNT11SLL%O2=M5B4NW1NNT11SLL|M5B4NW2NNT11SLL|M5B4NW3NNT11SLL%O3=M5B4NW1NNT11|M5B4NW2NNT11|M5B4NW3NNT11%O4=M5B4NW1NNT11SLL|M5B4NW2NNT11SLL|M5B4NW3NNT11SLL%O5=M5B4NW1NNT11SLL|M5B4NW2NNT11SLL|M5B4NW3NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL|M5B4NW2SLL|M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# iOS 4
Fingerprint Apple iOS 4.0
Class Apple | iOS | 4.X | phone
SEQ(SP=F1-107%GCD=1-6%ISR=102-10E%TI=RD%CI=RD%II=RI%TS=3)
OPS(O1=M56ANW2NNT11SLL%O2=M56ANW2NNT11SLL%O3=M56ANW2NNT11%O4=M56ANW2NNT11SLL%O5=M56ANW2NNT11SLL%O6=M56ANNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M56ANW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# iPhone OS Version 4.1
Fingerprint Apple iOS 4.1
Class Apple | iOS | 4.X | phone
SEQ(SP=EC-106%GCD=1-6%ISR=FC-108%TI=RD%II=RI%TS=4)
OPS(O1=M5B4NW2NNT11SLL%O2=M5B4NW2NNT11SLL%O3=M5B4NW2NNT11%O4=M5B4NW2NNT11SLL%O5=M5B4NW2NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# 4.0 (8A293) on iPhone 3G
# Ipad
Fingerprint Apple iPad tablet computer or iPhone mobile phone (iOS 4.0)
Class Apple | iOS | 4.X | phone
SEQ(SP=F1-103%GCD=1-6%ISR=FA-108%TI=RD%CI=RD|RI%II=RI%TS=5)
OPS(O1=M5B4NW2NNT11SLL%O2=M5B4NW2NNT11SLL%O3=M5B4NW2NNT11%O4=M5B4NW2NNT11SLL%O5=M5B4NW2NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# iPhone 4, iOS version 4.1(8B117)
Fingerprint Apple iPhone 4 mobile phone (iOS 4.1)
Class Apple | iOS | 4.X | phone
SEQ(SP=FD-107%GCD=1-6%ISR=102-10C%TI=RD%CI=RD|RI%II=RI%TS=3)
OPS(O1=M5B4NW2NNT11SLL%O2=M5B4NW2NNT11SLL%O3=M5B4NW2NNT11%O4=M5B4NW2NNT11SLL%O5=M5B4NW2NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 9.0.0d1 Darwin Kernel Version 9.0.0d1: Wed Oct 10 00:07:50 PDT 2007; root:xnu-933.0.0.204.obj~7/RELEASE_ARM_S5L8900XRB iPod1,1 Darwin, ipod touch 1.1.2 (jailbroken)
# Darwin 9.0.0d1 Darwin Kernel Version 9.0.0d1: Wed Dec 12 00:16:00 PST 2007; root:xnu-933.0.0.211.obj~2/RELEASE_ARM_S5L8900XRB iPod1,1 arm N45AP Darwin, ziphone 2.6b jailbroken ipod touch (1.1.4)
Fingerprint Apple iPod touch audio player (iPhone OS 1.1.2 - 1.1.4, Darwin 9.0.0d1)
Class Apple | iPhone OS | 1.X | media device
SEQ(SP=0-5%GCD=1-6%ISR=15-1F%TI=I%TS=1)
OPS(O1=M5B4NW0NNT11SLL%O2=M5B4NW0NNT11SLL%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11SLL%O5=M5B4NW0NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Ipod Touch 16Gb. With 1.1.3 upgrade,BSD Subsystem, Openssh, and some other utils. Darwin 9.0.0d1 Darwin Kernel Version 9.0.0d1: Wed Oct 10 00:07:50 PDT 2007; root:xnu-933.0.0.204.obj~7/RELEASE_ARM_S5L8900XRB iPod1,1 unknown
Fingerprint Apple iPod touch audio player (iPhone OS 1.1.3, Darwin 9.0.0d1)
Class Apple | iPhone OS | 1.X | media device
SEQ(SP=0-5%GCD=1-6%ISR=15-1F%TS=1)
OPS(O1=M3FD8NW0NNT11SLL%O2=M3FD8NW0NNT11SLL%O3=M3FD8NW0NNT11%O4=M3FD8NW0NNT11SLL%O5=M3FD8NW0NNT11SLL%O6=M3FD8NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N|Y%T=3B-45%TG=40%W=0|FFFF%O=|M3FD8NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# iPod touch Firmware 1.1.3, jailbroken, ssh installed
Fingerprint Apple iPod touch audio player (iPhone OS 1.1.3, Darwin 9.0.0d1)
Class Apple | iPhone OS | 1.X | media device
SEQ(SP=0-5%GCD=1-6%ISR=16-20%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11SLL%O2=M5B4NW0NNT11SLL%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11SLL%O5=M5B4NW0NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# iPhone, O/S version 2.1 (5F136)
# iPhone Modem Firmware 02.11.07, Version 2.1 (5F136)
Fingerprint Apple iPhone mobile phone (iPhone OS 2.1)
Class Apple | iPhone OS | 1.X | phone
SEQ(SP=FB-107%GCD=1-6%ISR=FD-10B%TI=I%TS=3)
OPS(O1=M5B4NW2NNT11SLL%O2=M5B4NW2NNT11SLL%O3=M5B4NW2NNT11%O4=M5B4NW2NNT11SLL%O5=M5B4NW2NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin iPhone 9.0.0d1 Darwin Kernel Version 9.0.0d1: Fri Jun 22 00:38:56 PDT 2007; root:xnu-933.0.1.178.obj~1/RELEASE_ARM_S5L8900XRB iPhone1,1 Darwin
# This is the fingerprint of an iPhone as of 2007-08-14 (all updates applied)
# Apple iPhone running kernel: "Darwin Kernel Version 9.0.0d1" and DropBear SSH daemon
# Apple iPhone, 8GB model, firmware version 1.0.2, WiFi connection
# iPhone Firmware 1.1.1
# Jailbroken iPod touch running firmware 1.1.1
# Darwin 9.0.0d1 Darwin Kernel Version 9.0.0d1: Thu Sep 20 00:27:53 PDT 2007; root:xnu-933.0.0.203.obj~24/RELEASE_ARM_S5L8900XRBiPod1,1 Darwin
# Darwin iPod 9.0.0d1 Darwin Kernel Version 9.0.0d1: Wed Oct 10 00:07:50 PDT 2007; root:xnu-933.0.0.204.obj~7/RELEASE_ARM_S5L8900XRB iPod1,1 Darwin, iPod Touche firmware 1.1.2 jailbroken (obviously)
# iPod Touch firmware 1.1.3 (jailbreaked)
Fingerprint Apple iPhone mobile phone or iPod touch audio player (iPhone OS 1.0.2 - 1.1.3, Darwin 9.0.0d1)
Class Apple | iPhone OS | 1.X | phone
Class Apple | iPhone OS | 1.X | media device
SEQ(SP=0-5%GCD=1-6%ISR=15-1F%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11SLL%O2=M5B4NW0NNT11SLL%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11SLL%O5=M5B4NW0NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# iPhone 3g, running firmware 2.1
# iPhone 3G, Firmware version 2.2
# Darwin Kernel Version 9.4.1: Mon Dec  8 20:59:30 PST 2008; root:xnu-1228.7.37~4/RELEASE_ARM_S5L8900X iPhone1,2 arm N82AP Darwin
Fingerprint Apple iPhone mobile phone (iPhone OS 2.1 - 2.2, Darwin 9.4.1)
Class Apple | iPhone OS | 2.X | media device
SEQ(SP=F2-108%GCD=1-6%ISR=F6-10A%TI=I%II=I%SS=S%TS=3)
OPS(O1=M3FD8NW2NNT11SLL%O2=M3FD8NW2NNT11SLL%O3=M3FD8NW2NNT11%O4=M3FD8NW2NNT11SLL%O5=M3FD8NW2NNT11SLL%O6=M3FD8NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Apple iPod Touch Firmware 2.1
Fingerprint Apple iPod touch audio player (iPhone OS 2.1)
Class Apple | iPhone OS | 2.X | media device
SEQ(SP=0-5%GCD=1-6%ISR=15-1F%TI=I%II=I%SS=S%TS=3)
OPS(O1=M5B4NW2NNT11SLL%O2=M5B4NW2NNT11SLL%O3=M5B4NW2NNT11%O4=M5B4NW2NNT11SLL%O5=M5B4NW2NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=41%TG=40%W=FFFF%O=M5B4NW2SLL%CC=N%Q=)
T1(R=Y%DF=N%T=41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=41%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=41%TG=40%CD=S)

# Apple iTouch First Gen, Model Number: MA623LL , running firmware version 2.1 (5F137)
Fingerprint Apple iPod touch audio player (iPhone OS 2.1)
Class Apple | iPhone OS | 2.X | media device
SEQ(SP=F4-FE%GCD=1-6%ISR=EE-F8%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=4988%W2=467C%W3=44B0%W4=4988%W5=4598%W6=4431)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4470%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# iPod touch 2nd generation, (Firmware) Version: 2.2 (5G77a), Model: MB528BT
Fingerprint Apple iPod touch audio player (iPhone OS 2.2)
Class Apple | iPhone OS | 2.X | media device
SEQ(R=N)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=Z%A=S+%F=AR%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# iPhone model MB500X firmware version 2.0.2 (5C1)
Fingerprint Apple iPhone mobile phone (iPhone OS 2.0.2)
Class Apple | iPhone OS | 2.X | phone
SEQ(SP=0-5%GCD=1-6%ISR=16-20%TI=I%II=I%SS=S%TS=3)
OPS(O1=M4D8NW2NNT11SLL%O2=M4D8NW2NNT11SLL%O3=M4D8NW2NNT11%O4=M4D8NW2NNT11SLL%O5=M4D8NW2NNT11SLL%O6=M4D8NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M4D8NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# UK iPhone 1st gen (EDGE/non 3G) OS Ver 2.1 (5F136), Model MB213B, Carrier O2 2.6
# iPhone 3G
# iPhone no-3G, firmware 2.1 jailbroken & unlocked via QuickPwn.
Fingerprint Apple iPhone mobile phone (iPhone OS 2.1)
Class Apple | iPhone OS | 2.X | phone
SEQ(SP=F0-109%GCD=1-6%ISR=100-10E%TI=I%II=I%SS=S%TS=4)
OPS(O1=M5B4NW2NNT11SLL%O2=M5B4NW2NNT11SLL%O3=M5B4NW2NNT11%O4=M5B4NW2NNT11SLL%O5=M5B4NW2NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# iPhone OS version 2.2
Fingerprint Apple iPhone mobile phone (iPhone OS 2.2)
Class Apple | iPhone OS | 2.X | phone
SEQ(SP=FA-108%GCD=1-6%ISR=100-10A%TI=I%II=I%SS=S%TS=2)
OPS(O1=M5B4NW2NNT11SLL%O2=M5B4NW2NNT11SLL%O3=M5B4NW2NNT11%O4=M5B4NW2NNT11SLL%O5=M5B4NW2NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# iPhone 8 Gig, Version 2.2.1 (5H11), Model # MB629C, Modem Firmware 02.30.03
Fingerprint Apple iPhone mobile phone (iPhone OS 2.2.1)
Class Apple | iPhone OS | 2.X | phone
SEQ(SP=FC-10A%GCD=1-6%ISR=100-10A%TI=I%II=I%SS=S%TS=3)
OPS(O1=M5B4NW2NNT11SLL%O2=M5B4NW2NNT11SLL%O3=M5B4NW2NNT11%O4=M5B4NW2NNT11SLL%O5=M5B4NW2NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# iphone OS 2.x phone generation 1
Fingerprint Apple iPhone mobile phone (iPhone OS)
Class Apple | iPhone OS | 2.X | phone
SEQ(SP=F9-105%GCD=1-6%ISR=FA-104%TI=I%II=I%SS=S%TS=3)
OPS(O1=M5B4NW2NNT11SLL%O2=M5B4NW2NNT11SLL%O3=M5B4NW2NNT11%O4=M5B4NW2NNT11SLL%O5=M5B4NW2NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=FFFF%O=M5B4NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# iPhone 3G 16GB
# Apple iPhone running 2.0 firmware
# iPhone OS 2.0, jailbroken with iPhone Dev-Team's Pwnage Tool 2.0, running on an iPod Touch. Darwin 9.3.1 ARM
# Unlocked Iphone running 2.0 Firmware with SSH open.
# unlocked ipod touch 32gb, running openssh 2.0
# Darwin 9.3.1 Darwin Kernel Version 9.3.1: Sun Jun 15 21:37:01 PDT 2008; root:xnu-1228.6.76~45/RELEASE_ARM_S5L8900X iPhone1,2 arm N82AP Darwin
# iPod Touch running iPhone OS 2.0.1
# Running iPhoneOS 2.0.2
Fingerprint Apple iPhone mobile phone or iPod touch audio player (iPhone OS 2.0.1 - 2.0.2, Darwin 9.3.1)
Class Apple | iPhone OS | 2.X | phone
Class Apple | iPhone OS | 2.X | media device
SEQ(SP=0-5%GCD=1-6%ISR=15-1F%TI=I%II=I%SS=S%TS=3)
OPS(O1=M5B4NW2NNT11SLL%O2=M5B4NW2NNT11SLL%O3=M5B4NW2NNT11%O4=M5B4NW2NNT11SLL%O5=M5B4NW2NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# iPhone OS version 2.1
# iPhone 2G - OS 2.1
# 1st gen iPhone running 2.1 OS.
# iPhone 3G OS Version: 21 (5F136)
# iPod Touch 1st generation 2.1 firmware
# iphone 3G 2.1 software
# iPhone OS version 2.1 build 5F137 for iPod Touch 1st Gen
# iPod Touch First Generation (MA627ZO), iPhoneO OS 2.1 (5F137)
# Apple iPhone Model MB046LL version 2.1 (5F136) Modem Firmware 02.11.07
# iPod Touch second generation with firmware 2.1.1
# iPod Touch, second generation. OS Version 2.2 (5G77a)
# iPod Touch 1st Generation 16GB running Jailbreak 2.2 (5G77) Firmware.
# Darwin 9.4.1 Darwin Kernel Version 9.4.1: Sat Nov  1 19:09:48 PDT 2008; root:xnu-1228.7.36~2/RELEASE_ARM_S5L8900X iPhone1,2 arm N82AP Darwin
# iPhone 2.2.2_5G77 release (current)
# Darwin 9.4.1 Darwin Kernel Version 9.4.1: Mon Dec  8 20:59:30 PST 2008; root:xnu-1228.7.37~4/RELEASE_ARM_S5L8900X iPhone1,1 arm M68AP Darwin
# iPod touch 2.2
# iPhone OS 2.2.1 (5H11) release.
Fingerprint Apple iPhone mobile phone or iPod touch media player (iPhone OS 2.1 - 2.2.2, Darwin 9.4.1)
Class Apple | iPhone OS | 2.X | phone
Class Apple | iPhone OS | 2.X | media device
SEQ(SP=F1-109%GCD=1-6%ISR=FC-10E%TI=I%II=I%SS=S%TS=3)
OPS(O1=M5B4NW2NNT11SLL%O2=M5B4NW2NNT11SLL%O3=M5B4NW2NNT11%O4=M5B4NW2NNT11SLL%O5=M5B4NW2NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# iPod Touch - Software Version 2.1 - Original Apple
Fingerprint Apple iPod touch media player (iPhone OS 2.1)
Class Apple | iPhone OS | 2.X | phone
Class Apple | iPhone OS | 2.X | media device
SEQ(SP=F4-10C%GCD=1-6%ISR=102-10C%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW2NNT11SLL%O2=M5B4NW2NNT11SLL%O3=M5B4NW2NNT11%O4=M5B4NW2NNT11SLL%O5=M5B4NW2NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# iPad Version 3.2 (7B367) Model MB292LL
Fingerprint Apple iPad tablet computer (iPhone OS 3.2)
Class Apple | iPhone OS | 3.X | general purpose
SEQ(SP=FB-105%GCD=1-6%ISR=FE-108%TI=RD%CI=RD%II=RI%TS=1)
OPS(O1=M5B4NW2NNT11SLL%O2=M5B4NW2NNT11SLL%O3=M5B4NW2NNT11%O4=M5B4NW2NNT11SLL%O5=M5B4NW2NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# 3.0 Beta 4 running on iPod Touch 1st generation
# iPhone 3gs, OS 3.1.2, Jailbroken w/ Blackra1n R3
Fingerprint Apple iPhone mobile phone or iPod touch media player (iPhone OS 3.0 - 3.1.2)
Class Apple | iPhone OS | 3.X | media device
Class Apple | iPhone OS | 3.X | phone
SEQ(SP=F5-FF%GCD=1-6%ISR=F2-10C%TI=RD%CI=RD|RI%II=RI%TS=3)
OPS(O1=M3FD8NW2NNT11SLL%O2=M3FD8NW2NNT11SLL%O3=M3FD8NW2NNT11%O4=M3FD8NW2NNT11SLL%O5=M3FD8NW2NNT11SLL%O6=M3FD8NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# iPhone 3GS running OS 3.2
Fingerprint Apple iPhone 3GS mobile phone (iPhone OS 3.2)
Class Apple | iPhone OS | 3.X | phone
SEQ(SP=FA-104%GCD=1-6%ISR=FF-109%TI=RD%CI=RD%II=RI%TS=5)
OPS(O1=M5B4NW2NNT11SLL%O2=M5B4NW2NNT11SLL%O3=M5B4NW2NNT11%O4=M5B4NW2NNT11SLL%O5=M5B4NW2NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Apple iPhone OS 3.0 Beta
# Apple iPhone 3G S, MC134B, iPhone OS 3.0 (7A341), Released: Friday 19 June 2009 in the UK
# iPhone 2G, Unlocked and Jailbroken
# Darwin 10.0.0d3 Darwin Kernel Version 10.0.0d3: Fri Sep 25 23:35:35 PDT 2009; root:xnu-1357.5.30~3/RELEASE_ARM_S5L8920X iPhone2,1 arm N88AP Darwin, iPhone 3GS 32MB running iPhone OS 3.1.2 (Build 7D11)
Fingerprint Apple iPhone mobile phone (iPhone OS 3.0 - 3.1.2)
Class Apple | iPhone OS | 3.X | phone
SEQ(SP=F9-10B%GCD=1-6%ISR=FF-111%TI=RD%CI=RD%II=RI%TS=4)
OPS(O1=M5B4NW2NNT11SLL%O2=M5B4NW2NNT11SLL%O3=M5B4NW2NNT11%O4=M5B4NW2NNT11SLL%O5=M5B4NW2NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# iPhone OS 3.0 (7A341 on iPhone 3G)
# iPhone OS 3.1 beta 3 (build 7C116a)
# Darwin s-iPhone 10.0.0d3 Darwin Kernel Version 10.0.0d3: Wed May 13 22:16:49 PDT 2009; root:xnu-1357.2.89~4/RELEASE_ARM_S5L8920X iPhone2,1 arm N88AP Darwin, Iphone OS 3.0.1
# iPhone 3GS Firmware 3.1.3 16GB (3rd Generation) Internet Tethering using USB
# iPhone 3GS running 3.2.1
Fingerprint Apple iPhone mobile phone (iPhone OS 3.0 - 3.2.1, Darwin 10.0.0d3)
Class Apple | iPhone OS | 3.X | phone
SEQ(SP=ED-10B%GCD=1-6%ISR=F6-10A%TI=RD%CI=RD|RI%II=RI%TS=3)
OPS(O1=M582NW2NNT11SLL%O2=M582NW2NNT11SLL%O3=M582NW2NNT11%O4=M582NW2NNT11SLL%O5=M582NW2NNT11SLL%O6=M582NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M582NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# iPhone OS Version 3 Beta
# iphone 3.0 7A341
# Jailbroken with redsn0w, running OS 3.0.1
# Iphone Os 3.1(7c144)
# iPhone 3GS running OS 3.2
# iPhone 3GS version 3.0 (7S341) Model: MB715LL
# iPhone 2G (original iPhone) model nr. A1203, Darwin 10.0.0d3 Darwin Kernel Version 10.0.0d3: Wed May 13 22:11:58 PDT 2009; root:xnu-1357.2.89~4/RELEASE_ARM_S5L8900X iPhone1,1 arm M68AP Darwin, iPhone OS 3.0
# iPhone OS v. 3.1.2(7D11) running on iPod Touch (2nd Gen)
# Iphone OS 3.1.3
Fingerprint Apple iPhone mobile phone or iPod touch media player (iPhone OS 3.0 - 3.2, Darwin 10.0.0d3)
Class Apple | iPhone OS | 3.X | phone
Class Apple | iPhone OS | 3.X | media device
SEQ(SP=F3-109%GCD=1-6%ISR=FA-10C%TI=RD%CI=RD|RI%II=RI%TS=3)
OPS(O1=M5B4NW2NNT11SLL%O2=M5B4NW2NNT11SLL%O3=M5B4NW2NNT11%O4=M5B4NW2NNT11SLL%O5=M5B4NW2NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Apple iPhone OS 3, not connected via USB to iTunes for sychronization (affecting sync port)
Fingerprint Apple iPhone OS 3
Class Apple | iPhone OS | 3.X | phone
SEQ(SP=FD-107%GCD=1-6%ISR=101-10B%TI=RD%CI=RD|RI%II=RI%TS=3)
OPS(O1=M5B4NW2NNT11SLL%O2=M5B4NW2NNT11SLL%O3=M5B4NW2NNT11%O4=M5B4NW2NNT11SLL%O5=M5B4NW2NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=FFFF%O=M5B4NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# iPhone OS 3.01
Fingerprint Apple iPhone OS 3.0.1
Class Apple | iPhone OS | 3.X | phone
SEQ(SP=FF-109%GCD=1-6%ISR=FC-106%TI=RD%CI=RD|RI%II=RI%TS=3)
OPS(O1=M55CNW2NNT11SLL%O2=M55CNW2NNT11SLL%O3=M55CNW2NNT11%O4=M55CNW2NNT11SLL%O5=M55CNW2NNT11SLL%O6=M55CNNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M55CNW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# firmware 3.1.2
Fingerprint Apple iPhone OS 3.1.2
Class Apple | iPhone OS | 3.X | phone
SEQ(SP=F8-102%GCD=1-6%ISR=103-10D%TI=RD%CI=RD%II=RI%TS=4)
OPS(O1=M552NW2NNT11SLL%O2=M552NW2NNT11SLL%O3=M552NW2NNT11%O4=M552NW2NNT11SLL%O5=M552NW2NNT11SLL%O6=M552NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=0|FFFF%O=M552NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# OS 3.1.2 Jailbreaked
# Apple iPad
# IOS 4.0
# Os Family: 4.0
# iPhone OS 4.2.1
Fingerprint Apple iPhone OS 3.1.2 - iOS 4.2.1
Class Apple | iPhone OS | 3.X | phone
Class Apple | iOS | 4.X | phone
SEQ(SP=F6-108%GCD=1-6%ISR=FD-10B%TI=RD%II=RI%TS=3)
OPS(O1=M5B4NW2NNT11SLL%O2=M5B4NW2NNT11SLL%O3=M5B4NW2NNT11%O4=M5B4NW2NNT11SLL%O5=M5B4NW2NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 2gdev 9.3.1 Darwin Kernel Version 9.3.1: Sun Jun 15 21:37:01 PDT 2008; root:xnu-1228.6.76~45/RELEASE_ARM_S5L8900X iPhone1,1 arm M68AP Darwin, scanned from localhost using Cydia packaged Nmap 4.50
Fingerprint Apple iPhone mobile phone (iPhone OS, Darwin 9.3.1)
Class Apple | iPhone OS || phone
SEQ(SP=0-5%GCD=1-6%ISR=15-1F%TI=I%II=I%SS=S%TS=3|4)
OPS(O1=M3FD8NW2NNT11SLL%O2=M3FD8NW2NNT11SLL%O3=M3FD8NW2NNT11%O4=M3FD8NW2NNT11SLL%O5=M3FD8NW2NNT11SLL%O6=M3FD8NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 5.5 Darwin Kernel Version 5.5: Thu May 30 14:51:26 PDT 2002; root:xnu/xnu-201.42.3-obj~1/Release_PPC Power Macintosh powerpc
Fingerprint Apple Mac OS X Server 10.1 (Darwin 5.5)
Class Apple | Mac OS X | 10.1.X | general purpose
SEQ(SP=F8-10A%GCD=1-6%ISR=FD-10F%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=8218%W2=8220%W3=8204%W4=80E8%W5=80F4%W6=807A)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=832C%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=807A%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Darwin Kernel Version 6.8: Wed Sep 10 15:20:55 PDT 2003; root:xnu/xnu-344.49.obj~2/RELEASE_PPC  Power Macintosh powerpc
# Darwin 6.8 Darwin Kernel Version 6.8: Wed Sep 10 15:20:55 PDT 2003; root:xnu/xnu-344.49.obj~2/RELEASE_PPC  Power Macintosh powerpc
Fingerprint Apple Mac OS X Server 10.2.8 (Jaguar) (Darwin 6.8, PowerPC)
Class Apple | Mac OS X | 10.2.X | general purpose
SEQ(SP=FB-111%GCD=1-6%ISR=104-10E%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=8218%W2=8220%W3=8204%W4=80E8%W5=80F4%W6=807A)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=832C%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=807A%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# MAC OS X 10.3.9 (7W98) on PowerPC (Darwin Kernel 7.9.0)
Fingerprint Apple Mac OS X 10.3.9 (Panther) (Darwin 7.9.0, PowerPC)
Class Apple | Mac OS X | 10.3.X | general purpose
SEQ(R=N)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45|7C-86%TG=40|80%S=Z%A=S+%F=AR%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=2B18%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin version 7.9.0: Wed mar 30 20:11:1 7 PST 2005; root:xnu/xnu-571.12.7.obj~1/RELEASE_PPC Power Macintosh powerpc
Fingerprint Apple Mac OS X 10.3.9 (Panther) (Darwin 7.9.0, PowerPC)
Class Apple | Mac OS X | 10.3.X | general purpose
SEQ(SP=F8-108%GCD=1-6%ISR=F6-110%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=8218%W2=8220%W3=8204%W4=80E8%W5=80F4%W6=807A)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=832C%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 7.9.0 Darwin Kernel Version 7.9.0: Wed Mar 30 20:11:17 PST 2005; root:xnu-517.12.7.obj~1/RELEASE_PPC Power Macintosh powerpc (Mac OS X v.10.3.9)
Fingerprint Apple Mac OS X 10.3.9 (Panther) (Darwin 7.9.0, PowerPC)
Class Apple | Mac OS X | 10.3.X | general purpose
SEQ(SP=FE-108%GCD=1-6%ISR=109-113%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 7.9.0 Darwin Kernel Version 7.9.0: Wed Mar 30 20:11:17 PST 2005; root:xnu/xnu-517.12.7.obj~1/RELEASE_PPC  Power Macintosh powerpc
Fingerprint Apple Mac OS X 10.3.9 (Panther) (Darwin 7.9.0, PowerPC)
Class Apple | Mac OS X | 10.3.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=106-110%TI=I%II=I%SS=S%TS=U)
OPS(O1=M3FD8%O2=M3FD8%O3=M3FD8%O4=M3FD8%O5=M3FD8%O6=M3FD8)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 7.9.0 Darwin Kernel Version 7.9.0: Wed Mar 30 20:11:17 PST 2005; root:xnu/xnu-517.12.7.obj~1/RELEASE_PPC  Power Macintosh powerpc
Fingerprint Apple Mac OS X 10.3.9 (Panther) (Darwin 7.9.0, PowerPC)
Class Apple | Mac OS X | 10.3.X | general purpose
SEQ(SP=FE-108%GCD=1-6%ISR=FF-111%TI=I%CI=I%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Apple Mac OS X 10.3.9 (Panther) - Darwin Kernel Version 7.9.0 Wed Mar 30 20:11:17 PST 2005; root:xnu/xnu-517.12.7.obj~1/RELEASE_PPC  Power Macintosh powerpc
# Apple Mac OS X 10.4.5 on PPC
Fingerprint Apple Mac OS X 10.3.9 (Panther) - 10.4.5 (Tiger) (Darwin 7.9.0 - 8.5.0, PowerPC)
Class Apple | Mac OS X | 10.3.X | general purpose
SEQ(SP=F9-10B%GCD=1-6%ISR=101-111%TI=I%II=I%SS=S%TS=1)
OPS(O1=M3FD8NW0NNT11%O2=M3FD8NW0NNT11%O3=M3FD8NW0NNT11%O4=M3FD8NW0NNT11%O5=M3FD8NW0NNT11%O6=M3FD8NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Apple eMac G4 1.25GHz, Mac OS X 10.4.7 (uname -a: Darwin 8.7.8 Darwin Kernel Version 8.7.8: Fri May 26 15:20:53 PDT 2006; root:xnu-792.6.76.obj~1/RELEASE_PPC Power Maciontosh powerpc)
# Apple Mac OS X 10.3.9 (PowerPC)
Fingerprint Apple Mac OS X 10.3.9 (Panther) - 10.4.7 (Tiger) (Darwin 7.9.0 - 8.7.8, PowerPC)
Class Apple | Mac OS X | 10.3.X | general purpose
Class Apple | Mac OS X | 10.4.X | general purpose
SEQ(SP=AC-108%GCD=1-6%ISR=EA-110%TI=I|RD%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N|Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N|Y%T=3B-45%TG=40%S=O|Z%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 7.9.0 Darwin Kernel Version 7.9.0: Wed Mar 30 20:11:17 PST 2005; root:xnu/xnu-517.12.7.obj~1/RELEASE_PPC  Power Macintosh powerpc (Mac OS X Server 10.3.9 (7W98))
Fingerprint Apple Mac OS X Server 10.3.9 (Panther) (Darwin 7.9.0, PowerPC)
Class Apple | Mac OS X | 10.3.X | general purpose
SEQ(SP=FC-10A%GCD=1-6%ISR=100-112%TI=I%II=I%SS=S%TS=0|1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=8218%W2=8220%W3=8204%W4=80E8%W5=80F4%W6=807A)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=832C%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 8.0.0 Darwin Keynel Version 8.0.0: Sat Mar 26 14:15:22 PST 2005; root:xnu-792.obj~1/RELEASE_PPC Power Macintosh powerpc
Fingerprint Apple Mac OS X 10.4 (Tiger) (Darwin 8.0.0)
Class Apple | Mac OS X | 10.4.X | general purpose
SEQ(SP=FD-10F%GCD=1-6%ISR=FE-10C%TI=I%II=I%SS=S%TS=1)
OPS(O1=M3FD8NW0NNT11%O2=M3FD8NW0NNT11%O3=M3FD8NW0NNT11%O4=M3FD8NW0NNT11%O5=M3FD8NW0NNT11%O6=M3FD8NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 8.10.0 Darwin Kernel Version 8.10.0: Wed May 23 16:50:59 PDT 2007; root:xnu-792.21.3~1/RELEASE_PPC Power Macintosh powerpc
Fingerprint Apple Mac OS X 10.4 (Tiger) (Darwin 8.10.0, PowerPC)
Class Apple | Mac OS X | 10.4.X | general purpose
SEQ(SP=C-16%GCD=1|>1000000%ISR=FA-104%TI=I|RD%II=I%TS=2)
OPS(O1=NNT11|M5B4NW0NNT11SLL%O2=NNT11|M5B4NW0NNT11SLL%O3=|NNT11|M5B4NW0NNT11%O4=|NNT11|M5B4NW0NNT11SLL%O5=|NNT11|M5B4NW0NNT11SLL%O6=|NNT11|M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=0|FFFF%W4=0|FFFF%W5=0|FFFF%W6=0|FFFF)
ECN(R=Y%DF=N|Y%T=3B-45%TG=40%W=0|FFFF%O=|M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 8.10.0 Darwin Kernel Version 8.10.0: Wed May 23 16:50:59 PDT 2007; root:xnu-792.21.3~1/RELEASE_PPC Power Macintosh powerpc
# Darwin 8.10.0 Darwin Kernel Version 8.10.0: Wed May 23 16:50:59 PDT 2007; root:xnu-792.21.3~1/RELEASE_PPC Power Macintosh powerpc
# Darwin 8.10.1 Darwin Kernel Version 8.10.1: Wed May 23 16:33:00 PDT 2007; root:xnu-792.22.5~1/RELEASE_I386 i386 i386
# Darwin 8.10.3 Darwin Kernel Version 8.10.3: Wed Jun 27 23:29:36 PDT 2007; root:xnu-792.23.3~1/RELEASE_I386 i386 i386
# Darwin 8.11.0 Darwin Kernel Version 8.11.0: Wed Oct 10 18:26:00 PDT 2007; root:xnu-792.24.17~1/RELEASE_PPC Power Macintosh powerpc
# Darwin 8.10.2 Darwin Kernel Version 8.10.2: Wed Jun 20 21:49:49 PDT 2007; root:xnu-792.22.6~1/RELEASE_I386 i386 i386
# Darwin 8.11.1 Darwin Kernel Version 8.11.1: Wed Oct 10 18:23:28 PDT 2007; root:xnu-792.25.20~1/RELEASE_I386 i386 i386
Fingerprint Apple Mac OS X 10.4.10 (Tiger) (Darwin 8.10.0 - 8.11.1)
Class Apple | Mac OS X | 10.4.X | general purpose
SEQ(SP=C-16%GCD=1|>1000000%ISR=E8-103%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11SLL%O2=M5B4NW0NNT11SLL%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11SLL%O5=M5B4NW0NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 8.10.0 Darwin Kernel Version 8.10.0: Wed May 23 16:50:59 PDT 2007; root:xnu-792.21.3~1/RELEASE_PPC Power Macintosh
# Darwin 8.10.1 Darwin Kernel Version 8.10.1: Wed May 23 16:33:00 PDT 2007; root:xnu-792.22.5~1/RELEASE_I386 i386 i386
# Darwin 8.10.1 Darwin Kernel Version 8.10.1: Wed May 23 16:33:00 PDT 2007; root:xnu-792.22.5~1/RELEASE_I386 i386 i386 (OS X 10.4.10)
# Darwin 8.10.0 Darwin Kernel Version 8.10.0: Wed May 23 16:50:59 PDT 2007; root:xnu-792.21.3~1/RELEASE_PPC Power Macintosh powerpc
# Darwin 8.10.1 Darwin Kernel Version 8.10.1: Wed May 23 16:33:00 PDT 2007; root:xnu-792.22.5~1/RELEASE_I386 i386 i386
# Darwin 8.10.2 Darwin Kernel Version 8.10.2: Wed Jun 20 21:49:49 PDT 2007; root:xnu-792.22.6~1/RELEASE_I386 i386 i386
# Darwin 8.11.1 Darwin Kernel Version 8.11.1: Wed Oct 10 18:23:28 PDT 2007; root:xnu-792.25.20~1/RELEASE_I386 i386 i386
Fingerprint Apple Mac OS X 10.4.10 (Tiger) (Darwin 8.10.0 - 8.11.1)
Class Apple | Mac OS X | 10.4.X | general purpose
SEQ(SP=C-16%GCD=1|>1000000%ISR=D4-102%TI=I%II=I%SS=S%TS=1)
OPS(O1=M3FD8NW0NNT11SLL%O2=M3FD8NW0NNT11SLL%O3=M3FD8NW0NNT11%O4=M3FD8NW0NNT11SLL%O5=M3FD8NW0NNT11SLL%O6=M3FD8NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 8.10.0 Darwin Kernel Version 8.10.0: Wed May 23 16:50:59 PDT 2007; root:xnu-792.21.3~1/RELEASE_PPC Power Macintosh powerpc
Fingerprint Apple Mac OS X 10.4.10 (Tiger) (Darwin 8.10.0, PowerPC)
Class Apple | Mac OS X | 10.4.X | general purpose
SEQ(SP=FA-10C%GCD=1-6%ISR=F7-105%TI=I%II=I%SS=S%TS=1|2)
OPS(O1=M5B4NW0NNT11SLL%O2=M5B4NW0NNT11SLL%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11SLL%O5=M5B4NW0NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 8.10.0 Darwin Kernel Version 8.10.0: Wed May 23 16:50:59 PDT 2007; root:xnu-792.21.3~1/RELEASE_PPC Power Macintosh powerpc
Fingerprint Apple Mac OS X 10.4.10 (Tiger) (Darwin 8.10.0, PowerPC)
Class Apple | Mac OS X | 10.4.X | general purpose
SEQ(SP=C-16%GCD=1|>1000000%ISR=F1-103%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW3NNT11SLL%O2=M5B4NW3NNT11SLL%O3=M5B4NW3NNT11%O4=M5B4NW3NNT11SLL%O5=M5B4NW3NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 8.10.1 Darwin Kernel Version 8.10.1: Wed May 23 16:33:00 PDT 2007; root:xnu-792.22.5~1/RELEASE_I386 i386 i386
Fingerprint Apple Mac OS X 10.4.10 (Tiger) (Darwin 8.10.1)
Class Apple | Mac OS X | 10.4.X | general purpose
SEQ(SP=B-15%GCD=1|>1000000%ISR=DF-103%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11SLL%O2=M5B4NW0NNT11SLL%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11SLL%O5=M5B4NW0NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin .8.10.0 Darwin Kernel  Version 8.10.0: Wed May 23 16:50:59 PDT 2007; root:xnu-792.21.3~1/RELEASE_PPC Power Macintosh powerpc
# Darwin 8.11.0 Darwin Kernel Version 8.11.0: Wed Oct 10 18:26:00 PDT 2007; root:xnu-792.24.17~1/RELEASE_PPC Power Macintosh powerpc (OS X 10.4.11)
Fingerprint Apple Mac OS X 10.4.11 (Tiger) (Darwin 8.10.0)
Class Apple | Mac OS X | 10.4.X | general purpose
SEQ(SP=7-17%GCD=1|>1000000%ISR=F2-102%TI=I%II=I%SS=S%TS=0|1)
OPS(O1=M5B4NW0NNT11SLL%O2=M5B4NW0NNT11SLL%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11SLL%O5=M5B4NW0NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=FFFF%O=M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Darwin 8.11.0 Darwin Kernel Version 8.11.0: Wed Oct 10 18:26:00 PDT 2007; root:xnu-792.24.17~1/RELEASE_PPC Power Macintosh powerpc
Fingerprint Apple Mac OS X 10.4.11 (Tiger) (Darwin 8.11.0)
Class Apple | Mac OS X | 10.4.X | general purpose
SEQ(SP=B-15%GCD=>1000000%ISR=A1-FF%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 8.11.0 Darwin Kernel Version 8.11.0: Wed Oct 10 18:26:00 PDT 2007; root:xnu-792.24.17~1/RELEASE_PPC Power Macintosh powerpc
Fingerprint Apple Mac OS X 10.4.11 (Tiger) (Darwin 8.11.0, PowerPC)
Class Apple | Mac OS X | 10.4.X | general purpose
SEQ(SP=FE-10C%GCD=1-6%ISR=F2-108%TI=I|RD%II=I%SS=O|S%TS=1)
OPS(O1=M538NW0NNT11SLL%O2=M538NW0NNT11SLL%O3=M538NW0NNT11%O4=M538NW0NNT11SLL%O5=M538NW0NNT11SLL%O6=M538NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N|Y%T=3B-45%TG=40%W=0|FFFF%O=|M538NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# 8.11.0 Darwin Kernel Version 8.11.0: Wed Oct 10 18:26:00 PDT 2007; root:xnu-792.24.17~1/RELEASE_PPC Power Macintosh powerpc
Fingerprint Apple Mac OS X 10.4.11 (Tiger) (Darwin 8.11.0, PowerPC)
Class Apple | Mac OS X | 10.4.X | general purpose
SEQ(SP=C-1DA%GCD=1-6|>1000000%ISR=D0-122%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW5NNT11SLL%O2=M5B4NW5NNT11SLL%O3=M5B4NW5NNT11%O4=M5B4NW5NNT11SLL%O5=M5B4NW5NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW5SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 8.8.0 Darwin Kernel Version 8.8.0: Fri Sep  8 17:18:57 PDT 2006; root:xnu-792.12.6.obj~1/RELEASE_PPC Power Macintosh powerpc - Apple MacOS X 10.4.8 (Panther) on PPC
# Darwin 8.9.0 Darwin Kernel Version 8.9.0: Thu Feb 22 20:54:07 PST 2007; root:xnu-792.17.14~1/RELEASE_PPC Power Macintosh powerpc
Fingerprint Apple Mac OS X 10.4.8 (Tiger) (Darwin 8.8.0 - 8.9.0, PowerPC)
Class Apple | Mac OS X | 10.4.X | general purpose
SEQ(SP=FB-107%GCD=1-6%ISR=108-112%TI=I%II=I%SS=S%TS=1)
OPS(O1=M3FD8NW3NNT11SLL%O2=M3FD8NW3NNT11SLL%O3=M3FD8NW3NNT11%O4=M3FD8NW3NNT11SLL%O5=M3FD8NW3NNT11SLL%O6=M3FD8NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 8.10.0 Darwin Kernel Version 8.10.0: Wed May 23 16:50:59 PDT 2007; root:xnu-792.21.3~1/RELEASE_PPC Power Macintosh powerpc
# Darwin 8.11.1 Darwin Kernel Version 8.11.1: Wed Oct 10 18:23:28 PDT 2007; root:xnu-792.25.20~1/RELEASE_I386 i386 i386 (Mac OS X 10.4.11)
# Apple Mac OS X 10.4.8 (PowerPC)
# Darwin 8.10.1 Darwin Kernel Version 8.10.1: Wed May 23 16:33:00 PDT 2007; root:xnu-792.22.5~1/RELEASE_I386 i386 i386 (macmini running OSX 10.4.10)
# Darwin 8.11.0 Darwin Kernel Version 8.11.0: Wed Oct 10 18:26:00 PDT 2007; root:xnu-792.24.17~1/RELEASE_PPC Power Macintosh powerpc
Fingerprint Apple Mac OS X 10.4.8 - 10.4.11 (Tiger) (Darwin 8.10.0 - 8.11.0)
Class Apple | Mac OS X | 10.4.X | general purpose
SEQ(SP=102-110%GCD=1-6%ISR=FE-10C%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW1NNT11SLL|M5B4NW3NNT11SLL|M5B4NW4NNT11SLL|M5B4NW6NNT11SLL%O2=M5B4NW1NNT11SLL|M5B4NW3NNT11SLL|M5B4NW4NNT11SLL|M5B4NW6NNT11SLL%O3=M5B4NW1NNT11|M5B4NW3NNT11|M5B4NW4NNT11|M5B4NW6NNT11%O4=M5B4NW1NNT11SLL|M5B4NW3NNT11SLL|M5B4NW4NNT11SLL|M5B4NW6NNT11SLL%O5=M5B4NW1NNT11SLL|M5B4NW3NNT11SLL|M5B4NW4NNT11SLL|M5B4NW6NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL|M5B4NW3SLL|M5B4NW4SLL|M5B4NW6SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Power Mac G5 running OS X 10.4.8
# Darwin 8.11.0 Darwin Kernel Version 8.11.0: Wed Oct 10 18:26:00 PDT 2007; root:xnu-792.24.17~1/RELEASE_PPC Power Macintosh powerpc
Fingerprint Apple Mac OS X 10.4.8 - 10.4.11 (Tiger) (Darwin 8.11.0, PowerPC)
Class Apple | Mac OS X | 10.4.X | general purpose
SEQ(SP=FA-104%GCD=1-6%ISR=FF-10D%TI=I%II=I%SS=S%TS=U)
OPS(O1=M3FD8SLL%O2=M3FD8SLL%O3=M3FD8%O4=M3FD8SLL%O5=M3FD8SLL%O6=M3FD8SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Apple Mac OS 10.4.8/ppc (Darwin 8.8.0 Darwin Kernel Version 8.8.0: Fri Sep  8 17:18:57 PDT
# Darwin 8.8.1 Darwin Kernel Version 8.8.1: Mon Sep 25 19:42:00 PDT 2006; root:xnu-792.13.8.obj~1/RELEASE_I386 i386 i386
# Apple Mac OS X 10.4.8 (Tiger) on x86 Core Duo
# Apple Mac OS X 10.4.9, Darwin Kernel Version 8.9.1: Thu Feb 22 20:55:00 PST 2007; root:xnu-792.18.15~1/RELEASE_I386 i386 i386
# Darwin 8.10.1 Darwin Kernel Version 8.10.1: Wed May 23 16:33:00 PDT 2007; root:xnu-792.22.5~1/RELEASE_I386 i386 i386 (OS X version 10.4.10, Intel version)
# Darwin 8.10.2 Darwin Kernel Version 8.10.2: RELEASE_I386 i386 i386 (Mac OS X 10.4.10)
# Darwin 8.11.0 Darwin Kernel Version 8.11.0: Wed Oct 10 18:26:00 PDT 2007; root:xnu-792.24.17~1/RELEASE_PPC Power Macintosh powerpc
Fingerprint Apple Mac OS X 10.4.8 - 10.4.11 (Tiger) (Darwin 8.8.0 - 8.11.0)
Class Apple | Mac OS X | 10.4.X | general purpose
SEQ(SP=BC-109%GCD=1-6%ISR=F4-10F%TI=I%II=I%SS=S%TS=1)
OPS(O1=M3FD8NW0NNT11SLL%O2=M3FD8NW0NNT11SLL%O3=M3FD8NW0NNT11%O4=M3FD8NW0NNT11SLL%O5=M3FD8NW0NNT11SLL%O6=M3FD8NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Apple Mac OS X 10.4.8 (Tiger) on x86 Core Duo (first-gen Intel iMac 17"/1.83): Darwin 8.8.1 Darwin Kernel Version 8.8.1: Mon Sep 25 19:42:00 PDT 2006 root:xnu-792.13.8.obj~1/RELEASE_I386 i386 i386)
# Darwin 8.8.0 Darwin Kernel Version 8.8.0: Fri Sep  8 17:18:57 PDT 2006; root:xnu-792.12.6.obj~1/RELEASE_PPC Power Macintosh powerpc
# Mac OS X Server 10.4.9 PowerPC Darwin 8.9.0
# Darwin 8.9.1 Darwin Kernel Version 8.9.1: Thu Feb 22 20:58:18 PST 2007; root:xnu-792.18.15~1/RELEASE_PPC Power Macintosh powerpc (MacOS 10.4.9 Server [PPC])
# OS X 10.4.8 (Intel)  -- Darwin 8.8.1 Darwin Kernel Version 8.8.1: Mon Sep 25 19:42:00 PDT 2006; root:xnu-792.13.8.obj~1/RELEASE_I386 i386 i386
# Mac OS X 10.4.10 (8R218) Darwin 8.10.0 Darwin Kernel Version 8.10.0 : Wed May 23 16:50:59 PDT 2007; root:xnu-792.21.3~1/RELEASE_PPC Power Macintosh powerpc
# Darwin 8.10.1 Darwin Kernel Version 8.10.1: Wed May 23 16:33:00 PDT 2007; root:xnu-792.22.5~1/RELEASE_I386 i386 i386
# Darwin 8.10.2 Darwin Kernel Version 8.10.2: Wed Jun 20 21:49:49 PDT 2007; root:xnu-792.22.6~1/RELEASE_I386 i386 i386
# Darwin 8.11.0 Darwin Kernel Version 8.11.0: Wed Oct 10 18:26:00 PDT 2007; root:xnu-792.24.17~1/RELEASE_PPC Power Macintosh powerpc
# Darwin 8.11.1 Darwin Kernel Version 8.11.1: Wed Oct 10 18:23:28 PDT 2007; root:xnu-792.25.20~1/RELEASE_I386 i386 i386
# AppleTV running v2.3.1
Fingerprint Apple Mac OS X 10.4.8 - 10.4.11 (Tiger) (Darwin 8.8.0 - 8.11.1)
Class Apple | Mac OS X | 10.4.X | general purpose
SEQ(SP=BC-10C%GCD=1-6%ISR=C7-111%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11SLL%O2=M5B4NW0NNT11SLL%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11SLL%O5=M5B4NW0NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Apple Mac OS X 10.4.9 on PowerPC G4 (1.5)
Fingerprint Apple Mac OS X 10.4.9 (Tiger) (PowerPC)
Class Apple | Mac OS X | 10.4.X | general purpose
SEQ(SP=103-10D%GCD=1-6%ISR=100-10E%TI=I%II=I%SS=S%TS=0|1)
OPS(O1=M3FD8NW0NNT11SLL%O2=M3FD8NW0NNT11SLL%O3=M3FD8NW0NNT11%O4=M3FD8NW0NNT11SLL%O5=M3FD8NW0NNT11SLL%O6=M3FD8NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 8.11.0 Darwin Kernel Version 8.11.0: Wed Oct 10 18:26:00 PDT 2007; root:xnu-792.24.17~1/RELEASE_PPC Power Macintosh powerpc
# Darwin 8.11.1 Darwin Kernel Version 8.11.1: Wed Oct 10 18:23:28 PDT 2007; root:xnu-792.25.20~1/RELEASE_I386 i386 i386
Fingerprint Apple Mac OS X 10.4.9 - 10.4.10 (Tiger) (Darwin 8.11.0 - 8.11.1, PowerPC)
Class Apple | Mac OS X | 10.4.X | general purpose
SEQ(SP=F8-10A%GCD=1-6%ISR=F1-107%TI=I%TS=1)
OPS(O1=M5B4NW0NNT11SLL%O2=M5B4NW0NNT11SLL%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11SLL%O5=M5B4NW0NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Mac OS X 10.5 Build 9A303
# Darwin 9.0.0 Darwin Kernel Version 9.0.0: Tue Oct  9 21:35:55 PDT 2007; root:xnu-1228~1/RELEASE_I386 i386
Fingerprint Apple Mac OS X 10.5 (Leopard) (Darwin 9.0.0)
Class Apple | Mac OS X | 10.5.X | general purpose
SEQ(SP=EF-10D%GCD=1-6%ISR=101-10B%TI=I%II=I%SS=S%TS=1)
OPS(O1=M3FD8NW1NNT11SLL|M3FD8NW5NNT11SLL%O2=M3FD8NW1NNT11SLL|M3FD8NW5NNT11SLL%O3=M3FD8NW1NNT11|M3FD8NW5NNT11%O4=M3FD8NW1NNT11SLL|M3FD8NW5NNT11SLL%O5=M3FD8NW1NNT11SLL|M3FD8NW5NNT11SLL%O6=M3FD8NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8NW1SLL|M3FD8NW5SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 9.0.0b4 Darwin Kernel Version 9.0.0b4: Wed Jul 18 23:23:23 PDT 2007; root:xnu-1155.2~1/RELEASE_I386 i386
Fingerprint Apple Mac OS X 10.5 (Leopard) (Darwin 9.0.0b4, x86)
Class Apple | Mac OS X | 10.5.X | general purpose
SEQ(SP=F2-10A%GCD=1-6%ISR=FA-110%TI=RD%II=RI%TS=3)
OPS(O1=M5B4NW3NNT11SLL%O2=M5B4NW3NNT11SLL%O3=M5B4NW3NNT11%O4=M5B4NW3NNT11SLL%O5=M5B4NW3NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 9.2.2 Darwin Kernel Version 9.2.2: Tue Mar  4 21:17:34 PST 2008; root:xnu-1228.4.31~1/RELEASE_I386 i386
Fingerprint Apple Mac OS X 10.5 (Leopard) (Darwin 9.2.2, x86)
Class Apple | Mac OS X | 10.5.X | general purpose
SEQ(SP=FF-10B%GCD=1-6%ISR=FC-10C%TI=RD%II=RI%TS=3)
OPS(O1=M550NW2NNT11SLL%O2=M550NW2NNT11SLL%O3=M550NW2NNT11%O4=M550NW2NNT11SLL%O5=M550NW2NNT11SLL%O6=M550NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M550NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 9.1.0 Darwin Kernel Version 9.1.0: Wed Oct 31 17:48:21 PDT 2007; root:xnu-1228.0.2~1/RELEASE_PPC Power Macintosh
# Darwin 9.0.0 Darwin Kernel Version 9.0.0: Tue Oct  9 21:35:55 PDT 2007; root:xnu-1228~1/RELEASE_I386 i386
# Mac OS 10.5 leopard 9A581
# Darwin 9.0.0 Darwin Kernel Version 9.0.0: Tue Oct  9 21:37:58 PDT 2007; root:xnu-1228~1/RELEASE_PPC Power Macintosh
# Darwin 9.1.0 Darwin Kernel Version 9.1.0: Wed Oct 31 17:46:22 PDT 2007; root:xnu-1228.0.2~1/RELEASE_I386 i386
# Darwin 9.2.0 Darwin Kernel Version 9.2.0: Tue Feb  5 16:15:19 PST 2008; root:xnu-1228.3.13~1/RELEASE_PPC Power Macintosh powerpc
# Darwin 9.2.0 Darwin Kernel Version 9.2.0: Tue Feb  5 16:13:22 PST 2008; root:xnu-1228.3.13~1/RELEASE_I386 i386, Mac OS X Version 10.5.2 Build 9C31
# Darwin 9.2.2 Darwin Kernel Version 9.2.2: Tue Mar  4 21:17:34 PST 2008; root:xnu-1228.4.31~1/RELEASE_I386 i386
# Darwin 9.3.0 Darwin Kernel Version 9.3.0: Fri May 23 00:49:16 PDT 2008; root:xnu-1228.5.18~1/RELEASE_I386 i386
# Darwin 9.4.0 Darwin Kernel Version 9.4.0: Mon Jun  9 19:30:53 PDT 2008; root:xnu-1228.5.20~1/RELEASE_I386 i386
# Darwin 9.5.0 Darwin Kernel Version 9.5.0: Wed Sep  3 11:29:43 PDT 2008; root:xnu-1228.7.58~1/RELEASE_I386 i386
# Darwin 9.6.0 Darwin Kernel Version 9.6.0: Mon Nov 24 17:37:00 PST 2008; root:xnu-1228.9.59~1/RELEASE_I386 i386
# 9.8.0 Darwin Kernel Version 9.8.0: Wed Jul 15 16:55:01 PDT 2009; root:xnu-1228.15.4~1/RELEASE_I386 i386
# Darwin 10.0.0 Darwin Kernel Version 10.0.0: Fri Jul 31 22:47:34 PDT 2009; root:xnu-1456.1.25~1/RELEASE_I386 i386
# Darwin 10.2.0 Darwin Kernel Version 10.2.0: Tue Nov  3 10:37:10 PST 2009; root:xnu-1486.2.11~1/RELEASE_I386 i386
# Darwin 10.3.0 Darwin Kernel Version 10.3.0: Fri Feb 26 11:58:09 PST 2010; root:xnu-1504.3.12~1/RELEASE_I386 i386, 10.6.3
Fingerprint Apple Mac OS X 10.5 - 10.6.3 (Leopard - Snow Leopard) (Darwin 9.0.0 - 10.3.0)
Class Apple | Mac OS X | 10.5.X | general purpose
Class Apple | Mac OS X | 10.6.X | general purpose
SEQ(SP=F1-107%GCD=1-6%ISR=FB-10C%TI=RD%II=RI%TS=3)
OPS(O1=M3FD8NW1NNT11SLL|M3FD8NW2NNT11SLL|M3FD8NW3NNT11SLL%O2=M3FD8NW1NNT11SLL|M3FD8NW2NNT11SLL|M3FD8NW3NNT11SLL%O3=M3FD8NW1NNT11|M3FD8NW2NNT11|M3FD8NW3NNT11%O4=M3FD8NW1NNT11SLL|M3FD8NW2NNT11SLL|M3FD8NW3NNT11SLL%O5=M3FD8NW1NNT11SLL|M3FD8NW2NNT11SLL|M3FD8NW3NNT11SLL%O6=M3FD8NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8NW1SLL|M3FD8NW2SLL|M3FD8NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 9.6.9: Darwin Kernel Version 9.6.0: date; root:xnu-1228.9~1/RELEASE_I386 i386
# Darwin 9.5.0 Darwin Kernel Version 9.5.0: Wed Sep 3 11:31:44 PDT 2008; root:xnu-1228.7.58~1/RELEASE_PPC Power Macintosh
# 9.2.0 Darwin Kernel Version 9.2.0
# Darwin <host> 10.2.0 Darwin Kernel Version 10.2.0: Tue Nov  3 10:37:10 PST 2009; root:xnu-1486.2.11~1/RELEASE_I386 i386
# Apple iOS 4.0.1
Fingerprint Apple Mac OS X 10.5.2 - 10.6.2 (Leopard - Snow Leopard) (Darwin 9.2.0 - 10.2.0)
Class Apple | Mac OS X | 10.5.X | general purpose
Class Apple | Mac OS X | 10.6.X | general purpose
SEQ(SP=F3-107%GCD=1-6%ISR=FA-110%TI=RD%CI=RI%II=RI%TS=3)
OPS(O1=M5B4NW2NNT11SLL|M5B4NW3NNT11SLL%O2=M5B4NW2NNT11SLL|M5B4NW3NNT11SLL%O3=M5B4NW2NNT11|M5B4NW3NNT11%O4=M5B4NW2NNT11SLL|M5B4NW3NNT11SLL%O5=M5B4NW2NNT11SLL|M5B4NW3NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW2SLL|M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 9.3.0 Darwin Kernel Version 9.3.0: Fri May 23 00:51:20 PDT 2008; root:xnu-1228.5.18~1/RELEASE_PPC Power Macintosh
Fingerprint Apple Mac OS X 10.5.3 (Leopard) (Darwin 9.3.0)
Class Apple | Mac OS X | 10.5.X | general purpose
SEQ(SP=FA-10A%GCD=1-6%ISR=FC-114%TI=RD%II=RI%TS=3)
OPS(O1=M3FD8NW3NNT11SLL%O2=M3FD8NW3NNT11SLL%O3=M3FD8NW3NNT11%O4=M3FD8NW3NNT11SLL%O5=M3FD8NW3NNT11SLL%O6=M3FD8NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8NW3SLL%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 9.3.0 Darwin Kernel Version 9.3.0: Fri May 23 00:49:16 PDT 2008; root:xnu-1228.5.18~1/RELEASE_I386 i386
# Darwin 9.4.0 Darwin Kernel Version 9.4.0: Mon Jun  9 19:30:53 PDT 2008; root:xnu-1228.5.20~1/RELEASE_I386 i386
Fingerprint Apple Mac OS X 10.5.3 - 10.5.4 (Leopard) (Darwin 9.3.0 - 9.4.0)
Class Apple | Mac OS X | 10.5.X | general purpose
SEQ(SP=ED-109%GCD=1-6%ISR=F5-10D%TI=RD%II=RI%TS=3)
OPS(O1=M5B4NW3NNT11SLL%O2=M5B4NW3NNT11SLL%O3=M5B4NW3NNT11%O4=M5B4NW3NNT11SLL%O5=M5B4NW3NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 9.4.0 Darwin Kernel Version 9.4.0: Mon Jun  9 19:30:53 PDT 2008; root:xnu-1228.5.20~1/RELEASE_I386 i386, Mac OS X 10.5.4
Fingerprint Apple Mac OS X 10.5.4 (Leopard) (Darwin 9.4.0)
Class Apple | Mac OS X | 10.5.X | general purpose
SEQ(SP=F3-10D%GCD=1-6%ISR=100-10E%TI=RD%II=RI%TS=3)
OPS(O1=M5B4NW3NNT11SLL%O2=M5B4NW3NNT11SLL%O3=M5B4NW3NNT11%O4=M5B4NW3NNT11SLL%O5=M5B4NW3NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 9.4.0 Darwin Kernel Version 9.4.0: Mon Jun  9 19:30:53 PDT 2008; root:xnu-1228.5.20~1/RELEASE_I386 i386
Fingerprint Apple Mac OS X 10.5.4 (Leopard) (Darwin 9.4.0)
Class Apple | Mac OS X | 10.5.X | general purpose
SEQ(SP=F0-104%GCD=1-6%ISR=FC-10A%TI=RD%II=RI%TS=3)
OPS(O1=M3FD8NW3NNT11SLL%O2=M3FD8NW3NNT11SLL%O3=M3FD8NW3NNT11%O4=M3FD8NW3NNT11SLL%O5=M3FD8NW3NNT11SLL%O6=M3FD8NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=2F-39%TG=40%W=FFFF%O=M3FD8NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=2F-39%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=2F-39%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=2F-39%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=2F-39%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=2F-39%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=2F-39%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=2F-39%TG=40%CD=S)

# Darwin Kernel Version 9.5.0: Wed Sep  3 11:29:43 PDT 2008; root:xnu-1228.7.58~1/RELEASE_I386 i386
Fingerprint Apple Mac OS X 10.5.5 (Leopard) (Darwin 9.5.0)
Class Apple | Mac OS X | 10.5.X | general purpose
SEQ(SP=FD-107%GCD=1-6%ISR=FE-108%TI=RD%TS=3)
OPS(O1=M5B4NW3NNT11SLL%O2=M5B4NW3NNT11SLL%O3=NNT11|M5B4NW3NNT11%O4=NNT11|M5B4NW3NNT11SLL%O5=M5B4NW3NNT11SLL%O6=NNT11|M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=|M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=816-E05E%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 9.5.0 Darwin Kernel Version 9.5.0: Wed Sep  3 11:29:43 PDT 2008; root:xnu-1228.7.58~1/RELEASE_I386 i386
# Darwin 9.6.0 Darwin Kernel Version 9.6.0: Mon Nov 24 17:37:00 PST 2008; root:xnu-1228.9.59~1/RELEASE_I386 i386
# Darwin 10.0.0 Darwin Kernel Version 10.0.0: Fri Jul 31 22:47:34 PDT 2009; root:xnu-1456.1.25~1/RELEASE_I386 i386
Fingerprint Apple Mac OS X 10.5.5 - 10.6.1 (Leopard - Snow Leopard) (Darwin 9.5.0 - 10.0.0)
Class Apple | Mac OS X | 10.5.X | general purpose
Class Apple | Mac OS X | 10.6.X | general purpose
SEQ(SP=FA-108%GCD=1-6%ISR=FE-112%TI=RD%II=RI%TS=3)
OPS(O1=M5B4NW3NNT11SLL%O2=M5B4NW3NNT11SLL%O3=M5B4NW3NNT11%O4=M5B4NW3NNT11SLL%O5=M5B4NW3NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 9.5.0 Darwin Kernel Version 9.5.0: Wed Sep 3  11:31:33 PDT 2008; root:xnu-1228.7.58~1/RELEASE_PPC Power Macintosh
Fingerprint Apple Mac OS X 10.5.6 (Leopard) (Darwin 9.5.0)
Class Apple | Mac OS X | 10.5.X | general purpose
SEQ(SP=F5-109%GCD=1-6%ISR=F9-10D%TI=RD%II=RI%TS=3|5|6)
OPS(O1=M524NW2NNT11SLL%O2=M524NW2NNT11SLL%O3=M524NW2NNT11%O4=NNT11|M524NW2NNT11SLL%O5=M524NW2NNT11SLL%O6=M524NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M524NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 9.6.0 Darwin Kernel Version 9.6.0: Mon Nov 24 17:39:01 PST 2008; root:xnu-1228.9.59~1/RELEASE_PPC Power Macintosh
Fingerprint Apple Mac OS X 10.5.6 (Leopard) (Darwin 9.6.0)
Class Apple | Mac OS X | 10.5.X | general purpose
SEQ(SP=F6-108%GCD=1-6%ISR=FF-10B%TI=RD%TS=3)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=5F-69%TG=80%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=5F-69%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=5F-69%TG=80%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=5F-69%TG=80%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=5F-69%TG=80%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=5F-69%TG=80%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=5F-69%TG=80%IPL=38%UN=0%RIPL=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=Y%T=5F-69%TG=80%CD=S)

# Darwin 9.6.0 Darwin Kernel Version 9.6.0: Mon Nov 24 17:37:00 PST 2008; root:xnu-1228.9.59~1/RELEASE_I386 i386
# 9.7.0 Darwin Kernel Version 9.7.0: Tue Mar 31 22:52:17 PDT 2009; root:xnu-1228.12.14~1/RELEASE_I386 i386
# Darwin 10.2.0 Darwin Kernel Version 10.2.0: Tue Nov  3 10:37:10 PST 2009; root:xnu-1486.2.11~1/RELEASE_I386 i386
Fingerprint Apple Mac OS X 10.5.6 10.6.2 (Leopard - Snow Leopard) (Darwin 9.6.0 - 10.2.0)
Class Apple | Mac OS X | 10.5.X | general purpose
Class Apple | Mac OS X | 10.6.X | general purpose
SEQ(SP=F5-10B%GCD=1-6%ISR=F8-10C%TI=RD%II=RI%TS=3)
OPS(O1=M3FD8NW2NNT11SLL|M3FD8NW3NNT11SLL%O2=M3FD8NW2NNT11SLL|M3FD8NW3NNT11SLL%O3=M3FD8NW2NNT11|M3FD8NW3NNT11%O4=M3FD8NW2NNT11SLL|M3FD8NW3NNT11SLL%O5=M3FD8NW2NNT11SLL|M3FD8NW3NNT11SLL%O6=M3FD8NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8NW2SLL|M3FD8NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin Kernel Version 9.7.0: Tue Mar 31 22:52:17 PDT 2009; root:xnu-1228.12.14~1/RELEASE_I386 i386
Fingerprint Apple Mac OS X 10.5.7 (Leopard) (Darwin 9.7.0)
Class Apple | Mac OS X | 10.5.X | general purpose
SEQ(SP=F4-10E%GCD=1-6%ISR=FD-10D%TI=RD%II=RI%TS=3)
OPS(O1=M556NW3NNT11SLL%O2=M556NW3NNT11SLL%O3=M556NW3NNT11%O4=M556NW3NNT11SLL%O5=M556NW3NNT11SLL%O6=M556NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M556NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 9.8.0 Darwin Kernel Version 9.8.0: Wed Jul 15 16:55:01 PDT 2009; root:xnu-1228.15.4~1/RELEASE_I386 i386
Fingerprint Apple Mac OS X 10.5.8 (Leopard) (Darwin 9.8.0)
Class Apple | Mac OS X | 10.5.X | general purpose
SEQ(SP=F7-101%GCD=1-6%ISR=FE-10A%TI=RD%II=RI%TS=4)
OPS(O1=M3FD8NW3NNT11SLL%O2=M3FD8NW3NNT11SLL%O3=M3FD8NW3NNT11%O4=M3FD8NW3NNT11SLL%O5=M3FD8NW3NNT11SLL%O6=M3FD8NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 9.8.0 Darwin Kernel Version 9.8.0: Wed Jul 15 16:55:01 PDT 2009; root:xnu-1228.15.4~1/RELEASE_I386 i386, 10.5.8
Fingerprint Apple Mac OS X 10.5.8 (Leopard) (Darwin 9.8.0)
Class Apple | Mac OS X | 10.5.X | general purpose
SEQ(SP=FF-109%GCD=1-6%ISR=FF-113%TI=RD%II=RI%TS=3)
OPS(O1=M57CNW3NNT11SLL%O2=M57CNW3NNT11SLL%O3=M57CNW3NNT11%O4=M57CNW3NNT11SLL%O5=M57CNW3NNT11SLL%O6=M57CNNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M57CNW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=7CE|29AF|6182|DEA7|E3A6%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 9.8.0 Darwin Kernel Version 9.8.0: Wed Jul 15 16:57:01 PDT 2009; root:xnu-1228.15.4~1/RELEASE_PPC Power Macintosh
Fingerprint Apple Mac OS X 10.5.8 (Leopard) (Darwin 9.8.0)
Class Apple | Mac OS X | 10.5.X | general purpose
SEQ(SP=EC-10A%GCD=1-6%ISR=FF-10D%TI=RD%CI=RD%II=RI%TS=3)
OPS(O1=M578NW3NNT11SLL%O2=M578NW3NNT11SLL%O3=M578NW3NNT11%O4=M578NW3NNT11SLL%O5=M578NW3NNT11SLL%O6=M578NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M578NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# PowerMac G5 running OS X Server 10.5 build 9A284
Fingerprint Apple Mac OS X Server 10.5 (Leopard) pre-release build 9A284
Class Apple | Mac OS X | 10.5.X | general purpose
SEQ(SP=D6-100%GCD=1-6%ISR=102-10C%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW5NNT11SLL%O2=M5B4NW5NNT11SLL%O3=M5B4NW5NNT11%O4=M5B4NW5NNT11SLL%O5=M5B4NW5NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW5SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 9.1.0 Darwin Kernel Version 9.1.0: Wed Oct 31 17:48:21 PDT 2007; root:xnu-1228.0.2~1/RELEASE_PPC Power Macintosh (Mac OS X Server 10.5.1)
Fingerprint Apple Mac OS X Server 10.5.1 (Leopard) (Darwin 9.1.0)
Class Apple | Mac OS X | 10.5.X | general purpose
SEQ(SP=FB-105%GCD=1-6%ISR=FD-10D%TI=RD%II=RI%TS=3|5)
OPS(O1=M57CNW2NNT11SLL%O2=M57CNW2NNT11SLL%O3=M57CNW2NNT11%O4=M57CNW2NNT11SLL%O5=M57CNW2NNT11SLL%O6=M57CNNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M57CNW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 10.0.0 Darwin Kernel Version 10.0.0: Fri Jul 31 22:47:34 PDT 2009; root:xnu-1456.1.25~1/RELEASE_I386 i386
Fingerprint Apple Mac OS X 10.6 (Snow Leopard) (Darwin 10.0.0)
Class Apple | Mac OS X | 10.6.X | general purpose
SEQ(SP=FC-10A%GCD=1-6%ISR=F7-111%TI=RD%CI=RD|RI%II=RI%TS=U)
OPS(O1=M3FD8SLL%O2=M3FD8SLL%O3=M3FD8%O4=M3FD8SLL%O5=M3FD8SLL%O6=M3FD8SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 10.0.0 Darwin Kernel Version 10.0.0: Fri Jul 31 22:47:34 PDT 2009; root:xnu-1456.1.25~1/RELEASE_I386 i386
Fingerprint Apple Mac OS X 10.6 (Snow Leopard) (Darwin 10.0.0)
Class Apple | Mac OS X | 10.6.X | general purpose
SEQ(TI=RI%CI=RD|RI%II=RI%SS=S%TS=3)
OPS(O1=M3FD8NW3NNT11SLL%O2=M3FD8NW3NNT11SLL%O3=M3FD8NW3NNT11%O4=M3FD8NW3NNT11SLL%O5=M3FD8NW3NNT11SLL%O6=M3FD8NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 10.2.0 Darwin Kernel Version 10.2.0: Tue Nov  3 10:35:19 PST 2009; root:xnu-1486.2.11~1/RELEASE_X86_64 x86_64
Fingerprint Apple Mac OS X 10.6.2 (Snow Leopard) (Darwin 10.2.0)
Class Apple | Mac OS X | 10.6.X | general purpose
SEQ(SP=FA-10A%GCD=1-6%ISR=102-10C%TI=RD|RI%II=RI%SS=O%TS=3)
OPS(O1=M5B4NW2NNT11SLL%O2=M5B4NW2NNT11SLL%O3=M5B4NW2NNT11%O4=M5B4NW2NNT11SLL%O5=M5B4NW2NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW2SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=O%A=Z%F=R%RD=0)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%RD=0)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 10.2.0 Darwin Kernel Version 10.2.0: Tue Nov 3 10:37:10 PST 2009; root:xnu-1486.2.11~1/RELEASE_I386 i386
Fingerprint Apple Mac OS X 10.6.2 (Snow Leopard) (Darwin 10.2.0)
Class Apple | Mac OS X | 10.6.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=FD-10F%TI=RD%CI=RD%II=RI%TS=3)
OPS(O1=MF78NW3NNT11SLL%O2=MF78NW3NNT11SLL%O3=MF78NW3NNT11%O4=MF78NW3NNT11SLL%O5=MF78NW3NNT11SLL%O6=MF78NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=MF78NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# 10.2.0 Darwin Kernel Version 10.2.0: Tue Nov  3 10:37:10 PST 2009; root:xnu-1486.2.11~1/RELEASE_I386 i386
Fingerprint Apple Mac OS X 10.6.2 (Snow Leopard) (Darwin 10.2.0)
Class Apple | Mac OS X | 10.6.X | general purpose
SEQ(SP=F7-109%GCD=1-6%ISR=F1-111%TI=RD%CI=RI%II=I%TS=3)
OPS(O1=M218NW3NNT11SLL%O2=M218NW3NNT11SLL%O3=M218NW3NNT11%O4=M218NW3NNT11SLL%O5=M218NW3NNT11SLL%O6=M218NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M218NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# Darwin 10.2.0 Darwin Kernel Version 10.2.0: Tue Nov  3 10:37:10 PST 2009; root:xnu-1486.2.11~1/RELEASE_I386 i386
# Darwin 10.4.0 Darwin Kernel Version 10.4.0: Fri Apr 23 18:28:53 PDT 2010; root:xnu-1504.7.4~1/RELEASE_I386 i386
Fingerprint Apple Mac OS X 10.6.2 - 10.6.4 (Snow Leopard) (Darwin 10.2.0 - 10.4.0)
Class Apple | Mac OS X | 10.6.X | general purpose
SEQ(SP=E7-105%GCD=1-6%ISR=F5-10D%TI=RD%II=RI%TS=U)
OPS(O1=M5B4SLL%O2=M5B4SLL%O3=M5B4%O4=M5B4SLL%O5=M5B4SLL%O6=M5B4SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 10.3.0 Darwin Kernel Version 10.3.0: Fri Feb 26 11:58:09 PST 2010; root:xnu-1504.3.12~1/RELEASE_I386 i386
Fingerprint Apple Mac OS X 10.6.3 (Snow Leopard) (Darwin 10.3.0)
Class Apple | Mac OS X | 10.6.X | general purpose
SEQ(SP=EB-10B%GCD=1-6%ISR=EE-10C%TI=RD%CI=RI%II=RI%TS=3)
OPS(O1=M5ACNW3NNT11SLL%O2=M5ACNW3NNT11SLL%O3=M5ACNW3NNT11%O4=M5ACNW3NNT11SLL%O5=M5ACNW3NNT11SLL%O6=M5ACNNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5ACNW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=37EE%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Darwin 10.4.0 Darwin Kernel Version 10.4.0: Fri Apr 23 18:28:53 PDT 2010; root:xnu-1504.7.4~1/RELEASE_I386 i386
Fingerprint Apple Mac OS X 10.6.4 (Snow Leopard) (Darwin 10.4.0)
Class Apple | Mac OS X | 10.6.X | general purpose
SEQ(SP=102-10C%GCD=1-6%ISR=105-10F%TI=RD%CI=RD%II=RI%TS=3)
OPS(O1=M3FD8NW3NNT11SLL%O2=M3FD8NW3NNT11SLL%O3=M3FD8NW3NNT11%O4=M3FD8NW3NNT11SLL%O5=M3FD8NW3NNT11SLL%O6=M3FD8NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M3FD8NW3NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Mac OS 8.6 on PPC
# Mac OS 8.1 running on Basilisk-II
# Mac OS 8.6 on PowerPC 8600/250
Fingerprint Apple Mac OS 8.1 - 8.6
Class Apple | Mac OS | 8.X | general purpose
SEQ(SP=0-2D%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=95-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4W0L%O2=M578W0L%O3=M280W0L%O4=M218W0L%O5=M218W0L%O6=M109)
WIN(W1=4470%W2=4718%W3=4600%W4=4518%W5=4518%W6=455B)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=4470%O=M5B4W0L%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=FA-104%TG=FF%W=455B%S=O%A=S+%F=AS%O=M109W0L%RD=0%Q=)
T4(R=Y%DF=Y%T=21-3D%TG=40%W=0%S=A%A=Z%F=R%O=%RD=2AB5E05E%Q=)
T5(R=Y%DF=Y%T=1F-38%TG=20|40%W=0%S=Z%A=S+%F=AR%O=%RD=896A56EB%Q=)
T6(R=Y%DF=Y%T=1E-3D%TG=40%W=0%S=A%A=Z%F=R%O=%RD=8829FB5F%Q=)
T7(R=Y%DF=Y%T=1E-3D%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=896A56EB%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# Mac OS 9.0.4 on SheepShaver (on Red Hat)
# Airport Extreme 07 with software version 7.2.1
# Mac OS 9.2
Fingerprint Apple Mac OS 9.0.4 - 9.2
Class Apple | Mac OS | 9.X | general purpose
SEQ(SP=4A-A0%GCD=1-6%ISR=9A-A8%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4W0NNNT11%O2=M578W0NNNT11%O3=M280W0NNNT11%O4=M218W0NNNT11%O5=M218W0NNNT11%O6=M109NNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=8000%O=M5B4W0N%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=E44A4E43%Q=)
T3(R=Y%DF=Y%T=FA-104%TG=FF%W=8000%S=O%A=S+%F=AS%O=M109W0NNNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=E44A4E43%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=EA6C967D%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=EA6C967D%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# Mac OS 9.2
Fingerprint Apple Mac OS 9.2
Class Apple | Mac OS | 9.X | general purpose
SEQ(R=N)
OPS(O1=|M5B4W0NNNT11%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0|8000%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=0%O=%CC=N%Q=U)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O|Z%A=S+%F=AR|AS%RD=0|BD1AB510%Q=)
T2(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=EA6C967D%Q=)
T3(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=EA6C967D%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=EA6C967D%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=EA6C967D%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# Apple Airport Express embedded
Fingerprint Apple AirPort Express WAP (NetBSD)
Class Apple | NetBSD | 4.X | general purpose
SEQ(SP=C6-E4%GCD=1-6%ISR=D7-E1%TI=I%CI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT01SNN%O2=M5B4NW0NNT01SNN%O3=M5B4NW0NNT01%O4=M5B4NW0NNT01SNN%O5=M5B4NW0NNT01SNN%O6=M5B4NNT01SNN)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M5B4NW0SNN%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=8000%S=O%A=S+%F=AS%O=M5B4NW0NNT01SNN%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Apple AirPort Extreme (802.11a/b/g/draft-n), Apple P/N A1143, S/W ver 7.0
# Apple Airport Extreme 7.1.1
# NetBSD 4.99.4 NetBSD 4.99.4 (E4500) #1: Tue Nov 28 10:25:20 EST 2006 i386
# Apple Airport Extreme base station 802.11n
# Apple Time Capsule NAS device
Fingerprint Apple AirPort Extreme WAP or Time Capsule NAS device (NetBSD 4.99)
Class Apple | NetBSD | 4.X | general purpose
SEQ(SP=BF-DA%GCD=1-6%ISR=D6-E1%TI=I%CI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT01SNN%O2=M5B4NW0NNT01SNN%O3=M5B4NW0NNT01%O4=M5B4NW0NNT01SNN%O5=M5B4NW0NNT01SNN%O6=M5B4NNT01SNN)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M5B4NW0SNN%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=8000%S=O%A=S+%F=AS%O=M5B4NW0NNT01SNN%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Arcor-Easy Box A300 WLAN, Firmware 1.00.624
Fingerprint Arcor-Easy Box A 300 WLAN wireless ADSL router
Class Arcor | embedded || broadband router
SEQ(SP=F-1D%GCD=1-6%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=5000%W2=5000%W3=5000%W4=5000%W5=5000%W6=5000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=5000%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=5000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=O|S|Y%T=3B-45%TG=40%CD=Z)

# Areca 1222 RAID controller.  It's version 1.47.
Fingerprint Areca ARC-1222 RAID controller
Class Areca | embedded || storage-misc
SEQ(SP=BE-C8%GCD=1-6%ISR=CD-D7%TI=I%CI=I%TS=U)
OPS(O1=M5A6%O2=M5A6%O3=M5A6%O4=M5A6%O5=M5A6%O6=M5A6)
WIN(W1=5A6%W2=5A6%W3=5A6%W4=5A6%W5=5A6%W6=5A6)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5A6%O=M5A6%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=400%S=A%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=5A6%S=O%A=S+%F=AS%O=M5A6%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=400%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=400%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=400%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=400%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(R=N)

# Argosy Research HD363N Network HDD
Fingerprint Argosy HD363N NAS device
Class Argosy | embedded || storage-misc
SEQ(SP=0-1D%GCD=1-6|6FC|DF8|14F4|1BF0|22EC%ISR=6C-76%II=I%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=1B-25%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=N%T=1B-25%TG=20%CD=S)

# External Hard Disk Argosy HD354N
# Freecom Network Drive. Firmware NAS2891-009T3 LOADER 3.2
# Iomega Home Network Hard Drive 500GB
Fingerprint Asmax NAS-USB print server; or Argosy HD354N, Freecom Network Drive, or Iomega Home Media Network Hard Drive NAS device
Class Argosy | embedded || storage-misc
Class Asmax | embedded || print server
Class Freecom | embedded || storage-misc
Class Iomega | embedded || storage-misc
SEQ(SP=0-9D%GCD=1-6%ISR=78-99%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=1B-25%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=1B-25%TG=20%CD=S)

# Develop INEO+ 203
# Konica Minolta C203 PS Multi-function printer.
# Konica Minaolta magicolor 5670 EN
# Arris TM602G, Firmware Revision:      6.1.77
# ARRIS DOCSIS 2.0 / PacketCable 1.0 Touchstone Telephony Modem HW_REV: 32
Fingerprint Arris TM602G cable modem, Develop ineo+203, or Konica Minolta C203 or MagiColor 5670 printer
Class Arris | embedded || broadband router
Class Develop | embedded || printer
Class Konica Minolta | embedded || printer
SEQ(SP=FE-10A%GCD=1-6%ISR=FC-10E%TI=I%CI=I%II=I%SS=S%TS=8)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Arris Cadant C3 cable modem termination system, Application image: 4.4.0.59, Apr 24 2007, 15:27:54, BootRom version 4.2.0.2, VxWorks5.4.2
Fingerprint Arris Cadant C3 cable modem terminator (VxWorks 5.4.2)
Class Arris | VxWorks | 5.X | router
SEQ(SP=96-A0%GCD=1-6%ISR=9C-A6%TI=I%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# ArubaOS (MODEL: Aruba200-US), Version 3.3.2.5
Fingerprint Aruba 200 wireless LAN controller (ArubaOS 3.3.2.5)
Class Aruba | ArubaOS | 3.X | remote management
SEQ(SP=101-10B%GCD=1-6%ISR=103-10D%TI=Z%II=I%TS=7)
OPS(O1=M4F6ST11NW0%O2=M4F6ST11NW0%O3=M4F6NNT11NW0%O4=M4F6ST11NW0%O5=M4F6ST11NW0%O6=M4F6ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=16D0%O=M4F6NNSNW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# ArubaOS (MODEL: Aruba6000-US), Version 3.3.2.5
# Aruba 3400, ArubaOS 3.3.2.15
Fingerprint Aruba 3400 or 6000 wireless LAN controller (ArubaOS 3.3.2)
Class Aruba | ArubaOS | 3.X | remote management
SEQ(SP=F7-10D%GCD=1-6%ISR=107-111%TI=Z%CI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW2%O2=M5B4ST11NW2%O3=M5B4NNT11NW2%O4=M5B4ST11NW2%O5=M5B4ST11NW2%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW2%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# ARUBA Wireless Networks Model 800
# Aruba Mobility Controller A800, Software: ArubaOS 3.3.1.16 (Linux-based)
Fingerprint Aruba A800 wireless LAN switch
Class Aruba | embedded || switch
SEQ(SP=100-10A%GCD=1-6%ISR=107-111%TI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# DI-524, HW Rev: G2
# ASUS  RT-N11 EZ Wireless N Router
Fingerprint ASUS RT-N11 EZ or D-Link DI-524 WAP
Class Asus | embedded || WAP
Class D-Link | embedded || WAP
SEQ(SP=0-1D%GCD=14|28|3C|50|64%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Asus WL-500gp home router
Fingerprint Asus WL-500gP wireless broadband router
Class Asus | embedded || WAP
SEQ(R=N)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(R=N)

# router Asus RT-N16
Fingerprint Asus RT-N16 WAP (Linux 2.6)
Class Asus | Linux | 2.6.X | WAP
SEQ(CI=Z%II=I)
OPS(R=N)
WIN(R=N)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW2%CC=N%Q=)
T1(R=N)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Linux 2.6.22 #153 Thu Sep 2 11:07:59 CST 2010 mips unknown, Asus RT-N16 wireless switch firmware version Version:: 1.0.1.9
Fingerprint Asus RT-N16 WAP (Linux 2.6.22)
Class Asus | Linux | 2.6.X | WAP
SEQ(SP=C3-CD%GCD=1-6%ISR=EA-F4%TI=Z%CI=Z%II=I%TS=7|8)
OPS(O1=M5B4ST11NW2%O2=M5B4ST11NW2%O3=M5B4NNT11NW2%O4=M5B4ST11NW2%O5=M5B4ST11NW2%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW2%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# AT&T NetGate SG8100 Router
Fingerprint AT&T NetGate SG8100 router
Class AT&T | embedded || router
SEQ(SP=C5-CF%GCD=1-6%ISR=C6-D0%TI=Z%II=I%TS=7)
OPS(O1=M507ST11NW0%O2=M507ST11NW0%O3=M507NNT11NW0%O4=M507ST11NW0%O5=M507ST11NW0%O6=M507ST11)
WIN(W1=13EC%W2=13EC%W3=13EC%W4=13EC%W5=13EC%W6=13EC)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=141C%O=M507NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=13EC%S=O%A=S+%F=AS%O=M507ST11NW0%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# AT&T 3G Microcell
Fingerprint AT&T 3G MicroCell WAP
Class AT&T | embedded || WAP
SEQ(SP=C6-D0%GCD=1-6%ISR=C8-D2%TI=I%CI=Z%II=I%SS=O%TS=A)
OPS(O1=M5ACST11NW1%O2=M5ACST11NW1%O3=M5ACNNT11NW1%O4=M5ACST11NW1%O5=M5ACST11NW1%O6=M5ACST11)
WIN(W1=1680%W2=1680%W3=1680%W4=1680%W5=1680%W6=1680)
ECN(R=Y%DF=N%T=3A-44%TG=40%W=16B0%O=M5ACNNSNW1%CC=N%Q=)
T1(R=Y%DF=N%T=3A-44%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=3A-44%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Atari TT 030 running Atari System V Release 4.0 (1.0), UniSoft UNIX System V Release 4.0
Fingerprint Atari Unix System V Release 4.0
Class Atari | Unix | SVR4 | general purpose
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=1000%O=M400%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# ATCOM AT-320 Ethernet Phone. Uses the PalmMicro PA168S chipset. H.323 firmware of version 1.53 from PalmMicro.
Fingerprint Atcom AT-320 VoIP phone
Class Atcom | embedded || VoIP phone
SEQ(SP=F4-102%GCD=1-6%ISR=FD-117%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=514%W2=514%W3=514%W4=514%W5=514%W6=514)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=514%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=7B-85%TG=80%W=514%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=7B-85%TG=80%CD=Z)

# AudioCodes Mediant 1000
Fingerprint AudioCodes Mediant 1000 VoIP gateway
Class AudioCodes | embedded || VoIP adapter
SEQ(SP=C-16%GCD=1E848|3D090|5B8D8|7A120|98968%ISR=9F-A9%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW1NNSNNT11%O2=M578NW1NNSNNT11%O3=M280NW1NNT11%O4=M5B4NW1NNSNNT11%O5=M218NW1NNSNNT11%O6=M109NNSNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW1NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Audiocodes MP-118-4FXS4FXO VoIP Gate
# Audiocodes MP-114 FXO
Fingerprint Audiocodes MP-114 or MP-118 VoIP gateway
Class AudioCodes | embedded || VoIP adapter
SEQ(SP=C-16%GCD=1E848|3D090|5B8D8|7A120|98968%ISR=9F-A9%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=209D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2238%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Avaya P130 workgroup switch, SW version 2.11.3
Fingerprint Avaya P130 workgroup switch
Class Avaya | embedded || switch
SEQ(R=N)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=Z%A=S+%F=AR%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Fingerprint Avaya Inc. - P330 Stackable Switch, SW version 4.1.6
Fingerprint Avaya P330 Stackable Switch
Class Avaya | embedded || switch
SEQ(SP=F-11%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=9B-9D%TI=I%II=I%SS=S%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=1000%O=%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Avaya Cajun Switch Agent v5.4.2 on P580 model
Fingerprint Avaya P580 switch running Cajun Switch Agent v5.4.2
Class Avaya | embedded || switch
SEQ(SP=0-92%GCD=9C4|1388|1D4C|2710|30D4|3A98|61A8|C350|124F8|186A0|1E848|249F0%ISR=8B-BB%TI=I%II=RI%SS=O|S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=19-23%TG=20%W=400%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=D33|90CE|98BF|DA0A|FBF9%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=19-23%TG=20%CD=S)

# Lucent Technologies Cajun Switch Agent v5.3.2 on P880 model
Fingerprint Avaya P880 switch running Cajun Switch Agent v5.3.2
Class Avaya | embedded || switch
SEQ(SP=0-95%GCD=9C4|1388|1D4C|2710|30D4|3A98%ISR=8B-BB%TI=I%II=RI%SS=O|S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=1A-24%TG=20%W=400%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=1A-24%TG=20%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=1A-24%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=1A-24%TG=20%IPL=38%UN=293|977C|9A49|A984|F0E2%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=1A-24%TG=20%CD=S)

Fingerprint Avaya Intuity Audix Multimedia Messaging System
Class Avaya | embedded || telecom-misc
SEQ(SP=A3-BF%GCD=1-6%ISR=B6-BC%TI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M280%O4=M400%O5=%O6=M109)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M400%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Avaya G360 Media Gateway running software version 26.36.0
Fingerprint Avaya G350 Media Gateway (VoIP gateway)
Class Avaya | embedded || VoIP adapter
SEQ(SP=94-9E%GCD=1-6%ISR=9B-A5%TI=I%II=RI%SS=O|S%TS=U)
OPS(O1=M550%O2=M550%O3=M550%O4=M550%O5=M550%O6=M550)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M550%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Avaya IP Office IP403
Fingerprint Avaya Office IP403 VoIP gateway
Class Avaya | embedded || VoIP adapter
SEQ(SP=11-2D%GCD=10000|20000|30000|40000|50000%ISR=CA-D4%TI=I%II=RI%SS=O%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=1111%W2=1111%W3=1111%W4=1111%W5=1111%W6=1111)
ECN(R=N)
T1(R=Y%DF=N%T=5E-68%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=5E-68%TG=80%W=1111%S=Z%A=S+%F=R%O=%RD=0%Q=)
T6(R=Y%DF=N%T=5E-68%TG=80%W=1111%S=Z%A=S+%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=5E-68%TG=80%W=1111%S=Z%A=S+%F=R%O=%RD=0%Q=)
U1(DF=N%T=5E-68%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=23-3D%TG=40%CD=S)

# Avaya IP500, Firmware 4.1 (9)
# avaya IP Office 500 . mixed-type PABX (analog + voip)
Fingerprint Avaya Office IP500 VoIP gateway
Class Avaya | embedded || VoIP adapter
SEQ(SP=0-13%GCD=10000|20000|30000|40000|50000|650000|CA0000|12F0000|1940000|1F90000%ISR=CB-D5%TI=I%II=RI%SS=O|S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=1111%W2=1111%W3=1111%W4=1111%W5=1111%W6=1111)
ECN(R=Y%DF=N%T=5E-68%TG=80%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=5E-68%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=5E-68%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=5E-68%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=5E-68%TG=80%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=5E-68%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=5E-68%TG=80%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=5E-68%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=5E-68%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=20-3C%TG=40%CD=S)

# Avaya Communication Manager for the Avaya G350. It runs a customized Linux: Red Hat Enterprise Linux ES release 4 (Nahant) Kernel 2.6.11-AV18 on an i686
Fingerprint Avaya Communication Manager (Linux 2.6.11)
Class Avaya | Linux | 2.6.X | telecom-misc
SEQ(SP=C3-CD%GCD=1-6%ISR=C3-CD%TI=Z%II=I%TS=U)
OPS(O1=M550NW2%O2=M550NW2%O3=M550NW2%O4=M550NW2%O5=M550NW2%O6=M550)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M550NW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Avaya G700 Telephony Media Gateway
# Konica Minolta 7145 printer
# Sun(tm) Advanced Lights Out Manager 1.5.2
Fingerprint Avaya G700 Telephony Media Gateway or Sun Advanced Lights Out Maganer 1.5.2 (VxWorks)
Class Avaya | VxWorks || VoIP adapter
Class Sun | VxWorks || remote management
SEQ(SP=18-1C%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=9D-A2%TI=I%II=I%SS=S%TS=1)
OPS(O1=M200NW0NNT11%O2=M200NW0NNT11%O3=M200NW0NNT11%O4=M200NW0NNT11%O5=M200NW0NNT11%O6=M200NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M200NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# AVM FRITZ!Box Fon 7170
Fingerprint AVM FRITZ!Box Fon 7170 ADSL modem
Class AVM | embedded || broadband router
SEQ(SP=FE-10E%GCD=1-6%ISR=108-112%TI=Z%II=RI%TS=7)
OPS(O1=M5A6ST11NW1%O2=M578ST11NW1%O3=M280NNT11NW1%O4=M22CST11NW1%O5=M218ST11NW1%O6=M109ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5A6NNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=N)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Netgear router DG834GT Firmware: V1.01.28
# AVM Fritz!Box FON WLAN 7050
# LINKSYS WAG200G Firmware Version: 1.00.09
# Linksys WAG200G, Firmware Version: 1.01.06
# Linksys WAG200G firmware: 1.01.05
Fingerprint AVM FRITZ!Box FON WLAN 7050, Linksys WAG200G, or Netgear DG834GT wireless broadband router
Class AVM | embedded || WAP
Class Netgear | embedded || WAP
Class Linksys | embedded || WAP
SEQ(SP=B6-CE%GCD=1-6%ISR=C7-D3%TI=Z%II=I%TS=7|8|9)
OPS(O1=NNT11|M5B4ST11NW0%O2=NNT11|M5B4ST11NW0%O3=NNT11|M5B4NNT11NW0%O4=NNT11|M5B4ST11NW0%O5=NNT11|M5B4ST11NW0%O6=NNT11|M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45|FA-104%TG=40|FF%W=16D0%O=|M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45|FA-104%TG=40|FF%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45|FA-104%TG=40|FF%W=16A0%S=O%A=O|S+%F=A|AS%O=NNT11|M5B4ST11NW0%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# AVM Fritzbox Fon WLAN 7170
Fingerprint AVM FRITZ!Box FON WLAN 7170 WAP
Class AVM | embedded || WAP
SEQ(SP=BF-D1%GCD=1-6%ISR=C0-D8%TI=Z%II=I%TS=7)
OPS(O1=M578ST11NW1%O2=M578ST11NW1%O3=M578NNT11NW1%O4=M578ST11NW1%O5=M578ST11NW1%O6=M578ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M578NNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Avocent SwitchView IP 1010
Fingerprint Avocent SwitchView 1010 remote access device
Class Avocent | embedded || remote management
SEQ(SP=CD-D7%GCD=1-6%ISR=D9-E3%TI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW2NNT01%O2=M5B4NW2NNT01%O3=M5B4NW2NNT01%O4=M5B4NW2NNT01%O5=M5B4NW2NNT01%O6=M5B4NNT01)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW2NNT01%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Avocent DSR1030 IP KVM
Fingerprint Avocent DSR1030 KVM over IP switch
Class Avocent | embedded || specialized
SEQ(SP=C4-CE%GCD=1-6%ISR=C8-D2%TI=Z%II=I%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%S=O%A=S+%F=AS%O=M5B4NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# AV-TECH Digital Video Recorder (device connected to a surveillance camera), AVT AVC 773W 4CH Network DVR
Fingerprint AVtech AVC 773W digital video recorder
Class AVtech | embedded || webcam
SEQ(SP=C-1E%GCD=1-6%ISR=1B-6F%TI=I%II=RI%SS=O|S%TS=U)
OPS(O1=M59E%O2=M578%O3=M280%O4=M59E%O5=M218%O6=M109)
WIN(W1=FAF0%W2=FAF0%W3=FAF0%W4=FAF0%W5=FAF0%W6=FAF0)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=FAF0%O=M59E%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=FA-104%TG=FF%W=FAF0%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=FAF0%S=A+%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=FAF0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=FAF0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=FAF0%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=24-40%TG=40%CD=S)

# Axcient Uptiva backup appliance. On boot-up the system flashes "AxOS".
Fingerprint Axceint Uptiva backup appliance
Class Axcient | embedded || storage-misc
SEQ(SP=BB-C5%GCD=1-6%ISR=C5-CF%TI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW7%O2=M5B4ST11NW7%O3=M5B4NNT11NW7%O4=M5B4ST11NW7%O5=M5B4ST11NW7%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW7%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW7%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Axis 70U Network document server
Fingerprint AXIS 70U Network Document Server
Class AXIS | embedded || specialized
SEQ(SP=0-16%GCD=40000|80000|C0000|100000|140000%ISR=0-9D%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5AC%O2=M578%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=4410%W2=4410%W3=4410%W4=4410%W5=4410%W6=4410)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0|4410%O=M5AC%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=4410%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4410%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Axis 207W Network Camera
Fingerprint AXIS 207W Network Camera
Class AXIS | embedded || webcam
SEQ(SP=BD-E3%GCD=1-6%ISR=CB-DF%TI=Z%CI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW1%O2=M5B4ST11NW1%O3=M5B4NNT11NW1%O4=M5B4ST11NW1%O5=M5B4ST11NW1%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW1%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW1%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Described as axis 2100 network cam on its webpage (port 80).
Fingerprint AXIS 2100 Network Camera
Class AXIS | embedded || webcam
SEQ(SP=100-10A%GCD=1-6%ISR=104-10E%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=3FE0%W2=3FE0%W3=3FE0%W4=3FE0%W5=3FE0%W6=3FE0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3FE0%O=M5B4%CC=S%Q=RU)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=3FE0%S=O%A=O|S+%F=ASF%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Axis 2100 Network Camera
Fingerprint AXIS 2100 Network Camera
Class AXIS | embedded || webcam
SEQ(SP=FB-108%GCD=1-6%ISR=102-10F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=3FE0%W2=3FE0%W3=3FE0%W4=3FE0%W5=3FE0%W6=3FE0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3FE0%O=M5B4%CC=N%Q=U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=3FE0%S=O%A=S+%F=ASF%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Axis 211 Network Camera
Fingerprint AXIS 211A Network Camera (Linux 2.6)
Class AXIS | Linux | 2.6.X | webcam
SEQ(CI=Z%II=I)
OPS(R=N)
WIN(R=N)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=N)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Axis 211A, 2.6.20
Fingerprint AXIS 211A Network Camera (Linux 2.6.20)
Class AXIS | Linux | 2.6.X | webcam
SEQ(CI=Z%II=I)
OPS(R=N)
WIN(R=N)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW1%CC=N%Q=)
T1(R=N)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# AXIS 207 network camera (Linux version 2.6.16 (fabrice@ant-4) (gcc version 3.4.4) #1 Mon Aug 28 15:57:57 CEST 2006)
# AXIS 241Q Video Server [firmware rev 4.40]
# AXIS 241Q video encoder.
# Linux 2.6.17 #2 Tue Apr 8 09:46:29 CEST 2008 cris, Axis 232D+ Network Dome Camera RELEASE="4.41"
# AXIS 221 Network Camera 4.45
# htc sapphire 32a running android 2.2 froyo
Fingerprint AXIS Network Camera (207, 221, or 232D+) or 241Q Video Server (Linux 2.6.16 - 2.6.17)
Class AXIS | Linux | 2.6.X | webcam
SEQ(SP=BD-E3%GCD=1-6%ISR=CB-DF%TI=Z%CI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW1%O2=M5B4ST11NW1%O3=M5B4NNT11NW1%O4=M5B4ST11NW1%O5=M5B4ST11NW1%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW1%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW1%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Barracuda Networks v3.5.05.003 (2006-05-12 15:59:59) Model 400
Fingerprint Barracuda Spam Firewall model 400
Class Barracuda Networks | embedded || firewall
SEQ(SP=FF-109%GCD=1-6%ISR=106-110%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=E000%W2=E000%W3=E000%W4=E000%W5=E000%W6=E000)
ECN(R=Y%DF=Y%T=34-3E%TG=40%W=E000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=34-3E%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=34-3E%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=34-3E%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=34-3E%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=34-3E%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=34-3E%TG=40%CD=S)

# Barracuda 340 Load Balancer
Fingerprint Barracuda 340 load balancer
Class Barracuda Networks | embedded || load balancer
SEQ(SP=C5-CF%GCD=1-6%ISR=C9-D3%TI=Z%CI=Z%II=I%TS=7)
OPS(O1=M5ACST11NW0%O2=M5ACST11NW0%O3=M5ACNNT11NW0%O4=M5ACST11NW0%O5=M5ACST11NW0%O6=M5ACST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=N%T=3D%TG=40%W=16D0%O=M5ACNNSNW0%CC=Y%Q=)
T1(R=Y%DF=N%T=3D%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3D%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5ACST11NW0%RD=0%Q=)
T4(R=Y%DF=N%T=3D%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3D%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3D%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3D%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3D%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3D%TG=40%CD=S)

# Basler AG ruL2098-10gc GiGE Vision Ethernet Camera
Fingerprint Basler ruL 2098-10gc GigE Vision Ethernet camera
Class Basler | embedded || webcam
SEQ(SP=0-19%GCD=1-6|174|17E|2E8|2FC|45C|47A|5D0|5F8|744|776%ISR=5A-64%TI=I%II=I%SS=S%TS=U)
OPS(O1=M200%O2=M200%O3=M200%O4=M200%O5=M200%O6=M109)
WIN(W1=200%W2=200%W3=200%W4=200%W5=200%W6=200)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=200%O=M200%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=FA-104%TG=FF%W=200%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=200%S=A+%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=200%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=200%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=200%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=24A2|301D|3BB6|477C|5365%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=24-39%TG=40%CD=S)

# Xerox DocuPrint N32
# Bay Networks Terminal Annex server. Converts serial connection to ethernet.
# ANNEX RA4000 Terminal server
Fingerprint Bay Networks Annex Ethernet-to-serial bridge or Xerox DocuPrint N32 printer
Class Bay Networks | embedded || bridge
Class Xerox | embedded || printer
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%II=I%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# BayStack 450-24T, Versions: HW:RevD  FW:V1.47 SW:v3.1.0.22  ISVN:1
Fingerprint Bay Networks BayStack 450 switch (software version 3.1.0.22)
Class Bay Networks | embedded || switch
SEQ(SP=20-BA%GCD=FA|1F4|2EE|3E8|4E2%ISR=8A-C0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0|400%O=|M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O|Z%A=O|S+%F=AR|AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0|400%S=O|Z%A=O|S+%F=AR|AS%O=|M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Bay Networks Switch BayStack 450-24T [FW:V1.48 SW:v4.2.0.16]
Fingerprint Bay Networks BayStack 450 switch (software version 4.2.0.16)
Class Bay Networks | embedded || switch
SEQ(SP=63-E3%GCD=1-6%ISR=8A-B0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=400%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0|400%S=O|Z%A=O|S+%F=AR|AS%O=|M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# BeaconMedaes http://www.beaconmedaes.com, PIPELINE ALARMS, TOTALALERT Medical Gas Alarm, MedPlus TotalAlert Alarm Network
Fingerprint BeaconMedaes TotalAlert medical gas alarm
Class BeaconMedaes | embedded || specialized
SEQ(SP=0-16%GCD=FA7F|1F4FE|2EF7D|3E9FC|4E47B%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B0%O2=M5B0%O3=M5B0%O4=M5B0%O5=M5B0%O6=M5B0)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2000%O=M5B0%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=19-23%TG=20%CD=S)

# BECK IPC Chip http://www.beck-ipc.com/en/products/index.asp
Fingerprint BECK IPC@CHIP
Class BECK | embedded || specialized
SEQ(SP=21-2B%GCD=61A8|C350|124F8|186A0|1E848%ISR=9F-A9%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNT11%O2=M578NW0NNT11%O3=M280NW0NNT11%O4=M5B4NW0NNT11%O5=M218NW0NNT11%O6=M109NNT11)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=209D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2238%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=209D%S=O%A=S+%F=AS%O=M109NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Belkin F1DE101N aka digitalv6 Kaveman IPKVM, running Kaveman firmware 2.5-041224.1742
Fingerprint Belkin F1DR101N KVM console
Class Belkin | embedded || terminal
SEQ(SP=3A-44%GCD=9C4|1388|1D4C|2710|30D4%ISR=9F-A9%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=209D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2238%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=209D%S=O%A=S+%F=AS%O=M109NW0NNSNNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Belkin Woreless Router F5D8233-4v3(01) Firmware 3.01.17 (Nov 29 2007 17:48:13)
Fingerprint Belkin F5D8233 WAP
Class Belkin | embedded || WAP
SEQ(SP=10-1C%GCD=1-6%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=1770%W2=1770%W3=1770%W4=1770%W5=1770%W6=1770)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1770%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1770%S=O%A=O|S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# Belkin advanced WAP F6D4630-4 v1
Fingerprint Belkin F6D4630-4 v1 WAP
Class Belkin | embedded || WAP
SEQ(SP=0-1D%GCD=1-6|64|C8|12C|190|1F4%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=1770%W2=1770%W3=1770%W4=1770%W5=1770%W6=1770)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1770%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1770%S=O%A=O|S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N|Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N|S|Y%T=3B-45%TG=40%CD=Z)

# Belkin N 150 wireless router, firmware version F6D4230-4_WW_1.00.03
Fingerprint Belkin N150 WAP
Class Belkin | embedded || WAP
SEQ(SP=0-5%GCD=80|100|180|200|280%ISR=4E-58%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M564%O3=M5B4%O4=M5B4%O5=M204%O6=MF5)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=16D0%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# Belkin Wireless Pre-N Router
# Firmware Version 1.01.03; Boot Version 2.01.08
Fingerprint Belkin Wireless Pre-N Router
Class Belkin | embedded || WAP
SEQ(SP=C2-CC%GCD=1-6%ISR=C9-D3%TI=Z%II=I%TS=7)
OPS(O1=%O2=NNT11|M5B4ST11NW0%O3=NNT11|M5B4NNT11NW0%O4=NNT11|M5B4ST11NW0%O5=NNT11|M5B4ST11NW0%O6=NNT11|M5B4ST11)
WIN(W1=16D0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=|M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O%F=A%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=O|S+%F=A|AS%O=NNT11|M5B4ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Livebox Inventel  v5.05.5-fr ADSL firmware A2pBT009.d16m-1
# Livebox home ADSL router (wifi enabled). Manufactured by Inventel.
# US Robotics SureConnect 9105
# Broadcom MIPS32 based router (Belkin F5D7633uk4A) (Linux version 2.4.17 (root@JoshuaNotebook) (gcc version 3.1) #13 Wed Jul 20 10:22:55 CST 2005)
# ZXDSL 831 router, Linux version 2.4.17 (leon_zhou@localhost.localdomain) (gcc version 3.1) #1 Fri Feb 4 09:43:54 CST 2005
# Sinus 1054 DSL router, Boot Code Version: 1.0.37-5.6, Software Version: 2.1
# Belkin f5d7633-4 wireless router
# Sinus 1054 DSL (WLAN Router with built-in DSL-modem), Boot Code Version: 1.0.37-5.6, ADSL Modem Code Version: BA09b6e
Fingerprint Belkin F5D7633, Inventel Livebox, or T-Sinus 1054 wireless broadband router; or USRobotics SureConnect 9105 or ZTE ZXDSL 831 ADSL modem
Class Belkin | Linux | 2.4.X | WAP
Class Inventel | embedded || WAP
Class Telekom | embedded || WAP
Class USRobotics | embedded || broadband router
Class ZTE | Linux | 2.4.X | broadband router
SEQ(SP=B0-CF%GCD=1-6%ISR=B5-D4%TI=Z%II=I%TS=8)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Plan 9 from Bell Labs (4th edition)
Fingerprint Bell Labs Plan 9 4th edition
Class Bell Labs | Plan 9 | 4th edition | general purpose
SEQ(SP=100-10C%GCD=1-6%ISR=104-10E%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4W1N%O2=M5B4W1N%O3=M5B4W1N%O4=M5B4W1N%O5=M5B4W1N%O6=M5B4)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=FFFF%O=M5B4W1N%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=FFFF%S=O%A=S+%F=AS%O=M5B4W1N%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Billion Electric ADSL VoIP Router Modem (Model BiPAC 7402VGP)
Fingerprint Billion 7402VGP DSL router
Class Billion | embedded || broadband router
SEQ(R=N)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=N)
T2(R=Y%DF=Y%T=7B-85%TG=80%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=Z%F=R%O=%RD=0%Q=)
U1(DF=N%T=96-A0%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Billion 7404VGO-M DSL Router [Firmware 5.52d]
# Zoom ADSL X6 (5590 series)
Fingerprint Billion 7404VGO-M or Zoom X6 DSL router
Class Billion | embedded || broadband router
Class Zoom | embedded || broadband router
SEQ(SP=74-80%GCD=1-6%ISR=84-8E%TI=I%CI=I%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=7B-85%TG=80%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=Z%F=R%O=%RD=0%Q=)
U1(DF=N%T=96-A0%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Billion 7404VGPM
Fingerprint Billion 7404VGP-M ADSL router
Class Billion | embedded || broadband router
SEQ(SP=C7-D1%GCD=1-6%ISR=CB-D5%TI=Z%TS=7|9)
OPS(O1=M584ST11NW5%O2=M584ST11NW5%O3=M584NNT11NW5%O4=M584ST11NW5%O5=M584ST11NW5%O6=M584ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M584NNSNW5%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=1F59B3D4%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=1F59B3D4%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=1F59B3D4%Q=)
T7(R=N)
U1(R=N)
IE(R=N)

# Billion WRT610N running Firmware Version: 1.00.02 B10
Fingerprint Billion WRT610n WAP
Class Billion | embedded || WAP
SEQ(SP=77-85%GCD=1-6%ISR=7F-8D%TI=I%CI=I%TS=U)
OPS(O1=M58C%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=4000%O=M58C%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=96-A0%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# BinTec BinGO!
Fingerprint BinTec BinGO! ISDN router
Class BinTec | embedded || router
SEQ(SP=66-80%GCD=1-6%ISR=8D-97%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=72-7C%TG=80%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=71-7C%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=72-7C%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=72-7C%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=72-7C%TG=80%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=72-7C%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=72-7C%TG=80%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=72-7C%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=72-7C%TG=80%IPL=38%UN=0%RIPL=G%RID=0%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=S%T=72-7C%TG=80%CD=S)

# Bintec Brick-XM
Fingerprint BinTec Brick-XM router
Class BinTec | embedded || router
SEQ(SP=61-71%GCD=1-6%ISR=8D-97%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=4B-55%TG=80%W=1000%O=M5B4%CC=N)
T1(R=Y%DF=N%T=4B-55%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=4B-55%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=4B-55%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=4B-55%TG=80%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=4B-55%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=4B-55%TG=80%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=4B-55%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=4B-55%TG=80%IPL=38%UN=0%RIPL=G%RID=0%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=S%T=4B-55%TG=80%CD=S)

# funkwerk bintec R3400 gateway
Fingerprint BinTec R3400 WAP
Class BinTec | embedded || router
SEQ(SP=27-6D%GCD=1-6%ISR=8A-94%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=76-80%TG=80%W=4000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=76-80%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=76-80%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=76-80%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=76-80%TG=80%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=76-80%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=76-80%TG=80%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=76-80%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=46-50|76-80%TG=80%IPL=38%UN=4E07%RIPL=G%RID=0%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=S%T=76-80%TG=80%CD=S)

# BINTEC-X4000 version V.7.1 Rev. 4 from 2004/10/06 00:00:00
Fingerprint BinTec X4000 access router
Class BinTec | embedded || router
SEQ(SP=64-6E%GCD=1-6%ISR=8A-94%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=71-7B%TG=80%W=4000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=71-7B%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=71-7B%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=71-7B%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=71-7B%TG=80%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=71-7B%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=71-7B%TG=80%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=71-7B%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=71-7B%TG=80%IPL=38%UN=0%RIPL=G%RID=0%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=S%T=71-7B%TG=80%CD=S)

# Funkwerk BinTec R1200
Fingerprint BinTec R1200 WAP
Class BinTec | embedded || WAP
SEQ(SP=4C-7C%GCD=1-6%ISR=8A-94%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=6E-78%TG=80%W=4000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=6D-78%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=6E-78%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=6E-78%TG=80%IPL=38%UN=0|128%RIPL=G%RID=0%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=S%T=6E-78%TG=80%CD=S)

# BlackBoard Transaction System IP Converter (serial-to-IP converter). COM/IPCONV IP Converter V5.6.
Fingerprint Blackboard transaction system serial-to-IP converter
Class Blackboard | embedded || bridge
SEQ(SP=E6-F0%GCD=1-6%ISR=EA-F4%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=209D)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2238%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Blue Coat proxy server running SGOS 3.2.4.8
Fingerprint Blue Coat proxy server (SGOS 3.2.4.8)
Class Blue Coat | SGOS | 3.X | proxy server
SEQ(SP=94-A2%GCD=1-6%ISR=9E-A8%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Blue Coat proxy server running SGOS 4.1.3.1, release 24075
# Blue Coat Proxy SG8000 w/ SGOS 4.2.3.12
Fingerprint Blue Coat proxy server (SGOS 4.1 - 4.2)
Class Blue Coat | SGOS | 4.X | proxy server
SEQ(SP=A0-B1%GCD=1-6%ISR=A5-C2%TI=RD%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M578NW0NNT11%O3=M280NW0NNT11%O4=M5B4NW0NNT11%O5=M218NW0NNT11%O6=M109NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Blue Coat SG200 Proxy - SGOS 4.2.2.8 release id: 26972
# SGOS 4.2.5.1, release 29951.
# Blue Coat SG200, Version: SGOS 4.2.6.1, Release id: 31079
Fingerprint Blue Coat SG200 proxy server (SGOS 4.2.2.8 - 4.2.6.1)
Class Blue Coat | SGOS | 4.X | proxy server
SEQ(SP=94-A0%GCD=1-6%ISR=9C-A6%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M578NW0NNT11%O3=M280NW0NNT11%O4=M5B4NW0NNT11%O5=M218NW0NNT11%O6=M109NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Blue Coat SG810 Series Software SGOS 4.2.3.26
Fingerprint Blue Coat SG810 proxy server (SGOS 4.2.3.26)
Class Blue Coat | SGOS | 4.X | proxy server
SEQ(SP=A0-B4%GCD=1-6%ISR=AB-BB%TS=1|2)
OPS(O1=M5B4NW0NNT11%O2=M578NW0NNT11%O3=M280NW0NNT11%O4=M5B4NW0NNT11%O5=M218NW0NNT11%O6=M109NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=4210%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Model: Blue Coat SG200 Series,  Software SGOS 5.1.4.4,  Software Release ID: 28724
Fingerprint Blue Coat SG200 proxy server (SGOS 5.1.4.4)
Class Blue Coat | SGOS | 5.X | proxy server
SEQ(SP=FF-109%GCD=1-6%ISR=104-112%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0ST11LLLL%O2=M5B4NW0ST11LLLL%O3=M5B4NW0NNT11%O4=M5B4NW0ST11LLLL%O5=M5B4NW0ST11LLLL%O6=M5B4ST11LLLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Blue Coat SG210-10. SGOS 5.2.3.9 Proxy edition software release 34077
# Blue Coat Proxy SG210 running SGOS 5.2.3.3
Fingerprint Blue Coat SG210 proxy server (SGOS 5.2.3.3 - 5.2.3.9)
Class Blue Coat | SGOS | 5.X | proxy server
SEQ(SP=FD-109%GCD=1-6%ISR=103-10D%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0ST11LLLL%O2=M5B4NW0ST11LLLL%O3=M5B4NW0NNT11%O4=M5B4NW0ST11LLLL%O5=M5B4NW0ST11LLLL%O6=M5B4ST11LLLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW0ST11LLLL%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Blue Coat 510-10 SGOS 5.2.2.5 Proxy Edition, Software release ID: 31082
Fingerprint Blue Coat SG510 proxy server (SGOS 5.2.2.5)
Class Blue Coat | SGOS | 5.X | proxy server
SEQ(SP=FE-108%GCD=1-6%ISR=106-110%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0ST11LLLL%O2=M5B4NW0ST11LLLL%O3=M5B4NW0NNT11%O4=M5B4NW0ST11LLLL%O5=M5B4NW0ST11LLLL%O6=M5B4ST11LLLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW0ST11LLLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Model: Blue Coat SG510 Series , Software: SGOS 5.1.3.7, Software Release ID: 27503
Fingerprint Blue Coat SG510-series proxy server (SGOS 5.1.3.7)
Class Blue Coat | SGOS | 5.X | proxy server
SEQ(SP=100-10C%GCD=1-6%ISR=104-10E%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNT11SLL%O2=M5B4NW0NNT11SLL%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11SLL%O5=M5B4NW0NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW0NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Blue Coat 810-10, SGOS 5.3.1.9 Proxy Edition
# Blue Coat SGOS Specific version 5.3.3.1
Fingerprint Blue Coat SG810 web proxy (SGOS 5.3.1.9 - 5.3.3.1)
Class Blue Coat | SGOS | 5.X | proxy server
SEQ(SP=F4-10C%GCD=1-6%ISR=102-110%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW6ST11LLLL%O2=M5B4NW6ST11LLLL%O3=M5B4NW6NNT11%O4=M5B4NW6ST11LLLL%O5=M5B4NW6ST11LLLL%O6=M5B4ST11LLLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW6SLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW6ST11LLLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Version: SGOS 5.5.3.1 Proxy Edition Release id: 46382
Fingerprint Blue Coat SGOS 5.5.3.1
Class Blue Coat | SGOS | 5.X | proxy server
SEQ(SP=FA-10A%GCD=1-6%ISR=103-10D%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW6ST11LLLL%O2=M5B4NW6ST11LLLL%O3=M5B4NW6NNT11%O4=M5B4NW6ST11LLLL%O5=M5B4NW6ST11LLLL%O6=M5B4ST11LLLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW6SLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW6ST11LLLL%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# BlueArc Titan 2100 firmware version 4.2.944b
Fingerprint BlueArc Titan 2100 NAS device
Class BlueArc | embedded || storage-misc
SEQ(SP=1D-2D%GCD=1-6%ISR=8A-94%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FAF0%W2=FAF0%W3=FAF0%W4=FAF0%W5=FAF0%W6=FAF0)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=FAF0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=FAF0%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=FAF0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=FAF0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=FAF0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=FAF0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# SuperDOS - very old OS...but still working. Still sold by www.dccs.com.
Fingerprint Bluebird SuperDOS
Class Bluebird | SuperDOS || general purpose
SEQ(SP=FA-104%GCD=1-6%ISR=F3-FD%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B0%O2=M578%O3=M200%O4=M5B0%O5=M5B0%O6=M5B0)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=76%TG=80%W=1000%O=M5B0%CC=N%Q=)
T1(R=Y%DF=N%T=76%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=76%TG=80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=76%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=76%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=76%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=76%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=76%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=4AA2%RUD=G)
IE(DFI=N%T=76%TG=80%CD=Z)

# Bluebird SuperDOS
Fingerprint Bluebird SuperDOS
Class Bluebird | SuperDOS || general purpose
SEQ(SP=C7-D1%GCD=1-6%ISR=D6-E0%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B0%O2=M578%O3=M200%O4=M5B0%O5=M5B0%O6=M5B0)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=78%TG=80%W=1000%O=M5B0%CC=N%Q=)
T1(R=Y%DF=N%T=78%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=78%TG=80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=78%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=78%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=78%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=78%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=78%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=5207%RUD=G)
IE(DFI=N%T=78%TG=80%CD=Z)

# Bosch Divar Security Systems embedded operating system
Fingerprint Bosch Divar security system
Class Bosch | embedded || security-misc
SEQ(SP=C-16%GCD=1E848|3D090|5B8D8|7A120|98968%ISR=9F-A9%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNT11%O2=M578NW0NNT11%O3=M280NW0NNT11%O4=M5B4NW0NNT11%O5=M218NW0NNT11%O6=M109NNT11)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=209D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2238%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=209D%S=O%A=S+%F=AS%O=M109NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# http://s2soft.com/boundless/anetterm.html
Fingerprint Boundless Technologies NetTerminal text terminal
Class Boundless Technologies | embedded || terminal
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=111C%W2=1068%W3=1180%W4=1000%W5=10C0%W6=1090)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1090%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# GS-Z3 Data logger, connected to an Energy Display Meter offered by www.energydisplaymeter.co.uk. BGB WebRTU Z3. Firmware Version : 2.05.03 (19), Config Filename: BGBConfig_07_01.bin
Fingerprint British Gas GS-Z3 data logger
Class British Gas | embedded || storage-misc
SEQ(CI=I%II=RI)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=N)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=800%S=A+%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=800%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=800%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=800%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# BroadMax Technology Limited LinkMAX HSA300A-2
Fingerprint BroadMax LinkMAX HSA300A-2 ADSL modem
Class BroadMax Technology | embedded || broadband router
SEQ(SP=0-41%GCD=1388|2710|3A98|4E20|61A8%ISR=8A-94%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1FB0%W2=1FB0%W3=1FB0%W4=1FB0%W5=1FB0%W6=1FB0)
ECN(R=Y%DF=N%T=3C%TG=40%W=1FB0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=1FB0%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=Y%T=3C%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3C%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=19-23%TG=20%CD=Z)

# Brocade Silkworm Switches, Kernel: 2.4.19, Fabric OS: v4.4.0b
Fingerprint Brocade SilkWorm switch
Class Brocade | embedded || switch
SEQ(SP=C3-CD%GCD=1-6%ISR=CE-D8%TI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=78C0%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Brother MFC-7840W
Fingerprint Brother MFC-7840W printer
Class Brother | embedded || print server
SEQ(SP=E-18%GCD=1E848|3D090|5B8D8|7A120|98968%ISR=9F-A9%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Brother NC-130h Node OS
Fingerprint Brother NC-130h print server
Class Brother | embedded || print server
SEQ(SP=C5-CF%GCD=1-6%ISR=D3-DD%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=N%T=79|B0-BA%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=79%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=79%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=79%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=79%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=79%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=8562%RUD=G)
IE(DFI=N%T=79%TG=80%CD=Z)

# External 10/100BASE-TX Print Server NC-2100p
Fingerprint Brother NC-2100p print server
Class Brother | embedded || print server
SEQ(SP=0-5%GCD=0%ISR=0-5%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=80%W2=80%W3=80%W4=80%W5=80%W6=80)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=80%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=80%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0|11A6%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Multiprotocol Print Server NC-3100h, Firmware Version: 3.20
Fingerprint Brother NC-3100h print server
Class Brother | embedded || print server
SEQ(SP=C5-CF%GCD=1-6%ISR=D5-DF%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M200%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=71%TG=80%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=71%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=71%TG=80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=71%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=71%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=71%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=71%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=71%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=1597%RUD=G)
IE(DFI=N%T=71%TG=80%CD=Z)

# Brother NC-3100h, Firmware Ver.3.20 (00.08.31)
Fingerprint Brother NC-3100h print server
Class Brother | embedded || print server
SEQ(SP=C8-D2%GCD=1-6%ISR=D5-DF%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M200%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=74%TG=80%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=74%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=74%TG=80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=74%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=74%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=74%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=74%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=74%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=1597%RUD=G)
IE(DFI=N%T=74%TG=80%CD=Z)

# Brother DCP-540CN printer, firmware ver.b
Fingerprint Brother DCP-540CN printer
Class Brother | embedded || printer
SEQ(SP=C8-D2%GCD=1-6%ISR=D5-DF%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=111C%W2=111C%W3=111C%W4=111C%W5=111C%W6=111C)
ECN(R=Y%DF=N%T=78%TG=80%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=78%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=78%TG=80%W=111C%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=78%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=78%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=78%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=78%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=78%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=835F%RUD=G)
IE(DFI=N%T=78%TG=80%CD=Z)

# Brother DCP-540CN Printer
Fingerprint Brother DCP-540CN printer
Class Brother | embedded || printer
SEQ(SP=CD-D7%GCD=1-6%ISR=D5-DF%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=111C%W2=111C%W3=111C%W4=111C%W5=111C%W6=111C)
ECN(R=Y%DF=N%T=79%TG=80%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=79%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=79%TG=80%W=111C%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=79%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=79%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=79%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=79%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=79%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=87B7%RUD=G)
IE(DFI=N%T=79%TG=80%CD=Z)

# DCP-8045D B/W Laser printer
Fingerprint Brother DCP-8045D printer
Class Brother | embedded || printer
SEQ(SP=E0-EA%GCD=1-6%ISR=DD-E7%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M200%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=76%TG=80%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=76%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=76%TG=80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=76%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=76%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=76%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=76%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=76%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=899B%RUD=G)
IE(DFI=N%T=76%TG=80%CD=Z)

# Brother NC-3100h Firmware Ver.3.20 (00.08.31), Brother NC-3100h Command Console
Fingerprint Brother HL-1270N printer
Class Brother | embedded || printer
SEQ(SP=C9-D3%GCD=1-6%ISR=D5-DF%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M200%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=73-7D%TG=80%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=73-7D%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=73-7D%TG=80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=73-7D%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=73-7D%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=73-7D%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=73-7D%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=73-7D%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=159C%RUD=G)
IE(DFI=N%T=73-7D%TG=80%CD=Z)

# Brother HL-2070N
Fingerprint Brother HL-2070N
Class Brother | embedded || printer
SEQ(SP=C3-CD%GCD=1-6%ISR=D6-E0%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=111C%W2=111C%W3=111C%W4=111C%W5=111C%W6=111C)
ECN(R=Y%DF=N%T=6F%TG=80%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=6F%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=6F%TG=80%W=111C%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=6F%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=6F%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=6F%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=6F%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=6F%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=8390%RUD=G)
IE(DFI=N%T=6F%TG=80%CD=Z)

# Brother HL-2070N printer (node type Brother NC-6200h, firmware version 1.33 2006-07-21)
Fingerprint Brother HL-2070N printer
Class Brother | embedded || printer
SEQ(SP=F8-102%GCD=1-6%ISR=F0-FA%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=111C%W2=111C%W3=111C%W4=111C%W5=111C%W6=111C)
ECN(R=Y%DF=N%T=76%TG=80%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=76%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=76%TG=80%W=111C%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=76%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=76%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=76%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=76%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=76%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=76%TG=80%CD=Z)

# Brother HL-2070N Networked Laser Printer
Fingerprint Brother HL-2070N printer
Class Brother | embedded || printer
SEQ(SP=D0-DA%GCD=1-6%ISR=D6-E0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=111C%W2=111C%W3=111C%W4=111C%W5=111C%W6=111C)
ECN(R=Y%DF=N%T=78%TG=80%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=78%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=78%TG=80%W=111C%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=78%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=78%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=78%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=78%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=78%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=78%TG=80%CD=Z)

# it is a brother HL-2070N network laster printer
Fingerprint Brother HL-2070N printer
Class Brother | embedded || printer
SEQ(SP=C6-D0%GCD=1-6%ISR=D5-DF%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=111C%W2=111C%W3=111C%W4=111C%W5=111C%W6=111C)
ECN(R=Y%DF=N%T=74%TG=80%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=74%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=74%TG=80%W=111C%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=74%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=74%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=74%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=74%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=74%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=74%TG=80%CD=Z)

# Brother HL-2070N Printer
Fingerprint Brother HL-2070N printer
Class Brother | embedded || printer
SEQ(SP=F8-102%GCD=1-6%ISR=EF-F9%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=111C%W2=111C%W3=111C%W4=111C%W5=111C%W6=111C)
ECN(R=Y%DF=N%T=70%TG=80%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=70%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=70%TG=80%W=111C%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=70%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=70%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=70%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=70%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=70%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=70%TG=80%CD=Z)

# Brother laser printer HL-2070N
Fingerprint Brother HL-2070N printer
Class Brother | embedded || printer
SEQ(SP=C8-D2%GCD=1-6%ISR=D7-E1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=111C%W2=111C%W3=111C%W4=111C%W5=111C%W6=111C)
ECN(R=Y%DF=N%T=78%TG=80%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=78%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=78%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=78%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=78%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=78%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=78%TG=80%CD=Z)

# HL 2070N, Printer Firmware Version 1.38, Network Firmware Version 1.38
Fingerprint Brother HL-2070N printer
Class Brother | embedded || printer
SEQ(SP=D1-DB%GCD=1-6%ISR=D5-DF%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=111C%W2=111C%W3=111C%W4=111C%W5=111C%W6=111C)
ECN(R=Y%DF=N%T=73%TG=80%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=73%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=73%TG=80%W=111C%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=73%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=73%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=73%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=73%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=73%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=73%TG=80%CD=Z)

# Brother HL-2070N
Fingerprint Brother HL-2070N printer
Class Brother | embedded || printer
SEQ(SP=C9-DF%GCD=1-6%ISR=D5-DF%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=111C%W2=111C%W3=111C%W4=111C%W5=111C%W6=111C)
ECN(R=Y%DF=N%T=71-7B%TG=80%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=76%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=76%TG=80%W=111C%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=76%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=76%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=76%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=76%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=76%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=76%TG=80%CD=Z)

# Brother 2070N
Fingerprint Brother HL-2070N printer
Class Brother | embedded || printer
SEQ(SP=C5-CF%GCD=1-6%ISR=D6-E0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=111C%W2=111C%W3=111C%W4=111C%W5=111C%W6=111C)
ECN(R=Y%DF=N%T=72%TG=80%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=72%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=72%TG=80%W=111C%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=72%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=72%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=72%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=72%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=72%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=72%TG=80%CD=Z)

# Brother HL-2070N series, Firmware Version 1.33
Fingerprint Brother HL-2070N printer
Class Brother | embedded || printer
SEQ(SP=D1-DB%GCD=1-6%ISR=D5-DF%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=111C%W2=111C%W3=111C%W4=111C%W5=111C%W6=111C)
ECN(R=Y%DF=N%T=74%TG=80%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=74%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=74%TG=80%W=111C%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=74%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=74%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=74%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=74%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=74%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=74%TG=80%CD=Z)

# Brother HL-2070N Laser Printer
Fingerprint Brother HL-2070N printer
Class Brother | embedded || printer
SEQ(SP=F8-102%GCD=1-6%ISR=F0-FA%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=111C%W2=111C%W3=111C%W4=111C%W5=111C%W6=111C)
ECN(R=Y%DF=N%T=79%TG=80%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=79%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=79%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=79%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=79%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=79%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=1615%RUD=G)
IE(DFI=N%T=79%TG=80%CD=Z)

# Brother HL-2070N
Fingerprint Brother HL-2070N printer
Class Brother | embedded || printer
SEQ(SP=CA-D4%GCD=1-6%ISR=D5-DF%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=N%T=71%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=71%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=71%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=71%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=71%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=71%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=1932%RUD=G)
IE(DFI=N%T=71%TG=80%CD=Z)

# Brother HL-2700CN printer
Fingerprint Brother HL-2700CN printer
Class Brother | embedded || printer
SEQ(SP=D1-DB%GCD=1-6%ISR=D7-E1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M200%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# Brother HL-5070N printer
Fingerprint Brother HL-5070N printer
Class Brother | embedded || printer
SEQ(SP=CC-D6%GCD=1-6%ISR=D6-E0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M200%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=70-7A%TG=80%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=70-7A%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=70-7A%TG=80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=70-7A%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=70-7A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=70-7A%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=70-7A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=70-7A%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=70-7A%TG=80%CD=Z)

# Printer Model 5070N by Brother Industries, Ltd.
Fingerprint Brother HL-5070N printer
Class Brother | embedded || printer
SEQ(SP=D1-DB%GCD=1-6%ISR=D6-E0%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=N%T=75%TG=80%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=75%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=75%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=75%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=75%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=75%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=75%TG=80%CD=Z)

# Brother HL-5170DN printer, firmware 1.11
Fingerprint Brother HL-5170DN printer
Class Brother | embedded || printer
SEQ(SP=C8-D2%GCD=1-6%ISR=D7-E1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M200%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=75%TG=80%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=75%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=75%TG=80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=75%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=75%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=75%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=75%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=75%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=859E%RUD=G)
IE(DFI=N%T=75%TG=80%CD=Z)

# Brother HL-5170DN printer, firmware 1.50
Fingerprint Brother HL-5170DN printer
Class Brother | embedded || printer
SEQ(SP=C2-CC%GCD=1-6%ISR=D5-DF%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M200%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=75%TG=80%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=75%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=75%TG=80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=75%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=75%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=75%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=75%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=75%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=8582%RUD=G)
IE(DFI=N%T=75%TG=80%CD=Z)

# Brother HL-5170DN Network-Ready Laser Printer with Duplex.
Fingerprint Brother HL-5170DN printer
Class Brother | embedded || printer
SEQ(SP=C8-D2%GCD=1-6%ISR=D7-E1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M200%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=76%TG=80%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=76%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=76%TG=80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=76%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=76%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=76%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=76%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=76%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=8582%RUD=G)
IE(DFI=N%T=76%TG=80%CD=Z)

# Brother HL-5170DN
Fingerprint Brother HL-5170DN printer
Class Brother | embedded || printer
SEQ(SP=F8-102%GCD=1-6%ISR=F1-FB%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M200%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=75%TG=80%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=75%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=75%TG=80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=75%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=75%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=75%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=75%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=75%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=8582%RUD=G)
IE(DFI=N%T=75%TG=80%CD=Z)

# Brother HL-5170DN printer
Fingerprint Brother HL-5170DN printer
Class Brother | embedded || printer
SEQ(SP=C5-D7%GCD=1-6%ISR=D4-DE%TI=I%II=I%SS=S%TS=U)
OPS(O1=|M5B4%O2=M578%O3=M200%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=71%TG=80%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=71%TG=80%S=O%A=S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=71%TG=80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=71%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=71%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=71%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=71%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=71%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=8563%RUD=G)
IE(DFI=N%T=71%TG=80%CD=Z)

# Brother Multifunction Printer, model MFC-420CN
# Brother MFC-420CN
Fingerprint Brother MFC-420CN multifunction printer
Class Brother | embedded || printer
SEQ(SP=D0-DA%GCD=1-6%ISR=D5-DF%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=70|72%TG=80%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=70|72%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=70|72%TG=80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=70|72%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=70|72%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=70|72%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=70|72%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=70|72%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=70|72%TG=80%CD=Z)

# Brother MFC425CN
Fingerprint Brother MFC-425CN multifunction printer
Class Brother | embedded || printer
SEQ(SP=CF-D9%GCD=1-6%ISR=D8-E2%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=111C%W2=111C%W3=111C%W4=111C%W5=111C%W6=111C)
ECN(R=Y%DF=N%T=74%TG=80%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=74%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=74%TG=80%W=111C%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=74%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=74%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=74%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=74%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=74%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=74%TG=80%CD=Z)

# Brother MFC-5840CN Multi-Function Center (print, scan, copy, fax)
Fingerprint Brother MFC-5840CN multifunction printer
Class Brother | embedded || printer
SEQ(SP=D1-DB%GCD=1-6%ISR=D7-E1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=74%TG=80%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=74%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=74%TG=80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=74%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=74%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=74%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=74%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=74%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=74%TG=80%CD=Z)

# Brother MFC-5860CN, F/W version = "E"
Fingerprint Brother MFC-5860CN multifunction printer
Class Brother | embedded || printer
SEQ(SP=C7-D1%GCD=1-6%ISR=D7-E1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=111C%W2=111C%W3=111C%W4=111C%W5=111C%W6=111C)
ECN(R=Y%DF=N%T=70%TG=80%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=70%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=70%TG=80%W=111C%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=70%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=70%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=70%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=70%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=70%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=70%TG=80%CD=Z)

# Brother MFC-640CW (via 802.11g)
# Sony Bravia KDL 40W5800 LDC-TV
Fingerprint Brother MFC-640CW multifunction printer
Class Brother | embedded || printer
SEQ(SP=CF-D9%GCD=1-6%ISR=D7-E1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=111C%W2=111C%W3=111C%W4=111C%W5=111C%W6=111C)
ECN(R=Y%DF=N%T=7B%TG=80%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=7B%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B%TG=80%W=111C%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=7B%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=7B%TG=80%CD=Z)

# Brother MFC-7820N
Fingerprint Brother MFC-7820N multifunction printer
Class Brother | embedded || printer
SEQ(SP=CB-D5%GCD=1-6%ISR=D5-DF%TI=I%II=I%SS=S%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45|7B-85%TG=40|80%S=O%A=S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# Brother MFC-7820N
Fingerprint Brother MFC-7820N multifunction printer
Class Brother | embedded || printer
SEQ(SP=CB-D5%GCD=1-6%ISR=D4-DE%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=7C%TG=80%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=7C%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7C%TG=80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=7C%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7C%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7C%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7C%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7C%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=7C%TG=80%CD=Z)

# Brother MFC-7820N all-in-one laser printer (NC-6200h firmware version K)
Fingerprint Brother MFC-7820N multifunction printer
Class Brother | embedded || printer
SEQ(SP=CC-D6%GCD=1-6%ISR=D5-DF%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=7C%TG=80%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=7C%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7C%TG=80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=7C%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7C%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7C%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7C%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7C%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=7C%TG=80%CD=Z)

# Brother MFC-7820N
Fingerprint Brother MFC-7820N multifunction printer
Class Brother | embedded || printer
SEQ(SP=D1-DB%GCD=1-6%ISR=D4-DE%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=75%TG=80%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=75%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=75%TG=80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=75%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=75%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=75%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=75%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=75%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=75%TG=80%CD=Z)

# Brother MFC-7820N, MFC Firmware Version E
Fingerprint Brother MFC-7820N multifunction printer
Class Brother | embedded || printer
SEQ(SP=C8-D8%GCD=1-6%ISR=D3-DD%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=79%TG=80%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=79%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=79%TG=80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=79%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=79%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=79%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=79%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=79%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=79%TG=80%CD=Z)

# Brother MFC-7820N
# Brother MFC9420CN printer/fax/scanner
Fingerprint Brother MFC-7820N or MFC-9420CN printer
Class Brother | embedded || printer
SEQ(SP=BE-D4%GCD=1-6%ISR=D5-DF%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=71%TG=40|80%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=71%TG=40|80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=71%TG=40|80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=71%TG=40|80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=71%TG=40|80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=71%TG=40|80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=71%TG=40|80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=71%TG=40|80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=N%T=71%TG=40|80%CD=Z)

# Brother MFC-7820N
Fingerprint Brother MFC-7820N printer
Class Brother | embedded || printer
SEQ(SP=C3-CD%GCD=1-6%ISR=D2-DC%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=N%T=79%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=79%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=79%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=79%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=79%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=79%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=82A2%RUD=G)
IE(DFI=N%T=79%TG=80%CD=Z)

# Brother MFC-9420CN
Fingerprint Brother MFC-9420CN printer
Class Brother | embedded || printer
SEQ(SP=C1-CB%GCD=1-6%ISR=D5-DF%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=6F%TG=80%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=6F%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=6F%TG=80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=6F%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=6F%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=6F%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=6F%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=6F%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=164B%RUD=G)
IE(DFI=N%T=6F%TG=80%CD=Z)

# BSD/OS 4.2 BSDI BSD/OS 4.2 Kernel #25: Mon Dec 16 13:09:15 PST 2002 i386
Fingerprint BSDI BSD/OS 4.2
Class BSDI | BSD/OS | 4.X | general purpose
SEQ(SP=8C-9E%GCD=1-6%ISR=99-A3%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW4NNT11%O2=M5B4NW0NNT11%O3=M5B4NW4NNT11%O4=M5B4NW4NNT11%O5=M5B4NW4NNT11%O6=M5B4NNT11)
WIN(W1=2238%W2=20D0%W3=2080%W4=2000%W5=2180%W6=2017)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2238%O=M5B4NW4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=2017%S=O%A=S+%F=AS%O=M5B4NW4NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# BT Vision+ set top box. Platform OS/Version: WinCE/5.0.1400. Bootstrap ROM version:2.8025.
# BT Vision+ box.  Manufactured by Pace (France).
Fingerprint BT Vision+ set-top box (Windows CE 5.0.1400)
Class BT | Windows | PocketPC/CE | media device
SEQ(SP=77-85%GCD=1-6%ISR=93-9D%TI=I%II=I%SS=S%TS=0)
OPS(O1=M5B2NW0NNT00NNS%O2=M5B2NW0NNT00NNS%O3=M5B2NW0NNT00%O4=M5B2NW0NNT00NNS%O5=M5B2NW0NNT00NNS%O6=M5B2NNT00NNS)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=8000%O=M5B2NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=7B-85%TG=80%W=8000%S=O%A=S+%F=AS%O=M5B2NW0NNT00NNS%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=B0%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=Z)

# Buffalo DriveStation FlexNet model HD-CE1.0TLU2
Fingerprint Buffalo DriveStation HD-CE1.0TLU2 NAS device
Class Buffalo | embedded || storage-misc
SEQ(SP=0-19%GCD=1-6|78E|F1C|16AA|1E38|25C6%ISR=6D-77%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=1B-25%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=1B-25%TG=20%CD=S)

# Buffalo Linkstation Live and the OS is linux based
Fingerprint Buffalo LinkStation Live NAS device
Class Buffalo | embedded || storage-misc
SEQ(SP=9B-103%GCD=1-6%ISR=E9-FF%TI=Z%CI=Z%II=I%TS=7)
OPS(O1=M1CC4ST11NW2%O2=M1CC4ST11NW2%O3=M1CC4NNT11NW2%O4=M1CC4ST11NW2%O5=M1CC4ST11NW2%O6=M1CC4ST11)
WIN(W1=3970%W2=3970%W3=3970%W4=3970%W5=3970%W6=3970)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=3988%O=M1CC4NNSNW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=3970%S=O%A=S+%F=AS%O=M1CC4ST11NW2%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=O%A=Z%F=R%RD=0)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%RD=0)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Buffalo Terastation File Server Model# HD-H1.0TGL/R5 Firmware Version 1.12
Fingerprint Buffalo TeraStation NAS device
Class Buffalo | embedded || storage-misc
SEQ(SP=C7-D1%GCD=1-6%ISR=CC-D6%TI=Z%II=I%TS=7)
OPS(O1=M1CC0ST11NW0%O2=M1CC0ST11NW0%O3=M1CC0NNT11NW0%O4=M1CC0ST11NW0%O5=M1CC0ST11NW0%O6=M1CC0ST11)
WIN(W1=3968%W2=3968%W3=3968%W4=3968%W5=3968%W6=3968)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=3980%O=M1CC0NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=3968%S=O%A=S+%F=AS%O=M1CC0ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Buffalo TeraStation (NAS)
# Wireless-G Access Point (Model WAP54G), Firmware rev: 3.05
Fingerprint Buffalo TeraStation NAS device or Linksys WAP54G WAP
Class Buffalo | embedded || storage-misc
Class Linksys | embedded || WAP
SEQ(SP=FC-107%GCD=1-6%ISR=FF-10F%TI=Z%II=I%TS=7)
OPS(O1=M564ST11NW0%O2=M564ST11NW0%O3=M564NNT11NW0%O4=M564ST11NW0%O5=M564ST11NW0%O6=M564ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M564NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Buffalo Terastation Pro II 2TB NAS, Model Name TS-RHTGL/R5 F/W 1.23
Fingerprint Buffalo TeraStation Pro II NAS device
Class Buffalo | embedded || storage-misc
SEQ(SP=C7-D1%GCD=1-6%ISR=CA-D4%TI=Z%II=I%TS=7)
OPS(O1=M25A4ST11NW2%O2=M25A4ST11NW2%O3=M25A4NNT11NW2%O4=M25A4ST11NW2%O5=M25A4ST11NW2%O6=M25A4ST11)
WIN(W1=4B30%W2=4B30%W3=4B30%W4=4B30%W5=4B30%W6=4B30)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4B48%O=M25A4NNSNW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4B30%S=O%A=S+%F=AS%O=M25A4ST11NW2%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# TS-RHTGL/R5 with firmware version 1.33 (latest), Terastation PRO II Rack (4GB model)
Fingerprint Buffalo TeraStation Pro II NAS device
Class Buffalo | embedded || storage-misc
SEQ(SP=BC-C6%GCD=1-6%ISR=C6-D0%TI=Z%II=I%TS=7)
OPS(O1=NNT11|M1CC4ST11NW2%O2=NNT11|M1CC4ST11NW2%O3=NNT11|M1CC4NNT11NW2%O4=NNT11|M1CC4ST11NW2%O5=NNT11|M1CC4ST11NW2%O6=NNT11|M1CC4ST11)
WIN(W1=3970%W2=3970%W3=3970%W4=3970%W5=3970%W6=3970)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=3988%O=|M1CC4NNSNW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=3970%S=O%A=O|S+%F=A|AS%O=NNT11|M1CC4ST11NW2%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Buffalo Terra-Station Pro II
Fingerprint Buffalo TeraStation Pro II NAS device
Class Buffalo | embedded || storage-misc
SEQ(SP=C7-D1%GCD=1-6%ISR=CE-D8%TI=RD%II=RI%TS=7)
OPS(O1=M4FEST11NW2%O2=M4FEST11NW2%O3=M4FENNT11NW2%O4=M4FEST11NW2%O5=M4FEST11NW2%O6=M4FEST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M4FENNSNW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=4AE|74CC|8D89|93C1|F9A7%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Buffalo TeraStation III Pro, Firmware 1.10
Fingerprint Buffalo TeraStation Pro III NAS device
Class Buffalo | embedded || storage-misc
SEQ(SP=F9-103%GCD=1-6%ISR=F5-FF%TI=Z%CI=Z%II=I%TS=7)
OPS(O1=M25A4ST11NW5%O2=M25A4ST11NW5%O3=M25A4NNT11NW5%O4=M25A4ST11NW5%O5=M25A4ST11NW5%O6=M25A4ST11)
WIN(W1=4B30%W2=4B30%W3=4B30%W4=4B30%W5=4B30%W6=4B30)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4B48%O=M25A4NNSNW5%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4B30%S=O%A=S+%F=AS%O=M25A4ST11NW5%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# http://www.burny.com/pc-based_cnc_controls.asp, Windows embedded
Fingerprint Burny CNC controller (Microsoft Windows XP Embedded)
Class Burny | Windows | XP | specialized
SEQ(SP=FE-108%GCD=1-6%ISR=105-10F%TI=I%CI=RD%II=I%SS=S%TS=0)
OPS(O1=M546NW0NNT00NNS%O2=M546NW0NNT00NNS%O3=M546NW0NNT00%O4=M546NW0NNT00NNS%O5=M546NW0NNT00NNS%O6=M546NNT00NNS)
WIN(W1=448E%W2=448E%W3=4100%W4=40E8%W5=40E8%W6=402E)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=448E%O=M546NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C-46%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C-46%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C-46%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C-46%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C-46%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=B0%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=Z)

# Bush Freesat HD receiver - BFSAT01HD
Fingerprint Bush BFSAT01HD satellite receiver
Class Bush | embedded || media device
SEQ(SP=0-85%GCD=1-6|2293|4526|67B9|8A4C|ACDF%ISR=7D-87%TI=I%CI=I%II=RI%SS=O%TS=U)
OPS(O1=M53C%O2=M53C%O3=M280%O4=M53C%O5=M218%O6=M109)
WIN(W1=53C0%W2=53C0%W3=53C0%W4=53C0%W5=53C0%W6=53C0)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=53C0%O=M53C%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=FA-104%TG=FF%W=53C0%S=O%A=O|S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=53C0%S=A+%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=53C0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=53C0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=53C0%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=21-3C%TG=40%CD=S)

# industrial label printer for marking (brand name "A4+/300") by company "cab Produkttechnik GmbH & Co KG", Firmware V3.19 (Apr 27 2009), Bootloader V1.19 (Mar 13 2008)
Fingerprint cab A4+/300 label printer
Class cab | embedded || printer
SEQ(SP=8B-FD%GCD=1-6|7|E|15|1C|23%ISR=96-E4%TI=I%CI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4SW0T10L%O2=M5B4SW0T10L%O3=M5B4SW0T10L%O4=M5B4SW0T10L%O5=M5B4SW0T10L%O6=M5B4ST10)
WIN(W1=2000%W2=8000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2000%O=M5B4SW0LLL%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=2000%S=O%A=O%F=A%O=T10LL%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=19-23%TG=20%CD=S)

# Cabletron ELS100-24TXM
# 3Com Corporation HiPer Access Router, Dialup-MODEM concentrador
Fingerprint Cabletron ELS100-24TXM Switch
Class Cabletron | embedded || switch
SEQ(SP=0-87%GCD=9C4|1388|1D4C|2710|30D4%ISR=8A-B0%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Cabletron Systems ELS100-24TXM, Switch
# IC-7800 radio, Ver 2.20
Fingerprint Cabletron ELS100-24TXM Switch or Icom IC-7800 radio transceiver
Class Cabletron | embedded || switch
Class Icom | embedded || specialized
SEQ(SP=0-63%GCD=61A8|C350|124F8|186A0|1E848|249F0%ISR=8A-B0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Enterasys Networks 6G306-06 Rev 05.06.04  10/27/03--13:35 ofc
# Cabletron Systems, Inc. 6H258-17 Rev 05.08.18  12/06/05--12:41 ofc
# Cabletron Systems, Inc. 6H262-18 Rev 05.08.09  01/18/05--15:19 ofc
# Enterasys Networks 6H302-48 Rev 05.07.12  04/27/04--17:19 ofc
Fingerprint Cabletron or Enterasys switch (6G- or 6H-series)
Class Cabletron | embedded || switch
Class Enterasys | embedded || switch
SEQ(SP=77-91%GCD=200|400|600|800|A00|C00%ISR=BF-D1%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1000%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=Z)

# CAEN Sy2527 High Voltage Power Supply, Software Version 2.01.00 (used, for example, in physics experiments). Uses some DOS-based embedded system I know no details about.
Fingerprint CAEN SY2527 high voltage power supply
Class CAEN | embedded || power-device
SEQ(SP=103-10D%GCD=1-6%ISR=105-10F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=7FE0%W2=7FE0%W3=7FE0%W4=7FE0%W5=7FE0%W6=7FE0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=7FE0%O=M5B4%CC=S%Q=RU)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=7FE0%S=O%A=S+%F=ASF%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# This is a Calix C7 cabinet.  It's running R5.0.71
# Calix C7 shelf running 5.0.43
Fingerprint Calix C7 switch (R5.0)
Class Calix | embedded || switch
SEQ(SP=0-5%GCD=FA01|1F402|2EE03|3E804|4E205%ISR=95-9F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=2710%W2=2710%W3=2710%W4=2710%W5=2710%W6=2710)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2710%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=FA-104%TG=FF%CD=Z)

# iR1024
Fingerprint Canon imageRUNNER 1024 laser printer
Class Canon | embedded || printer
SEQ(SP=0-69%GCD=1-6|10001|20002|30003|40004|50005%ISR=95-9F%TI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=5B4%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=5B4%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=5B4%S=A%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=5B4%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=FA-104%TG=FF%CD=Z)

# Canon iR2020n department printer
# Kyocera FS-4000DN, System Firmware: 2F9_3000.010.004, Engine Firmware: 2GA_1000.010.001
Fingerprint Canon imageRUNNER 2020 or Kyocera FS-4000DN printer
Class Canon | embedded || printer
Class Kyocera | embedded || printer
SEQ(SP=0-5%GCD=10001|20002|30003|40004|50005%ISR=96-A0%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=5B4%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=5B4%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=5B4%S=A%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=5B4%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=FA-104%TG=FF%CD=Z)

# Canon iR6570 laser printer
# Canon iR2270 Laser Printer
# Canon iR4570 Laser Printer
# ReactOS Operating System, version 0.3.11-20091212-r44553
Fingerprint Canon imageRUNNER 2270, 4570, or 6570 laser printer
Class Canon | embedded || printer
SEQ(SP=97-A1%GCD=1-6%ISR=9D-A7%TI=I%TS=1|2)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=O|S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)

# Canon Image Runner 3300
# Motorola SBG900 Cable Modem
Fingerprint Canon imageRUNNER 3300 printer or Motorola SURFboard SBG900 wireless cable modem
Class Canon | embedded || printer
Class Motorola | embedded || WAP
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M200NW0%O2=M200NW0%O3=M200NW0%O4=M200NW0%O5=M200NW0%O6=M200)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M200NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Canon net printer/scanner/fax IR3100C
Fingerprint Canon imageRUNNER C3100 multifunction printer
Class Canon | embedded || printer
SEQ(SP=13-1D%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=98-A2%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

Fingerprint Canon imageRUNNER C3200 multifunction printer
Class Canon | embedded || printer
SEQ(SP=16-20%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=9B-A5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Canon iRC3580 colour photocopier
Fingerprint Canon imageRUNNER C3580 printer
Class Canon | embedded || printer
SEQ(SP=F5-109%GCD=1-6%ISR=FF-10F%TI=I%CI=I%II=I%SS=S%TS=6)
OPS(O1=M514NW0NNT11%O2=M514NW0NNT11%O3=M514NW0NNT11%O4=M514NW0NNT11%O5=M514NW0NNT11%O6=M514NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M514NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M514NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C-46%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Canon ImageRunner C5185 Printer
Fingerprint Canon imageRUNNER C5185 printer
Class Canon | embedded || printer
SEQ(SP=F9-103%GCD=1-6%ISR=100-10A%TI=I%CI=I%II=I%SS=S%TS=6)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Canon iR6800C EUR printer/scanner/copier
Fingerprint Canon imageRUNNER C6800 multifunction printer
Class Canon | embedded || printer
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Canon MF4360-4390 Printer
# Canon 4370dn network laser all-in-one printer
Fingerprint Canon MF4360-4390 or 4370dn printer
Class Canon | embedded || printer
SEQ(SP=0-5%GCD=FA01|1F402|2EE03|3E804|4E205%ISR=95-9F%TI=BI%CI=BI%II=BI%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=2710%W2=2710%W3=2710%W4=2710%W5=2710%W6=2710)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2710%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=R%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=R%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=Z)

# Canon PIXMA iX7000
Fingerprint Canon PIXMA iX7000 printer
Class Canon | embedded || printer
SEQ(SP=0-1D%GCD=3200|6400|9600|C800|FA00|BB800%ISR=B2-BC%TI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=2D00%W2=2D00%W3=2D00%W4=2D00%W5=2D00%W6=2D00)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2D00%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2D00%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# multifunction printer Canon Pixma MP620
# Canon MX860 Multifunction Device
# Canon MP876 MFP
# Canon MP560 series, Firmware Version:       1.040
# Canon MX870 Series, FW 1.010, Canon Pixma IP4000R printer
Fingerprint Canon PIXMA MP560, MP620, or MX800-series printer
Class Canon | embedded || printer
SEQ(SP=0-5C%GCD=3200|6400|9600|C800|FA00%ISR=C0-11E%TI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=2D00%W2=2D00%W3=2D00%W4=2D00%W5=2D00%W6=2D00)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2D00%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2D00%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Canon mp600r
# Canon Pixma MX700 printer
Fingerprint Canon PIXMA MP600R or MX700 multifunction printer
Class Canon | embedded || printer
SEQ(SP=E-2A%GCD=10000|20000|30000|40000|50000%ISR=C5-CF%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M5B4%O4=M5B4%O5=M218%O6=M109)
WIN(W1=F800%W2=F800%W3=F800%W4=F800%W5=F800%W6=F800)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=F800%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=F800%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=F800%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# Canon Pixma MX860 network printer/scanner/fax.
# Canon Pixma MX870.
Fingerprint Canon PIXMA MP620, MX860, or MX870 printer
Class Canon | embedded || printer
SEQ(SP=0-91%GCD=200|400|600|800|A00%ISR=FE-112%TI=RD%CI=RD|RI%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=2D00%W2=2D00%W3=2D00%W4=2D00%W5=2D00%W6=2D00)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2D00%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2D00%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Canon 4000r printer
# Canon MP800R printer
Fingerprint Canon PIXMA MP800R or 4000R printer
Class Canon | embedded || printer
SEQ(SP=E-2A%GCD=10000|20000|30000|40000|50000|60000%ISR=C6-D0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M5B4%O4=M5B4%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O|S+%F=A|AS%O=|M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# Canon MP980 printer/copier
Fingerprint Canon PIXMA MP980 printer
Class Canon | embedded || printer
SEQ(SP=0-5%GCD=>1000000%ISR=10B-115%TI=RD%CI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=2D00%W2=2D00%W3=2D00%W4=2D00%W5=2D00%W6=2D00)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2D00%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2D00%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# PIXMA MX850 multi function printer
Fingerprint Canon PIXMA MX850 printer
Class Canon | embedded || printer
SEQ(SP=0-1D%GCD=388|710|A98|E20|11A8%ISR=64-7A%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# Casio QT600/QT6100 cash registering machine
Fingerprint Casio QT-6000 or QT-6100 point-of-sale machine
Class Casio | embedded || specialized
SEQ(CI=I%II=I%TS=U)
OPS(O1=M5B4%O2=%O3=%O4=%O5=%O6=)
WIN(W1=1000%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# Linux 2.6.23.17 #28 Thu May 14 12:28:51 MYT 2009 ppc unknown, CT-730 WiMAX-WiFi Wireless Router
Fingerprint Ceedtec CD-730 WiMAX WAP (Linux 2.6.23)
Class Ceedtec | Linux | 2.6.X | WAP
SEQ(SP=C2-CC%GCD=1-6%ISR=C5-CF%TI=Z%CI=Z%TS=7|9)
OPS(O1=M5B4NNT11%O2=M5B4NNT11%O3=M5B4NNT11%O4=M5B4NNT11%O5=M5B4NNT11%O6=M5B4NNT11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Check Point SBox-200, Version: 1.2G, Running: 8.0.34x
Fingerprint Check Point SBox-200 firewall
Class Check Point | embedded || firewall
SEQ(SP=C7-D1%GCD=1-6%ISR=CD-D7%TI=Z%CI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=1A3A%W2=1A3A%W3=1A3A%W4=1A3A%W5=1A3A%W6=1A3A)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1A5E%O=M5B4NNSNW0%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# CheckPoint UTM-1 Edge X, Firmware Version 7.5.42x, Hardware Type SBox-200
Fingerprint Check Point UTM-1 Edge X firewall
Class Check Point | embedded || firewall
SEQ(SP=C5-CF%GCD=1-6%ISR=CA-D4%TI=Z%II=I%TS=7)
OPS(O1=M564ST11NW0%O2=M564ST11NW0%O3=M564NNT11NW0%O4=M564ST11NW0%O5=M564ST11NW0%O6=M564ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3C-46%TG=40%W=16D0%O=M564NNSNW0%CC=Y%Q=)
T1(R=Y%DF=Y%T=3C-46%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3C-46%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3C-46%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3C-46%TG=40%CD=S)

# VPN-1 Edge X ADSL, Embedded NGX, Firmware version: 7.0.34x
Fingerprint Check Point VPN-1 UTM appliance
Class Check Point | embedded || firewall
SEQ(SP=BA-CE%GCD=1-6%ISR=C3-D7%TI=Z%CI=Z%II=I%TS=9|A|B)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=Y)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%RD=0)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%RD=0)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%RD=0)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%RD=0)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Zonealarm Z100G Firewall/wireless router. (checkpoint)
Fingerprint Check Point ZoneAlarm Z100G firewall
Class Check Point | embedded || firewall
SEQ(SP=BE-C8%GCD=1-6%ISR=D0-DA%TI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# IPSO 4.2 Build 106a04 running R65 HFA_60
Fingerprint Check Point NGX R65 firewall (IPSO 4.2)
Class Check Point | IPSO | 4.X | firewall
SEQ(SP=FD-10B%GCD=1-6%ISR=107-113%TI=I%II=I%SS=S%TS=1)
OPS(O1=M400NW0NNT11%O2=M400NW0NNT11%O3=M400NW0NNT11%O4=M400NW0NNT11%O5=M400NW0NNT11%O6=M400NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4334%W5=4180%W6=403D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4470%O=M400NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Check Point VPN-1(TM) & FireWall-1(R) NGX (R60) HFA_03, Hotfix 603 - Build 015  & IPSO fw-001 4.1-BUILD016 releng 1515  05.19.2006-052320 i386
# This is Check Point VPN-1(TM) & FireWall-1(R) NGX (R60) HFA_03, Hotfix 603 - Build 015
# IPSO fw-001 4.1-BUILD016 releng 1515  05.19.2006-052320 i386
Fingerprint Check Point VPN-1 firewall (IPSO 4.1)
Class Check Point | IPSO | 4.X | firewall
SEQ(SP=C0-10C%GCD=1-6%ISR=107-10B%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4110%W5=4180%W6=403D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Linux 2.4.21-21cpsmp #1 SMP Sun Feb 11 18:18:33 IST 2007 i686 i686 i386 GNU/Linux (Check Point SecurePlatform NGX (R65) Build 123 (ClusterXL))
Fingerprint Check Point firewall (Linux 2.4.21)
Class Check Point | Linux | 2.4.X | firewall
SEQ(SP=BF-C9%GCD=1-6%ISR=C6-D0%TI=Z%II=I%TS=U)
OPS(O1=M5B4NNSNW0%O2=M5B4NNSNW0%O3=M5B4NW0%O4=M5B4NNSNW0%O5=M5B4NNSNW0%O6=M5B4NNS)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%S=O%A=S+%F=AS%O=M5B4NNSNW0%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=B732%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Linux CP-1 2.4.21-21cpsmp #1 SMP Thu Sep 11 17:01:25 IDT 2008 i686 i686 i386 GNU/Linux, Checkpoint Secure Platform R65
Fingerprint Check Point NGX R65 firewall (Linux 2.4.21)
Class Check Point | Linux | 2.4.X | firewall
SEQ(SP=F1-107%GCD=1-6%ISR=106-110%TI=Z%CI=Z%II=I%TS=U)
OPS(O1=M5B4NNSNW0%O2=M578NNSNW0%O3=M280NW0%O4=M22CNNSNW0%O5=M218NNSNW0%O6=M109NNS)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Check Point Edge X Appliance, firmware 6.5.43x
# Check Point VPN-1 Edge
# Check Point VPN-1 Edge, Firmware Version 6.5.43x
Fingerprint Check Point VPN-1 UTM appliance
Class Check Point | Linux | 2.4.X | firewall
SEQ(SP=BA-CE%GCD=1-6%ISR=C3-D7%TI=Z%CI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Linux 2.6.18-92cp #1 SMP Wed Feb 4 17:35:21 IST 2009 i686 i686 i386 GNU/Linux, Check Point VPN-1(TM) & FireWall-1(R) R70 - Build 143
Fingerprint Check Point VPN-1 firewall (Linux 2.6.18)
Class Check Point | Linux | 2.6.X | firewall
SEQ(SP=CA-D4%GCD=1-6%ISR=CD-D7%TI=Z%II=I%TS=U)
OPS(O1=M5B4NNSNW7%O2=M5B4NNSNW7%O3=M5B4NW7%O4=M5B4NNSNW7%O5=M5B4NNSNW7%O6=M5B4NNS)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW7%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%S=O%A=S+%F=AS%O=M5B4NNSNW7%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Embedded Linux on a XtremePC. http://www.chippc.com/thin-clients/xtreme-pc/
Fingerprint Chip PC XtremePC thin client
Class Chip PC | Linux || terminal
SEQ(SP=C0-CA%GCD=1-6%ISR=C5-CF%TI=Z%CI=Z%II=I%TS=6)
OPS(O1=M5B4ST11NW4%O2=M5B4ST11NW4%O3=M5B4NNT11NW4%O4=M5B4ST11NW4%O5=M5B4ST11NW4%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Ciperlab 5100 Programmable Data Terminal. http://www.cipherlab.com/catalog.asp?CatID=59&ProdID=41
# Ciperlab A5100 Time and Attendance terminal.
Fingerprint CipherLab 5100 time and attendance terminal
Class CipherLab | embedded || specialized
SEQ(SP=0-2B%GCD=1-6|64|C8|12C|190|1F4%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=A346|900D%RID=G%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Cisco CE590 running Application and Content Networking System Software Release 5.5.5 (build b4 Dec 27 2006)
Fingerprint Cisco Content Engine CE590 running Application and Content Networking System Software 5.5.5
Class Cisco | ACNS | 5.X | proxy server
SEQ(SP=C6-D0%GCD=1-6%ISR=C7-D1%TI=Z%II=I%TS=U)
OPS(O1=M5B4NNS%O2=M578NNS%O3=M280%O4=M218NNS%O5=M218NNS%O6=M109NNS)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%S=O%A=S+%F=AS%O=M109NNS%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=3B-45%TG=40%CD=S)

# Cisco Wide Area Engine WAE-512 running ACNS 5.5.5.4
Fingerprint Cisco WAE-512 Wide Area Application Engine (ACNS 5.5.5.4)
Class Cisco | ACNS | 5.X | proxy server
SEQ(SP=C3-CD%GCD=1-6%ISR=C7-D1%TI=Z%II=I%TS=U)
OPS(O1=|M5B4NNS%O2=|M578NNS%O3=|M280%O4=|M218NNS%O5=|M218NNS%O6=|M109NNS)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=|M5B4NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%S=O%A=O|S+%F=A|AS%O=|M109NNS%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=3B-45%TG=40%CD=S)

# Cisco IronPort C650 running AsyncOS v7.0.1-010.
Fingerprint Cisco IronPort C650 email security appliance (AsyncOS 7.0.1)
Class Cisco | AsyncOS | 7.X | firewall
SEQ(SP=FA-10C%GCD=1-6%ISR=107-111%TS=U)
OPS(O1=M5B4SLL%O2=M5B4SLL%O3=M5B4%O4=M5B4SLL%O5=M5B4SLL%O6=M5B4SLL)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3A-44%TG=40%W=4000%O=M5B4SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3A-44%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3A-44%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3A-44%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3A-44%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3A-44%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3A-44%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3A-44%TG=40%CD=S)

# Cisco Catalyst WS-C5000 Software, Version McpSW: 4.5(1) NmpSW: 4.5(1)
Fingerprint Cisco Catalyst WS-C5000 switch (CatOS 4.5(1))
Class Cisco | CatOS | 4.X | switch
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3C%TG=40%CD=S)

# WS-C2948 Software, Version NmpSW: 6.3(5)
Fingerprint Cisco 2948G switch (CatOS 6.3)
Class Cisco | CatOS | 6.X | switch
SEQ(SP=FE-10A%GCD=1-6%ISR=105-10F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=19-23%TG=20%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3C%TG=40%CD=S)

# Cisco 2820 Switch w/ OS v5.37
Fingerprint Cisco Catalyst 2820 switch (CatOS 5.37)
Class Cisco | CatOS | 6.X | switch
SEQ(SP=42-6A%GCD=1-6%ISR=46-5E%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=U)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=U)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=U)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Cisco Catalyst  Model WS-C6509 with WS-X6K-SUP1A-2GE running CatOS 6.3(3)
Fingerprint Cisco Catalyst WS-C6509 switch (CatOS 6.3)
Class Cisco | CatOS | 6.X | switch
SEQ(SP=F5-FF%GCD=1-6%ISR=108-112%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3C%TG=40%CD=S)

# WS-C6509 Software, Version NmpSW: 8.4(3)
# Cisco Catalyst 4003 CatOS 7.6(17) WS-C4003 Software, Version NmpSW: 7.6(17)
# Cisco Catalyst 4006 CatOS 7.6(17) WS-C4006 Software, Version NmpSW: 7.6(17)
# WS-C2948G with cat4000-k9.8-4-11-GLX
Fingerprint Cisco Catalyst 2948G, 4003, 4006, or 6509 switch (CatOS 7.6(17) - 8.4(3))
Class Cisco | CatOS | 7.X | switch
Class Cisco | CatOS | 8.X | switch
SEQ(SP=FC-108%GCD=1-6%ISR=FA-112%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1000%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# WS-C6506 Software, Version NmpSW: 7.6(16)
Fingerprint Cisco Catalyst WS-C6506 switch (CatOS 7.6(16))
Class Cisco | CatOS | 7.X | switch
SEQ(SP=E5-109%GCD=1-6%ISR=107-111%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1000%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3C%TG=40%CD=S)

# Cisco WS-C4506, Cisco Catalyst Operating System Software, Version 8.1(1)
Fingerprint Cisco Catalyst WS-C4506 switch (CatOS 8.1(1))
Class Cisco | CatOS | 8.X | switch
SEQ(SP=EB-FC%GCD=1-6%ISR=109-10E%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1000%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco Catalist WS-C2950G-24-EI, Software: 12.1(22)EA4a
Fingerprint Cisco Catalyst WS-C2950G switch
Class Cisco | CatOS || switch
SEQ(SP=FB-107%GCD=1-6%ISR=FF-109%TI=Z%II=I|RI%TS=U)
OPS(O1=M218LLNL|M218LLNN|M218NLNL|M218NNLL%O2=M218LLNL|M218LNLL|M218NNLL%O3=M218LLNL|M218NLLN|M218NLNL%O4=M218LLLL|M218LLNL|M218NLLL%O5=M218LLLL|M218LLNN|M218NLLL|M218NNLL%O6=M109LLNL|M109LLNN|M109NLNL|M109NNLL)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M218LLNN|M218NLNL|M218NNLL%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M218LLS|M218LLNL|M218NNLL%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# CISCO 827H
Fingerprint Cisco 827H ADSL router
Class Cisco | embedded || broadband router
SEQ(SP=EF-113%GCD=1-6%ISR=102-114%TI=Z%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# CISCO C827H (MPC855T) ADSL ROUTER, IOS (tm) C820 Software (C820-Y6-M), Version 12.2(15)T5,  RELEASE SOFTWARE (fc1)
Fingerprint Cisco 827H ADSL router
Class Cisco | embedded || broadband router
SEQ(SP=FE-108%GCD=1-6%ISR=106-110%TI=Z%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=4918|8712|9F38|E172|FC57%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Scientific Atlanta WebSTAR EPX2203 cable modem
# WebSTAR EPX2203 (Hardware Version: v2.0) (Software Version: v2.0.2r1152-060125epx2203-v202r1152-060125c-us-5-358.bin)
# Webstar EPX2203 Series cable modem
# ZyXEL ES-1528 Switch Firmware Version V1.12(ARD.3) Not ZynOS as it is not a layer 3 switch, only layer 2.
# Cisco EPC3212, Bootloader Version  2.3.0_R1
Fingerprint Cisco EPC3212 or Scientific Atlanta WebSTAR EPX2203 cable modem
Class Cisco | embedded || broadband router
Class Scientific Atlanta | embedded || broadband router
SEQ(SP=CE-106%GCD=1-6%ISR=F6-10E%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=43E0%W5=4180%W6=403D)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=403D%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Cisco MARS 50, some type of Linux OS
Fingerprint Cisco MARS 50 firewall version 4.2.1
Class Cisco | embedded || firewall
SEQ(SP=C4-CE%GCD=1-6%ISR=C2-CC%TI=Z%II=I%TS=7)
OPS(O1=M55CST11NW0%O2=M55CST11NW0%O3=M55CNNT11NW0%O4=M55CST11NW0%O5=M55CST11NW0%O6=M55CST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M55CNNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP WP110 print server, Firmware Version: 02.00, Firmware Build Date: 2001-09-14, Boot+Version: 01.00, Boot Build Date: 2001-07-23
# The printer is a XEROX Document Centre 405
# Cisco Micro Webserver 200, Cisco MicroWeb II, Software Version: Eclipse 1.0.1(100)
# Tektronix oscilloscope model TDS-3034B, Firmware V3.29. (c) 2001
Fingerprint Cisco Micro Webserver 200, HP WP110 print server, Tektronix TDS3034B oscilloscope, or Xerox Document Centre 405 printer
Class Cisco | embedded || general purpose
Class HP | embedded || print server
Class Tektronix | embedded || specialized
Class Xerox | embedded || printer
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco SCE (Service Control Engine) 2020 (It runs VxWorks (unknown version) internally) Version 3.1.0 Build 108
Fingerprint Cisco SCE 2020 Service Control Engine load balancer
Class Cisco | embedded || load balancer
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M200%O2=M200%O3=M200%O4=M200%O5=M200%O6=M200)
WIN(W1=A000%W2=A000%W3=A000%W4=A000%W5=A000%W6=A000)
ECN(R=Y%DF=N%T=3A-44%TG=40%W=A000%O=M200%CC=N%Q=)
T1(R=Y%DF=N%T=3A-44%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3A-44%TG=40%W=A000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3A-44%TG=40%W=A000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3A-44%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3A-44%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3A-44%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3A-44%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3A-44%TG=40%CD=S)

# Cisco Systems, Inc./VPN 3000 Concentrator Version 4.1.7.O
Fingerprint Cisco VPN 3000 Concentrator VPN platform (software version 4.1.7.O)
Class Cisco | embedded || proxy server
SEQ(SP=D3-DD%GCD=1-6%ISR=DB-E5%TI=RD%II=RI%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=2000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=A05|41CF|41D1|5108|D8A5%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=S)

# Cisco VPN Concentrator, software revision: "Cisco Systems, Inc./VPN 3000 Concentrator Version 4.7.2.D Dec 20 2005 15:26:54"
Fingerprint Cisco VPN 3000 Concentrator VPN platform (software version 4.7.2.D)
Class Cisco | embedded || proxy server
SEQ(SP=D0-DA%GCD=1-6%ISR=DA-E4%TI=I%II=RI%SS=O|S%TS=1|2)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=2000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=127%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=S)

# Cisco Concentrator 3030
Fingerprint Cisco VPN 3030 Concentrator VPN platform
Class Cisco | embedded || proxy server
SEQ(SP=D6-E0%GCD=1-6%ISR=D8-E2%TI=RD%II=RI%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=2000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=245F|7B1F|AC10%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=S)

# Cisco Systems, Inc./VPN 3000 Concentrator Version 4.7.2.F (VPN Concentrator Type: 3030)
Fingerprint Cisco VPN 3030 Concentrator VPN platform (software 4.7.2.F)
Class Cisco | embedded || proxy server
SEQ(SP=CE-D8%GCD=1-6%ISR=CF-D9%TI=RD%II=RI%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=2000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=127|4B53|4BD7%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=S)

# Cisco Wireless LAN Controller model 4402 (management port). sw version is 5.0.148.0.
# Cisco 4400 Series Wireless LAN Controller, AIR-WLC4402-25-K9
Fingerprint Cisco 4402 wireless LAN controller
Class Cisco | embedded || remote management
SEQ(SP=C4-CE%GCD=1-6%ISR=C3-D1%TI=Z%TS=A)
OPS(O1=M56EST11NW2%O2=M56EST11NW2%O3=M56ENNT11NW2%O4=M56EST11NW2%O5=M56EST11NW2%O6=M56EST11)
WIN(W1=1588%W2=1588%W3=1588%W4=1588%W5=1588%W6=1588)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=15B8%O=M56ENNSNW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# c1700-k9o3sy7-mz.124-8.bin
Fingerprint Cisco 1700 router
Class Cisco | embedded || router
SEQ(SP=F9-107%GCD=1-6%ISR=103-10D%TI=RD%II=RI%TS=U)
OPS(O1=M514%O2=M514%O3=M514%O4=M514%O5=M514%O6=M514)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M514%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco 1700 series router
Fingerprint Cisco 1700-series router
Class Cisco | embedded || router
SEQ(SP=FD-10B%GCD=1-6%ISR=FE-10E%TI=Z%CI=I%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco Network Analysis Module (NME-NAM-80S) Software version 4.1(1) RELEASE SOFTWARE [fc2] (Probably Linux --Ed.)
Fingerprint Cisco NME-NAM-80S network analysis module
Class Cisco | embedded || specialized
SEQ(SP=C5-CF%GCD=1-6%ISR=C2-CC%TI=Z%II=I%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Cisco RFGW-1-D Universal Edge QAM Release 02.02.15
Fingerprint Cisco RFGW-1-D radio
Class Cisco | embedded || specialized
SEQ(SP=F2-10A%GCD=1-6%ISR=103-10D%TI=I%II=I%SS=S%TS=U)
OPS(O1=NNM564SNW0%O2=NNM564SNW0%O3=M564NW0%O4=NNM564SNW0%O5=NNM564SNW0%O6=NNM564S)
WIN(W1=2710%W2=2710%W3=2710%W4=2710%W5=2710%W6=2710)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2710%O=NNM564SNW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=80%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=100%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=138%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=Z)

# Cisco 1900 switch
Fingerprint Cisco Catalyst 1900 switch
Class Cisco | embedded || switch
SEQ(SP=E-18%GCD=9C4|1388|1D4C|2710|30D4%ISR=8A-94%TI=I%II=I%SS=S%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=N)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=O|S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Cisco Catalyst 1900 running Cisco Catalyst 1900/2820 Enterprise Edition Software Version V8.01.01
# This device is a Cisco 1900 Series Switch, running IOS v 9.00.04
# RAD (http://www.rad.com) TDM OVER IP MULTIPLEXER IPMUX-1/DC/E1/UPT/STC-E1, Boot version - 1.21, Application version - 4.07
Fingerprint Cisco Catalyst 1900 switch or RAD IPMUX-1 TDM-over-IP multiplexer
Class Cisco | embedded || switch
Class RAD Data Communications | embedded || switch
SEQ(SP=10-84%GCD=9C4|1388|1D4C|2710|30D4|6B6C|D6D8|14244|1ADB0|2191C%ISR=8A-AE%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Cisco Systems Catalyst 1900,V9.00.03, 19XX's runs neither IOS nor CatOS
Fingerprint Cisco Catalyst 1900 Switch, Software v9.00.03
Class Cisco | embedded || switch
SEQ(SP=F2-F6%GCD=1-6%ISR=106-108%TI=I|RD%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Cisco Catalyst 1912 A Switch (FW: V9.00.04)
# It runs neither IOS nor CatOS.
# The MIB says :
# RFC1213-MIB::sysDescr.0 = STRING: "Cisco Systems Catalyst 1900,V9.00.04    "
# RFC1213-MIB::sysObjectID.0 = OID: CISCO-SMI::workgroup.31
# Firmware is: V9.00.04    : Standard Edition
Fingerprint Cisco Catalyst 1912 switch
Class Cisco | embedded || switch
SEQ(SP=13-29%GCD=9C4|1388|1D4C|2710|30D4|3A98%ISR=8A-94%TI=I|RD%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=O|S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Cisco Switch CE500
Fingerprint Cisco Catalyst Express 500 switch
Class Cisco | embedded || switch
SEQ(SP=FF-109%GCD=1-6%ISR=103-10F%TI=RD%CI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M7A6%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# HP Switch: "PROCURVE J9028B" adm Software version PB.02.09, Hardware version R01
# HP ProCurve 1800-24G J9028B running firmware version PB.03.02
# Cisco Small Business Switch SLM2008 Firmware Revision 2.0.0.10
Fingerprint Cisco SLM2008 or HP ProCurve 1800-24G switch
Class Cisco | embedded || switch
Class HP | embedded || switch
SEQ(SP=C-16%GCD=A|14|1E|28|32%ISR=1E-28%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=600%W2=600%W3=600%W4=600%W5=600%W6=600)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=600%O=M5B4%CC=N%Q=|U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=80%S=A%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=100%S=A%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=400%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Cisco Communications Manager 7.1.1
Fingerprint Cisco Unified Communications Manager VoIP gateway
Class Cisco | embedded || VoIP adapter
SEQ(SP=FE-10A%GCD=1-6%ISR=104-112%TI=Z%CI=RD%II=I%TS=A)
OPS(O1=M564ST11NW2%O2=M564ST11NW2%O3=M564NNT11NW2%O4=M564ST11NW2%O5=M564ST11NW2%O6=M564ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=N)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=22-3C%TG=40%W=80%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=21-3D%TG=40%W=100%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=1F-3E%TG=20|40%W=400%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=1E-3E%TG=20|40%W=8000%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=1E-3E%TG=20|40%W=FFFF%S=A%A=S%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Cisco Unified Call Manager 7.1.3.32900-4
Fingerprint Cisco Unified Communications Manager VoIP gateway
Class Cisco | embedded || VoIP adapter
SEQ(SP=C6-D0%GCD=1-6%ISR=C9-D3%TI=Z%II=I%TS=A)
OPS(O1=M5B4ST11NW2%O2=M5B4ST11NW2%O3=M5B4NNT11NW2%O4=M5B4ST11NW2%O5=M5B4ST11NW2%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=N)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# 7936 Cisco IP Conference Station
# CISCO Unified IP Conference Station 7935. Polycom hardware with CISCO software.
Fingerprint Cisco 7935 or 7936 IP Conference State VoIP phone
Class Cisco | embedded || VoIP phone
SEQ(SP=13-1D%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Cisco IP Conference Station Model 7936
Fingerprint Cisco 7936 IP Conference State VoIP phone
Class Cisco | embedded || VoIP phone
SEQ(SP=17-21%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=9C-A6%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M200%O2=M200%O3=M200%O4=M200%O5=M200%O6=M200)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M200%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Cisco IP Phone 7941/7961 Phone,       uname -a reports:      CNU-OS  8.2(1.19) 3.3(0.2) CP-7941G BCM1100-C1(MIPS32)
# Cisco IP Phone 7941 Series
# Cisco IP Phone CP-7911G
# Cisco IP Phone CP-7970G, Version SCCP70.8-2-2SR2S
Fingerprint Cisco IP Phone (7911, 7941, 7961, or 7970)
Class Cisco | embedded || VoIP phone
SEQ(SP=FF-10B%GCD=1-8%ISR=101-111%TI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M578%O4=M578%O5=M578%O6=M578)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=N)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=1B-25%TG=20%W=2000%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=2000%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=2000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=2000%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Cisco IP Phone 7910
Fingerprint Cisco IP Phone 7910
Class Cisco | embedded || VoIP phone
SEQ(SP=0-5%GCD=5800|B000|10800|16000|1B800%ISR=88-92%TI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M578%O4=M578%O5=M578%O6=M578)
WIN(W1=578%W2=578%W3=578%W4=578%W5=578%W6=578)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=578%O=M578%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=578%S=O%A=S+%F=AS%O=M578%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=578%S=Z%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=578%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=578%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=578%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Cisco IP Phone 7911
Fingerprint Cisco IP Phone 7911
Class Cisco | embedded || VoIP phone
SEQ(SP=E5-EF%GCD=C|18|24|30|3C%ISR=105-10F%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M578%O4=M578%O5=M578%O6=M578)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Cisco IP Phone 7912 Series
Fingerprint Cisco IP Phone 7912-series
Class Cisco | embedded || VoIP phone
SEQ(SP=0-35%GCD=1000|2000|3000|4000|5000|B000|16000|21000|2C000|37000%ISR=90-9A%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B0%O2=M5B0%O3=M5B0%O4=M5B0%O5=M5B0%O6=M5B0)
WIN(W1=578%W2=578%W3=578%W4=578%W5=578%W6=578)
ECN(R=Y%DF=N%T=F5-FF%TG=FF%W=578%O=M5B0%CC=N%Q=)
T1(R=Y%DF=N%T=F5-FF%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=F5-FF%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=F5-FF%TG=FF%W=578%S=O%A=S+%F=AS%O=M5B0%RD=0%Q=)
T4(R=Y%DF=N%T=F5-FF%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=F5-FF%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=F5-FF%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=F5-FF%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=F5-FF%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=F5-FF%TG=FF%CD=S)

# Cisco IP Phone 7912G (SCCP) Software Version        6.01.00(051208A)
Fingerprint Cisco IP Phone 7912G
Class Cisco | embedded || VoIP phone
SEQ(SP=FC-106%GCD=1-6%ISR=102-10C%TI=I%II=I%SS=S%TS=U)
OPS(O1=M564%O2=M564%O3=M564%O4=M564%O5=M564%O6=M564)
WIN(W1=578%W2=578%W3=578%W4=578%W5=578%W6=578)
ECN(R=Y%DF=N%T=F6-100%TG=FF%W=578%O=M564%CC=N%Q=)
T1(R=Y%DF=N%T=F6-100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=23-3D%TG=40%W=80%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=23-35%TG=40%W=100%S=A%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=21-2D|33-3E%TG=40%W=400%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=N%T=F6-100%TG=FF%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=21-3D%TG=40%W=8000%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=2B-3F%TG=40%W=FFFF%S=A%A=S+%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=N%T=F6-100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=F6-100%TG=FF%CD=S)

# Cisco IP Phone 7941
Fingerprint Cisco IP Phone 7941
Class Cisco | embedded || VoIP phone
SEQ(SP=101-10B%GCD=1-6%ISR=107-111%TI=I%II=I%SS=S%TS=U)
OPS(O1=M564%O2=M564%O3=M564%O4=M564%O5=M564%O6=M564)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Cisco 7941 phone running SIP firmware 8.3(3)SR2
# Cisco CP-7961G-GE, SCCP41.8-3-3SR2S
# Cisco CP-7941G, SCCP41.8-3-4SR1S
# Cisco IP Phone 7975
Fingerprint Cisco IP Phone 7941, 7961, or 7975
Class Cisco | embedded || VoIP phone
SEQ(SP=C9-109%GCD=1-6%ISR=FE-112%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M578%O4=M578%O5=M578%O6=M578)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Cisco CP-7970G running software SCCP70.8-2-2SR1S
Fingerprint Cisco IP Phone CP-7970G
Class Cisco | embedded || VoIP phone
SEQ(SP=C9-DB%GCD=40|80|C0|100|140%ISR=102-10C%TI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M578%O4=M578%O5=M578%O6=M578)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=N)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=1B-25%TG=20%W=2000%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=2000%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=2000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=2000%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Cisco IP Phone 7905G, SIP Firmware 8.0.0
# Cisco IP Phone 7960 series phone
Fingerprint Cisco Unified IP Phone 7905G or 7960
Class Cisco | embedded || VoIP phone
SEQ(SP=0-1B%GCD=1000|2000|3000|4000|5000|A000|14000|1E000|28000|32000%ISR=90-9A%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B0%O2=M5B0%O3=M5B0%O4=M5B0%O5=M5B0%O6=M5B0)
WIN(W1=3E80%W2=3E80%W3=3E80%W4=3E80%W5=3E80%W6=3E80)
ECN(R=Y%DF=N%T=F5-FF%TG=FF%W=3E80%O=M5B0%CC=N%Q=)
T1(R=Y%DF=N%T=F5-FF%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=F5-FF%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=F5-FF%TG=FF%W=3E80%S=O%A=O|S+%F=A|AS%O=|M5B0%RD=0%Q=)
T4(R=Y%DF=N%T=F5-FF%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=F5-FF%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=F5-FF%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=F5-FF%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=F5-FF%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=F5-FF%TG=FF%CD=S)

Fingerprint Cisco Unified IP Phone 7960
Class Cisco | embedded || VoIP phone
SEQ(SP=102-10C%GCD=1-6%ISR=104-10E%TI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M578%O4=M578%O5=M578%O6=M578)
WIN(W1=578%W2=578%W3=578%W4=578%W5=578%W6=578)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=578%O=M578%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=578%S=O%A=S+%F=AS%O=M578%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=578%S=Z%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=578%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=578%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=578%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Cisco Wireless IP Phone 7920-ETSI
Fingerprint Cisco Wireless IP Phone 7920-ETSI
Class Cisco | embedded || VoIP phone
SEQ(R=N)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=N)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Cisco IOS XR Software, Version 3.4.1[00]
# Cisco IOS XR Software, Version 3.6.2[00] cisco CRS-16/S (7457) processor
Fingerprint Cisco CRS-1 router (IOS XR 3.4.1 - 3.6.2)
Class Cisco | IOS XR | 3.X | router
SEQ(SP=F9-109%GCD=1-6%ISR=100-110%TI=Z%II=RI%TS=U)
OPS(O1=M4D8W0L%O2=M4D8W0L%O3=M280W0L%O4=M218W0L%O5=M218W0L%O6=M109)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=4000%O=M4D8W0L%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IOS (tm) 3000 Software (IGS-I-L), Version 10.3(7), RELEASE SOFTWARE (fc1)
Fingerprint Cisco 3000 switch (IOS 10.3)
Class Cisco | IOS | 10.X | switch
SEQ(R=N)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=N)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=N)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco 2500 (68030) IGS-I-L, Version 11.1(24)
Fingerprint Cisco 2500 router (IOS 11.1)
Class Cisco | IOS | 11.X | router
SEQ(SP=3B-51%GCD=1-6%ISR=9A-A4%TI=Z%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=860%W2=860%W3=860%W4=860%W5=860%W6=860)
ECN(R=Y%DF=N%T=100%TG=FF%W=860%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=100%TG=FF%W=860%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco Internetwork Operating System Software  IOS (tm) C2900XL Software (C2900XL-H-M), Version 11.2(8)SA5, RELEASE SOFTWARE (fc1)
# IOS (tm) C2900XL Software (C2900XL-HS-M), Version 11.2(8.11)SA6, MAINTENANCE INTERIM SOFTWARE
Fingerprint Cisco 2900XL switch (IOS 11.2)
Class Cisco | IOS | 11.X | switch
SEQ(SP=64-94%GCD=1-6%ISR=9A-A4%TI=Z%II=RI%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=10C0%W2=10C0%W3=10C0%W4=10C0%W5=10C0%W6=10C0)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=10C0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=O|S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=10C0%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IOS (tm) C2900XL Software (C2900XL-HS-M), Version 11.2(8.6)SA6
Fingerprint Cisco 2900XL switch (IOS 11.2)
Class Cisco | IOS | 11.X | switch
SEQ(SP=3F-8D%GCD=1-6%ISR=9A-A4%TI=Z%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=10C0%W2=10C0%W3=10C0%W4=10C0%W5=10C0%W6=10C0)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=10C0%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=O%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=10C0%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco WS-C3512-XL
# Cisco IOS (tm) C3500XL Software (C3500XL-C3H2S-M), Version 12.0(5)WC10
# IOS (tm) C2900XL Software (C2900XL-C3H2S-M), Version 12.0(5)WC17, RELEASE SOFTWARE (fc1)
# IOS (tm) C3500XL Software (C3500XL-C3H2S-M), Version 12.0(5)WC17, RELEASE SOFTWARE (fc1)
# Cisco 3548XL switch, IOS 12.0(5)WC16 Enterprise Edition
# IOS (tm) C2600 Software (C2600-I-M), Version 11.3(11b)T5,  RELEASE SOFTWARE (fc1)
# IOS (tm) C2950 Software (C2950-C3H2S-M), Version 12.0(5.3)WC(1)
Fingerprint Cisco Catalyst 2600-, 2900- or 3500 XL-series switch (IOS 11.3 - 12.0)
Class Cisco | IOS | 11.X | switch
Class Cisco | IOS | 12.X | switch
SEQ(SP=ED-10B%GCD=1-6%ISR=102-10E%TI=Z%II=RI%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco IOS Software, SOHO97 Software (SOHO97-K9OY1-M), Version 12.4(25a)
Fingerprint Cisco SOHO 97 ADSL router
Class Cisco | IOS | 12.X | broadband router
SEQ(SP=FD-109%GCD=1-6%ISR=102-10C%TI=RD%CI=RD%II=RI%TS=A)
OPS(O1=M5B4SNNT11LL%O2=M578SNNT11LL%O3=M280T11LL%O4=M218SNNT11LL%O5=M218SNNT11LL%O6=M109SNNT11LL)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M5B4SLL%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco ubr10012 DOCSIS router
Fingerprint Cisco uBR10012 broadband router
Class Cisco | IOS | 12.X | broadband router
SEQ(SP=100-10A%GCD=1-6%ISR=103-10D%TI=RD%CI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=Y%T=FB-105%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=FB-105%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=FB-105%TG=FF%W=1020%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FB-105%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FB-105%TG=FF%CD=S)

# IOS (tm) 10000 Software (UBR10K2-K8P6U2-M), Version 12.3(23)BC4
Fingerprint Cisco 10000 router (IOS 12.3)
Class Cisco | IOS | 12.X | router
SEQ(SP=F9-109%GCD=1-6%ISR=FF-10F%TI=Z%CI=I%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# IOS (tm) C1700 Software (C1700-BNR2SY-M), Version 12.0(0.18)PI, BETA TEST SOFTWARE
Fingerprint Cisco 1700 router (IOS 12.0)
Class Cisco | IOS | 12.X | router
SEQ(SP=33-5D%GCD=1-6%ISR=9A-A4%TI=Z%II=RI%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco 3640 IOS ver 12.4.12
# Cisco 1812 router
# Cisco IOS Software, 3700 Software (C3725-ADVENTERPRISEK9-M), Version 12.4(7), RELEASE SOFTWARE (fc6)
Fingerprint Cisco 1812, 3640, or 3700 router (IOS 12.4)
Class Cisco | IOS | 12.X | router
SEQ(SP=FA-10A%GCD=1-6%ISR=103-10D%TI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# c1841-adventerprisek9-mz.124-24.T2.bin Router Cisco model 1841
Fingerprint Cisco 1841 router (IOS 12)
Class Cisco | IOS | 12.X | router
SEQ(SP=101-10B%GCD=1-6%ISR=105-10F%TI=RD%CI=RD%II=RI%TS=U)
OPS(O1=M55C%O2=M55C%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FB-105%TG=FF%W=1020%O=M55C%CC=N%Q=)
T1(R=Y%DF=N%T=FB-105%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FB-105%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FB-105%TG=FF%CD=S)

# Cisco 1841 IOS 12.4(15)
Fingerprint Cisco 1841 router (IOS 12.4)
Class Cisco | IOS | 12.X | router
SEQ(SP=F4-10C%GCD=1-6%ISR=ED-111%TI=RD%CI=RD|RI%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FB-105%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FB-105%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FB-105%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FB-105%TG=FF%CD=S)

# Cisco IOS (tm) 2500 Software (C2500-P7-L), Version 12.1(27b), RELEASE SOFTWARE (fc1)
Fingerprint Cisco 2500 router (IOS 12.1)
Class Cisco | IOS | 12.X | router
SEQ(SP=F0-10A%GCD=1-6%ISR=100-110%TI=Z%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=100%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco IOS 12.3(24) IP-PLUS featureset on a Cisco 2509 Router
Fingerprint Cisco 2509 router (IOS 12.3)
Class Cisco | IOS | 12.X | router
SEQ(SP=FF-109%GCD=1-6%ISR=106-110%TI=Z%II=RI%TS=U)
OPS(O1=M5B4SLL%O2=M578SLL%O3=M280%O4=M218SLL%O5=M218SLL%O6=M109SLL)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M5B4SLL%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco 2514 router running IOS 12.1(2)
Fingerprint Cisco 2514 router (IOS 12.1)
Class Cisco | IOS | 12.X | router
SEQ(SP=76-80%GCD=1-6%ISR=9A-A4%TI=Z%II=RI%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=100%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# IOS (tm) C2600 Software (C2600-K4P-M), Version 12.0(13.5)S, EARLY DEPLOYMENT MAINTENANCE INTERIM SOFTWARE
Fingerprint Cisco 2600 router (IOS 12.0)
Class Cisco | IOS | 12.X | router
SEQ(SP=4B-79%GCD=1-6%ISR=9A-A4%TI=Z%CI=I%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=10C0%W2=10C0%W3=10C0%W4=10C0%W5=10C0%W6=10C0)
ECN(R=Y%DF=N%T=100%TG=FF%W=10C0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=100%TG=FF%W=10C0%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco IOS C2600 Software (C2600-IS-M) Version 12.1(3a)T4 release software (fc1)
Fingerprint Cisco 2600 router (IOS 12.1)
Class Cisco | IOS | 12.X | router
SEQ(SP=49-57%GCD=1-6%ISR=9A-A4%TI=Z%II=RI%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=100%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco 2611 IOS 12.3(15a)
Fingerprint Cisco 2611 router (IOS 12.3)
Class Cisco | IOS | 12.X | router
SEQ(SP=C7-D1%GCD=1-6%ISR=C6-D0%TI=Z%CI=RD|RI%II=RI%TS=A)
OPS(O1=M5B4ST11%O2=M5B4ST11%O3=M5B4NNT11%O4=M5B4ST11%O5=M5B4ST11%O6=)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=0)
ECN(R=Y%DF=N%T=23-3A%TG=40%W=0%O=%CC=N%Q=R)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=25-39%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco IOS C2600 Software (C2600-I-M), Version 12.3(19) running on a Cisco 2620 router
# Cisco-3620 Cisco Internetwork Operating System Software IOS (tm) 3600 Software (C3620-I-M), Version 12.1(1)
Fingerprint Cisco 2620 or 3620 router (IOS 12.1 - 12.3)
Class Cisco | IOS | 12.X | router
SEQ(SP=100-10A%GCD=1-6%ISR=FE-112%TI=Z%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# IOS (tm) C2600 Software (C2600-I-M), Version 12.0(7)T,  RELEASE SOFTWARE (fc2), cisco 2620 (MPC860), ROM: System Bootstrap, Version 12.1(3r)T2, RELEASE SOFTWARE (fc1)
Fingerprint Cisco 2620 router (IOS 12.0)
Class Cisco | IOS | 12.X | router
SEQ(SP=4F-59%GCD=1-6%ISR=9A-A4%TI=Z%CI=I%II=RI%TS=U)
OPS(O1=M22C%O2=M22C%O3=M22C%O4=M22C%O5=M22C%O6=M22C)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FB-105%TG=FF%W=1020%O=M22C%CC=N%Q=)
T1(R=Y%DF=N%T=FB-105%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FB-105%TG=FF%W=1020%S=O%A=S+%F=AS%O=M22C%RD=0%Q=)
T4(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FB-105%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FB-105%TG=FF%CD=S)

# Cisco IOS Software, 2800 Software (C2800NM-ADVSECURITYK9-M), Version 12.4(15)T7, RELEASE SOFTWARE (fc3)
Fingerprint Cisco 2800 router (IOS 12.4)
Class Cisco | IOS | 12.X | router
SEQ(R=N)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=100%TG=FF%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=A%A=S+%F=AR%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco 2811 Router
Fingerprint Cisco 2811 router (IOS 12.X)
Class Cisco | IOS | 12.X | router
SEQ(SP=FA-10C%GCD=1-6%ISR=FD-10F%TI=RD%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FB-105%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FB-105%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FB-105%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FB-105%TG=FF%CD=S)

# Cisco 2821 running ios c2800nm-advipservicesk9-mz.124-20.YA2.bin
Fingerprint Cisco 2821 router
Class Cisco | IOS | 12.X | router
SEQ(SP=100-10C%GCD=1-6%ISR=102-112%TI=RD|RI%II=RI%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M218%O5=M5B4%O6=M5B4)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco 2821 ISR which is running Call Manager Express
# Cisco 7206 Series VXR router.
# IOS (tm) s72033_rp Software (s72033_rp-IPSERVICESK9-M), Version 12.2(18)SXF6, cisco WS-C6506 (R7000) processor
Fingerprint Cisco 2821, 6506, or 7206VXR router (IOS 12.2)
Class Cisco | IOS | 12.X | router
SEQ(SP=F5-109%GCD=1-6%ISR=FD-10F%TI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FC-106%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FC-106%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FC-106%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FC-106%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FC-106%TG=FF%CD=S)

# Cisco WS-C2960G-24TC-L, Version 12.2(25)SEE1
# Cisco IOS 12.2(2)XA1, EARLY DEPLOYMENT; Running on Cisco cable modem
# Cisco WS-C3750G-48TS-S  Version 12.2(25r)SE1
# Cisco 3750 running Version 12.2(25r)SE1
# Cisco IOS Software, C3560 Software (C3560-IPBASE-M), Version 12.2(25)SEB4, RELEASE SOFTWARE (fc1)
# IOS (tm) C2950 Software (C2950-I6K2L2Q4-M), Version 12.1(22)EA8a, RELEASE SOFTWARE (fc1)
# cisco WS-C2950T-24, System image file is "flash:c2950-i6k2l2q4-mz.121-22.EA9.bin"
# 7200 Software (C7200-BOOT-M), Version 12.0(17)S, EARLY DEPLOYMENT RELEASE SOFTWARE (fc1) (7206VXR router)
# Cisco uBR7111 (CMTS)
# Cisco Cat6509, IOS (tm) MSFC2 Software (C6MSFC2-PK2SV-M), Version 12.1(8a)E5
Fingerprint Cisco 2900-series, 3650, or 3750 switch; 6509 or 7206VXR router; or uBR925 or uBR7111 cable modem (IOS 12.1 - 12.2)
Class Cisco | IOS | 12.X | router
Class Cisco | IOS | 12.X | switch
Class Cisco | IOS | 12.X | broadband router
SEQ(SP=F7-10D%GCD=1-6%ISR=FF-111%TI=Z%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IOS (tm) C2940 Software (C2940-I6Q4L2-M), Version 12.1(22)EA8a, RELEASE SOFTWARE (fc1)
Fingerprint Cisco 2940 router (IOS 12.1)
Class Cisco | IOS | 12.X | router
SEQ(SP=FB-105%GCD=1-6%ISR=100-114%TI=Z%CI=I%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IOS (tm) 2500 Software (C2500-I-L), Version 12.1(27b), RELEASE SOFTWARE (fc1)
# cisco 2509  IOS 12.1(21)
# cisco 2509 IOS 12.1(27a)
# Cisco Catalyst 4948-10GE
# Cisco Catalyst Express 500 with IOS 12.2(25)FY
# Cisco Router 2500 series - IOS (tm) 2500 Software (C2500-IK8S-L), Version 12.2(5), RELEASE SOFTWARE (fc1)
# Cisco Catalyst 3560 Layer3 Switch
# Cisco IOS 12.1 mainline: Cisco Catalyst 5000/5500 RSFC
# cisco WS-C2950C-24 running IOS (tm) C2950 Software (C2950-I6K2L2Q4-M), Version 12.1(22)EA9, RELEASE SOFTWARE (fc1)
# Cisco Router 4500 - IOS (tm) 4500 Software (C4500-JK9S-M), Version 12.2(27), RELEASE SOFTWARE (fc3)
# IOS (tm) C3750 Software (C3750-I9-M), Version 12.2(20)SE4, RELEASE SOFTWARE (fc1)
# C2960 Boot Loader (C2960-HBOOT-M) Version 12.2(25r)SEE1
# Cisco WS-C3550-24-PWR (PowerPC) C3550-I5K2L2Q3-M, Version 12.1(22)EA6
# Catalyst 3550 Series WS-C3550-24-SMI IOS VERSION: 12.2(25)SEB4
# Cisco 4506 Sup 4 running: Catalyst 4000 L3 Switch Software (cat4000-I5K91S-M), Version 12.2(25)EW, RELEASE SOFTWARE (fc1)
# Cisco Catalyst 6506 (IOS 12.2)
# IOS (tm) Catalyst 4000 L3 Switch Software (cat4000-IS-M), Version 12.1(12c)EW1
Fingerprint Cisco 500, 2000-, 3000-, 4000-, 5000-series, or 6506 switch; or 2500- or 4500-series router (IOS 12.1 - 12.2)
Class Cisco | IOS | 12.X | router
Class Cisco | IOS | 12.X | switch
SEQ(SP=F6-107%GCD=1-6%ISR=F5-115%TI=Z%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=100%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# cisco 5300 12.3 IOS
Fingerprint Cisco 5300 router (IOS 12.3)
Class Cisco | IOS | 12.X | router
SEQ(SP=FD-107%GCD=1-6%ISR=108-112%TI=Z%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FB-105%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FB-105%TG=FF%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FB-105%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FB-105%TG=FF%CD=S)

# Cisco 7206VXR (NPE-G2) router running 12.4(11)T
Fingerprint Cisco 7206VXR router (IOS 12.4)
Class Cisco | IOS | 12.X | router
SEQ(SP=FD-107%GCD=1-6%ISR=104-10E%TI=RD%II=RI%TS=A)
OPS(O1=M5A8SNNT11LL%O2=M578SNNT11LL%O3=M280T11LL%O4=M218SNNT11LL%O5=M218SNNT11LL%O6=M109SNNT11LL)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M5B4SLL%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco 7600 router running IOS 12.2(33)SRE
Fingerprint Cisco 7600 router (IOS 12.2)
Class Cisco | IOS | 12.X | router
SEQ(SP=FE-108%GCD=1-6%ISR=107-111%TI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=100%TG=FF%W=1020%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco 857W CISCO857W-G-A-K9 Cisco IOS Software, C850 Software (C850-ADVSECURITYK9-M), Version 12.4(6)T7, RELEASE SOFTWARE (fc5)
# Cisco IOS 12.X version 12.4 Cisco 7301 (NPE)
# Cisco IOS Software, C2600 Software (C2600-ADVSECURITYK9-M), Version 12.4(17)
# Cisco IOS Software, C870 Software (C870-ADVSECURITYK9-M), Version 12.4(4)T7
# Cisco 3825 Version 12.4(13r)T
# Cisco IOS Software, 2800 Software (C2800NM-ADVIPSERVICESK9-M), Version 12.4(9)T1
# Cisco IOS Software, C837 Software (C837-K9O3Y6-M), Version 12.4(16), RELEASE SOFTWARE (fc1)
# Cisco 1801, ios: c180x-advipservicesk9-mz.124-15.T1.bin
# Cisco 2651XM router running 12.4(12a) Advanced Enterprise Services.
# Cisco IOS Software, 3800 Software (C3825-ADVIPSERVICESK9-M), Version 12.4(16b), RELEASE SOFTWARE (fc3)
# Cisco 857 ADSL router running IOS 12.4(6)T8
# Cisco IOS Software, 7200 Software (C7200-ADVIPSERVICESK9-M), Version 12.4(11)T3
# Cisco IOS Software, Catalyst 4000 L3 Switch Software (cat4000-I9S-M), Version 12.2(25)EWA8, RELEASE SOFTWARE (fc1)
# cisco AIR-AP1121G-A-K9 C1100 Software (C1100-K9W7-M), Version 12.3(8)JEB1
# Cisco Aironet 1242AG wireless access point running IOS 12.4(3g)JA
# Cisco 871 (C870-ADVSECURITYK9-M), Version 12.4(4)T7.
Fingerprint Cisco 800-series, 1801, 2000-series, 3800, 4000, or 7000-series router; or 1100 or 1242G WAP (IOS 12.2 - 12.4)
Class Cisco | IOS | 12.X | router
Class Cisco | IOS | 12.X | WAP
SEQ(SP=FD-109%GCD=1-6%ISR=103-111%TI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco 1712 router running IOS 12.2(15)
# Cisco 806 <IOS (tm) C806 Software (C806-OY6-M), Version 12.2(8)T5,RELEASE SOFTWARE (fc1)>
# Cisco 1721 router IOS (tm) C1700 Software (C1700-Y-M), Version 12.2(4)YA2, EARLY DEPLOYMENT RELEASE SOFTWARE (fc1)
# IOS (tm) C2600 Software (C2600-IPVOICE-M), Version 12.3(3)
Fingerprint Cisco 806, 1712, 1721, or 2600 router (IOS 12.2 - 12.3)
Class Cisco | IOS | 12.X | router
SEQ(SP=F6-10A%GCD=1-6%ISR=FD-10F%TI=Z%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-105%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-105%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-105%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-105%TG=FF%W=1020%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=FA-105%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-105%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-105%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-105%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-105%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-105%TG=FF%CD=S)

# IOS (tm) C820 Software (C820-K9OSV6Y6-M), Version 12.3(20), RELEASE SOFTWARE (fc2)
# IOS (tm) 2500 Software (C2500-IS-L), Version 12.3(23), RELEASE SOFTWARE (fc5)
# Cisco 1721 router running IOS version 12.3(6c)
# Cisco 1751 router with IOS 12.3(14)T6.
# Cisco 1750 router (IOS 12.3)
Fingerprint Cisco 820, 1721, 1750, 1751, or 2514 router (IOS 12.3)
Class Cisco | IOS | 12.X | router
SEQ(SP=E2-107%GCD=1-6%ISR=108-10C%TI=Z%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco IOS Software, C831 Software (C831-K9O3SY6-M), Version 12.4(15)T10
# Cisco IOS 12.4(25b) on a 1760 router
Fingerprint Cisco 831 switch or 1760 router (IOS 12.4)
Class Cisco | IOS | 12.X | router
Class Cisco | IOS | 12.X | switch
SEQ(SP=F8-108%GCD=1-6%ISR=100-112%TI=RD%CI=RD|RI%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco IOS Software, C836 Software (C836-K9O3S8Y6-M), Version 12.4(23), RELEASE SOFTWARE (fc1), ROM: System Bootstrap, Version 12.2(11r)YV, RELEASE SOFTWARE (fc1)
# Cisco IOS Software, 1841 Software (C1841-ADVENTERPRISEK9-M), Version 12.4(24)T, RELEASE SOFTWARE (fc1)
# Cisco IOS Software, 2800 Software (C2800NM-ADVENTERPRISEK9-M), Version 12.4(23), RELEASE SOFTWARE (fc1)
# Cisco 1751 router running IOS 12.4.23 with ADSL feature set.
# Cisco IOS Software, 1841 Software (C1841-ADVENTERPRISEK9-M), Version 15.0(1)M
# Cisco IOS Software, C890 Software (C890-UNIVERSALK9-M), Version 12.4(22)YB, RELEASE SOFTWARE (fc2), Cisco 891 (MPC8300) processor (revision 1.0)
Fingerprint Cisco 836, 890, 1751, 1841, or 2800 router (IOS 12.4 - 15.0)
Class Cisco | IOS | 12.X | router
SEQ(SP=F6-10C%GCD=1-6%ISR=FF-111%TI=RD%CI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco IOS Software, C860 Software (C860-UNIVERSALK9-M), Version 12.4(15)XZ2
# Cisco IOS Software, C870 Software (C870-ADVSECURITYK9-M), Version 12.4(24)T
Fingerprint Cisco 860 or 870 router (IOS 12.4)
Class Cisco | IOS | 12.X | router
SEQ(SP=F4-10A%GCD=1-6%ISR=104-112%TI=RD%CI=RD|RI%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco IOS Software, C870 Software (C870-ADVIPSERVICESK9-M), Version 12.4(15)T1, RELEASE SOFTWARE (fc2)
Fingerprint Cisco 870 router (IOS 12.4)
Class Cisco | IOS | 12.X | router
SEQ(SP=FA-104%GCD=1-6%ISR=FA-104%TI=RD%CI=RD%II=RI%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M578%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco sw2960 + IOS 12.2(46)SE
# Cisco IOS Software, C870 Software (C870-ADVIPSERVICESK9-M), Version 12.4(4)T8, RELEASE SOFTWARE (fc3)
Fingerprint Cisco 870 router or 2960 switch (IOS 12.2 - 12.4)
Class Cisco | IOS | 12.X | router
Class Cisco | IOS | 12.X | switch
SEQ(SP=FF-109%GCD=1-6%ISR=100-112%TI=RD|RI%II=RI%SS=O%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco Router 877, 124-15.T11
Fingerprint Cisco 877 router (IOS 12.4)
Class Cisco | IOS | 12.X | router
SEQ(SP=FD-10B%GCD=1-6%ISR=105-10F%TI=RD%II=RI%TS=U)
OPS(O1=M591%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FB-105%TG=FF%W=1020%O=M591%CC=N%Q=)
T1(R=Y%DF=N%T=FB-105%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FB-105%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FB-105%TG=FF%CD=S)

# Cisco 2610XM IOS 12.4(19b) Advanced Security Feature Set c2600-advsecurityk9-mz.124-19b.bin
# Cisco Aironet 1200 Series (AIR-LAP-1232AG-E-K9)
# Cisco Aironet 1250 Series (AIR-AP1252AG-A-K9) Software version: 12.4(10b)JDA3
Fingerprint Cisco Aironet 1200-series WAP or 2610XM router (IOS 12.4)
Class Cisco | IOS | 12.X | router
Class Cisco | IOS | 12.X | WAP
SEQ(SP=FE-108%GCD=1-6%ISR=FC-112%TI=RD%CI=RD|RI%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco 1811 Router, IOS 12.4(6)T6
# Cisco IOS Software, 2800 Software (C2800NM-ADVIPSERVICESK9-M), Version 12.4(11)T2
# Cisco IOS Software, C1250 Software (C1250-K9W7-M), Version 12.4(10b)JA1, RELEASE SOFTWARE (fc2)
# Cisco Aironet 1240AG Series Access Point
# Cisco VG 224 Analog Phone Gateway
Fingerprint Cisco Aironet 1240AG or 1250 WAP, 1811 or 2800 router, or VG 224 VoIP gateway (IOS 12.4)
Class Cisco | IOS | 12.X | router
Class Cisco | embedded || VoIP adapter
SEQ(SP=F7-10D%GCD=1-6%ISR=FE-110%TI=RD%CI=RD|RI%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco Aironet 1200 Air-AP1220
# Cisco IOS Software, C831 Software (C831-K9O3Y6-M), Version 12.3(2)XE3, RELEASE SOFTWARE (fc1)
Fingerprint Cisco Aironet 350 or 1200 WAP or 831 router (IOS 12.3)
Class Cisco | IOS | 12.X | router
Class Cisco | IOS | 12.X | WAP
SEQ(SP=102-10E%GCD=1-6%ISR=103-10D%TI=Z%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco IOS (tm) 3600 Software (C3620-IK9O3S6-M), Version 12.3(16), RELEASE SOFTWARE (fc 4)
Fingerprint Cisco C3620 router (IOS 12.3)
Class Cisco | IOS | 12.X | router
SEQ(SP=FD-107%GCD=1-6%ISR=103-10F%TI=Z%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=7B-85%TG=80%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco IOS Software, C870 Software (C870-ADVSECURITYK9-M), Version 12.4(15)T5, RELEASE SOFTWARE (fc4)
Fingerprint Cisco C870 router (IOS 12.4)
Class Cisco | IOS | 12.X | router
SEQ(SP=FC-106%GCD=1-6%ISR=107-111%TI=RD%CI=RD%TS=A)
OPS(O1=T11LL|M5A8SNNW2NT11LLLLLL%O2=T11LL|M578SNNW2NT11LLLLLL%O3=T11LL|M280W2NT11LLLLS|M280W2NT11LLLLLL%O4=T11LL|M218SNNW2NT11LLLLLL%O5=T11LL|M218SNNW2NT11LLLLLL%O6=T11LL|M109SNNT11LL)
WIN(W1=FF3C|FFFF%W2=FF3C|FFFF%W3=FF3C|FFFF%W4=FF3C|FFFF%W5=FF3C|FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=FB-105%TG=FF%W=FF3C|FFFF%O=|M5B4SNNW2LLLLL%CC=N|Y%Q=)
T1(R=Y%DF=N%T=FB-105%TG=FF%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A|O%A=O|S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A|O%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A|O%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FB-105%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FB-105%TG=FF%CD=S)

# Cisco DOCSIS CMTS running IOS 12.1  (this is a cable modem termination server)
# IOS (tm) 7200 Software (UBR7200-IK1S-M), Version 12.1(8.5)EC, EARLY DEPLOYMENT MAINTENANCE INTERIM SOFTWARE
Fingerprint Cisco DOCSIS cable modem termination server (IOS 12.1)
Class Cisco | IOS | 12.X | specialized
SEQ(SP=F8-FF%GCD=1-6%ISR=107-109%TI=Z%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco 2924-XL Switch running IOS C2900XL Software (C2900XL-C3H2S-M), Version 12.0(5)XU, RELEASE SOFTWARE (fc1)
# IOS (tm) 2500 Software (C2500-D-L), Version 12.0(10), RELEASE SOFTWARE (fc1)
Fingerprint Cisco 2500 or 2924XL switch (IOS 12.0)
Class Cisco | IOS | 12.X | switch
SEQ(SP=7D-9D%GCD=1-6%ISR=9A-A4%TI=Z%II=RI%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IOS (tm) C2900XL Software (C2900XL-C3H2S-M), Version 12.0(5)WC17, RELEASE SOFTWARE (fc1)
Fingerprint Cisco 2900XL switch (IOS 12.0)
Class Cisco | IOS | 12.X | switch
SEQ(SP=100-10A%GCD=1-6%ISR=104-112%TI=Z%II=RI%TS=U)
OPS(O1=M22CSLL%O2=M22CSLL%O3=M22CSLL%O4=M22CSLL%O5=M22CSLL%O6=M22CSLL)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M22CSLL%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M22CSLL%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco WS-C2924M-XL (PowerPC403GA) C2900XL-C3H2S-M, Version 12.0(5)WC16
# IOS (tm) C3500XL Software (C3500XL-C3H2S-M), Version 12.0(5)WC16, Release Software (fc1)
# WS-C2924-XL-A Version 12.0(5)WC17
# IOS (tm) C2950 Software (C2950-C3H2S-M), Version 12.0(5.3)WC(1), MAINTENANCE INTERIM SOFTWARE
Fingerprint Cisco 2924M XL, 2950, or 3500XL switch (IOS 12.0)
Class Cisco | IOS | 12.X | switch
SEQ(SP=FE-10A%GCD=1-6%ISR=FA-110%TI=Z%II=RI%TS=U)
OPS(O1=M22C%O2=M22C%O3=M22C%O4=M22C%O5=M22C%O6=M22C)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M22C%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M22C%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# C2950 software (C2950-I6Q4L2-M) Version 12.1(22)EA4a
Fingerprint Cisco 2950 switch (IOS 12.1)
Class Cisco | IOS | 12.X | switch
SEQ(SP=FD-107%GCD=1-6%ISR=104-112%TI=Z%II=RI%TS=U)
OPS(O1=M5B4LLNN%O2=M578LLNN%O3=M280LLNN%O4=M218LLNN%O5=M218LLNN%O6=M109LLNL|M109LLNN|M109NNLL)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4LLNN%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4LLNN%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IOS (tm) C2950 Software (C2950-I6Q4L2-M), Version 12.1(22)EA4a
Fingerprint Cisco 2950 switch (IOS 12.1)
Class Cisco | IOS | 12.X | switch
SEQ(SP=FF-109%GCD=1-6%ISR=105-10F%TI=Z%CI=I%II=RI%TS=U)
OPS(O1=M218LLLL|M218LLLN%O2=M218LLLL|M218LNLL%O3=M218LSL|M218LLLL|M218LNLL%O4=M218LSL|M218LLLL|M218LLLN%O5=M218LSL|M218LLLL|M218LLLN%O6=M109LLLL|M109LLLN)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M218LLLN|M218LNLL%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M218LLLN|M218LNLL%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# cisco 2950-24 IOS 12.1(22)EA13, Standard Image
Fingerprint Cisco 2950 switch (IOS 12.1)
Class Cisco | IOS | 12.X | switch
SEQ(SP=FD-107%GCD=1-6%ISR=10A-114%TI=RD%CI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=O%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IOS (tm) C2950 Software (C2950-I6Q4L2-M), Version 12.1(22)EA4
Fingerprint Cisco 2950 switch (IOS 12.1)
Class Cisco | IOS | 12.X | switch
SEQ(SP=FC-106%GCD=1-6%ISR=100-10A%TI=Z%CI=I%II=RI%TS=U)
OPS(O1=M5B4LLLL%O2=M578LLLL%O3=M280LLLL|M280LLNN%O4=M218LLLL%O5=M218LLLL|M218LLNN%O6=M109LLLL)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4LLLL%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4LLLL%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IOS (tm) C2950 Software (C2950-I6Q4L2-M), Version 12.1(22)EA4a, RELEASE SOFTWARE (fc1)
Fingerprint Cisco 2950 switch (IOS 12.1)
Class Cisco | IOS | 12.X | switch
SEQ(SP=F4-10A%GCD=1-6%ISR=F8-112%TI=Z%CI=I%II=RI%TS=U)
OPS(O1=M5B4LLLL|M5B4LLNL%O2=M578LLLN|M578LLNL%O3=M280LLLL|M280LLLN|M280LLNL%O4=M218LLLN|M218LLNL|M218NLLL%O5=M218LLLL|M218LLLN|M218LLNL%O6=M109LLLN|M109LLNL)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4LLLN|M5B4LLNL%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4LLLN|M5B4LLNL%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IOS (tm) C2950 Software (C2950-I6Q4L2-M), Version 12.1(22)EA4a, RELEASE SOFTWARE (fc1)
Fingerprint Cisco 2950 switch (IOS 12.1)
Class Cisco | IOS | 12.X | switch
SEQ(SP=FD-10B%GCD=1-6%ISR=103-10D%TI=Z%CI=I%II=RI%TS=U)
OPS(O1=M218LLLN|M218LLNL%O2=M218LLLN|M218LLNL%O3=|M218LLLN|M218LLNL%O4=|M218LLLN|M218LLNL%O5=|M218LLLN|M218LLNL%O6=|M109LLNL)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M218LLNL|M218NLLL%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco Catalyst WS-C3750G-12S-E IOS 12.2(35)SE2
# cisco WS-C2950C-24 IOS (tm) C2950 Software (C2950-I6K2L2Q4-M), Version 12.1(22)EA10a
# IOS (tm) C2950 Software (C2950-I6K2L2Q4-M), Version 12.1(22)EA10a, RELEASE SOFTWARE (fc2)
# cisco 6509 IOS 122-18.SXF1
# Cisco IOS Software, C3750 Software (C3750-ADVIPSERVICESK9-M), Version 12.2(35)SE2, RELEASE SOFTWARE (fc1)
# 6500 Switch
# Cisco Catalyst 4510R Switch
# Cisco IOS 12.1E: Catalyst 6000
# Cisco IOS Software, C3560 Software (C3560-ADVIPSERVICESK9-M), Version 12.2(44)SE, RELEASE SOFTWARE (fc1)
# Cisco IOS Software, C3550 Software (C3550-IPSERVICESK9-M), Version 12.2(44)SE2
# NME-16ES-1G, IOS 12.2(25)SEE4, C3750-IPSERVICESK9-M
# cisco WS-C2960-8TC-L (PowerPC405) processor (revision A0)
Fingerprint Cisco 2950, 2960, 3000-series, 4510R, 6000-series, or 6500-series switch (IOS 12.1 or 12.2)
Class Cisco | IOS | 12.X | switch
SEQ(SP=FA-108%GCD=1-6%ISR=100-110%TI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=100%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# model: WS-C2960G-24TC-L sw version: 12.2(50)SE1
# IOS (tm) C2950 Software (C2950-I6K2L2Q4-M), Version 12.1(22)EA13
# Cisco IOS Software, C3550 Software (C3550-IPSERVICESK9-M), Version 12.2(50)SE3
# Cisco IOS Software, C3560 Software (C3560-IPSERVICESK9-M), Version 12.2(50)SE3
Fingerprint Cisco 2950, 2960, 3550, 3560, or 3750 switch (IOS 12.1 - 12.2)
Class Cisco | IOS | 12.X | switch
SEQ(SP=FD-10F%GCD=1-6%ISR=104-110%TI=RD%CI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco IOS Software, C3750 Software (C3750-IPSERVICESK9-M), Version 12.2(50)SE2, RELEASE SOFTWARE (fc2)
# Cisco IOS (tm) C2950 Software (C2950-I6K2L2Q4-M), Version 12.1(22)EA12, RELEASE SOFTWARE (fc1)
# Cisco IOS Software, C3560 Software (C3560-IPBASEK9-M), Version 12.2(46)SE, RELEASE SOFTWARE (fc2)
# Cisco IOS Software, C3550 Software (C3550-IPBASEK9-M), Version 12.2(46)SE, RELEASE SOFTWARE (fc2)
# Cisco IOS Software, C2960 Software (C2960-LANBASEK9-M), Version 12.2(46)SE, RELEASE SOFTWARE (fc2)
Fingerprint Cisco 2950, 2960, 3550, 3560, or 3750 switch (IOS 12.1 - 12.2)
Class Cisco | IOS | 12.X | switch
SEQ(SP=F2-10C%GCD=1-6%ISR=FE-10E%TI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FB-105%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FB-105%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FB-105%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FB-105%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FB-105%TG=FF%CD=S)

# Cisco catalyst 3500 XL
Fingerprint Cisco 3500 switch
Class Cisco | IOS | 12.X | switch
SEQ(SP=F6-108%GCD=1-6%ISR=FE-10E%TI=Z%II=RI%TS=A)
OPS(R=N)
WIN(R=N)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M5B4SNN%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=100%TG=FF%W=1020%S=O%A=S+%F=AS%O=M109SNNT11LL%RD=0%Q=)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco IOS Software, C3560 Software (C3560-IPBASEK9-M), Version 12.2(25)SEE3, RELEASE SOFTWARE (fc2)
Fingerprint Cisco 3560 switch (IOS 12.2)
Class Cisco | IOS | 12.X | switch
SEQ(SP=100-10A%GCD=1-6%ISR=104-110%TI=Z%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=100%TG=FF%W=1020%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco 3560G-24TS
Fingerprint Cisco 3560G switch (IOS 12.2)
Class Cisco | IOS | 12.X | switch
SEQ(SP=FB-105%GCD=1-6%ISR=104-10E%TI=Z%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco IOS Software, C3750E Software (C3750E-UNIVERSALK9-M), Version 12.2(44)
# Cisco 6500 supervisor 720 IOS ver 12.2(33)
Fingerprint Cisco 3750 or 6500 switch (IOS 12.2)
Class Cisco | IOS | 12.X | switch
SEQ(SP=102-10C%GCD=1-6%ISR=103-10D%TI=RD%CI=RD|RI%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=Y%T=100%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=100%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco IOS Software, C3750 Software (C3750-IPBASE-M), Version 12.2(25)SEB4
Fingerprint Cisco 3750 switch (IOS 12.2)
Class Cisco | IOS | 12.X | switch
SEQ(SP=FB-107%GCD=1-6%ISR=FE-112%TI=Z%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco IOS Software, C3750 Software (C3750-IPSERVICESK9-M), Version 12.2(46)SE, RELEASE SOFTWARE (fc2)
# Cisco IOS Software, C880 Software (C880DATA-UNIVERSALK9-M), Version 15.0(1)XA2, RELEASE SOFTWARE (fc2)
Fingerprint Cisco 880 router (IOS 15.0) or 3750 switch (IOS 12.2)
Class Cisco | IOS | 12.X | switch
Class Cisco | IOS | 15.X | router
SEQ(SP=FF-109%GCD=1-6%ISR=FC-10E%TI=RD%II=RI%TS=U)
OPS(O1=M564%O2=M564%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M564%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FC-106%TG=FF%W=80%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FC-106%TG=FF%W=100%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FC-106%TG=FF%W=400%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FC-106%TG=FF%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FC-106%TG=FF%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# WS-C2912-XL-A Version 12.0(5)XU
Fingerprint Cisco Catalyst 2912 switch (IOS 12.0)
Class Cisco | IOS | 12.X | switch
SEQ(SP=65-8F%GCD=1-6%ISR=9A-A4%TI=Z%II=RI%TS=U)
OPS(O1=M22C%O2=M22C%O3=M22C%O4=M22C%O5=M22C%O6=M22C)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M22C%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M22C%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Catalyst 2950 series 48 Port
Fingerprint Cisco Catalyst 2950 switch
Class Cisco | IOS | 12.X | switch
SEQ(SP=FE-108%GCD=1-6%ISR=102-114%TI=Z%II=RI%TS=U)
OPS(O1=M5B4LLLL|M5B4LLNL%O2=M578LLLL|M578LLNL%O3=M280LLLL|M280LLNL%O4=M218LLLL|M218LLNL|M218NLLL%O5=M218LLLL|M218LLNL%O6=M109LLLL|M109LLNL|M109NLLL)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4LLNL%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# WS-C2950-24, Version 12.1(22)EA13
# IOS (tm) C2950 Software (C2950-I6K2L2Q4-M), Version 12.1(22)EA13
Fingerprint Cisco Catalyst 2950 switch (IOS 12.1)
Class Cisco | IOS | 12.X | switch
SEQ(SP=FD-10B%GCD=1-6%ISR=102-112%TI=RD%CI=RD|RI%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco Catalyst 2950 Series WS-C2950-12
Fingerprint Cisco Catalyst 2950-series switch
Class Cisco | IOS | 12.X | switch
SEQ(SP=100-10A%GCD=1-6%ISR=103-10D%TI=Z%II=RI%TS=U)
OPS(O1=%O2=M578LLLN%O3=M280LLLN%O4=%O5=M218LLLN%O6=M109LLLL)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4LLLN%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4LLLN%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# CIsco 2960
# IOS (tm) 3600 Software (C3640-IK9S-M), Version 12.3(20), RELEASE SOFTWARE (fc2)
Fingerprint Cisco Catalyst 2960 or 3600 switch
Class Cisco | IOS | 12.X | switch
SEQ(SP=FE-108%GCD=1-6%ISR=102-10C%TI=Z%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco IOS 12.2(44)SE running on a Cisco Catalyst 2960 switch
Fingerprint Cisco Catalyst 2960 switch (IOS 12.2)
Class Cisco | IOS | 12.X | switch
SEQ(SP=F9-109%GCD=1-6%ISR=107-111%TI=RD%II=RI%TS=U)
OPS(O1=M5A8SNNT11LL%O2=M578SNNT11LL%O3=|M280SNNLLLLLLLL|M280SNNNLLLLLLL%O4=M218SNNT11LL%O5=M218SNNT11LL%O6=M109SNNT11LL)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4SNN%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco Catalyst 2960 IOS 12.2(35)SE5
# cisco 2960 8 port switch
Fingerprint Cisco Catalyst 2960 switch (IOS 12.2)
Class Cisco | IOS | 12.X | switch
SEQ(SP=102-10C%GCD=1-6%ISR=102-112%TI=RD%CI=I%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# 12.2(55)SE on Cisco Switch WS-X2960-24TT-L
Fingerprint Cisco Catalyst 2960 switch (IOS 12.2)
Class Cisco | IOS | 12.X | switch
SEQ(SP=F5-109%GCD=1-6%ISR=106-112%TI=RD%CI=RD%II=RI%TS=A|U)
OPS(O1=M5B4SNNT11LL%O2=M578SNNT11LL%O3=M280SNNLLLLLLLL%O4=M218SNNT11LL%O5=M218SNNT11LL%O6=M109SNNT11LL)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4SNN%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5E2%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# WS-C3550-24-SMI, Version 12.2(50)SE
# Cisco IOS Software, C3560 Software (C3560-IPSERVICESK9-M), Version 12.2(50)SE
# cisco catalyst c2960
Fingerprint Cisco Catalyst 2960, 3550, or 3560 switch (IOS 12.2)
Class Cisco | IOS | 12.X | switch
SEQ(SP=FD-107%GCD=1-6%ISR=103-113%TI=RD|RI%II=RI%SS=O%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco IOS Software, C2960 Software (C2960-LANBASE-M), Version 12.2(35)SE5, RELEASE SOFTWARE (fc1)
# Cisco IOS Version 12.2(18)SXF8 running on Supervisor II / MSFC II module in a Cisco Catalyst 6500 switch
# Cisco WS-C3560-48PS
# Cisco IOS Software, C3560 Software (C3560-ADVIPSERVICESK9-M), Version 12.2(25)SEE4
Fingerprint Cisco Catalyst 2960, 3560, or 6500 switch (IOS 12.2)
Class Cisco | IOS | 12.X | switch
SEQ(SP=FF-109%GCD=1-6%ISR=100-10E%TI=RD%CI=RD|RI%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=100%TG=FF%W=1020%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# C3500XL Software (C3500XL-C3H2S-M), Version 12.0(5)WC15
Fingerprint Cisco Catalyst 3500 XL switch (IOS 12.0)
Class Cisco | IOS | 12.X | switch
SEQ(SP=DE-100%GCD=1-6%ISR=105-10F%TI=Z%II=RI%TS=U)
OPS(O1=M22C%O2=M22C%O3=M22C%O4=M22C%O5=M22C%O6=M22C)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M22C%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IOS (tm) C3550 Software (C3550-I9Q3L2-M), Version 12.1(22)EA1a
Fingerprint Cisco Catalyst 3550 switch (IOS 12.1)
Class Cisco | IOS | 12.X | switch
SEQ(SP=FB-10B%GCD=1-6%ISR=108-112%TI=Z%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=100%TG=FF%W=1020%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Cisco IOS Software, C3550 Software (C3550-IPBASEK9-M), Version 12.2(44)SE2, RELEASE SOFTWARE (fc2)
Fingerprint Cisco Catalyst 3550 switch (IOS 12.2)
Class Cisco | IOS | 12.X | switch
SEQ(SP=FA-108%GCD=1-6%ISR=103-10D%TI=RD%CI=RD|RI%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco Catalyst 6509 (setup to perform routing)
# IOS (tm) c6sup2_rp Software (c6sup2_rp-JK2S-M), Version 12.1(26)E4, RELEASE SOFTWARE (fc1)
# Cisco Catalyst 6500 running 12.1(11r)E1, RELEASE SOFTWARE (fc1)
# Cisco Catalyst 3560 switch [WS-C3560-48PS] running IOS 12.2(35)SE1.
Fingerprint Cisco Catalyst 3560 or 6500-series switch (IOS 12.1 - 12.2)
Class Cisco | IOS | 12.X | switch
SEQ(SP=E6-107%GCD=1-6%ISR=105-114%TI=RD%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# 6513-core-switch# Cisco IOS Software, s72033_rp Software (s72033_rp-ADVENTERPRISEK9_WAN-M), Version 12.2(33)SXI
# Cisco IOS Software, Catalyst 4500 L3 Switch Software (cat4500e-IPBASEK9-M), Version 12.2(52)XO, RELEASE SOFTWARE (fc1)
# WS-C3560X-48       12.2(53)SE2           C3560E-UNIVERSALK9-M
Fingerprint Cisco Catalyst 3560, 4500, or 6513 swich (IOS 12.2)
Class Cisco | IOS | 12.X | switch
SEQ(SP=F8-10C%GCD=1-6%ISR=106-110%TI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IOS 12.2(33)SXI3 running on 6509-E
Fingerprint Cisco Catalyst 6509-E switch (IOS 12.2)
Class Cisco | IOS | 12.X | switch
SEQ(SP=FB-105%GCD=1-6%ISR=102-10C%TI=RD%CI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=8000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco LS1010 Cat8510MSR WA5-5 Software (Cat8510M-WP-M), Version 12.0(10)W5(18b)
Fingerprint Cisco Catalyst 8510MSR switch (IOS 12.0)
Class Cisco | IOS | 12.X | switch
SEQ(SP=48-5C%GCD=1-6%ISR=9A-A4%TI=Z%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=100%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=100%TG=FF%W=1020%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Catalyst Express 500
Fingerprint Cisco Catalyst Express 500 switch
Class Cisco | IOS | 12.X | switch
SEQ(SP=FA-108%GCD=1-6%ISR=103-10D%TI=Z%CI=I%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M7A6%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco Catalyst Express 500, IOS 12.2(25)SEG
Fingerprint Cisco Catalyst Express 500 switch (IOS 12.2)
Class Cisco | IOS | 12.X | switch
SEQ(SP=100-10A%GCD=1-6%ISR=109-113%TI=Z%CI=I%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Catalyst Express 520
Fingerprint Cisco Catalyst Express 520 switch
Class Cisco | IOS | 12.X | switch
SEQ(SP=100-10A%GCD=1-6%ISR=104-10E%TI=RD%CI=I%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1020%S=O%A=S+%F=AS%O=M7A6%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# cisco 1131AG wireless access point running IOS 12.3(8)JA2
Fingerprint Cisco 1131AG WAP (IOS 12.3)
Class Cisco | IOS | 12.X | WAP
SEQ(SP=FF-109%GCD=1-6%ISR=109-113%TI=Z%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR|EAR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R|ER%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR|EAR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR|EAR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Aironet 1130 (AIR-AP1131AG-A-K9) rinning IOS 12.4(3g)JA (c1130-k9w7-tar.124-3g.JA)
Fingerprint Cisco Aironet 1130 WAP (IOS 12.4)
Class Cisco | IOS | 12.X | WAP
SEQ(SP=101-10B%GCD=1-6%ISR=107-111%TI=RD%CI=I%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco Aironet 1200 IOS Version  12.3(2)JA4
Fingerprint Cisco Aironet 1200 WAP (IOS 12.3)
Class Cisco | IOS | 12.X | WAP
SEQ(SP=F9-109%GCD=1-6%ISR=106-110%TI=Z%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco Aironet 1200 Series (AIR-LAP-1232AG-E-K9)
Fingerprint Cisco Aironet 1200 WAP (IOS 12.3)
Class Cisco | IOS | 12.X | WAP
SEQ(SP=100-10A%GCD=1-6%ISR=101-10F%TI=RD%CI=RD|RI%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=EAR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=ER%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=EAR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# cisco AIR-AP1232AG-E-K9 Cisco IOS Software, C1200 Software (C1200-K9W7-M), Version 12.3(7)JA2, RELEASE SOFTWARE (fc1)
# Cisco IOS Software, C1240 Software (C1240-K9W7-M), Version 12.3(8)JA2, RELEASE SOFTWARE (fc1)
Fingerprint Cisco Aironet 1230 or 1240-series WAP (IOS 12.3)
Class Cisco | IOS | 12.X | WAP
SEQ(SP=CF-10D%GCD=1-6%ISR=101-10D%TI=Z%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco AP1231G 12.3(8)JEC2 IOS Filename: c1200-k9w7-mx.123-8.JEC2
Fingerprint Cisco Aironet 1231G WAP (IOS 12.3)
Class Cisco | IOS | 12.X | WAP
SEQ(SP=FC-106%GCD=1-6%ISR=103-10F%TI=Z%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=80%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=100%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco Aironet 1240AG Access Point running system software 12.4(10b)JA
Fingerprint Cisco Aironet 1240AG WAP
Class Cisco | IOS | 12.X | WAP
SEQ(SP=F3-10D%GCD=1-6%ISR=F7-10D%TI=RD%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Aironet 1250 series running IOS 12.4
Fingerprint Cisco Aironet 1250 WAP (IOS 12.4)
Class Cisco | IOS | 12.X | WAP
SEQ(SP=FB-105%GCD=1-6%ISR=FE-10E%TI=RD%CI=RD|RI%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco IOS Software, C350 Software (C350-K9W7-M), Version 12.3(8)JA2, RELEASE SOFTWARE (fc1) / Cisco Aironet 350
# IOS 12.3(7)JA2 on a Cisco Aironet model AIR-AP1131AG-E-K9
# Cisco Aironet AIR-AP1200 running IOS 12.3(8)JA
# Cisco Aironet 1100
# C2600 Software (C2600-I-M), Version 12.3(20)
# Model: AIR-AP-1131AG-A-K9, Firmware Version:12.3(7) IOS
Fingerprint Cisco Aironet 350, 1100, 1200, or 1131AG WAP; or Cisco 2600 router (IOS 12.3)
Class Cisco | IOS | 12.X | WAP
Class Cisco | IOS | 12.X | router
SEQ(SP=DF-10D%GCD=1-6%ISR=107-10F%TI=Z%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco AIR-AP1141N-E-K9 running IOS 12.4(21a)JA1
Fingerprint Cisco Aironet AIR-AP1141N WAP (IOS 12.4)
Class Cisco | IOS | 12.X | WAP
SEQ(SP=F8-10A%GCD=1-6%ISR=106-110%TI=RD%CI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1020%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Cisco 2811 Router, running C2800NM-ADVENTERPRISEK9-M Version 15.1(2)T1
Fingerprint Cisco 2811 router (IOS 15.1)
Class Cisco | IOS | 15.X | router
SEQ(SP=FF-10B%GCD=1-6%ISR=10A-114%TI=RD%CI=RD%II=RI%TS=U)
OPS(O1=M5B4SLL%O2=M578SLL%O3=M280%O4=M218SLL%O5=M218SLL%O6=M109SLL)
WIN(W1=1020%W2=1020%W3=1020%W4=1020%W5=1020%W6=1020)
ECN(R=Y%DF=N%T=FB-105%TG=FF%W=1020%O=M5B4SLL%CC=Y%Q=)
T1(R=Y%DF=N%T=FB-105%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FB-105%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FB-105%TG=FF%CD=S)

# Cisco c7200 router running in GNS3 on Windows XP 
Fingerprint Cisco C7200 router (IOS 15)
Class Cisco | IOS | 15.X | router
SEQ(SP=100-10A%GCD=1-6%ISR=FD-107%TI=I%CI=RI%II=RI%SS=O|S%TS=0)
OPS(O1=M5B4NW0NNT00NNS%O2=M5B4NW0NNT00NNS%O3=M5B4NW0NNT00%O4=M5B4NW0NNT00NNS%O5=M5B4NW0NNT00NNS%O6=M5B4NNT00NNS)
WIN(W1=4470%W2=41A0%W3=4100%W4=40E8%W5=40E8%W6=402E)
ECN(R=Y%DF=N%T=7D-87%TG=80%W=4470%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=7D-87%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=C3B4%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Linux Cisco-NAC 2.6.11-perfigo #1 Mon Jun 11 17:01:41 PDT 2007 i686 i686 i386 GNU/Linux
Fingerprint Linux 2.6.11
Class Cisco | Linux | 2.6.X | firewall
SEQ(SP=B7-C1%GCD=1-6%ISR=BE-C8%TI=Z%II=I%TS=A)
OPS(O1=M564ST11NW2%O2=M564ST11NW2%O3=M564NNT11NW2%O4=M564ST11NW2%O5=M564ST11NW2%O6=M564ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M564NNSNW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=BB16%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Linux AP541N-E-K9 2.6.21.5 #1 Thu Sep 10 13:14:03 EDT 2009 mips64 unknown, Cisco AP541N access point
Fingerprint Cisco AP541N WAP (Linux 2.6.21, MIPS)
Class Cisco | Linux | 2.6.X | WAP
SEQ(SP=FD-107%GCD=1-6%ISR=104-10E%TI=I%CI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Cisco NX-OS 4.2(1) on an 7010 Chassis
Fingerprint Cisco 7010 switch (NX-OS 4.2(1))
Class Cisco | NX-OS | 4.X | switch
SEQ(SP=F4-FE%GCD=1-6%ISR=109-113%CI=I%II=RI%TS=3|4)
OPS(O1=M5B4NNT11%O2=M578NNT11%O3=M280NNT11%O4=M5B4NNT11%O5=M218NNT11%O6=M109NNT11)
WIN(W1=4334%W2=4334%W3=44B0%W4=4598%W5=4598%W6=462B)
ECN(R=Y%DF=N%T=41%TG=40%W=4728%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco Nexus 5010, NX-OS Version 4.1(3)N1(1)
# Cisco Nexus 5010 Switch, system:    version 4.1(3)N2(1)
Fingerprint Cisco Nexus 5010 switch (NX-OS 4.1)
Class Cisco | NX-OS | 4.X | switch
SEQ(SP=F3-105%GCD=1-6%ISR=105-10F%TI=I%CI=I%II=RI%SS=S%TS=3)
OPS(O1=M200NNT11%O2=M200NNT11%O3=M200NNT11%O4=M200NNT11%O5=M200NNT11%O6=M200NNT11)
WIN(W1=4334%W2=4334%W3=44B0%W4=4650%W5=47A4%W6=4825)
ECN(R=Y%DF=N%T=41%TG=40%W=4B1C%O=M200%CC=N%Q=)
T1(R=Y%DF=N%T=41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco NX-OS(tm) n7000, Software (n7000-s1-dk9), Version 4.2(4), RELEASE SOFTWARE
Fingerprint Cisco Nexus 7000 switch (NX-OS 4.2(4))
Class Cisco | NX-OS | 4.X | switch
SEQ(SP=FF-109%GCD=1-6%ISR=107-111%TI=I%CI=I%II=RI%SS=O|S%TS=3)
OPS(O1=M218NNT11%O2=M218NNT11%O3=M218NNT11%O4=M218NNT11%O5=M218NNT11%O6=M109NNT11)
WIN(W1=9E20|A214|A608|A9FC|ADF0%W2=9E20|A214|A608|A9FC|ADF0%W3=9F74|A45C|A6D0|ABB8|AE2C%W4=9FA8|A5CC|A7D8|ABF0|B008%W5=9FA8|A5CC|A7D8|ABF0|B008%W6=A01A|A608|A802|ABF6|B0E7)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=A214|A608|A9FC|ADF0|B1E4%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# NX-OS 4.0(1a) image on a Cisco Nexus 7000-series switch supervisor module
Fingerprint Cisco Nexus 7000-series switch (NX-OS 4.0(1a))
Class Cisco | NX-OS | 4.X | switch
SEQ(SP=FD-10D%GCD=1-6%ISR=FA-10F%TI=I%II=RI%SS=O|S%TS=3)
OPS(O1=M200NNT11%O2=M200NNT11%O3=M200NNT11%O4=M200NNT11%O5=M200NNT11%O6=M200NNT11)
WIN(W1=5EE0|62D4|66C8|6ABC|6EB0%W2=5EE0|62D4|66C8|6ABC|6EB0%W3=5FAC|6494|6708|6BF0|70D8%W4=5FB4|6590|6784|6D60|7148%W5=6034|6658|6864|6E88|72A0%W6=60DA|66C8|68C2|6EB0|72A4)
ECN(R=Y%DF=N%T=41%TG=40%W=62D4|66C8|6ABC|6EB0|72A4%O=M200%CC=N%Q=)
T1(R=Y%DF=N%T=41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=41%TG=40%W=62D4|66C8|6ABC|6EB0|72A4%S=O%A=S+%F=AS%O=M200NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Nexus 7010 running 4.0(4)
Fingerprint Cisco Nexus 7010 switch (NX-OS 4.0(4))
Class Cisco | NX-OS | 4.X | switch
SEQ(SP=F9-109%GCD=1-6%ISR=FB-10D%TI=I%CI=I%II=RI%SS=S%TS=3|4)
OPS(O1=M200NNT11%O2=M200NNT11%O3=M200NNT11%O4=M200NNT11%O5=M200NNT11%O6=M200NNT11)
WIN(W1=4728|4F10|56F8|5AEC|5EE0%W2=4728|4F10|56F8|5AEC|5EE0%W3=4998|50F4|5850|5D38|5FAC%W4=4A38|5208|59D8|5DC0|5FB4%W5=4BBC|53EC|5A10|5E28|6034%W6=4C19|5401|5AEC|5EE0|60DA)
ECN(R=Y%DF=N%T=3C-46%TG=40%W=4F10|56F8|5AEC|5EE0|62D4%O=M200%CC=N%Q=)
T1(R=Y%DF=N%T=3C-46%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C-46%TG=40%W=4F10%S=O%A=S+%F=AS%O=M200NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C-46%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C-46%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C-46%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C-46%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FB-105%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FB-105%TG=FF%CD=S)

# Software 4.0(1a)N1(1)
Fingerprint Cisco NX-OS 4.0(1a)N1(1)
Class Cisco | NX-OS | 4.X | switch
SEQ(SP=F8-10A%GCD=1-6%ISR=100-10E%TI=I%CI=RD|RI%II=RI%SS=S%TS=3)
OPS(O1=M200NNT11%O2=M200NNT11%O3=M200NNT11%O4=M200NNT11%O5=M200NNT11%O6=M200NNT11)
WIN(W1=A214|A9FC|ADF0|B1E4|B5D8%W2=A214|A9FC|ADF0|B1E4|B5D8%W3=A45C|ABB8|AE2C|B314|B7FC%W4=A604|ABE0|AFC8|B3B0|B98C%W5=A7D8|ABF0|B008|B420|BA44%W6=A802|ABF6|B0E7|B4DB|BAC9)
ECN(R=Y%DF=N%T=41%TG=40%W=A9FC|ADF0|B1E4|B5D8|BDC0%O=M200%CC=N%Q=)
T1(R=Y%DF=N%T=41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=80%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=100%TG=FF%W=100%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=100%TG=FF%W=400%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=41%TG=40%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Cisco 5510 with ASA 8.2(1) OS.
Fingerprint Cisco ASA 5510 firewall (PIX OS 8.2)
Class Cisco | PIX OS | 6.X | firewall
SEQ(SP=101-10B%GCD=1-6%ISR=101-10B%TI=RD%CI=RD|RI%II=RI%TS=U)
OPS(O1=M564%O2=M564%O3=M564%O4=M564%O5=M564%O6=M564)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2000%O=M564%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=80%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=100%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=7A69%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Cisco PIX firewall running verios 6.3(5) software
# Cisco PIX Firewall Version 6.3(3). Hardware:   PIX-515E, 64 MB RAM, CPU Pentium II 433 MHz
Fingerprint Cisco PIX firewall (PIX OS 6.3(5))
Class Cisco | PIX OS | 6.X | firewall
SEQ(SP=FA-106%GCD=1-6%ISR=108-114%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=80%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1000%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=7A69%S=A%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=8000%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=FFFF%S=A%A=S+%F=UAPR%O=WFNM109T10S%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Cisco Adaptive Security Appliance Software (ASA) Version 7.2(4)
Fingerprint Cisco Adaptive Security Appliance (PIX OS 7.2)
Class Cisco | PIX OS | 7.X | firewall
SEQ(SP=FF-109%GCD=1-6%ISR=100-10A%TI=RD%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2000%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=7B-85%TG=80%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Cisco ASA 5540. ASA version 8.0(4)
Fingerprint Cisco ASA 5540 firewall (PIX OS 8.0)
Class Cisco | PIX OS | 8.X | firewall
SEQ(SP=100-10A%GCD=1-6%ISR=101-10B%TI=RD%CI=RD%II=RI%TS=U)
OPS(O1=M564%O2=M564%O3=M564%O4=M564%O5=M564%O6=M564)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2000%O=M564%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=80%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=100%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Cisco AP340 (First-Generation WAP), Code Release: 12.05, VxWorks version 5.4 (Circa 2002)
Fingerprint Cisco AP340 WAP (VxWorks 5.4)
Class Cisco | VxWorks | 5.X | WAP
SEQ(SP=13-1D%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Citrix NetScaler load balancer
Fingerprint Citrix NetScaler load balancer
Class Citrix | embedded || load balancer
SEQ(SP=101-10B%GCD=1-6%ISR=107-111%CI=BI%II=RI%TS=U)
OPS(O1=M5B4%O2=M564%O3=M218%O4=M218%O5=M218%O6=M80)
WIN(W1=1FFE%W2=1FFE%W3=1FFE%W4=1FFE%W5=1FFE%W6=1FFE)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1FFE%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=2009%S=A%A=S%F=R%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=2014%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=2014%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=2009%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=2009%S=A%A=S+%F=R%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=Z)

# Citrix Access Gateway model 2000, software release 4.5.8. Rebadged Supermicro 5013C-M. The operating system itself is some form of Linux.
Fingerprint Citrix Access Gateway VPN gateway
Class Citrix | embedded || proxy server
SEQ(SP=C6-D0%GCD=1-6%ISR=CC-D6%TI=Z%II=I%TS=U)
OPS(O1=M586NNSNW0%O2=M586NNSNW0%O3=M586NW0%O4=M586NNSNW0%O5=M586NNSNW0%O6=M586NNS)
WIN(W1=1618%W2=1618%W3=1618%W4=1618%W5=1618%W6=1618)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1618%O=M586NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Citrix XenServer Version : 5.5.0 Build number : 25727p
# 2.6.18-128.1.6.el5.xs5.5.0.505.1024xen #1 SMP Mon Nov 16 09:08:33 EST 2009 i686 i686 i386 GNU/Linux, XenServer release 5.5.0-15119p (xenenterprise)
Fingerprint Citrix XenServer (Linux 2.6.18)
Class Citrix | Linux | 2.6.X | general purpose
SEQ(SP=BE-CE%GCD=1-6%ISR=C7-D1%TI=Z%CI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW7%O2=M5B4ST11NW7%O3=M5B4NNT11NW7%O4=M5B4ST11NW7%O5=M5B4ST11NW7%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW7%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Cobalt Cube1 / 2700WG (Cobalt Linux release 2.2 (Fargo) Kernel 2.0.34C52_SK on a mips)
Fingerprint Cobalt Qube 1 2700WG (Linux 2.0.34)
Class Cobalt | Linux | 2.0.X | general purpose
SEQ(SP=FB-107%GCD=1-6%ISR=102-10C%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=7FE0%W2=7FE0%W3=7FE0%W4=7FE0%W5=7FE0%W6=7FE0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=7FE0%O=M5B4%CC=N%Q=U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=7FE0%S=O%A=S+%F=ASF%O=M109%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=EF2D%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Cognex DataMan 200 (running http://www.sics.se/~adam/lwip/)
Fingerprint Cognex DataMan 200 ID reader (lwIP TCP/IP stack)
Class Cognex | embedded || specialized
SEQ(SP=0-59%GCD=1-6|CE|19C|26A|338|406%ISR=55-5F%TI=I%CI=I%II=RI%SS=O%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=800%W2=800%W3=800%W4=800%W5=800%W6=800)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=800%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=800%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=800%S=O|A+%A=O|S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=800%S=A|O%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=800%S=A|O%A=O|S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=800%S=A|O%A=O|S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=128|7CBB|B4CA|B518%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# iPAQ Connection Point CP-2W 4 port + 802.11b router, Hardware Version 1.01, Software Version 2.09 Jan 21, 2003
Fingerprint Compaq iPAQ CP-2W Connection Point WAP
Class Compaq | embedded || WAP
SEQ(R=N)
OPS(O1=|M578%O2=|M578%O3=|M578%O4=|M578%O5=|M578%O6=|M578)
WIN(W1=0|800%W2=0|800%W3=0|800%W4=0|800%W5=0|800%W6=0|800)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=0|800%O=|M578%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=Z%A=S+%F=AR|AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=800%S=Z%A=O|S+%F=AS%O=M578%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Compaq Tru64 4.0F
Fingerprint Compaq Tru64 UNIX V4.0F
Class Compaq | Tru64 UNIX | 4.X | general purpose
SEQ(SP=E2-EC%GCD=10|20|30|40|50%ISR=104-10E%TI=I%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=832C%W2=8340%W3=8200%W4=8000%W5=81D0%W6=805C)
ECN(R=Y%DF=Y%T=3C%TG=40%W=832C%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3C%TG=40%W=805C%S=O%A=S+%F=AS%O=M5B4NW0%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# /etc/motd: Compaq Tru64 UNIX V5.1 (Rev. 732); Sat Mar 20 11:57:19 EST 2004
Fingerprint Compaq Tru64 UNIX 5.1
Class Compaq | Tru64 UNIX | 5.X | general purpose
SEQ(SP=E3-ED%GCD=10|20|30|40|50%ISR=107-111%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=F000%W2=F000%W3=F000%W4=F000%W5=F000%W6=F000)
ECN(R=Y%DF=N%T=3C%TG=40%W=F000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=F000%S=O%A=S+%F=AS%O=M5B4NW0%RD=0%Q=)
T4(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Compaq Tru64 UNIX V5.1 (Rev. 732)
# VMS v7.3-1
# VMS 7.3-1 on a VAX
Fingerprint Compaq Tru64 UNIX 5.1 or HP OpenVMS 7.3-1
Class Compaq | Tru64 UNIX | 5.X | general purpose
Class HP | OpenVMS | 7.X | general purpose
SEQ(SP=93-9D%GCD=1-6%ISR=99-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=F000%W2=F000%W3=F000%W4=F000%W5=F000%W6=F000)
ECN(R=Y%DF=N%T=3C%TG=40%W=F000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=F000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP OpenVMS V7.3-2 on AlphaServer ES45 Model 2
# Compaq Tru64 UNIX V5.1B (Rev. 2650)
Fingerprint Compaq Tru64 UNIX 5.1 or HP OpenVMS 7.3-2
Class Compaq | Tru64 UNIX | 5.X | general purpose
Class HP | OpenVMS | 7.X | general purpose
SEQ(SP=DC-E9%GCD=10|20|30|40|50|60%ISR=107-111%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=F000%W2=F000%W3=F000%W4=F000%W5=F000%W6=F000)
ECN(R=Y%DF=N%T=3C%TG=40%W=F000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=F000%S=O%A=S+%F=AS%O=M5B4NW0%RD=0%Q=)
T4(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Compaq Tru64 UNIX V5.1B
# OpenVMS/Alpha V8.2
# OpenVMS (TM) Alpha Operating System, Version V8.3
Fingerprint Compaq Tru64 UNIX 5.1B or HP OpenVMS 8.2 - 8.3
Class Compaq | Tru64 UNIX | 5.X | general purpose
Class HP | OpenVMS | 8.X | general purpose
SEQ(SP=FB-109%GCD=1-6%ISR=FF-10B%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=F53C%W2=F0A0%W3=F000%W4=F000%W5=F0C8%W6=F028)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=F53C%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=F028%S=O%A=S+%F=AS%O=M5B4NW0%RD=0%Q=)
T4(R=Y%DF=N|Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N|Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N|Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N|Y%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Ethernet to wall socket connector provided by BT. Runs 10Mbps ethernet through house electrics.
# Acbel Polytech Ethernet over Powerline 200Mbit/sec bridge
Fingerprint AcBel or Comtrend powerline Ethernet adapter
Class Comtrend | embedded || bridge
Class AcBel | embedded || bridge
SEQ(SP=0-16%GCD=9C4|1388|1D4C|2710|30D4%ISR=0-67%TI=I%TS=U)
OPS(O1=M578%O2=M578%O3=M578%O4=M578%O5=M578%O6=M578)
WIN(W1=7805%W2=7805%W3=7805%W4=7805%W5=7805%W6=7805)
ECN(R=Y%DF=N%T=22-38%TG=40%W=7805%O=M578%CC=N%Q=)
T1(R=Y%DF=N%T=22-36%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=23-3A%TG=40%W=7805%S=O%A=S+%F=AS%O=M578%RD=0%Q=)
T4(R=Y%DF=N%T=20-2E|31-3E%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=21-38%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=Y%DF=N%T=22-2E|35-3F%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Router Comtrend 5361 RoHS
Fingerprint Comtrend 5361 ADSL router
Class Comtrend | embedded || broadband router
SEQ(SP=C1-CB%GCD=1-6%ISR=C7-D1%TI=Z%II=I%TS=8)
OPS(O1=M5ACST11NW0%O2=M5ACST11NW0%O3=M5ACNNT11NW0%O4=M5ACST11NW0%O5=M5ACST11NW0%O6=M5ACST11)
WIN(W1=1680%W2=1680%W3=1680%W4=1680%W5=1680%W6=1680)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16B0%O=M5ACNNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1680%S=O%A=S+%F=AS%O=M5ACST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Comtrend CT-800 SIP gateway
Fingerprint Comtrend CT-800 VoIP gateway
Class Comtrend | embedded || VoIP adapter
SEQ(SP=14-1E%GCD=7A00|F400|16E00|1E800|26200%ISR=91-9B%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4074%W5=4180%W6=403D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=403D%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# conceptronic CHD3NET
Fingerprint Conceptronic CHD3NET NAS device
Class Conceptronic | embedded || storage-misc
SEQ(SP=0-5%GCD=596B|B2D6|10C41|165AC|1BF17%ISR=89-93%TI=RD%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%S=O%A=O|S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=1B-25%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=1B-25%TG=20%CD=S)

# Coraid Linux NAS v. 6, debian based Storage System, made by CoRAID
Fingerprint CoRAID NAS device
Class CoRAID | embedded || storage-misc
SEQ(SP=BE-CE%GCD=1-6%ISR=C8-D2%TI=Z%II=I%TS=8)
OPS(O1=M1040ST11NW2%O2=M1040ST11NW2%O3=M1040NNT11NW2%O4=M1040ST11NW2%O5=M1040ST11NW2%O6=M1040ST11)
WIN(W1=309C%W2=309C%W3=309C%W4=309C%W5=309C%W6=309C)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=30C0%O=M1040NNSNW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=309C%S=O%A=S+%F=AS%O=M1040ST11NW2%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# 2.0.5.60 unicosmk CRAY T3E, Vendor: Cray, OS: Unicos/mk
Fingerprint Cray UNICOS/mk 2.0.5.60
Class Cray | UNICOS | 2.X | general purpose
SEQ(SP=98-A2%GCD=1-6%ISR=9F-A9%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M10D8WANT11LL%O2=M10D8W0NT11LL%O3=M10D8W5NT11LL%O4=M10D8WANT11LL%O5=M10D8WANT11LL%O6=M10D8T11LL)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3C%TG=40%W=8000%O=M10D8WAN%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3C%TG=40%W=20%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Dedicated Micros Digital Sprite 2, Version 4.4 (029)
# Crestron AV2 with a C2ENET-2 card, firmware 3.155.1240
# Crestron CP2e and firmware 3.155.1240
# Crestron TPS-6x touchpanel with firmware 3.001.0030
Fingerprint Crestron AV2 or CP2E automation system or TPS-6x touchpanel (2-Series), or Dedicated Micros Digital Sprite 2 DVR
Class Crestron | 2-Series || specialized
Class Dedicated Micros | embedded || media device
SEQ(SP=FE-10A%GCD=1-6%ISR=103-111%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=3E80%W2=3E80%W3=3E80%W4=3E80%W5=3E80%W6=3E80)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=3E80%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=ARF%O=%RD=0%Q=)
T3(R=Y%DF=N%T=1B-25%TG=20%W=3E80%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=RF%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=ARF%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=RF%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=ARF%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=1B-25%TG=20%CD=S)

# Crestron Xpanel Series 2 unit
Fingerprint Crestron XPanel control system
Class Crestron | 2-Series || specialized
SEQ(CI=I%II=I)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Crestron CNMSX-AV with expansion CNX-ENET+ Ethernet card.
Fingerprint Crestron CNMSX-AV control and automation system
Class Crestron | embedded || specialized
SEQ(SP=CF-D9%GCD=1-6%ISR=D5-DF%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=38-42%TG=40%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=38-42%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=38-42|74-7E%TG=40|80%W=1000%S=O%A=O|S+%F=A|AS%O=|M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=38-42%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=38-42%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=38-42%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=38-42%TG=40%W=0%S=A%A=S+%F=A%O=%RD=0%Q=)
U1(DF=N%T=38-42%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=38-42%TG=40%CD=Z)

# Crestron Electronics, Product: MC2E, Firmware: v4.000.0226
# Crestron Pro2 processor
# MP2e firmware 4.000.0226
# Crestron QM-RMC with firmware 4.000.0226
# Crestron Pro2 with optional ethernet interface C2ENET-1
# HP StorageWorks MSL4048 Tape Library, Product ID MSL G3, Library Firmware 6.00 / 2.60e
Fingerprint Crestron MC2E, MP2E, PRO2, or QM-RMC control and automation system, or HP StorageWorks MSL4048 tape library
Class Crestron | embedded || specialized
Class HP | embedded || storage-misc
SEQ(SP=EE-10C%GCD=1-6%ISR=FF-10F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=3E80%W2=3E80%W3=3E80%W4=3E80%W5=3E80%W6=3E80)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=3E80%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=3E80%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# D-Link DI-704P
# Dlink dl-604 router
Fingerprint D-Link DI-504 or DI-704P broadband router
Class D-Link | embedded || broadband router
SEQ(SP=0-1B%GCD=32|64|96|C8|FA%ISR=4A-54%TI=BI%II=BI%SS=S%TS=U)
OPS(O1=|M5B4%O2=|M5B4%O3=|M5B4%O4=|M5B4%O5=|M5B4%O6=|M5B4)
WIN(W1=0|16D0%W2=0|16D0%W3=0|16D0%W4=0|16D0%W5=0|16D0%W6=0|16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0|16D0%O=|M5B4%CC=N%Q=U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=Z%A=S+%F=AR%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=O|S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# D-Link DI-604 provided by Verizon in about 2007 for residential FIOS.
Fingerprint D-Link DI-604 wireless broadband router
Class D-Link | embedded || broadband router
SEQ(SP=C-16%GCD=FA7F|1F4FE|2EF7D|3E9FC|4E47B%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B0%O2=M5B0%O3=M5B0%O4=M5B0%O5=M5B0%O6=M5B0)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=7F%TG=80%W=2000%O=M5B0%CC=N%Q=)
T1(R=Y%DF=N%T=7F%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7F%TG=80%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=7F%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=7F%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=91CD%RUD=G)
IE(DFI=N%T=7F%TG=80%CD=S)

# CANOPY CMM 2.2 Build 2a Oct 12 2006 15:14:19
# D-Link DIR-100 Router with switch firmware 2.00_b5_sw
Fingerprint D-Link DIR-100 DSL router or Motorola Canopy cluster management module 2.2
Class D-Link | embedded || broadband router
Class Motorola | embedded || specialized
SEQ(SP=8B-99%GCD=1-6%ISR=97-A3%TI=I%II=I%SS=S%TS=1|2)
OPS(O1=M5A8NW0NNT11%O2=M5A8NW0NNT11%O3=M5A8NW0NNT11%O4=M5A8NW0NNT11%O5=M5A8NW0NNT11%O6=M5A8NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=43E0%W5=4180%W6=403D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=403D|4431|4A1F|500D|54FE%S=O%A=O|S+%F=AS%O=M5A8NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=134%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# D-Link DSL-500 firmware R2.21.002.03.b13au
Fingerprint D-Link DSL-500 ADSL router
Class D-Link | embedded || broadband router
SEQ(R=N)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=Y%T=3C%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=Z%A=S%F=AR%RD=0%Q=)
T2(R=Y%DF=Y%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=3C%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3C%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=19-23%TG=20%CD=Z)

# D-Link ADSL router, model DSL-500G
# D-Link DSL-500G Generation IV ADSL Router
# D-LINK DSL-500G, Generation II, Ver.: C5
Fingerprint D-Link DSL-500G ADSL router
Class D-Link | embedded || broadband router
SEQ(SP=F7-10D%GCD=1-6%ISR=FA-110%TI=I%II=I%SS=S%TS=U)
OPS(O1=M584%O2=M584%O3=M584%O4=M584%O5=M584%O6=M584)
WIN(W1=3E80%W2=3E80%W3=3E80%W4=3E80%W5=3E80%W6=3E80)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3E80%O=M584%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=3E80%S=O%A=S+%F=AS%O=M584%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=ARF%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# D-Link DSL-504 ADLS modem/router
Fingerprint D-Link DSL-504 ADSL modem
Class D-Link | embedded || broadband router
SEQ(SP=0-29%GCD=9C4|1388|1D4C|2710|30D4|61A8|C350|124F8|186A0|1E848%ISR=8A-94%TI=I%II=I%SS=S%TS=U)
OPS(O1=MFD8%O2=MFD8%O3=MFD8%O4=MFD8%O5=MFD8%O6=MFD8)
WIN(W1=5DC%W2=5DC%W3=5DC%W4=5DC%W5=5DC%W6=5DC)
ECN(R=Y%DF=N%T=3C%TG=40%W=5DC%O=MFD8%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=5DC%S=O%A=S+%F=AS%O=MFD8%RD=0%Q=)
T4(R=Y%DF=Y%T=3C%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3C%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=19-23%TG=20%CD=Z)

# D-Link Modem DSL2-300G, Hardware revision: A1, Firmware: R7.00.b1.TQ.t7, The firmware is a special revision for Telus Québec (*.TQ.*).
Fingerprint D-Link DSL2-300G DSL modem
Class D-Link | embedded || broadband router
SEQ(SP=70-88%GCD=1-6%ISR=7C-90%TI=I%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=4000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=Z%F=R%O=%RD=0%Q=)
U1(DF=N%T=96-A0%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# D-Link DFL 700 Router/Firewall
Fingerprint D-Link DFL-700 firewall
Class D-Link | embedded || firewall
SEQ(SP=102-10C%GCD=1-6%ISR=104-10E%TI=RD%TS=U)
OPS(O1=M564%O2=M564%O3=M564%O4=M564%O5=M564%O6=M564)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M564%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(R=N)
IE(R=N)

# D-Link NetDefend OS
Fingerprint D-Link NetDefend firewall
Class D-Link | embedded || firewall
SEQ(SP=F4-FE%GCD=1-6%ISR=106-110%TI=RD%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=8000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(R=N)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# D-Link DP-G310 wireless print server (hardware version A1, firmware version 1.40)
# Hamlet HPS01UU USB Print Server
Fingerprint D-Link DP-300U, DP-G310, or Hamlet HPS01UU print server
Class D-Link | embedded || print server
Class Hamlet | embedded || print server
SEQ(SP=0-1D%GCD=37|6E|A5|DC|113%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=B68%W2=B68%W3=B68%W4=B68%W5=B68%W6=B68)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=B68%O=M5B4%CC=N%Q=U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=B68%S=O%A=S+%F=ASF%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=FA-104%TG=FF%CD=Z)

# D-Link DPR-1260 Firmware:1.20
# Dlink Gamer Lounge  DGL-4300
# DLink DIR-655, running Ubicom's ipOS operarating system.
# Tranzeo TR-5a 5GHz Client radio with built-in antenna
# DGL-4300 - Wireless 108G Gaming Router, Firmware version: 1.8,    2007/03/01
# DLINK DIR-615 wireless access router Firmware Version: 2.25RU
# D-LINK DIR-855 Wireless N Quadband Gigabit Router
# D-Link Systems DGL-4500.
Fingerprint D-Link DPR-1260 print server; or DGL-4300, DGL-4500, DIR-615, DIR-625, DIR-655, or DIR-855 WAP
Class D-Link | embedded || print server
Class D-Link | embedded || WAP
SEQ(SP=95-B5%GCD=1-6%ISR=A9-BB%TI=I%II=I%SS=S%TS=U)
OPS(O1=|M5B4%O2=|M5B4%O3=|M5B4%O4=|M5B4%O5=|M5B4%O6=|M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=|M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O|S+%F=A|AS%O=|M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# Linksys wireless-N router WRT300N
# Linksys WRT300N V2 firmware 2.0.17 (ETSI)
# D-Link DNS-323, Firmware version: 1.07
Fingerprint D-Link DNS-323 NAS device or Linksys WRT300N wireless broadband router
Class D-Link | embedded || storage-misc
Class Linksys | embedded || WAP
SEQ(SP=BB-CB%GCD=1-6%ISR=C3-CF%TI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW1%O2=M5B4ST11NW1%O3=M5B4NNT11NW1%O4=M5B4ST11NW1%O5=M5B4ST11NW1%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# D-LINK DES-3010G L2 managed switch
# Linksys DES-3010G Fast Ethernet Switch, Firmware Version: Build 3.00.036
# Switch: DES-3010F, Boot PROM: Build 1.01.007, Firmware Version: Build 4.00.018
Fingerprint D-Link DES-3010F or DES-3010G switch
Class D-Link | embedded || switch
SEQ(SP=8D-97%GCD=1-6%ISR=92-9C%TI=I%II=RI%SS=O|S%TS=1)
OPS(O1=M5A4NW0NNT11%O2=M5A4NW0NNT11%O3=M5A4NW0NNT11%O4=M5A4NW0NNT11%O5=M5A4NW0NNT11%O6=M5A4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2000%O=M5A4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=0|2000%S=O|Z%A=O|S+%F=A|AR|AS%O=|NNT11NNLLLLLLLLLL|M5A4NW0NNT11NNLLLLLLLLLL%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=19-23%TG=20%CD=S)

# D-Link DGS-3200-10 Gigabit Ethernet Switch
Fingerprint D-Link DES-3010G switch
Class D-Link | embedded || switch
SEQ(SP=8C-98%GCD=1-6%ISR=92-9C%TI=I%II=RI%SS=S%TS=1)
OPS(O1=M5A4NW0NNT11%O2=M5A4NW0NNT11%O3=M5A4NW0NNT11%O4=M5A4NW0NNT11%O5=M5A4NW0NNT11%O6=M5A4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2000%O=M5A4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=2000%S=O%A=S+%F=AS%O=M5A4NW0NNT11NNLLLLLLLLLL%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# D-Link DES-3326 Switch
Fingerprint D-Link DES-3326 switch
Class D-Link | embedded || switch
SEQ(SP=8D-97%GCD=1-6%ISR=91-9B%TI=I%II=RI%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=Z%A=S+%F=A|AR|AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=128%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=19-23%TG=20%CD=S)

# DES-3526 Fast-Ethernet Switch, Firmware Version  : Build 5.01-B21
# DES-3550 Fast Ethernet Switch Command Line Interface Firmware: Build 5.01.B65
Fingerprint D-Link DES-3526 or DES-3550 switch
Class D-Link | embedded || switch
SEQ(SP=8D-97%GCD=1-6%ISR=92-9C%TI=I%CI=I%II=RI%SS=O|S%TS=1)
OPS(O1=M5A4NW0NNT11%O2=M5A4NW0NNT11%O3=M5A4NW0NNT11%O4=M5A4NW0NNT11%O5=M5A4NW0NNT11%O6=M5A4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2000%O=M5A4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=2000%S=O%A=S+%F=AS%O=M5A4NW0NNT11NNLLLLLLLLLL%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=128%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=19-23%TG=20%CD=S)

# d-link des 3526, Firmware Version 5.00-B28
Fingerprint D-Link DES-3526 switch
Class D-Link | embedded || switch
SEQ(SP=8D-97%GCD=1-6%ISR=92-9C%TI=I|RD%II=RI%SS=S%TS=1)
OPS(O1=M5A4NW0NNT11%O2=M5A4NW0NNT11%O3=M5A4NW0NNT11%O4=M5A4NW0NNT11%O5=M5A4NW0NNT11%O6=M5A4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2000%O=M5A4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=2000%S=O%A=S+%F=AS%O=M5A4NW0NNT11NNLLLLLM800L|M5A4NW0NNT11NNNNLLLM800L%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=100|128%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=19-23%TG=20%CD=S)

# D-Link DES-3550 Firmware: Build 5.01.B52
Fingerprint D-Link DES-3550 switch
Class D-Link | embedded || switch
SEQ(SP=8B-95%GCD=1-6%ISR=91-9B%TI=I%CI=I%II=RI%SS=S%TS=1)
OPS(O1=M5A4NW0NNT11%O2=M5A4NW0NNT11%O3=M5A4NW0NNT11%O4=M5A4NW0NNT11%O5=M5A4NW0NNT11%O6=M5A4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2000%O=M5A4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=2000%S=O%A=S+%F=AS%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=128%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=19-23%TG=20%CD=S)

# DES-7210 Modular Layer 3 Chassis Ethernet Switch, System hardware version: A1.0, System software version: v10.3(5), Release(67526)
Fingerprint D-Link DES-7210 switch
Class D-Link | embedded || switch
SEQ(SP=0-5%GCD=388|710|A98|E20|11A8%ISR=64-6E%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3A-44%TG=40%W=1000%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=3A-44%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3A-44%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3A-44%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3A-44%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3A-44%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3A-44%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=5002%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# D-Link DGS-1210-24 switch
Fingerprint D-Link DGS-1210-24 switch
Class D-Link | embedded || switch
SEQ(SP=0-5%GCD=388|710|A98|E20|11A8%ISR=64-6E%TI=I%CI=I%II=I%SS=S%TS=7)
OPS(O1=M109NNT11|M578NNT11%O2=M578NNT11%O3=M578NNT11%O4=M578NNT11%O5=M218NNT11%O6=M109NNT11)
WIN(W1=2400%W2=2400%W3=2400%W4=2400%W5=2400%W6=2400)
ECN(R=Y%DF=N%T=37-41%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=37-41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=37-41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=37-41%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=37-41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=37-41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=37-41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=37-41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# D-Link DGS-3024
Fingerprint D-Link DGS-3024 switch
Class D-Link | embedded || switch
SEQ(SP=8E-98%GCD=1-6%ISR=92-9C%TI=I%II=RI%SS=O|S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=2000%S=O%A=S+%F=AS%O=|M5B4NW0NNT11NNLLLLLLLLLL%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=127|128%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=19-23%TG=20%CD=S)

# D-Link DGS-3324SR xStack 24-Port Layer3 Gigabit Stack Switch
# D-Link DES-3828 switch
Fingerprint D-Link DGS-3324SR, DSG-3612G, or DES-3828 switch
Class D-Link | embedded || switch
SEQ(SP=8B-95%GCD=1-6%ISR=91-9B%TI=I%II=RI%SS=O|S%TS=1)
OPS(O1=M5A4NW0NNT11%O2=M5A4NW0NNT11%O3=M5A4NW0NNT11%O4=M5A4NW0NNT11%O5=M5A4NW0NNT11%O6=M5A4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=1A-24%TG=20%W=2000%O=M5A4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=1A-24%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=1A-24%TG=20%W=2000%S=O%A=S+%F=AS%O=M5A4NW0NNT11NNLLLLLLLLLL%RD=0%Q=)
T4(R=Y%DF=N%T=1A-24%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1A-24%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1A-24%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1A-24%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=1A-24%TG=20%IPL=38%UN=128%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# DGS-3627G Gigabit Ethernet Switch, Firmware: Build 2.50.T31
Fingerprint D-Link DGS-3627G stack
Class D-Link | embedded || switch
SEQ(SP=8E-98%GCD=1-6%ISR=92-9C%TI=I|RD%II=RI%SS=O%TS=1)
OPS(O1=M5C2NW0NNT11%O2=M5C2NW0NNT11%O3=M5C2NW0NNT11%O4=M5C2NW0NNT11%O5=M5C2NW0NNT11%O6=M5C2NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=1A-24%TG=20%W=2000%O=M5C2NW0%CC=N%Q=)
T1(R=Y%DF=N%T=1A-24%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=1A-24%TG=20%W=2000%S=O%A=S+%F=AS%O=M5C2NW0NNT11NNLLLLLLLLLL%RD=0%Q=)
T4(R=Y%DF=N%T=1A-24%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1A-24%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1A-24%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1A-24%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=1A-24%TG=20%IPL=38%UN=128%RIPL=G%RID=G%RIPCK=G%RUCK=61F5%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# D-Link VoIP Gateway DVG-4022S
Fingerprint D-Link DVG-4022S VoIP gateway
Class D-Link | embedded || VoIP adapter
SEQ(SP=8F-99%GCD=1-6%ISR=92-9C%TI=I%II=RI%SS=O%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=2000%S=O%A=O|S+%F=A|AS%O=NNT11NNLLLLLLLLLN|M5B4NW0NNT11NNLLLLLLLLLN%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=128%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=19-23%TG=20%CD=S)

# D-Link VoIP Router DVG-5112S, Firmware Version: GE_1.00
Fingerprint D-Link DVG-5112S VoIP gateway
Class D-Link | embedded || VoIP adapter
SEQ(SP=BF-C9%GCD=1-6%ISR=CB-D5%TI=Z%CI=Z%II=RI%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=S)

# D-Link DI-604 Ethernet Broadband Router, Firmware Version: V3.15b05
# D-Link DI-524 Airplus G Wireless Router Firmware Version: V2.03, Fri, Dec 09 2005
# SMC 7004 VBR EU (european edition)
# DI-604 Ethernet Broadband Router, Firmware Version: V3.10
# DI-524, Firmware Version: V2.05
# DI 524 H/W revision B4: Current Firmware Version: V2.06
# DI-604 Firmware Version : V3.14, Thu, Dec 15 2005
# ZyXEL Prestige 320W, P-320W 802.11g
Fingerprint D-Link DI-524 or DI-604, SMC SMC7004VBR, or ZyXEL Prestige 320W broadband router
Class D-Link | embedded || WAP
Class SMC | embedded || broadband router
Class ZyXEL | embedded || broadband router
SEQ(SP=0-5D%GCD=32|64|96|C8|FA%ISR=4B-6F%TI=BI%CI=BI%II=BI%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# D-Link WBR-2310 Hardware: A1 Firmware: 1.04
# D-Link DI-524
Fingerprint D-Link DI-524 or WBR-2310 wireless broadband router
Class D-Link | embedded || WAP
SEQ(SP=C-7E%GCD=FA7F|1F4FE|2EF7D|3E9FC|4E47B%ISR=97-E3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B0%O2=M5B0%O3=M5B0%O4=M5B0%O5=M5B0%O6=M5B0)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=7F%TG=80%W=2000%O=M5B0%CC=N%Q=)
T1(R=Y%DF=N%T=7F%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=7F%TG=80%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7F%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7F%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7F%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7F%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7F%TG=80%CD=S)

# d-link Di-524
Fingerprint D-Link DI-524 wireless broadband router
Class D-Link | embedded || WAP
SEQ(SP=0-5%GCD=64|C8|12C|190|1F4%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7B-85%TG=80%CD=S)

# DI-524 wireless router running Firmware Version: 3.23 , Wed, 28 Jun 2006
Fingerprint D-Link DI-524 wireless broadband router
Class D-Link | embedded || WAP
SEQ(SP=C-16%GCD=FA7F|1F4FE|2EF7D|3E9FC|4E47B%ISR=97-A1%TI=I%CI=RI%TS=U)
OPS(O1=M5B0%O2=M5B0%O3=M5B0%O4=M5B0%O5=M5B0%O6=M5B0)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=2000%O=M5B0%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=A%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=O|S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(R=N)
IE(R=N)

# D-Link Wireless Router / Access Point DI-714P+, firmware Version: V1.33
Fingerprint D-Link DI-714P+ wireless broadband router
Class D-Link | embedded || WAP
SEQ(SP=C-16%GCD=1F4|3E8|5DC|7D0|9C4%ISR=4B-55%TI=I%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# D-Link DI-824VUP Wireless VPN Router Firmware Version: v1.05, Mon, Apr 25 2005
Fingerprint D-Link DI-824VUP Wireless VPN Router
Class D-Link | embedded || WAP
SEQ(SP=F-11%GCD=32|64|96|C8|FA|12C%ISR=4F-51%TI=I%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# router D-Link Dir-300
Fingerprint D-Link DIR-300 WAP
Class D-Link | embedded || WAP
SEQ(SP=C9-D3%GCD=1-6%ISR=CA-D4%TI=Z%II=I%TS=8)
OPS(O1=M618ST11NW1%O2=M618ST11NW1%O3=M618NNT11NW1%O4=M618ST11NW1%O5=M618ST11NW1%O6=M618ST11)
WIN(W1=1224%W2=1224%W3=1224%W4=1224%W5=1224%W6=1224)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1248%O=M618NNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# D-Link DSA-3100/firmware version: 3.01WW
# Linksys WRT54GL running DD-WRT v23 SP2 VPN edition.
# Model: PePLink Balance 30, Firmware: v4.1.1 build 1089
Fingerprint D-Link DSA-3100 or Linksys WRT54GL (DD-WRT v23) WAP, or Peplink Balance 30 router
Class D-Link | embedded || WAP
Class Linksys | embedded || WAP
Class Peplink | embedded || router
SEQ(SP=C2-D2%GCD=1-6%ISR=C5-D3%TI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# D-Link DWL-2100AP
Fingerprint D-Link DWL-2100AP wireless access point
Class D-Link | embedded || WAP
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A|O%A=O|S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A|O%A=O|S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(R=N)

# D-Link DWL-624+ WAN Router (Connected thru Wi-FI, default network configurations, no cryptography.)
#  d-link vdi-624 Airplus XtremeG 2.4GHz Wireless Router, firmware 2.43DDM 1/12/2005 (Wireless broadband router produced by D-Link for Verizon FIOS customers.  D-Link calls it a 'di-624' but this version (for Verizon FIOS customers) is called a 'vdi-624'.)
# TrendNet Wireless AP tew-432brp
# DI-624revD2 w/firmware 4.03
# D-Link DWL-2000AP, firmware 3.13, 16 Jun 2004
Fingerprint D-Link DWL-624+ or DWL-2000AP, or TRENDnet TEW-432BRP WAP
Class D-Link | embedded || WAP
Class TRENDnet | embedded || WAP
SEQ(R=N)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=N%T=7A-84%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=7A-84%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7A-84%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7A-84%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7A-84%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7A-84%TG=80%CD=S)

# d-link dwl 900ap access point
Fingerprint D-Link DWL-900AP WAP
Class D-Link | embedded || WAP
SEQ(SP=C9-D3%GCD=1-6%ISR=CD-D7%TI=Z%CI=Z%II=I%TS=7)
OPS(O1=M500ST11NW0%O2=M500ST11NW0%O3=M500NNT11NW0%O4=M500ST11NW0%O5=M500ST11NW0%O6=M500ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M500NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M500ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# DWL-900AP+ Wireless Access Point
# USRobotics USR5450 802.11g Wireless Turbo Multi-Function Access Point. Running firmware version 1.53b10.
# PLANET WAP-1966
Fingerprint D-Link DWL-900AP+, Planet WAP-1966, or USRobotics USR5450 WAP
Class D-Link | embedded || WAP
Class Planet | embedded || WAP
Class USRobotics | embedded || WAP
SEQ(SP=B-15%GCD=FA7F|1F4FE|2EF7D|3E9FC|4E47B|5DEFA%ISR=96-A0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=7F%TG=80%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=7F%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7F%TG=80%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=7F%TG=80%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7F%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7F%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7F%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7F%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7F%TG=80%CD=S)

# D-Link DWL-G810 Wlan/Ethernet Bridge
Fingerprint D-Link DWL-G810 WAP
Class D-Link | embedded || WAP
SEQ(SP=C-16%GCD=FA7F|1F4FE|2EF7D|3E9FC|4E47B%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=7A-84%TG=80%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=7A-84%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=7A-84%TG=80%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7A-84%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7A-84%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7A-84%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7A-84%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7A-84%TG=80%CD=S)

# Netgear WPN824 -- hwversion:V2H1 -- fwversion:V2.0.6_1.2.17NA
# Linksys WAP55AG Firmware Version: 1.1(ETSI), Mar 17, 2005
# It is a ReplayTV 5500.
# It is a WAP51AB
# HP/Compaq Remote Insight Lights Out Edition II running firmware v1.21
# Proxim Wireless Networks AP-4000M, v3.6.0(1168)
# Compaq Remote Insight Lights-Out Edition II
# Cisco Wireless Access Point, AIR-AP1010-E-K9,  Software Version 4.0.206.0
# Sun(tm) Advanced Lights Out Manager 1.2
# D-Link DWL-2100AP running Atheros Access Point Rev 4.0.0.167 firmware
# VxWorks? --Ed.
Fingerprint WAP (Cisco Aironet 1010, D-Link DWL-2100AP, Linksys WAP51AB or WAP55AG, Netgear WPN824, or Proxim ORiNOCO AP-4000M), Lights-Out remote server management, or ReplayTV 5500 DVR
Class D-Link | embedded || WAP
Class Cisco | embedded || WAP
Class Compaq | embedded || remote management
Class HP | embedded || remote management
Class Linksys | embedded || WAP
Class Netgear | embedded || WAP
Class Proxim | embedded || WAP
Class SONICblue | embedded || media device
Class Sun | embedded || remote management
SEQ(SP=13-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# DCS-5300G  >  High Speed 2.4GHz (802.11g) Wireless Internet Camera
# D-Link DCS-3220
Fingerprint D-Link DCS-3220 or DCS-5300G webcam
Class D-Link | embedded || webcam
SEQ(SP=0-21%GCD=A|14|1E|28|32|64|C8|12C|190|1F4%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# D-LINK DCS-3220 2-way Audio Internet Camera
Fingerprint D-Link DCS-3220 webcam
Class D-Link | embedded || webcam
SEQ(SP=0-16%GCD=A|14|1E|28|32|64|C8|12C|190|1F4%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=100%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Linksys BEFSR41 V3 Cable/DSL Router (Firmware Version: 1.05.00)
# it is actually a DCS-6620G wireless IP camera
Fingerprint Linksys BEFSR41 EtherFast router or D-Link DCS-6620G webcam
Class D-Link | embedded || webcam
Class Linksys | embedded || router
SEQ(R=N)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=N%T=91-9B%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=91-9B%TG=FF%W=100%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=91-9B%TG=FF%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=91-9B%TG=FF%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=91-9B%TG=FF%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=91-9B%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=91-9B%TG=FF%CD=S)

# KWGR614: http://www.netgear.de/Produkte/Router/Wireless/KWGR614/
# Netgear Firewall Router RT614
# D-link DIR-100 router
# Tomato 1.27 Operating system (Linux)
# Netgear WG602 Wireless Access Point
Fingerprint D-Link DIR-100; or Netgear KWRGR614, RT614, or WG602 router (Linux 2.4)
Class D-Link | Linux | 2.4.X | WAP
Class Netgear | Linux | 2.4.X | router
Class Netgear | Linux | 2.4.X | WAP
SEQ(SP=BE-D4%GCD=1-6%ISR=C4-D8%TI=Z%CI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# D-Link DSL-G624T ADSL Router, Linux version 2.4.17_mvl21-malta-mips_fp_le (root@Jackal) (gcc version 2.95.3 20010315 (release/MontaVista))
# DG834G V4.01.19
# ADSL Modem Router Netgear DG834Bv3 V4.01.27
Fingerprint D-Link DSL-G624T wireless ADSL router (MontaVista embedded Linux 2.4.17), or Netgear DG834Bv3 ADSL router or DG834G WAP
Class D-Link | Linux | 2.4.X | WAP
Class Netgear | embedded || broadband router
Class Netgear | embedded || WAP
SEQ(SP=C4-CE%GCD=1-6%ISR=C9-D3%TI=Z%II=I%TS=7|8|9)
OPS(O1=NNT11|M5B4ST11NW0%O2=NNT11|M5B4ST11NW0%O3=NNT11|M5B4NNT11NW0%O4=NNT11|M5B4ST11NW0%O5=NNT11|M5B4ST11NW0%O6=NNT11|M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45|FA-104%TG=40|FF%W=16D0%O=|M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45|FA-104%TG=40|FF%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45|FA-104%TG=40|FF%W=16A0%S=O%A=O|S+%F=A|AS%O=NNT11|M5B4ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Linux 2.4.18-MIPS-01.00 (davidhsu@LNX103) (gcc version 3.3.3) #8 Mon Mar 20 14:34:57 CST 2006, D-Link DWL-G700AP wireless access point, with firmware version v2.13.
Fingerprint D-Link DWL-G700AP WAP (Linux 2.4.18)
Class D-Link | Linux | 2.4.X | WAP
SEQ(SP=C3-CD%GCD=1-6%ISR=C6-D0%TI=Z%CI=Z%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=O|S+%F=AS%O=M5B4ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=6401%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=I)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# DNS-323 NAS
# Linux 2.6.12.6-arm1 #32 Wed Jun 24 15:19:48 CST 2009 armv5tejl unknown
Fingerprint D-Link DNS-323 NAS device (Linux 2.6.12)
Class D-Link | Linux | 2.6.X | storage-misc
SEQ(SP=C3-CF%GCD=1-6%ISR=C9-D3%TI=Z%CI=I%II=I%TS=7)
OPS(O1=MB94ST11NW1%O2=MB94ST11NW1%O3=MB94NNT11NW1%O4=MB94ST11NW1%O5=MB94ST11NW1%O6=MB94ST11)
WIN(W1=2298%W2=2298%W3=2298%W4=2298%W5=2298%W6=2298)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=22BC%O=MB94NNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=2298%S=O%A=S+%F=AS%O=MB94ST11NW1%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# DNS-323 Network Attached Storage
# Linux 2.6.12.6-arm1 #30 Mon Aug 18 14:19:14 CST 2008 armv5tejl unknown, D-Link DNS-323 NAS enclosure running firmware 1.0.6
# Linux 2.6.12.6-arm1 #47 Mon Nov 30 12:06:02 CST 2009 armv5tejl unknown, DNS-323 Firmware 1.09
Fingerprint D-Link DNS-323 NAS device (Linux 2.6.12)
Class D-Link | Linux | 2.6.X | storage-misc
SEQ(SP=BD-D5%GCD=1-6%ISR=C3-CF%TI=Z%CI=I|RD%II=I%TS=7)
OPS(O1=M2304ST11NW1%O2=M2304ST11NW1%O3=M2304NNT11NW1%O4=M2304ST11NW1%O5=M2304ST11NW1%O6=M2304ST11)
WIN(W1=45F0%W2=45F0%W3=45F0%W4=45F0%W5=45F0%W6=45F0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4608%O=M2304NNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=45F0%S=O%A=S+%F=AS%O=M2304ST11NW1%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# barcode pistol (datalogic kyman) with windows CE 5.0
Fingerprint Datalogic Kyman barcode scanner (Windows CE 5.0)
Class Datalogic | Windows | PocketPC/CE | specialized
SEQ(SP=74-84%GCD=1-6%ISR=93-9D%TI=I%CI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT00NNS%O2=M5B4NW0NNT00NNS%O3=M5B4NW0NNT00%O4=M5B4NW0NNT00NNS%O5=M5B4NW0NNT00NNS%O6=)
WIN(W1=832C%W2=8340%W3=8200%W4=81D0%W5=81D0%W6=0)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=0%O=%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=B0%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=Z)

# OSF1 v4.0 1229 on DEC ALPHA
Fingerprint DEC Digital UNIX OSF1 v4.0 1229
Class DEC | Digital UNIX | 4.X | general purpose
SEQ(SP=E4-EE%GCD=1-6%ISR=FE-108%TI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT00NNS%O2=M5B4NW0NNT00NNS%O3=M5B4NW0NNT00%O4=M5B4NW0NNT00NNS%O5=M5B4NW0NNT00NNS%O6=M5B4NNT00NNS)
WIN(W1=4470%W2=41A0%W3=4100%W4=40E8%W5=40E8%W6=402E)
ECN(R=Y%DF=N%T=7C-86%TG=80%W=4470%O=M5B4NW0NNS%CC=N%Q=|U)
T1(R=Y%DF=N%T=7C-86%TG=80%S=O%A=S+%F=AS%RD=0%Q=|U)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=25A3%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# DEC Digital UNIX 4.X
# DEC Digital UNIX 4.X (AlphaServer 1000A 5/400 Digital UNIX V4.0F (Rev. 1229))
Fingerprint DEC Digital UNIX v4.0F
Class DEC | Digital UNIX | 4.X | general purpose
SEQ(SP=91-9B%GCD=1-6%ISR=98-A2%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=832C%W2=8340%W3=8200%W4=8000%W5=81D0%W6=805C)
ECN(R=Y%DF=Y%T=3C%TG=40%W=832C%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3C%TG=40%W=805C%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=8000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# DEC Digital UNIX 5.X
Fingerprint DEC Digital UNIX 5.X
Class DEC | Digital UNIX | 5.X | general purpose
SEQ(SP=DB-E9%GCD=10|20|30|40|50%ISR=103-10D%II=I%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=F000%W2=F000%W3=F000%W4=F000%W5=F000%W6=F000)
ECN(R=N)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3D-47%TG=40%W=400%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3D-47%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# OSF1 V5.0 910 alpha, DEC 3000/600 workstation/server with 175MHz alpha CPU, 96MB RAM
# OpenVMS 7.2 for Alpha processors
Fingerprint DEC Digital UNIX OSF1 v5.0 910 or OpenVMS 7.2
Class DEC | Digital UNIX | 5.X | general purpose
Class DEC | OpenVMS | 7.X | general purpose
SEQ(SP=91-9B%GCD=1-6%ISR=99-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=832C%W2=8340%W3=8200%W4=8000%W5=81D0%W6=805C)
ECN(R=Y%DF=N%T=3C%TG=40%W=832C%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=805C%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=8000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# DEC OpenVMS V7.1-2
# DEC OpenVMS V7.1
Fingerprint DEC OpenVMS 7.1
Class DEC | OpenVMS | 7.X | general purpose
SEQ(SP=E-18%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%TI=I%II=I%SS=S%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=1000%O=%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# OpenVMS (TM) VAX Operating System, Version V7.1
Fingerprint DEC OpenVMS 7.1
Class DEC | OpenVMS | 7.X | general purpose
SEQ(SP=C-36%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-AD%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B0W0N%O2=M5B0W0N%O3=M5B0W0N%O4=M5B0W0N%O5=M5B0W0N%O6=M5B0)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=1000%O=M5B0W0N%CC=N)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=1000%S=O%A=O%F=A%RD=0)
T4(R=Y%DF=N%T=7B-85%TG=80%W=1000%S=A%A=Z%F=R%RD=0)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=1042%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# OpenVMS/VAX V7.3-1 on a DEC VAXstation 4000 Model 60
Fingerprint DEC OpenVMS 7.3-1
Class DEC | OpenVMS | 7.X | general purpose
SEQ(SP=33-87%GCD=20|40|60|80|A0%ISR=95-9F%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=111C%W2=1068%W3=C80%W4=BB8%W5=C90%W6=C6C)
ECN(R=Y%DF=N%T=37-41%TG=40%W=111C%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=37-41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=37-41%TG=40%W=C6C%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=37-41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=37-41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=37-41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# tops-20 running in emulation on klh
Fingerprint DEC TOPS-20
Class DEC | TOPS-20 || general purpose
SEQ(SP=E-18%GCD=30000|60000|90000|C0000|F0000%ISR=97-A1%TI=I%II=RI%SS=O|S%TS=U)
OPS(O1=|M5B4%O2=|M5B4%O3=|M5B4%O4=|M5B4%O5=|M5B4%O6=M5B4)
WIN(W1=0|5B4%W2=0|5B4%W3=0|5B4%W4=0|5B4%W5=0|5B4%W6=5B4)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=5B4%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O|Z%A=S+%F=AR|AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=5B4%S=O%A=O|S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=914|915|916|918|919%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Decru Datafort FW version 3.0P1
Fingerprint Decru Datafort firewall
Class Decru | embedded || firewall
SEQ(SP=EE-10A%GCD=1-6%ISR=106-110%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11NNS%O2=M5B4NW0NNT11NNS%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11NNS%O5=M5B4NW0NNT11NNS%O6=M5B4NNT11NNS)
WIN(W1=E000%W2=E000%W3=E000%W4=E000%W5=E000%W6=E000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=E000%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N|Y%T=3B-45%TG=40%W=E000%S=O%A=O|S+%F=AS%O=M5B4NW0NNT11NNS%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Dell Color Laser 1320c
Fingerprint Dell 1320c printer
Class Dell | embedded || printer
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=96-A0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=3000%W2=3000%W3=3000%W4=3000%W5=3000%W6=3000)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=3000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=1B-25%TG=20%W=3000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=3000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Dell Laser Printer 1600n
Fingerprint Dell 1600n printer
Class Dell | embedded || printer
SEQ(SP=0-5%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=95-9F%TI=I%II=I%SS=O%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=%O6=)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Lexmark E250dn, Kernel  EC.KA.K127b-0
# Dell Laser Printer 1720dn
# Lexmark E352dn
Fingerprint Dell 1720dn, or Lexmark E250dn or E352dn printer
Class Dell | embedded || printer
Class Lexmark | embedded || printer
SEQ(SP=AE-D2%GCD=1-6%ISR=C1-D7%TI=Z%CI=I%II=I%TS=A)
OPS(O1=M5B4ST11NW1%O2=M5B4ST11NW1%O3=M5B4NNT11NW1%O4=M5B4ST11NW1%O5=M5B4ST11NW1%O6=M5B4ST11)
WIN(W1=B50%W2=B50%W3=B50%W4=B50%W5=B50%W6=B50)
ECN(R=Y%DF=Y%T=FE%TG=FF%W=B68%O=M5B4NNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=FE%TG=FF%W=B50%S=O%A=S+%F=AS%O=M5B4ST11NW1%RD=0%Q=)
T4(R=Y%DF=Y%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# Dell 1815dn Printer
Fingerprint Dell 1815dn printer
Class Dell | embedded || printer
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Dell Laser Printer 2335dn, Network Firmware Version is V4.01.24(2335dn MFP) 11-21-2008.
# Dell 2335dn mono laser printer
# dell MFP 2335dn Printer.
Fingerprint Dell 2335dn printer
Class Dell | embedded || printer
SEQ(SP=0-5%GCD=FA01|1F402|2EE03|3E804|4E205%ISR=95-9F%TI=I%II=I%SS=S%TS=U)
OPS(O1=NNM5B4SNW0%O2=NNM5B4SNW0%O3=M5B4NW0%O4=NNM5B4SNW0%O5=NNM5B4SNW0%O6=NNM5B4S)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=NNM5B4SNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=R%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=138%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=Z)

# Dell 3000 Printer
Fingerprint Dell 3000 printer
Class Dell | embedded || printer
SEQ(R=N)
OPS(O1=M5B4%O2=|M5B4%O3=%O4=%O5=%O6=)
WIN(W1=3000%W2=3000%W3=3000%W4=3000%W5=3000%W6=3000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=3000%O=%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=3000%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=3000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=4E4%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Dell 3100cn Laser Printer
Fingerprint Dell 3100cn printer
Class Dell | embedded || printer
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=3000%W2=3000%W3=3000%W4=3000%W5=3000%W6=3000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=3000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=3000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=3000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=4E4%RID=G%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Dell Laser Printer 3100cn V6.26
# Dell Color Laser 3110cn printer.
# Xerox Phaser 6180DN
# Dell MFP Laser 3115cn
Fingerprint Dell 3100cn-series or Xerox Phaser 6180DN printer
Class Dell | embedded || printer
Class Xerox | embedded || printer
SEQ(SP=0-16%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=3000%W2=3000%W3=3000%W4=3000%W5=3000%W6=3000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=3000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=3000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=3000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=4E4%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Mitel 3300CX IP PBX controller with 7.1 firmware. Probably using VxWorks.
# Enterasys SecureStack B2, Model B2G124-48
# Hewlett-Packard Integrity Integrated Lights-Out 2 Revision T.03.06
# Ethernet Routing Switch 5520-48T-PWR, HW:34       FW:5.0.0.4   SW:v5.1.0.014
# Mitel 3300 IP Communications Platform
# Enterasys Matrix N Series Platinum Version 06.11.01.0040
# Dell MFP Laser 3115cn, Firmware Version 200809190845
# Enterasys Networks, Inc. A2H124-24 Rev 02.01.03.0005
# VxWorks? --Ed.
Fingerprint Dell 3115cn printer, Enterasys switch, HP Integrity iLO 2 remote management interface, Mitel 3300 PBX controller, or Nortel 5520 switch
Class Dell | embedded || printer
Class Enterasys | embedded || switch
Class HP | iLO || remote management
Class Mitel | embedded || PBX
SEQ(SP=93-9D%GCD=1-6%ISR=9A-A4%TI=I%II=I%SS=O|S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Lexmark T642 Printer
# Lexmark T644 (Network Printer)
# Lexmark T640
# Dell 5210n laser printer
# Lexmark C534dn color laser printer
# Lexmark C530, Firmware Version: NSF.NP.N016
Fingerprint Dell 5210n or Lexmark C530-series, T640, T642, or T644 printer
Class Dell | embedded || printer
Class Lexmark | embedded || printer
SEQ(SP=BA-D1%GCD=1-6%ISR=CB-D5%TI=Z%II=I%TS=A)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=B50%W2=B50%W3=B50%W4=B50%W5=B50%W6=B50)
ECN(R=Y%DF=Y%T=FE%TG=FF%W=B68%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=FE%TG=FF%W=B50%S=O%A=S+%F=AS%O=M5B4ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# Dell Remote Access Controller 4/I
# Remote Access Controller (RAC) Version 3.38
Fingerprint Dell Embedded Remote Access (ERA) Controller 3.38 or 4/I
Class Dell | embedded || remote management
SEQ(SP=FD-109%GCD=1-6%ISR=FF-10D%TI=RD|RI%II=RI%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Dell Remote Access Controller 4/I (DRAC 4/I) Version 1.35 (Build 09.27)
# Dell Remote Access Controller 4/I (DRAC 4/I) Version 1.33 (Build 08.04)
Fingerprint Dell Embedded Remote Access (ERA) Controller 4/I
Class Dell | embedded || remote management
SEQ(SP=F9-10A%GCD=1-6%ISR=106-110%TI=RD|RI%II=RI%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Dell iDRAC6 Express remote access controller firmware revision 1.20 (Probably Linux --Ed.)
Fingerprint Dell Integrated Remote Access Controller (iDRAC6)
Class Dell | embedded || remote management
SEQ(SP=B5-E1%GCD=1-6%ISR=C7-DD%TI=Z%CI=Z%II=I%TS=7)
OPS(O1=M45FST11NW2%O2=M45FST11NW2%O3=M45FNNT11NW2%O4=M45FST11NW2%O5=M45FST11NW2%O6=M45FST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M45FNNSNW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# PowerEdge 2650
Fingerprint Dell PowerEdge 2650 server Embedded Remote Access (ERA)
Class Dell | embedded || remote management
SEQ(SP=F8-108%GCD=1-6%ISR=FC-110%TI=RD|RI%II=RI%SS=O|S%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=41%TG=40%W=1000%O=%CC=N%Q=)
T1(R=Y%DF=N%T=41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Dell Remote Access Controller 5 (DRAC 5), Firmware Version 1.40 (Build 08.08.22)
Fingerprint Dell Remote Access Controller (DRAC 5)
Class Dell | embedded || remote management
SEQ(SP=C4-CE%GCD=1-6%ISR=C5-CF%TI=Z%CI=RD%II=I%TS=7)
OPS(O1=M578ST11NW0%O2=M578ST11NW0%O3=M578NNT11NW0%O4=M578ST11NW0%O5=M578ST11NW0%O6=M578ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M578NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C-46%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C-46%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C-46%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C-46%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C-46%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Integrated Dell Remote Access Controller 6 - Enterprise"
Fingerprint Dell Remote Access Controller (DRAC 6)
Class Dell | embedded || remote management
SEQ(SP=CF-105%GCD=1-6%ISR=DB-103%TI=Z%II=I%TS=7|9)
OPS(O1=M564NNT11NW2%O2=M564NNT11NW2%O3=M564NNT11NW2%O4=M564NNT11NW2%O5=M564NNT11NW2%O6=M564NNT11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M564NW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# 'Dell Remote Assistance Card 4' or 'DRAC4' in short, running firmware version 1.60.
# Dell Remote Access Controller 4/I
Fingerprint Dell Remote Access Controller 4 (DRAC 4)
Class Dell | embedded || remote management
SEQ(SP=102-10C%GCD=1-6%ISR=100-10E%TI=RD|RI%II=RI%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Dell Remote Access Controller 4/I, on a PowerEdge 2850 server.
Fingerprint Dell Remote Access Controller 4/I
Class Dell | embedded || remote management
SEQ(SP=FC-108%GCD=1-6%ISR=FA-10E%TI=RD|RI%II=RI%SS=O|S%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Dell Remote Access Controller 5, Hardware Version A03, Firmware Version 1.40 (08.08.22) (Probably Linux --Ed.)
Fingerprint Dell Remote Access Controller 5 (DRAC 5)
Class Dell | embedded || remote management
SEQ(SP=F1-10B%GCD=1-6%ISR=FF-111%TI=Z%CI=Z%II=I%TS=7)
OPS(O1=M57EST11NW0%O2=M578ST11NW0%O3=M280NNT11NW0%O4=M22CST11NW0%O5=M218ST11NW0%O6=M109ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M57ENNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Dell DRAC 5/i remote management card
Fingerprint Dell Remote Access Controller 5/I (DRAC 5/I)
Class Dell | embedded || remote management
SEQ(SP=B9-C9%GCD=1-6%ISR=C4-D0%TI=Z%II=I%TS=7)
OPS(O1=M56CST11NW0%O2=M56CST11NW0%O3=M56CNNT11NW0%O4=M56CST11NW0%O5=M56CST11NW0%O6=M56CST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M56CNNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Dell PowerVault 124T LTO-3 Autoloader
# Dell PowerVault 124T (LTO3 tape device with autoloader)
Fingerprint Dell PowerVault 124T LTO-3 tape autoloader
Class Dell | embedded || storage-misc
SEQ(SP=C-16%GCD=FA7F|1F4FE|2EF7D|3E9FC|4E47B%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=50|2AE2|A930|FFFF%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=19-23%TG=20%CD=S)

# Dell Powervault 132T tape library
Fingerprint Dell PowerVault 132T tape library
Class Dell | embedded || storage-misc
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=578%W2=578%W3=578%W4=578%W5=578%W6=578)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=578%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=578%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=578%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Dell PowerVault 705N (NAS Appliance)
Fingerprint Dell PowerVault 705N NAS appliance
Class Dell | embedded || storage-misc
SEQ(SP=C-16%GCD=3200|6400|9600|C800|FA00%ISR=97-A1%TI=I%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2238%W2=2238%W3=2238%W4=2238%W5=2238%W6=2238)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2238%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=19-23%TG=20%W=2238%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(R=N)

# Dell MD3000i
# TP-Link TL-WR340GD router 4.3.3 Build 090812 Rel.61475n
Fingerprint Dell PowerVault MD3000i NAS appliance or TP-Link TL-WR340GD WAP
Class Dell | embedded || storage-misc
Class TP-Link | embedded || WAP
SEQ(SP=94-9E%GCD=1-6%ISR=9B-A5%TI=I%CI=I%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(R=N)

# Netgear GS724TP (PoE 24port gigabit switch)
# Dell PowerConnect 2748, Firmware Version 1.0.0.33, Boot Version 1.0.0.05
# Linksys SLM224P switch, Boot Version   1.0.4, Firmware Version   1.0.1
# Netgear FS728TP switch
# SLM2048
# APC SNMP Adapter
# SLM2024 Gigabit switch (24 port)
# FS728TP Smart Switch
Fingerprint Dell PowerConnect 2748, Linksys SLM2024, SLM2048, or SLM224P, or Netgear FS728TP or GS724TP switch
Class Dell | embedded || switch
Class Linksys | embedded || switch
Class Netgear | embedded || switch
SEQ(SP=FB-10D%GCD=1-6%ISR=103-113%TI=RD%II=RI%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=S+%F=AS%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Dell PowerConnect 3024, Hardware Version: PC-3024-00, Boot ROM Version: 4.2, Software Version: 5.1.4
Fingerprint Dell PowerConnect 3024 switch
Class Dell | embedded || switch
SEQ(SP=0-1C%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=1)
OPS(O1=M400NW0NNT11%O2=M400NW0NNT11%O3=M400NW0NNT11%O4=M400NW0NNT11%O5=M400NW0NNT11%O6=M400NNT11)
WIN(W1=2000%W2=2000%W3=2080%W4=2000%W5=2180%W6=2017)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M400NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2017%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Dell Powerconnect 3248 Switch 2.0.0.21
Fingerprint Dell PowerConnect 3248 switch
Class Dell | embedded || switch
SEQ(SP=8B-95%GCD=1-6%ISR=91-9B%TI=I%CI=I%II=RI%SS=O|S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Dell PowerConnect 3324
Fingerprint Dell PowerConnect 3324 switch
Class Dell | embedded || switch
SEQ(SP=FF-109%GCD=1-6%ISR=104-10E%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=800%W2=800%W3=800%W4=800%W5=800%W6=800)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=800%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=800%S=O%A=S+%F=AS%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Dell PowerConnect 3348
Fingerprint Dell PowerConnect 3348 switch
Class Dell | embedded || switch
SEQ(SP=FD-107%GCD=1-6%ISR=FE-110%TI=I%II=I%SS=S%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=100%W2=100%W3=100%W4=100%W5=100%W6=100)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=100%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=100%S=O%A=S+%F=AS%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Dell PowerConnect 5316M
Fingerprint Dell PowerConnect 5316M switch
Class Dell | embedded || switch
SEQ(SP=0-75%GCD=14|28|3C|50|64%ISR=4B-6F%TI=RD%II=RI%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=200%W2=200%W3=200%W4=200%W5=200%W6=200)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=200%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=200%S=O%A=S+%F=AS%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Dell PowerConnect 5324
# Linux 2.4.21-37.0.1.ELsmp #1 SMP Wed Jan 11 18:44:17 EST 2006 i686 i686 i386 GNU/Linux, Red Hat Enterprise Linux ES release 3 (Taroon Update 6).
Fingerprint Dell PowerConnect 5324 switch
Class Dell | embedded || switch
SEQ(SP=0-8B%GCD=14|28|3C|50|64%ISR=4B-71%TI=I%II=I%SS=S%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=200%W2=200%W3=200%W4=200%W5=200%W6=200)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=200%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=200%S=O%A=S+%F=AS%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# PowerConnect 3324, Unit No.: Unit 1, Software Version 1.1.0.42, Boot Version 1.0.0.13, Hardware Version: 00.00.02.
Fingerprint Dell PowerConnect 5324 switch
Class Dell | embedded || switch
SEQ(SP=F5-FF%GCD=1-6%ISR=FF-109%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=200%W2=200%W3=200%W4=200%W5=200%W6=200)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=200%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=200%S=O%A=S+%F=AS%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# PowerConnect 6200 series
Fingerprint Dell PowerConnect 6200-series switch
Class Dell | embedded || switch
SEQ(SP=8A-94%GCD=1-6%ISR=97-A1%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=11C%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=Z)

# Dell PowerConnect 6248P
# Dell PowerConnect M6220
# Enterasys SecureStack C2 router switch C2H124-48
# Enterasys Networks, Inc. G3G124-24 Rev 01.00.03.0002 (router switch)
# Enterasys Networks, Inc. B2H124-48 Rev 04.02.06.0004
# Enterasys Networks, Inc. B3G124-48 Rev 01.02.04.0005
# Enterasys Networks, Inc. C3G124-48 Rev 01.02.02.0009
# VxWorks? --Ed.
Fingerprint Dell PowerConnect or Enterasys switch
Class Dell | embedded || switch
Class Enterasys | embedded || switch
SEQ(SP=8C-D2%GCD=1-6%ISR=9B-BF%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=11C%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=Z)

# EqualLogic PeerStorage PS100E iSCSI storage array, firmware version "2.2.3 (R75)", uname is NetBSD 1.6.2 NetBSD 1.6.2 (EQL.PSS) #0: Thu Sep  1 20:15:43 EDT 2005 ps.release/EQL.PSS sbmips
Fingerprint Dell EqualLogic PeerStorage PS100E NAS device (NetBSD 1.6.2)
Class Dell | NetBSD | 1.X | general purpose
SEQ(SP=CC-DE%GCD=1-6%ISR=D8-E2%TI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT01%O2=M578NW0NNT01%O3=M280NW0NNT01%O4=M0NW0NNT01%O5=M218NW0NNT01%O6=M109NNT01)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M109NW0NNT01%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Dell Equilogic iscsi SAN, product Family PS5000, model 70-0115
# NetBSD vmeql1 1.6.2 NetBSD 1.6.2 (EQL.PSS) #0: Wed Mar 25 13:59:08 EDT 2009 build@m58:/buildarea/V4.1.4__Wed_Mar_25_2009_13_40_04_EDT/bin/destdir.sbmips.rel ease/EQL.PSS sbmips, EqualLogic PeerStorage PS100E iSCSI storage array running firmware v4.1.4.
Fingerprint Dell EqualLogic PS100E or PS5000 iSCSI NAS device (NetBSD 1.6.2)
Class Dell | NetBSD | 1.X | storage-misc
SEQ(SP=C9-DB%GCD=1-6%ISR=DB-F1%TI=RI%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT01%O2=M578NW0NNT01%O3=M280NW0NNT01%O4=M5B4NW0NNT01%O5=M218NW0NNT01%O6=M109NNT01)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M109NW0NNT01%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Denon AVR-3808Ci
Fingerprint Denon AVR-3808CI audio/video receiver
Class Denon | embedded || media device
SEQ(SP=C-16%GCD=FA7F|1F4FE|2EF7D|3E9FC|4E47B%ISR=97-A1%TI=I%II=I%SS=O|S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=1A-24%TG=20%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1A-24%TG=20%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=1A-24%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1A-24%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1A-24%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=1A-24%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=1A-24%TG=20%CD=S)

# Philips Wireless Music Adapter SLA5500, Firmwareversion 2.0.11.6416
# This is a Philips WAK3300 Alarm clock !
# Terratec NOXON Audio system. (http://entertainen.terratec.net/modules.php?op=modload&name=News&file=article&sid=228)
# Terratec Noxon2Audio Streaming Client
# Terratec Noxon iRadio (standalone ethernet+wifi internet radio)
# Denon AVR-3808CI, a high-end home theater receiver
# Philips SLA5520 Wireless Music Adapter
Fingerprint Denon AVR-3808CI audio/video receiver, Philips SLA5500 or SLA5520 Wireless Music Adapter or WAK3300 wireless alarm clock, or Terratec NOXON audio system
Class Denon | embedded || media device
Class Philips | embedded || media device
Class Terratec | embedded || media device
SEQ(SP=C-16%GCD=FA7F|1F4FE|2EF7D|3E9FC%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=19-23%TG=20%CD=S)

# Develop Ineo 350. Develop is a Konica Minolta reseller with it's own brands / marketing names. (The 250 and 350 builds seem to be identical.)
Fingerprint Develop ineo 250 or 350 printer
Class Develop | embedded || printer
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW1NNT11%O2=M5B4NW1NNT11%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11%O5=M5B4NW1NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW1%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Develop Ineo 600. Develop is a Konica Minolta reseller with it's own brands / marketing names. (The 600 and 700 builds seem to be identical.)
Fingerprint Develop ineo 600 or 700 printer
Class Develop | embedded || printer
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(R=N)

# Dick Smith Electronics XH1169 USB & 4x LAN ADSL Router
# Vendor: Ambit. modem-router provided by neuf telecom in france known as neufbox trio3c
# Netgear WGR614v6. VxWorks: http://forum.openwrt.org/viewtopic.php?id=3843 http://www.dd-wrt.com/phpBB2/viewtopic.php?t=44439&highlight=wgr614v6
Fingerprint Broadband router (VxWorks): Dick Smith Electronics XH1169, Netgear WGR614v6, or Neuf Box Trio 3C
Class Dick Smith Electronics | VxWorks || broadband router
Class Netgear | VxWorks || WAP
Class Neuf | VxWorks || broadband router
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# DIGI One SP RS232-Ethernet Bridge
Fingerprint Digi One SP serial-to-Ethernet bridge
Class Digi | embedded || bridge
SEQ(SP=D-17%GCD=1-6%ISR=4B-55%TI=1%CI=RI%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=21-3B%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=23-3E%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=25-3E%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=3B-45%TG=40%IPL=8E%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# digi PortServer TS 16 Rack Firmware Version: Version 82000684_U1
Fingerprint Digi PortServer TS 16 Rack serial-to-Ethernet bridge
Class Digi | embedded || bridge
SEQ(CI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=27-45%TG=40%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=24-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=2A-3D%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=23-3B%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=24-3D%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=28-3F%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=104%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# PortServer TS4; PortServer  TS 4(55000629-03)
Fingerprint Digi PortServer TS 4 H MEI serial-to-Ethernet bridge
Class Digi | embedded || bridge
SEQ(R=N)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=33-45%TG=40%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=29-36|3B-45%TG=40%S=Z%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=27-38|3B-45%TG=40%W=2000%S=Z%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=Y%T=22-40%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=29-3D%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=2E-3F%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=20-39%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=8E%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Digi PortServer TS 4 w/ Firmware 82000747_U2
# Digi PortServer TS 4 MEI, release_82000747_U3
Fingerprint Digi PortServer TS 4 serial-to-Ethernet bridge
Class Digi | embedded || bridge
SEQ(SP=C-42%GCD=1-6|A|14|1E|28|32%ISR=4B-55%TI=1%CI=RD|RI%II=RI%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=21-3D%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=26-39%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=26-3F%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=20-3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=8E%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Digi Portserver TS RS232 to Etherenet connector
Fingerprint Digi PortServer TS serial-to-Ethernet bridge
Class Digi | embedded || bridge
SEQ(R=N)
OPS(O1=|M5B4%O2=|M578%O3=|M280%O4=|M218%O5=|M218%O6=|M109)
WIN(W1=0|2000%W2=0|2000%W3=0|2000%W4=0|2000%W5=0|2000%W6=0|2000)
ECN(R=Y%DF=N%T=25-30|34-45%TG=40%W=0|2000%O=|M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=20-2C|31-45%TG=40%S=O|Z%A=S+%F=AR|AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=23-40%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=22-3A%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=23-3E%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=23-39%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=8E%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Digi WR44 - Sarian OS
# Digi DR64 MKII
Fingerprint Digi TransPort DR64 or WR44 wireless router
Class Digi | embedded || WAP
SEQ(SP=102-10C%GCD=1-6%ISR=105-10F%TI=I%CI=I%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=F5-FF%TG=FF%W=2000%O=M578%CC=N%Q=)
T1(R=Y%DF=N%T=F5-FF%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=F5-FF%TG=FF%W=0%S=Z%A=O%F=R%O=%RD=0%Q=)
T3(R=Y%DF=N%T=F5-FF%TG=FF%W=2000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=F5-FF%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=F5-FF%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=F5-FF%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=F5-FF%TG=FF%W=0%S=Z%A=O%F=R%O=%RD=0%Q=)
U1(DF=N%T=F5-FF%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# NET+OS7 ( http://www.digi.com/products/embeddedsolutions/devkits/digiconnectmewimedevkitdocs.jsp )
Fingerprint Digi NET+OS 7
Class Digi | NET+OS | 7 | specialized
SEQ(SP=CC-D6%GCD=1-6%ISR=D4-DE%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4W0L%O2=M5B4W0L%O3=M5B4W0L%O4=M5B4W0L%O5=M5B4W0L%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=6F%TG=80%W=2000%O=M5B4W0L%CC=N%Q=)
T1(R=Y%DF=N%T=6F%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=6F%TG=80%W=2000%S=O%A=S+%F=AS%O=M5B4W0L%RD=0%Q=)
T4(R=Y%DF=N%T=6F%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=6F%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=6F%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=6F%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=6F%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=855D%RUD=G)
IE(DFI=N%T=6F%TG=80%CD=Z)

# Regular NET+OS from Digi. Digi based its NET+OS on ThreadX and this NET+OS can be changed/reprogrammed.
# NetOS 7.x
Fingerprint Digi NET+OS 7
Class Digi | NET+OS | 7 | specialized
SEQ(SP=7E-8A%GCD=1-6%ISR=97-A1%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=43E0%W5=4180%W6=403D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4470%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Digitus DN-13008 USB MFP Server, Firmware Version: 2.50
# Sitecom MFP-Server
Fingerprint Digitus DN-13008 or Sitecom print server
Class Digitus | embedded || print server
Class Sitecom | embedded || print server
SEQ(SP=8C-9C%GCD=1-6%ISR=96-A0%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5A8NW0NNT11%O2=M56CNW0NNT11%O3=M274NW0NNT11%O4=M5A8NW0NNT11%O5=M20CNW0NNT11%O6=MFDNNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=43E0%W5=4180%W6=403D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=403D%S=O%A=S+%F=AS%O=MFDNW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=3401%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Digital Monitoring Products (DMP) XR500
Fingerprint DMP XR500 remote alarm monitor
Class DMP | embedded || specialized
SEQ(SP=0-1E7%GCD=1-6|>1000000%ISR=E2-100%TI=I|RD%II=RI%SS=S%TS=U)
OPS(O1=M580%O2=M578%O3=M280%O4=M580%O5=M218%O6=M109)
WIN(W1=B00%W2=B00%W3=B00%W4=B00%W5=B00%W6=B00)
ECN(R=Y%DF=Y%T=FE%TG=FF%W=B00%O=M580%CC=N%Q=)
T1(R=Y%DF=Y%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=FE%TG=FF%W=B00%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=Y%T=FE%TG=FF%W=B00%S=A+%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FE%TG=FF%W=B00%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FE%TG=FF%W=B00%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FE%TG=FF%W=B00%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FE%TG=FF%IPL=38%UN=0-FFFF%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=23-38%TG=40%CD=S)

Fingerprint DragonFly BSD 1.10.1
Class DragonFly BSD | DragonFly BSD | 1.X | general purpose
SEQ(SP=FF-109%GCD=1-6%ISR=103-10F%TI=I%TS=7)
OPS(O1=M3FD8NW0NNT11NNS%O2=M3FD8NW0NNT11NNS%O3=M3FD8NW0NNT11%O4=M3FD8NW0NNT11NNS%O5=M3FD8NW0NNT11NNS%O6=M3FD8NNT11NNS)
WIN(W1=E000%W2=E000%W3=E000%W4=E000%W5=E000%W6=E000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=E000%O=M3FD8NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=E000%S=O%A=O|S+%F=AS%O=M3FD8NW0NNT11NNS%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# DragonFly BSD 1.8.0-RELEASE on i386
# DragonflyBSD 1.10.1 installed on vmware server
Fingerprint DragonFly BSD 1.8.0-RELEASE - 1.10.1 (x86)
Class DragonFly BSD | DragonFly BSD | 1.X | general purpose
SEQ(SP=FB-105%GCD=1-6%ISR=10A-114%TI=I%II=I%SS=O|S%TS=7)
OPS(O1=M5B4NW0NNT11NNS%O2=M5B4NW0NNT11NNS%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11NNS%O5=M5B4NW0NNT11NNS%O6=M5B4NNT11NNS)
WIN(W1=E000%W2=E000%W3=E000%W4=E000%W5=E000%W6=E000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=E000%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=E000%S=O%A=O|S+%F=AS%O=M5B4NW0NNT11NNS%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# DragonFly-2.3.2, soon to be DragonFly-2.4
Fingerprint DragonFly BSD 2.3.2
Class DragonFly BSD | DragonFly BSD | 2.X | general purpose
SEQ(SP=FB-10B%GCD=1-6%ISR=109-113%TI=RD%CI=RD|RI%TS=7)
OPS(O1=M3FD8NW5NNT11NNS%O2=M3FD8NW5NNT11NNS%O3=M3FD8NW5NNT11%O4=M3FD8NW5NNT11NNS%O5=M3FD8NW5NNT11NNS%O6=M3FD8NNT11NNS)
WIN(W1=E000%W2=E000%W3=E000%W4=E000%W5=E000%W6=E000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=E000%O=M3FD8NW5NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=E000%S=O%A=S+%F=AS%O=M3FD8NW5NNT11NNS%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Mitel 5212 SIP Phone
# DragonWave Horizon 24GHz radio: get sw version -> Bootloader software: NCC 1.1.0
Fingerprint DragonWave Horizon WAP or Mitel 5212 SIP Phone
Class DragonWave | embedded || WAP
Class Mitel | embedded || VoIP phone
SEQ(SP=102-10C%GCD=1-6%ISR=106-110%TI=I%II=I%SS=S%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=111C%W2=111C%W3=111C%W4=111C%W5=111C%W6=111C)
ECN(R=Y%DF=N%T=3C%TG=40%W=111C%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=111C%S=O%A=S+%F=AS%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=150%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=Z)

# DVTel DVT-9540DW Network Camera
Fingerprint DVTel DVT-9540DW network camera
Class DVTel | embedded || webcam
SEQ(SP=CC-122%GCD=1-6%ISR=D4-10E%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=6B-75%TG=80%W=4000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=6B-75%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=6B-75%TG=80%W=4000%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=6B-75%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=6B-75%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=6B-75%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=6B-75%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=6B-75%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=1CAC%RUD=G)
IE(DFI=N%T=6B-75%TG=80%CD=Z)

# Efficient 5930 DMT Router (5930-001) v6.1.020
Fingerprint Efficient Networks 5930 ADSL router
Class Efficient Networks | embedded || broadband router
SEQ(R=N)
OPS(O1=M400%O2=|M400%O3=|M400%O4=%O5=%O6=)
WIN(W1=1000%W2=0|1000%W3=0|1000%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=38-42%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=38-42%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=38-42%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=15C%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# Efficient Networks ADSL modem, Speedstream 5100
Fingerprint Efficient Networks SpeedStream 5100 ADSL router
Class Efficient Networks | embedded || broadband router
SEQ(SP=FB-105%GCD=1-6%ISR=F2-FC%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5AC%O2=M5AC%O3=M5AC%O4=M5AC%O5=M5AC%O6=M5AC)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Eicon Shiva series VPN gateway. Running an embedded Linux-based operating system.
Fingerprint Eicon Shiva VPN gateway
Class Eicon | embedded || proxy server
SEQ(SP=101-10B%GCD=1-6%ISR=105-10F%TI=I%II=RI%SS=S%TS=U)
OPS(O1=WAN%O2=M578%O3=%O4=%O5=M218%O6=M109)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=N)
T1(R=Y%DF=N%T=12D-137%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=5C-70%TG=80%W=0%S=Z%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T6(R=Y%DF=N%T=6B-75%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=6B-75%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=6B-75%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=CCF1%RUD=G)
IE(DFI=S%T=12D-137%TG=FF%CD=S)

# Elsag datamat sas200 italian adsl router
Fingerprint Elsag Datamat SAS-200 ADSL modem
Class Elsag Datamat | embedded || broadband router
SEQ(SP=0-5%GCD=388|710|A98|E20|11A8%ISR=64-6E%TI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M564%O3=M26C%O4=M578%O5=M204%O6=MF5)
WIN(W1=200%W2=200%W3=200%W4=200%W5=200%W6=200)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=200%O=M578%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR|EAR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR|EAR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=R|ER%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR|EAR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=R|ER%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR|EAR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Ember InSight Adapter EM2XX chip programmer/debugger
Fingerprint Ember InSight Adapter for programming EM2XX-family embedded devices
Class Ember | embedded || specialized
SEQ(SP=0%GCD=FFF7|1FFEE|2FFE5|3FFDC|4FFD3|5FFCA%ISR=95-9F%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=N)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# EMC Celerra SAN 
Fingerprint EMC Celerra NAS device
Class EMC | embedded || storage-misc
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=RI%TS=1|3)
OPS(O1=M5B4NNSNW3NNT11%O2=M5B4NNSNW3NNT11%O3=M5B4NW3NNT11%O4=M5B4NNSNW3NNT11%O5=M5B4NNSNW3NNT11%O6=M5B4NNSNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NNSNW3%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# EMC Celerra NS350 version 5.5.25-2
# EMC Celerra File Server
# EMC Celerra File Server  Version: T5.5.29.1
Fingerprint EMC Celerra NS350 NAS device
Class EMC | embedded || storage-misc
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%II=I%TS=1|2|3)
OPS(O1=M5B4NNSNW3NNT11%O2=M5B4NNSNW3NNT11%O3=M5B4NW3NNT11%O4=M5B4NNSNW3NNT11%O5=M5B4NNSNW3NNT11%O6=M5B4NNSNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NNSNW3%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N|Y%T=3B-45|FA-104%TG=40|FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# EMC Celerra File Serrver, Build: T5.6.44.408 Version 4.0
# EMC Celerra File Serrver, Build: T5.6.44.408 Version 5.0
# EMC Clariion NS700G DataMover running OS (DART Version) 5.6.44
Fingerprint EMC Celerra or Clarion NAS device
Class EMC | embedded || storage-misc
SEQ(SP=F-19%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%CI=I%II=I%TS=1|2|3)
OPS(O1=M5B4NNSNW3NNT11%O2=M5B4NNSNW3NNT11%O3=M5B4NW3NNT11%O4=M5B4NNSNW3NNT11%O5=M5B4NNSNW3NNT11%O6=M5B4NNSNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NNSNW3%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NNSNW3NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# IPCop V1.4.11 (1.4.10 updated to 1.4.11)
# Linux 2.4.34 #1 Tue Jan 9 01:40:56 GMT 2007 i586 GenuineIntel unknown GNU/Linux (IPCop firewall v1.4.15)
# IPCOP 1.4.15; Linux 2.4.34 #1 Fri Mar 9 23:51:29 GMT 2007 i586 pentium-mmx i386 GNU/Linux running IPCOP v. 1.4.15 w/ Copfilter v. 0.82.1
# Ipcop 1.4.18
# IPcop firewall1.4.21, Linux 2.4.36 #1 Tue Jul 22 13:13:24 GMT 2008 i686 pentium2 i386 GNU/Linux      IPCOP1.4.21
# Linux 2.6.22.19-72.e19 #1 SMP Thu Nov 26 12:12:03 EST 2009 i686 i686 i386 GNU/Linux, gui indicates Endian Firewall Appliance release 2.3-1 (Deployset #0) (c) 2004-2009
Fingerprint Endian 2.3 or IPCop firewall 1.4.10 - 1.4.21 (Linux 2.4.31 - 2.6.22)
Class Endian | Linux | 2.4.X | firewall
Class IPCop | Linux | 2.4.X | firewall
SEQ(SP=BA-D2%GCD=1-6%ISR=C6-D4%TI=Z%II=I%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Enerium 200; Energy monitoring device
# Mitsubishi Electric Projector XD1000
Fingerprint Enerdis Enerium 200 energy monitoring device or Mitsubishi XD1000 projector
Class Enerdis | embedded || power-device
Class Mitsubishi | embedded || media device
SEQ(SP=F8-10C%GCD=1-6%ISR=100-114%TI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=1FF%W2=1FF%W3=1FF%W4=1FF%W5=1FF%W6=1FF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1FF%O=M400%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1FF%S=O%A=S+%F=AS%O=M400%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# enistic.com power zone controller
Fingerprint Enistic Zone Controller WAP
Class Enistic | embedded || WAP
SEQ(SP=C9-D3%GCD=1-6%ISR=CF-D9%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=7F%W2=7F%W3=7F%W4=7F%W5=7F%W6=7F)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=7F%O=M400%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Enterasys XSR Security Router
Fingerprint Enterasys XSR firewall
Class Enterasys | embedded || firewall
SEQ(SP=8D-9B%GCD=1-6%ISR=95-9F%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4074%W5=4180%W6=403D)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=403D%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=134%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Enterasys Networks, Inc. B3G124-48P Rev 06.03.02.0006
# Enterasys Networks, Inc. B3G124-24P Rev 06.03.02.0006
# Enterasys Networks, Inc. D2G124-12P Rev 06.03.02.0006
Fingerprint Enterasys B3 BG3124 or D2 D2G124 switch
Class Enterasys | embedded || switch
SEQ(SP=0-B8%GCD=1-7|FA01|1F402|2EE03|3E804|4E205%ISR=96-AE%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=NNM5B4SNW0%O2=NNM5B4SNW0%O3=M5B4NW0%O4=NNM5B4SNW0%O5=NNM5B4SNW0%O6=NNM5B4S)
WIN(W1=2710%W2=2710%W3=2710%W4=2710%W5=2710%W6=2710)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2710%O=NNM5B4SNW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=R%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=138%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=Z)

# HP Color LaserJet 3600 JetDirect Model Number: J7973E Firmware Version: V.30.31.BA
# Enterasys Networks, Inc. Matrix C1 C1H124-48 Rev 02.00.19 04/28/2005--09:00 ofc
Fingerprint Enterasys Matrix C1 switch or HP LaserJet 3600 printer
Class Enterasys | embedded || switch
Class HP | embedded || printer
SEQ(SP=93-9D%GCD=1-6%ISR=9A-A4%TI=I%II=I%SS=S%TS=1|2)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Matrix 1H582-51
Fingerprint Enterasys Matrix E1 switch
Class Enterasys | embedded || switch
SEQ(SP=F0-104%GCD=1-6%ISR=F4-108%TI=I%II=I%SS=S%TS=1)
OPS(O1=M200NW0NNT11%O2=M200NW0NNT11%O3=M200NW0NNT11%O4=M200NW0NNT11%O5=M200NW0NNT11%O6=M200NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M200NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# It's an Enterasys E1 router switch Matrix 1G587-09
# Enterasys E1 1H582-51  Rev 03.07.31 0000 08/21/2008--17:21 ofc
Fingerprint Enterasys Matrix E1 switch
Class Enterasys | embedded || switch
SEQ(SP=93-9F%GCD=1-6%ISR=9C-A6%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Enterasys N7 switch with routing functionality.
Fingerprint Enterasys Matrix N7 switch
Class Enterasys | embedded || switch
SEQ(SP=96-A0%GCD=1-6%ISR=9C-A6%TI=I%CI=I%II=RI%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Enterasys SecureStack C2, Chassis Firmware Revision:  05.00.28
Fingerprint Enterasys SecureStack C2 switch
Class Enterasys | embedded || switch
SEQ(SP=0-5%GCD=FA01|1F402|2EE03|3E804|4E205%ISR=95-9F%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=NNT11M5B4NW0%O2=NNT11M578NW0%O3=NNT11M280NW0%O4=NNT11M218NW0%O5=NNT11M218NW0%O6=NNT11M109NW0)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=11C%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=Z)

# Enterasys XP 8600 SSR 8600 router switch
# XP-8000 - Enterasys Networks Firmware Version: E10.0.0.13 PROM Version: prom-E3.3.0.0
# SSR 2000 - Enterasys Networks Firmware Version: E10.0.0.16 PROM Version: prom-E3.2.0.0
# XP 2400 - Enterasys Networks Firmware Version: E10.0.0.16 PROM Version: prom-E3.3.0.0
Fingerprint Enterasys SSR router or XP switch
Class Enterasys | embedded || switch
Class Enterasys | embedded || router
SEQ(SP=92-9C%GCD=1-6%ISR=97-A1%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4074%W5=4180%W6=403D)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=403D%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Epson Colour AcuLaser C1100
Fingerprint Epson AcuLaser C1100 or CX11NF printer
Class Epson | embedded || printer
SEQ(SP=97-A1%GCD=1-6%ISR=9B-A5%TI=I%TS=1)
OPS(O1=M5C8NW0NNT11%O2=M5C8NW0NNT11%O3=M5C8NW0NNT11%O4=M5C8NW0NNT11%O5=M5C8NW0NNT11%O6=M5C8NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5C8NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=2000%S=O%A=O%F=AS%O=M5C8NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(R=N)

# Epson AcuLaser C1100N laser printer. Software version: Ver. 02.30.
Fingerprint Epson AcuLaser C1100N printer
Class Epson | embedded || printer
SEQ(SP=94-9E%GCD=1-6%ISR=9B-A5%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5C8NW0NNT11%O2=M5C8NW0NNT11%O3=M5C8NW0NNT11%O4=M5C8NW0NNT11%O5=M5C8NW0NNT11%O6=M5C8NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5C8NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=2000%S=O%A=O%F=AS%O=M5C8NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Epson Artisan 810 Printer
Fingerprint Epson Artisan 810 printer
Class Epson | embedded || printer
SEQ(SP=BE-C8%GCD=1-6%ISR=C2-CC%TI=Z%CI=Z%TS=7)
OPS(O1=M5ACST11NW1%O2=M5ACST11NW1%O3=M5ACNNT11NW1%O4=M5ACST11NW1%O5=M5ACST11NW1%O6=M5ACST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5ACNNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# World Wide Packets LightningEdge (tm) LE-427 Access Distributor
# World Wide Packets LightningEdge (tm) LE-311 Access Concentrator
# World Wide Packets LightningEdge (tm) LE-327 Access Concentrator
# Ericsson BusinessPhone telephone exchange
Fingerprint Ericsson BusinessPhone PBX, or World Wide Packets LE-311, LE-327, or LE-427 LightningEdge switch
Class Ericsson | embedded || PBX
Class World Wide Packets | embedded || switch
SEQ(SP=44-4E%GCD=3E8|7D0|BB8|FA0|1388%ISR=99-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# EtherWerX PT-1000 PPPoE Terminator
Fingerprint EtherWerX PT-1000 PPPoE terminator
Class EtherWerX | embedded || router
SEQ(SP=CB-DD%GCD=1-6%ISR=D9-E3%TI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW3NNT01%O2=M5B4NW3NNT01%O3=M5B4NW3NNT01%O4=M5B4NW3NNT01%O5=M5B4NW3NNT01%O6=M5B4NNT01)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=N)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Exabyte 221L LTO3 Backup Device, Firmware Version : 11.6.1
Fingerprint Exabyte 221L LTO-3 tape library
Class Exabyte | embedded || storage-misc
SEQ(SP=FF-109%GCD=1-6%ISR=101-10D%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=111C%W2=111C%W3=111C%W4=111C%W5=111C%W6=111C)
ECN(R=Y%DF=N%T=3C%TG=40%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=111C%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=Z)

# Linux bubba 2.6.32.6 #1 Thu Jan 28 13:58:17 CET 2010 ppc GNU/Linux, running Debian Linux for PPC: http://www.excito.com/bubba/products/technical-specifications.html
Fingerprint Excito Bubba|Two file server (Linux 2.6.32)
Class Excito | Linux | 2.6.X | general purpose
SEQ(SP=B9-C3%GCD=1-6%ISR=C8-D2%TI=Z%II=I%TS=8)
OPS(O1=M5B4ST11NW4%O2=M5B4ST11NW4%O3=M5B4NNT11NW4%O4=M5B4ST11NW4%O5=M5B4ST11NW4%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW4%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW4%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Linux 2.6.32.6 #1 Thu Jan 28 13:58:17 CET 2010 ppc GNU/Linux
Fingerprint Linux 2.6.32
Class Excito | Linux | 2.6.X | general purpose
SEQ(SP=C5-CF%GCD=1-6%ISR=C8-D2%TI=Z%CI=Z%II=I%TS=8)
OPS(O1=M400CST11NW4%O2=M400CST11NW4%O3=M400CNNT11NW4%O4=M400CST11NW4%O5=M400CST11NW4%O6=M400CST11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8018%O=M400CNNSNW4%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=8000%S=O%A=S+%F=AS%O=M400CST11NW4%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Summit48i switch running ExtremeWare 7.3
# Extremeware Version 7.1.1
Fingerprint Extreme Networks Summit48si switch (ExtremeWare 7.1 - 7.8)
Class Extreme Networks | ExtremeWare | 7.X | switch
SEQ(SP=80-8E%GCD=1-6%ISR=88-92%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=134%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=S)

# Extreme Networks summit48si switch running ExtremeWare 7.6
# Software Version 7.8.2b1
# Extremeware  Version 7.4.3.5 [ssh] [base] by Release_Master on 12/12/05 13:34:02
Fingerprint Extreme Networks Summit48si switch (ExtremeWare 7.4 - 7.8)
Class Extreme Networks | ExtremeWare | 7.X | switch
SEQ(SP=64-8C%GCD=1-6%ISR=83-91%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=1A-24%TG=20%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1A-24%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=1A-24%TG=20%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1A-24%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1A-24%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1A-24%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7C-86%TG=80%IPL=38%UN=0%RIPL=134%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=7C-86%TG=80%CD=S)

# Extreme Networks x250e-48p layer 3 switch, ExtremeXOS version 12.0.1.11
# Extreme Networks Summit x350-48lt, ExtremeXOS version 12.0.3.16 v1203b16
Fingerprint Extreme Networks x250e or x350 switch (ExtremeXOS 12.0.1 - 12.0.3)
Class Extreme Networks | ExtremeXOS | 12.X | switch
SEQ(SP=C3-CD%GCD=1-6%ISR=C5-D3%TI=Z%CI=Z%II=I%TS=7)
OPS(O1=M5B4NNT11NW0%O2=M5B4NNT11NW0%O3=M5B4NNT11NW0%O4=M5B4NNT11NW0%O5=M5B4NNT11NW0%O6=M5B4NNT11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4NNT11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# f5 3650 big ip ltm
Fingerprint F5 BIG-IP 3650 Local Traffic Manager load balancer
Class F5 Networks | embedded || load balancer
SEQ(SP=FF-109%GCD=1-6%ISR=105-10F%TI=RD%CI=RD%II=I%TS=A)
OPS(O1=M5B4NW0NNT11SLL%O2=M5B4NW0NNT11SLL%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11SLL%O5=M5B4NW0NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=111C%W2=1068%W3=780%W4=648%W5=648%W6=31B)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=111C%O=M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# BIG-IP 6400, "BIG-IP 9.4.4 Build 73.1 Hotfix HF1"
Fingerprint F5 BIG-IP 6400 load balancer
Class F5 Networks | embedded || load balancer
SEQ(SP=C1-CB%GCD=1-6%ISR=C2-CC%TI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=269E%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# F5 BigIP.  Base OS is RedHat linux 2.4.
Fingerprint F5 BIG-IP load balancer
Class F5 Networks | embedded || load balancer
SEQ(SP=C0-D0%GCD=1-6%ISR=C8-D4%TI=Z%II=I%TS=U)
OPS(O1=M5B4NNSNW0%O2=M5B4NNSNW0%O3=M5B4NW0%O4=M5B4NNSNW0%O5=M5B4NNSNW0%O6=M5B4NNS)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%S=O%A=S+%F=AS%O=M5B4NNSNW0%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=29F9%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# BIG-IP Kernel 4.2PTF-10 Build95
Fingerprint F5 BIG-IP load balancer
Class F5 Networks | embedded || load balancer
SEQ(SP=F7-10B%GCD=1-6%ISR=FD-10B%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW4NNT11%O2=M5B4NW0NNT11%O3=M5B4NW4NNT11%O4=M5B4NW4NNT11%O5=M5B4NW4NNT11%O6=M5B4NNT11)
WIN(W1=4470%W2=41A0%W3=4100%W4=4000%W5=40E8%W6=402E)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4470%O=M5B4NW4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=402E%S=O%A=S+%F=AS%O=M5B4NW4NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# BIG-IP Version 10.0.0 5400.0 Final Edition
# BIG-IP 10.0.1 Build 283.0 Final
Fingerprint F5 BIG-IP load balancer
Class F5 Networks | embedded || load balancer
SEQ(SP=C5-D9%GCD=1-6%ISR=C9-D3%TI=I%II=I%SS=O%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# F5 Networks Big IP device running TMOS (proprietary Linux)with LTM and SSL offload modules.
Fingerprint F5 BIG-IP load balancer
Class F5 Networks | embedded || load balancer
SEQ(SP=FA-104%GCD=1-6%ISR=FC-106%TI=Z%II=I%TS=U)
OPS(O1=M564NNSNW0%O2=M564NNSNW0%O3=M564NW0%O4=M564NNSNW0%O5=M564NNSNW0%O6=M564NNS)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M564NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=8AA1%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# F5 BIG IP LTM load balancer running OS version 9.1.0.3.0, Linux kernel version 2.4.21.
Fingerprint F5 BIG-IP Local Traffic Manager load balancer
Class F5 Networks | embedded || load balancer
SEQ(SP=C1-CB%GCD=1-6%ISR=C4-CE%TI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# Force10 Operating System Version: 1.0, Force10 Application Software Version: 8.3.1.1, System Type: S50N
Fingerprint Force10 S50N switch (FTOS 1.0)
Class Force10 | FTOS | 1.X | switch
SEQ(SP=D1-DB%GCD=1-6%ISR=D8-E2%TI=I%CI=I%II=I%SS=S%TS=0)
OPS(O1=M564NW0NNT01%O2=M564NW0NNT01%O3=M564NW0NNT01%O4=M564NW0NNT01%O5=M564NW0NNT01%O6=M564NNT01)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M564NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M564NW0NNT01%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Force10 Networks S-Series switch running SFTOS 2.5.1.3
Fingerprint Force10 Networks S-Series switch (SFTOS 2.5.1.3)
Class Force10 | SFTOS | 2.X | switch
SEQ(SP=0-5%GCD=FA01|1F402|2EE03|3E804|4E205%ISR=95-9F%TI=I%II=I%SS=S%TS=A)
OPS(O1=NNT11M5B4NW0%O2=NNT11M578NW0%O3=NNT11M280NW0%O4=NNT11M218NW0%O5=NNT11M218NW0%O6=NNT11M109NW0)
WIN(W1=2710%W2=2710%W3=2710%W4=2710%W5=2710%W6=2710)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2710%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=11C%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=Z)

# FORE Systems ForeThought 4.1.0 1.76
Fingerprint FORE Systems ForeThought ATM switch
Class FORE Systems | embedded || switch
SEQ(SP=0-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=1000%W2=1000%W3=F00%W4=1000%W5=EA8%W6=F87)
ECN(R=Y%DF=N%T=3C%TG=40%W=1000%O=M400%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=F87%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Fortinet Fortigate FGT-50B - OS Version : 4.0 MR2
# Fortigate 310B
Fingerprint Fortinet FortiGate-50B or 310B firewall
Class Fortinet | embedded || firewall
SEQ(SP=F9-10B%GCD=1-6%ISR=105-10F%TI=BI|RD%TS=7|9)
OPS(O1=M5B4ST11NW1%O2=M5B4ST11NW1%O3=M5B4NNT11NW1%O4=M5B4ST11NW1%O5=M5B4ST11NW1%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=N)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(R=N)
IE(R=N)

# Fortinet 100A
# FortiGate 60B, firmware: v4.0,build0192,091222 (MR1 Patch 2)
Fingerprint Fortinet FortiGate-60B or -100A firewall
Class Fortinet | embedded || firewall
SEQ(SP=102-10C%GCD=1-6%ISR=105-10F%TI=BI%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=N)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Foundry Networks EdgeIron ethernet switch
Fingerprint Foundry EdgeIron switch
Class Foundry | embedded || switch
SEQ(SP=8F-99%GCD=1-6%ISR=92-9C%TI=I%II=RI%SS=O%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=M5B4NW0NNT11SSNNLLLLLL|M5B4NW0NNT11NNLLLLLLLLLL%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# foundry FastIron 400 Router, SYSIF version 21
Fingerprint Foundry FastIron 400 switch
Class Foundry | embedded || switch
SEQ(SP=74-96%GCD=1-6%ISR=7F-93%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=4000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=U)
T3(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=U)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=U)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=U)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Foundry MLX-16 (mpls router)
Fingerprint Foundry NetIron MLX-16 switch (IronWare)
Class Foundry | embedded || switch
SEQ(SP=7E-92%GCD=1-6%ISR=88-94%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FDE8%W2=FDE8%W3=FDE8%W4=FDE8%W5=FDE8%W6=FDE8)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FDE8%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=1%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Foundry FES2402
# Foundry Server Iron 4G
# Foundry ServerIron GT EGx2 load balancer, SW: Version 11.0.00aTD2 Copyright (c) 1996-2007 Foundry Networks, Inc.
Fingerprint Foundry Networks FES2402 switch, ServerIron 4G proxy server, or ServerIron GT EGx2 load balancer
Class Foundry | embedded || switch
Class Foundry | embedded || proxy server
Class Foundry | embedded || load balancer
SEQ(SP=79-95%GCD=1-6%ISR=79-91%TI=I%CI=I%II=I%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=U)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=U)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=U)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=U)
U1(DF=N%T=3B-45%TG=40%IPL=44%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=I)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# BigIron RX Router IronWare : Version 2.2.1pT143
Fingerprint Foundry BigIron RX switch (IronWare 2.2.1)
Class Foundry | IronWare | 2.X | switch
SEQ(SP=78-94%GCD=1-6%ISR=78-92%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FDE8%W2=FDE8%W3=FDE8%W4=FDE8%W5=FDE8%W6=FDE8)
ECN(R=Y%DF=N%T=41%TG=40%W=FDE8%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=U)
T3(R=Y%DF=Y%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
T4(R=Y%DF=Y%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=U)
T5(R=Y%DF=Y%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
T6(R=Y%DF=Y%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=U)
T7(R=Y%DF=Y%T=41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=U)
U1(DF=N%T=41%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=41%TG=40%CD=S)

# Foundry BigIronRX IronWare Version 2.2.1lT157
Fingerprint Foundry BigIron RX switch (IronWare 2.2.1lT157)
Class Foundry | IronWare | 2.X | switch
SEQ(SP=8C-96%GCD=1-6%ISR=8A-94%TI=I%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FDE8%W2=FDE8%W3=FDE8%W4=FDE8%W5=FDE8%W6=FDE8)
ECN(R=Y%DF=N%T=41%TG=40%W=FDE8%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=U)
T3(R=Y%DF=Y%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
T4(R=Y%DF=Y%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=U)
T5(R=Y%DF=Y%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
T6(R=Y%DF=Y%T=41%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=U)
T7(R=Y%DF=Y%T=41%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=U)
U1(DF=N%T=41%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=41%TG=40%CD=S)

# Foundry BigIron RX (Image Version 2.2.1)
# Netiron 4000 XMR IronWare : Version 3.6.0aT177
# Foundry Networks BigIron RX IronWare 2.4.0cT143
# Foundry BigIron RX version 2.4.0cT145
Fingerprint Foundry BigIron RX switch, NetIron MLX switch, or NetIron 4000 XMR switch (IronWare 2.2.1 - 3.6.0)
Class Foundry | IronWare | 2.X | switch
Class Foundry | IronWare | 3.X | switch
SEQ(SP=7B-95%GCD=1-6%ISR=7D-9B%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FDE8%W2=FDE8%W3=FDE8%W4=FDE8%W5=FDE8%W6=FDE8)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FDE8%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=U)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=U)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=U)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=U)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Foundry FI-4802 L2/L3 switch running version 08.0.00bT53
# Foundry FastIron 4802 running 08.0.00bT53
# Foundry FastIron FESX (Image Version 3.1.0)
# HP ProCurve 9304 HP J4139A
# Foundry Networks FastIron II Plus running SW Version 07.2.06T51
# 4.x of the code and is a FastIron GS 648p
# Foundry Workgroug Switch Model FX448
Fingerprint Foundry FastIron switch (4802, FESX, GS 648P, X448, or II Plus) (IronWare)
Class Foundry | IronWare | 3.X | switch
Class Foundry | IronWare | 4.X | switch
SEQ(SP=6E-A2%GCD=1-6%ISR=6C-92%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=U)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=U)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=U)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=U)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Netiron XMR, IronWare : Version 3.8.0fT177
Fingerprint Foundry NetIron MLX switch (IronWare 3.8.0)
Class Foundry | IronWare | 3.X | switch
SEQ(SP=7A-9C%GCD=1-6%ISR=7F-8F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FDE8%W2=FDE8%W3=FDE8%W4=FDE8%W5=FDE8%W6=FDE8)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FDE8%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=U)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=U)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=1%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=U)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=U)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Foundry Networks BigIron 8000 router, IronWare 07.8.02eT53
Fingerprint Foundry Networks BigIron 8000 switch (IronWare 07.8.02eT53)
Class Foundry | IronWare | 7.X | switch
SEQ(SP=FE-108%GCD=1-6%ISR=104-10E%TI=I|RD%II=I%SS=O|S%TS=U)
OPS(O1=M564%O2=M564%O3=M564%O4=M564%O5=M564%O6=M564)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M564%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=80%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=100%S=A+%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=FFFF%S=A+%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Free Freebox V5
Fingerprint Free Freebox V5 ADSL modem
Class Free | Linux || broadband router
SEQ(SP=BC-C6%GCD=1-6%ISR=C6-D0%TI=Z%II=I%TS=7)
OPS(O1=M564ST11NW2%O2=M564ST11NW2%O3=M564NNT11NW2%O4=M564ST11NW2%O5=M564ST11NW2%O6=M564ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M564NNSNW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M564ST11NW2%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# FreeBSD 2.2.9 (default everything, vmware)
# 2.2.8-STABLE FreeBSD 2.2.8-STABLE  i386
Fingerprint FreeBSD 2.2.8-STABLE - 2.2.9 (x86)
Class FreeBSD | FreeBSD | 2.X | general purpose
SEQ(SP=92-9E%GCD=1-6%ISR=98-A2%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4074%W5=4180%W6=403D)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=403D%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# FreeBSD 3.5.1
Fingerprint FreeBSD 3.5.1 (x86)
Class FreeBSD | FreeBSD | 3.X | general purpose
SEQ(SP=8F-99%GCD=1-6%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4470%W2=41A0%W3=4100%W4=4000%W5=40E8%W6=402E)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4470%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=402E%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# FreeBSD 4.10-RELEASE FreeBSD 4.10-RELEASE #0: Tue May 25 22:47:12 GMT 2004 i386
Fingerprint FreeBSD 4.10-RELEASE (x86)
Class FreeBSD | FreeBSD | 4.X | general purpose
SEQ(SP=FC-10A%GCD=1-6%ISR=100-110%TI=I%II=I%SS=S%TS=7)
OPS(O1=M564NW0NNT11%O2=M564NW0NNT11%O3=M564NW0NNT11%O4=M564NW0NNT11%O5=M564NW0NNT11%O6=M564NNT11)
WIN(W1=E000%W2=E000%W3=E000%W4=E000%W5=E000%W6=E000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=E000%O=M564NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Submitted on Wed, 13 Sep 2006 04:04:14 -0700
# uname -a: FreeBSD 4.11-RELEASE-p25 FreeBSD 4.11-RELEASE-p25 #0: Wed Oct  4 10:47:27 CEST 2006 i386
# FreeBSD 5.4-SECURITY FreeBSD 5.4-SECURITY #0: Tue Apr 18 06:15:11 UTC 2006 i386
Fingerprint FreeBSD 4.10-RELEASE - 5.4-SECURITY
Class FreeBSD | FreeBSD | 4.X | general purpose
Class FreeBSD | FreeBSD | 5.X | general purpose
SEQ(SP=DF-10D%GCD=1-6%ISR=107-10D%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=E000%W2=E000%W3=E000%W4=E000%W5=E000%W6=E000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=E000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=E000%S=O%A=O|S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 4.10-STABLE FreeBSD 4.10-STABLE #2: Wed Jun 16 16:44:09 PDT 2004 i386
# FreeBSD 4.11-SECURITY (i386)
# 4.10-SECURITY FreeBSD 4.10-SECURITY #0: Wed Jun 29 20:49:39 GMT 2005
Fingerprint FreeBSD 4.10-STABLE - 4.11-SECURITY
Class FreeBSD | FreeBSD | 4.X | general purpose
SEQ(SP=F7-105%GCD=1-6%ISR=FB-10F%TI=I%II=I%SS=S%TS=7)
OPS(O1=M3FD8NW0NNT11%O2=M3FD8NW0NNT11%O3=M3FD8NW0NNT11%O4=M3FD8NW0NNT11%O5=M3FD8NW0NNT11%O6=M3FD8NNT11)
WIN(W1=E000%W2=E000%W3=E000%W4=E000%W5=E000%W6=E000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=E000%O=M3FD8NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=E000%S=O%A=S+%F=AS%O=M3FD8NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 4.11-RELEASE FreeBSD 4.11-RELEASE #5: Tue Sep  6 13:34:07 PDT 2005 i386
Fingerprint FreeBSD 4.11-RELEASE
Class FreeBSD | FreeBSD | 4.X | general purpose
SEQ(SP=FA-10A%GCD=1-6%ISR=106-110%TI=RD%II=RI%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=E000%W2=E000%W3=E000%W4=E000%W5=E000%W6=E000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=E000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=E000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 4.11-RELEASE-p26 FreeBSD 4.11-RELEASE-p26 #1: Tue Jun 26 12:53:19 NOVST 2007 i386
Fingerprint FreeBSD 4.11-RELEASE
Class FreeBSD | FreeBSD | 4.X | general purpose
SEQ(SP=F0-10A%GCD=1-6%ISR=108-112%TI=RD%II=RI%TS=8)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=E000%W2=E000%W3=E000%W4=E000%W5=E000%W6=E000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=E000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=E000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 4.11 (vmware)
# FreeBSD 4.11-RELEASE-p26 FreeBSD 4.11-RELEASE-p26 #0: Fri Jan 19 19:10:38 EST 2007  i386
Fingerprint FreeBSD 4.11-RELEASE (x86)
Class FreeBSD | FreeBSD | 4.X | general purpose
SEQ(SP=DE-110%GCD=1-6%ISR=102-110%TI=I%II=I%SS=S%TS=7)
OPS(O1=M586NW0NNT11|M5B4NW0NNT11%O2=M586NW0NNT11|M5B4NW0NNT11%O3=M586NW0NNT11|M5B4NW0NNT11%O4=M586NW0NNT11|M5B4NW0NNT11%O5=M586NW0NNT11|M5B4NW0NNT11%O6=M586NNT11|M5B4NNT11)
WIN(W1=E000%W2=E000%W3=E000%W4=E000%W5=E000%W6=E000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=E000%O=M586NW0|M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=E000%S=O%A=O|S+%F=AS%O=M586NW0NNT11|M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 4.11-STABLE FreeBSD 4.11-STABLE #19: Tue Aug  8 01:35:43 JST 2006 i386
Fingerprint FreeBSD 4.11-STABLE
Class FreeBSD | FreeBSD | 4.X | general purpose
SEQ(SP=F2-106%GCD=1-6%ISR=100-10E%TI=RD%II=RI%TS=7)
OPS(O1=M3FD8NW0NNT11%O2=M3FD8NW0NNT11%O3=M3FD8NW0NNT11%O4=M3FD8NW0NNT11%O5=M3FD8NW0NNT11%O6=M3FD8NNT11)
WIN(W1=E000%W2=E000%W3=E000%W4=E000%W5=E000%W6=E000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=E000%O=M3FD8NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=E000%S=O%A=S+%F=AS%O=M3FD8NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 4.11-STABLE FreeBSD 4.11-STABLE #7: Thu Jul 19 02:04:40 CEST 2007 i386
Fingerprint FreeBSD 4.11-STABLE
Class FreeBSD | FreeBSD | 4.X | general purpose
SEQ(SP=FF-109%GCD=1-6%ISR=107-111%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=E000%W2=E000%W3=E000%W4=E000%W5=E000%W6=E000)
ECN(R=Y%DF=Y%T=41%TG=40%W=E000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=41%TG=40%W=E000%S=O%A=O|S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=41%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=41%TG=40%CD=S)

# FreeBSD 4.3-RELEASE FreeBSD 4.3-RELEASE #0: Sat Apr 21 10:54:49 GMT 2001
# AIX 3 5 0002EBEF4C00, AIX 5.3 on System P machine
# AIX oslevel: 5300-08-01-0819 (Version 5.3, Technology Level 8, Service Pack 1 / 2008 Week 19)
# AIX 1 6 00C1636E4C00
Fingerprint FreeBSD 4.3-RELEASE or IBM AIX 5.3 - 6.1
Class FreeBSD | FreeBSD | 4.X | general purpose
Class IBM | AIX | 5.X | general purpose
SEQ(SP=F6-108%GCD=1-6%ISR=101-10D%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4470%W2=41A0%W3=4100%W4=4000%W5=40E8%W6=402E)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4470%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=402E%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# FreeBSD 4.6.2-RELEASE FreeBSD 4.6.2-RELEASE #0: Wed Aug 14 21:23:26 GMT 2002 i386
Fingerprint FreeBSD 4.6.2-RELEASE
Class FreeBSD | FreeBSD | 4.X | general purpose
SEQ(SP=102-10C%GCD=1-6%ISR=106-112%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=E000%W2=E000%W3=E000%W4=E000%W5=E000%W6=E000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=E000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=E000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 4.7-STABLE FreeBSD 4.7-STABLE #0: Mon Feb  3 00:57:16 PST 2003 i386
Fingerprint FreeBSD 4.7-STABLE
Class FreeBSD | FreeBSD | 4.X | general purpose
SEQ(R=N)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=41%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=41%TG=40%S=Z%A=S+%F=AR%RD=0%Q=)
T2(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=41%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=41%TG=40%CD=S)

# FreeBSD 4.9-RELEASE-p7
Fingerprint FreeBSD 4.9-RELEASE
Class FreeBSD | FreeBSD | 4.X | general purpose
SEQ(SP=FB-10B%GCD=1-6%ISR=FF-10D%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=E000%W2=E000%W3=E000%W4=E000%W5=E000%W6=E000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=E000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 5.1
Fingerprint FreeBSD 5.1
Class FreeBSD | FreeBSD | 5.X | general purpose
SEQ(SP=FA-104%GCD=1-6%ISR=100-10E%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW1NNT11%O2=M5B4NW1NNT11%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11%O5=M5B4NW1NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 5.2.1-RC2 FreeBSD 5.2.1
Fingerprint FreeBSD 5.2.1-RC2
Class FreeBSD | FreeBSD | 5.X | general purpose
SEQ(SP=101-10B%GCD=1-6%ISR=103-10F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 5.2.1-RELEASE FreeBSD 5.2.1-RELEASE #0
Fingerprint FreeBSD 5.2.1-RELEASE
Class FreeBSD | FreeBSD | 5.X | general purpose
SEQ(SP=FC-106%GCD=1-6%ISR=FD-10F%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW1NNT11%O2=M5B4NW1NNT11%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11%O5=M5B4NW1NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 5.5-RELEASE
# FreeBSD 5.4 on VMware (x86)
# FreeBSD 5.4-RELEASE FreeBSD 5.4-RELEASE #0: Wed Aug 31 15:36:36 MSD 2005 i386
# Kylin v2.1, derived from FreeBSD 5.3
# FreeBSD 5.3-RELEASE FreeBSD 5.3-RELEASE #1: Thu Dec 23 00:27:47 CST 2004     root@mydomain.com:/usr/obj/usr/src/sys/NS  i386
Fingerprint FreeBSD 5.3 or 5.5 (x86)
Class FreeBSD | FreeBSD | 5.X | general purpose
SEQ(SP=D6-10C%GCD=1-6%ISR=105-111%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW1NNT11NNS%O2=M5B4NW1NNT11NNS%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11NNS%O5=M5B4NW1NNT11NNS%O6=M5B4NNT11NNS)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11NNS%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 5.4-RELEASE FreeBSD 5.4-RELEASE #1: Sat Oct  8 12:26:06 SAST 2005 i386
Fingerprint FreeBSD 5.4-RELEASE
Class FreeBSD | FreeBSD | 5.X | general purpose
SEQ(SP=F7-105%GCD=1-6%ISR=105-113%TI=I%TS=U)
OPS(O1=M5B4NNS%O2=M5B4NNS%O3=M5B4%O4=M5B4NNS%O5=M5B4NNS%O6=M5B4NNS)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M5B4NNS%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 5.4-RELEASE-p12 FreeBSD 5.4-RELEASE-p12 #1: Wed Mar 29 08:16:11 EST 2006
Fingerprint FreeBSD 5.4-RELEASE
Class FreeBSD | FreeBSD | 5.X | general purpose
SEQ(SP=101-10B%GCD=1-6%ISR=104-10E%TS=7)
OPS(O1=M5B4NW0NNT11NNS%O2=M5B4NW0NNT11NNS%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11NNS%O5=M5B4NW0NNT11NNS%O6=M5B4NNT11NNS)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 5.4-RELEASE FreeBSD 5.4-RELEASE #0: Sun May  8 10:21:06 UTC 2005 i386
Fingerprint FreeBSD 5.4-RELEASE
Class FreeBSD | FreeBSD | 5.X | general purpose
SEQ(SP=F8-102%GCD=1-6%ISR=108-112%II=I%TS=7)
OPS(O1=M5B4NW1NNT11NNS%O2=M5B4NW1NNT11NNS%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11NNS%O5=M5B4NW1NNT11NNS%O6=M5B4NNT11NNS)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW1NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# FreeBSD 5.4-RELEASE-p7 FreeBSD 5.4-RELEASE-p7 #0: Sun Oct  2 08:13:15 EDT 2005 amd64
Fingerprint FreeBSD 5.4-RELEASE
Class FreeBSD | FreeBSD | 5.X | general purpose
SEQ(SP=EB-109%GCD=1-6%ISR=105-10F%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW1NNT11NNS%O2=M5B4NW1NNT11NNS%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11NNS%O5=M5B4NW1NNT11NNS%O6=M5B4NNT11NNS)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11NNS%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 5.4-STABLE FreeBSD 5.4-STABLE #1: Sun Aug 20 15:55:44 CEST 2006 i386
Fingerprint FreeBSD 5.4-STABLE
Class FreeBSD | FreeBSD | 5.X | general purpose
SEQ(SP=FE-108%GCD=1-6%ISR=104-10E%TI=I%TS=7)
OPS(O1=M3FD8NW0NNT11NNS%O2=M3FD8NW0NNT11NNS%O3=M3FD8NW0NNT11%O4=M3FD8NW0NNT11NNS%O5=M3FD8NW0NNT11NNS%O6=M3FD8NNT11NNS)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M3FD8NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=8000%S=O%A=O|S+%F=AS%O=M3FD8NW0NNT11NNS%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 5.4-STABLE FreeBSD 5.4-STABLE #1: Fri Jul 15 21:00:42 EEST 2005
Fingerprint FreeBSD 5.4-STABLE
Class FreeBSD | FreeBSD | 5.X | general purpose
SEQ(CI=I)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=Z%A=S+%F=AR%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 5.5-STABLE FreeBSD 5.5-STABLE #0: Fri Aug 25 18:10:37 CEST 2006
Fingerprint FreeBSD 5.5-STABLE
Class FreeBSD | FreeBSD | 5.X | general purpose
SEQ(SP=101-10B%GCD=1-6%ISR=108-112%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 5.5-STABLE FreeBSD 5.5-STABLE #0: Sat Feb 21 01:12:59 CET 2009 amd64
Fingerprint FreeBSD 5.5-STABLE
Class FreeBSD | FreeBSD | 5.X | general purpose
SEQ(SP=102-10C%GCD=1-6%ISR=106-112%TI=I%CI=I|RD%TS=A)
OPS(O1=M5B4NW1NNT11NNS%O2=M5B4NW1NNT11NNS%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11NNS%O5=M5B4NW1NNT11NNS%O6=M5B4NNT11NNS)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=FFFF%O=M5B4NW1NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=7B-85%TG=80%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11NNS%RD=0%Q=)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=S)

# FreeBSD 6.0-RELEASE FreeBSD 6.0-RELEASE #0: Wed Dec 28 10:43:37 UTC 2005 i386
Fingerprint FreeBSD 6.0-RELEASE
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=F8-10E%GCD=1-6%ISR=104-10E%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW1NNT11%O2=M5B4NW1NNT11%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11%O5=M5B4NW1NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.0-RELEASE (x86, custom compiled)
# FreeBSD 6.2-RELEASE-p1 FreeBSD 6.2-RELEASE-p1 #2: Thu Feb 15 04:32:59 CET 2007 i386
Fingerprint FreeBSD 6.0-RELEASE - 6.2-RELEASE
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=FB-107%GCD=1-6%ISR=FF-10F%TI=I%II=I%SS=S%TS=A)
OPS(O1=M3FD8NW1NNT11SLL%O2=M3FD8NW1NNT11SLL%O3=M3FD8NW1NNT11%O4=M3FD8NW1NNT11SLL%O5=M3FD8NW1NNT11SLL%O6=M3FD8NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M3FD8NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.0-SECURITY FreeBSD 6.0-SECURITY #0: Tue Feb 28 22:53:43 UTC 2006  i386
Fingerprint FreeBSD 6.0-SECURITY (x86)
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=ED-101%GCD=1-6%ISR=102-114%TI=I%TS=A)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=91-9B%TG=FF%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=91-9B%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=91-9B%TG=FF%W=FFFF%S=O%A=O|S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=91-9B%TG=FF%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=91-9B%TG=FF%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=91-9B%TG=FF%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=91-9B%TG=FF%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=91-9B%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=91-9B%TG=FF%CD=S)

# 6.0-STABLE FreeBSD 6.0-STABLE #2: Fri Mar 31 19:33:47 CST 2006  :/usr/obj/usr/src/sys/SECUREFILE  amd6
# FreeBSD 6.2-RELEASE #2: Wed Feb  7 14:48:24 PST 2007, custom kernel, i386.
Fingerprint FreeBSD 6.0-STABLE - 6.2-RELEASE
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=FF-10D%GCD=1-6%ISR=104-10E%TI=RI%TS=A)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.1-RELEASE FreeBSD 6.1-RELEASE #0: Tue May  9 23:24:39 MDT 2006 i386
Fingerprint FreeBSD 6.1-RELEASE
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=104-10E%GCD=1-6%ISR=100-10A%II=I%TS=21)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# FreeBSD 6.1-RELEASE FreeBSD 6.1-RELEASE #0: Thu Jul  6 03:22:03 MSD 2006 i386
Fingerprint FreeBSD 6.1-RELEASE
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=EF-10D%GCD=1-6%ISR=103-10D%II=I%TS=U)
OPS(O1=M5B4SLL%O2=M5B4SLL%O3=M5B4%O4=M5B4SLL%O5=M5B4SLL%O6=M5B4SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=FFFF%O=M5B4SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=S)

# FreeBSD 6.1-RELEASE-p1 FreeBSD 6.1-RELEASE-p1 #6: Thu Jun  8 18:52:03 UTC 2006 i386
Fingerprint FreeBSD 6.1-RELEASE
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=FA-10A%GCD=1-6%ISR=104-10E%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4SLL%O2=M5B4SLL%O3=M5B4%O4=M5B4SLL%O5=M5B4SLL%O6=M5B4SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.1-RELEASE FreeBSD 6.1-RELEASE #0: Sun May  7 04:32:43 UTC 2006 i386
Fingerprint FreeBSD 6.1-RELEASE
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=F5-107%GCD=1-6%ISR=108-112%TI=I%CI=I%II=I%SS=S%TS=8|9)
OPS(O1=M4BENW1NNT11SLL%O2=M4BENW1NNT11SLL%O3=M4BENW1NNT11%O4=M4BENW1NNT11SLL%O5=M4BENW1NNT11SLL%O6=M4BENNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M4BENW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.1-RELEASE FreeBSD 6.1-RELEASE #0: Sun May  7 04:42:56 UTC 2006
# 6.2-BETA3
# FreeBSD 6.2-PRERELEASE FreeBSD 6.2-PRERELEASE #0: Mon Dec 11 11:43:36 GMT 2006  sparc64
# FreeBSD 6.2-STABLE FreeBSD 6.2-STABLE #3: Mon Apr  2 17:12:55 MSD 2007  i386
# FreeBSD/i386 6.2-RELEASE-p2
# FreeBSD 6.2-PRERELEASE FreeBSD 6.2-PRERELEASE #10: Sun Oct  1 19:30:52 NZDT 2006 i386
# FreeBSD 6.2-RELEASE FreeBSD 6.2-RELEASE #0: Fri Jan 12 11:05:30 UTC 2007 i386
Fingerprint FreeBSD 6.1-RELEASE - 6.2
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=FA-10A%GCD=1-6%ISR=FE-116%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3A-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3A-45%TG=40%CD=S)

# FreeBSD 6.1-RELEASE FreeBSD 6.1-RELEASE #0: Sun May  7 04:32:43 UTC 2006 i386
# FreeBSD 6.2-RELEASE FreeBSD 6.2-RELEASE #0: Mon Feb 26 23:28:44 EET 2007 i386
Fingerprint FreeBSD 6.1-RELEASE - 6.2-RELEASE
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=FE-10A%GCD=1-6%ISR=FF-113%TI=I%II=I%SS=S%TS=9)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.1-RELEASE-p10 FreeBSD 6.1-RELEASE-p10 #1: Wed Oct 18 23:33:34 CEST 2006 amd64
Fingerprint FreeBSD 6.1-RELEASE-p10 (x86_64)
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=B7-FF%GCD=1-6%ISR=106-110%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5ACNW1NNT11SLL%O2=M5ACNW1NNT11SLL%O3=M5ACNW1NNT11%O4=M5ACNW1NNT11SLL%O5=M5ACNW1NNT11SLL%O6=M5ACNNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3A-44%TG=40%W=FFFF%O=M5ACNW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3A-44%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3A-44%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5ACNW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3A-44%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3A-44%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3A-44%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3A-44%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3A-44%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3A-44%TG=40%CD=S)

# FreeBSD 6.1-STABLE FreeBSD 6.1-STABLE #1: Thu Aug  3 15:45:50 OMSST 2006 i386
Fingerprint FreeBSD 6.1-STABLE
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=FD-109%GCD=1-6%ISR=108-112%TS=U)
OPS(O1=M5B4SLL%O2=M5B4SLL%O3=M5B4%O4=M5B4SLL%O5=M5B4SLL%O6=M5B4SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M5B4SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.2-RELEASE FreeBSD 6.2-RELEASE #0: Fri Jan 12 10:40:27 UTC 2007 i386
# FreeBSD 6.1-STABLE FreeBSD 6.1-STABLE #0: Thu Nov 30 12:23:06 EST 2006     <LocalID>  i386
Fingerprint FreeBSD 6.1-STABLE - 6.2-RELEASE
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=FE-108%GCD=1-6%ISR=102-10C%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

Fingerprint FreeBSD 6.2-RC1
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=FB-105%GCD=1-6%ISR=107-111%TI=I%II=I%SS=O|S%TS=C)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.2-RELEASE FreeBSD 6.2-RELEASE #0: Fri Jan 12 10:40:27 UTC 2007 i386
# FreeBSD 6.2-RELEASE FreeBSD 6.2-RELEASE #1: Tue Oct 30 20:56:32 UTC 2007 i386 (running pf with scrub in all fragment reassemble and sysctl set net.inet.tcp.rfc1323=0)
Fingerprint FreeBSD 6.2-RELEASE
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=F5-10B%GCD=1-6%ISR=FF-10F%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.2-RELEASE FreeBSD 6.2-RELEASE #0: Fri Jan 12 10:40:27 UTC 2007 i386
Fingerprint FreeBSD 6.2-RELEASE
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=107-111%TI=I%TS=A)
OPS(R=N)
WIN(R=N)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# FreeBSD  6.2-RELEASE FreeBSD 6.2-RELEASE #0: Fri Jan 12 11:05:30 UTC 2007 i386
Fingerprint FreeBSD 6.2-RELEASE
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=FF-109%GCD=1-6%ISR=107-111%TI=I%TS=A)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.2-RELEASE FreeBSD 6.2-RELEASE #0: Fri Jan 12 11:05:30 UTC 2007 i386
Fingerprint FreeBSD 6.2-RELEASE (x86)
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=FF-109%GCD=1-6%ISR=105-113%TI=I%TS=A)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=1%S=Z%A=O|S%F=AR%O=%RD=0%Q=U)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=1%S=Z%A=O|S%F=AR%O=%RD=0%Q=U)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.2-RELEASE-p2 #1: Wed Mar  7 18:04:02 CET 2007 i386 SMP with pf (+scrub in all) enabled
Fingerprint FreeBSD 6.2-RELEASE-p2 (pf with scrub enabled)
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=106-110%TI=I%TS=7)
OPS(O1=M5B4NW1NNT11NNS%O2=M5B4NW1NNT11NNS%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11NNS%O5=M5B4NW1NNT11NNS%O6=M5B4NNT11NNS)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3A-44%TG=40%W=FFFF%O=M5B4NW1NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3A-44%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=O|S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.2-STABLE FreeBSD 6.2-STABLE #0: Fri Sep 14 23:02:01 CEST 2007 i386
# FreeBSD 6.2-STABLE FreeBSD 6.2-STABLE #3: Wed Aug 22 18:13:08 CEST 2007 i386
# FreeBSD 6.3-PRERELEASE FreeBSD 6.3-PRERELEASE #2: Wed Nov  7 13:58:41 NOVT 2007
# FreeBSD 6.3-RELEASE FreeBSD 6.3-RELEASE #1: Mon Feb  4 11:40:47 UTC 2008 /CUSTOM  i386
# FreeBSD 6.4-STABLE FreeBSD 6.4-STABLE #0: Tue Mar 31 05:47:32 YEKST 2009 i386
Fingerprint FreeBSD 6.2-STABLE - 6.4-STABLE
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=FA-10A%GCD=1-6%ISR=104-1A0%TI=I%TS=A)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.3-PRERELEASE FreeBSD 6.3-PRERELEASE #0
Fingerprint FreeBSD 6.3-PRERELEASE
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=F2-FC%GCD=1-6%ISR=10B-115%TI=I%II=I%SS=O|S%TS=U)
OPS(O1=M5B4SLL%O2=M5B4SLL%O3=M5B4%O4=M5B4SLL%O5=M5B4SLL%O6=M5B4SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M5B4SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.3-PRERELEASE FreeBSD 6.3-PRERELEASE #2: Wed Nov  7 10:54:48 EST 2007 i386
Fingerprint FreeBSD 6.3-PRERELEASE
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=F9-10B%GCD=1-6%ISR=106-110%TI=RD%II=RI%TS=A)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.3-RELEASE FreeBSD 6.3-RELEASE #8: Fri Jan 18 14:12:55 PST 2008 i386
Fingerprint FreeBSD 6.3-RELEASE
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=103-10D%GCD=1-6%ISR=101-10B%II=I%TS=A)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.3-RELEASE-p11 FreeBSD 6.3-RELEASE-p11 #0: Wed Jun 10 02:41:41 UTC 2009 i386
Fingerprint FreeBSD 6.3-RELEASE
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=F8-10C%GCD=1-6%ISR=105-10F%TI=I%CI=I%TS=A)
OPS(O1=M3FD8NW1NNT11SLL%O2=M3FD8NW1NNT11SLL%O3=M3FD8NW1NNT11%O4=M3FD8NW1NNT11SLL%O5=M3FD8NW1NNT11SLL%O6=M3FD8NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.3-RELEASE-p2 FreeBSD 6.3-RELEASE-p2 #2: Fri Jul 11 14:00:55 PDT 2008 i386
Fingerprint FreeBSD 6.3-RELEASE
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=FE-108%GCD=1-6%ISR=100-10A%TI=I%II=I%SS=S%TS=21)
OPS(R=N)
WIN(R=N)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M558NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# 6.3-RELEASE-p1 FreeBSD 6.3-RELEASE-p1 #0: Fri Feb 15 17:27:45 EET 2008 i386
Fingerprint FreeBSD 6.3-RELEASE-p1
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=FB-10B%GCD=1-6%ISR=107-111%TI=I%TS=A)
OPS(O1=M3FD8NW1NNT11SLL%O2=M3FD8NW1NNT11SLL%O3=M3FD8NW1NNT11%O4=M3FD8NW1NNT11SLL%O5=M3FD8NW1NNT11SLL%O6=M3FD8NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M3FD8NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M3FD8NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.3-STABLE FreeBSD 6.3-STABLE #4: Tue Aug  5 15:43:22 CEST 2008 i386
Fingerprint FreeBSD 6.3-STABLE
Class FreeBSD | FreeBSD | 6.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=104-10E%TS=A)
OPS(O1=M550NW1NNT11SLL%O2=M550NW1NNT11SLL%O3=M550NW1NNT11%O4=M550NW1NNT11SLL%O5=M550NW1NNT11SLL%O6=M550NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M550NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M550NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.2-RELEASE-p11 FreeBSD 6.2-RELEASE-p11 #0: Sun Feb 17 09:52:57 CET 2008     root@pcbsd62:/usr/obj/freenas/usr/src/sys/FREENAS-i386  i386
Fingerprint FreeNAS (FreeBSD 6.2-RELEASE)
Class FreeBSD | FreeBSD | 6.X | storage-misc
SEQ(SP=EA-10C%GCD=1-6%ISR=103-10F%TI=I%II=I%SS=S%TS=9)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.4-RELEASE-p3 (revision 199506)
Fingerprint FreeNAS (FreeBSD 6.4-RELEASE-p3)
Class FreeBSD | FreeBSD | 6.X | storage-misc
SEQ(SP=FC-10A%GCD=1-6%ISR=106-110%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11SLL%O2=M5B4NW0NNT11SLL%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11SLL%O5=M5B4NW0NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.4-RELEASE-p3 FreeBSD 6.4-RELEASE-p3 #0: Fri Jan 16 22:41:42 UTC 2009 i386, FreeNAS
Fingerprint FreeNAS (FreeBSD 6.4-RELEASE-p3)
Class FreeBSD | FreeBSD | 6.X | storage-misc
SEQ(SP=FE-108%GCD=1-6%ISR=102-10C%TI=I%CI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeNAS 0.671, OS Version: FreeBSD 6.1-STABLE (revison 199506), Platform: generic-pc on Intel Pentium III
Fingerprint FreeNAS 0.671 (FreeBSD 6.1-STABLE)
Class FreeBSD | FreeBSD | 6.X | storage-misc
SEQ(SP=F5-F6%GCD=1-6%ISR=105-107%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeNAS 0.686 running FreeBSD 6.2-RELEASE-p9 (revison 199506)
Fingerprint FreeNAS 0.686 (FreeBSD 6.2-RELEASE)
Class FreeBSD | FreeBSD | 6.X | storage-misc
SEQ(SP=100-10A%GCD=1-6%ISR=105-10F%TI=RI%TS=7|9)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeNAS v0.686. It is built on FreeBSD 6.2-RELEASE-p9 (revison 199506),
# VMware ESX Server 3i (The version that boots from a usb key), IPv4 stack only
# FreeBSD 6.2-RELEASE-p9 FreeBSD 6.2-RELEASE-p9 #0: Tue Dec 25 11:18:29 CET 2007 FREENAS-i386  i386
# VMware ESXi 4.0
# ESXi Server 4.0.0 build 181792
# VMWares ESXi 4.0 64bit hyperserver.  Take note that ESX != ESXi.
# VMware ESXi 4.0.0 build-193498
Fingerprint FreeNAS 0.686 (FreeBSD 6.2-RELEASE) or VMware ESXi Server 3.0 - 4.0
Class FreeBSD | FreeBSD | 6.X | storage-misc
Class VMware | ESX Server | 3.X | specialized
Class VMware | ESX Server | 4.X | specialized
SEQ(SP=F0-10A%GCD=1-6%ISR=100-110%TI=I%CI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.2-RELEASE-p8 (revison 199506), FreeNas server 0.686b1
# FreeBSD 6.2-RELEASE-p8 FreeBSD 6.2-RELEASE-p8 #0: Mon Oct 29 20:21:28 CET 2007 i386, FreeNAS Network Attached Storage
Fingerprint FreeNAS 0.686b (FreeBSD 6.2-RELEASE)
Class FreeBSD | FreeBSD | 6.X | storage-misc
SEQ(SP=FA-106%GCD=1-6%ISR=E9-111%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.4-RELEASE-p3 FreeBSD 6.4-RELEASE-p3 #0: Sat Apr 18 22:17:59 UTC 2009 i386, FreeNAS 0.69.1 Omnius (revision 4554)
Fingerprint FreeNAS 0.69.1 (FreeBSD 6.4-RELEASE-p3)
Class FreeBSD | FreeBSD | 6.X | storage-misc
SEQ(SP=F4-10A%GCD=1-6%ISR=FF-111%TI=I%II=I%SS=S%TS=9)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.3-STABLE FreeBSD 6.3-STABLE #0: Mon May  5 20:02:53 CEST 2008 i386
# FreeBSD 6.3-STABLE FreeBSD 6.3-STABLE #0: Sun Aug  3 17:53:28 CEST 2008 i386
# FreeBSD 6.4-RELEASE-p5 (revision 199506), FreeNAS 0.69.2
Fingerprint FreeNAS 0.69.2 (FreeBSD 6.3-STABLE - 6.4-RELEASE)
Class FreeBSD | FreeBSD | 6.X | storage-misc
SEQ(SP=FF-10B%GCD=1-6%ISR=101-10F%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.4-RELEASE-p5 FreeBSD 6.4-RELEASE-p5 #0: Wed Jun 10 23:45:29 UTC 2009 i386, FreeNAS 0.69.2 Muad'Dib (revision 4700)
Fingerprint FreeNAS 0.69.2 (FreeBSD 6.4-RELEASE)
Class FreeBSD | FreeBSD | 6.X | storage-misc
SEQ(SP=F9-103%GCD=1-6%ISR=105-113%CI=I%II=I%TS=7)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.4-RELEASE FreeBSD 6.4-RELEASE #0: Sun Nov 30 10:41:35 UTC 2008 i386, FreeNAS 0.69RC2 Rev. 4084
# FreeBSD 6.4-RELEASE-p5 FreeBSD 6.4-RELEASE-p5 #0: Wed Jun 10 23:45:29 UTC 2009 i386
Fingerprint FreeNAS 0.69RC2 (FreeBSD 6.4-RELEASE)
Class FreeBSD | FreeBSD | 6.X | storage-misc
SEQ(SP=FB-10B%GCD=1-6%ISR=FF-10F%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 6.4-RELEASE-p3 FreeBSD 6.4-RELEASE-p3 #0: Fri Jan 16 22:41:42 UTC 2009 i386, FreeNAS 0.69 Kwisatz Haderach (revision 4276)
# FreeBSD 6.4-RELEASE-p3 FreeBSD 6.4-RELEASE-p3 #0: Sat Apr 18 22:20:57 UTC 2009, amd64FreeNAS 0.69.1 (build 4554-AMD64)
Fingerprint FreeNAS 0.69RC2 (FreeBSD 6.4-RELEASE-p3)
Class FreeBSD | FreeBSD | 6.X | storage-misc
SEQ(SP=FC-10A%GCD=1-6%ISR=F6-112%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-CURRENT FreeBSD 7.0-CURRENT #19: Thu Aug  2 07:59:58 CST 2007 i386
# FreeBSD 7.0-STABLE FreeBSD 7.0-STABLE #222: Fri Sep 28 07:48:47 CST 2007 amd64
# FreeBSD 7.0-PRERELEASE FreeBSD 7.0-PRERELEASE #0: Mon Oct 15 20:12:38 PDT 2007 i386
# FreeBSD 7.0-RELEASE-p3 FreeBSD 7.0-RELEASE-p3 #2: Thu Jul 24 22:06:36 EDT 2008 i386
Fingerprint FreeBSD 7.0
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=108-112%TI=I%II=I%SS=S%TS=21|22)
OPS(O1=M5B4NW3NNT11|M5B4NW8NNT11%O2=M578NW3NNT11|M578NW8NNT11%O3=M280NW3NNT11|M280NW8NNT11%O4=M5B4NW3NNT11|M5B4NW8NNT11%O5=M218NW3NNT11|M218NW8NNT11%O6=M109NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3|M5B4NW8%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW3NNT11|M109NW8NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-BETA2 FreeBSD 7.0-BETA2 #0: Sun Nov 11 14:51:01 SAST 2007 i386
Fingerprint FreeBSD 7.0-BETA2 (custom compiled)
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=F9-10B%GCD=1-6%ISR=106-110%TI=I%TS=20|21)
OPS(O1=M5B4NW3NNT11%O2=M578NW3NNT11%O3=M280NW3NNT11%O4=M3FD8NW3NNT11%O5=M218NW3NNT11%O6=M109NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW3NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-BETA4 FreeBSD 7.0-BETA4 #3: Fri Dec 14 01:02:11 CET 2007
Fingerprint FreeBSD 7.0-BETA4
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=FF-109%GCD=1-6%ISR=106-110%TI=RD%TS=21)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLN%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# FreeBSD 7.0-BETA4 FreeBSD 7.0-BETA4 #7: Fri Dec 21 20:15:13 CET 2007 i386
# FreeBSD 7.0-RC1 FreeBSD 7.0-RC1  #0: Mon Dec 24 12:18:24 UTC 2007 i386 (VMWare)
# FreeBSD 7.0-PRERELEASE FreeBSD 7.0-PRERELEASE #7: Sat Jan 26 12:48:51 CST 2008 amd64
# FreeBSD 7.0-STABLE FreeBSD 7.0-STABLE #9: Fri Feb 29 19:59:08 CET 2008 i386
# FreeBSD 7.0-RELEASE FreeBSD 7.0-RELEASE #0: Sun Feb 24 19:59:52 UTC 2008 i386
# FreeBSD 7.0-RELEASE-p1 FreeBSD 7.0-RELEASE-p1
# FreeBSD 7.0-PRERELEASE FreeBSD 7.0-PRERELEASE #6: Fri Jan 25 10:44:09 BRST 2008 i386
# FreeBSD 7.0-RELEASE FreeBSD 7.0-RELEASE #0: Sun Feb 24 19:59:52 UTC 2008 i386
# FreeBSD 7.0-RELEASE-p4 FreeBSD 7.0-RELEASE-p4 #0: Tue Sep  219:32:35 UTC 2008 i386
Fingerprint FreeBSD 7.0-BETA4 - 7.0
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=F1-10B%GCD=1-6%ISR=FD-10F%TI=I%II=I%SS=S%TS=20|21|22)
OPS(O1=M5B4NW3ST11|M5B4NW4ST11|M5B4NW6ST11%O2=M578NW3ST11|M578NW4ST11|M578NW6ST11%O3=M280NW3NNT11|M280NW4NNT11|M280NW6NNT11%O4=M5B4NW3ST11|M5B4NW4ST11|M5B4NW6ST11%O5=M218NW3ST11|M218NW4ST11|M218NW6ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLN|M5B4NW4SLN|M5B4NW6SLN%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW3ST11|M109NW4ST11|M109NW6ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-CURRENT-200702 FreeBSD 7.0-CURRENT-200702 #0: Tue Feb  6 15:23:17 UTC 2007 sparc64
Fingerprint FreeBSD 7.0-CURRENT
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=FA-10A%GCD=1-6%ISR=104-10E%TI=I%TS=21|22)
OPS(O1=M5B4NW8NNT11SLL%O2=M578NW8NNT11SLL%O3=M280NW8NNT11%O4=M5B4NW8NNT11SLL%O5=M218NW8NNT11SLL%O6=M109NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW8SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW8NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-CURRENT FreeBSD 7.0-CURRENT #2: Thu Aug  9 08:08:02 CEST 2007 i386
Fingerprint FreeBSD 7.0-CURRENT
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=101-10D%GCD=1-6%ISR=108-112%TI=RD%II=RI%TS=20|21|22)
OPS(O1=M5B4NW8NNT11%O2=M578NW8NNT11%O3=M280NW8NNT11%O4=M5B4NW8NNT11%O5=M218NW8NNT11%O6=M109NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW8%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW8NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-CURRENT FreeBSD 7.0-CURRENT #0: Sat Aug 11 11:33:14 CEST 2007 i386
Fingerprint FreeBSD 7.0-CURRENT
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=EC-106%GCD=1-6%ISR=FF-113%TI=I%TS=21|22)
OPS(O1=M5B4NW8NNT11%O2=M578NW8NNT11%O3=M280NW8NNT11%O4=M3FD8NW8NNT11%O5=M218NW8NNT11%O6=M109NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW8%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M109NW8NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-CURRENT FreeBSD 7.0-CURRENT #2: Wed Oct 25 10:28:40 UTC 2006 i386
Fingerprint FreeBSD 7.0-CURRENT
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=F2-110%GCD=1-6%ISR=108-114%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW1NNT11SLL%O2=M578NW1NNT11SLL%O3=M280NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M218NW1NNT11SLL%O6=M109NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-CURRENT #52: Wed Dec 13 11:33:08 CET 2006
Fingerprint FreeBSD 7.0-CURRENT (pre-release)
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=F6-10A%GCD=1-6|8|10|18|20|28|30%ISR=F1-111%TI=I%TS=20|21|22)
OPS(O1=M5B4NW1NNT11SLL%O2=M578NW1NNT11SLL%O3=M280NW1NNT11%O4=M3FD8NW1NNT11SLL%O5=M218NW1NNT11SLL%O6=M109NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M109NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-RC1 FreeBSD 7.0-RC1 #4: Wed Jan  2 11:46:18 MST 2008
Fingerprint FreeBSD 7.0-RC1
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=101-10B%GCD=1-6%ISR=108-112%TI=I%TS=21)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M3FD8NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLN%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW3ST11%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-RELEASE FreeBSD 7.0-RELEASE #0: Mon Feb 25 09:35:41 UTC 2008 sparc64, PF firewall running.
# FreeBSD 7.0-RELEASE FreeBSD 7.0-RELEASE #0: Sun Feb 24 19:59:52 UTC 2008 i386
Fingerprint FreeBSD 7.0-RELEASE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=FF-109%GCD=1-6%ISR=106-110%TI=I%II=I%SS=S%TS=21|22)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLN%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-RELEASE-p2 FreeBSD 7.0-RELEASE-p2 #0: Wed Jun 18 07:33:20 UTC 2008 i386
Fingerprint FreeBSD 7.0-RELEASE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=F5-10D%GCD=1-6%ISR=109-113%TI=I%II=I%SS=S%TS=21)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-RELEASE FreeBSD 7.0-RELEASE #0 : Sun Feb 24 10:35:36 UTC 2008:/usr/obj/usr/src/sys/GENERIC  amd64
Fingerprint FreeBSD 7.0-RELEASE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=FC-106%GCD=1-6%ISR=106-110%TS=21)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLN%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=O|S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-RELEASE FreeBSD 7.0-RELEASE #0: Wed Dec 17 04:23:19 BRST 2008 i386
Fingerprint FreeBSD 7.0-RELEASE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=FA-104%GCD=1-6%ISR=102-10C%TI=RD%II=RI%TS=21)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLN%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-RELEASE FreeBSD 7.0-RELEASE #1
Fingerprint FreeBSD 7.0-RELEASE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=FD-107%GCD=1-6%ISR=101-10D%TI=I%II=I%SS=S%TS=21)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLN%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-RELEASE FreeBSD 7.0-RELEASE #0: Wed May 21 10:13:51 UTC 2008 amd64
Fingerprint FreeBSD 7.0-RELEASE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=F9-107%GCD=1-6%ISR=103-111%CI=I%TS=21)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M3FD8NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLN%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M109NW3ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-RELEASE FreeBSD 7.0-RELEASE #1: Mon Dec  1 15:22:47 MSK 2008 amd64
Fingerprint FreeBSD 7.0-RELEASE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=FC-10A%GCD=2|4|6|8|A%ISR=101-111%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4SLN%O2=M578SLN%O3=M280%O4=M5B4SLN%O5=M218SLN%O6=M109SLN)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4SLN%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109SLN%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-RELEASE-p11 FreeBSD 7.0-RELEASE-p11 #0: Sun Mar 22 07:08:52 UTC 2009 i386
# FreeBSD 7.1-RELEASE-p5 FreeBSD 7.1-RELEASE-p5 #5: Tue May  5 11:40:07 PDT 2009 i386
# FreeBSD 7.2-RELEASE-p1 FreeBSD 7.2-RELEASE-p1 #6: Mon Jun 15 01:46:37 PDT 2009 i386
# FreeBSD 8.0-STABLE
Fingerprint FreeBSD 7.0-RELEASE - 8.0-STABLE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=F7-111%GCD=1-6%ISR=107-111%TI=I%II=I%SS=S%TS=21|22)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW3ST11%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-RELEASE-p1 FreeBSD 7.0-RELEASE-p1 #0: Thu Jun  5 22:12:06 CDT 2008 amd64
Fingerprint FreeBSD 7.0-RELEASE-p1
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=108-112%TI=I%II=I%SS=S%TS=21)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLN%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW3ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-RELEASE-p1 FreeBSD 7.0-RELEASE-p1 #0: Sun Apr 27 21:47:56 EDT 2008 i386
# FreeBSD 7.0-STABLE FreeBSD 7.0-STABLE #8: Tue Apr 29 11:35:56 CEST 2008 i386
# FreeBSD 7.0-RELEASE-p3 FreeBSD 7.0-RELEASE-p3 #7: Sun Jul 13 21:02:29 PDT 2008 i386
# FreeBSD 7.1-PRERELEASE FreeBSD 7.1-PRERELEASE #1: Thu Sep 11 19:53:15 UTC 2008
# FreeBSD 7.1-PRERELEASE FreeBSD 7.1-PRERELEASE #0: Wed Oct  1 20:54:06 MSD 2008 i386
# FreeBSD 7.0-RELEASE-p5 FreeBSD 7.0-RELEASE-p5 #0: Wed Oct  1 10:10:12 UTC 2008 i386
# FreeBSD 7.1-RELEASE FreeBSD 7.1-RELEASE #0: Thu Jan  1 14:37:25 UTC 2009 i386
# FreeBSD 7.2-RELEASE FreeBSD 7.2-RELEASE #0: Fri May  1 08:49:13 UTC 2009 i386
# FreeBSD 7.2-STABLE FreeBSD 7.2-STABLE #0: Thu Jun 11 21:55:32 CEST 2009 i386
# FreeBSD 7.3-RELEASE FreeBSD 7.3-RELEASE #0: Mon May 17 19:49:57 EEST 2010 sparc64
# FreeBSD 8.0-CURRENT
# FreeBSD 8.0-RELEASE-p1 FreeBSD 8.0-RELEASE-p1 #10: Wed Dec 16 13:38:00 PST 2009 i386
# FreeBSD 7.3 x64
# FreeBSD 8.1-RC2
# FreeBSD 8.1-RELEASE-p1 FreeBSD 8.1-RELEASE-p1 #0: Sat Oct 16 23:26:34 CEST 2010 arm, Seagate FreeAgent Dockstar
Fingerprint FreeBSD 7.0-RELEASE-p1 - 8.1-RELEASE-p1
Class FreeBSD | FreeBSD | 7.X | general purpose
Class FreeBSD | FreeBSD | 8.X | general purpose
SEQ(SP=EC-10E%GCD=1-6%ISR=FC-112%TI=I%CI=I%II=I%SS=S%TS=20|21|22)
OPS(O1=M5B4NW3ST11|M5B4NW9ST11%O2=M578NW3ST11|M578NW9ST11%O3=M280NW3NNT11|M280NW9NNT11%O4=M5B4NW3ST11|M5B4NW9ST11%O5=M218NW3ST11|M218NW9ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL|M5B4NW9SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW3ST11|M109NW9ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-RELEASE-p2 FreeBSD 7.0-RELEASE-p2 #0: Thu Jun 19 22:57:42 CEST 2008 i386
# FreeBSD 7.0-STABLE FreeBSD 7.0-STABLE #12: Wed Aug  6 17:22:12 EEST 2008 i386
# FreeBSD 7.1-PRERELEASE FreeBSD 7.1-PRERELEASE #0: Thu Sep 11 14:26:13 CEST 2008 i386
Fingerprint FreeBSD 7.0-RELEASE-p2 - 7.1-PRERELEASE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=FA-108%GCD=1-6%ISR=105-10F%TI=I%TS=21|22)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M3FD8NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M109NW3ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-RELEASE-p5 FreeBSD 7.0-RELEASE-p5 #0: Wed Oct  1 10:10:12 UTC 2008 i386
Fingerprint FreeBSD 7.0-RELEASE-p5
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=100-10A%TI=RD%II=RI%TS=21)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=70A1|ABFB|DFB7|ED9D|F0AA%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-STABLE FreeBSD 7.0-STABLE #0: Wed Apr  2 14:42:45 MSD 2008 amd64
Fingerprint FreeBSD 7.0-STABLE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=DC-10A%GCD=1-6|12|24|36|48|5A%ISR=108-112%TI=I%TS=20|21)
OPS(O1=M5B4NW3NNT11SLL%O2=M578NW3NNT11SLL%O3=M280NW3NNT11%O4=M3FD8NW3NNT11SLL%O5=M218NW3NNT11SLL%O6=M109NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M109NW3NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.0-STABLE FreeBSD 7.0-STABLE #4: Wed Apr 30 20:04:35 MSD 2008 amd64
Fingerprint FreeBSD 7.0-STABLE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=FA-10C%GCD=1-6%ISR=106-110%TS=21|22)
OPS(O1=M5B4NW3NNT11SLL%O2=M578NW3NNT11SLL%O3=M280NW3NNT11%O4=M5B4NW3NNT11SLL%O5=M218NW3NNT11SLL%O6=M109NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=8D-97%TG=FF%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=8D-97%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=8D-97%TG=FF%W=FFFF%S=O%A=S+%F=AS%O=M109NW3NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=8D-97%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=8D-97%TG=FF%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=8D-97%TG=FF%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=8D-97%TG=FF%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=8D-97%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=8D-97%TG=FF%CD=S)

# FreeBSD 7.0-STABLE FreeBSD 7.0-STABLE #6: Thu Aug  7 05:11:38 EDT 2008   i386
Fingerprint FreeBSD 7.0-STABLE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=109-113%TS=22)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M3FD8NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# 7.0-STABLE FreeBSD 7.0-STABLE #2: Tue Mar 11 07:28:04 CDT 2008   amd64
Fingerprint FreeBSD 7.0-STABLE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=102-10C%GCD=1-6%ISR=104-10E%TS=21)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLN%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M109NW3ST11%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.1-PRERELEASE FreeBSD 7.1-PRERELEASE #42: Thu Sep 11 09:07:25 EDT 2008 i386
Fingerprint FreeBSD 7.1-PRERELEASE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=F6-10C%GCD=1-6%ISR=FE-112%TI=I%II=I%SS=S%TS=21|22)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.1-PRERELEASE FreeBSD 7.1-PRERELEASE #8: Tue Nov 18 20:28:43 MST 2008 i386
# FreeBSD 7.2-STABLE FreeBSD 7.2-STABLE #6: Wed Jun 10 17:45:09 CDT 2009 amd64
Fingerprint FreeBSD 7.1-PRERELEASE 7.2-STABLE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=102-10C%GCD=1-6%ISR=106-110%TI=I%TS=21|22)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# 7.1-RELEASE FreeBSD 7.1-RELEASE #0: Thu Jan  1 14:37:25 UTC 2009 i386
Fingerprint FreeBSD 7.1-RELEASE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=F5-10D%GCD=1-6%ISR=105-10F%TI=I%II=I%SS=S%TS=22)
OPS(O1=M5ACNW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5ACNW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=0-FFFF%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.1-RELEASE FreeBSD 7.1-RELEASE #0: Thu Jan  1 14:37:25 UTC 2009 i386
Fingerprint FreeBSD 7.1-RELEASE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=EF-F9%GCD=2|4|6|8|A%ISR=105-10F%TI=I%II=I%SS=O|S%TS=21)
OPS(O1=M538NW3ST11%O2=M538NW3ST11%O3=M280NW3NNT11%O4=M538NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M538NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW3ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.1-RELEASE
Fingerprint FreeBSD 7.1-RELEASE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=EE-108%GCD=1-6%ISR=F3-10F%TI=I%II=I%SS=S%TS=21|22)
OPS(O1=M58ANW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M58ANW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M58ANW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW3ST11%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.1-RELEASE FreeBSD 7.1-RELEASE #0: Thu Jan  1 14:37:25 UTC 2009 i386
Fingerprint FreeBSD 7.1-RELEASE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=FD-107%GCD=1-6%ISR=105-111%TI=I%CI=I%II=I%SS=S%TS=21|22)
OPS(O1=M5ACNW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5ACNW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5ACNW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N|Y%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M109NW3ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 8.0-BETA2 [...] GENERIC sparc64
# FreeBSD 7.2-STABLE FreeBSD 7.2-STABLE #8: Sat May 30 17:26:18 MSD 2009 i386
# FreeBSD 7.1-RELEASE FreeBSD 7.1-RELEASE #0: Thu Jan  1 14:37:25 UTC 2009 i386
# FreeBSD 8.0 RELEASE i386
Fingerprint FreeBSD 7.1-RELEASE - 8.0-RELEASE
Class FreeBSD | FreeBSD | 7.X | general purpose
Class FreeBSD | FreeBSD | 8.X | general purpose
SEQ(SP=F5-109%GCD=2|4|6|8|A%ISR=FF-113%TI=I%CI=I%II=I%SS=S%TS=20|21|22)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.2-RELEASE-p2 FreeBSD 7.2-RELEASE-p2 #0: Thu Jul 23 20:31:34 EDT 2009 i386
Fingerprint FreeBSD 7.2-RELEASE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=FD-109%GCD=1-6%ISR=FE-112%TI=I%II=I%SS=S%TS=21|22)
OPS(O1=M5A0NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5A0NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3A-44%TG=40%W=FFFF%O=M5A0NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3A-44%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3A-44%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW3ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3A-44%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.2-RELEASE FreeBSD 7.2-RELEASE #1: Mon Sep 21 10:32:35 CEST 2009 i386
Fingerprint FreeBSD 7.2-RELEASE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=FB-10B%GCD=2|4|6|8|A%ISR=100-10E%TI=I%II=I%SS=S%TS=21|22)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW3ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.2-RELEASE-p4 FreeBSD 7.2-RELEASE-p4 #0: Tue Nov 10 15:34:04 CST 2009 i386
# FreeBSD freenas.local 7.2-RELEASE-p6 FreeBSD 7.2-RELEASE-p6 #0: Tue Jan  5 23:20:02 UTC 2010 root@vmbsd72i386:/usr/obj/freenas/usr/src/sys/FREENAS-i386 i386
Fingerprint FreeBSD 7.2-RELEASE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=106-110%TI=RD%II=RI%TS=21|22)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW3ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.2-RELEASE-p4 FreeBSD 7.2-RELEASE-p4 #0: Mon Oct  5 22:37:41 UTC 2009 i386
# FreeBSD 8.0-RELEASE-p1 FreeBSD 8.0-RELEASE-p1 #0: Tue Jan  5 09:17:26 EST 2010 sullrich@FreeBSD_8.0_pfSense_2.0-snaps.pfsense.org:/usr/obj.pfSense/usr/pfSensesrc/src/sys/pfSense.8  i386
Fingerprint FreeBSD 7.2-RELEASE - 8.0-RELEASE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=FD-107%GCD=2|4|6|8|A%ISR=FA-112%TI=I%TS=21)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=1-FFFF%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.2-STABLE FreeBSD 7.2-STABLE #0: Tue Jun  9 14:38:09 MSD 2009 amd64
Fingerprint FreeBSD 7.2-STABLE
Class FreeBSD | FreeBSD | 7.X | general purpose
SEQ(SP=FE-10C%GCD=2|4|6|8|A%ISR=106-110%TI=I%TS=21|22)
OPS(O1=M55CNW3ST11%O2=M55CNW3ST11%O3=M280NW3NNT11%O4=M55CNW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M55CNW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW3ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.2-RELEASE-p1 FreeBSD 7.2-RELEASE-p1 #0: Fri Jun 19 20:56:48 UTC 2009 i386, Freenas embedded 0.7RC1 Sardaukar (revision 4735)
# FreeNAS 0.7, FreeBSD 7.2-RELEASE (revision 199506)
# Freenas server  Version 0.7.1 Shere (revision 4967) FreeBSD 7.2-RELEASE-p5 (revision 199506)
Fingerprint FreeNAS 0.7 (FreeBSD 7.2-RELEASE)
Class FreeBSD | FreeBSD | 7.X | storage-misc
SEQ(SP=F5-10B%GCD=1-6%ISR=104-110%TI=I%II=I%SS=S%TS=20|21|22)
OPS(O1=M5B4NW6ST11%O2=M578NW6ST11%O3=M280NW6NNT11%O4=M5B4NW6ST11%O5=M218NW6ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW6SLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW6ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD freenas.localdomain 7.2-RELEASE-p4 FreeBSD 7.2-RELEASE-p4 #0: Fri Oct 16 16:45:05 UTC 2009     root@vmbsd72i386:/usr/obj/freenas/usr/src/sys/FREENAS-i386  i386
Fingerprint FreeNAS 0.7 (FreeBSD 7.2-RELEASE)
Class FreeBSD | FreeBSD | 7.X | storage-misc
SEQ(SP=EE-10A%GCD=2|4|6|8|A%ISR=104-112%CI=I%II=I%TS=21|22)
OPS(O1=M5B4NW6ST11%O2=M578NW6ST11%O3=M280NW6NNT11%O4=M5B4NW6ST11%O5=M218NW6ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW6SLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW6ST11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.2-RELEASE-p4 FreeBSD 7.2-RELEASE-p4 #0: Fri Oct 16 16:45:05 UTC 2009     root@vmbsd72i386:/usr/obj/freenas/usr/src/sys/FREENAS-i386  i386, FreeNAS 0.7 Khasadar (revision 4919)
Fingerprint FreeNAS 0.7 (FreeBSD 7.2-RELEASE-p4)
Class FreeBSD | FreeBSD | 7.X | storage-misc
SEQ(SP=FF-109%GCD=2|4|6|8|A%ISR=101-10B%TI=I%CI=I%II=I%SS=S%TS=21)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M109NW3ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 7.3-RELEASE-p3 FreeBSD 7.3-RELEASE-p3 #0: Sat Oct  9 21:30:38 CEST 2010 i386
Fingerprint FreeNAS 0.7.2 (FreeBSD 7.3-RELEASE)
Class FreeBSD | FreeBSD | 7.X | storage-misc
SEQ(SP=F5-10B%GCD=1-6%ISR=104-110%TI=I%II=I%SS=S%TS=20|21|22)
OPS(O1=M5B4NW7ST11%O2=M578NW7ST11%O3=M280NW7NNT11%O4=M5B4NW7ST11%O5=M218NW7ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW7SLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW7ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 8.0-BETA2 FreeBSD 8.0-BETA2 #7: Wed Jul 29 01:05:27 PDT 2009 amd64
# FreeBSD 8.0-RC2 FreeBSD 8.0-RC2 #1: Wed Nov  4 20:01:07 GMT 2009 amd64
# FreeBSD 8.0-RELEASE FreeBSD 8.0-RELEASE #1: Sun Dec  6 22:27:00 CET 2009 i386
# FreeBSD 8.0-STABLE FreeBSD 8.0-STABLE #10: Tue Dec 22 13:04:25 CET 2009 i386
Fingerprint FreeBSD 8.0-BETA2 - 8.0-RELEASE
Class FreeBSD | FreeBSD | 8.X | general purpose
SEQ(SP=F9-10B%GCD=1-6%ISR=102-110%TI=I%CI=I%TS=20|21|22)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M3FD8NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW3ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 8.0-CURRENT FreeBSD 8.0-CURRENT #0: Fri Feb  6 15:13:43 UTC 2009 i386
Fingerprint FreeBSD 8.0-CURRENT
Class FreeBSD | FreeBSD | 8.X | general purpose
SEQ(SP=FC-106%GCD=1-6%ISR=107-111%TI=RD%TS=21)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=O|S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=O|S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=1515|6303|7911|BB65|E0DC%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# 8.0-RC1-p1 FreeBSD 8.0-RC1-p1 #0: Sat Oct  3 23:39:38 UTC 2009 amd64
Fingerprint FreeBSD 8.0-RC1-p1
Class FreeBSD | FreeBSD | 8.X | general purpose
SEQ(SP=FD-10B%GCD=2|4|6|8|A%ISR=106-110%TS=21|22)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW3ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=N)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 8.0-RELEASE FreeBSD 8.0-RELEASE #0: Sat Nov 21 15:48:17 UTC 2009 i386
Fingerprint FreeBSD 8.0-RELEASE
Class FreeBSD | FreeBSD | 8.X | general purpose
SEQ(SP=FF-109%GCD=2|4|6|8|A%ISR=10A-114%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4SLL%O2=M578SLL%O3=M280%O4=M5B4SLL%O5=M218SLL%O6=M109SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 8.0-RELEASE-p4 FreeBSD 8.0-RELEASE-p4 #0: Mon Jul 12 20:55:11 UTC 2010 amd64
Fingerprint FreeBSD 8.0-RELEASE
Class FreeBSD | FreeBSD | 8.X | general purpose
SEQ(SP=FD-107%GCD=2|4|6|8|A%ISR=101-10D%TI=I%CI=I%TS=21|22)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M109NW3ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 8.0-RELEASE-p3 FreeBSD 8.0-RELEASE-p3 #0: Tue May 25 20:54:11 UTC 2010 amd64
Fingerprint FreeBSD 8.0-RELEASE
Class FreeBSD | FreeBSD | 8.X | general purpose
SEQ(SP=102-10C%GCD=1-6%ISR=100-10C%CI=I%II=I%TS=21|22)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 8.0-STABLE FreeBSD 8.0-STABLE #0: Sun Dec  6 00:30:42 EET 2009 i386
Fingerprint FreeBSD 8.0-STABLE
Class FreeBSD | FreeBSD | 8.X | general purpose
SEQ(SP=F5-10D%GCD=1-6%ISR=105-10F%TI=I%II=I%SS=S%TS=22)
OPS(O1=M5A0NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5A0NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5A0NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=0-FFFF%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 8.0-STABLE
Fingerprint FreeBSD 8.0-STABLE
Class FreeBSD | FreeBSD | 8.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=106-110%TI=I%CI=I%II=I%SS=S%TS=21)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M2300NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW3ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 8.0-STABLE
Fingerprint FreeBSD 8.0-STABLE
Class FreeBSD | FreeBSD | 8.X | general purpose
SEQ(SP=101-10B%GCD=2|4|6|8|A%ISR=106-110%TI=I%CI=I%II=I%SS=S%TS=21)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# FreeBSD 8.0-STABLE FreeBSD 8.0-STABLE
Fingerprint FreeBSD 8.0-STABLE
Class FreeBSD | FreeBSD | 8.X | general purpose
SEQ(SP=FC-108%GCD=1-6%ISR=FE-110%II=I%TS=21|22)
OPS(O1=M58ANW6ST11%O2=M578NW6ST11%O3=M280NW6NNT11%O4=M58ANW6ST11%O5=M218NW6ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=61-69%TG=80%W=FFFF%O=M58ANW6SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=61-69%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=61-69%TG=80%W=FFFF%S=O%A=S+%F=AS%O=M109NW6ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=61-69%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=61-69%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=61-69%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=61-69%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=61-69%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=61-69%TG=80%CD=S)

# FreeBSD 8.1-STABLE #1 r19M: Wed Aug  4 20:51:38 IRKST 2010 amd64
Fingerprint FreeBSD 8.1-STABLE
Class FreeBSD | FreeBSD | 8.X | general purpose
SEQ(SP=103-10D%GCD=2|4|6|8|A%ISR=104-10E%TI=I%CI=I|RI%II=I%SS=S%TS=21|22)
OPS(O1=M5B4NW3ST11%O2=M578NW3ST11%O3=M280NW3NNT11%O4=M5B4NW3ST11%O5=M218NW3ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0|G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Freecom Network Drive
Fingerprint Freecom Network Drive NAS device
Class Freecom | embedded || storage-misc
SEQ(SP=0-5B%GCD=1-6|120|240|360|480|5A0%ISR=56-60%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=1B-25%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=1B-25%TG=20%CD=S)

# Windows XP Embedded Edition on Fuji Drypix (Medical Imager)
Fingerprint Fuji DryPix medical imager (Microsoft Windows XP Embedded)
Class Fuji | Windows | XP | specialized
SEQ(SP=7B-85%GCD=1-6%ISR=95-9F%TI=I%TS=0)
OPS(O1=NNT11|M5B4NW0NNT00NNS%O2=NNT11|M5B4NW0NNT00NNS%O3=NNT11|M5B4NW0NNT00%O4=NNT11|M5B4NW0NNT00NNS%O5=NNT11|M5B4NW0NNT00NNS%O6=)
WIN(W1=FAF0%W2=FAF0%W3=FAF0%W4=FAF0%W5=FAF0%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Fujian Ruijie Star-S2800
Fingerprint Fujian Ruijie Star-S2800 switch
Class Fujian Ruijie | embedded || switch
SEQ(SP=0-5%GCD=388|710|A98|E20|11A8%ISR=63-6D%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FB-105%TG=FF%W=2000%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FB-105%TG=FF%S=O|Z%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FB-105%TG=FF%W=2000%S=O|Z%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FB-105%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C-46%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3C-46%TG=40%CD=Z)

# BS2000/OSD (mainframe OS made by Fujitsu Siemens, running on /390 hardware)
# BS2000/OSD (mainframe OS made by Fujitsu Siemens, running on SPARC hardware)
Fingerprint Fujitsu Siemens BS2000/OSD
Class Fujitsu Siemens | BS2000/OSD || general purpose
SEQ(SP=13-69%GCD=1-6%ISR=7A-84%TI=I%II=I%SS=S%TS=U)
OPS(O1=M58CNNSNW5%O2=M58CNNSNW5%O3=M58CNW5%O4=M58CNNSNW5%O5=M58CNNSNW5%O6=M58CNNS)
WIN(W1=111C%W2=111C%W3=B18%W4=B18%W5=B18%W6=B18)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=111C%O=M58CNNSNW5%CC=Y%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=1B-25%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=1B-25%TG=20%CD=S)

# Fujitsu Siemens, integrated Remote Control Board on a FSC RX300.
Fingerprint Fujitsu Siemens PRIMERGY RX300 S4 server
Class Fujitsu Siemens | embedded || general purpose
SEQ(SP=C-16%GCD=FA7F|1F4FE|2EF7D|3E9FC|4E47B%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=MF8%O2=MF8%O3=MF8%O4=MF8%O5=MF8%O6=MF8)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2000%O=MF8%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=19-23%TG=20%CD=S)

# Fujitsu Siemens PRIMERGY Remote Manager; Chassis Type: RX100S4; Bios Version: 4.06 Rev. 1.00.2532; System Type: PRIMERGY RX100 S4;
Fingerprint Fujitsu Siemens PRIMERGY RX100 S4 remote manager
Class Fujitsu Siemens | embedded || specialized
SEQ(SP=8A-94%GCD=1-6%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=800%W2=800%W3=800%W4=800%W5=800%W6=800)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=800%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=FA-104%TG=FF%CD=Z)

# Fujitsu Siemens "PRIMERGY TX300 S3" Server Remote Management Board. Firmware Version 1.52A.
Fingerprint Fujitsu Siemens PRIMERGY TX300 SS remote manager
Class Fujitsu Siemens | embedded || specialized
SEQ(SP=8B-95%GCD=1-6%ISR=99-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=Z)

# ReliantUNIX-N aka. SINIX-N running on RM400 machine (SVR4 derivative made by Fujitsu Siemens, running on MIPS R4000 hardware)
Fingerprint Fujitsu Siemens ReliantUNIX-N (SINIX-N) on RM400
Class Fujitsu Siemens | ReliantUNIX || general purpose
SEQ(SP=91-9B%GCD=1-6%ISR=99-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=7FFF%W2=7FFF%W3=7FFF%W4=7FFF%W5=7FFF%W6=7FFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=7FFF%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=7FFF%S=O%A=O%F=AS%O=M5B4NW0%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=7FFF%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# FujitsuSiemens PocketLoox 750, Windows Mobile 5
Fingerprint Fujitsu Siemens Pocket LOOX 750 GPS device (Windows Mobile 5)
Class Fujitsu Siemens | Windows | PocketPC/CE | PDA
SEQ(SP=72-7C%GCD=1-6%ISR=92-9C%TI=I%II=I%SS=S%TS=0)
OPS(O1=M1F4ANW0NNT00NNS%O2=M1F4ANW0NNT00NNS%O3=M1F4ANW0NNT00%O4=M1F4ANW0NNT00NNS%O5=M1F4ANW0NNT00NNS%O6=M1F4ANNT00NNS)
WIN(W1=832C%W2=8340%W3=8200%W4=81D0%W5=81D0%W6=805C)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=832C%O=M1F4ANW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=7B-85%TG=80%W=805C%S=O%A=S+%F=AS%O=M1F4ANW0NNT00NNS%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=B0%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=Z)

# funkwerk artem WI3040
Fingerprint Funkwerk Artem WI3040 WAP
Class Funkwerk | embedded || WAP
SEQ(SP=63-6D%GCD=1-6%ISR=8A-94%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=6F-79%TG=80%W=4000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=6F-79%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=6F-79%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=6F-79%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=6F-79%TG=80%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=6F-79%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=6F-79%TG=80%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=6F-79%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=39-43%TG=40%IPL=38%UN=5E09%RIPL=G%RID=2%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=S%T=6F-79%TG=80%CD=S)

# Galaxy Metal Gear HDD Enclosure, Model # 3507LR-SA USB2.0 + Ethernet (LAN) NAS
Fingerprint GalaxyMetalGear 3507LR-SA NAS device
Class GalaxyMetalGear | embedded || storage-misc
SEQ(SP=0-6E%GCD=1-6|1710|1714|2E20|2E28|4530|453C|5C40|5C50|7350|7364%ISR=7A-84%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=8000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=1B-25%TG=20%W=8000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=1B-25%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=N%T=1B-25%TG=20%CD=S)

# Linux IB-NAS4220-B 2.6.15 #126 Tue Dec 9 16:13:08 CST 2008 armv4l unknown, IcyBox NAS, running BusyBox.
# Galaxy Metal Gear 4500MGB Quad Bay Pro NAS storage device
#  Linux TAURUS-LAN 2.6.15 #160 Thu May 29 14:11:48 CST 2008 armv4l unknown (MRT Dual GigaNAS, Storlink SL3516)
Fingerprint NAS device (Linux 2.6.15): GalaxyMetalGear 4500MGB, Icy Box IB-NAS4220-B, or MRT Dual GigaNAS
Class GalaxyMetalGear | Linux | 2.6.X | storage-misc
Class Icy Box | Linux | 2.6.X | storage-misc
Class MRT | Linux | 2.6.X | storage-misc
SEQ(SP=C2-D0%GCD=1-6%ISR=C8-D4%TI=Z%II=I%TS=7)
OPS(O1=M5A0ST11NW2%O2=M5A0ST11NW2%O3=M5A0NNT11NW2%O4=M5A0ST11NW2%O5=M5A0ST11NW2%O6=M5A0ST11)
WIN(W1=1650%W2=1650%W3=1650%W4=1650%W5=1650%W6=1650)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1680%O=M5A0NNSNW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1650%S=O%A=S+%F=AS%O=M5A0ST11NW2%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Siemens SE515 DSL Router
# Gemtek systems model: P360 Wi-Fi "Hot-Spot in a Box"
# Comtrend 96348GW-11, 1.0.37-5.17, A101-221JAZ-C01_R02.A2pB017l.d15h
Fingerprint Gemtek P360 WAP or Siemens Gigaset SE515dsl wireless broadband router
Class Gemtek | embedded || WAP
Class Siemens | embedded || WAP
SEQ(SP=BB-D3%GCD=1-6%ISR=CB-D5%TI=Z%CI=Z%II=I%TS=8)
OPS(R=N)
WIN(R=N)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4NNT11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Generex SNMP/Web Adapter CS121 L Budget
Fingerprint Generex CS121 L BUDGET SNMP adapter
Class Generex | embedded || power-device
SEQ(SP=0-15%GCD=F4240|1E8480|2DC6C0|3D0900|4C4B40%ISR=B6-C0%TI=BI%II=RI%SS=O|S%TS=U)
OPS(O1=M5B4NNNN%O2=M578NNNN%O3=M218NNNN%O4=M218NNNN%O5=M218NNNN%O6=M128NNNN)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=1000%O=M5B4NNNN%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=Z)

# Gennet router with a linux 2.6.11 kernel. http://broadband.gennetsa.com/oxygen_router.html
Fingerprint Gennet OxyGEN wireless ADSL router (Linux 2.6.11)
Class Gennet | Linux | 2.6.X | WAP
SEQ(SP=C9-D3%GCD=1-6%ISR=CB-D5%TI=Z%CI=I%II=I%TS=9)
OPS(O1=M5B4ST11NW1%O2=M5B4ST11NW1%O3=M5B4NNT11NW1%O4=M5B4ST11NW1%O5=M5B4ST11NW1%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# "IPM DataCom Sppedtouch ADSL Modem" (really a Solwise SAR110 with firmware sar1130-110-260304)/
# huawei mt880 smartax
# Router Globespan Virata GS8100 (IPM DataCom SpeedWeb Ethernet)
Fingerprint GlobespanVirata GS8100, Huawei MT880, or Solwise SAR 100 ADSL modem
Class GlobespanVirata | embedded || broadband router
Class Huawei | embedded || broadband router
Class Solwise | embedded || broadband router
SEQ(SP=FA-10C%GCD=1-6%ISR=100-112%TI=I%II=I%SS=S%TS=U)
OPS(O1=M58C%O2=M58C%O3=M58C%O4=M58C%O5=M58C%O6=M58C)
WIN(W1=3E80%W2=3E80%W3=3E80%W4=3E80%W5=3E80%W6=3E80)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3E80%O=M58C%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=N)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# GNU hurd 0.3 GNU-Mach 1.3.99/Hurd-0.3 i686-AT386 GNU
Fingerprint GNU Hurd 0.3
Class GNU | Hurd || general purpose
SEQ(SP=0-27%GCD=2710|4E20|7530|9C40|C350|1ADB0|35B60|50910|6B6C0|86470%ISR=9A-A4%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4ST11NW0%O2=M578ST11NW0%O3=M280NNT11NW0%O4=M218ST11NW0%O5=M218ST11NW0%O6=M109ST11)
WIN(W1=7D78%W2=7DC8%W3=7F80%W4=7FB8%W5=7FB8%W6=7F53)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=7D78%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=7F53%S=O%A=S+%F=AS%O=M109ST11NW0%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# GNU 0.3 GNU-Mach 1.3.99/Hurd-0.3 i686-AT386 GNU (Debian)
Fingerprint GNU Hurd 0.3
Class GNU | Hurd || general purpose
SEQ(CI=I%II=I)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=Z%A=S+%F=AR%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Google Mini Search Appliance version 5 or above.
Fingerprint Google Mini search appliance
Class Google | embedded || specialized
SEQ(SP=C3-CD%GCD=1-6%ISR=C4-CE%TI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW9%O2=M5B4ST11NW9%O3=M5B4NNT11NW9%O4=M5B4ST11NW9%O5=M5B4ST11NW9%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW9%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Grandstream Handytone HT-488
Fingerprint Grandstream HandyTone HT-488 analog VoIP adapter
Class Grandstream | embedded || VoIP adapter
SEQ(SP=0-5%GCD=0%ISR=0-5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5A6%O2=M5A6%O3=M5A6%O4=M5A6%O5=M5A6%O6=M5A6)
WIN(W1=5A6%W2=578%W3=280%W4=280%W5=218%W6=109)
ECN(R=Y%DF=Y%T=FE%TG=FF%W=5A6%O=M5A6%CC=N%Q=U)
T1(R=Y%DF=Y%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=FE%TG=FF%W=80%S=A%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=FE%TG=FF%W=109%S=O%A=S+%F=AS%O=M5A6%RD=0%Q=)
T4(R=Y%DF=Y%T=FE%TG=FF%W=400%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FE%TG=FF%W=7A69%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FE%TG=FF%W=8000%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FE%TG=FF%W=FFFF%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=F5-FF%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=F5-FF%TG=FF%CD=Z)

# Grandstream BudgeTone-100 VoIP phone
Fingerprint Grandstream BudgeTone 100 VoIP phone
Class Grandstream | embedded || VoIP phone
SEQ(SP=2B-35%GCD=1-6%ISR=3D-47%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5A6%O2=M5A6%O3=M5A6%O4=M5A6%O5=M5A6%O6=M5A6)
WIN(W1=5A6%W2=578%W3=280%W4=280%W5=218%W6=109)
ECN(R=Y%DF=Y%T=FE%TG=FF%W=5A6%O=M5A6%CC=N%Q=U)
T1(R=Y%DF=Y%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=FE%TG=FF%W=80%S=A%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=FE%TG=FF%W=109%S=O%A=S+%F=AS%O=M5A6%RD=0%Q=)
T4(R=Y%DF=Y%T=FE%TG=FF%W=400%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FE%TG=FF%W=7A69%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FE%TG=FF%W=8000%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FE%TG=FF%W=FFFF%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=F5-FF%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=F5-FF%TG=FF%CD=Z)

# Grandstream Budge Tone-100
Fingerprint Grandstream BudgeTone 100 VoIP phone
Class Grandstream | embedded || VoIP phone
SEQ(SP=F-19%GCD=1-6%ISR=24-2E%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5A6%O2=M5A6%O3=M5A6%O4=M5A6%O5=M5A6%O6=M5A6)
WIN(W1=5A6%W2=578%W3=280%W4=280%W5=218%W6=109)
ECN(R=Y%DF=Y%T=FE%TG=FF%W=5A6%O=M5A6%CC=N%Q=U)
T1(R=Y%DF=Y%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=FE%TG=FF%W=80%S=A%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=FE%TG=FF%W=109%S=O%A=S+%F=AS%O=M5A6%RD=0%Q=)
T4(R=Y%DF=Y%T=FE%TG=FF%W=400%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FE%TG=FF%W=7A69%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FE%TG=FF%W=8000%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FE%TG=FF%W=FFFF%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=F5-FF%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=F5-FF%TG=FF%CD=Z)

# Grandstream GXP2000, Program-- 1.1.4.18    Bootloader-- 1.1.4.6
Fingerprint Grandstream GXP2000 VoIP phone
Class Grandstream | embedded || VoIP phone
SEQ(SP=4A-62%GCD=1-6%ISR=88-92%TI=I%TS=U)
OPS(O1=M584%O2=M584%O3=M584%O4=M584%O5=M584%O6=M584)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2000%O=M584%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=O%A=S+%F=AS%O=M584%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A+%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=1B-25|3B-45%TG=20|40%CD=S)

# Grandstream voip phone 2020
Fingerprint Grandstream GXP2020 VoIP phone
Class Grandstream | embedded || VoIP phone
SEQ(SP=2C-8C%GCD=1-6%ISR=AB-B5%TI=I%II=RI%SS=O%TS=U)
OPS(O1=M5AC%O2=M5AC%O3=M5AC%O4=M5AC%O5=M5AC%O6=M5AC)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2000%O=M5AC%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A+%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(R=N)
IE(DFI=S%T=1B-25|3B-45%TG=20|40%CD=S)

# Greenhills RTOS
Fingerprint Green Hills RTOS
Class Green Hills | RTOS || specialized
SEQ(SP=0-5%GCD=FA01|1F402|2EE03|3E804|4E205%ISR=95-9F%TI=BI%II=BI%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M578NW0%O3=M280NW0%O4=M218NW0%O5=M218NW0%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=Z)

# Hawking Technologies PN7127P 10/100 Print Server
Fingerprint Hawking PN7127P print server
Class Hawking | embedded || print server
SEQ(SP=0-5%GCD=60000|C0000|120000|180000|1E0000%ISR=AA-B4%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=B68%W2=B68%W3=B68%W4=B68%W5=B68%W6=B68)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=B68%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=1B-25%TG=20%W=B68%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=1B-25%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=1B-25%TG=20%CD=S)

# hawking printserver model PS12U Firmware Version: 6.09.17H (2003/04/18 16:55:07)
# TRENDnet TE100-P2U1P print server
# Repotec RP-1805B-V2 print server, firmware version 3.41.10
Fingerprint Hawking PS12U, Repotech RP-1805B-V2, or TRENDnet TE100 P2U1P print server
Class Hawking | embedded || print server
Class Repotech | embedded || print server
Class TRENDnet | embedded || print server
SEQ(SP=0-5%GCD=64000|C8000|12C000|190000|1F4000%ISR=AB-B5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=B68%W2=B68%W3=B68%W4=B68%W5=B68%W6=B68)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=B68%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=1B-25%TG=20%W=B68%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=1B-25%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=1B-25%TG=20%CD=S)

# HID ES400 Solo (Probably Linux 2.4 --Ed.)
Fingerprint HID EdgePlus Solo ES400 firewall
Class HID | embedded || firewall
SEQ(SP=C3-CD%GCD=1-6%ISR=CA-D4%TI=Z%CI=Z%TS=9)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Hioki 8855 Memory Hicorder Digital Oscilloscope, The software version is 2.53
Fingerprint Hioki MEMORY HiCORDER 8855 digital oscilloscope
Class Hioki | embedded || specialized
SEQ(SP=0-5%GCD=64|C8|12C|190|1F4%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4470%W2=4470%W3=4470%W4=4470%W5=4470%W6=4470)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Railswitch Release L2E-03\.0\.01
Fingerprint Hirschmann L2E Rail switch
Class Hirschmann | embedded || switch
SEQ(SP=7E-88%GCD=1-6%ISR=96-A0%TI=I%CI=I%TS=3)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(R=N)

# RS2 16M 2MM SC, SW Version 9.03 May 25 2005 11:15:10
Fingerprint Hirschmann RS2-16M 2MM SC switch
Class Hirschmann | embedded || switch
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=S)

# Hotway LAN-Drive, HDC-U2LA, RDC NAS-BASIC45a
# Vantec NexStar LX NAS enclosure
# RDC Semiconductor, External LAN disk
Fingerprint Hotway HDC-U2LA or Vantec NexStar LX NAS device
Class Hotway | embedded || storage-misc
SEQ(SP=0-40%GCD=1-6|132A|2654|397E|4CA8|5FD2%ISR=78-A6%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=8000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=1B-25%TG=20%W=8000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=1B-25%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=1B-25%TG=20%CD=S)

# HP ProCurve Switch 1810G-8 Model J9449A
# HP ProCurve 1810G-24 Switch with Firmware P.1.6
# HP ProCurve 1810G-24 Switch with firmware P.1.17
# HP ProCurve 1810G - 24 GE, P.1.17, eCos-2.0
# Netgear GS108v2 Semi Managed Switch
Fingerprint HP ProCurve 1810G or Netgear GS108v2 switch (eCos 2.0)
Class HP | eCos | 2.X | switch
Class Netgear | eCos | 2.X | switch
SEQ(SP=F5-10B%GCD=1-6%ISR=FB-10C%TI=I%CI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=10F8%W2=1044%W3=112C%W4=1194%W5=1060%W6=10CD)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=111C%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=10CD%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP JetDirect J3258B version F.08.20, ROM version F.08.08, EEPROM F.08.20
# HP JETDIRECT J3113A FIRMWARE G.08.49 DATE MANUFACTURED 09/1999
Fingerprint HP 170X print server or Inkjet 3000 printer
Class HP | embedded || print server
Class HP | embedded || printer
SEQ(SP=0-5%GCD=1-6%ISR=15-1F%TI=I%II=I%SS=S%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=Z)

# HP USB G Wireless Print Server model 2101nw
Fingerprint HP 2101nw wireless print server
Class HP | embedded || print server
SEQ(SP=0-8B%GCD=1-6%ISR=41-61%TI=I%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=2000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=2000%S=A+%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=2000%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=2000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=2000%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(R=N)

# HP 4200 PSA (Print Server Appliance) model J4117A
Fingerprint HP 4200 PSA (Print Server Appliance) model J4117A
Class HP | embedded || print server
SEQ(SP=BE-C8%GCD=1-6%ISR=C2-CC%TI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# HP Jetdirect 175x Fast Ethernet Print Server (J6035G) with a HP LaserJet 1012 attached.
# HP JetDirect 610n (J4169A) Fast Ethernet Print Server
Fingerprint HP JetDirect 175x (J6035G) or 610n (J4169A) print server
Class HP | embedded || print server
SEQ(SP=92-9C%GCD=1-6%ISR=9A-A4%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=16D0%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=16D0%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=16D0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP Digital Sender (Scan to Email Device) Model 9100C (Older) running a JetDirect Card as Network Interface
# HP Jetdirect 175X, J6035G, Firmware Version:    M.25.54
Fingerprint HP JetDirect 175x print server (J6035G) or 9100c Digital Sender multifunction printer
Class HP | embedded || print server
Class HP | embedded || printer
SEQ(SP=96-A0%GCD=1-6%ISR=9B-A5%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O|S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP JetDirect - J3110A - Firmware versioin G.08.40
# Printserver is an HP 2591A.
Fingerprint HP JetDirect 2591A print server
Class HP | embedded || print server
SEQ(SP=0%GCD=1-6%ISR=16-20%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3C%TG=40%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=16D0%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=Z)

# JetDirect 635n print server Firmware version TJ6-TAJM_2.0.0.3
# JetDirect 635n print server Model Nr.: J7961G Firmware version V.38.05
# It's an IPANEMA device.
Fingerprint HP JetDirect 635n print server
Class HP | embedded || print server
SEQ(SP=FA-10A%GCD=1-6%ISR=104-112%TI=I%II=I%SS=S%TS=6)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N|Y%T=3B-45%TG=40%W=5B4%S=O%A=O|S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP Jetdirect that resides in a HP Laserjet 2200dn.
Fingerprint HP LaserJet 2200DN printer
Class HP | embedded || print server
SEQ(SP=77-85%GCD=1-6%ISR=97-A1%TI=I%II=I%SS=S)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HPColorLaserjet Printer 3550
# HP LaserJet 1320NW (network+wireless network interface) over its wireless interface.
# HP LaserJet 2550N Color LaserJet
# HP LaserJet1300n
Fingerprint HP 1320nw, 1300n, or 3550 Color LaserJet printer
Class HP | embedded || printer
SEQ(SP=94-9E%GCD=1-6%ISR=9B-A5%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=16D0%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=16D0%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=16D0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP 9100C Digital Sender (J3113A)
Fingerprint HP 9100c Digital Sender multifunction printer (J3113A)
Class HP | embedded || printer
SEQ(R=N)
OPS(O1=M5B4%O2=M5B4%O3=|M5B4%O4=%O5=%O6=)
WIN(W1=800%W2=800%W3=0|800%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=3C%TG=40%W=0|800%O=|M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=Z%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3C%TG=40%CD=S)

# HP Color Laserjet 3600, J7973E, Firmware Version: V.30.31.BA
Fingerprint HP Color LaserJet 3600 (J7973E)
Class HP | embedded || printer
SEQ(SP=7A-B0%GCD=1-6|B|16|21|2C|37%ISR=9E-A8%TI=I%II=I%SS=S%TS=1|2)
OPS(O1=M558NW0NNT11%O2=M558NW0NNT11%O3=M558NW0NNT11%O4=M558NW0NNT11%O5=M558NW0NNT11%O6=M558NNT11)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=16D0%O=M558NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=16D0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# hp color LaserJet 5550 with Model Number: J7934A
Fingerprint HP Color LaserJet 5550 (J7934A)
Class HP | embedded || printer
SEQ(SP=94-9E%GCD=1-6%ISR=9A-A4%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2DA0%W2=2DA0%W3=2DA0%W4=2DA0%W5=2DA0%W6=2DA0)
ECN(R=Y%DF=N%T=41%TG=40%W=2DA0%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=41%TG=40%W=2DA0%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=41%TG=40%W=2DA0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=41%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=41%TG=40%CD=S)

# HP Color Laserjet 1312NFI (all in one printer)
Fingerprint HP Color LaserJet CM1312
Class HP | embedded || printer
SEQ(SP=BF-C9%GCD=1-6%ISR=B9-C3%TI=RI%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=209D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2238%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP Color LaserJet CM6040 MFP Series / Q3939A
Fingerprint HP Color LaserJet CM6040 printer
Class HP | embedded || printer
SEQ(SP=FD-10B%GCD=1-6%ISR=104-112%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=5B4%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP Color LaserJet CM6040 MFP Series printer.
Fingerprint HP Color LaserJet CM6040 printer
Class HP | embedded || printer
SEQ(SP=F5-10D%GCD=1-6%ISR=100-10C%TI=RD%II=RI%TS=7)
OPS(O1=M538NW0NNT11%O2=M538NW0NNT11%O3=M538NW0NNT11%O4=M538NW0NNT11%O5=M538NW0NNT11%O6=M538NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=5B4%O=M538NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=75DE|8DC8|B699|DAA4|F7F0%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP Designjet Z3100ps 24in Photo
# HP Designjet T1100ps firmware version: TJ6-TAJ6_5.0.1.2
Fingerprint HP Designjet T1100ps or Z3100ps printer
Class HP | embedded || printer
SEQ(SP=BB-D1%GCD=1-6%ISR=CB-D5%TI=Z%CI=Z%II=I%TS=A)
OPS(O1=M5B4ST11NW2%O2=M5B4ST11NW2%O3=M5B4NNT11NW2%O4=M5B4ST11NW2%O5=M5B4ST11NW2%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW2%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# hp LaserJet 1320 series, Formatter Number: E7206LL, Service ID: 16053, Firmware Datecode: 20041024, Network Statistics Firmware Version: V.28.05
# HP LaserJet 2550N Color LaserJet
# Deskjet 1220C
# TippingPoint IPS TOS Version 2.5.5.6994 Model Number 110
Fingerprint HP DeskJet 1220, or LaserJet 1320 or 2550n printer; or TippingPoint 110 IPS
Class HP | embedded || printer
Class TippingPoint | embedded || firewall
SEQ(SP=94-9E%GCD=1-6%ISR=9B-A5%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP Photosmart 8400   Model HPF2109W040W firmware version:QF1P133G
# HP DeskJet 6127
# HP Officejet 7400
# HP Deskjet 6840
# HP Officejet Pro K550
# HP Photosmart 2710 all-in-one printer
Fingerprint HP DeskJet 6127 or 6840, Officejet 7400, Officejet Pro K550, or Photosmart 2710 or 8400 printer
Class HP | embedded || printer
SEQ(SP=B-15%GCD=1E848|3D090|5B8D8|7A120|98968|B71B0%ISR=9F-A9%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=B50%W2=AD8%W3=9D0%W4=B50%W5=830%W6=8E5)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=B68%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=8E5%S=O%A=O|S+%F=A|AS%O=NNT11|M109NW0NNSNNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP03424C Deskjet 6940 series
Fingerprint HP Deskjet 6940 printer
Class HP | embedded || printer
SEQ(SP=39-43%GCD=9C4|1388|1D4C|2710|30D4%ISR=9E-A8%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=B50%W2=AD8%W3=9D0%W4=B50%W5=830%W6=8E5)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=B68%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=8E5%S=O%A=S+%F=AS%O=M109NW0NNSNNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP Laserjet 4100 (firmware 2001206 01.009.0)
# HP LaserJet 4100 Series rev L.21.11
# DesignJet 500 (C7770B)
# HP Business InkJet 2300, Firmware version 20040813 RMR2015A
# HP LaserJet 8150 Series
Fingerprint HP InkJet 2300, DesignJet 500, or LaserJet 4100 or 8150 printer
Class HP | embedded || printer
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP Color LaserJet 2600n printer, Firmware Datecode: 20051208
# HP LaserJet 3390
# "HP Color LaserJet 2605dn", firmware datecode 20060510
# HP LaserJet P2015dn (firmware 20061010)
# HP Color Laserjet 2600
# HP Color Laserjet 2605dn
# HP LaserJet 3055
# HP LaserJet 3052
# This is an HP 3055 Laser printer
# HP 2015x
# HP Color LaserJet 2605dtn
# HP Color LaserJet 2840 All-In-One printer copier fax scanner
# HP LaserJet 1022n printer
# Brother HL-5250DN, Printer firmware version 1.07, Network firmware version 1.01
# Brother MFC-8860DN.
# Brother MFC-7840N, firmware version F, sub-firmware version 1.00, and NC-6600h print server firmware version 1.02.
Fingerprint HP LaserJet (1020-, 2010-, 2600-, 2800-, 3050-, or 3390-series), or Brother (HL-5250DN, MFC-7840N, or MFC-8860DN) printer
Class HP | embedded || printer
Class Brother | embedded || printer
SEQ(SP=0-16%GCD=1E848|3D090|5B8D8|7A120|98968|B71B0%ISR=9F-A9%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=209D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2238%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=209D%S=O%A=S+%F=AS%O=M109NW0NNSNNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP color laserjet 1017 mfp
Fingerprint HP LaserJet 1017 printer
Class HP | embedded || printer
SEQ(R=N)
OPS(O1=NNT11|M5B4NW0NNSNNT11%O2=NNT11|M578NW0NNSNNT11%O3=NNT11|M280NW0NNT11%O4=%O5=%O6=)
WIN(W1=21F0%W2=2088%W3=2258%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP LaserJet 1102w
Fingerprint HP LaserJet 1102w printer
Class HP | embedded || printer
SEQ(SP=AC-B6%GCD=1-6%ISR=AA-B4%TS=A)
OPS(O1=M5B4NNSNNT11%O2=M578NNSNNT11%O3=M280NNT11%O4=M5B4NNSNNT11%O5=M218NNSNNT11%O6=M109NNSNNT11)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=209D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2238%O=M5B4NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP LaserJet 1200
Fingerprint HP LaserJet 1200 printer
Class HP | embedded || printer
SEQ(SP=13-1D%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=98-A2%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=16D0%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=16D0%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=16D0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP LaserJet P3005
# HP Color LaserJet CP4005 Printer. The web interface reports the following in the "Server:" header: "HP-ChaiSOE/1.0".
# HP LaserJet P3005, Firmware Version   : V.33.55, HP JetDirect       : J7979E
# LaserJet 2420
# HP LaserJet P4014, Model:CB507A, Firmware: 20080528 04.045.2
# HP LaserJet 2055dn printer
Fingerprint HP LaserJet 2055dn, 2420, P3005, CP4005, or P4014 printer
Class HP | embedded || printer
SEQ(SP=FB-10B%GCD=1-6%ISR=102-110%TI=I%CI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=5B4%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# hp LaserJet 3030 printer, JetDirect J6061A, microcode S.25.39
# HP LaserJet 4300
# HP LaserJet 2200
Fingerprint HP LaserJet 2200, 3030, or 4300 printer
Class HP | embedded || printer
SEQ(SP=5B-9D%GCD=1-6%ISR=9B-A5%TI=I|RD%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP LaserJet 2200dtn
Fingerprint HP LaserJet 2200dtn printer
Class HP | embedded || printer
SEQ(SP=94-9E%GCD=1-6%ISR=9B-A5%TI=I%TS=1|2)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=41%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=41%TG=40%W=5B4%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=41%TG=40%W=5B4%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=41%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(R=N)

# HP LaserJet 2200DTN (2200 Series)
Fingerprint HP LaserJet 2200dtn printer
Class HP | embedded || printer
SEQ(SP=0-1B%GCD=1-6%ISR=15-1F%TI=I%II=I%SS=O%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=16D0%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# HP LaserJet 2300N
Fingerprint HP LaserJet 2300N printer
Class HP | embedded || printer
SEQ(SP=93-9D%GCD=1-6%ISR=9B-A5%TI=I%II=I%SS=S%TS=1)
OPS(O1=M576NW0NNT11%O2=M576NW0NNT11%O3=M576NW0NNT11%O4=M576NW0NNT11%O5=M576NW0NNT11%O6=M576NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5B4%O=M576NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# hp LaserJet 2420, Printer Model: Q5957A
Fingerprint HP LaserJet 2420 printer
Class HP | embedded || printer
SEQ(SP=93-9D%GCD=1-6%ISR=9A-A4%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=N)
T1(R=Y%DF=N%T=42%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=42%TG=40%W=5B4%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=42%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=42%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=42%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=42%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=42%TG=40%CD=S)

# HP Color LaserJet 2600n Printer
Fingerprint HP LaserJet 2600n printer
Class HP | embedded || printer
SEQ(SP=F-19%GCD=1E848|3D090|5B8D8|7A120|98968%ISR=9C-A6%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=209D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2238%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=Z%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=209D%S=Z%A=S+%F=AS%O=M109NW0NNSNNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP Color LaserJet 2600n
Fingerprint HP LaserJet 2600n printer
Class HP | embedded || printer
SEQ(CI=I%II=I)
OPS(O1=NNT11|M5B4NW0NNSNNT11%O2=%O3=%O4=%O5=%O6=)
WIN(W1=21F0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# hp color laserjet 2605dn
Fingerprint HP LaserJet 2605dn printer
Class HP | embedded || printer
SEQ(SP=0-15%GCD=1E848|3D090|5B8D8|7A120|98968%ISR=9E-A8%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=209D)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2238%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=209D%S=O%A=S+%F=AS%O=M109NW0NNSNNT11%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP Color LaserJet 2840 fw 20070524
Fingerprint HP LaserJet 2840 printer
Class HP | embedded || printer
SEQ(SP=B-15%GCD=1E848|3D090|5B8D8|7A120|98968%ISR=9E-A8%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=209D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2238%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=209D%S=O%A=S+%F=AS%O=M109NW0NNSNNT11%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# hp color LaserJet 4600 / model C9692A / firmware 20030627 03.012.3
# hp LaserJet 4200       Printer Model: Q2426A     Firmware Datecode: 20030530 04.016.1
# HP LaserJet 4050 series printer
# HP LaserJet 5100 Series printer (J7934A), Firmware Version:  V.28.06
# HP Laserjet 3330
Fingerprint HP LaserJet 3330/4050/4200/4600/5100 printer
Class HP | embedded || printer
SEQ(SP=95-9F%GCD=1-6%ISR=9B-A5%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP Color LaserJet 3600n
Fingerprint HP LaserJet 3600n printer
Class HP | embedded || printer
SEQ(SP=95-9F%GCD=1-6%ISR=9B-A5%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=16D0%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=16D0%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=16D0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP LaserJet 4050 PN J3113A ROM G.08.08 EEPROM G.08.04
Fingerprint HP LaserJet 4050
Class HP | embedded || printer
SEQ(SP=0-5%GCD=1-6%ISR=15-1F%TI=I%II=I%SS=O%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3C%TG=40%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=16D0%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=Z)

# HP LaserJet 4050, model J3113A, version G.07.20
# jetdirect 170x
# LaserJet 4000n
# This is a HP JetDirect EX Plus3 running firmware D.08.49
Fingerprint HP LaserJet 4050 or 4000n printer or JetDirect EX Plus 3 print server
Class HP | embedded || printer
Class HP | embedded || print server
SEQ(R=N)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=3C%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=A%A=S+%F=AR%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=Z)

# HP Laserjet 4100
Fingerprint HP LaserJet 4100 printer
Class HP | embedded || printer
SEQ(SP=0-5%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=95-9F%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP laserjet 4100n
Fingerprint HP LaserJet 4100N printer
Class HP | embedded || printer
SEQ(SP=13-1D%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP 4100N printer. HP JetDirect:   J4169A. Firmware Version:       L.25.08.
Fingerprint HP LaserJet 4100N printer
Class HP | embedded || printer
SEQ(SP=94-9E%GCD=1-6%ISR=9A-A4%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=16D0%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=16D0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP Laserjet 4200 - network printer
Fingerprint HP LaserJet 4200 printer
Class HP | embedded || printer
SEQ(SP=92-9C%GCD=1-6%ISR=9C-A6%TI=I%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(R=N)

# HP Laserjet 4250 using JetDirect J7949E
Fingerprint HP LaserJet 4250 (JetDirect) printer
Class HP | embedded || printer
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=16D0%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=16D0%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=16D0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP Laserjet 4250
Fingerprint HP LaserJet 4250 printer
Class HP | embedded || printer
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP LaserJet 4250 printer, Firmware Version: V.28.47.FF
# hp LaserJet 4250 model Q5402A, V.28.47, J7949E
Fingerprint HP LaserJet 4250 printer (J7949E)
Class HP | embedded || printer
SEQ(SP=13-1D%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP LaserJet 4345
# HP LaserJet 9040
Fingerprint HP LaserJet 4250dtn, 4345, or 9040 (JetDirect) printer
Class HP | embedded || printer
SEQ(SP=18-1C%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=9D-A3%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP LaserJet 4300 JetDirect FW R.25.57
Fingerprint HP LaserJet 4300 printer
Class HP | embedded || printer
SEQ(SP=94-9E%GCD=1-6%ISR=9B-A5%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP LASERJET 4345MFP, Firmware 20070628 09.081.6
Fingerprint HP LaserJet 4345 printer
Class HP | embedded || printer
SEQ(SP=16-20%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=9B-A5%TI=I%II=I%SS=S%TS=2)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP LaserJet 4350 Firmware Datecode 20060718 08.012.1
Fingerprint HP LaserJet 4350 printer
Class HP | embedded || printer
SEQ(SP=FC-10C%GCD=1-6%ISR=107-111%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2DA0%W2=2DA0%W3=2DA0%W4=2DA0%W5=2DA0%W6=2DA0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2DA0%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N|Y%T=3B-45%TG=40%W=2DA0%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP 4350 Laserjet
Fingerprint HP LaserJet 4350 printer
Class HP | embedded || printer
SEQ(SP=13-1D%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HpLaserjet4000TN
# jetdirect J2552
# JetDirect Card in an HP LaserJet 4 MV
Fingerprint HP LaserJet 4MV or 4000TN printer
Class HP | embedded || printer
SEQ(SP=0-1B%GCD=1-6%ISR=15-1F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3C%TG=40%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=16D0%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=Z)

# HP Laserjet 4Si
# HP Laserjet 4 plus
Fingerprint HP LaserJet 4Si or LaserJet 4 Plus printer
Class HP | embedded || printer
SEQ(SP=0-1D%GCD=1-6%ISR=16-20%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2238%W2=2238%W3=2238%W4=2238%W5=2238%W6=2238)
ECN(R=Y%DF=N%T=3C%TG=40%W=2238%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=2238%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=Z)

# HP LaserJet 5, Firmware Datecode = 19960115, HP JetDirect = J2552B
Fingerprint HP LaserJet 5 printer
Class HP | embedded || printer
SEQ(CI=I%II=I)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=37-41%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=37-41%TG=40%S=A%A=S+%F=AR%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=37-41%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=37-41%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=37-41%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=37-41%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=37-41%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=N%T=37-41%TG=40%CD=Z)

# LaserJet 5m.
Fingerprint HP LaserJet 5M printer
Class HP | embedded || printer
SEQ(SP=0-1B%GCD=1-6%ISR=15-1F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=860%W2=860%W3=860%W4=860%W5=860%W6=860)
ECN(R=Y%DF=N%T=3C%TG=40%W=860%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=860%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=Z)

# HP LaserJet 5M with JetDirect card.
Fingerprint HP LaserJet 5M printer
Class HP | embedded || printer
SEQ(SP=0-1B%GCD=1-6%ISR=15-1F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=860%W2=860%W3=860%W4=860%W5=860%W6=860)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=860%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=860%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# HP LaserJet 8100 Series, firmware G.06.00
Fingerprint HP LaserJet 8100 Series printer
Class HP | embedded || printer
SEQ(SP=0%GCD=1-6%ISR=14-1E%TI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=860%W2=860%W3=860%W4=860%W5=860%W6=860)
ECN(R=Y%DF=N%T=3C%TG=40%W=860%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=860%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=Z)

# HP LaserJet P2015 Series printer
# HP CM1017 printer
Fingerprint HP LaserJet CM1017 or P2015 printer
Class HP | embedded || printer
SEQ(SP=0-5%GCD=1E848|3D090|5B8D8|7A120|98968%ISR=9C-A6%TI=I%CI=I%II=I%SS=O%TS=A)
OPS(O1=NNT11|M5B4NW0NNSNNT11%O2=NNT11|M578NW0NNSNNT11%O3=NNT11|M280NW0NNT11%O4=NNT11|M5B4NW0NNSNNT11%O5=%O6=)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=0%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP Color LaserJet CP1518ni
Fingerprint HP LaserJet CP1518ni printer
Class HP | embedded || printer
SEQ(SP=AF-B9%GCD=1-6%ISR=AD-B7%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=209D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2238%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP LaserJet M1120n MFP
# HP LaserJet CP2525N or CP2525DN
# HP LaserJet M1522n MFP
Fingerprint HP LaserJet M1120n or M1522n multifunction printer
Class HP | embedded || printer
SEQ(SP=A0-BE%GCD=1-6%ISR=A5-B7%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=209D)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2238%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP LaserJet M1522nf MFP (25284A)
Fingerprint HP LaserJet M1522nf printer
Class HP | embedded || printer
SEQ(SP=74-D2%GCD=1-6%ISR=96-CA%TI=I%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=209D)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2238%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# HP LaserJet M2727nf MFP
# HP LaserJet M27227
Fingerprint HP LaserJet M2727 printer
Class HP | embedded || printer
SEQ(SP=C5-D1%GCD=1-6%ISR=BD-C7%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=209D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2238%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP LaserJet M2727nf MFP
Fingerprint HP LaserJet M2727nf printer
Class HP | embedded || printer
SEQ(SP=70-86%GCD=1-6%ISR=A1-AB%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=209D)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2238%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP LaserJet P1505n
Fingerprint HP LaserJet P1505n printer
Class HP | embedded || printer
SEQ(SP=AB-B5%GCD=1-6%ISR=AC-B6%TI=I%TS=7)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=209D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2238%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP LaserJet 3055 printer, firmware date 20060117
# HP Color LaserJet 2600n
# HP LaserJet P2015 Series
# Sony Network Camerea model SNC-Z20N
Fingerprint HP LaserJet P2015, 2600n, or 3055 printer; or Sony SNC-Z20N network camera
Class HP | embedded || printer
Class Sony | embedded || webcam
SEQ(SP=B-15%GCD=1E848|3D090|5B8D8|7A120|98968%ISR=9E-A8%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=209D)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2238%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=209D%S=O%A=O|S+%F=A|AS%O=NNT11|M109NW0NNSNNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP LaserJet P2055dn built-in jetdirect
Fingerprint HP LaserJet P2055dn printer
Class HP | embedded || printer
SEQ(SP=F4-10C%GCD=1-6%ISR=100-112%TI=I%CI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP LaserJet p2055x
Fingerprint HP LaserJet P2055x printer
Class HP | embedded || printer
SEQ(SP=FD-109%GCD=1-6%ISR=FA-112%TI=I%CI=I%II=I%SS=S%TS=7)
OPS(O1=M564NW0NNT11%O2=M564NW0NNT11%O3=M564NW0NNT11%O4=M564NW0NNT11%O5=M564NW0NNT11%O6=M564NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=5B4%O=M564NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=5B4%S=O%A=S+%F=AS%O=M564NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP LaserJet P3005 Printers
Fingerprint HP LaserJet P3005 printer
Class HP | embedded || printer
SEQ(SP=100-10A%GCD=1-6%ISR=102-10C%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP LaserJet 4050
# HP Laserjet 4100
# HP JetDirect       : J6057A   Firmware Version   : R.25.47 (HP 8150 printer)
Fingerprint HP LaserJet printer (4050, 4100, 4200, or 8150)
Class HP | embedded || printer
SEQ(SP=93-9D%GCD=1-6%ISR=9A-A4%TI=I%II=I%SS=S%TS=1|2)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Internal NIC on HP LaserJet 2035
# HP Color LaserJet CM2320fxiMFP
# HP Color LaserJet CM1312nfi MFP
# HP CP1515N
# Network printer HP LaserJet M1120n MFP
# HP LaserJet M1522n MFP
# HP Color LaserJet CP1518ni
# HP LaserJet M1522nf MFP
# HP Color LaserJet CP2025dn, Firmware Datecode: 20081216
# HP LaserJet M1120n network printer
# HP LaserJet P2035n Firmware Datecode 20080814
# HP LaserJet M2727nf MFP
# HP Color LaserJet CP1515n
Fingerprint HP LaserJet printer (CM1312nfi, CM2320, CP1500-series, CP2025dn, M1120-series, M1522-series, M2727nf, or P2035) or MGE MX 5000 RT UPS
Class HP | embedded || printer
Class MGE | embedded || power-device
SEQ(SP=79-C2%GCD=1-6%ISR=9A-BA%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=209D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2238%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Product Name     HP Officejet J4680 series Firmware Version         YWM2FN0904AR
Fingerprint HP Officejet J4680 printer
Class HP | embedded || printer
SEQ(SP=7B-89%GCD=1-6%ISR=99-A3%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=B50%W2=AD8%W3=9D0%W4=B50%W5=830%W6=8E5)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=B68%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP J6480 printer
# HP UPS Management Module
Fingerprint HP Officejet J6480 printer
Class HP | embedded || printer
SEQ(SP=A4-C0%GCD=1-6%ISR=AA-B6%TI=I%CI=I%II=I%SS=S%TS=A|B|C)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=43E0%W5=4180%W6=403D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4470%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Photosmart 8400 series, HPF2109W040W
Fingerprint HP Photosmart 8400 printer
Class HP | embedded || printer
SEQ(SP=C-16%GCD=1E848|3D090|5B8D8|7A120|98968%ISR=9F-A9%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=B50%W2=AD8%W3=9D0%W4=B50%W5=830%W6=8E5)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=B68%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP Photosmart 8750 (part of the 8700 series). Firmware: OF1P151A
Fingerprint HP Photosmart 8750 printer
Class HP | embedded || printer
SEQ(SP=C-16%GCD=1E848|3D090|5B8D8|7A120|98968%ISR=9F-A9%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=B50%W2=AD8%W3=9D0%W4=B50%W5=830%W6=8E5)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=B68%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=8E5%S=O%A=S+%F=AS%O=M109NW0NNSNNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP Photosmart Premium C309g-m, Firmware Version: WHM1FN0931BR
# HP Officejet 7000 Wide
# Printer Photosmart C4780 wireless
Fingerprint HP PhotoSmart C390 or C4780, or Officejet 7000 printer
Class HP | embedded || printer
SEQ(SP=38-C6%GCD=1-6%ISR=8A-BE%TI=RD|RI%CI=RI%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=B50%W2=AD8%W3=9D0%W4=B50%W5=830%W6=8E5)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=B68%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP Photosmart C4380
Fingerprint HP Photosmart C4380 printer
Class HP | embedded || printer
SEQ(SP=A4-AE%GCD=1-6%ISR=A8-B2%TI=I%II=I%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=B50%W2=AD8%W3=9D0%W4=B50%W5=830%W6=8E5)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=B68%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP Photosmart C7280
# Hp OfficeJet j6450
# HP Photosmart C4500 series printer
Fingerprint HP Photosmart C4500 or C7280, or Officejet J6450 printer
Class HP | embedded || printer
SEQ(SP=7F-89%GCD=1-6%ISR=97-AB%TI=I%CI=RD|RI%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=B50%W2=AD8%W3=9D0%W4=B50%W5=830%W6=8E5)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=B68%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP PhotoSmart D7260 printer
# HP Photosmart C4380
# HP PhotoSmart C7200 Series Printer
# HP Photosmart C7280 All-in-One, Wireless interface
# HP Photosmart D7260, with firmware version RExxFN0721BR
# HP Officejet J6400 series
# HP Officejet 6500 E709n (Wireless)
# HP Photosmart C8100 (C8180) series
# Photosmart C6200 wired connected printer
# HP OfficeJet J6450
# HP OfficeJet 6500 Wireless
Fingerprint HP printer: Photosmart 4300-, 6500-, 7200-, or 8100-series, or Officejet 6000-series
Class HP | embedded || printer
SEQ(SP=A3-E2%GCD=1-6%ISR=A9-D9%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=B50%W2=AD8%W3=9D0%W4=B50%W5=830%W6=8E5)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=B68%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP Photosmart C6180 All-in-One
# HP Deskjet 6980 series
# HP Photosmart 2575
# HP DeskJet 6980dt
# HP PSC5100 Series Printer
# Officejet 6300 Series
# HP Officejet Pro L7600
# HP Deskjet 6940
# HP OfficeJet Pro L7780 Embedded Webserver (EWS)
# HP Officejet Pro K5400
# HP Photosmart C6180, Firmware Version: R0631MxNxxN0
# HP Officejet Pro K550
# HP Officejet Pro L7700, Model Number: C8192A, Firmware Version: R2004NxNxeN0
Fingerprint HP printer: Photosmart All-in-One (2575, PSC5100, C5180, C6100, or C6180); DeskJet (6940 or 6980); Officejet 6300-series; or Officejet Pro (K550, K5400, L7600, or L7780)
Class HP | embedded || printer
SEQ(SP=34-44%GCD=9C4|1388|1D4C|2710|30D4%ISR=9F-A9%TI=I%II=I%SS=S%TS=A|B)
OPS(O1=NNT11|M5B4NW0NNSNNT11%O2=NNT11|M578NW0NNSNNT11%O3=NNT11|M280NW0NNT11%O4=NNT11|M5B4NW0NNSNNT11%O5=NNT11|M218NW0NNSNNT11%O6=NNT11|M109NNSNNT11)
WIN(W1=B50%W2=AD8%W3=9D0%W4=B50%W5=830%W6=8E5)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=B68%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=8E5%S=O%A=S+%F=AS%O=NNT11|M109NW0NNSNNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# ProFibre Storage Array DF-4000 with firmware 9.40.0.0
# HP LaserJet 2420
# "Siemens C-110" ADSL Modem (Not Wireless)
# Kaiomy Modem Roteador ADSL Wireless 2014PW
# PLANET ADSL MODEM ROUTER ADE-4110
Fingerprint Kaiomy AL-2014PW, Planet ADE-4110, or Siemens C-110 ADSL modem; HP LaserJet 2420 printer; or IBM DF-4000 ProFibre Storage Array
Class HP | embedded || printer
Class IBM | embedded || storage-misc
Class Kaiomy | embedded || WAP
Class Planet | embedded || broadband router
Class Siemens | embedded || broadband router
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP Onboard Administrator, Firmware Version 2.04
Fingerprint HP Onboard Administrator management console
Class HP | embedded || remote management
SEQ(SP=C4-CE%GCD=1-6%ISR=C8-D2%TI=Z%II=I%TS=8)
OPS(O1=M5B4ST11NW1%O2=M5B4ST11NW1%O3=M5B4NNT11NW1%O4=M5B4ST11NW1%O5=M5B4ST11NW1%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# BladeSystem c7000 Enclosure
# HP Onboard Administator (v2.25), Bladesystem (aka bladecenter) c7000
# Onboard Administrator for HP BladeSystem c-Class enclosures. It uses embedded Linux based on the 2.6 kernel.
Fingerprint HP Onboard Administrator remote management for BladeSystem server enclosures
Class HP | embedded || remote management
SEQ(SP=C6-D0%GCD=1-6%ISR=CB-D5%TI=Z%II=I%TS=8)
OPS(O1=M5B4NNT11NW1%O2=M5B4NNT11NW1%O3=M5B4NNT11NW1%O4=M5B4NNT11NW1%O5=M5B4NNT11NW1%O6=M5B4NNT11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# SonicWALL SOHO3 CPU: Toshiba 3927 H2 / 133 Mhz Firmware version: 6.5.0.4 ROM version: 6.2.0.0
# HP Network Storage Router, model E1200. Firmware 5.4.25, BIOS "BIOS 4.23", Booter "BOOTER 4.11"
Fingerprint HP E1200 Network Storage Router NAS device or SonicWALL SOHO3 firewall
Class HP | embedded || storage-misc
Class SonicWALL | embedded || firewall
SEQ(SP=87-9F%GCD=1-6%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# hp MSA2324sa (msa2000 series). http-server identifies itself as "WindRiver-WebServer/4.4".
Fingerprint HP MSA2324sa NAS device
Class HP | embedded || storage-misc
SEQ(SP=96-A0%GCD=1-6%ISR=9C-A6%TI=I%CI=I%II=I%SS=O|S%TS=1|3)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP StorageWorks MSL6000 Tape Library, 10BaseT NIC
Fingerprint HP StorageWorks MSL6000 tape library
Class HP | embedded || storage-misc
SEQ(SP=52-B6%GCD=1000|2000|3000|4000|5000%ISR=BC-10A%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4T11NN%O2=M5B4%O3=M5B4T11NN%O4=M5B4T11NN%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3C%TG=40%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=16D0%S=O%A=S+%F=AS%O=M5B4T11NN%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=70%UN=128%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=Z)

# HP J4093A ProCurve Switch 2424M Firmware revision C.09.28
Fingerprint HP 2424M ProCurve switch (J4093A)
Class HP | embedded || switch
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=96-A0%TI=I%TS=U)
OPS(O1=M5AC%O2=M5AC%O3=M5AC%O4=M5AC%O5=M5AC%O6=M5AC)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M5AC%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O|S+%F=AS%O=M5AC%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP ProCurve Switch 4000M Firmware revision C.09.22
Fingerprint HP 4000M ProCurve switch (J4121A)
Class HP | embedded || switch
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5AC%O2=M5AC%O3=M5AC%O4=M5AC%O5=M5AC%O6=M5AC)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M5AC%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP ProCurve Switch 4000M Firmware revision C.09.22
Fingerprint HP 4000M ProCurve switch (J4121A)
Class HP | embedded || switch
SEQ(R=N)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP ProCurve Switch 4108GL, G.04.05
Fingerprint HP 4108GL ProCurve switch
Class HP | embedded || switch
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# HP Advanced Stack Switch 2000 HP J3100B
Fingerprint HP Advanced Stack Switch 2000
Class HP | embedded || switch
SEQ(SP=0%GCD=1-6|68|D0|138|1A0|208|270%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M100%O2=M100%O3=M100%O4=M100%O5=M100%O6=M100)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=19-23%TG=20%W=400%O=M100%CC=N%Q=U)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=U)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=400%S=O%A=S+%F=AS%O=M100%RD=0%Q=U)
T4(R=Y%DF=N%T=19-23%TG=20%W=400%S=A%A=Z%F=R%O=%RD=0%Q=U)
T5(R=Y%DF=N%T=19-23%TG=20%W=400%S=A%A=O%F=R%O=%RD=0%Q=U)
T6(R=Y%DF=N%T=19-23%TG=20%W=400%S=A%A=O%F=R%O=%RD=0%Q=U)
T7(R=Y%DF=N%T=19-23%TG=20%W=400%S=A%A=O%F=R%O=%RD=0%Q=U)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=19-23%TG=20%CD=S)

# Brocade 1600 SAN Switch running firmware version 3.2.0a.
Fingerprint HP Brocade 1600 switch
Class HP | embedded || switch
SEQ(SP=13-1D%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP Brocade 4Gb SAN Switch for HP p-Class Bladesystems running firmware version 5.3.0
Fingerprint HP Brocade 4Gb SAN switch
Class HP | embedded || switch
SEQ(SP=C2-CC%GCD=1-6%ISR=C7-D1%TI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW2%O2=M5B4ST11NW2%O3=M5B4NNT11NW2%O4=M5B4ST11NW2%O5=M5B4ST11NW2%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# GbE2c Ethernet Blade Switch for HP c-Class BladeSystem
Fingerprint HP GbW2c Ethernet Blade Switch
Class HP | embedded || switch
SEQ(SP=A4-B4%GCD=1-6%ISR=9E-B2%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=4000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP J3289A ProCurve 10/100 Hub 24M
Fingerprint HP ProCurve 10/100 hub
Class HP | embedded || switch
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP ProCurve Switch 1810G-8 running P.1.17 version
Fingerprint HP ProCurve 1810G switch
Class HP | embedded || switch
SEQ(SP=F5-109%GCD=1-6%ISR=F7-111%TI=I%CI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=10F8%W2=1044%W3=112C%W4=1194%W5=1060%W6=10CD)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=111C%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP ProCurve 2520-8-poe switch, S.14.03
Fingerprint HP ProCurve 2520 switch
Class HP | embedded || switch
SEQ(SP=A2-AC%GCD=1-6%ISR=A9-B3%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW1NNSNNT11%O2=M578NW1NNSNNT11%O3=M280NW1NNT11%O4=M5B4NW1NNSNNT11%O5=M218NW1NNSNNT11%O6=M109NNSNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP J4813A Procurve 2524
Fingerprint HP ProCurve 2524 switch (J4813A)
Class HP | embedded || switch
SEQ(SP=95-9F%GCD=1-6%ISR=9A-A4%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=M5B4NW0%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP 9100c Digital Sender  (scanner)
# HP ProCurve Switch 2524
Fingerprint HP ProCurve 2524 switch or 9100c Digital Sender printer
Class HP | embedded || switch
Class HP | embedded || printer
SEQ(R=N)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP Procurve 2524 (firmware F.05.34)
# HP Procurve 2524 (firmware F.05.17)
# HP Jetdirect 175x Model J6035A, Firmware version M.21.21
# Brocade Switch Explorer
Fingerprint HP ProCurve 2524 switch or JetDirect 175x print server (J6035A)
Class HP | embedded || switch
Class HP | embedded || printer
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=99-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# System Name: HP ProCurve Switch 2650, Product: HP J4899B ProCurve Switch 2650, Version: H.08.60, ROM H.08.02
Fingerprint HP ProCurve 2650 switch
Class HP | embedded || switch
SEQ(SP=13-1D%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%TI=I%II=I%SS=S%TS=1)
OPS(O1=M200NW0NNT11%O2=M200NW0NNT11%O3=M200NW0NNT11%O4=M200NW0NNT11%O5=M200NW0NNT11%O6=M200NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M200NW0%CC=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=M200NW0NNT11%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP Procurve Switch J4899A (2650) SW-Version H.07.50
Fingerprint HP ProCurve 2650 switch (J4899A)
Class HP | embedded || switch
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=O|S%TS=U)
OPS(O1=M578NW0%O2=M578NW0%O3=M578NW0%O4=M578NW0%O5=M578NW0%O6=M578)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M578NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Konica Minolta Bizhub C450 with Default Emperon Controller
# HP ProCurve 2650 (Product number: HP J4899B)
Fingerprint HP ProCurve 2650 switch or Konica Minolta bizhub C450 printer
Class HP | embedded || switch
Class Konica Minolta | embedded || printer
SEQ(SP=13-1D%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=98-A2%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP Procurve 5300xl series switch, Image stamp: /sw/code/build/alpmo(m35), Oct 31 2007 15:49:10 E.10.71 588
# ProCurve J4903A Switch 2824, Software revision I.10.43
# HP ProCurve 2650-PWR switch running software revision H.10.38
# ProCurve J4899B Switch 2650 Software revision H.10.45
Fingerprint HP ProCurve 2650, 2824, 2848, or 5300xl switch
Class HP | embedded || switch
SEQ(SP=96-A0%GCD=1-6%ISR=9C-A6%TI=I%TS=1)
OPS(O1=M200NW0NNT11%O2=M200NW0NNT11%O3=M200NW0NNT11%O4=M200NW0NNT11%O5=M200NW0NNT11%O6=M200NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M200NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O|S+%F=AS%O=M200NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP ProCurve 2910al-48 running software image W.14.30
Fingerprint HP ProCurve 2910al switch
Class HP | embedded || switch
SEQ(SP=DF-E9%GCD=1-6%ISR=E4-EE%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW1NNSNNT11%O2=M578NW1NNSNNT11%O3=M280NW1NNT11%O4=M23C6NW1NNSNNT11%O5=M218NW1NNSNNT11%O6=M109NNSNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=41%TG=40%W=FFFF%O=M5B4NW1NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=100%TG=FF%CD=S)

# ProCurve J9147A 2910al-48G Switch, revision W.14.38
# ProCurve 2910al-24G Switch (J9145A) W.14.49, ROM W.14.04
Fingerprint HP ProCurve 2910al switch
Class HP | embedded || switch
SEQ(SP=F4-102%GCD=1-6%ISR=F1-FB%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW1NNSNNT11%O2=M578NW1NNSNNT11%O3=M280NW1NNT11%O4=M5B4NW1NNSNNT11%O5=M218NW1NNSNNT11%O6=M109NNSNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# ProCurve J9091A Switch 8212zl, Software revision K.14.41
# ProCurve J9311A Switch 3500yl-48G-PoE+, Software revision K.14.52
Fingerprint HP ProCurve 3500yl or 8212zl switch
Class HP | embedded || switch
SEQ(SP=A5-AF%GCD=1-6%ISR=A6-B0%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW1NNSNNT11%O2=M578NW1NNSNNT11%O3=M280NW1NNT11%O4=M23C6NW1NNSNNT11%O5=M218NW1NNSNNT11%O6=M109NNSNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP Procurve 3500 YL
# UTStarcom F1000, Firmware Version: 4.50st
# ProCurve J8697A Switch 5406zl, revision K.13.25
# ProCurve Switch 6200yl-24G (J8992A) Ver. K.13.60
Fingerprint HP ProCurve 3500yl, 5406zl, or 6200yl switch
Class HP | embedded || switch
Class UTStarcom | embedded || VoIP phone
SEQ(SP=F7-10D%GCD=1-6%ISR=103-10D%TI=I%II=I%SS=S%TS=5)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N|Y%T=3B-45%TG=40%W=4000%S=O%A=O|S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP J4121A ProCurve Switch 4000M Firmware revision C.09.16
Fingerprint HP ProCurve 4000M switch (J4121A)
Class HP | embedded || switch
SEQ(SP=E-18%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%TI=I%TS=U)
OPS(O1=M5AC%O2=M5AC%O3=M5AC%O4=M5AC%O5=M5AC%O6=M5AC)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M5AC%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=Y%T=3B-45%TG=40%CD=S)

# HP Procurve switch 4104gl
# HP ProCurve Switch 4104GL
# HP J4865A ProCurve Swtich 4108GL
Fingerprint HP ProCurve 4104gl or 4108gl switch
Class HP | embedded || switch
SEQ(SP=96-A0%GCD=1-6%ISR=9C-A6%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O|S+%F=AS%O=M5B4NW0%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP ProCurve 5406zl
Fingerprint HP ProCurve 5406zl switch
Class HP | embedded || switch
SEQ(SP=70-8A%GCD=1-6%ISR=9A-A4%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW1NNSNNT11%O2=M578NW1NNSNNT11%O3=M280NW1NNT11%O4=M5B4NW1NNSNNT11%O5=M218NW1NNSNNT11%O6=M109NNSNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP ProCurve Switch 5412zl (J8698A)
Fingerprint HP ProCurve 5412zl switch
Class HP | embedded || switch
SEQ(SP=C2-CC%GCD=1-6%ISR=BB-C5%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW1NNSNNT11%O2=M578NW1NNSNNT11%O3=M280NW1NNT11%O4=M5B4NW1NNSNNT11%O5=M218NW1NNSNNT11%O6=M109NNSNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# J4138A HP ProCurve Routing Switch 9308M, Software Version 07.6.04cT53
# HP ProCurve Routing Switch 9304m
Fingerprint HP ProCurve 9304m or 9308m switch
Class HP | embedded || switch
SEQ(SP=8B-99%GCD=1-6%ISR=8C-96%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=U)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=U)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=U)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=U)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# ProCurve J9019A Switch 2510-24, Software revision Q.10.01
# ProCurve J4903A Switch 2824 Software revision I.08.105
# HP Procurve 2626-PWR, firmware H.08.98
# HP ProCurve Switch 5304XL - HP J4850A Switch 5304XL
# ProCurve Switch 2848
# HP ProCurve 5304xl (5300xl series) Modular Router/Switch (ROM version E.05.04, firmware revision E.10.37)
# Hewlett-Packard J4819A ProCurve Switch 5308xl [Software revision E.10.61]
# HP Procurve 2810-48G switch
# Thomson ST2030 VoIP Business Phone
# Thomson VoIP phone  ST2030
# ProCurve J8164A Switch 2626-PWR, Software revision H.10.38
# Thomson ST 2022 VoIP phone
Fingerprint HP ProCurve switch (2500-, 2600-, 2800-, or 5300xl-series), or Thomson ST 2020 or 2030 VoIP phone
Class HP | embedded || switch
Class Thomson | embedded || VoIP phone
SEQ(SP=95-A1%GCD=1-6%ISR=9B-A6%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O|S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Nortel switch rebranned by HP for p-Class blade enclosers. Model p-Class C-Gbe2 running firmware version 3.2.3.
Fingerprint HP ProLiant BL p-Class C-Gbe2 switch
Class HP | embedded || switch
SEQ(SP=86-D8%GCD=1-6%ISR=8C-C8%TI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1000%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP ProCurve MSM422 Access Point, Firmware 5.3.3.0-01-7357
Fingerprint HP ProCurve MSM422 WAP
Class HP | embedded || WAP
SEQ(SP=C4-CE%GCD=1-6%ISR=CE-D8%TI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=B50%W2=B50%W3=B50%W4=B50%W5=B50%W6=B50)
ECN(R=N)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# HP-UX B.09.00 A 9000/42T 080009148e6a two-user license
Fingerprint HP HP-UX B.09.00
Class HP | HP-UX | 09.X | general purpose
SEQ(SP=0-1D%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=95-9F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# HP-UX B.10.20 C 9000/810
# HP-UX B.10.20 U 9000/861 2015893443
# HP-UX B.10.20 E 9000/803
Fingerprint HP HP-UX B.10.20
Class HP | HP-UX | 10.X | general purpose
SEQ(SP=0-1D%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=95-9F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=8000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# HP-UX B10.20 A 9000/712
Fingerprint HP HP-UX B.10.20
Class HP | HP-UX | 10.X | general purpose
SEQ(SP=0-5%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=95-9F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# HP-UX B.11.00 A 9000/785 2013724412 two-user license
# HP-UX B.11.00 U 9000/806 1949367251 unlimited-user license
Fingerprint HP HP-UX B.11.00
Class HP | HP-UX | 11.X | general purpose
SEQ(SP=73-B3%GCD=1-6%ISR=94-A4%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4W0NNNT11%O2=M578W0NNNT11%O3=M280W0NNNT11%O4=M218W0NNNT11%O5=M218W0NNNT11%O6=M109NNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=8000%O=M5B4W0N%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=E44A4E43%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=O%A=S+%F=AS%O=M109W0NNNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=E44A4E43%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=EA6C967D%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=EA6C967D%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# HP-UX B.11.00 U 9000/800 664359393 unlimited-user license
Fingerprint HP HP-UX B.11.00
Class HP | HP-UX | 11.X | general purpose
SEQ(SP=99-A9%GCD=1-6%ISR=A5-B3%TI=I%II=I%SS=S%TS=7)
OPS(O1=M564NNSW0NNNT11%O2=M564NNSW0NNNT11%O3=M280W0NNNT11%O4=M218NNSW0NNNT11%O5=M218NNSW0NNNT11%O6=M109NNSNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M564NNSW0N%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=22-3E%TG=40%W=80%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=2A-40%TG=40%W=100%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=24-3B%TG=40%W=400%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=Y%T=23-2F|31-40%TG=40%W=8000%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=27-3E%TG=40%W=FFFF%S=A%A=S%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# HP-UX B.11.00 C 9000/800 160901537 32-user license
# HP-UX B.11.11 U 9000/800 194404687 unlimited-user license
# HP-UX B.11.11 U 9000/803 2008500218 unlimited-user license
# HP-UX B.11.23 U ia64 0798527821 unlimited-user license
# HP-UX B.11.23 U ia64 0700834332 unlimited-user license
# HP-UX B.11.23 U ia64 3853031127 unlimited-user license
# HP-UX B.11.00 U 9000/800 551740568
# HP-UX B.11.00 U 9000/712 2006764246 unlimited-user license
# HP-UX B.11.31 U ia64 4267365567 unlimited-user license
Fingerprint HP HP-UX B.11.00 - B.11.31
Class HP | HP-UX | 11.X | general purpose
SEQ(SP=85-A6%GCD=1-6%ISR=99-A8%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NNSW0NNNT11%O2=M578NNSW0NNNT11%O3=M280W0NNNT11%O4=M218NNSW0NNNT11%O5=M218NNSW0NNNT11%O6=M109NNSNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M5B4NNSW0N%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=E44A4E43%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=8000%S=O%A=S+%F=AS%O=M109NNSW0NNNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=E44A4E43%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=EA6C967D%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=EA6C967D%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# HP-UX B.11.11 U 9000/782 2010612016 unlimited-user license
Fingerprint HP HP-UX B.11.11
Class HP | HP-UX | 11.X | general purpose
SEQ(SP=96-A0%GCD=1-6%ISR=A2-AC%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NNSW0NNNT11%O2=M578NNSW0NNNT11%O3=M280W0NNNT11%O4=M218NNSW0NNNT11%O5=M218NNSW0NNNT11%O6=M109NNSNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M5B4NNSW0N%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=E44A4E43%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=EA6C967D%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=EA6C967D%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# HP-UX B.11.11 U 9000/785 2015845248 unlimited-user license
Fingerprint HP HP-UX B.11.11
Class HP | HP-UX | 11.X | general purpose
SEQ(SP=FC-10A%GCD=1-6%ISR=104-110%TI=I%II=I%SS=S%TS=7)
OPS(O1=M564NNSW0NNNT11%O2=M564NNSW0NNNT11%O3=M280W0NNNT11%O4=M218NNSW0NNNT11%O5=M218NNSW0NNNT11%O6=M109NNSNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M564NNSW0N%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=80%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=100%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=O%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# HP-UX hostname B.11.23 U 9000/800 3724842035 unlimited-user license
Fingerprint HP HP-UX B.11.23
Class HP | HP-UX | 11.X | general purpose
SEQ(SP=81-8B%GCD=1-6%ISR=96-A0%TI=I%II=I%SS=O|S%TS=7)
OPS(O1=M5B4NNSW0NNNT11%O2=M578NNSW0NNNT11%O3=M280W0NNNT11%O4=M218NNSW0NNNT11%O5=M218NNSW0NNNT11%O6=M109NNSNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=8000%O=M5B4NNSW0N%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=8000%S=O%A=O|S+%F=AS%O=M109NNSW0NNNT11%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=76FB|76FE|7701|7704|7707%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# HP-UX B.11.23 U ia64 1913913181 unlimited-user license
Fingerprint HP HP-UX B.11.23
Class HP | HP-UX | 11.X | general purpose
SEQ(SP=FB-105%GCD=1-6%ISR=101-10B%TI=I|RD%II=I%SS=S%TS=7)
OPS(O1=M564NNSW0NNNT11%O2=M564NNSW0NNNT11%O3=M280W0NNNT11%O4=M218NNSW0NNNT11%O5=M218NNSW0NNNT11%O6=M109NNSNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M564NNSW0N%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=80%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=100%TG=FF%W=100%S=A+%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=100%TG=FF%W=400%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=O%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=FFFF%S=A+%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# HP-UX B.11.31 U ia64
Fingerprint HP HP-UX B.11.31
Class HP | HP-UX | 11.X | general purpose
SEQ(SP=EB-107%GCD=1-6%ISR=EE-106%TI=I%II=I%SS=S%TS=7)
OPS(O1=M564NNSW0NNNT11%O2=M564NNSW0NNNT11%O3=M280W0NNNT11%O4=M218NNSW0NNNT11%O5=M218NNSW0NNNT11%O6=M109NNSNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M564NNSW0N%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=O%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=N)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# HP-UX B.11.31 U ia64
Fingerprint HP HP-UX B.11.31
Class HP | HP-UX | 11.X | general purpose
SEQ(SP=69-A7%GCD=1-6%ISR=95-AB%TI=I%II=I%SS=S%TS=7)
OPS(O1=M514NNSW0NNNT11%O2=M514NNSW0NNNT11%O3=M280W0NNNT11%O4=M218NNSW0NNNT11%O5=M218NNSW0NNNT11%O6=M109NNSNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M514NNSW0N%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=E44A4E43%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=8000%S=O%A=S+%F=AS%O=M109NNSW0NNNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=E44A4E43%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=EA6C967D%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=EA6C967D%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# HP-UX B.11.31 U ia64 2867251542 unlimited-user license
# HP-UX B.11.31 U 9000/800 3454442876 unlimited-user license
Fingerprint HP HP-UX B.11.31
Class HP | HP-UX | 11.X | general purpose
SEQ(SP=FB-107%GCD=1-6%ISR=100-112%TI=I%CI=RD|RI%II=I%SS=S%TS=7)
OPS(O1=M5B4NNSW0NNNT11%O2=M578NNSW0NNNT11%O3=M280W0NNNT11%O4=M218NNSW0NNNT11%O5=M218NNSW0NNNT11%O6=M109NNSNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M5B4NNSW0N%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=E44A4E43%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=8000%S=O%A=O|S+%F=AS%O=M109NNSW0NNNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=E44A4E43%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=EA6C967D%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=EA6C967D%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# HP-UX B.11.00 C 9000/800 71977 32-user license
# HP-UX B.11.23 U ia64 3431083894 unlimited-user license
# HP-UX B.11.23 U ia64 3431083894 unlimited-user license
Fingerprint HP-UX B.11.00 - B.11.23
Class HP | HP-UX | 11.X | general purpose
SEQ(SP=92-A0%GCD=1-6%ISR=9D-AB%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NNSW0NNNT11%O2=M578NNSW0NNNT11%O3=M280W0NNNT11%O4=M218NNSW0NNNT11%O5=M218NNSW0NNNT11%O6=M109NNSNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M5B4NNSW0N%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=E44A4E43%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=EA6C967D%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# HP-UX B.11.11 U 9000/800 3684009682 unlimited-user license
Fingerprint HP-UX B.11.11
Class HP | HP-UX | 11.X | general purpose
SEQ(SP=97-A1%GCD=1-6%ISR=9B-A5%TI=I%II=I%SS=S%TS=7)
OPS(O1=M218NNSW0NNNT11%O2=M218NNSW0NNNT11%O3=M218W0NNNT11%O4=M218NNSW0NNNT11%O5=M218NNSW0NNNT11%O6=M109NNSNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=N%T=3F%TG=40%W=8000%O=M218NNSW0N%CC=N%Q=)
T1(R=Y%DF=N%T=3F%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3F%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=E44A4E43%Q=)
T3(R=Y%DF=N%T=3F%TG=40%W=8000%S=O%A=S+%F=AS%O=M109NNSW0NNNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3F%TG=40%W=0%S=A%A=Z%F=R%O=%RD=E44A4E43%Q=)
T5(R=Y%DF=N%T=3F%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=Y%T=3F%TG=40%W=0%S=A%A=Z%F=R%O=%RD=EA6C967D%Q=)
T7(R=Y%DF=N%T=3F%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=EA6C967D%Q=)
U1(DF=N%T=FE%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# HP-UX B.11.11 U 9000/800 4165063165 unlimited-user license
Fingerprint HP-UX B.11.11
Class HP | HP-UX | 11.X | general purpose
SEQ(SP=95-B9%GCD=1-6%ISR=A9-B3%TI=I%II=I%SS=S%TS=8)
OPS(O1=M5B4NNSW0NNNT11%O2=M578NNSW0NNNT11%O3=M280W0NNNT11%O4=M218NNSW0NNNT11%O5=M218NNSW0NNNT11%O6=M109NNSNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M5B4NNSW0N%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=E44A4E43%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=8000%S=O%A=S+%F=AS%O=M109NNSW0NNNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=E44A4E43%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=EA6C967D%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=EA6C967D%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# HP-UX B.11.31 U ia64
Fingerprint HP-UX B.11.31
Class HP | HP-UX | 11.X | general purpose
SEQ(SP=90-B4%GCD=1-6%ISR=99-B5%TI=I%CI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NNSW2NNNT11%O2=M578NNSW2NNNT11%O3=M280W2NNNT11%O4=M218NNSW2NNNT11%O5=M218NNSW2NNNT11%O6=M109NNSNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NNSW2N%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=E44A4E43%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NNSW2NNNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=E44A4E43%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=EA6C967D%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=EA6C967D%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# HP-UX B.11.31 U ia64
Fingerprint HP-UX B.11.31
Class HP | HP-UX | 11.X | general purpose
SEQ(SP=8D-BB%GCD=1-6%ISR=9F-B1%TI=I%CI=RD%II=I%SS=S%TS=7)
OPS(O1=M5B4NNSW2NNNT11%O2=M578NNSW2NNNT11%O3=M280W2NNNT11%O4=M218NNSW2NNNT11%O5=M218NNSW2NNNT11%O6=M109NNSNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NNSW2N%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=E44A4E43%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NNSW2NNNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=E44A4E43%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=BD1AB510%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=EA6C967D%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=EA6C967D%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# iLO 3 firmware version 1.15 on HP ProLiant DL360G7
Fingerprint HP iLO 3 remote management interface
Class HP | iLO | 3.X | remote management
SEQ(SP=F0-FA%GCD=1-6%ISR=EE-F8%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=8218%W2=8220%W3=8204%W4=8218%W5=80F4%W6=807A)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=832C%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Management Interface - iLO = integrated LightsOut (LightsOut 100i Standard, HP Proliant DL 140 G3)
Fingerprint HP iLO 100i Standard remote management interface
Class HP | iLO || remote management
SEQ(SP=8B-95%GCD=1-6%ISR=98-A2%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=800%W2=800%W3=800%W4=800%W5=800%W6=800)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=800%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=Z)

# HP Integrated Lights Out II
# HP Remote Insight Lights-Out Edition II
Fingerprint HP iLO 2 remote management interface
Class HP | iLO || remote management
SEQ(SP=0-35%GCD=1-6|68|D0|138|1A0|208%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3%O=%CC=N%Q=U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=80%S=A%A=Z%F=R%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=100%S=A%A=Z%F=R%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=400%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# HP Remote Insight Lights-Out Edition II
Fingerprint HP iLO 2 remote management interface
Class HP | iLO || remote management
SEQ(SP=10-1C%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=1|2)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=Y%T=3B-45%TG=40%CD=S)

# ProLiant BL460c G1, iLO 2 Firmware Version: 1.50 03/12/2008
# iLO-2 embedded management processor
# HP iLO 2 version 1.70
# iLO 2, Ver. 1.77, 04/23/2009
# HP ProLiant DL370G6 iLO 2
Fingerprint HP iLO 2 remote management interface
Class HP | iLO || remote management
SEQ(SP=F8-10C%GCD=1-6%ISR=FB-113%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2DA0%W2=2DA0%W3=2DA0%W4=2DA0%W5=2DA0%W6=2DA0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3%O=%CC=N%Q=U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=80%S=A%A=Z%F=R%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=100%S=A%A=Z%F=R%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=400%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# HP iLO2, Firmware Version 1.70 Dec 02 2008 (BL460C)
Fingerprint HP iLO 2 remote management interface
Class HP | iLO || remote management
SEQ(SP=FF-109%GCD=1-6%ISR=103-10D%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2DA0%W2=2DA0%W3=2DA0%W4=2DA0%W5=2DA0%W6=2DA0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3%O=%CC=N%Q=U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=80%S=A%A=Z%F=R%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=100%S=A%A=Z%F=R%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=400%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=N)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# version 2.0 of the HP/compaq iLO 2 firmware.
Fingerprint HP iLO 2 remote management interface version 2.0
Class HP | iLO || remote management
SEQ(SP=F6-10C%GCD=1-6%ISR=105-111%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2DA0%W2=2DA0%W3=2DA0%W4=2DA0%W5=2DA0%W6=2DA0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3%O=%CC=N%Q=U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=400%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# "HP Integrated Lights-Out", only iLO, not iLO2
# "HP Integrated Lights-Out 2". This is version 2 of the HP iLO remote management product.
# iLO card on HP Proliant DL580-G2
# iLO Advanced, iLO Firmware Version: 1.82
Fingerprint HP iLO or iLO 2 remote management interface
Class HP | iLO || remote management
SEQ(SP=0-5%GCD=64|C8|12C|190|1F4%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3%O=%CC=N%Q=U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=80%S=A%A=Z%F=R%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=100%S=A%A=Z%F=R%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=400%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# HP DL320 iLO2 interface
Fingerprint HP ProLiant DL320 iLO 2 remote management interface
Class HP | iLO || remote management
SEQ(SP=B-15%GCD=1-6%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3%O=%CC=N%Q=U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=100%S=A%A=Z%F=R%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=400%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# HP Integrated Lights Out (for HP Proliant DL 320s)
# The ILO from a HP Proliant ML310 G3
Fingerprint HP ProLiant DL320s or ML310 iLO remote management interface
Class HP | iLO || remote management
SEQ(SP=FE-10C%GCD=1-6%ISR=FF-111%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3%O=%CC=N%Q=U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=80%S=A%A=Z%F=R%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=100%S=A%A=Z%F=R%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=400%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# iLO Firmware 1.82 on a Proliant ML350 G4p System ROM D19 08/19/2005
Fingerprint HP ProLiant ML350 iLO remote management interface
Class HP | iLO || remote management
SEQ(R=N)
OPS(R=N)
WIN(R=N)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3%O=%CC=N%Q=U)
T1(R=N)
T2(R=Y%DF=N%T=3B-45%TG=40%W=80%S=A%A=Z%F=R%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=100%S=A%A=Z%F=R%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=400%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# HPe3000a500 Mini computer running HP MPE/iX Version 7.5
Fingerprint HP MPE/iX 7.5
Class HP | MPE/iX | 7.X | general purpose
SEQ(SP=C-16%GCD=1-6%ISR=32-3C%II=RI%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=6000%W2=6000%W3=6000%W4=6000%W5=6000%W6=6000)
ECN(R=Y%DF=N%T=C3-CD%TG=FF%W=6000%O=|M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=C3-CD%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=C3-CD%TG=FF%W=6000%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=Y%T=C3-CD%TG=FF%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=C3-CD%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=C3-CD%TG=FF%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=C3-CD%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=C3-CD%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=C3-CD%TG=FF%CD=S)

# Tandem Guardian. NonStop OSS. It is an HP TANDEM of some sort.
Fingerprint HP NonStop OS
Class HP | NonStop OS || general purpose
SEQ(SP=8F-9D%GCD=1-6%ISR=95-9F%CI=RD%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2238%W2=20D0%W3=2080%W4=2000%W5=2180%W6=2017)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2238%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=2017%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=F8-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=F8-104%TG=FF%CD=S)

# VAX/VMS V6.1  on node <redacted>  20-JUL-2008 08:17:41.30   Uptime  0 00:27:01
Fingerprint HP OpenVMS 6.1
Class HP | OpenVMS | 6.X | general purpose
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B0W0N%O2=M5B0W0N%O3=M5B0W0N%O4=M5B0W0N%O5=M5B0W0N%O6=M5B0)
WIN(W1=BB8%W2=BB8%W3=BB8%W4=BB8%W5=BB8%W6=BB8)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=BB8%O=M5B0W0N%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=BB8%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=BB8%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenVMS V7.2  on node <Redacted>  20-JUN-2008 07:27:46.55  Uptime  0 00:40:51
Fingerprint HP OpenVMS 7.2
Class HP | OpenVMS | 7.X | general purpose
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=832C%W2=8340%W3=8200%W4=8000%W5=81D0%W6=805C)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=832C%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=805C%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# TCP/IP Services for OpenVMS Alpha Version V5.1 - ECO 5 on a DEC 3000 running OpenVMS 7.2
Fingerprint HP OpenVMS 7.2
Class HP | OpenVMS | 7.X | general purpose
SEQ(SP=92-9C%GCD=1-6%ISR=97-A1%TI=I%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=111C%W2=1068%W3=C80%W4=BB8%W5=C90%W6=C6C)
ECN(R=Y%DF=N%T=3C%TG=40%W=111C%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=C6C%S=O%A=O|S+%F=AS%O=M5B4NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=3C%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3C%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3C%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3C%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# OpenVMS v7.2-1
Fingerprint HP OpenVMS 7.2-1
Class HP | OpenVMS | 7.X | general purpose
SEQ(SP=8C-AA%GCD=1-6%ISR=97-A1%II=I%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=4470%W2=41A0%W3=4100%W4=4000%W5=40E8%W6=402E)
ECN(R=Y%DF=N%T=3C%TG=40%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=402E%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# OpenVMS/VAX V7.3
Fingerprint HP OpenVMS 7.3
Class HP | OpenVMS | 7.X | general purpose
SEQ(SP=DD-E7%GCD=10|20|30|40|50%ISR=109-113%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=F000%W2=F000%W3=F000%W4=F000%W5=F000%W6=F000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=F000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=F000%S=O%A=O|S+%F=AS%O=M5B4NW0%RD=0%Q=)
T4(R=Y%DF=N|Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N|Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N|Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N|Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# OpenVMS 7.3 VAX
Fingerprint HP OpenVMS 7.3
Class HP | OpenVMS | 7.X | general purpose
SEQ(SP=5C-66%GCD=40|80|C0|100|140%ISR=97-A1%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=F000%W2=F000%W3=F000%W4=F000%W5=F000%W6=F000)
ECN(R=Y%DF=N%T=3C%TG=40%W=F000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=F000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# OpenVMS 7.3 running MultiNet 5.2 TCP/IP Services
# HP OpenVMS Industry Standard 64 Operating System, Version V8.3
Fingerprint HP OpenVMS 7.3 - 8.3
Class HP | OpenVMS | 7.X | general purpose
Class HP | OpenVMS | 8.X | general purpose
SEQ(SP=E9-10B%GCD=1-6%ISR=102-112%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=1800%W2=1800%W3=1800%W4=1800%W5=1800%W6=1800)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1800%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1800%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenVMS 7.3-1 Hobbyist with telnet, ftp and nfs. Hardware: Alpha ES40.
Fingerprint HP OpenVMS 7.3-1
Class HP | OpenVMS | 7.X | general purpose
SEQ(SP=D5-EF%GCD=10|20|30|40|50%ISR=106-110%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=F000%W2=F000%W3=F000%W4=F000%W5=F000%W6=F000)
ECN(R=Y%DF=N%T=3C%TG=40%W=F000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=F000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# OpenVMS Alpha 7.3-1
Fingerprint HP OpenVMS 7.3-1
Class HP | OpenVMS | 7.X | general purpose
SEQ(SP=DF-E9%GCD=10|20|30|40|50%ISR=108-112%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=F000%W2=F000%W3=F000%W4=F000%W5=F000%W6=F000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=F000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N|Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# OpenVMS (TM) Alpha Operating System, Version V7.3-2
Fingerprint HP OpenVMS 7.3-2
Class HP | OpenVMS | 7.X | general purpose
SEQ(SP=DC-E6%GCD=10|20|30|40|50%ISR=106-110%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=111C%W2=1068%W3=C80%W4=BB8%W5=C90%W6=C6C)
ECN(R=Y%DF=N%T=3C%TG=40%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=C6C%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# OpenVMS/AXP version 8.2 (TCP/IP V5.5-11)
Fingerprint HP OpenVMS 8.2
Class HP | OpenVMS | 8.X | general purpose
SEQ(SP=DA-E4%GCD=10|20|30|40|50%ISR=107-111%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=F000%W2=F000%W3=F000%W4=F000%W5=F000%W6=F000)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=F000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=F000%S=O%A=S+%F=AS%O=M5B4NW0%RD=0%Q=)
T4(R=Y%DF=N|Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N|Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N|Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N|Y%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# OpenVMS/Alpha V8.3
Fingerprint HP OpenVMS 8.3
Class HP | OpenVMS | 8.X | general purpose
SEQ(SP=F4-FE%GCD=1-6%ISR=F9-103%TI=I|RD%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=F53C%W2=F0A0%W3=F000%W4=F000|F53C%W5=F0C8%W6=F028)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=F53C%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=F028%S=O%A=O|S+%F=AS%O=M5B4NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP OpenVMS Industry Standard 64 Operating System, Version V8.3
Fingerprint HP OpenVMS 8.3
Class HP | OpenVMS | 8.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=108-112%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=111C%W2=1068%W3=C80%W4=BB8%W5=C90%W6=C6C)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=111C%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=C6C%S=O%A=O|S+%F=AS%O=M5B4NW0%RD=0%Q=)
T4(R=Y%DF=N|Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N|Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N|Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N|Y%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# OSF1 V5.1 2650 alpha
Fingerprint HP Tru64 UNIX 5.1 (Alpha)
Class HP | Tru64 UNIX | 5.X | general purpose
SEQ(SP=E2-EC%GCD=10|20|30|40|50|60%ISR=107-111%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=F000%W2=F000%W3=F000%W4=F000%W5=F000%W6=F000)
ECN(R=Y%DF=N%T=3C%TG=40%W=F000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=F000%S=O%A=S+%F=AS%O=M5B4NW0%RD=0%Q=)
T4(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N|Y%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=6401%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=I)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP Tru64 UNIX, OS Version is 5.1A -- this was also known as Compaq Tru64 Unix and DEC Tru64 Unix
Fingerprint HP Tru64 UNIX 5.1A
Class HP | Tru64 UNIX | 5.X | general purpose
SEQ(SP=D3-DD%GCD=10|20|30|40|50%ISR=108-112%II=I%TS=U)
OPS(O1=M58CNW0%O2=M58CNW0%O3=M58CNW0%O4=M58CNW0%O5=M58CNW0%O6=M58C)
WIN(W1=F000%W2=F000%W3=F000%W4=F000%W5=F000%W6=F000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=F000%O=M58CNW0%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=F000%S=O%A=S+%F=AS%O=M58CNW0%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HP Tru64 UNIX V5.1B (Rev. 2650)
Fingerprint HP Tru64 UNIX 5.1B
Class HP | Tru64 UNIX | 5.X | general purpose
SEQ(SP=FB-107%GCD=1-6%ISR=102-10C%II=I%TS=U)
OPS(O1=M5B4NW0NNS%O2=M5B4NW0NNS%O3=M5B4NW0NNS%O4=M5B4NW0NNS%O5=M5B4NW0NNS%O6=M5B4NNS)
WIN(W1=F53C%W2=F0A0%W3=F000%W4=F000%W5=F0C8%W6=F028)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=F53C%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=F028%S=O%A=S+%F=AS%O=M5B4NW0NNS%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# SB5100E-2.3.2.3-SCM00-NOSH
# HP Procurve 2650 Switch Model HP J4899A
Fingerprint HP LaserJet 3600 printer, HP ProCurve 2650 switch, or Motorola SURFboard SB5100E cable modem
Class HP | VxWorks || printer
Class HP | VxWorks || switch
Class Motorola | VxWorks || broadband router
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I|RD%TS=U)
OPS(O1=M200NW0%O2=M200NW0%O3=M200NW0%O4=M200NW0%O5=M200NW0%O6=M200)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# HTC Touch Pro
Fingerprint HTC Touch mobile phone (Windows Mobile 6)
Class HTC | Windows | PocketPC/CE | phone
SEQ(R=N)
OPS(O1=M559NW1NNT00NNS%O2=%O3=%O4=%O5=%O6=)
WIN(W1=FFFF%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N|Y%T=7B-85%TG=80%W=0|FFFF%O=|M559NW1NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=B0%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=Z)

# ZyXel Prestige 623ME-T1 ADSL dual link router
# Huawei SmartAX MT800u-T
# ZyXEL Prestige 2602R-61
# Zyxel Prestige 782R, firmware ZyNOS 2.50(BH.4) | 8/6/2002
# Zyxel 643
Fingerprint ADSL router: Huawei MT800u-T; or ZyXEL Prestige 623ME-T1, 643, 782, or 2602R-61
Class Huawei | embedded || broadband router
Class ZyXEL | ZyNOS | 2.X | broadband router
SEQ(SP=0-31%GCD=1000|2000|3000|4000|5000|A000|14000|1E000|28000|32000|3C000|64000|C8000|12C000|190000|1F4000|258000%ISR=AB-B5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M200%O2=M200%O3=M200%O4=M200%O5=M200%O6=M200)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FE%TG=FF%W=400%O=M200%CC=N%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# Zoom X5 ADSL Modem (CastleNet AS80x branded as a ZoomX5 ADSL Modem)
# ZTE ZXDSL 831 ADSL MODEM
# ADSL/Modem Tenda TED8620R, ** Welcome to Viking **, GlobespanVirata Inc., Software Release VIK-2.1.041001a
# Huawei MT-800 ADSL router.
Fingerprint Huawei MT-800, Tenda TED8620R, Zoom X5, or ZTE ZXDSL 831 ADSL modem
Class Huawei | embedded || broadband router
Class Tenda | embedded || broadband router
Class Zoom | embedded || broadband router
Class ZTE | embedded || broadband router
SEQ(SP=FA-10A%GCD=1-6%ISR=103-10D%TI=I%II=I%SS=S%TS=U)
OPS(O1=M58C%O2=M58C%O3=M58C%O4=M58C%O5=M58C%O6=M58C)
WIN(W1=3E80%W2=3E80%W3=3E80%W4=3E80%W5=3E80%W6=3E80)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3E80%O=M58C%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=3E80%S=O%A=S+%F=AS%O=M58C%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=ARF%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# http://www.huawei.com/mobileweb/en/products/view.do?id=486&pageId=null
Fingerprint Huawei MT880 ADSL modem
Class Huawei | embedded || broadband router
SEQ(SP=103-10D%GCD=1-6%ISR=104-10E%TI=I%TS=U)
OPS(O1=M570%O2=M570%O3=M570%O4=M570%O5=M570%O6=M570)
WIN(W1=3E80%W2=3E80%W3=3E80%W4=3E80%W5=3E80%W6=3E80)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3E80%O=M570%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=ARF%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Huawei MT882 adsl modem router [conexant viking 2+]
Fingerprint Huawei MT882 ADSL modem
Class Huawei | embedded || broadband router
SEQ(SP=FB-10B%GCD=1-6%ISR=106-110%TI=I%II=I%SS=S%TS=U)
OPS(O1=M58C%O2=M58C%O3=M58C%O4=M58C%O5=M58C%O6=M58C)
WIN(W1=3E80%W2=3E80%W3=3E80%W4=3E80%W5=3E80%W6=3E80)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3E80%O=M58C%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=3E80%S=O%A=S+%F=AS%O=M58C%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=ARF%O=%RD=0%Q=)
T6(R=N)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=ARF%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Huawei SmartAX MT800u-T ADSL Router (DSL Version: 3.1.1.4, S/W Version:      V100R002C10B020SP01 Hungary| 2005/06/07)
# Zyxel ES-4024A L3 Ethernet switch V3.60(TV.1)20070301 | 03/01/2007
# Prestige model 650HW-31; UPnP/1.0
Fingerprint Huawei SmartAX MT800u-T ADSL router, ZyXEL ES-4024A switch, or ZyXEL Prestige 650HW ADSL router
Class Huawei | embedded || broadband router
Class ZyXEL | ZyNOS | 3.X | switch
Class ZyXEL | ZyNOS | 3.X | broadband router
SEQ(R=N)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=FE%TG=FF%W=0%O=%CC=Y%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=Z%A=S+%F=AR%RD=0%Q=)
T2(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# Huawei SmartAX MT880
Fingerprint Huawei SmartAX MT880 ADSL modem
Class Huawei | embedded || broadband router
SEQ(SP=7E-88%GCD=1-6%ISR=82-8C%TI=I%II=I%SS=S%TS=U)
OPS(O1=M58C%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=1194%W2=1194%W3=1194%W4=1194%W5=1194%W6=1194)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=1194%O=M58C%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=7B-85%TG=80%W=1194%S=A%A=Z%F=R%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=1194%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=Z%F=R%O=%RD=0%Q=)
U1(DF=N%T=96-A0%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7B-85%TG=80%CD=S)

# HUawei AR28 Version AR28-09 8040V300R003B04D040SP14 (COMWAREV300R002B62D014), RELEASE SOFTWARE
Fingerprint Huawei AR 28 router
Class Huawei | embedded || router
SEQ(SP=FA-10E%GCD=1-6%ISR=101-10F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M58C%O2=M58C%O3=M58C%O4=M58C%O5=M58C%O6=M58C)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2000%O=M58C%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1FC4%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Huawei MA5200
Fingerprint Huawei MA5200 router
Class Huawei | embedded || router
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=96-A0%CI=I|RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2000%O=M5B4%CC=N)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1FC4%S=O%A=O%F=A%RD=0)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Huawei Qwidway S5600 Switch
Fingerprint Huawei Quidway S5600 switch
Class Huawei | embedded || switch
SEQ(SP=102-10C%GCD=1-6%ISR=106-110%TI=I%CI=I%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=N)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# HWg-STE Ethernet thermometer/hygrometer http://www.hw-group.com
Fingerprint HW group HWg-STE Ethernet thermometer
Class HW group | embedded || specialized
SEQ(SP=0-C1%GCD=1-6%ISR=15-95%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M109)
WIN(W1=C90%W2=C90%W3=C90%W4=C90%W5=C90%W6=C90)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=C90%O=M109|M218%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=C90%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Poseidon model 3265 temperature monitor
Fingerprint HW group Poseidon 3265 Ethernet thermometer
Class HW group | embedded || specialized
SEQ(SP=0-5%GCD=1-6%ISR=15-1F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M109|M5B4%O2=M109|M578%O3=M109|M280%O4=M109|M280%O5=M109|M218%O6=M109)
WIN(W1=C90%W2=C90%W3=C90%W4=C90%W5=C90%W6=C90)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=C90%O=M109%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=C90%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# AIX 3 4 001120814C00
Fingerprint AIX 4.3
Class IBM | AIX | 4.X | general purpose
SEQ(SP=FE-108%GCD=1-6%ISR=107-111%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3C%TG=40%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX Version 4.2
Fingerprint IBM AIX 4.2
Class IBM | AIX | 4.X | general purpose
SEQ(SP=EA-F4%GCD=1-6%ISR=108-112%TI=I%II=I%SS=S%TS=U)
OPS(O1=M200%O2=M200%O3=M200%O4=M200%O5=M200%O6=M200)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=3F25)
ECN(R=Y%DF=N%T=3C%TG=40%W=4000%O=M200%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3C%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 3 4
# AIX 3 4 00C5D2534C00
Fingerprint IBM AIX 4.3
Class IBM | AIX | 4.X | general purpose
SEQ(SP=FC-10A%GCD=1-6%ISR=106-114%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=3EBC%W2=3C28%W3=3E80%W4=4000%W5=3ED0%W6=3F25)
ECN(R=Y%DF=N%T=3C%TG=40%W=3EBC%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3C%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 3 4 00052629C000, oslevel=4.3.3.0, Maintenance Level=11
Fingerprint IBM AIX 4.3
Class IBM | AIX | 4.X | general purpose
SEQ(SP=FF-109%GCD=1-6%ISR=F9-103%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5AC%O2=M5AC%O3=M5AC%O4=M5AC%O5=M5AC%O6=M5AC)
WIN(W1=3E64%W2=3C28%W3=3E80%W4=4000%W5=3ED0%W6=3F25)
ECN(R=Y%DF=Y%T=38-42%TG=40%W=3E64%O=M5AC%CC=N%Q=)
T1(R=Y%DF=Y%T=38-42%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=38-42%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=38-42%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=38-42%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=38-42%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# AIX 3 4 000284354C00, IBM RS/6000, AIX 4.3.3.0
Fingerprint IBM AIX 4.3
Class IBM | AIX | 4.X | general purpose
SEQ(SP=102-10C%GCD=1-6%ISR=102-10C%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=3EBC%W2=3C28%W3=3E80%W4=4000%W5=3ED0%W6=3F25)
ECN(R=Y%DF=N%T=3C%TG=40%W=3EBC%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3C%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 4.3.2 on RS/6000
Fingerprint IBM AIX 4.3.2 on RS/6000
Class IBM | AIX | 4.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=107-111%TI=I%II=I%SS=S%TS=U)
OPS(O1=M200%O2=M200%O3=M200%O4=M200%O5=M200%O6=M200)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=3F25)
ECN(R=Y%DF=N%T=3C%TG=40%W=4000%O=M200%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3C%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 3 4 000E41854C00
# AIX 3 4 004235974C00
Fingerprint IBM AIX AIX 4.3
Class IBM | AIX | 4.X | general purpose
SEQ(SP=102-10C%GCD=1-6%ISR=103-10D%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=3EBC%W2=3C28%W3=3E80%W4=4000%W5=3ED0%W6=3F25)
ECN(R=Y%DF=Y%T=3C%TG=40%W=3EBC%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3C%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX REMOVEDHOSTNAME 1 5 (aix 5.1)
Fingerprint IBM AIX 5.1
Class IBM | AIX | 5.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=108-112%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=832C%W2=8340%W3=8200%W4=8000%W5=81D0%W6=805C)
ECN(R=Y%DF=Y%T=3C%TG=40%W=832C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3C%TG=40%W=805C%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=8000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IBM AIX 5.1.0.0
# AIX 1 5, This is an IBM RS/6000, 7030-3AT running AIX 5.1L.
# AIX 2 5 5.2.0.0 IBM,7026-H70
# AIX Version 05.02.0000.0030
Fingerprint IBM AIX 5.1 or 5.2
Class IBM | AIX | 5.X | general purpose
SEQ(SP=F7-10C%GCD=1-6%ISR=F9-111%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4470%W2=41A0%W3=4100%W4=4000%W5=40E8%W6=402E)
ECN(R=Y%DF=N%T=3C%TG=40%W=4470%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=402E%S=O%A=O|S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=4000%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX s1421a 2 5 000F745C4C00
Fingerprint IBM AIX 5.2
Class IBM | AIX | 5.X | general purpose
SEQ(SP=102-10C%GCD=1-6%ISR=106-110%TI=RD%II=I%TS=1|2)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=FE88%W2=FED4%W3=FFFF%W4=FFC0|FFFF%W5=FFDC%W6=FFF7)
ECN(R=Y%DF=N%T=3C%TG=40%W=FFFF%O=M5B4NW1%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=FFF7%S=O%A=O|S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 2 5 0050AA7A4C00
Fingerprint IBM AIX 5.2
Class IBM | AIX | 5.X | general purpose
SEQ(SP=101-10B%GCD=1-6%ISR=104-10E%TI=I%II=I%SS=O|S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4470%W2=41A0%W3=4100%W4=4000%W5=40E8%W6=402E)
ECN(R=Y%DF=Y%T=3C%TG=40%W=4470%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3C%TG=40%W=402E%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 2 5 0057256F4C00, oslevel=5.2.0.0, Maintenance Level=08
Fingerprint IBM AIX 5.2
Class IBM | AIX | 5.X | general purpose
SEQ(SP=101-10B%GCD=1-6%ISR=105-10F%II=I%TS=1)
OPS(O1=M5B4NW2NNT11%O2=M5B4NW3NNT11%O3=M5B4NW3NNT11%O4=M5B4NW2NNT11%O5=M5B4NW3NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3C%TG=40%W=FFFF%O=M5B4NW3%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW2NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 2 5 00589A8A4C00
Fingerprint IBM AIX 5.2
Class IBM | AIX | 5.X | general purpose
SEQ(SP=FF-109%GCD=1-6%ISR=107-111%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=FE88%W2=FED4%W3=FF20%W4=FE88%W5=FFDC%W6=FFF7)
ECN(R=Y%DF=N%T=3C%TG=40%W=FFFF%O=M5B4NW1%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=FFF7%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 2 5 00573F3A4C00
Fingerprint IBM AIX 5.2
Class IBM | AIX | 5.X | general purpose
SEQ(SP=FF-109%GCD=1-6%ISR=108-112%II=I%TS=1)
OPS(O1=M5B4NW0NNT11NNS%O2=M5B4NW0NNT11NNS%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11NNS%O5=M5B4NW0NNT11NNS%O6=M5B4NNT11NNS)
WIN(W1=FE88%W2=FED4%W3=FF20%W4=FE88%W5=FFDC%W6=FFF7)
ECN(R=Y%DF=N%T=3C%TG=40%W=FFFF%O=M5B4NW1NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=FFF7%S=O%A=O|S+%F=AS%O=M5B4NW0NNT11NNS%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 2 5 0050211A4C00
Fingerprint IBM AIX 5.2
Class IBM | AIX | 5.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=103-10D%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3C%TG=40%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3C%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=FFFF%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 2 5 00001E6ED100
# AIX 2 5 000BBAFE4C00
Fingerprint IBM AIX 5.2
Class IBM | AIX | 5.X | general purpose
SEQ(SP=101-10B%GCD=1-6%ISR=108-112%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3C%TG=40%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3C%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 2 5 00CEDA6E4C00
Fingerprint IBM AIX 5.2
Class IBM | AIX | 5.X | general purpose
SEQ(SP=101-10B%GCD=1-6%ISR=105-10F%TI=RI%CI=RI%II=RI%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3C%TG=40%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 2 5 004C2B9A4C00 5200-01 (AIX 5.2 ML 01)
Fingerprint IBM AIX 5.2 ML 1
Class IBM | AIX | 5.X | general purpose
SEQ(SP=FF-109%GCD=1-6%ISR=101-10B%II=I%TS=1)
OPS(O1=M5B4NW3NNT11%O2=M5B4NW4NNT11%O3=M5B4NW4NNT11%O4=M5B4NW3NNT11%O5=M5B4NW4NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3C%TG=40%W=FFFF%O=M5B4NW4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW3NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IBM AIX 5.2 on Power5
# IBM AIX 5.2 oslevel 3 on RS/6000
Fingerprint IBM AIX 5.2 on Power5
Class IBM | AIX | 5.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=104-10E%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3C%TG=40%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IBM AIX 5.2.0.0 Maintenance Level 2 on F50
Fingerprint IBM AIX 5.2.0.0 Maintenance Level 2
Class IBM | AIX | 5.X | general purpose
SEQ(SP=F6-106%GCD=1-6%ISR=100-10A%II=I%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4470%W2=41A0%W3=4100%W4=4000%W5=40E8%W6=402E)
ECN(R=Y%DF=Y%T=3C%TG=40%W=4470%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3C%TG=40%W=402E%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IBM AIX 5.3 TL-05 SP3
# IBM AIX 5.3 (Maint. Pack 5) on RS/6000
# IBM Power5 P570 running AIX 5.3 64bit [uname -a: AIX 3 5 00CF679E4C00]
# AIX 3 5 00CE39AB4C00
Fingerprint IBM AIX 5.3
Class IBM | AIX | 5.X | general purpose
SEQ(SP=F9-109%GCD=1-6%ISR=FF-111%II=I%TS=1)
OPS(O1=M5B4NW2NNT11%O2=M5B4NW3NNT11%O3=M5B4NW3NNT11%O4=M5B4NW2NNT11%O5=M5B4NW3NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3C%TG=40%W=FFFF%O=M5B4NW3%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3C%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M5B4NW2NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 3 5
Fingerprint IBM AIX 5.3
Class IBM | AIX | 5.X | general purpose
SEQ(SP=FA-104%GCD=1-6%ISR=106-110%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=FE88%W2=FED4%W3=FF20%W4=FE88%W5=FFDC%W6=FFF7)
ECN(R=Y%DF=Y%T=3C%TG=40%W=FFFF%O=M5B4NW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 3 5 000BBF5F4C00
Fingerprint IBM AIX 5.3
Class IBM | AIX | 5.X | general purpose
SEQ(SP=FF-109%GCD=1-6%ISR=104-10E%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4470%W2=41A0%W3=4100%W4=4000%W5=40E8%W6=402E)
ECN(R=Y%DF=N%T=3C%TG=40%W=4470%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=402E%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 3 5 000007544C00 AIX
Fingerprint IBM AIX 5.3
Class IBM | AIX | 5.X | general purpose
SEQ(SP=FB-105%GCD=1-6%ISR=106-110%TI=I%II=I%SS=S%TS=1|2)
OPS(O1=M5B4NW4NNT11%O2=M5B4NW4NNT11%O3=M5B4NW4NNT11%O4=M5B4NW4NNT11%O5=M5B4NW4NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3C%TG=40%W=FFFF%O=M5B4NW4%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3C%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW4NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IBM AIX 3 5 00088392D700
# AIX 3 5
Fingerprint IBM AIX 5.3
Class IBM | AIX | 5.X | general purpose
SEQ(SP=FD-107%GCD=1-6%ISR=105-10F%TI=I|RD%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=FE88%W2=FED4%W3=FF20%W4=FE88%W5=FFDC%W6=FFF7)
ECN(R=Y%DF=Y%T=3C%TG=40%W=FFFF%O=M5B4NW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3C%TG=40%W=FFF7%S=O%A=O|S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 3 5 00042870D700, oslevel -s: 5300-06-03-0732
Fingerprint IBM AIX 5.3
Class IBM | AIX | 5.X | general purpose
SEQ(SP=F9-103%GCD=1-6%ISR=101-10B%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3C%TG=40%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 3 5 00CF77014C00
Fingerprint IBM AIX 5.3
Class IBM | AIX | 5.X | general purpose
SEQ(SP=101-10B%GCD=1-6%ISR=107-111%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW2NNT11%O2=M5B4NW3NNT11%O3=M5B4NW3NNT11%O4=M5B4NW2NNT11%O5=M5B4NW3NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3C%TG=40%W=FFFF%O=M5B4NW3%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW2NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 3 5 00C638AD4C00
Fingerprint IBM AIX 5.3
Class IBM | AIX | 5.X | general purpose
SEQ(SP=FB-105%GCD=1-6%ISR=104-10E%II=I%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3C%TG=40%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3C%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 3 5
Fingerprint IBM AIX 5.3
Class IBM | AIX | 5.X | general purpose
SEQ(SP=FE-108%GCD=1-6%ISR=107-111%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=FE88%W2=FED4%W3=FF20%W4=FE88%W5=FFDC%W6=FFF7)
ECN(R=Y%DF=Y%T=3C%TG=40%W=FFFF%O=M5B4NW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3C%TG=40%W=FFF7%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 3 5
# AIX 1 6 00C33E0A4C00
Fingerprint IBM AIX 5.3 - 6.1
Class IBM | AIX | 5.X | general purpose
Class IBM | AIX | 6.X | general purpose
SEQ(SP=FD-107%GCD=1-6%ISR=100-10A%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3C%TG=40%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IBM AIX 5.3 (ML05) - 5300-05-04 - on p-Series (Processor Type: PowerPC_POWER5)
# IBM AIX 5.3 (Maintenance Pack 5) on RS/6000
# AIX 5.3 64-bit (5300-04) / IBM pSeries P5 550 (9113-550)
# IBM AIX 5.3 (Technology Level 4) on RS/6000
# AIX 5.3 ML 04
# AIX-RS/6000, version: 5.4.3.0
# AIX 3 5 00CC377F4C00, (Technology Level 7 , Service Pack 2)
# AIX 1 6 00075EF1D600
Fingerprint IBM AIX 5.3 - 6.1
Class IBM | AIX | 5.X | general purpose
SEQ(SP=F2-10A%GCD=1-6%ISR=FB-112%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3C%TG=40%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3C%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 5L V5.3 (4/2008) - freshly installed, AIX 3 5 00CFFBA14C00
# IBM AIX 6.1.0.0
# AIX 3 5 00CC377F4C00 AIX 5.3 Technology Level 9 Service Pack 1
# IBM VIOS 2.1
Fingerprint IBM AIX 5.3 - 6.1
Class IBM | AIX | 5.X | general purpose
Class IBM | AIX | 6.X | general purpose
SEQ(SP=F7-109%GCD=1-6%ISR=100-10F%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3C%TG=40%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3C%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IBM Aix 5.3 (on 44p Workstation)
# IBM AIX 5.3 ML05 SP04 (POWER5)
# AIX 5.3 IBM B50
# IBM AIX 5300-05 on p570
# IBM F50 running AIX 5.3 32-bit 5300-05
# AIX 6.100
Fingerprint IBM AIX 5.3 - 6.1
Class IBM | AIX | 5.X | general purpose
SEQ(SP=FA-10A%GCD=1-6%ISR=105-10F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4470%W2=41A0%W3=4100%W4=4000%W5=40E8%W6=402E)
ECN(R=Y%DF=Y%T=3C%TG=40%W=4470%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3C%TG=40%W=402E%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 3 5 00C758FE4C00
# 6.1.0.0
# AIX 3 5 00CAEA804C00
# AIX 1 6 00F615DB4C00, IOS version from ioslevel command: 2.1.3.10-FP-23.
Fingerprint IBM AIX 5.3 - 6.1
Class IBM | AIX | 5.X | general purpose
Class IBM | AIX | 6.X | general purpose
SEQ(SP=EE-10A%GCD=1-6%ISR=104-110%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW2NNT11%O2=M5B4NW3NNT11%O3=M5B4NW3NNT11%O4=M5B4NW2NNT11%O5=M5B4NW3NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3C%TG=40%W=FFFF%O=M5B4NW3%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3C%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW2NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX 5.3 ML 4
# IBM PowerPC CHRP Computer
Fingerprint IBM AIX 5.3 ML 4
Class IBM | AIX | 5.X | general purpose
SEQ(SP=E4-EE%GCD=1-6%ISR=100-10A%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3C%TG=40%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3C%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# 5300-04-CSP, AIX 5.3 with SP4, running on a 7026-B80 (Power4)
Fingerprint IBM AIX 5.3 SP4
Class IBM | AIX | 5.X | general purpose
SEQ(SP=102-10C%GCD=1-6%ISR=107-111%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2238%W2=20D0%W3=2080%W4=2000%W5=2180%W6=2017)
ECN(R=Y%DF=Y%T=3C%TG=40%W=2238%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3C%TG=40%W=2017%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# AIX Version 6
Fingerprint IBM AIX 6
Class IBM | AIX | 6.X | general purpose
SEQ(SP=FD-107%GCD=1-6%ISR=104-114%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW2NNT11%O2=M5B4NW3NNT11%O3=M5B4NW3NNT11%O4=M5B4NW2NNT11%O5=M5B4NW3NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3C%TG=40%W=FFFF%O=M5B4NW3%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3C%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW2NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(R=N)

# AIX 1  6  00014AAAD400
Fingerprint IBM AIX 6.1
Class IBM | AIX | 6.X | general purpose
SEQ(SP=102-10C%GCD=1-6%ISR=106-110%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3C%TG=40%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IBM 6400 Printer - version: 7.0.9.6
# Telnet Banner: Network Printer Server Version 7.0.9.6
Fingerprint IBM 6400 Printer (software version 7.0.9.6)
Class IBM | embedded || printer
SEQ(SP=0-15%GCD=1-6%ISR=0-D%TI=I%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M1AE%O5=M218%O6=M109)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=0%O=M578%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=1B-25%TG=20%W=0%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(R=N)

# IBM Infoprint 1140 Ethernet (Firmware Version 54.30.06)
Fingerprint IBM InfoPrint 1140 printer
Class IBM | embedded || printer
SEQ(SP=C4-CE%GCD=1-6%ISR=CC-D6%TI=Z%II=Z%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=5A8%W2=5A8%W3=5A8%W4=5A8%W5=5A8%W6=5A8)
ECN(R=Y%DF=Y%T=FE%TG=FF%W=5B4%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=FE%TG=FF%W=5A8%S=O%A=O|S+%F=A|AS%O=NNT11|M5B4ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FE%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FE%TG=FF%CD=S)

# IBM Websphere DataPower XI50
Fingerprint IBM Websphere DataPower XI50 proxy server
Class IBM | embedded || proxy server
SEQ(SP=C1-CB%GCD=1-6%ISR=C9-D3%TI=Z%II=I%TS=8)
OPS(O1=M5B4ST11NW8%O2=M5B4ST11NW8%O3=M5B4NNT11NW8%O4=M5B4ST11NW8%O5=M5B4ST11NW8%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=C3%TG=FF%W=16D0%O=M5B4NNSNW8%CC=Y%Q=)
T1(R=Y%DF=Y%T=C3%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=C3%TG=FF%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW8%RD=0%Q=)
T4(R=Y%DF=Y%T=C3%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=C3%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=C3%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=C3%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=C3%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=C3%TG=FF%CD=S)

# Model 204, needs c3270 program to access on port 23
# I don't know if this constitutes an OS on its own, but there are no other close matches. --Ed.
Fingerprint IBM Model 204 DBMS
Class IBM | embedded || specialized
SEQ(SP=E7-F1%GCD=1-6%ISR=FD-107%CI=I%TS=A)
OPS(O1=M22F8NW3NNT11%O2=M22F8NW3NNT11%O3=M22F8NW3NNT11%O4=M22F8NW3NNT11%O5=M22F8NW3NNT11%O6=M22F8NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M22F8NW3%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# IBM BladeCenter management module, firmware BRET85L
# HP StorageWorks MSL2024 Tape Library
# IBM TS3100 (3573-TL) Tape Library running Nucleus PLUS on AT91RM9200
# IBM TL3200 Tape Library Management Card
Fingerprint IBM BladeCenter management module (firmware BRET85L), IBM System Storage TS3100/TS3200 Express Model tape library, or HP StorageWorks MSL2024 tape library
Class IBM | embedded || storage-misc
Class IBM | embedded || remote management
Class HP | embedded || storage-misc
SEQ(SP=FB-109%GCD=1-6%ISR=FB-111%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=3E80%W2=3E80%W3=3E80%W4=3E80%W5=3E80%W6=3E80)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3E80%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=3E80%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Data Direct Networks (DDN) storage controller, DCS9900 Fibre Couplet Controller Model CP1, Firmware Version: 5.03C
Fingerprint IBM DCS9900 NAS device
Class IBM | embedded || storage-misc
SEQ(SP=FD-109%GCD=1-6%ISR=104-10E%TI=I%CI=I%II=I%SS=S%TS=6)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N|Y%T=3B-45%TG=40%W=4000%S=O%A=O|S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# IBM DS 4700
Fingerprint IBM System Storage DS4700 NAS device
Class IBM | embedded || storage-misc
SEQ(SP=C6-D0%GCD=1-6%ISR=CA-D4%TI=Z%II=I%TS=A)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# IBM DS4800 storage array, which is a rebadged OEM LSI/Engenio system
Fingerprint ICM DS4800 NAS device
Class IBM | embedded || storage-misc
SEQ(SP=94-9E%GCD=1-6%ISR=9A-A4%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# OS/400 V5R2
Fingerprint IBM i5/OS V5R2
Class IBM | i5/OS | V5 | general purpose
SEQ(SP=AA-B4%GCD=1-6%ISR=AD-B7%TI=RD%TS=A|D)
OPS(O1=M204NW0NNT11|M59CNW0NNT11%O2=M204NW0NNT11|M560NW0NNT11%O3=M204NW0NNT11|M268NW0NNT11%O4=M200NW0NNT11%O5=M200NW0NNT11%O6=MF1NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N|Y%T=3B-45%TG=40%W=2000%O=M210NW0|M5ACNW0%CC=N%Q=)
T1(R=Y%DF=N|Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# i5/OS V5R3
Fingerprint IBM i5/OS V5R3
Class IBM | i5/OS | V5 | general purpose
SEQ(SP=9F-AF%GCD=1-6|8%ISR=AA-BC%TI=I%II=I|RI%SS=S%TS=A)
OPS(O1=M59CNW4NNT11%O2=M560NW4NNT11%O3=M268NW4NNT11%O4=M200NW4NNT11%O5=M200NW4NNT11%O6=MF1NNT11)
WIN(W1=F424%W2=F424%W3=F424%W4=F424%W5=F424%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=F424%O=M5ACNW4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# iSeries 9406-820 Running OS/400 V5R3M0
Fingerprint IBM i5/OS V5R3M0
Class IBM | i5/OS | V5 | general purpose
SEQ(SP=AA-B4%GCD=1-6%ISR=A6-BE%TI=I%II=I%SS=S%TS=A)
OPS(O1=M54CNW1NNT11%O2=M54CNW1NNT11%O3=M268NW1NNT11%O4=M200NW1NNT11%O5=M200NW1NNT11%O6=MF1NNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M564NW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=23-40%TG=40%W=80%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=25-42%TG=40%W=100%S=A%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=23-3B%TG=40%W=400%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=25-31|33-3F%TG=40%W=8000%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=22-38%TG=40%W=FFFF%S=A%A=S+%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# IBM i5/OS V5R4M0 running on an IBM iSeries 520
Fingerprint IBM i5/OS V5R4
Class IBM | i5/OS | V5 | general purpose
SEQ(SP=A4-C6%GCD=1-6|8%ISR=B1-C7%TI=I%II=I%SS=S%TS=A|B)
OPS(O1=M5ACNW0NNT11%O2=M578NW0NNT11%O3=M280NW0NNT11%O4=M5ACNW0NNT11%O5=M218NW0NNT11%O6=M109NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5ACNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# IBM i5/OS Version 5 Release 4
Fingerprint IBM i5/OS V5R4
Class IBM | i5/OS | V5 | general purpose
SEQ(SP=A6-B0%GCD=1-6|8%ISR=AB-B5%TI=I%II=I%SS=S%TS=A)
OPS(O1=M514NW0NNT11%O2=M514NW0NNT11%O3=M280NW0NNT11%O4=M514NW0NNT11%O5=M218NW0NNT11%O6=M109NNT11)
WIN(W1=FB80%W2=FB80%W3=FB80%W4=FB80%W5=FB80%W6=FB80)
ECN(R=Y%DF=Y%T=3A-44%TG=40%W=FB80%O=M514NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3A-44%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3A-44%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3A-44%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3A-44%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3A-44%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3A-44%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3A-44%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3A-44%TG=40%CD=S)

# IBM i5/OS V5r4m0 on an IBM "System i "(formerly known as an "i5", and an "E-Server - i Series", and "AS/400")
# IBM OS/400 V5
# IBM i5/OS V5R4
# System I5 running i5/OS V5R4
# OS400-V6R1
Fingerprint IBM i5/OS V5R4 - V6R1
Class IBM | i5/OS | V5 | general purpose
Class IBM | i5/OS | V6 | general purpose
SEQ(SP=9B-B3%GCD=1-6%ISR=A2-B8%TI=I%II=I%SS=S%TS=A|B)
OPS(O1=M5ACNW0NNT11%O2=M578NW0NNT11%O3=M280NW0NNT11%O4=M5ACNW0NNT11%O5=M218NW0NNT11%O6=M109NNT11)
WIN(W1=2000|FA00%W2=2000|FA00%W3=2000|FA00%W4=2000|FA00%W5=2000|FA00%W6=2000|FA00)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000|FA00%O=M5ACNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# i5/OS V5R4, CUMPTF C6297540, TCP/IP Group PTF 4, running on a iSeries Modell 270, Power4 based
Fingerprint IBM i5/OS V5R4 on an IBM iSeries (PPC)
Class IBM | i5/OS | V5 | general purpose
SEQ(SP=A8-B2%GCD=1-6%ISR=AB-B5%TI=I%II=I%SS=S%TS=A)
OPS(O1=M570NW0NNT11%O2=M570NW0NNT11%O3=M280NW0NNT11%O4=M570NW0NNT11%O5=M218NW0NNT11%O6=M109NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M570NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# IBM i5/OS V6R1
Fingerprint IBM i5/OS V6R1
Class IBM | i5/OS | V6 | general purpose
SEQ(SP=AA-B8%GCD=1-6%ISR=AD-B7%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5ACNW0NNT11%O2=M578NW0NNT11%O3=M280NW0NNT11%O4=M5ACNW0NNT11%O5=M218NW0NNT11%O6=M109NNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M5ACNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# OS/2 Warp 3.0
Fingerprint IBM OS/2 Warp 3.0
Class IBM | OS/2 | 3.X | general purpose
SEQ(SP=D-1F%GCD=3200|6400|9600|C800|FA00%ISR=96-A0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5AA%O2=M5AA%O3=M5AA%O4=M5AA%O5=M5AA%O6=M5AA)
WIN(W1=7000%W2=7000%W3=7000%W4=7000%W5=7000%W6=7000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=7000%O=M5AA%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=7000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=7000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# This is OS/2 with 32-Bit stack.
Fingerprint IBM OS/2 Warp 2.0
Class IBM | OS/2 | 4.X | general purpose
SEQ(CI=I%II=I%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=8000%O=WANM5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=O%A=S+%F=AS%O=WANM109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# OS/2 V4 Warp with Fixpack 15
Fingerprint IBM OS/2 Warp 4.0 (FixPak 15)
Class IBM | OS/2 | 4.X | general purpose
SEQ(SP=8A-9C%GCD=1-6%ISR=90-9A%TI=I|RD%II=I%SS=S%TS=U)
OPS(O1=|M5B4NW0%O2=|M5B4NW0%O3=|M5B4NW0%O4=|M5B4NW0%O5=|M5B4NW0%O6=|M5B4)
WIN(W1=832C%W2=8340%W3=8200%W4=832C%W5=81D0%W6=805C)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=832C%O=|M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=805C%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# IBM os/2 4.50 x86
Fingerprint IBM OS/2 Warp 4.50
Class IBM | OS/2 | 4.X | general purpose
SEQ(SP=8E-9C%GCD=1-6%ISR=92-9C%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=832C%W2=8340%W3=8200%W4=832C%W5=81D0%W6=805C)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=832C%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=805C%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# OS/2 Warp Server for e-business Version 4.52 German
Fingerprint IBM OS/2 Warp Server 4.52
Class IBM | OS/2 | 4.X | general purpose
SEQ(SP=8F-9D%GCD=1-6%ISR=91-9B%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=832C%W2=8340%W3=8200%W4=8000%W5=81D0%W6=805C)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=832C%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=805C%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# IBM OS/390 V2
Fingerprint IBM OS/390 V2
Class IBM | OS/390 | V2 | general purpose
SEQ(SP=76-8C%GCD=1-6%ISR=93-9D%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW3NNT11%O2=M5B4NW3NNT11%O3=M5B4NW3NNT11%O4=M5B4NW3NNT11%O5=M5B4NW3NNT11%O6=M5B4NNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=8000%O=M5B4NW3%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=O%A=S+%F=AS%O=M5B4NW3NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# IBM OS/400, runs System version V4R2M0.
Fingerprint IBM OS/400 V4R2M0
Class IBM | OS/400 | V4 | general purpose
SEQ(SP=84-8E%GCD=1-6%ISR=8A-94%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5AC%O2=M5AC%O3=M5AC%O4=M5AC%O5=M5AC%O6=M5AC)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5AC%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=M5AC%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# IBM OS/400 v4r3 on 720 machine
Fingerprint IBM OS/400 V4R3
Class IBM | OS/400 | V4 | general purpose
SEQ(SP=6F-8D%GCD=1-6%ISR=8D-97%TI=I%II=I|RI%SS=O|S%TS=U)
OPS(O1=M5AC%O2=M5AC%O3=M5AC%O4=M5AC%O5=M5AC%O6=M5AC)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5AC%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=M5AC%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# OS400 v4r3, Hardware platform 740
Fingerprint IBM OS/400 V4R3
Class IBM | OS/400 | V4 | general purpose
SEQ(SP=37-8D%GCD=1-6%ISR=8A-94%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5AC%O2=M5AC%O3=M5AC%O4=M5AC%O5=M5AC%O6=M5AC)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5AC%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=M5AC%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# OS/400 V4R5, CUMPTF 02050
Fingerprint IBM OS/400 V4R5
Class IBM | OS/400 | V4 | general purpose
SEQ(SP=0-5%GCD=1-6%ISR=0-5%TI=I%II=I%SS=S%TS=A)
OPS(O1=M59CNW0NNT11%O2=M560NW0NNT11%O3=M268NW0NNT11%O4=M200NW0NNT11%O5=M200NW0NNT11%O6=MF1NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N|Y%T=3B-45%TG=40%W=2000%O=M5ACNW0%CC=N%Q=)
T1(R=Y%DF=N|Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N|Y%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=MF1NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# AS/400 model 270 with OS/400 V5R1M0
Fingerprint IBM OS/400 V5R1M0
Class IBM | OS/400 | V5 | general purpose
SEQ(SP=A2-B4%GCD=1-6%ISR=AD-B7%TI=I%II=I%SS=S%TS=A)
OPS(O1=M59CNW0NNT11%O2=M560NW0NNT11%O3=M268NW0NNT11%O4=M200NW0NNT11%O5=M200NW0NNT11%O6=MF1NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5ACNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=MF1NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# IBM AS/400 - OS/400 - V5R2M0 L00
# This is specifically for a "V5R3M0 L00" installed release of OS/400.
Fingerprint IBM OS/400 V5R2 - V5R3
Class IBM | OS/400 | V5 | general purpose
SEQ(SP=76-BA%GCD=1-6|10|20|30|40|50%ISR=AE-B8%TI=I%TS=A)
OPS(O1=M59CNW0NNT11%O2=M560NW0NNT11%O3=M268NW0NNT11%O4=M200NW0NNT11%O5=M200NW0NNT11%O6=MF1NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5ACNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=O|S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=O|S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# IBM OS/400 V05R02M00
Fingerprint IBM OS/400 V5R2M0
Class IBM | OS/400 | V5 | general purpose
SEQ(SP=A4-AE%GCD=1-6%ISR=AF-B9%TI=I%II=I%SS=S%TS=A)
OPS(O1=M59CNW0NNT11%O2=M560NW0NNT11%O3=M268NW0NNT11%O4=M200NW0NNT11%O5=M200NW0NNT11%O6=MF1NNT11)
WIN(W1=59C%W2=560%W3=268%W4=200%W5=200%W6=F1)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5AC%O=M5ACNW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0|F1%S=O|Z%A=O|S|S+%F=AR|AS%O=|MF1NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=37-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# IBM OS/400 V5 Release 3 Modification 0
Fingerprint IBM OS/400 V5R3
Class IBM | OS/400 | V5 | general purpose
SEQ(SP=A8-B6%GCD=1-6|8|10|18|20|28%ISR=A6-B8%TI=I%II=I%SS=S%TS=A)
OPS(O1=M59CNW6NNT11%O2=M560NW6NNT11%O3=M268NW6NNT11%O4=M200NW6NNT11%O5=M200NW6NNT11%O6=MF1NNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M5ACNW6%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# V5 R3 of the OS/400
Fingerprint IBM OS/400 V5R3
Class IBM | OS/400 | V5 | general purpose
SEQ(SP=6F-B3%GCD=1-6|10%ISR=AF-B9%TI=I%II=I%SS=S%TS=A)
OPS(O1=M564NW1NNT11%O2=M560NW1NNT11%O3=M268NW1NNT11%O4=M200NW1NNT11%O5=M200NW1NNT11%O6=MF1NNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M570NW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# OS/400 version is V5R3  (other values are V5R4, V6R1)
Fingerprint IBM OS/400 V5R3
Class IBM | OS/400 | V5 | general purpose
SEQ(SP=8A-C8%GCD=1-6%ISR=AD-B7%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M564NW0NNT11%O2=M560NW0NNT11%O3=M268NW0NNT11%O4=M200NW0NNT11%O5=M200NW0NNT11%O6=MF1NNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M570NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# z/OS 1.10
Fingerprint IBM z/OS 1.10
Class IBM | z/OS | 1.10.X | general purpose
SEQ(SP=7F-8B%GCD=1-6%ISR=91-9B%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNT11%O2=M5B4NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=8000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# IBM z/OS 1.4.2
Fingerprint IBM z/OS 1.4.2
Class IBM | z/OS | 1.4.X | general purpose
SEQ(SP=77-A1%GCD=1-6%ISR=96-AA%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5ACNW1NNT11%O2=M5ACNW1NNT11%O3=M5ACNW1NNT11%O4=M5ACNW1NNT11%O5=M5ACNW1NNT11%O6=M5ACNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5ACNW1%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5ACNW1NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# zOS 1.6
Fingerprint IBM z/OS 1.6
Class IBM | z/OS | 1.6.X | general purpose
SEQ(SP=7B-89%GCD=1-6%ISR=93-9D%TI=I%II=I%SS=S%TS=A)
OPS(O1=M22F8NW1NNT11%O2=M22F8NW1NNT11%O3=M22F8NW1NNT11%O4=M22F8NW1NNT11%O5=M22F8NW1NNT11%O6=M22F8NNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=8000%O=M22F8NW1%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=O%A=S+%F=AS%O=M22F8NW1NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# zOS 1.6
Fingerprint IBM z/OS 1.7
Class IBM | z/OS | 1.7.X | general purpose
SEQ(SP=76-8A%GCD=1-6%ISR=95-9F%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5ACNW1NNT11%O2=M5ACNW1NNT11%O3=M5ACNW1NNT11%O4=M5ACNW1NNT11%O5=M5ACNW1NNT11%O6=M5ACNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5ACNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3A-44%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3A-44%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5ACNW1NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3A-44%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3A-44%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3A-44%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3A-44%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3A-44%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3A-44%TG=40%CD=S)

# z/OS 01.08.00
Fingerprint IBM z/OS 01.08.00
Class IBM | z/OS | 1.8.X | general purpose
SEQ(SP=7D-8B%GCD=1-6%ISR=94-9E%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5ACNW4NNT11%O2=M5ACNW4NNT11%O3=M5ACNW4NNT11%O4=M5ACNW4NNT11%O5=M5ACNW4NNT11%O6=M5ACNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5ACNW4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5ACNW4NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# z/OS 1.8.0
Fingerprint IBM z/OS 1.8.0
Class IBM | z/OS | 1.8.X | general purpose
SEQ(SP=7F-89%GCD=1-6%ISR=93-9D%TI=I%II=I%SS=S%TS=A)
OPS(O1=M218NW3NNT11%O2=M218NW3NNT11%O3=M218NW3NNT11%O4=M218NW3NNT11%O5=M218NW3NNT11%O6=M218NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M218NW3%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M218NW3NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# z/OS 1.9.x
Fingerprint IBM z/OS 1.9
Class IBM | z/OS | 1.9.X | general purpose
SEQ(SP=7D-89%GCD=1-6%ISR=91-9B%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNT11%O2=M5B4NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=8000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# IBM z/OS v1r8
Fingerprint IBM z/OS v1r8
Class IBM | z/OS || general purpose
SEQ(SP=89-9B%GCD=1-6%ISR=99-A3%TS=A)
OPS(O1=M5ACNW0NNT11%O2=M5ACNNT11%O3=M5ACNW0NNT11%O4=M5ACNW0NNT11%O5=M5ACNW0NNT11%O6=M5ACNNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=N%T=3A-44%TG=40%W=8000%O=M5ACNW0%CC=N%Q=)
T1(R=Y%DF=N%T=3A-44%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=26-3F%TG=40%W=80%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=24-43%TG=40%W=100%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=30-43%TG=40%W=400%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=N%T=3A-44%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=23-3E%TG=40%W=8000%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=24-34|36-43%TG=40%W=FFFF%S=A%A=S%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=N%T=3A-44%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3A-44%TG=40%CD=S)

# IBM zVM/CMS 4.2 rsu 0402 (TCPIP 430 rsu 402) on z890
Fingerprint IBM z/VM 4.2
Class IBM | z/VM | 4.X | general purpose
SEQ(SP=77-89%GCD=1-6%ISR=93-9D%TS=A)
OPS(O1=M22F8NW0NNT11%O2=M22F8NNT11%O3=M22F8NW0NNT11%O4=M22F8NW0NNT11%O5=M22F8NW0NNT11%O6=M22F8NNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=8000%O=M22F8NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=O%A=S+%F=AS%O=M22F8NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# z/VM 5.2
Fingerprint IBM z/VM 5.2
Class IBM | z/VM | 5.X | general purpose
SEQ(SP=55-79%GCD=64|C8|12C|190|1F4%ISR=8F-A9%TI=I%II=RI%SS=S%TS=U)
OPS(O1=M5B4W1NNNT11%O2=M5B4W1NNNT11%O3=M5B4W1NNNT11%O4=M5B4W1NNNT11%O5=M5B4W1NNNT11%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3C%TG=40%W=2000%O=M5B4W1NNNT10%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=2000%S=O%A=S+%F=AS%O=M5B4W1NNNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=S)

# IBM z/VM
Fingerprint IBM z/VM
Class IBM | z/VM || general purpose
SEQ(SP=68-82%GCD=64|C8|12C|190|1F4%ISR=9B-AF%TI=I%II=RI%SS=O|S%TS=U)
OPS(O1=M5B4W1NNNT11%O2=M5B4W1NNNT11%O3=M5B4W1NNNT11%O4=M5B4W1NNNT11%O5=M5B4W1NNNT11%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3C%TG=40%W=2000%O=M5B4W1NNNT10%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=2000%S=O%A=S+%F=AS%O=M5B4W1NNNT11%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=S)

# iDirect Protocol Processor (customised Red Hat Enterprise Linux ES release 3 (Taroon Update 3))
# This is a part of the iDirect satellite hub system, responsible for processing IP data into the custom layer-2 protocol used to communicate with iDirect Hub Line Cards (HLC) for transmission to a geosynchronous satellite.
Fingerprint iDirect Protocol Processor (Red Hat Enterprise Linux 3)
Class iDirect | Linux | 2.4.X | specialized
SEQ(SP=C5-CF%GCD=1-6%ISR=C9-D3%TI=Z%II=I%TS=7)
OPS(O1=M5B8ST11NW0%O2=M5B8ST11NW0%O3=M5B8NNT11NW0%O4=M5B8ST11NW0%O5=M5B8ST11NW0%O6=M5B8ST11)
WIN(W1=16B0%W2=16B0%W3=16B0%W4=16B0%W5=16B0%W6=16B0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1128%O=M5B8NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16B0%S=O%A=S+%F=AS%O=M5B8ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# IEI Secure Ethernet Gateway Module (SEG-M). Used in IEI HubMax II access control systems.
Fingerprint IEI SEG-M Ethernet-to-serial bridge
Class IEI | embedded || bridge
SEQ(CI=I%II=I%TS=U)
OPS(O1=|M400%O2=%O3=%O4=%O5=|M400%O6=)
WIN(W1=0|7FF%W2=0%W3=0%W4=0%W5=0|7FF%W6=0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=0%CC=N)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O|Z%A=O|S+%F=AR|AS%RD=0)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%RD=0)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%RD=0)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%RD=0)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%RD=0)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%RD=0)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%RD=0)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# IGEL UD3 thin client, runs their IGEL linux, probably with a 2.6 kernel.
Fingerprint IGEL UD3 thin client (Linux 2.6)
Class IGEL | Linux | 2.6.X | terminal
SEQ(SP=C3-CD%GCD=1-6%ISR=CC-D6%TI=Z%II=I%TS=8)
OPS(O1=M570ST11NW5%O2=M570ST11NW5%O3=M570NNT11NW5%O4=M570ST11NW5%O5=M570ST11NW5%O6=M570ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M570NNSNW5%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Infrant ReadyNAS NV NAS Appliance with firmware RAIDiator v3.00c1-p2 [1.00a025]
Fingerprint Infrant ReadyNAS NV NAS device (RAIDiator 3.00)
Class Infrant | RAIDiator | 3.X | storage-misc
SEQ(SP=BC-C6%GCD=1-6%ISR=C6-D0%TI=Z%II=I%TS=7)
OPS(O1=M1ED8ST11NW0%O2=M1ED8ST11NW0%O3=M1ED8NNT11NW0%O4=M1ED8ST11NW0%O5=M1ED8ST11NW0%O6=M1ED8ST11)
WIN(W1=3D98%W2=3D98%W3=3D98%W4=3D98%W5=3D98%W6=3D98)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=3DB0%O=M1ED8NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=3D98%S=O%A=S+%F=AS%O=M1ED8ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# ReadyNAS NV+ RAIDiator 4.1.4 [1.00a042]
Fingerprint Infrant ReadyNAS NV+ NAS device (RAIDiator 4.1.4)
Class Infrant | RAIDiator | 4.X | storage-misc
SEQ(SP=C7-D1%GCD=1-6%ISR=CA-D4%TI=Z%CI=Z%II=I%TS=7)
OPS(O1=M550ST11NW4%O2=M550ST11NW4%O3=M550NNT11NW4%O4=M550ST11NW4%O5=M550ST11NW4%O6=M550ST11)
WIN(W1=1510%W2=1510%W3=1510%W4=1510%W5=1510%W6=1510)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1540%O=M550NNSNW4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1510%S=O%A=O|S+%F=A|AS%O=NNT11|M550ST11NW4%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Inova Solutions Digital Clock, Welcome to OnTime Clock Version 1.2.P
Fingerprint Inova OnTime Clock Version 1.2.P
Class Inova | embedded || specialized
SEQ(SP=FD-107%GCD=1-6%ISR=105-10F%TI=Z%CI=Z%II=RI%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1000%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=Z)

# Intel Express Switch 460T, Firmware v1.00.26
Fingerprint Intel Express 460T switch
Class Intel | embedded || switch
SEQ(SP=0-5%GCD=61A8|C350|124F8|186A0|1E848%ISR=8A-94%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=|U)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Intel 510T managed switch
Fingerprint Intel Express 510T switch
Class Intel | embedded || switch
SEQ(SP=D-1D%GCD=10|20|30|40|50%ISR=4B-55%TI=I%TS=U)
OPS(O1=M58C%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=400%O=M58C%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Intel Express 510T Switch
# Intel Express 550T Routing Switch, firmware 2.76
# Intel Express 520T Routing Switch, firmware 2.76
Fingerprint Intel Express 510T, 520T, or 550T switch
Class Intel | embedded || switch
SEQ(SP=F-19%GCD=10|20|30|40|50%ISR=4B-55%TI=I%TS=U)
OPS(O1=M58C%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=400%O=M58C%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=400%S=O%A=O|S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Interbell IB305 (VoIP phone)
Fingerprint Interbell IB-305 VoIP phone
Class Interbell | embedded || VoIP phone
SEQ(SP=0-16%GCD=FA|1F4|2EE|3E8|4E2|6590|CB20|130B0|19640|1FBD0%ISR=8A-94%TI=I%II=RI%SS=O%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=3180%W2=3180%W3=3180%W4=3180%W5=3180%W6=3180)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3180%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=3180%S=O%A=O%F=AS|APF%O=|M109%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Interflex TimeCollector (IF-LP1735)
Fingerprint Interflex IF-1735 timeclock
Class Interflex | embedded || specialized
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=19-23%TG=20%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=16D0%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=16D0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Intermec EasyCoder PM4i
Fingerprint Intermec PM4i label printer
Class Intermec | embedded || printer
SEQ(SP=F2-106%GCD=1-6%ISR=F7-113%TI=RD%II=RI%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4000%W5=4180%W6=403D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=134%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Intermec EasyCoder PM4i
Fingerprint Intermec PM4i label printer
Class Intermec | embedded || printer
SEQ(SP=92-9C%GCD=1-6%ISR=99-A3%TI=RD%CI=RD|RI%II=RI%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4000%W5=4180%W6=403D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=403D%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=134%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Windows CE 4.20 running on Intermec CK31
Fingerprint Intermec CK31 PDA (Windows CE 4.20)
Class Intermec | Windows | PocketPC/CE | PDA
SEQ(SP=59-7F%GCD=1-6%ISR=98-A2%TI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT00NNS%O2=M5B4NW0NNT00NNS%O3=M5B4NW0NNT00%O4=M5B4NW0NNT00NNS%O5=M5B4NW0NNT00NNS%O6=)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=0)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=0%O=%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=Z)

# ADSL modem - Intertex IX66 edflc
Fingerprint Intertex IX66-EDFLC ADSL modem
Class Intertex | embedded || broadband router
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(R=N)

# iOgear USB 1.1 print server - Model GPSU01 firmware ver: 1.0.7
Fingerprint IOGear GPSU01 USB print server
Class IOGear | embedded || print server
SEQ(SP=0%GCD=A000|14000|1E000|28000|32000|3C000|6E000|DC000|14A000|1B8000|226000|294000%ISR=AB-B5%TI=I|RD%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=B68%W2=B68%W3=B68%W4=B68%W5=B68%W6=B68)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=B68%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=1B-25%TG=20%W=B68%S=O%A=O|S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=1B-25%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=1B-25%TG=20%CD=S)

# ION Networks SA5600 Appliance - Linux 2.6.14 based
Fingerprint ION Networks SA5600-series firewall
Class ION Networks | embedded || firewall
SEQ(SP=7D-89%GCD=1-6%ISR=89-93%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=1B-25%TG=20%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=7B-85%TG=80%CD=S)

# IPAD-OS embedded network operating system connected as LAN gateway. IPAD-OS is made by IPAD Owners Association www.ipadowners.org.
Fingerprint IPAD-OS
Class IPAD Owners Association | IPAD-OS || specialized
SEQ(SP=E8-F6%GCD=1-6%ISR=F0-FA%TI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=1800%W2=1800%W3=1800%W4=1800%W5=1800%W6=1800)
ECN(R=Y%DF=N%T=C2-CC%TG=FF%W=1800%O=M400%CC=N%Q=)
T1(R=Y%DF=N%T=C2-CC%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=C2-CC%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=C2-CC%TG=FF%W=1800%S=O%A=S+%F=AS%O=M400%RD=0%Q=)
T4(R=Y%DF=N%T=C2-CC%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=C2-CC%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=C2-CC%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=C2-CC%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=C2-CC%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=C2-CC%TG=FF%CD=S)

# Linux 2.4.34 i586 pentium-mmx i386 GNU/Linux
Fingerprint IPCop firewall 1.4.16 (Linux 2.4.34)
Class IPCop | Linux | 2.4.X | firewall
SEQ(SP=C1-CB%GCD=1-6%ISR=C0-CA%TI=Z%II=I%TS=U)
OPS(O1=M400C%O2=M400C%O3=M400C%O4=M400C%O5=M400C%O6=M400C)
WIN(W1=7FFF%W2=7FFF%W3=7FFF%W4=7FFF%W5=7FFF%W6=7FFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=7FFF%O=M400C%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# IronPort C100 v4.7.1-009 - English
Fingerprint IronPort C100 email security appliance (AsyncOS 4.7.1)
Class IronPort | AsyncOS | 4.X | firewall
SEQ(SP=FC-106%GCD=1-6%ISR=109-113%TI=I%II=I%SS=O|S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=O|S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Ironport (www.ironport.com) C100 email appliance. This is version 6.01.
# AsyncOS 6.3 for IronPort C650
# CISCO Aironport Anti Spam appliance
Fingerprint IronPort C100 or C650 email security appliance (AsyncOS 6.01 - 6.3)
Class IronPort | AsyncOS | 6.X | firewall
SEQ(SP=EC-108%GCD=1-6%ISR=104-10E%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4SLL%O2=M5B4SLL%O3=M5B4%O4=M5B4SLL%O5=M5B4SLL%O6=M5B4SLL)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Ironport C150 running AsyncOS 6.5.2-101
Fingerprint IronPort C150 email security appliance (AsyncOS 6.5.2)
Class IronPort | AsyncOS | 6.X | firewall
SEQ(SP=F6-10C%GCD=1-6%ISR=FD-117%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4SLL%O2=M5B4SLL%O3=M5B4%O4=M5B4SLL%O5=M5B4SLL%O6=M5B4SLL)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# IronPort C150 Antispam Appliance wit hAsyncOS v6.3.5-003
Fingerprint IronPort C150 email security appliance (AsyncOS 6.5.3)
Class IronPort | AsyncOS | 6.X | firewall
SEQ(SP=102-10C%GCD=1-6%ISR=102-110%TI=I%II=I%SS=O|S%TS=U)
OPS(O1=M5B4SLL%O2=M5B4SLL%O3=M5B4%O4=M5B4SLL%O5=M5B4SLL%O6=M5B4SLL)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3A-44%TG=40%W=4000%O=M5B4SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3A-44%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3A-44%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4SLL%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=3A-44%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3A-44%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3A-44%TG=40%CD=S)

# Isilon IQ200
Fingerprint Isilon IQ 200 NAS device
Class Isilon | OneFS || storage-misc
SEQ(SP=FF-109%GCD=1-6%ISR=103-10D%TI=I%II=I%SS=S%TS=7)
OPS(O1=M564NW2NNT11%O2=M564NW2NNT11%O3=M564NW2NNT11%O4=M564NW2NNT11%O5=M564NW2NNT11%O6=M564NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M564NW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# ISS Proventia GX3002 IPS and Firewall. Firmware revision 1.5, express update level 28.030. Linux version 2.4.18-1000.ISS.54 (support@iss.net) (gcc version 3.2 20020903 (Red Hat Linux 8.0 3.2-7)) #1 Mon Jan 22 13:46:03 EST 2007
# Linux 2.4.18-1000.ISS.54 #1 Mon Jan 22 13:46:03 EST 2007 i686 i686 i386 GNU/Linux (Management port on IBM / ISS Proventia GX3002 network IPS with firmware 1.5)
Fingerprint ISS Proventia GX3002 firewall (Linux 2.4.18)
Class ISS | Linux | 2.4.X | firewall
SEQ(SP=C0-CE%GCD=1-6%ISR=C0-D0%TI=Z%II=I%TS=9|A|B|C)
OPS(O1=M550ST11NW0%O2=M550ST11NW0%O3=M550NNT11NW0%O4=M550ST11NW0%O5=M550ST11NW0%O6=M550ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M550NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=O|S+%F=AS%O=M550ST11NW0%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Linux 2.4.18-1000.ISS.54 #1 Mon Jan 22 13:46:03 EST 2007 i686
Fingerprint ISS Proventia GX3002C firewall (Linux 2.4.18)
Class ISS | Linux | 2.4.X | firewall
SEQ(SP=BE-C8%GCD=1-6%ISR=C9-D3%TI=Z%II=I%TS=9|C)
OPS(O1=M550ST11NW0%O2=M550ST11NW0%O3=M550NNT11NW0%O4=M550ST11NW0%O5=M550ST11NW0%O6=M550ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M550NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=O|S+%F=AS%O=M550ST11NW0%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Juniper SSG-20-WLAN, Firmware: 5.4.0r3a.0 (Firewall+VPN)
Fingerprint Juniper Networks SSG 20 firewall
Class Juniper | embedded || firewall
SEQ(SP=FC-106%GCD=1-6%ISR=108-112%TI=I%II=I%SS=S%TS=U)
OPS(O1=M564%O2=M564%O3=M564%O4=M564%O5=M564%O6=M564)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M564%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Specifically this is a VRRP ip between two Juniper J4350
Fingerprint Juniper J4350 router
Class Juniper | embedded || router
SEQ(SP=101-10B%GCD=1-6%ISR=105-10F%TI=I%II=RI%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=O|S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Juniper M7I
Fingerprint Juniper M7i router
Class Juniper | embedded || router
SEQ(SP=FA-108%GCD=1-6%ISR=103-111%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNT11SLL%O2=M5B4NW0NNT11SLL%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11SLL%O5=M5B4NW0NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT11SLL%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Juniper Edge Routing Switch ERX-700Copyright (c) 1999-2006 Juniper Networks, Inc.  All rights reserved.System Release: erx_8-0-0.relJuniper Edge Routing Switch ERX-700 Version: 8.0.0 release-0.0 [BuildId 6547]   (December 27, 2006  18:24)
Fingerprint Juniper Networks ERX-700 router
Class Juniper | embedded || router
SEQ(SP=FC-108%GCD=1-6%ISR=102-112%II=RI%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7A-84%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=7A-84%TG=80%CD=S)

# Juniper WXC-590, JUNOS Software version: 5.4.4.0
Fingerprint Juniper Networks WXC-590 proxy server (JUNOS 5.4.4.0)
Class Juniper | JUNOS | 5.X | proxy server
SEQ(SP=95-9F%GCD=1-6%ISR=9B-A5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Junos 7.3 R6
Fingerprint Juniper Networks JUNOS 7.3R6
Class Juniper | JUNOS | 7.X | router
SEQ(SP=101-10B%GCD=1-6%ISR=102-110%CI=I%II=I%TS=7)
OPS(O1=M578NW0NNT11%O2=M578NW0NNT11%O3=M578NW0NNT11%O4=M578NW0NNT11%O5=M578NW0NNT11%O6=M578NNT11)
WIN(W1=E000%W2=E000%W3=E000%W4=E000%W5=E000%W6=E000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=E000%O=M578NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=E000%S=O%A=S+%F=AS%O=M578NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Juniper M320 Version 7.4R3.4
# Juniper M10 Version 7.4R3.4
Fingerprint Juniper Networks M10 or M320 router (JUNOS 7.4R3.4)
Class Juniper | JUNOS | 7.X | router
SEQ(SP=FE-108%GCD=1-6%ISR=104-110%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=E000%W2=E000%W3=E000%W4=E000%W5=E000%W6=E000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=E000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=E000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Juniper Networks Olive running JUNOS 7.5-20060511.0 built 2006-05-11 08:09:15 UTC
Fingerprint Juniper Networks Olive (JUNOS 7.5-20060511)
Class Juniper | JUNOS | 7.X | router
SEQ(SP=E4-104%GCD=1-6%ISR=106-110%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B0NW0NNT11%O2=M5B0NW0NNT11%O3=M5B0NW0NNT11%O4=M5B0NW0NNT11%O5=M5B0NW0NNT11%O6=M5B0NNT11)
WIN(W1=E000%W2=E000%W3=E000%W4=E000%W5=E000%W6=E000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=E000%O=M5B0NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=E000%S=O%A=S+%F=AS%O=M5B0NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Juniper J2320 running JUNOS 8.5R3.4
# Juniper EX4200-24T running Junos 9.5R1.8
# Juniper EX4200-24F
# JUNOS 10.0.R1.8 JUNOS 10.0.R!.8 #0: 2009-11-03 09:00:32 UTC builder@ormonth.juniper.net:/volume/build/junos/10.0/release/10.0R1.8/obj-i386/bsd/sys/compile/JUNIPER i386
# Juniper EX3200 Switch
Fingerprint Juniper Networks J2320 router, or EX3200 or EX4200 switch (JUNOS 8.5 - 10.0)
Class Juniper | JUNOS | 8.X | router
Class Juniper | JUNOS | 9.X | switch
Class Juniper | JUNOS | 10.X | switch
SEQ(SP=F8-10C%GCD=1-6%ISR=105-111%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Juniper j4350, JUNOS Software Release [8.3R1.5] (Export edition)
Fingerprint Juniper Networks J4350 router (JUNOS 8.3R1.5)
Class Juniper | JUNOS | 8.X | router
SEQ(SP=F8-10A%GCD=1-6%ISR=106-110%TI=I%II=RI%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=E000%W2=E000%W3=E000%W4=E000%W5=E000%W6=E000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=E000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=E000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# --- JUNOS 8.5B2.5 built 2007-09-07 01:02:08 UTC
Fingerprint Juniper Networks JUNOS 8.5B2.5
Class Juniper | JUNOS | 8.X | router
SEQ(SP=FC-10C%GCD=1-6%ISR=102-112%TI=I%II=I%SS=S%TS=A)
OPS(O1=M556NW1NNT11SLL%O2=M556NW1NNT11SLL%O3=M556NW1NNT11%O4=M556NW1NNT11SLL%O5=M556NW1NNT11SLL%O6=M556NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M556NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M556NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Juniper JUNOS M Series - 8.3R2.8
Fingerprint Juniper Networks M series router (JUNOS 8.3R2.8)
Class Juniper | JUNOS | 8.X | router
SEQ(SP=F8-108%GCD=1-6%ISR=FC-110%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=E000%W2=E000%W3=E000%W4=E000%W5=E000%W6=E000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=E000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=E000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# JUNOS 9.2R1.10 built 2008-08-07 06:14:51 UTC
Fingerprint Juniper JUNOS 9.2R1.10
Class Juniper | JUNOS | 9.X | router
SEQ(SP=101-10B%GCD=1-6%ISR=103-111%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Junos9.4R2.9
Fingerprint Juniper JUNOS 9.4R2.9
Class Juniper | JUNOS | 9.X | router
SEQ(SP=FE-10A%GCD=1-6%ISR=107-113%II=I%TS=A)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Model: mx960 JUNOS Base OS boot [9.5R3.7]
Fingerprint Juniper MX960 router (JUNOS 9.5R3.7)
Class Juniper | JUNOS | 9.X | router
SEQ(SP=F6-10A%GCD=1-6%ISR=FF-111%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNT11SLL%O2=M5B4NW0NNT11SLL%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11SLL%O5=M5B4NW0NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=4000%O=M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=FA-104%TG=FF%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT11SLL%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# JUNOS 9.0R2.10 JUNOS 9.0R2.10 #0: 2008-03-06 10:51:50 UTC     builder@nidhogg.juniper.net:/volume/build/junos/9.0/release/9.0R2.10/obj-i386/sys/compile/JSERIES  i386
Fingerprint Juniper Networks JUNOS 9.0R2.10
Class Juniper | JUNOS | 9.X | router
SEQ(SP=FA-104%GCD=1-6%ISR=103-10D%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=Y%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Juniper Steel-Belted Radius Enterprise Edition version 5.30.2009 on a Windows 2000 Server with SP4 appliance
Fingerprint Juniper Networks Steel-Belted Radius (SBR) server (Windows 2000 SP4)
Class Juniper | Windows | 2000 | security-misc
SEQ(SP=FF-109%GCD=1-6%ISR=106-110%TI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT00NNS%O2=M5B4NW0NNT00NNS%O3=M5B4NW0NNT00%O4=M5B4NW0NNT00NNS%O5=M5B4NW0NNT00NNS%O6=M5B4NNT00NNS)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=FFFF%O=M5B4NW0NNS%CC=N%Q=U)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=U)
T3(R=Y%DF=Y%T=7B-85%TG=80%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW0NNT00NNS%RD=0%Q=U)
T4(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=Z)

# KA9Q NOS 911229 (PA0GRI v1.8b) - over 17 years old software
Fingerprint KA9Q NOS TCP/IP stack for packet radio
Class KA9Q | KA9Q || specialized
SEQ(SP=2-CA%GCD=1000|2000|3000|4000|5000|7000|E000|15000|1C000|23000|2D3000|5A6000|879000|B4C000|E1F000%ISR=AB-E5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=4C%TG=80%W=400%O=M400%CC=N%Q=)
T1(R=Y%DF=N%T=4C%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=4C%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=4C%TG=80%W=400%S=O%A=O%F=AS%O=M400%RD=0%Q=)
T4(R=Y%DF=N%T=4C%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=4C%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=4C%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=4C%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=4C%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=4C%TG=80%CD=S)

# Kapsch ETC Antenna
Fingerprint Kapsch electronic toll collection system
Class Kapsch | embedded || specialized
SEQ(SP=C4-D6%GCD=1-6%ISR=D5-DF%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4W0L%O2=M5B4W0L%O3=M5B4W0L%O4=M5B4W0L%O5=M5B4W0L%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=6F-79%TG=80%W=2000%O=M5B4W0L%CC=N%Q=)
T1(R=Y%DF=N%T=6F-79%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=6F-79%TG=80%W=2000%S=O%A=S+%F=AS%O=M5B4W0L%RD=0%Q=)
T4(R=Y%DF=N%T=6F-79%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=6F-79%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=6F-79%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=6F-79%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=6F-79%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=9B54%RUD=G)
IE(DFI=N%T=6F-79%TG=80%CD=Z)

# KCorp KLG-575 Lifestyle GOLD Series Gateway Router
Fingerprint KCorp KLG-575 WAP
Class KCorp | embedded || WAP
SEQ(SP=B-15%GCD=FA7F|1F4FE|2EF7D|3E9FC|4E47B%ISR=96-A0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B0%O2=M5B0%O3=M5B0%O4=M5B0%O5=M5B0%O6=M5B0)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=2000%O=M5B0%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=7B-85%TG=80%CD=S)

# Kodak ESP 5250 wireless printer.
Fingerprint Kodak ESP 5250 printer
Class Kodak | embedded || printer
SEQ(SP=39-97%GCD=1000|2000|3000|4000|5000|63000|C6000|129000|18C000|1EF000%ISR=BA-100%TI=RD%II=RI%TS=U)
OPS(O1=M5B4T11NN%O2=M5B4%O3=M5B4T11NN%O4=M5B4T11NN%O5=M5B4%O6=M5B4)
WIN(W1=B680%W2=B680%W3=B680%W4=B680%W5=B680%W6=B680)
ECN(R=Y%DF=N%T=39-3F%TG=40%W=B680%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=39-3F%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=39-3F%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=39-3F%TG=40%IPL=38%UN=0%RIPL=G%RID=72E|306B|6D14|9054|E508%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=39-3F%TG=40%CD=Z)

# Kodak ESP 5250 Printer
Fingerprint Kodak ESP 5250 printer
Class Kodak | embedded || printer
SEQ(SP=5F-69%GCD=1000|2000|3000|4000|5000%ISR=BC-C6%TI=I%CI=I%II=I%SS=O%TS=U)
OPS(O1=M5B4T11NN%O2=M5B4%O3=M5B4T11NN%O4=M5B4T11NN%O5=%O6=)
WIN(W1=B680%W2=B680%W3=B680%W4=B680%W5=0%W6=0)
ECN(R=Y%DF=N%T=39-3F%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=39-3F%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=39-3F%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=39-3F%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=39-3F%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=39-3F%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=39-3F%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=39-3F%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=39-3F%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=39-3F%TG=40%CD=Z)

# Kongsberg Seatex AIS Basestation BS 410. It is used in the maritime environment (AIS is an identification system, offering ship-ship-shore identification and communication facilities).
Fingerprint Kongsberg Seatex BS410 AIS base station (maritime communication component)
Class Kongsberg Seatex | embedded || specialized
SEQ(R=N)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=6B-75%TG=80%W=0%O=%CC=N%Q=U)
T1(R=Y%DF=N%T=6B-75%TG=80%S=Z%A=S+%F=AR%RD=0%Q=)
T2(R=Y%DF=N%T=6B-75%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=6B-75%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=6B-75%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=6B-75%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=6B-75%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=6B-75%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=6B-75%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=49E9%RUD=G)
IE(DFI=N%T=6B-75%TG=80%CD=Z)

# KONICA MINOLTA Printer, model bizhub 250
Fingerprint Konica Minolta bizhub 250 printer
Class Konica Minolta | embedded || printer
SEQ(SP=0-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW1NNT11%O2=M5B4NW1NNT11%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11%O5=M5B4NW1NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW1%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Konica BizHub250
Fingerprint Konica Minolta bizhub 250 printer
Class Konica Minolta | embedded || printer
SEQ(CI=I%II=I)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=N)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Technichan said Linux is running on the Controller (Fiery X3eTY 35C-KM) of this copy machine - Konica Minolta Bizhub C450 with Fiery Controller
Fingerprint Konica Minolta bizhub C450 printer with optional Fiery Controller
Class Konica Minolta | embedded || printer
SEQ(SP=13-1D%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=98-A2%TI=I%II=I%SS=O%TS=1)
OPS(O1=M200NW0NNT11%O2=M200NW0NNT11%O3=M200NW0NNT11%O4=M200NW0NNT11%O5=M200NW0NNT11%O6=M200NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3A-44%TG=40%W=2000%O=M200NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3A-44%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3A-44%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Konica Minolta C203
Fingerprint Konica Minolta C203 printer
Class Konica Minolta | embedded || printer
SEQ(SP=F3-109%GCD=1-6%ISR=FF-111%TI=I%CI=I%II=I%SS=S%TS=8)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=1%W2=1%W3=1%W4=1%W5=1%W6=1)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# KONICA MINOLTA Di2510f
Fingerprint Konica Minolta Di2510f printer
Class Konica Minolta | embedded || printer
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW1NNT11%O2=M5B4NW1NNT11%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11%O5=M5B4NW1NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=FFFF%O=M5B4NW1%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=FFFF%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Minolta magicolor 2300 DL
Fingerprint Konica Minolta MagiColor 2300 DL printer
Class Konica Minolta | embedded || printer
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=1%W2=1%W3=1%W4=1%W5=1%W6=1)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# KONICA MINOLTA magicolor 2430 DL
Fingerprint Konica Minolta MagiColor 2430 printer
Class Konica Minolta | embedded || printer
SEQ(SP=96-A0%GCD=1-6%ISR=9A-A4%TI=I%II=I%SS=S%TS=1|2)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=1%W2=1%W3=1%W4=1%W5=1%W6=1)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1%S=O%A=O%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# KONICA MINOLTA magicolor 5430 DL
Fingerprint Konica Minolta MagiColor 5430 DL printer
Class Konica Minolta | embedded || printer
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=99-A3%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=1%W2=1%W3=1%W4=1%W5=1%W6=1)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Koukaam Device: NETIO-230A Firmware: V 2.31
Fingerprint Koukaam NETIO-230A power control device
Class Koukaam | embedded || power-device
SEQ(SP=0-2B%GCD=A|14|1E|28|32|29E|53C|7DA|A78|D16%ISR=60-6A%TI=I%CI=I%II=RI%SS=O|S%TS=U)
OPS(O1=M5BA%O2=M5BA%O3=M5BA%O4=M5BA%O5=M5BA%O6=M5BA)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=8000%O=M5BA%CC=N%Q=U)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=80%S=A%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=100%S=A%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=7A69%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=8000%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=FFFF%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# InterCon-PrintServer KYOCERA, Software version 7.1.30F (Released May 20 1998), Model IC3-ETHER-KYO-FS (R2), http://www.seh.de/english/products/ps1/ic3/ic3sup.htm
Fingerprint Kyocera InterCon print server
Class Kyocera | embedded || print server
SEQ(SP=0-15%GCD=1000|2000|3000|4000|5000%ISR=88-92%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=800%W2=800%W3=800%W4=800%W5=800%W6=800)
ECN(R=Y%DF=N%T=5F-69%TG=80%W=800%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=5F-69%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=5F-69%TG=80%W=800%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=Y%T=19-23%TG=20%W=0%S=A%A=Z%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=19-23%TG=20%W=0%S=A%A=Z%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=31-44%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=23-38%TG=40%CD=S)

# Kyocera FS-1118MFP
Fingerprint Kyocera FS-1118MFP printer
Class Kyocera | embedded || printer
SEQ(SP=C2-D4%GCD=1-6%ISR=C5-CF%TI=Z%II=I%TS=7)
OPS(O1=M58CST11NW0%O2=M58CST11NW0%O3=M58CNNT11NW0%O4=M58CST11NW0%O5=M58CST11NW0%O6=M58CST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M58CNNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M58CST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Kyocera FS-3800 Network printer
Fingerprint Kyocera FS-3800 network printer
Class Kyocera | embedded || printer
SEQ(SP=0-B3%GCD=1-6|10001|20002|30003|40004|50005|60006%ISR=96-A0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=100%W2=100%W3=100%W4=100%W5=100%W6=100)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=100%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=100%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=100%S=A%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=100%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=FA-104%TG=FF%CD=Z)

# LaCie 1TB NAS running Windows XP Embedded, Software Version 5.1.0, BIOS Version CLE266 - 42302e31
# LaCie NAS. Windows XP Embedded. Software version 5.1.2, Bios version CLE266 - 42302e31
Fingerprint LaCie NAS device (Windows XP Embedded)
Class LaCie | Windows | XP | storage-misc
SEQ(SP=100-10A%GCD=1-6%ISR=107-113%TI=I%CI=I%II=I%SS=O|S%TS=U)
OPS(O1=M5B4NNS%O2=M5B4NNS%O3=M5B4%O4=M5B4NNS%O5=M5B4NNS%O6=M5B4NNS)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=4000%O=M5B4NNS%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=7B-85%TG=80%W=4000%S=O%A=O|S+%F=AS%O=M5B4NNS%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=Z)

# LANCOM 1711 VPN router, firmware 6.32.0021
# LCOS version 6.32.0021 running on Lancom 1821+
Fingerprint Lancom 1711 or 1821 broadband router
Class Lancom | LCOS | 6.X | broadband router
SEQ(SP=0-106%GCD=1-6|920444|1240888|1B60CCC|2481110|2DA1554|3870494|70E0928|A950DBC|E1C1250|11A316E4%ISR=D6-112%TI=I%II=I%SS=S%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=578%W2=578%W3=578%W4=578%W5=578%W6=578)
ECN(R=Y%DF=N%T=3C%TG=40%W=578%O=%CC=S%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=S)

# LANCOM L-54ag Wireless 7.30.0015 / 20.03.2008
# LANCOM 1721 VPN (Annex B) | Ver. 7.28.0031 / 07.02.2008 / 6.26/e74.02.41.2
Fingerprint Lancom 1721 ADSL modem or L-54ag WAP (LCOS)
Class Lancom | LCOS || broadband router
Class Lancom | LCOS || WAP
SEQ(SP=FC-106%GCD=1-6%ISR=103-113%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=578%W2=578%W3=578%W4=578%W5=578%W6=578)
ECN(R=Y%DF=Y%T=3C%TG=40%W=578%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=S)

# LANCOM L-54g Wireless 7.52.0058
Fingerprint Lancom L-54g WAP (LCOS)
Class Lancom | LCOS || WAP
SEQ(SP=101-10B%GCD=1-6%ISR=F7-10F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M534%O2=M534%O3=M534%O4=M534%O5=M534%O6=M534)
WIN(W1=578%W2=578%W3=578%W4=578%W5=578%W6=578)
ECN(R=Y%DF=Y%T=38-42%TG=40%W=578%O=M534%CC=N%Q=)
T1(R=Y%DF=Y%T=38-42%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=38-42%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T3(R=Y%DF=N%T=38-42%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=38-42%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=38-42%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=38-42%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=38-42%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
U1(DF=N%T=38-42%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=38-42%TG=40%CD=S)

# Lanier LS232c Multifunction Printer
# Panasonic Network Camera Model Number BL-C1CE
# Panasonic BL-C10CE, Firmware(Boot)  1.25, Firmware(Application)   1.25
# Panasonic BB-HCM331 V1.30 Webcam
# Panasonic BB-HCM381 Model 6220000702010001 Firmware(Boot) 1.32 Firmware(Application) 1.32 Firmware(Camera) 2.01
# BCL-30A Webcam
# NetBSD  1.5.2 NetBSD 1.5.2 (GENERIC) #3: Sat Aug 18 23:37:05 CEST 2001
# NRG (Nashuatec Ricoh Gstetner group) Color Laserprinter DSc428
# SAVIN, RNPB53BDA, 8055, System/Copy     1.14.1
# NetBSD 1.4.2 NetBSD 1.4.2 (DVASK) #0: Thu Jun 22 10:06:44 CEST 2000 vax, MicroVAX II
# Ricoh NRG MP 161
# Ricoh Afficio 2020
Fingerprint NetBSD 1.4.2 - 1.5.2; Lanier LS232c, NRG DSc428, Ricoh Aficio 2020, Ricoh NRG MP 161, or Savin 8055 printer; or Panasonic Network Camera (BB-HCM331, BB-HCM381, BCL-30A, BL-C1CE, or BL-C10CE)
Class Lanier | embedded || printer
Class NetBSD | NetBSD | 1.X | general purpose
Class NRG | embedded || printer
Class Panasonic | embedded || webcam
Class Ricoh | embedded || printer
Class Savin | embedded || printer
SEQ(SP=C5-DD%GCD=1-6%ISR=D6-E0%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Lanier Image Scanner (IS100e).
# Philips SOPHOS iS3030 PBX
Fingerprint Lanier IS100e scanner or Philips Sopho iS3030 PBX
Class Lanier | embedded || specialized
Class Philips | embedded || PBX
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Lantronix Xpress DR+ flashed with their "Modbus" firmware.
Fingerprint Lantronix XPress-DR+ serial-to-Ethernet bridge
Class Lantronix | embedded || bridge
SEQ(SP=0-E4%GCD=1-6|100|200|300|400|500%ISR=55-E1%TI=I|RD%II=I%SS=O%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# This is a lantronix ETS4P device server.
Fingerprint Lantronix ETS4P print server
Class Lantronix | embedded || print server
SEQ(SP=70-7E%GCD=1-6%ISR=90-9A%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3C%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=Z)

# Lantronix Micro Print Server MPS1 Version V3.6/1(991115)
Fingerprint Lantronix MPS1 printer server
Class Lantronix | embedded || print server
SEQ(SP=82-94%GCD=1-6%ISR=95-9F%TI=I%TS=U)
OPS(O1=M57A%O2=M57A%O3=M57A%O4=M57A%O5=M57A%O6=M57A)
WIN(W1=E00%W2=E00%W3=E00%W4=E00%W5=E00%W6=E00)
ECN(R=Y%DF=N%T=37-41%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=37-41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=37-41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=37-41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=37-41%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=37-41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=37-41%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=37-41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=37-41%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(R=N)

# Lantronix Model UDS-1100, Firmware 6.5.0.7, Web Configuration version 1.6.0.0
Fingerprint Lantronix UDS1100 external serial device server
Class Lantronix | embedded || remote management
SEQ(SP=C2-D0%GCD=1-6%ISR=CB-D9%TI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=1FF%W2=1FF%W3=1FF%W4=1FF%W5=1FF%W6=1FF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1FF%O=M400%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1FF%S=O%A=S+%F=AS%O=M400%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Lantronix USD200 External Device Serial Port Server
Fingerprint Lantronix UDS200 external serial device server
Class Lantronix | embedded || remote management
SEQ(SP=FF-109%GCD=1-6%ISR=107-111%TI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=1FF%W2=1FF%W3=1FF%W4=1FF%W5=1FF%W6=1FF)
ECN(R=Y%DF=Y%T=3A-44%TG=40%W=1FF%O=M400%CC=N%Q=)
T1(R=Y%DF=Y%T=3A-44%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3A-44%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3A-44%TG=40%W=1FF%S=O%A=S+%F=AS%O=M400%RD=0%Q=)
T4(R=Y%DF=Y%T=3A-44%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3A-44%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3A-44%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3A-44%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3A-44%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3A-44%TG=40%CD=S)

# Lantronix XPort Embedded Ethernet device - http://www.lantronix.com/device-networking/embedded-device-servers/xport.html
Fingerprint Lantronix XPort embedded Ethernet device server
Class Lantronix | embedded || remote management
SEQ(SP=0-F2%GCD=1-6|100|200|300|400|500%ISR=46-EC%TI=I|RD%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=1FF%W2=1FF%W3=1FF%W4=1FF%W5=1FF%W6=1FF)
ECN(R=N)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Lantronix XPort in a GPS/Transponder Decoder Device by Pronet GmbH, Germany (ProtimeEliteDecoder)
Fingerprint Lantronix XPort embedded Ethernet device server
Class Lantronix | embedded || remote management
SEQ(SP=B8-D2%GCD=1-6%ISR=CD-D7%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M578%O4=M578%O5=M218%O6=M109)
WIN(W1=1FF%W2=1FF%W3=1FF%W4=1FF%W5=1FF%W6=1FF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1FF%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1FF%S=O%A=S+%F=AS%O=M578%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Lantronix XPort-03 Firmware v1.80 Embedded Serial to IP adaptor
Fingerprint Lantronix XPort-03 embedded serial device server (firmware 1.80)
Class Lantronix | embedded || remote management
SEQ(SP=FC-106%GCD=1-6%ISR=101-10F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=1FF%W2=1FF%W3=1FF%W4=1FF%W5=1FF%W6=1FF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1FF%O=M400%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Lantronix Xport-03 Embedded serial device server with FW 6.1.0.3
Fingerprint Lantronix Xport-03 embedded serial device server (firmware 6.1.0.3)
Class Lantronix | embedded || remote management
SEQ(SP=C8-D2%GCD=1-6%ISR=D0-DA%TI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=1FF%W2=1FF%W3=1FF%W4=1FF%W5=1FF%W6=1FF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1FF%O=M400%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1FF%S=O%A=S+%F=AS%O=M400%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Lantronix MSSLITE
Fingerprint Lantronix MSSLite device server
Class Lantronix | embedded || specialized
SEQ(SP=6C-7A%GCD=1-6%ISR=90-9A%TI=I%II=I%SS=O|S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=E00%W2=E00%W3=E00%W4=E00%W5=E00%W6=E00)
ECN(R=Y%DF=N%T=3C%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=Z)

# Lantronix ETS32PR Terminal Server
# lantronix lrs-16 terminal server
Fingerprint Lantronix ETS32Pr or LRS16 terminal server
Class Lantronix | embedded || terminal server
SEQ(SP=36-66%GCD=1-6%ISR=90-9A%TI=BI%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3C%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=Z)

# Operating System Name: Evolution OS, Used on embedded devices.
Fingerprint Lantronix Evolution OS
Class Lantronix | Evolution OS || specialized
SEQ(SP=27-47%GCD=100|200|300|400|500%ISR=8D-97%TI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=1FF%W2=1FF%W3=1FF%W4=1FF%W5=1FF%W6=1FF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1FF%O=M400%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1FF%S=O%A=S+%F=AS%O=M400%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Larus 54580 NTP clock.
Fingerprint Larus 54580 NTP server
Class Larus | embedded || specialized
SEQ(SP=C5-D1%GCD=1-6%ISR=CD-DB%TI=I%II=I%SS=S%TS=U)
OPS(O1=|M400%O2=|M400%O3=|M400%O4=|M400%O5=|M400%O6=|M400)
WIN(W1=0|7F%W2=0|7F%W3=0|7F%W4=0|7F%W5=0|7F%W6=0|7F)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=0|7F%O=|M400%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O|Z%A=S+%F=AR|AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=7F%S=O%A=O|S+%F=AS%O=M400%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Leolink LEO-6400DL running Conexant software
# EDIMAX
Fingerprint Leolink LEO-6400DL ADSL router
Class Leolink | embedded || broadband router
SEQ(SP=13-1D%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=20