NT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Netgear FR114P (Firmware Version:  V1.5_14)
Fingerprint Netgear FR114P ProSafe VPN firewall
Class Netgear | embedded || firewall
SEQ(SP=0-5%GCD=80|100|180|200|280%ISR=4E-58%TI=I%II=I%SS=S%TS=U)
OPS(O1=M4D8%O2=M4D8%O3=M4D8%O4=M4D8%O5=M204%O6=MF5)
WIN(W1=C00%W2=C00%W3=C00%W4=C00%W5=C00%W6=C00)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=C00%O=M4D8%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=C00%S=O%A=S+%F=AS%O=M4D8%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# Netgear FR114P ProSafe VPN firewall
Fingerprint Netgear FR114P ProSafe VPN firewall
Class Netgear | embedded || firewall
SEQ(SP=C3-CD%GCD=1-6%ISR=C6-D0%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M564%O3=M5B4%O4=M5B4%O5=M204%O6=MF5)
WIN(W1=C00%W2=C00%W3=C00%W4=C00%W5=C00%W6=C00)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=C00%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=C00%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# Netgear Digital Entertainer EVA700
Fingerprint Netgear EVA700 Digital Entertainer set top box
Class Netgear | embedded || media device
SEQ(SP=35-49%GCD=1000|2000|3000|4000|5000%ISR=AA-B4%TS=A)
OPS(O1=M5B4T11W0LLL%O2=M5B4T11W0LLL%O3=M5B4T11W0LLL%O4=M5B4T11W0LLL%O5=M5B4T11W0LLL%O6=M5B4T11W0LLL)
WIN(W1=5B40%W2=5B40%W3=5B40%W4=5B40%W5=5B40%W6=5B40)
ECN(R=Y%DF=N%T=FE%TG=FF%W=5B40%O=M5B4T10W0LLL%CC=N%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FE%TG=FF%W=5B40%S=O%A=O|S+%F=AS%O=M5B4T11W0LLL%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# Netgear EVA-8000 media player
Fingerprint Netgear EVA8000 Digital Entertainer set top box
Class Netgear | embedded || media device
SEQ(SP=CA-D4%GCD=1-6%ISR=C4-CE%TI=Z%II=I%TS=7)
OPS(O1=M5B4NNT11NW0%O2=M5B4NNT11NW0%O3=M5B4NNT11NW0%O4=M5B4NNT11NW0%O5=M5B4NNT11NW0%O6=M5B4NNT11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4NNT11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# NETGEAR PrintServer PS105
Fingerprint Netgear PS105 print server
Class Netgear | embedded || print server
SEQ(R=N)
OPS(O1=M400%O2=%O3=%O4=%O5=%O6=)
WIN(W1=400%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=400%O=M400%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=APS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=1B-25%TG=20%W=400%S=O%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(R=N)

# Netear SC101 NAS Box
Fingerprint Netgear SC101 Storage Central NAS device
Class Netgear | embedded || storage-misc
SEQ(CI=I)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=N)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(R=N)

# Netgear FS700TS Smart Switch
Fingerprint Netgear FS700TS Smart Switch
Class Netgear | embedded || switch
SEQ(SP=0-9B%GCD=14|28|3C|50|64%ISR=4B-7F%TI=RD%II=RI%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=S+%F=AS%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Netgear GSM7224 switch, firmware version 6.2.0.14
Fingerprint Netgear GSM7224 switch
Class Netgear | embedded || switch
SEQ(SP=96-A0%GCD=1-6%ISR=9C-A6%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1000%S=O%A=O%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# "smart" (semi-manageable) Ethernet switch, model GS724T, with firmware version 1.0.3_33.
Fingerprint Netgear ProSafe GS724T switch
Class Netgear | embedded || switch
SEQ(SP=0-1D%GCD=0|A|14|1E|28|32%ISR=0-41%TI=I%II=RI%SS=O|S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M5B4%O4=M5B4%O5=M218%O6=M109)
WIN(W1=1800%W2=1800%W3=1800%W4=1800%W5=1800%W6=1800)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=3%O=%CC=N%Q=U)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=FA-104%TG=FF%W=80%S=A%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=FA-104%TG=FF%W=100%S=A%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=400%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=7A69%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=8000%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=FFFF%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Netgear CG814WG v2 (Comcast)
# Thomson TWG870U  DOCSIS 3.0-compliant VoIP cable modem with software STBA.01.05.
Fingerprint Netgear CG814WG v2 or Thomson TWG870U wireless cable modem
Class Netgear | embedded || WAP
Class Thomson | embedded || WAP
SEQ(SP=E7-107%GCD=1-6%ISR=EF-10B%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4074%W5=4180%W6=403D)
ECN(R=N)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Netgear Wireless ADSL2+ Modem Router DG834G firmware version V5.01.14
Fingerprint Netgear DG834G WAP
Class Netgear | embedded || WAP
SEQ(II=I)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Netgear DG834GB firmware 3.01.25
Fingerprint Netgear DG834GB wireless broadband router
Class Netgear | embedded || WAP
SEQ(SP=C0-CA%GCD=1-6%ISR=C6-D0%TI=Z%TS=7|9)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=B6|67DD|A099|ABDB|EB89%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Netgear ProSafe Wireless Access Point WG302v2
Fingerprint Netgear ProSafe WG302 v2 WAP
Class Netgear | embedded || WAP
SEQ(SP=C2-CC%GCD=1-6%ISR=C6-D0%TI=Z%II=I%TS=7)
OPS(O1=M5C8ST11NW0%O2=M5C8ST11NW0%O3=M5C8NNT11NW0%O4=M5C8ST11NW0%O5=M5C8ST11NW0%O6=M5C8ST11)
WIN(W1=1134%W2=1134%W3=1134%W4=1134%W5=1134%W6=1134)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1158%O=M5C8NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1134%S=O%A=S+%F=AS%O=M5C8ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# WGR614 V7
Fingerprint Netgear WGR614v7 WAP
Class Netgear | embedded || WAP
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Netgear WGR614 v7 router
Fingerprint Netgear WGR614v7 wireless broadband router
Class Netgear | embedded || WAP
SEQ(SP=13-1D%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%TI=I|RD%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# WGR614v7 Netgear router, Firmware Version V2.0.30_2.0.30
Fingerprint Netgear WGR614v7 wireless broadband router
Class Netgear | embedded || WAP
SEQ(CI=I%II=I)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# ReadyNAS NV+ running RAIDiator 4.00c1-p2 firmware, Linux 2.6.17.8ReadyNAS #1 Mon Dec 17 19:35:18 PST 2007 padre unknown
# ReadyNAS NV+ - in this specific case, RND4250 running Infrant/Netgear embedded Linux distro - "RAIDiator  4.00c1-p2 [1.00a037]", Linux readynas 2.6.17.8ReadyNAS #1 Mon Dec 17 19:35:18 PST 2007 padre unknown
# Linux nas1 2.6.17.8ReadyNAS #1 Tue Jul 22 04:48:09 PDT 2008 padre unknown
# ReadyNas NV+ 4000
# ReadyNAS Duo, RAIDiator 4.1.6 [1.00a043]
Fingerprint Netgear RND4000 or RND4250 ReadyNAS NV+ NAS device (Linux 2.6.17)
Class Netgear | Linux | 2.4.X | storage-misc
SEQ(SP=BF-D2%GCD=1-6%ISR=C7-D5%TI=Z%CI=Z%II=I%TS=7)
OPS(O1=M1ED8ST11NW4%O2=M1ED8ST11NW4%O3=M1ED8NNT11NW4%O4=M1ED8ST11NW4%O5=M1ED8ST11NW4%O6=M1ED8ST11)
WIN(W1=3D98%W2=3D98%W3=3D98%W4=3D98%W5=3D98%W6=3D98)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=3DB0%O=M1ED8NNSNW4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=3D98%S=O%A=S+%F=AS%O=M1ED8ST11NW4%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Linux version 2.2.14openrg (JUNGO@) ()
Fingerprint Netgear WG602v1 WAP (Linux 2.2.14)
Class Netgear | Linux | 2.4.X | WAP
SEQ(SP=B4-BE%GCD=1-6%ISR=BD-C7%TI=I%CI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4ST11NW0%O2=M578ST11NW0%O3=M280NNT11NW0%O4=M218ST11NW0%O5=M218ST11NW0%O6=M109ST11)
WIN(W1=3908%W2=3C28%W3=3C00%W4=3CB8%W5=3CB8%W6=3C0A)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=3908%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=3C0A%S=O%A=S+%F=AS%O=M109ST11NW0%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Netgear ReadyNAS Duo Firmware: RAIDiator 4.1.4 [1.00a042] (Probably Linux --Ed.)
Fingerprint Netgear ReadyNAS Duo NAS device (RAIDiator 4.1.4)
Class Netgear | RAIDiator | 4.X | storage-misc
SEQ(SP=C4-CE%GCD=1-6%ISR=CD-D7%TI=Z%II=I%TS=7|8)
OPS(O1=NNT11|M5B4ST11NW4%O2=NNT11|M5B4ST11NW4%O3=NNT11|M5B4NNT11NW4%O4=NNT11|M5B4ST11NW4%O5=NNT11|M5B4ST11NW4%O6=NNT11|M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=N)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# VxWorks (for Netgear WPN824v2) version VxWorks5.4.2. Kernel: WIND version 2.5. Made on Oct  2 2006, 19:10:19.
# Netgear WGR614v7
# Netgear WPN824
# Netgear WGT624 v3 Wireless Firewall Router
Fingerprint Netgear WGR614v7, WGT624v3, or WPN824v2 WAP (VxWorks 5.4.2)
Class Netgear | VxWorks | 5.X | WAP
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Netgear HE102 Wireless 802.11a AccessPoint with VxWorks embedded OS
Fingerprint Netgear HE102 WAP (VxWorks)
Class Netgear | VxWorks || WAP
SEQ(SP=13-1D%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=9A-A4%II=I%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Motorola Netopia Model 2247-62 AnnexA High-Power Wireless DSL Ethernet Managed Switch, PBC, Running Netopia SOC OS version 7.8.2 (build r2)
Fingerprint Netopia 2247 ADSL router
Class Netopia | embedded || broadband router
SEQ(SP=FF-109%GCD=1-6%ISR=104-10E%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=800%W2=800%W3=800%W4=800%W5=800%W6=800)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=800%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=800%S=O%A=O|S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Netopia 3366N
# Netopia 3366 Router w/ Integrated ADSL modem
Fingerprint Netopia 3366 ADSL router
Class Netopia | embedded || broadband router
SEQ(SP=FB-109%GCD=1-6%ISR=FE-110%TI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Netopia 3386-ENT Router OS
Fingerprint Netopia 3386 ADSL router
Class Netopia | embedded || broadband router
SEQ(SP=FF-109%GCD=1-6%ISR=FF-109%TI=I|RD%II=I%SS=O|S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Netopia 3387WG-ENT via wifi
# Netopia 3387WG-ENT, firmware version 8.7.4r1
# Netopia 3387WG-ENT v8.7.4r1
Fingerprint Netopia 3387WG-ENT broadband router
Class Netopia | embedded || broadband router
SEQ(SP=FA-108%GCD=1-6%ISR=101-113%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# NetopiaAnalog ADSL Router 3346N
# Netopia 3397GPB  VDSL Router OS Version 7.7.1r3
# Netopia 3347NWG, Software Release        7.6.1r6
# Netopia 3347NWG Software Version 7.4.2r2
# Netopia 3347W wireless ADSL router; SOC OS 7.3.3 (build r0)
Fingerprint Netopia 3300-series ADSL router
Class Netopia | SOC OS | 7.X | broadband router
Class Netopia | SOC OS | 7.X | WAP
SEQ(SP=F7-109%GCD=1-6%ISR=FF-10F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=800%W2=800%W3=800%W4=800%W5=800%W6=800)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=800%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=800%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Netopia Model 3346N-VGx DSL Ethernet Managed Switch, Running Netopia SOC OS version 7.8.5 (build r1)
Fingerprint Netopia 3346N-VGx ADSL router
Class Netopia | SOC OS | 7.X | broadband router
SEQ(SP=F6-10A%GCD=1-6%ISR=104-112%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=800%W2=800%W3=800%W4=800%W5=800%W6=800)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=800%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=800%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# NetOptics iBypass Switch
Fingerprint NetOptics iBypass switch
Class NetOptics | embedded || switch
SEQ(SP=73-10B%GCD=100|200|300|400|500|10000|20000|30000|40000|50000%ISR=10A-114%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=800%W2=800%W3=800%W4=800%W5=800%W6=800)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=800%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# BorierGuard 1000  (BG00BAS) "StorageTek BG-DPF1 Console V5.1-1 22-Apr-1999 17:25"
Fingerprint Network Systems BorderGuard 1000 firewall
Class Network Systems | embedded || firewall
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=1B-25%TG=20%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Network Alchemy "Argent Branch" hardware PBX
Fingerprint NetworkAlchemy ArgentBranch PBX
Class NetworkAlchemy | embedded || PBX
SEQ(SP=16-2C%GCD=10000|20000|30000|40000|50000%ISR=CB-D5%TI=I%II=RI%SS=O|S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=1111%W2=1111%W3=1111%W4=1111%W5=1111%W6=1111)
ECN(R=N)
T1(R=Y%DF=N%T=5E-68%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=5E-68%TG=80%W=1111%S=Z%A=S+%F=R%O=%RD=0%Q=)
T6(R=Y%DF=N%T=5E-68%TG=80%W=1111%S=Z%A=S+%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=5E-68%TG=80%W=1111%S=Z%A=S+%F=R%O=%RD=0%Q=)
U1(DF=N%T=5E-68%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=21-2D|30-3C%TG=40%CD=S)

# NetworksAOK appliance made by http://www.interloci.com/
Fingerprint NetworksAOK network monitoring applicance
Class NetworksAOK | embedded || firewall
SEQ(SP=C8-D2%GCD=1-6%ISR=CE-D8%TI=Z%TS=7)
OPS(O1=M584ST11NW0%O2=M584ST11NW0%O3=M584NNT11NW0%O4=M584ST11NW0%O5=M584ST11NW0%O6=M584ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M584NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(R=N)
IE(R=N)

# Foxconn VoIP TRIO 3C, F01L010.00_LDCOM/V1.6.19_AV225165 Build V060419 MAC:000E9B8BB948
Fingerprint Neuf Box Trio 3C DSL modem
Class Neuf | embedded || broadband router
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%RD=0)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# "NeufBox Trio3d" DSL Modem/router/Voip/Tv   firmware V1.7.19_AV225165
Fingerprint Neuf Box Trio 3D DSL modem
Class Neuf | embedded || broadband router
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Newave Concept UPS snmp adapter "CS121-SNMP v 2.48.15 Model: C-2003"
Fingerprint Newave UPS SNMP adapter
Class Newave | embedded || power-device
SEQ(SP=FE-10A%GCD=1-6%ISR=103-111%TI=BI%TS=U)
OPS(O1=M564NNS%O2=M564NNS%O3=M564NNS%O4=M564NNS%O5=M218NNS%O6=M128NNS)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=0%O=%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=2C-41%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Nexsan, Device: ATABoy RAID Subsystem
Fingerprint NexStor Nexsan ATABoy NAS device
Class NexStor | embedded || storage-misc
SEQ(SP=F-1F%GCD=1000|2000|3000|4000|5000%ISR=AB-B5%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4T11W0LLL%O2=M5B4T11W0LLL%O3=M5B4T11W0LLL%O4=M5B4T11W0LLL%O5=M5B4T11W0LLL%O6=M5B4T11W0LLL)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FE%TG=FF%W=2000%O=M5B4T10W0LLL%CC=N%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FE%TG=FF%W=2000%S=O%A=O%F=AS%O=M5B4T11W0LLL%RD=0%Q=)
T4(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# Nexsan ATAboy2X network-capable fibre-channel disk array
Fingerprint NexStor Nexsan ATABoy2x NAS device
Class NexStor | embedded || storage-misc
SEQ(R=N)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=FE%TG=FF%W=0%O=%CC=Y%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=Z%A=S+%F=AR%RD=0%Q=)
T2(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FE%TG=FF%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FE%TG=FF%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# NeXTSTEP 3.3, Patch level 3. This is the m68k version on a NeXTStation.
# OpenSTEP 4.2 on 68040 ("black hardware")
Fingerprint NeXT NEXTSTEP 3.3 (patch level 3, m68k) or OPENSTEP 4.2
Class NeXT | NEXTSTEP | 3.X | general purpose
Class NeXT | OPENSTEP | 4.X | general purpose
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=1000%W2=1000%W3=F00%W4=1000%W5=EA8%W6=F87)
ECN(R=Y%DF=N%T=3C%TG=40%W=1000%O=M400%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=F87%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=1000%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenSTEP 4.2 on my Sun SparcStation 10
Fingerprint NeXT OPENSTEP 4.2
Class NeXT | OPENSTEP | 4.X | general purpose
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=1000%W2=1000%W3=F00%W4=1000%W5=EA8%W6=F87)
ECN(R=Y%DF=N%T=3C%TG=40%W=1000%O=M400%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OPENSTEP 4.2pl4 box with a 3com 3c905b NIC
Fingerprint NeXT OPENSTEP 4.2
Class NeXT | OPENSTEP || general purpose
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I|RD%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=1000%W2=1000%W3=F00%W4=1000%W5=EA8%W6=F87)
ECN(R=Y%DF=N%T=3C%TG=40%W=1000%O=M400%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=F87%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Nintendo DS running DSFTP FTP server. (Sometimes reported by Nmap as a Xerox printer.)
Fingerprint Nintendo DS game console
Class Nintendo | embedded || game console
SEQ(SP=C1-DF%GCD=40|80|C0|100|140%ISR=FC-116%TI=BI|RD%II=BI%SS=S%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=578%W2=0|578%W3=578%W4=0|578%W5=0|578%W6=0|578)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=578%O=%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T3(R=Y%DF=N%T=7B-85%TG=80%W=578%S=O%A=O|S+%F=AS%O=%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=7B-85%TG=80%CD=S)

# Nintendo Wii, loaded the homebrew TCP loader on port 8080 to get an open port.
Fingerprint Nintendo Wii game console
Class Nintendo | embedded || game console
SEQ(SP=F8-108%GCD=1-6%ISR=105-111%II=I%TS=U)
OPS(O1=M5B4NNS%O2=M578NNS%O3=M280NNS%O4=M218NNS%O5=M218NNS%O6=M109NNS)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5B4NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=M109NNS%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Wii running Homebrew Channel; port 4299 is open
# Firmware 4.0U
Fingerprint Nintendo Wii game console
Class Nintendo | embedded || game console
SEQ(SP=F8-108%GCD=1-6%ISR=105-111%II=I%TS=U)
OPS(O1=M5B4NNS%O2=M578NNS%O3=M280NNS%O4=M218NNS%O5=M218NNS%O6=M109NNS)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5B4NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=M109NNS%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Wii System Update 4.1U
Fingerprint Nintendo Wii game console
Class Nintendo | embedded || game console
SEQ(CI=I%II=I%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Nokia IPSO 4.1Build19 firewall
Fingerprint Nokia firewall (IPSO 4.1Build19)
Class Nokia | IPSO | 4.X | firewall
SEQ(SP=F8-102%GCD=1-6%ISR=105-10F%TI=I|RD%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4334%W5=4180%W6=403D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AR|AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(R=N)
IE(R=N)

# IPSO v4.1 build 50 running on an IP330
# IPSO Nokia.com 4.2-BUILD096 releng 1515  12.05.2008-053151 i386
Fingerprint Nokia IP330 firewall appliance (IPSO 4.1 - 4.2)
Class Nokia | IPSO | 4.X | firewall
SEQ(SP=FB-109%GCD=1-6%ISR=103-10F%TI=I%II=I%SS=S%TS=1)
OPS(O1=M400NW0NNT11%O2=M400NW0NNT11%O3=M400NW0NNT11%O4=M400NW0NNT11%O5=M400NW0NNT11%O6=M400NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4334%W5=4180%W6=403D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4470%O=M400NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IPSO 4.0-BUILD023 releng 1515  10.05.2005-011351 i386
Fingerprint Nokia IP650 firewall (IPSO 4.0 and CheckPoint Firewall-1/VPN-1 software)
Class Nokia | IPSO | 4.X | firewall
SEQ(SP=F0-10E%GCD=1-6%ISR=FB-109%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4334%W5=4180%W6=403D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Linux Nokia-N800-43-7 2.6.21-omap1 #1 Thu Dec 25 12:14:00 GMT 2008 armv6l unknown, Nokia N800, firmware (Maemo) versioned OS2008/Diablo, RX-34+RX-44+RX-48_DIABLO_5.2008.43-7_PR_MR0
Fingerprint Nokia N800 Internet tablet (Linux 2.6.21, ARM)
Class Nokia | Linux | 2.6.X | general purpose
SEQ(SP=C4-CE%GCD=1-6%ISR=C8-D2%TI=Z%II=I%TS=7)
OPS(O1=M400CST11%O2=M400CST11%O3=M400CNNT11%O4=M400CST11%O5=M400CST11%O6=M400CST11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8018%O=M400CNNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=8000%S=O%A=S+%F=AS%O=M400CST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Linux 2.6.28-omap1 #1 PREEMPT Thu Apr 15 09:47:09 EEST 2010 armv7l unknown
Fingerprint Nokia N900 mobile phone (Linux 2.6.28)
Class Nokia | Linux | 2.6.X | phone
SEQ(SP=C0-CA%GCD=1-6%ISR=C0-CA%TI=Z%CI=Z%TS=7|9)
OPS(O1=NNT11|M539ST11NW4%O2=NNT11|M539ST11NW4%O3=NNT11|M539NNT11NW4%O4=NNT11|M539ST11NW4%O5=NNT11|M539ST11NW4%O6=NNT11|M539ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=|M539NNSNW4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=O|S+%F=A|AS%O=NNT11|M539ST11NW4%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# execute the program SymSMB in the Nokia 5800 and run nmap.
Fingerprint Nokia 5800 mobile phone (Symbian OS 9.4)
Class Nokia | Symbian OS | 9.X | phone
SEQ(SP=F7-101%GCD=1-6%ISR=104-10E%TI=I%CI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT00NNS%O2=M5B4NW0NNT00NNS%O3=M5B4NW0NNT00%O4=M5B4NW0NNT00NNS%O5=M5B4NW0NNT00NNS%O6=M5B4NNT00NNS)
WIN(W1=4470%W2=41A0%W3=4100%W4=40E8%W5=40E8%W6=402E)
ECN(R=Y%DF=N%T=7C-86%TG=80%W=4470%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=7C-86%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=40-4A%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=40-4A%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=DE73%RUD=G)
IE(DFI=N%T=40-4A%TG=80%CD=S)

# Nokia N95 - Symbian Series 60, Release 3, V 10.0.018, 15-03-07, RM-159
# Nokia N95 running Symbian OS 9.2
# Nokia e90 communicator running Symbian 9.2
# Nokia S60 Series 3
# Nokia E51
Fingerprint Nokia E51, E90 Communicator, or N95 mobile phone (Symbian OS 9.2 - 10.0)
Class Nokia | Symbian OS | 9.X | phone
Class Nokia | Symbian OS | 10.X | phone
SEQ(SP=A0-B0%GCD=1-6%ISR=AB-B9%TI=I%II=I%SS=S%TS=D|13|14)
OPS(O1=M5B4NNT11NW0NNS%O2=M5B4NNT11NW0NNS%O3=M5B4NNT11NW0%O4=M5B4NNT11NW0NNS%O5=M5B4NNT11NW0NNS%O6=M5B4NNT11NNS)
WIN(W1=FAF0%W2=FAF0%W3=FAF0%W4=FAF0%W5=FAF0%W6=FAF0)
ECN(R=Y%DF=Y%T=40-4A%TG=80%W=FAF0%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=40-4A%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=40-4A%TG=80%W=FAF0%S=O%A=S+%F=AS%O=M5B4NNT11NW0NNS%RD=0%Q=)
T4(R=Y%DF=N%T=40-4A%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=40-4A%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=40-4A%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=40-4A%TG=80%CD=S)

# Nokia E70 S60 3.0 (S60 3rd Edition) / Symbian OS 9.1
Fingerprint Nokia E70 mobile phone (Symbian OS 9.1)
Class Nokia | Symbian OS | 9.X | phone
SEQ(SP=A7-B1%GCD=1-6%ISR=AD-BB%TI=I%II=I%SS=S%TS=12|14|18)
OPS(O1=M5B4T11W0SL%O2=M5B4T11W0SL%O3=M5B4T11W0LLL%O4=M5B4T11W0SL%O5=M5B4T11W0SL%O6=M5B4T11S)
WIN(W1=BC34%W2=BC34%W3=BC34%W4=BC34%W5=BC34%W6=BC34)
ECN(R=Y%DF=Y%T=40-4A%TG=80%W=BC34%O=M5B4W0SLLL%CC=N%Q=)
T1(R=Y%DF=Y%T=40-4A%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=40-4A%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=40-4A%TG=80%CD=S)

# Nokia 3600i, V 03.41, 11-04-08, RM-337, Variant: 00.00
Fingerprint Nokia 3600i mobile phone
Class Nokia | Symbian OS || phone
SEQ(SP=F-19%GCD=4E2|9C4|EA6|1388|186A%ISR=60-6A%TI=I%CI=I%II=I%SS=S%TS=5)
OPS(O1=NNT11|M5B4T11S%O2=NNT11|M5B4T11S%O3=NNT11|M5B4T11LL%O4=NNT11|M5B4T11S%O5=NNT11|M5B4T11S%O6=NNT11|M5B4T11S)
WIN(W1=6B78%W2=71DC%W3=70D8%W4=7094%W5=7094%W6=6FAD)
ECN(R=N)
T1(R=N)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Nokia E55 mobile phone
Fingerprint Nokia E55 mobile phone (Symbian OS)
Class Nokia | Symbian OS || phone
SEQ(SP=A6-B2%GCD=1-6%ISR=AF-B9%TI=I%CI=I%II=I%SS=S%TS=12|14)
OPS(O1=M5B4NNT11NW1NNS%O2=M5B4NNT11NW1NNS%O3=M5B4NNT11NW1%O4=M5B4NNT11NW1NNS%O5=M5B4NNT11NW1NNS%O6=M5B4NNT11NNS)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FAF0)
ECN(R=Y%DF=Y%T=40-4A%TG=80%W=FFFF%O=M5B4NW1NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=40-4A%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=40-4A%TG=80%W=FFFF%S=O%A=S+%F=AS%O=M5B4NNT11NW1NNS%RD=0%Q=)
T4(R=Y%DF=N%T=40-4A%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=40-4A%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=40-4A%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=40-4A%TG=80%CD=S)

# Nokia E60 wifi enabled mobile phone, firmware version 3.
Fingerprint Nokia E60 mobile phone (Symbian OS)
Class Nokia | Symbian OS || phone
SEQ(SP=FF-109%GCD=1-6%ISR=108-112%TI=RD%TS=A)
OPS(O1=M5B4NW8NNT11SLL%O2=M5B4NW8NNT11SLL%O3=M5B4NW8NNT11%O4=M5B4NW8NNT11SLL%O5=M5B4NW8NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FECC%W2=FECC%W3=FECC%W4=FECC%W5=FECC%W6=FECC)
ECN(R=Y%DF=Y%T=41%TG=40%W=FECC%O=M5B4NW8SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=41%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=40-4A%TG=80%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=40-4A%TG=80%IPL=38%UN=0%RIPL=G%RID=E0A|255A|323B|AF23|FC79%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=40-4A%TG=80%CD=S)

# Nokia E61 Symbian OS - firmware version 3.0633.0904/20-11-06
# Nokia E65 mobile phone
# Nokia E70 Firmware 3.0633.09.04
# 3.0633.09.04 20-11-06 RM-49 Nokia E60 (output of *#0000#)
Fingerprint Nokia E60, E61, E65, or E70 mobile phone (Symbian OS)
Class Nokia | Symbian OS || phone
SEQ(SP=9E-B0%GCD=1-6%ISR=AF-B9%TI=I%II=I%SS=S%TS=13|14)
OPS(O1=M5B4T11W0SL%O2=M5B4T11W0SL%O3=M5B4T11W0LLL%O4=M5B4T11W0SL%O5=M5B4T11W0SL%O6=M5B4T11S)
WIN(W1=BC34%W2=BC34%W3=BC34%W4=BC34%W5=BC34%W6=BC34)
ECN(R=Y%DF=Y%T=40-4A%TG=80%W=BC34%O=M5B4W0SLLL%CC=N%Q=)
T1(R=Y%DF=Y%T=40-4A%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=40-4A%TG=80%W=BC34%S=O%A=S+%F=AS%O=M5B4T11W0SL%RD=0%Q=)
T4(R=Y%DF=N%T=40-4A%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=40-4A%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=40-4A%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=40-4A%TG=80%CD=S)

# Nokia E65 phone with Wifi turned on, *#0000# says "2.0633.65.01 03-10-07 RM 208 Nokia e65"
Fingerprint Nokia E65 mobile phone (Symbian OS)
Class Nokia | Symbian OS || phone
SEQ(SP=CB-D5%GCD=1-6%ISR=C8-D2%TI=Z%II=I%TS=8)
OPS(O1=M5B4ST11NW5%O2=M5B4ST11NW5%O3=M5B4NNT11NW5%O4=M5B4ST11NW5%O5=M5B4ST11NW5%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW5%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=40-4A%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=40-4A%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=40-4A%TG=80%CD=S)

# Nokia E70 Mobile Phone connected by Wifi, Software version 2.0618.07.10
Fingerprint Nokia E70 mobile phone (Symbian OS)
Class Nokia | Symbian OS || phone
SEQ(SP=A3-AD%GCD=1-6%ISR=B1-BB%TI=I%II=I%SS=O|S%TS=13|14)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=Y%T=40-4A%TG=80%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=40-4A%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=40-4A%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=40-4A%TG=80%CD=S)

# symbian s60 3rd edition ...nokia 81, test behind cisco asa in different vlan without acl
Fingerprint Nokia N81 mobile phone (Symbian OS)
Class Nokia | Symbian OS || phone
SEQ(SP=EE-10A%GCD=1-6%ISR=EC-110%TI=I%II=I%SS=S%TS=U)
OPS(O1=M564%O2=M564%O3=M564%O4=M564%O5=M564%O6=M564)
WIN(W1=BC34%W2=BC34%W3=BC34%W4=BC34%W5=BC34%W6=BC34)
ECN(R=Y%DF=Y%T=40-4A%TG=80%W=BC34%O=M564%CC=N%Q=)
T1(R=Y%DF=Y%T=40-4A%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=40-4A%TG=80%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=40-4A%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=40-4A%TG=80%CD=S)

# This is a Nortel CS1000M VOIP Call server
# Xerox Phaser 8560DT
Fingerprint Nortel CS1000M VoIP PBX or Xerox Phaser 8560DT printer
Class Nortel | embedded || PBX
Class Xerox | embedded || printer
SEQ(SP=FF-109%GCD=1-6%ISR=102-110%TI=I%TS=6)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=5F-69%TG=80%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=5F-69%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=5F-69%TG=80%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=5F-69%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=5F-69%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=5F-69%TG=80%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=5F-69%TG=80%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=5F-69%TG=80%IPL=70%UN=0%RIPL=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=5F-69%TG=80%CD=S)

# Nortel Ethernet Routing Switch 5530-24TFD, BOSS 4.2, HW:32  FW:4.2.0.12  SW:v4.2.0.002
Fingerprint Nortel 5530 Ethernet Routing Switch
Class Nortel | embedded || router
SEQ(SP=94-A2%GCD=1-6%ISR=9F-A9%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=2000%S=O%A=O%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# *** Ethernet Routing Switch 5520-48T-PWR                    ***
# *** BOSS 5.0 SSH                                            ***
#  *** HW:31       FW:5.0.0.2   SW:v5.0.0.011                  ***
# Nortel v5.0.1.0 Ethernet routing switch
Fingerprint Nortel 5520 Ethernet Routing Switch
Class Nortel | embedded || switch
SEQ(SP=95-9F%GCD=1-6%ISR=9B-A5%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Nortel DMS-10 telephony switch
Fingerprint Nortel DMS-10 telephony switch
Class Nortel | embedded || switch
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=1)
OPS(O1=M200NW0NNT11%O2=M200NW0NNT11%O3=M200NW0NNT11%O4=M200NW0NNT11%O5=M200NW0NNT11%O6=M200NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2017)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M200NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# ERS-8606 (5.1.1.1)
# Ethernet Routing Switch 8010 Software Release 4.1.2.0
Fingerprint Nortel ERS 8010 or 8606 switch
Class Nortel | embedded || switch
SEQ(SP=94-9E%GCD=1-6%ISR=9B-A5%TI=I%CI=I%II=RI%SS=O|S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Nortel Ethernet Routing Switch 4550T-PWR, v5.1.4.008
Fingerprint Nortel Ethernet Routing Switch 4550T-PWR
Class Nortel | embedded || switch
SEQ(SP=102-10C%GCD=1-6%ISR=105-10F%TI=I%CI=RD|RI%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=2A-42%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Sprint branded, Novatel MiFi 2200. WiFi to 3G modem. AP 11.43.7, Router 012, Modem 133
Fingerprint Novatel MiFi 2200 3G WAP
Class Novatel | embedded || WAP
SEQ(SP=C1-EB%GCD=1-6%ISR=D9-E9%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4W0L%O2=M5B4W0L%O3=M5B4W0L%O4=M5B4W0L%O5=M5B4W0L%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=6F-79%TG=80%W=2000%O=M5B4W0L%CC=N%Q=)
T1(R=Y%DF=N%T=6F-79%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=6F-79%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=6F-79%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=6F-79%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=6F-79%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=6F-79%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=8499%RUD=G)
IE(DFI=N%T=6F-79%TG=80%CD=Z)

# Novetel's MiFi 2200 device issued on Verizon's network, from WLAN interface
Fingerprint Novatel MiFi 2200 3G WAP
Class Novatel | embedded || WAP
SEQ(SP=CE-D8%GCD=1-6%ISR=D5-DF%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=N%T=75-7F%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=75-7F%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=75-7F%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=75-7F%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=75-7F%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=75-7F%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=215F%RUD=G)
IE(DFI=N%T=75-7F%TG=80%CD=Z)

# Novell NetWare 4.11 running under VMWare
# Netware 4.11 Virgin Install, with TCPIP NLM bound to Ethernet_II adapter on a VMWare Player instance
Fingerprint Novell NetWare 4.11
Class Novell | NetWare | 4.X | general purpose
SEQ(SP=C-16%GCD=10|20|30|40|50%ISR=3C-46%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=7D0%W2=7D0%W3=7D0%W4=7D0%W5=7D0%W6=7D0)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=7D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=7D0%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7B-85%TG=80%CD=S)

# Novell Netware 5
Fingerprint Novell NetWare 5
Class Novell | NetWare | 5.X | general purpose
SEQ(SP=FD-107%GCD=1-6%ISR=105-10F%TI=BI%II=BI%SS=S%TS=U)
OPS(O1=M5B4W0NSNN%O2=M578W0NSNN%O3=M280W0N%O4=M5B4W0NSNN%O5=M218W0NSNN%O6=M109SNN)
WIN(W1=17FF%W2=17FF%W3=17FF%W4=17FF%W5=17FF%W6=17FF)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=17FF%O=M5B4W0NSNN%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7B-85%TG=80%CD=S)

# Novell Netware 5.1
Fingerprint Novell NetWare 5.1
Class Novell | NetWare | 5.X | general purpose
SEQ(SP=F5-FF%GCD=1-6%ISR=107-111%TI=BI%II=BI%SS=O|S%TS=U)
OPS(O1=M5B4W0NSNN%O2=M578W0NSNN%O3=M280W0N%O4=M5B4W0NSNN%O5=M218W0NSNN%O6=M109SNN)
WIN(W1=17FF%W2=17FF%W3=17FF%W4=17FF%W5=17FF%W6=17FF)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=17FF%O=M5B4W0NSNN%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7B-85%TG=80%CD=S)

# Neware 6.5 with SP5
# Novell NetWare 6.0 Support Pack 5 on x86
# Novell NetWare 6.5 SP5 CPR Release, Server Version 5.70.05
# Novell Netware 6.5 German
# Novell Netware 6 Support Pack Revision 05, Server Version 5.60.05 May 27, 2004
Fingerprint Novell NetWare 6.0 or 6.5 SP5
Class Novell | NetWare | 6.X | general purpose
SEQ(SP=F5-10D%GCD=1-6%ISR=9A-111%TI=BI|RD|RI%II=BI|RI%SS=S%TS=U)
OPS(O1=M5B4W0NSNN%O2=M578W0NSNN%O3=M280W0N%O4=M5B4W0NSNN%O5=M218W0NSNN%O6=M109SNN)
WIN(W1=1800%W2=1800%W3=1800%W4=1800%W5=1800%W6=1800)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=1800%O=M5B4W0NSNN%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7B-85%TG=80%CD=S)

# novell netware 6.0
Fingerprint Novell NetWare 6.0 or 6.5 SP5
Class Novell | NetWare | 6.X | general purpose
SEQ(SP=FF-109%GCD=1-6%ISR=107-111%TI=BI%CI=BI%II=BI%SS=S%TS=U)
OPS(O1=M5B4W1NSNN%O2=M578W1NSNN%O3=M280W1N%O4=M5B4W1NSNN%O5=M218W1NSNN%O6=M109SNN)
WIN(W1=1800%W2=1800%W3=1800%W4=1800%W5=1800%W6=1800)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=1800%O=M5B4W1NSNN%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7B-85%TG=80%CD=S)

# Novell NetWare 6.5
Fingerprint Novell NetWare 6.5
Class Novell | NetWare | 6.X | general purpose
SEQ(SP=F1-FB%GCD=1-6%ISR=FC-106%TI=RD%II=BI|RI%TS=U)
OPS(O1=M5B4W2NSNN%O2=M578W2NSNN%O3=M280W2N%O4=M5B4W2NSNN%O5=M218W2NSNN%O6=M109SNN)
WIN(W1=1800%W2=1800%W3=1800%W4=1800%W5=1800%W6=1800)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=1800%O=M5B4W2NSNN%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7B-85%TG=80%CD=S)

# 6.5 sp 3 or sp 5
Fingerprint Novell NetWare 6.5
Class Novell | NetWare | 6.X | general purpose
SEQ(SP=F7-105%GCD=1-6%ISR=109-113%TI=BI%CI=BI%TS=U)
OPS(O1=M5B4W2NSNN%O2=M578W2NSNN%O3=M280W2N%O4=M5B4W2NSNN%O5=M218W2NSNN%O6=M109SNN)
WIN(W1=1800%W2=1800%W3=1800%W4=1800%W5=1800%W6=1800)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=1800%O=M5B4W2NSNN%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(R=N)
IE(R=N)

# Novell Open Enterprise Server 6.5 Server Version 5.7.06
Fingerprint Novell NetWare 6.5 Open Enterprise Server
Class Novell | NetWare | 6.X | general purpose
SEQ(R=N)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=0%O=%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=Z%A=S+%F=AR%RD=0%Q=)
T2(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7B-85%TG=80%CD=S)

# Novell Open Enterprise Server, NetWare 6.5, Support Pack 06
# Novell NetWare 6.5
Fingerprint Novell NetWare 6.5 Open Enterprise Server SP6
Class Novell | NetWare | 6.X | general purpose
SEQ(SP=FE-10D%GCD=1-6%ISR=105-10F%TI=BI%II=BI%SS=S%TS=U)
OPS(O1=M5B4W2NSNN%O2=M578W2NSNN%O3=M280W2N%O4=M5B4W2NSNN%O5=M218W2NSNN%O6=M109SNN)
WIN(W1=1800%W2=1800%W3=1800%W4=1800%W5=1800%W6=1800)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=1800%O=M5B4W2NSNN%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7B-85%TG=80%CD=S)

# Novell Open Enterprise Server (NW6.5) SP3 - Running Bordermanager 3.8 SP4
Fingerprint Novell NetWare 6.5 SP3 Open Enterprise Server
Class Novell | NetWare | 6.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=104-10E%TI=BI%II=BI%SS=S%TS=U)
OPS(O1=M5B4W0NSNN%O2=M578W0NSNN%O3=M280W0N%O4=M5B4W0NSNN%O5=M218W0NSNN%O6=M109SNN)
WIN(W1=17FF%W2=17FF%W3=17FF%W4=17FF%W5=17FF%W6=17FF)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=17FF%O=M5B4W0NSNN%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7B-85%TG=80%CD=S)

# Novell NetWare 6.5 SP 5
# Novell Open Enterprise Server, Netware 6.5
Fingerprint Novell NetWare 6.5 SP5
Class Novell | NetWare | 6.X | general purpose
SEQ(SP=FD-10B%GCD=1-6%ISR=108-112%TI=BI|RD|RI%II=BI|RI%SS=S%TS=U)
OPS(O1=M5B4W0NSNN%O2=M578W0NSNN%O3=M280W0N%O4=M5B4W0NSNN%O5=M218W0NSNN%O6=M109SNN)
WIN(W1=1800%W2=1800%W3=1800%W4=1800%W5=1800%W6=1800)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=1800%O=M5B4W0NSNN%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7B-85%TG=80%CD=S)

# Netware 6.5 SP7
Fingerprint Novell NetWare 6.5 SP7
Class Novell | NetWare | 6.X | general purpose
SEQ(SP=101-10B%GCD=1-6%ISR=103-10D%TI=BI%II=BI%SS=S%TS=U)
OPS(O1=M5B4W2N%O2=M578W2N%O3=M280W2N%O4=M5B4W2N%O5=M218W2N%O6=M109)
WIN(W1=1800%W2=1800%W3=1800%W4=1800%W5=1800%W6=1800)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=1800%O=M5B4W2N%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7B-85%TG=80%CD=S)

# NRG C7521n printer
Fingerprint NRG C7521n printer
Class NRG | embedded || printer
SEQ(SP=CC-DC%GCD=1-6%ISR=D8-E2%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# NRG MP C 4500 printer/multifunction
Fingerprint NRG MP C4500 printer
Class NRG | embedded || printer
SEQ(SP=D0-DC%GCD=1-6%ISR=D7-E1%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Device is a NTI Enviromux-Mini at firmware version 1.38 http://www.networktechinc.com/enviro-mini.html
Fingerprint NTI Enviromux-Mini environmental monitoring appliance
Class NTI | embedded || specialized
SEQ(SP=0-5%GCD=388|710|A98|E20|11A8%ISR=64-6E%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1800%W2=1800%W3=1800%W4=1800%W5=1800%W6=1800)
ECN(R=Y%DF=N%T=100%TG=FF%W=1800%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=100%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=100%TG=FF%W=1800%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=4801%RID=4210%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=N%T=100%TG=FF%CD=Z)

# The Nut/OS 4.3.2 beta operating system from Egnite, running on an ARM AT91SAM7X evaluation kit board with the HTTP server demo app. (Web site: http://www.ethernut.de/)
Fingerprint Nut/OS 4.3.2 beta (ARM)
Class Nut/OS | Nut/OS | 4.X | general purpose
SEQ(SP=0-5%GCD=1-6%ISR=14-1E%TI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=C90%W2=C90%W3=C90%W4=C90%W5=C90%W6=C90)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=C90%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=C90%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Oki Model number B4545
Fingerprint Oki B4545 printer
Class Oki | embedded || printer
SEQ(SP=FA-106%GCD=1-6%ISR=103-10D%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1388%W2=1388%W3=1388%W4=1388%W5=1388%W6=1388)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1388%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1388%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# OKI Printing Solutions C5510 MFP
Fingerprint Oki C5510 multifunction printer
Class Oki | embedded || printer
SEQ(SP=76-8E%GCD=1-6%ISR=98-A2%TI=I)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=2000%S=O%A=O%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(R=N)

# OKI Network Printer OKI-C5600-340179
# OKI printer, model C5650
Fingerprint Oki C5600 or C5650 printer
Class Oki | embedded || printer
SEQ(SP=F7-101%GCD=1-6%ISR=107-111%TI=I%II=I%SS=S%TS=5|6)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3A-44%TG=40%W=8000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3A-44%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3A-44%TG=40%W=8000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3A-44%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3A-44%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3A-44%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3A-44%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3A-44%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3A-44%TG=40%CD=S)

#  bootsector of the disk image: .........On Time RTOS-32 3.0 Disk Loader (c) 1996,2000 On Time Informatik GmbH.. (QEMU/KVM)
Fingerprint On Time RTOS-32 3.0
Class On Time | RTOS | 3.X | specialized
SEQ(SP=0-5%GCD=1-6%ISR=16-20%II=I%TS=A)
OPS(O1=M5B4T11NN%O2=M5B4T11NN%O3=M5B4T11NN%O4=M5B4T11NN%O5=M5B4T11NN%O6=M5B4T11NN)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3C%TG=40%W=16D0%O=M5B4T11NN%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=16D0%S=O%A=S+%F=AS%O=M5B4T11NN%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=Z)

# OnTime RTOS
Fingerprint On Time RTOS
Class On Time | RTOS || specialized
SEQ(SP=30-52%GCD=1000|2000|3000|4000|5000%ISR=94-AC%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4T11NN%O2=M5B4%O3=M5B4T11NN%O4=M5B4T11NN%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3C%TG=40%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=16D0%S=O%A=S+%F=AS%O=M5B4T11NN%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=Z)

# OneAccess One20 ADSL router (On UK LLU ADSL Line) From Internet (ADSL) side
Fingerprint OneAccess ONE20 ADSL router
Class OneAccess | embedded || broadband router
SEQ(SP=0-1D%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%TI=I%II=I%SS=S%TS=1)
OPS(O1=M200NW0NNT11%O2=M200NW0NNT11%O3=M200NW0NNT11%O4=M200NW0NNT11%O5=M200NW0NNT11%O6=M200NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M200NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=4801%RID=4210%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# OneAccess One20 ADSL Router (UK LLU ADSL) From Ethernet side.
Fingerprint OneAccess ONE20 ADSL router
Class OneAccess | embedded || broadband router
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=4801%RID=4210%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# uname -a = "OpenBSD <hostname> 2.8 BOBCAT#1 pmonmips"; Appliance = ONStor Bobcat 2220 NAS Gateway; Firmware = 1.3.3.5;
Fingerprint ONStor Bobcat 2220 NAS Gateway (runs OpenBSD 2.8)
Class ONStor | OpenBSD | 2.X | storage-misc
SEQ(SP=86-A0%GCD=1-6%ISR=98-A2%TI=RD%II=RI%TS=1)
OPS(O1=M200NNSNW0NNT11%O2=M200NNSNW0NNT11%O3=M200NW0NNT11%O4=M200NNSNW0NNT11%O5=M200NNSNW0NNT11%O6=M200NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M200NNSNW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M200NNSNW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=134%RID=G%RIPCK=I%RUCK=7A89%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 2.9 GENERIC#653 i386
Fingerprint OpenBSD 2.9 (x86)
Class OpenBSD | OpenBSD | 2.X | general purpose
SEQ(SP=FC-106%GCD=1-6%ISR=FF-10D%TI=RD%II=RI%TS=1)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4000%W5=4180%W6=403D)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4470%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=403D%S=O%A=S+%F=AS%O=M5B4NNSNW0NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=134%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 3.2 GENERIC#25 i386
Fingerprint OpenBSD 3.2 (x86)
Class OpenBSD | OpenBSD | 3.X | general purpose
SEQ(SP=EC-100%GCD=1-6%ISR=E2-10E%TI=RD%II=RI%TS=1)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4000%W5=4180%W6=403D)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4470%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=403D%S=O%A=O|S+%F=AS%O=M5B4NNSNW0NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=134%RID=G%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 3.3 GENERIC#25 i386
Fingerprint OpenBSD 3.3
Class OpenBSD | OpenBSD | 3.X | general purpose
SEQ(SP=F6-108%GCD=1-6%ISR=FF-10B%TI=RD%CI=RI%II=RI%TS=1)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4000%W5=4180%W6=403D)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4470%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=134%RID=G%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 3.4 GENERIC#18 i386     Device acting like firewall       pf version
Fingerprint OpenBSD 3.4 (x86)
Class OpenBSD | OpenBSD | 3.X | general purpose
SEQ(SP=F9-FF%GCD=1-6%ISR=100-107%TI=RD%II=RI%TS=1)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4000%W5=4180%W6=403D)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4470%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=403D%S=O%A=S+%F=AS%O=M5B4NNSNW0NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 3.5 GENERIC#34 i386
Fingerprint OpenBSD 3.5
Class OpenBSD | OpenBSD | 3.X | general purpose
SEQ(SP=FE-108%GCD=1-6%ISR=103-10D%TI=RD%II=RI%TS=1)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 3.6 GENERIC.MP#173 i386
Fingerprint OpenBSD 3.6 (x86)
Class OpenBSD | OpenBSD | 3.X | general purpose
SEQ(SP=F8-104%GCD=1-6%ISR=FF-109%TI=RD%II=RI%TS=1)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=O%A=O|S+%F=AS%O=M5B4NNSNW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 3.8 GENERIC#138 i386
# OpenBSD 4.6 GENERIC#58 i386
Fingerprint OpenBSD 3.8 - 4.6
Class OpenBSD | OpenBSD | 3.X | general purpose
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=FC-106%GCD=1-6%ISR=FE-10E%TI=RD%CI=RI%II=RI%TS=21|22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 3.9 GENERIC#3 i386 (pf and packet scrubbing turned off)
Fingerprint OpenBSD 3.9
Class OpenBSD | OpenBSD | 3.X | general purpose
SEQ(SP=101-10B%GCD=1-6%ISR=102-10C%TI=RD%II=RI%TS=21)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NNSNW0NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 3.9 GENERIC#0 i386
Fingerprint OpenBSD 3.9
Class OpenBSD | OpenBSD | 3.X | general purpose
SEQ(SP=F3-FD%GCD=1-6%ISR=FB-105%TI=RD%II=RI%TS=21|22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.0 sparc64
# OpenBSD 4.1 GENERIC#1435 i386
# OpenBSD 4.2 GENERIC#14 i386
# OpenBSD 3.9 GENERIC#617 i386 (Running pf with scrub in all)
Fingerprint OpenBSD 3.9 - 4.2
Class OpenBSD | OpenBSD | 3.X | general purpose
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=E5-109%GCD=1-6%ISR=FF-10B%TI=RD%II=I%TS=21|22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 3.9 GENERIC#759 sparc64 , Sun Ultra 5, UltraSPARC-IIi
# OpenBSD 3.9-stable (GENERIC) #0: Tue Aug 29 06:52:40 CDT 2006 (i386)
# OpenBSD 4.0 GENERIC#953 sparc64 SUNW,UltraSPARC-II @ 295.998 MHz, version 0 FPU
# OpenBSD 4.2 GENERIC#375 i386 (VMWare)
# OpenBSD 4.3 GENERIC#698 i386
# OpenBSD 4.4 GENERIC#1 i386
Fingerprint OpenBSD 3.9 - 4.4
Class OpenBSD | OpenBSD | 3.X | general purpose
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=CB-10C%GCD=1-6%ISR=FA-110%TI=RD%II=RI%TS=21|22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=O|S+%F=AS%O=M5B4NNSNW0NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.0-current (GENERIC) #1349: Tue Jan 16 16:55:56 MST 2007
Fingerprint OpenBSD 4.0
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=FA-104%GCD=1-6%ISR=FE-10A%TI=RD%TS=20|21)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# OpenBSD 4.0 POSTERN#0 i386
Fingerprint OpenBSD 4.0
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=F9-103%GCD=1-6%ISR=FE-108%TI=RD%II=RI%TS=21)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.0 GENERIC#1107 i386
Fingerprint OpenBSD 4.0
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=F4-104%GCD=1-6%ISR=F9-107%TI=RD%II=I%TS=20|21|22)
OPS(R=N)
WIN(R=N)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M578NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(R=N)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.0 (x86)
Fingerprint OpenBSD 4.0 (x86)
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=F3-106%GCD=1-6%ISR=100-10A%TI=RD%II=RI%TS=20|21|22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=O%A=O|S+%F=AS%O=M5B4NNSNW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.0 GENERIC#1107 i386
Fingerprint OpenBSD 4.0 (x86)
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=FE-108%GCD=1-6%ISR=102-10C%TI=RD%TS=21|22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# miniKabuki router developed by Computer Net Solutions running OpenBSD 4.1 NET4801#0 i386 on a Soekris 4801
Fingerprint OpenBSD 4.1
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=103-10D%TI=RD%II=RI%TS=22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.1 GENERIC#1435 i386
Fingerprint OpenBSD 4.1
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=103-10D%TI=RD%II=RI%TS=21)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.1 GENERIC#1435 i386
Fingerprint OpenBSD 4.1
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=F7-101%GCD=1-6%ISR=FC-106%TI=RD%II=RI%TS=22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.1 NET4801#1 i386
Fingerprint OpenBSD 4.1 (x86)
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=FE-108%GCD=1-6%ISR=FE-108%TI=RD%TS=22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NNSNW0NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.2 GENERIC#375 i386
# OpenBSD 4.1 GENERIC#0 i386
# OpenBSD 4.3 GENERIC#698 i386
# OpenBSD 4.3 GENERIC#698 i386
Fingerprint OpenBSD 4.1 - 4.3
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=100-10C%GCD=1-6%ISR=103-10F%TI=RD%II=RI%TS=21)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.1 GENERIC#1435 i386 (box acting as a router/traffic shaper.)
# OpenBSD 4.7 GENERIC.MP#130 amd64
Fingerprint OpenBSD 4.1 - 4.7
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=F4-106%GCD=1-6%ISR=FA-112%TI=RD%II=RI%TS=21|22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.2 running on Soekris 4801 acting as firewall/gateway
Fingerprint OpenBSD 4.2
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=F8-102%GCD=1-6%ISR=102-10C%TI=RD%TS=21)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NNSNW0NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.2 GENERIC#0 i386
Fingerprint OpenBSD 4.2
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=FD-107%GCD=1-6%ISR=107-111%TI=RD%II=RI%TS=21)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.2 GENERIC.MP#252 i386
Fingerprint OpenBSD 4.2
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=101-10F%TI=RD%TS=21)
OPS(O1=M8190NNSNW0NNT11%O2=M8190NNSNW0NNT11%O3=M8190NW0NNT11%O4=M8190NNSNW0NNT11%O5=M8190NNSNW0NNT11%O6=M8190NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M8190NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=O|S+%F=AS%O=M8190NNSNW0NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.2 GENERIC#375 i386
# OpenBSD 4.4 GENERIC amd64
Fingerprint OpenBSD 4.2 - 4.4
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=103-10D%GCD=1-6%ISR=104-110%TI=RD%II=RI%TS=22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.3 custom#6 amd64
Fingerprint OpenBSD 4.3
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=FD-107%GCD=1-6%ISR=107-111%TI=RD%II=RI%TS=22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.3 GENERIC#698 i386
Fingerprint OpenBSD 4.3
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=F5-FF%GCD=1-6%ISR=104-10E%TI=RD%TS=20)
OPS(R=N)
WIN(R=N)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=1223|55A7|5F73|5FB9|6723%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.3 GENERIC#698 i386
Fingerprint OpenBSD 4.3
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=FA-104%GCD=1-6%ISR=103-10D%TI=RD%TS=21)
OPS(R=N)
WIN(R=N)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=6127|813E|8A43|A205|AD7F%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.3 GENERIC#698 i386
Fingerprint OpenBSD 4.3
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=F9-105%GCD=1-6%ISR=105-10F%TI=RD%II=RI%TS=21|22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NNSNW0NNT11%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.3 GENERIC#698 i386
Fingerprint OpenBSD 4.3
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=FE-108%GCD=1-6%ISR=100-10E%TI=RD%II=RI%TS=21|22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=80%S=A%A=Z%F=R%O=%RD=44BD347E%Q=)
T3(R=Y%DF=N%T=1B-25%TG=20%W=100%S=A%A=Z%F=R%O=%RD=9C2E7B31%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=400%S=A%A=Z%F=R%O=%RD=44BD347E%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=8000%S=A%A=Z%F=R%O=%RD=44BD347E%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%S=A%A=Z%F=R%O=%RD=44BD347E%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.3 GENERIC.MP#587 i386
Fingerprint OpenBSD 4.3
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=F5-10B%GCD=1-6%ISR=107-111%TI=RD%TS=21)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=5F-69%TG=80%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=5F-69%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=5F-69%TG=80%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=5F-69%TG=80%W=4000%S=O%A=O|S+%F=AS%O=M5B4NNSNW0NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=5F-69%TG=80%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=5F-69%TG=80%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=5F-69%TG=80%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=5F-69%TG=80%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=250-25A%TG=FF%IPL=38%UN=0%RIPL=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=250-25A%TG=FF%CD=S)

# OpenBSD zaurus 4.3 GENERIC#207 zaurus
Fingerprint OpenBSD 4.3
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=FF-109%GCD=1-6%ISR=103-10D%TI=RD%II=RI%TS=21|22)
OPS(O1=M4D8NNSNW0NNT11%O2=M4D8NNSNW0NNT11%O3=M4D8NW0NNT11%O4=M4D8NNSNW0NNT11%O5=M4D8NNSNW0NNT11%O6=M4D8NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M4D8NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M4D8NNSNW0NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.4 GENERIC#968 i386
Fingerprint OpenBSD 4.4
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=F3-109%GCD=1-6%ISR=FC-114%TI=RD%II=RI%TS=21|22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NNSNW0NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.4 GENERIC#1021 i386
Fingerprint OpenBSD 4.4
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(R=N)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=Z%A=S+%F=AR%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.4 GENERIC#1021 i386
Fingerprint OpenBSD 4.4
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=101-10D%GCD=1-6%ISR=109-113%TI=RD%II=RI%TS=21|22)
OPS(O1=M578NNSNW0NNT11%O2=M578NNSNW0NNT11%O3=M578NW0NNT11%O4=M578NNSNW0NNT11%O5=M578NNSNW0NNT11%O6=M578NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M578NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.4 GENERIC#1021 i386
Fingerprint OpenBSD 4.4
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=FA-108%GCD=1-6%ISR=107-113%TI=RD%II=RI%TS=21|22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=80%S=A%A=Z%F=R%O=%RD=44BD347E%Q=)
T3(R=N)
T4(R=Y%DF=N%T=1B-25%TG=20%W=400%S=A%A=Z%F=R%O=%RD=44BD347E%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=8000%S=A%A=Z%F=R%O=%RD=44BD347E%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%S=A%A=Z%F=R%O=%RD=44BD347E%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.4 NET45xx#0 i386
Fingerprint OpenBSD 4.4
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=FB-109%GCD=1-6%ISR=104-10E%TI=RD%II=RI%TS=21|22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NNSNW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.4 GENERIC#1021 i386
Fingerprint OpenBSD 4.4
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=EE-108%GCD=1-6%ISR=F9-111%TI=RD%CI=RI%II=RI%TS=21|22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.4 GENERIC#1021 i386
# OpenBSD 4.6 KINTARO#0 i386
Fingerprint OpenBSD 4.4 - 4.6
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=F9-107%GCD=1-6%ISR=FF-10B%TI=RD%CI=RD%II=RI%TS=20)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=O|S+%F=AS%O=M5B4NNSNW0NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.5 GENERIC#1749 i386
Fingerprint OpenBSD 4.5
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=FF-109%GCD=1-6%ISR=106-112%TI=RD%II=RI%TS=21|22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.5 GENERIC#1749 i386
Fingerprint OpenBSD 4.5
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=F8-102%GCD=1-6%ISR=108-112%TI=RD%CI=RD%II=RI%TS=21)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.6 GENERIC#53 amd64
Fingerprint OpenBSD 4.6
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=FF-109%GCD=1-6%ISR=104-10E%TI=RD%CI=RI%II=RI%TS=21|22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.6 GENERIC#58 i386
# OpenBSD 4.6 GENERIC#58 i386, match in all scrub (no-df)
Fingerprint OpenBSD 4.6
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=102-10C%TI=RD%CI=RI%II=RI%TS=21)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.6 GENERIC#58 i386
Fingerprint OpenBSD 4.6
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=105-10F%TI=RD%CI=RI%II=RI%TS=U)
OPS(O1=M535%O2=M535%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=0%O=M535%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.6 GENERIC#0 i386
Fingerprint OpenBSD 4.6
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=101-10B%GCD=1-6%ISR=107-111%TI=RD%CI=RI%II=RI%TS=21|22)
OPS(O1=M5B4NNSNW0NNT11%O2=M5B4NNSNW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NNSNW0NNT11%O5=M5B4NNSNW0NNT11%O6=M5B4NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.7 GENERIC#558 i386
Fingerprint OpenBSD 4.7
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=FD-107%GCD=1-6%ISR=100-110%TI=RD%CI=RI%II=RI%TS=21|22)
OPS(O1=M558NNSNW0NNT11%O2=M558NNSNW0NNT11%O3=M558NW0NNT11%O4=M558NNSNW0NNT11%O5=M558NNSNW0NNT11%O6=M558NNSNNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M558NNSNW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# OpenBSD 4.8 GENERIC#0 i386
Fingerprint OpenBSD 4.8
Class OpenBSD | OpenBSD | 4.X | general purpose
SEQ(SP=FD-107%GCD=1-6%ISR=107-111%TI=RD%II=RI%TS=21)
OPS(O1=M5C0NNSNW3NNT11%O2=M5C0NNSNW3NNT11%O3=M5C0NW3NNT11%O4=M5C0NNSNW3NNT11%O5=M5C0NNSNW3NNT11%O6=M5C0NNSNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5C0NNSNW3%CC=Y%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# OpenIndiana build 147
Fingerprint OpenIndiana oi_147
Class OpenIndiana | OpenIndiana || general purpose
SEQ(SP=B0-BA%GCD=1-6%ISR=B4-BE%TI=I%CI=I%II=I%SS=S%TS=7)
OPS(O1=ST11M5B4NW1%O2=ST11M5B4NW1%O3=NNT11M5B4NW1%O4=ST11M5B4NW1%O5=ST11M5B4NW1%O6=ST11M5B4)
WIN(W1=FBB4%W2=FC1E%W3=FA38%W4=FABE%W5=FABE%W6=FFF7)
ECN(R=Y%DF=Y%T=38-42%TG=40%W=FAF0%O=M5B4NNSNW1%CC=Y%Q=)
T1(R=Y%DF=Y%T=38-42%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=38-42%TG=40%W=FA09%S=O%A=S+%F=AS%O=ST11M5B4NW1%RD=0%Q=)
T4(R=Y%DF=Y%T=3C-46%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C-46%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3C-46%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FB-105%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FB-105%TG=FF%CD=S)

# Linux 2.6.18-028stab023.1+31-openvz-smp, OpenVZ VE kernel.
Fingerprint OpenVZ Linux virtualization kernel (Linux 2.6.18-028stab023.1+31-openvz-smp)
Class OpenVZ | Linux | 2.6.X | general purpose
SEQ(SP=C4-CE%GCD=1-6%ISR=CA-D4%TI=Z%II=I%TS=A)
OPS(O1=M59CST11NW3%O2=M59CST11NW3%O3=M59CNNT11NW3%O4=M59CST11NW3%O5=M59CST11NW3%O6=M59CST11)
WIN(W1=1640%W2=1640%W3=1640%W4=1640%W5=1640%W6=1640)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1670%O=M59CNNSNW3%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1640%S=O%A=S+%F=AS%O=M59CST11NW3%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# USR/Sagem F@st 334 router (Wanadoo Livebox) (Wikipedia said : VxWorks and tweaked Linux)
# Orange.fr ISP adsl2 modem/router (aka LiveBox)
# Orange Livebox (Home ADSL Router)
Fingerprint Orange Livebox wireless DSL router or Sagem F@st 334 or 3304 DSL router
Class Orange | embedded || WAP
Class Sagem Communication | embedded || WAP
SEQ(SP=8E-98%GCD=1-6%ISR=92-9C%TI=I%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4074%W5=4180%W6=403D)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(R=N)

# Packard Bell NetStore 3500 network hard drive
Fingerprint Packard Bell NetStore 3500
Class Packard Bell | embedded || storage-misc
SEQ(SP=0-44%GCD=1-6%ISR=71-7B%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=4000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=1B-25%TG=20%W=4000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=1B-25%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=1B-25%TG=20%CD=S)

# Packet8 Broadband Phone Adapter BPA410
Fingerprint Packet8 BPA410 broadband phone adapter
Class Packet8 | embedded || VoIP adapter
SEQ(SP=0-5%GCD=834E00|1069C00|189EA00|20D3800|2908600|5210C00%ISR=E8-F2%TI=I%II=I%SS=S%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=578%W2=578%W3=578%W4=578%W5=578%W6=578)
ECN(R=N)
T1(R=Y%DF=Y%T=73-7D%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=73-7D%TG=80%W=578%S=O%A=S+%F=AS%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=73-7D%TG=80%W=578%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=73-7D%TG=80%W=578%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=73-7D%TG=80%W=578%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=73-7D%TG=80%W=578%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=73-7D%TG=80%IPL=148%UN=BA4C%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=I)
IE(DFI=Y%T=73-7D%TG=80%CD=Z)

# Packeteer 100 - Packeteer PacketShaper 5.2.0
Fingerprint Packeteer PacketShaper firewall version 5.2.0
Class Packeteer | embedded || firewall
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=96-A0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B0%O2=M5B0%O3=M5B0%O4=M5B0%O5=M5B0%O6=M5B0)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M5B0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Packeteer Packetshaper 6500/ISP runing 7.3.1g1
Fingerprint Packeteer PacketShaper 6500/ISP
Class Packeteer | pSOS || load balancer
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5B4%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# PacketFront DRG Ease DRG601-Access
Fingerprint PacketFront DRG Ease DRG601-Access switch
Class PacketFront | embedded || switch
SEQ(SP=9-13%GCD=9C4|1388|1D4C|2710|30D4%ISR=5A-6C%TI=I%CI=I%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=BB8%W2=BB8%W3=BB8%W4=BB8%W5=BB8%W6=BB8)
ECN(R=Y%DF=N%T=23-40%TG=40%W=BB8%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=25-40%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=20-3F%TG=40%W=BB8%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=20-3F%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=20-3A%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=Y%DF=N%T=23-3E%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Palmmicro VoIP phone (model AR1688, running version 0.22 of the firmware
Fingerprint Palmmicro AR1688 VoIP module
Class Palmmicro | embedded || VoIP phone
SEQ(SP=F7-107%GCD=1-6|8|10|18|20|28%ISR=103-113%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=5B4%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=7B-85%TG=80%W=5B4%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=7B-85%TG=80%CD=Z)

# Panasas ActiveStor Version 3.0.6.d
Fingerprint Panasas ActiveStor storage device (version 3.0.6.d)
Class Panasas | embedded || storage-misc
SEQ(SP=F2-10A%GCD=1-6%ISR=104-10E%TI=RI%II=I%SS=S%TS=A)
OPS(O1=M5B4NW4NNT11%O2=M5B4NW4NNT11%O3=M5B4NW4NNT11%O4=M5B4NW4NNT11%O5=M5B4NW4NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW4NNT11%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Panasonic DP-3520 (color laser printer)
# Panasonic DP-3510
Fingerprint Panasonic DB-3500 series printer
Class Panasonic | embedded || printer
SEQ(SP=B-21%GCD=A|14|1E|28|32|3C%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Panasonic DP-8045 digital imaging system
Fingerprint Panasonic DP-8045 printer
Class Panasonic | embedded || printer
SEQ(SP=D1-DB%GCD=1-6%ISR=D7-E1%TI=I%CI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT01%O2=M5B4NW0NNT01%O3=M5B4NW0NNT01%O4=M5B4NW0NNT01%O5=M5B4NW0NNT01%O6=M5B4NNT01)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=S+%F=AS%O=M5B4NW0NNT01%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Panasonic BB-HCM511A, Version 3.51R00
# BL-C140A web cam
Fingerprint Panasonic BB-HCM511A or BL-C140A Network Camera
Class Panasonic | embedded || webcam
SEQ(SP=CF-D9%GCD=1-6%ISR=D7-E1%TI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT01%O2=M5B4NW0NNT01%O3=M5B4NW0NNT01%O4=M5B4NW0NNT01%O5=M5B4NW0NNT01%O6=M5B4NNT01)
WIN(W1=800%W2=800%W3=800%W4=800%W5=800%W6=800)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=800%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=800%S=O%A=S+%F=AS%O=M5B4NW0NNT01%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Panasonic BL-C140
Fingerprint Panasonic BL-C140 Network Camera
Class Panasonic | embedded || webcam
SEQ(SP=CB-DD%GCD=1-6%ISR=D6-E0%TI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT01%O2=M5B4NW0NNT01%O3=M5B4NW0NNT01%O4=M5B4NW0NNT01%O5=M5B4NW0NNT01%O6=M5B4NNT01)
WIN(W1=800%W2=800%W3=800%W4=800%W5=800%W6=800)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=800%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=800%S=O%A=S+%F=AS%O=M5B4NW0NNT01%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Panasonic KX-HCM270, Firmware(Boot) 1.62, Firmware(Application) 1.62
Fingerprint Panasonic KX-HCM270 Network Camera
Class Panasonic | embedded || webcam
SEQ(SP=0-43%GCD=5|A|F|14|19|64|C8|12C|190|1F4%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Panasonic WV-NS202A
Fingerprint Panasonic WV-NS202A security camera
Class Panasonic | embedded || webcam
SEQ(SP=0-5%GCD=7A120|F4240|16E360|1E8480|2625A0%ISR=AD-B7%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M578NW0%O3=M280NW0%O4=M5B4NW0%O5=M218NW0%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=F3FBE867%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=F3FBE867%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=F3FBE867%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# 'papouch.com' Ethernet IP Thermometer of model type 'TME'
Fingerprint Papouch TME Ethernet thermometer
Class Papouch | embedded || specialized
SEQ(CI=I)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1FF%O=M400%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# TME Ethernet thermometer. TME v 1.6 www.papouch.com
Fingerprint Papouch TME Ethernet thermometer
Class Papouch | embedded || specialized
SEQ(SP=BF-DD%GCD=1-6%ISR=C0-DE%TI=I%II=I%SS=S%TS=U)
OPS(O1=|M400%O2=|M400%O3=|M400%O4=|M400%O5=|M400%O6=|M400)
WIN(W1=0|1FF%W2=0|1FF%W3=0|1FF%W4=0|1FF%W5=0|1FF%W6=0|1FF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=0|1FF%O=|M400%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O|Z%A=S+%F=AR|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=0|1FF%S=O|Z%A=S+%F=AR|AS%O=|M400%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Patton/Inalp (www.patton.com) Smartnode 4960 VoIP Gateway. OS is Smartware 4.2.
Fingerprint Patton SmartNode 4960 VoIP gateway (SmartWare 4.2)
Class Patton | SmartWare | 4.X | VoIP adapter
SEQ(SP=0-1D%GCD=0|8000|10000|18000|20000|28000%ISR=0-FB%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=7B-85%TG=80%W=1%S=Z%A=S%F=AR%O=%RD=0%Q=U)
T3(R=N)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=1%S=A%A=Z%F=R%O=%RD=0%Q=U)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=1%S=Z%A=S+%F=AR%O=%RD=0%Q=U)
T6(R=Y%DF=Y%T=7B-85%TG=80%W=1%S=A%A=Z%F=R%O=%RD=0%Q=U)
T7(R=Y%DF=Y%T=7B-85%TG=80%W=1%S=Z%A=S%F=AR%O=%RD=0%Q=U)
U1(DF=N%T=7B-85%TG=80%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7B-85%TG=80%CD=S)

# PC-BSD 1.3 (based on FreeBSD 6)
Fingerprint PC-BSD 1.3
Class PC-BSD | PC-BSD || general purpose
SEQ(SP=FC-10A%GCD=1-6%ISR=107-111%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Peplink Balance 380
Fingerprint Peplink Balance 380 router
Class Peplink | embedded || router
SEQ(SP=101-10B%GCD=1-6%ISR=105-10F%TI=Z%II=I%TS=8)
OPS(O1=M54EST11NW4%O2=M54EST11NW4%O3=M280NNT11NW4%O4=M22CST11NW4%O5=M218ST11NW4%O6=M109ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M54ENNSNW4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# PerfectOne IP-301 VOIP Phone.
Fingerprint Perfectone IP-301 VoIP phone
Class Perfectone | embedded || VoIP phone
SEQ(R=N)
OPS(O1=WANM5B4T10S%O2=M578W0ST10L%O3=T10NNW5NM280%O4=ST10WAL%O5=M218ST10WAL%O6=M109ST10)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=41%TG=40%W=0%O=WANM5B4SNN%CC=N%Q=R)
T1(R=Y%DF=N%T=41%TG=40%S=Z%A=S+%F=AR%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=41%TG=40%W=0%S=A%A=Z%F=R%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T6(R=Y%DF=Y%T=41%TG=40%W=0%S=A%A=Z%F=R%O=WANM109T10S%RD=0%Q=)
T7(R=N)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# IOLan DS1 serial io box by perle systems
Fingerprint Perle IOLAN DS1 Ethernet-to-serial bridge
Class Perle | embedded || bridge
SEQ(SP=C5-E1%GCD=1-6%ISR=CF-E1%TI=Z%II=I%TS=9)
OPS(O1=M5B4ST11NW1%O2=M5B4ST11NW1%O3=M5B4NNT11NW1%O4=M5B4ST11NW1%O5=M5B4ST11NW1%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW1%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Jetstream 8500 Terminal Server
# Perle JETset 3.6.0.G "CONSOLESERVER 9000"
# Specialix JETSTREAM 8500 RS232
Fingerprint Perle JetStream 8500 or CS 9000 remote access server
Class Perle | embedded || remote management
Class Perle | embedded || terminal server
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=800%W2=800%W3=800%W4=800%W5=800%W6=800)
ECN(R=Y%DF=N%T=3C%TG=40%W=800%O=M400%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=7FC%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# PharLap ETS 13 running LabVIEW Real-Time 8.5
Fingerprint Phar Lap ETS 13
Class Phar Lap | ETS | 13 | specialized
SEQ(SP=D7-E1%GCD=1-6%ISR=DB-E5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=130-13A%TG=FF%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=130-13A%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=130-13A%TG=FF%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=130-13A%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=6D-77%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=6D-77%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=6D-77%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=6D-77%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=82DC%RUD=G)
IE(DFI=N%T=6D-77%TG=80%CD=Z)

# PheeNet 802.11b/g High power access point
Fingerprint PheeNet WAP-854GP WAP
Class PheeNet | embedded || WAP
SEQ(SP=AF-CF%GCD=1-6%ISR=C7-D1%TI=Z%II=I%TS=8)
OPS(O1=M5B4ST11NW7%O2=M5B4ST11NW7%O3=M5B4NNT11NW7%O4=M5B4ST11NW7%O5=M5B4ST11NW7%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=35-3F%TG=40%W=16D0%O=M5B4NNSNW7%CC=N%Q=)
T1(R=Y%DF=Y%T=35-3F%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=36-40%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Philips ADSL Modem Multiservices PSTN Voice V2 Model: CIA6720NB/18
Fingerprint Philips CIA6720NB ADSL modem
Class Philips | embedded || broadband router
SEQ(SP=41-4B%GCD=1-6%ISR=49-53%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=1770%W2=1770%W3=1770%W4=1770%W5=1770%W6=1770)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1770%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N|Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N|S|Y%T=3B-45%TG=40%CD=Z)

# VoIP Phone. Philips DTERM. Vendor of nic is Nitsuko Corporation (00-60-b9).
Fingerprint Philips DTERM VoIP phone
Class Philips | embedded || media device
SEQ(SP=0-4E%GCD=3E8|7D0|BB8|FA0|1388|1E848|3D090|5B8D8|7A120|98968%ISR=9F-A9%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNSNNT11%O2=M578NW0NNSNNT11%O3=M280NW0NNT11%O4=M5B4NW0NNSNNT11%O5=M218NW0NNSNNT11%O6=M109NNSNNT11)
WIN(W1=21F0%W2=2088%W3=2258%W4=21F0%W5=20C0%W6=209D)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2238%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=209D%S=O%A=S+%F=AS%O=M109NW0NNSNNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Linux 2.1.24-TiVo-2.5 (ppc)
# Sony SVR-2000 Series 1 TiVo (runs Linux 2.1.24-TiVo-2.5 ppc)
# TiVo Series 1 Standalone [uname -a: Linux (none) 2.1.24-TiVo-2.5 #8 Wed May 8 15:38:27 PDT 2002 ppc unknown] (It's a Philips HDR112 (non-DirecTV))
# Philips TiVo DVR 2204 running software version 3.0-01-1-000, Linux (none) 2.1.24-TiVo-2.5 #8 Wed May 8 15:38:27 PDT 2002 ppc unknown
Fingerprint TiVo series 1 (Sony SVR-2000 or Philips HDR112) (Linux 2.1.24-TiVo-2.5, PowerPC)
Class Philips | Linux | 2.1.X | media device
Class Sony | Linux | 2.1.X | media device
SEQ(SP=AF-10A%GCD=1-6%ISR=105-111%TI=I|RD%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Pingtel xpressa VoIP phone
Fingerprint Pingtel Xpressa VoIP phone
Class Pingtel | embedded || VoIP phone
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B0NW0%O2=M5B0NW0%O3=M5B0NW0%O4=M5B0NW0%O5=M5B0NW0%O6=M5B0)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B0NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Pirelli DP10 GSM/VOIP Phone
Fingerprint Pirelli DP-10 VoIP phone
Class Pirelli | embedded || VoIP phone
SEQ(SP=E8-10A%GCD=1-6%ISR=106-110%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=3E80%W2=3E80%W3=3E80%W4=3E80%W5=3E80%W6=3E80)
ECN(R=Y%DF=N%T=7F%TG=80%W=3E80%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=7F%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7F%TG=80%W=3E80%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=7F%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7F%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7F%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7F%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7F%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7F%TG=80%CD=S)

# Pirelli Broadband Solutions:  pirelli modem adsl+wi-fi+voip, DRG A226M
Fingerprint Pirelli DRG A226M wireless ADSL modem
Class Pirelli | embedded || WAP
SEQ(SP=C0-CA%GCD=1-6%ISR=C0-CA%TI=Z%II=I%TS=8)
OPS(O1=M5B4ST11NW1%O2=M5B4ST11NW1%O3=M5B4NNT11NW1%O4=M5B4ST11NW1%O5=M5B4ST11NW1%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=19-23%TG=20%W=16D0%O=M5B4NNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=19-23%TG=20%W=16A0%S=O%A=O|S+%F=A|AS%O=NNT11|M5B4ST11NW1%RD=0%Q=)
T4(R=Y%DF=Y%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=19-23%TG=20%CD=S)

# Planet VoIP adapter, ATA-150S
Fingerprint Planet ATA-150S VoIP adapter
Class Planet | embedded || VoIP adapter
SEQ(SP=BE-C8%GCD=1-6%ISR=BF-C9%TI=Z%CI=Z%II=I%TS=7)
OPS(O1=M55CST11NW0%O2=M55CST11NW0%O3=M55CNNT11NW0%O4=M55CST11NW0%O5=M55CST11NW0%O6=M55CST11)
WIN(W1=1540%W2=1540%W3=1540%W4=1540%W5=1540%W6=1540)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1570%O=M55CNNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1540%S=O%A=S+%F=AS%O=M55CST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Planet VIP-550PT VoIP Phone
Fingerprint Planet VIP-550PT VoIP phone
Class Planet | embedded || VoIP phone
SEQ(SP=96-A0%GCD=1-6%ISR=9C-A6%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=8B-95%TG=FF%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=8B-95%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=8B-95%TG=FF%W=2000%S=O%A=O%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=8B-95%TG=FF%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=8B-95%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=8B-95%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=8B-95%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=8B-95%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=8B-95%TG=FF%CD=S)

# Planet WAP-1950, Firmware Version: 2.9.4, Hardware Version: 3.1
Fingerprint Planet WAP-1950 WAP
Class Planet | embedded || WAP
SEQ(SP=0-19%GCD=A|14|1E|28|32|6E|DC|14A|1B8|226%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=N)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Planet WAP 4000v2 soft ver. 2.05
Fingerprint Planet WAP-4000 v2 WAP
Class Planet | embedded || WAP
SEQ(SP=C-16%GCD=FA7F|1F4FE|2EF7D|3E9FC|4E47B%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=7F%TG=80%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=7F%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=7F%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=7F%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7F%TG=80%CD=S)

# Planet VoIP Phone Model VIP-154T, OS: MicroC/OS-II, uC/OS-II
Fingerprint Planet VIP-154T VoIP phone (MicroC/OS-II)
Class Planet | MicroC/OS-II || VoIP phone
SEQ(SP=0-21%GCD=FA|1F4|2EE|3E8|4E2%ISR=8A-94%TI=I%II=RI%SS=O%TS=U)
OPS(O1=WANM5B4T10S%O2=M578W0ST10L%O3=T10NNW5NM280%O4=ST10WAL%O5=M218ST10WAL%O6=M109ST10)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=WANM5B4SNN%CC=N%Q=R)
T1(R=Y%DF=N%T=3B-45%TG=40%S=Z%A=S+%F=AR%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IP 601
# IP 301
Fingerprint Polycom SoundPoint 301 or 601 IP phone
Class Polycom | embedded || VoIP phone
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M200%O2=M200%O3=M200%O4=M200%O5=M200%O6=M200)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M200%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=1042%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Polycom SoundPoint 320 (firmware 2.1.1.0037)
# Polycom SoundPoint IP 430, SIP stack version 2.1.0.2708
# Polycom SoundPoint IP 330/320.
# Polycom SoundPoint 550 IP phone
# Polycom IP650
Fingerprint Polycom SoundPoint 320, 330, 430, 550, or 650 IP phone
Class Polycom | embedded || VoIP phone
SEQ(SP=96-A0%GCD=1-6%ISR=9B-A5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=2000%S=O%A=O%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Polycom SoundPoint IP 601 Assembly: 2345-11605-001 Rev:A BootBlock: 2.6.0 (11605_001) Bootrom: 3.1.2.0011 06-Oct-05 14:29 ( Sip Version 1.6.4.0064 Poly DSP Orion Mem2 FS1 Version 1.3.3.0010 )
# Polycom version 2.12.0078
# SoundPoint IP 500
Fingerprint Polycom SoundPoint 500 or 601 IP phone
Class Polycom | embedded || VoIP phone
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Polycom Soundpoint 501
Fingerprint Polycom SoundPoint 501 IP phone
Class Polycom | embedded || VoIP phone
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# SoundPoint IP 501
Fingerprint Polycom SoundPoint 501 IP phone
Class Polycom | embedded || VoIP phone
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M564%O2=M564%O3=M564%O4=M564%O5=M564%O6=M564)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M564%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=80%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=100%S=A%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=400%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=8000%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=A%A=S+%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Polycom IP-301  Firmware Version:          Mon Jul 9 10:11:39 2007
Fingerprint Polycom SoundPoint IP 301 VoIP phone
Class Polycom | embedded || VoIP phone
SEQ(SP=0-5%GCD=3E8|7D0|BB8|FA0|1388%ISR=8A-94%TI=I%II=RI%SS=O%TS=U)
OPS(O1=M5B4|WANM5B4T10S%O2=M578|M578W0ST10L%O3=M280|T10NNW5NM280%O4=M5B4|ST10WAL%O5=M218ST10WAL%O6=M109ST10)
WIN(W1=0|3180%W2=0|3180%W3=0|3180%W4=0|3180%W5=0%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=WANM5B4SNN%CC=N%Q=R)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O|Z%A=S+%F=AR|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# PolyCom IP-301 VoIP Desktop Phone, I believe the polycom phones run embedded VxWorks OS.
Fingerprint Polycom SoundPoint IP 301 VoIP phone
Class Polycom | embedded || VoIP phone
SEQ(SP=97-A1%GCD=1-6%ISR=9C-A6%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Polycom IP 430 SIP VoIP Phone
Fingerprint Polycom SoundPoint IP 430 VoIP phone
Class Polycom | embedded || VoIP phone
SEQ(SP=95-9F%GCD=1-6%ISR=9B-A5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Polycom MGC Video Bridge (MCU) running software version 6.03
Fingerprint Polycom MGC videoconferencing system
Class Polycom | embedded || webcam
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Polycom ViewStation 4000 PRI T1 MP Release 6.0.5 FX
Fingerprint Polycom ViewStation 4000 video conferencing system
Class Polycom | embedded || webcam
SEQ(SP=0-16%GCD=0|6257C2|C4AF84|1270746|1895F08|1EBB6CA%ISR=0-C2%TI=I%CI=I%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=5B40%W2=5B40%W3=5B40%W4=5B40%W5=5B40%W6=5B40)
ECN(R=Y%DF=N%T=3C%TG=40%W=0|5B40%O=|M218%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=5B40%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=Y%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3C%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=70%UN=0|9CD7%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3C%TG=40%CD=Z)

# Polycom ViewStation DCP, Release 7.5.2 - 24 Dec 2003
Fingerprint Polycom ViewStation DCP 7.5.2 video conferencing system
Class Polycom | embedded || webcam
SEQ(SP=0-5%GCD=0%ISR=0-5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=5B40%W2=5B40%W3=5B40%W4=5B40%W5=5B40%W6=5B40)
ECN(R=Y%DF=N%T=3C%TG=40%W=5B40%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=5B40%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=Y%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=70%UN=EB93%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3C%TG=40%CD=Z)

# Polycom ViewStation 4000 PRI T1 MP, Release 6.0.5 FX - 08 Jun 2005
# Polycom ViewStation FX4 / Software Release 6.0.5 FX - 08 Jun 2005 / Boot Software BootUI Version 19.2 FX
# Polycom Viewstation FX Model: PN4-14xx
Fingerprint Polycom ViewStation video conferencing system
Class Polycom | embedded || webcam
SEQ(SP=0-18%GCD=1-6|>1000000%ISR=0-151%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=5B40%W2=5B40%W3=5B40%W4=5B40%W5=5B40%W6=5B40)
ECN(R=Y%DF=N%T=3C%TG=40%W=5B40%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=5B40%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=Y%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=70%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3C%TG=40%CD=Z)

# Polycom VS4000 Video conference codec.
Fingerprint Polycom VS4000 video conferencing system
Class Polycom | embedded || webcam
SEQ(SP=C-16%GCD=284D455|509A8AA|78E7CFF|A135154|C9825A9%ISR=CE-D8%TI=I%II=I%SS=S%TS=U)
OPS(O1=|M5B4%O2=|M5B4%O3=|M5B4%O4=|M5B4%O5=|M5B4%O6=|M5B4)
WIN(W1=0|5B40%W2=0|5B40%W3=0|5B40%W4=0|5B40%W5=0|5B40%W6=0|5B40)
ECN(R=Y%DF=N%T=3C%TG=40%W=0|5B40%O=|M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O|Z%A=S+%F=AR|AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=5B40%S=O%A=O|S+%F=A|AS%O=|M5B4%RD=0%Q=)
T4(R=Y%DF=Y%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=70%UN=3353%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3C%TG=40%CD=Z)

# Polycom VSFX4, Release 6.0.5 FX - 08 Jun 2005
Fingerprint Polycom VSFX4 video conferencing system
Class Polycom | embedded || webcam
SEQ(SP=0-16%GCD=8497DA1|1092FB42|18DC78E3|2125F684|296F7425%ISR=0-E5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=5B40%W2=5B40%W3=5B40%W4=5B40%W5=5B40%W6=5B40)
ECN(R=Y%DF=N%T=3C%TG=40%W=5B40%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=5B40%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=Y%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=70%UN=1D17|2520|29F6|E028%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3C%TG=40%CD=Z)

# Polycom Video Conferencing Device VSX 7000a, Release 8.5.3.2 - 17Apr2007 15:09
Fingerprint Polycom VSX 7000a video conferencing system
Class Polycom | embedded || webcam
SEQ(SP=3-7F%GCD=FA7F|1F4FE|2EF7D|3E9FC|4E47B%ISR=96-E6%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5A2%O2=M578%O3=M280%O4=M5A2%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=7F%TG=80%W=2000%O=M5A2%CC=N%Q=)
T1(R=Y%DF=N%T=7F%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7F%TG=80%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=7F%TG=80%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7F%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7F%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7F%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7F%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7F%TG=80%CD=S)

# Polycom VSX 7000e Video Conference
# Polycom VSX 8000 Video Conference
Fingerprint Polycom VSX 7000e/8000 video conferencing system
Class Polycom | embedded || webcam
SEQ(SP=C-16%GCD=FA7F|1F4FE|2EF7D|3E9FC|4E47B%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5A2%O2=M578%O3=M280%O4=M5A2%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2000%O=M5A2%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=19-23%TG=20%CD=S)

# Polycom VSX 8000 embedded OS.
Fingerprint Polycom VSX 8000 video conferencing system
Class Polycom | embedded || webcam
SEQ(SP=C-16%GCD=FA7F|1F4FE|2EF7D|3E9FC|4E47B%ISR=97-A1%II=I%TS=U)
OPS(O1=M5A2%O2=M578%O3=M280%O4=M5A2%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=2000%O=M5A2%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7B-85%TG=80%CD=S)

# Portech GSM VoIP GSM:900/1800MHz v6.0 gateway
Fingerprint PORTech GSM VoIP gateway
Class PORTech | embedded || VoIP adapter
SEQ(SP=0-16%GCD=FA|1F4|2EE|3E8|4E2|61A8|C350|124F8|186A0|1E848%ISR=8A-94%TI=I%II=RI%SS=O|S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=3180%W2=3180%W3=3180%W4=3180%W5=3180%W6=3180)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3180%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=3180%S=O%A=O|S+%F=APS%O=M109%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# VoIP GSM Gateway model: MV-370
Fingerprint PORTech MV-370 GSM VoIP gateway
Class PORTech | embedded || VoIP adapter
SEQ(SP=A-14%GCD=FA|1F4|2EE|3E8|4E2%ISR=8A-94%TI=I%II=RI%SS=S%TS=U)
OPS(O1=M5B4|WANM5B4T10S%O2=M578|M578W0ST10L%O3=M280|T10NNW5NM280%O4=M5B4|ST10WAL%O5=M218|M218ST10WAL%O6=M109ST10)
WIN(W1=3180%W2=3180%W3=3180%W4=3180%W5=3180%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=WANM5B4SNN%CC=N%Q=R)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O|Z%A=S+%F=AR|AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Printmax T5304r Printer using Ethernet Firmware 1.4.3.3
Fingerprint Printronix T5304 label printer
Class Printronix | embedded || printer
SEQ(SP=D-1B%GCD=1-6%ISR=30-3A%TI=I%CI=I%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M1AE%O5=M218%O6=M109)
WIN(W1=35C%W2=35C%W3=35C%W4=35C%W5=35C%W6=35C)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=35C%O=M578%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=1B-25%TG=20%W=35C%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(R=N)

# Priva building management system w/ HX08 IP module (www.priva.nl)
Fingerprint Priva building management system
Class Priva | embedded || specialized
SEQ(SP=C9-D3%GCD=1-6%ISR=D5-DF%TI=I%II=I%SS=S%TS=U)
OPS(O1=M54C|M5B4%O2=M54C|M578%O3=M280%O4=M200|M54C%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M54C|M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# Linux 2.6.15 #639 Sat Jun 21 02:13:26 CST 2008 ppc unknown (Synology DS207, Firmware version: DSM 2.0-0640)
# Linux ns2300n_050161 2.6.20.SR1 #103 Wed Mar 12 15:46:25 CST 2008 ppc unknown, SmartStor NS2300, Firmware version 01.05.0000.12
Fingerprint Promise SmartStor NS2300 or Synology DS207 NAS device (Linux 2.6.15 - 2.6.20)
Class Promise | Linux | 2.6.X | storage-misc
Class Synology | Linux | 2.6.X | storage-misc
SEQ(SP=BE-CD%GCD=1-6%ISR=C3-D1%TI=Z%II=I%TS=8)
OPS(O1=MF78ST11NW1%O2=MF78ST11NW1%O3=MF78NNT11NW1%O4=MF78ST11NW1%O5=MF78ST11NW1%O6=MF78ST11)
WIN(W1=2E44%W2=2E44%W3=2E44%W4=2E44%W5=2E44%W6=2E44)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2E68%O=MF78NNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=2E44%S=O%A=S+%F=AS%O=MF78ST11NW1%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Proxim Tsunami MP11a BSU (802.11a).
Fingerprint Proxim Tsunami MP.11a WAP
Class Proxim | embedded || WAP
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B8NW0NNT11%O2=M5B8NW0NNT11%O3=M5B8NW0NNT11%O4=M5B8NW0NNT11%O5=M5B8NW0NNT11%O6=M5B8NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B8NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# user mode network gateway in QEMU 0.12.3, built from MacPorts 1.8.2 on Mac OS X 10.6.2. (qemu -net nic -net user)
Fingerprint QEMU user mode network gateway
Class QEMU | QEMU || general purpose
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=96-A0%TI=I%CI=I|RD%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# QNAP TS-209 Pro running Linux 2.6.12.6-arm1
Fingerprint QNAP TS-209 NAS device (Linux 2.6.12.6-arm1)
Class QNAP | embedded || storage-misc
SEQ(SP=C5-CF%GCD=1-6%ISR=CC-D6%TI=Z%II=I%TS=7)
OPS(O1=M2304ST11NW2%O2=M2304ST11NW2%O3=M2304NNT11NW2%O4=M2304ST11NW2%O5=M2304ST11NW2%O6=M2304ST11)
WIN(W1=45F0%W2=45F0%W3=45F0%W4=45F0%W5=45F0%W6=45F0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4608%O=M2304NNSNW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=45F0%S=O%A=S+%F=AS%O=M2304ST11NW2%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# QNX 6.2, Hardware platform is JACE6
Fingerprint QNX 6.2
Class QNX | QNX | 6.X | general purpose
SEQ(SP=C4-DE%GCD=1-6%ISR=D7-E1%TI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT01%O2=M5B4NW0NNT01%O3=M5B4NW0NNT01%O4=M5B4NW0NNT01%O5=M5B4NW0NNT01%O6=M5B4NNT01)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# QNX 6.2.1 x86pc x86 on AMD K6/III 400 MHz
Fingerprint QNX 6.2.1 (x86)
Class QNX | QNX | 6.X | general purpose
SEQ(SP=C7-D7%GCD=1-6%ISR=D8-E2%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# QNX 6.3 with ftp and telnet enabled (VMWare)
Fingerprint QNX 6.3
Class QNX | QNX | 6.X | general purpose
SEQ(SP=C7-DB%GCD=1-6%ISR=D5-DF%TI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT01%O2=M5B4NW0NNT01%O3=M5B4NW0NNT01%O4=M5B4NW0NNT01%O5=M5B4NW0NNT01%O6=M5B4NNT01)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT01%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Guardian OS running on a Quantum Snap Server 2200 (now owned by Adaptec)
# SnapAppliance SnapServer 4100
Fingerprint Quantum Snap Server 2200 or 4100 NAS device
Class Quantum | embedded || storage-misc
SEQ(SP=0-5%GCD=12C00|25800|38400|4B000|5DC00%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2238%W2=2238%W3=2238%W4=2238%W5=2238%W6=2238)
ECN(R=Y%DF=N%T=1E%TG=20%W=2238%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1E%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=1E%TG=20%W=2238%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=1E%TG=20%W=2238%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1E%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1E%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1E%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Quantum Autoloader 3, identifies as V43.0 (002B.0h) (Changer part), 1923 (drive part)
Fingerprint Quantum SuperLoader 3 tape autoloader
Class Quantum | embedded || storage-misc
SEQ(SP=C-16%GCD=FA7F|1F4FE|2EF7D|3E9FC|4E47B%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=58F2|98E5|9D75|BF9B|C0D2%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=19-23%TG=20%CD=S)

# Quantum SuperLoader 3
Fingerprint Quantum SuperLoader 3 tape autoloader
Class Quantum | embedded || storage-misc
SEQ(SP=C-16%GCD=FA7F|1F4FE|2EF7D|3E9FC|4E47B%ISR=97-A1%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=200%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=19-23%TG=20%CD=S)

# desqview/x version 2.10, originally Quarterdeck they were bought out by symantec years ago
Fingerprint Quarterdeck DESQview/X 2.10
Class Quarterdeck | DESQview/X | 2.X | general purpose
SEQ(SP=0-16%GCD=10001|20002|30003|40004|50005|EFFFF|1DFFFE|2CFFFD|3BFFFC|4AFFFB%ISR=0-AC%TI=I%II=I%SS=S%TS=U)
OPS(O1=M240%O2=M578%O3=M240%O4=M240%O5=M218%O6=M109)
WIN(W1=480%W2=AF0%W3=480%W4=480%W5=430%W6=212)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=480%O=M240%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=O%A=O%F=AS%O=M240%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# RAD (www.rad.com) equipment - a RAD ACE 3200
Fingerprint RAD ACE-3200 telephony switch
Class RAD Data Communications | embedded || switch
SEQ(SP=92-A0%GCD=1-6%ISR=9B-A5%TI=I%TS=1)
OPS(O1=M606NW0NNT11%O2=M606NW0NNT11%O3=M606NW0NNT11%O4=M606NW0NNT11%O5=M606NW0NNT11%O6=M606NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M606NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=2000%S=O%A=O%F=AS%O=M606NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(R=N)

# AS2 - aplication switch 2 LinkProof Application Switch - with SynApps, DoS Shield v4.35.07
Fingerprint Radware LinkProof load balancer
Class Radware | embedded || load balancer
SEQ(SP=FF-109%GCD=1-6%ISR=103-10D%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=800%W2=800%W3=800%W4=800%W5=800%W6=800)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=800%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=800%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Raritan Dominion KX-II KVM switch, which runs linux: RFC1213-MIB::sysObjectID.0 = OID: NET-SNMP-TC::linux
Fingerprint Raritan Dominion KX II KVM switch
Class Raritan | embedded || specialized
SEQ(SP=C4-CE%GCD=1-6%ISR=CA-D4%TI=Z%TS=A)
OPS(O1=M5B4ST11NW1%O2=M5B4ST11NW1%O3=M5B4NNT11NW1%O4=M5B4ST11NW1%O5=M5B4ST11NW1%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3D-47%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3D-47%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3D-47%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3D-47%TG=40%W=0%S=A|O%A=O|S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3D-47%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# RCA Comcast DCM425C cable modem, firmware ST52.03.00
Fingerprint RCA DCM425C cable modem
Class RCA | embedded || broadband router
SEQ(SP=F4-FE%GCD=1-6%ISR=F4-102%TI=I%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4074%W5=4180%W6=403D)
ECN(R=Y%DF=Y%T=41%TG=40%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=41%TG=40%W=403D%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=41%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(R=N)

# ReactOS 0.3.7 with some default services started (shipped with ReactOS)
Fingerprint ReactOS 0.3.7
Class ReactOS | ReactOS | 0.3.X | general purpose
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%CI=I%TS=1)
OPS(O1=M200NW0NNT11%O2=M200NW0NNT11%O3=M200NW0NNT11%O4=M200NW0NNT11%O5=M200NW0NNT11%O6=M200NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M200NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(R=N)
IE(R=N)

# Red-M Communications Red-Alert PRO bluetooth/wifi activity detector
# MULTIBAND PROBE - Red-Alert PRO v4.1.20/2.6.5; http://www.red-m.com
# Linksys WET54G Version 3 Firmware version 2.07
Fingerprint Linksys WET54G wireless bridge or Red-M Communications Red-Alert PRO wireless activity detector
Class Red-M | embedded || firewall
Class Linksys | embedded || bridge
SEQ(SP=91-9B%GCD=1-6%ISR=98-A2%TI=RD%II=RI%TS=1)
OPS(O1=M5A8NW0NNT11%O2=M5A8NW0NNT11%O3=M5A8NW0NNT11%O4=M5A8NW0NNT11%O5=M5A8NW0NNT11%O6=M5A8NNT11)
WIN(W1=43E0%W2=4110|467C|4BE8|5154|56C0%W3=423C|44B0|4998|50F4|55DC%W4=43E0%W5=4180|4598|49B0|4FD4|55F8%W6=403D|4431|4A1F|500D|54FE)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=403D|4431|4A1F|500D|54FE%S=O%A=O|S+%F=AS%O=M5A8NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=3401%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Redback Networks router running SmartEdge OS Version SEOS-5.0.3.2-Release
# RedBack SmartEdge 100 SmartEdge OS 5.0.3.2
Fingerprint Redback Networks SmartEdge router running SmartEdge OS 5.0.3.2-Release
Class Redback | SmartEdge OS | 5.0.3.2 | broadband router
SEQ(SP=CD-DB%GCD=1-6%ISR=D8-E2%TI=I%II=I%SS=S%TS=1)
OPS(O1=M578NW0NNT11%O2=M578NW0NNT11%O3=M578NW0NNT11%O4=M578NW0NNT11%O5=M578NW0NNT11%O6=M578NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M578NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Revo Blik WiFi, a device using a Frontier Silicon Venice6 module using the Chorus2 DSP/processor.
Fingerprint Revo Blik Internet radio
Class Revo | embedded || media device
SEQ(SP=0-41%GCD=1-6|399-39F%ISR=64-6E%TI=I%II=RI%SS=O%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A+%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=51D4-51E1%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=24-3D%TG=40%CD=S)

# RFCode RFID Reader
Fingerprint RF Code RFID reader
Class RF Code | embedded || specialized
SEQ(SP=A3-B1%GCD=1-6%ISR=AD-B7%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=200%W2=200%W3=200%W4=200%W5=200%W6=200)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=200%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=200%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# RGB spectrum MediaWall 1500 video processor
Fingerprint RGB Spectrum MediaWall 1500 video processor
Class RGB Spectrum | embedded || media device
SEQ(SP=C5-CF%GCD=1-6%ISR=CA-D4%TI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW1%O2=M5B4ST11NW1%O3=M5B4NNT11NW1%O4=M5B4ST11NW1%O5=M5B4ST11NW1%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW1%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Ricoh Aficio 1022
Fingerprint Ricoh Aficio 1022 copier
Class Ricoh | embedded || printer
SEQ(SP=9C-A6%GCD=1-6%ISR=A7-B1%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# RICOH Aficio 1060 - version 3.53.3, network control service version 3.74
Fingerprint Ricoh Aficio 1060 copier
Class Ricoh | embedded || printer
SEQ(SP=9D-A7%GCD=1-6%ISR=A7-B1%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Aficio Ricoh AP400N Network Printer
# RICOH Aficio 1224C  2.07.2, Firmware Version: 3.74
Fingerprint Ricoh Aficio 1224C or AP400N printer
Class Ricoh | embedded || printer
SEQ(SP=98-B8%GCD=1-6%ISR=A7-B5%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Ricoh Aficio 2035e  System: 2.40 NIB: 4.12 Printer
Fingerprint Ricoh Aficio 2035e printer
Class Ricoh | embedded || printer
SEQ(SP=93-AF%GCD=1-6%ISR=A8-B2%TI=I%II=I%SS=S%TS=1|2)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# RICOH Aficio 3245C Copier, Printer, Scanner, Fax (MFP)
# RICOH Aficio 3045 - Copier, Printer, Scanner, Fax (MFP)
Fingerprint Ricoh Aficio 3045/3245C multifunction printer
Class Ricoh | embedded || printer
SEQ(SP=C2-DA%GCD=1-6%ISR=D7-E1%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Ricoh Aficio BP20N
Fingerprint Ricoh Aficio BP20N printer
Class Ricoh | embedded || printer
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# RICOH Aficio MP C2550
Fingerprint Ricoh Aficio MP C2550 printer
Class Ricoh | embedded || printer
SEQ(SP=CF-D9%GCD=1-6%ISR=D7-E1%TI=I%CI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT01%O2=M5B4NW0NNT01%O3=M5B4NW0NNT01%O4=M5B4NW0NNT01%O5=M5B4NW0NNT01%O6=M5B4NNT01)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT01%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# RICOH Aficio MP C6000 (printer, multifunction)
# Ricoh GX 3050N printer
Fingerprint Ricoh Aficio MP C6000 or GX3050N printer
Class Ricoh | embedded || printer
SEQ(SP=BA-DE%GCD=1-6%ISR=D9-E3%TI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT01%O2=M5B4NW0NNT01%O3=M5B4NW0NNT01%O4=M5B4NW0NNT01%O5=M5B4NW0NNT01%O6=M5B4NNT01)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# RICOH Aficio SP 4100N, Network Control Service Ver. 6.06
Fingerprint Ricoh Aficio SP 4100N printer
Class Ricoh | embedded || printer
SEQ(SP=CA-D8%GCD=1-6%ISR=D8-E2%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Ricoh SF210C Color Laser Printer
Fingerprint Ricoh Aficio SP C210SF printer
Class Ricoh | embedded || printer
SEQ(SP=F9-103%GCD=1-6%ISR=F1-FB%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=76-80%TG=80%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=76-80%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=76-80%TG=80%W=1000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=76-80%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=76-80%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=76-80%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=76-80%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=76-80%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=18D5%RUD=G)
IE(DFI=N%T=76-80%TG=80%CD=Z)

# Ricoh Aficio SP C311N
Fingerprint Ricoh Aficio SP C311N printer
Class Ricoh | embedded || printer
SEQ(SP=94-9E%GCD=1-6%ISR=9A-A4%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=5B4%S=O%A=O%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# RICOH Aficio SP C420DN printer
Fingerprint Ricoh Aficio SP C420DN printer
Class Ricoh | embedded || printer
SEQ(SP=C0-E4%GCD=1-6%ISR=D8-E2%TI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT01%O2=M5B4NW0NNT01%O3=M5B4NW0NNT01%O4=M5B4NW0NNT01%O5=M5B4NW0NNT01%O6=M5B4NNT01)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# RICOH Aficio SP 4100N printer
Fingerprint Ricoh Aficion SP 4100N printer
Class Ricoh | embedded || printer
SEQ(SP=D0-DA%GCD=1-6%ISR=D6-E0%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# DNNA RioKarma, MP3 player
Fingerprint Rio Karma media player
Class Rio | embedded || media device
SEQ(SP=89-9D%GCD=1-6%ISR=93-A1%TI=RD%CI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4470%W2=41A0%W3=4100%W4=4470%W5=40E8%W6=402E)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4470%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=402E%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=3401%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Risc OS 4.39 on an Acorn A7000+ running an FTP server.
# RISC OS Version 4.39
Fingerprint RISCOS Ltd RISC OS 4.39
Class RISCOS Ltd | RISC OS | 4.X | general purpose
SEQ(SP=93-9D%GCD=1-6%ISR=97-A1%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4180%W5=4180%W6=403D)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=403D%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Riverbed Steelhead 200
Fingerprint Riverbed Steelhead 200 proxy server
Class Riverbed | embedded || proxy server
SEQ(SP=C9-D3%GCD=1-6%ISR=C7-D1%TI=Z%II=I%TS=A)
OPS(O1=M550ST11NW2%O2=M550ST11NW2%O3=M550NNT11NW2%O4=M550ST11NW2%O5=M550ST11NW2%O6=M550ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M550NNSNW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Roberts Stream 202 internet radio
Fingerprint Roberts STREAM 202 Internet radio
Class Roberts | embedded || media device
SEQ(SP=0-61%GCD=1-6|DB8D3|DB8D6|1B71A6|1B71AC|292A79|292A82|36E34C|36E358|449C1F|449C2E%ISR=B4-BE%TI=I%CI=I%II=RI%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A+%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=8D3B|9F40%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=28-40%TG=40%CD=S)

# Rockwell Automation 1761-NET-ENI EtherNet/IP to RS-232-C Interface Module
Fingerprint Rockwell Automation 1761-NET-ENI Ethernet-to-RS-232-C interface module
Class Rockwell Automation | embedded || specialized
SEQ(R=N)
OPS(O1=M400%O2=M400%O3=M400%O4=%O5=%O6=)
WIN(W1=FF%W2=FF%W3=FF%W4=0%W5=0%W6=0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Rockwell Automation 1761-NET-ENI
Fingerprint Rockwell Automation 1761-NET-ENI Ethernet-to-RS-232-C interface module
Class Rockwell Automation | embedded || specialized
SEQ(SP=35-3F%GCD=100|200|300|400|500%ISR=8B-95%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=FF%W2=FF%W3=FF%W4=FF%W5=FF%W6=FF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FF%O=M400%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FF%S=Z%A=S+%F=AS%O=M400%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Rockwell 1769-L23E-QB1 PLC
Fingerprint Rockwell Automation 1769-L23E-QB1 PLC
Class Rockwell Automation | embedded || specialized
SEQ(SP=96-A0%GCD=1-6%ISR=9C-A6%TI=I|RD%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=|M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Roku HD1500 high definition network streaming appliance.
Fingerprint Roku HD1500 media player
Class Roku | embedded || media device
SEQ(SP=BB-C5%GCD=1-6%ISR=BE-C8%TI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=41%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=41%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=100%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=100%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=100%TG=FF%CD=S)

# Roku SoundBridge 1001, running software version 3.0.44
Fingerprint Roku SoundBridge M1001 music player
Class Roku | embedded || media device
SEQ(SP=10-1A%GCD=FA7F|1F4FE|2EF7D|3E9FC|4E47B%ISR=99-A3%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M108)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Roku Soundbridge Radio software version 3.0.44
# Roku SoundBridge M500 running software version 3.0.44
# Roku Soundbridge model M1000 firmware 3.0.44
Fingerprint Roku SoundBridge M500 or M1000 music player
Class Roku | embedded || media device
SEQ(SP=F-89%GCD=FA7F|1F4FE|2EF7D|3E9FC|4E47B%ISR=99-DB%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M108)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# RSA SecurID Appliance
Fingerprint RSA SecurID authentication appliance
Class RSA | embedded || specialized
SEQ(SP=C6-D0%GCD=1-6%ISR=C9-D3%TI=RD%CI=Z%II=I%TS=U)
OPS(O1=M514NW0NNS%O2=M514NW0NNS%O3=M514NW0NNS%O4=M514NW0NNS%O5=M514NW0NNS%O6=M514NNS)
WIN(W1=AC8|16D0%W2=AC8|16D0%W3=AC8|16D0%W4=AC8|16D0%W5=AC8|16D0%W6=AC8|16D0)
ECN(R=Y%DF=Y%T=3E%TG=40%W=AC8|16D0%O=M514NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3E%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3E%TG=40%W=AC8|16D0%S=O%A=S+%F=AS%O=M514NW0NNS%RD=0%Q=)
T4(R=Y%DF=Y%T=3F%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3E%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3F%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3F%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=40%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=40%TG=40%CD=S)

# Ruckus Wireless Zone Director model ZD1050 [Linux --Ed.]
Fingerprint Ruckus ZD1050 WAP
Class Ruckus | embedded || WAP
SEQ(SP=C9-D3%GCD=1-6%ISR=CE-D8%TI=Z%CI=I%II=I%TS=A)
OPS(O1=M5B4ST11NW3%O2=M5B4ST11NW3%O3=M5B4NNT11NW3%O4=M5B4ST11NW3%O5=M5B4ST11NW3%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW3%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# DSL router SAGEM F@st 3302, unknown firmware
Fingerprint Sagem F@st 3302 DSL router
Class Sagem Communication | embedded || broadband router
SEQ(SP=14-1E%GCD=7A00|F400|16E00|1E800|26200|2DC00%ISR=91-9B%TI=I%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4074%W5=4180%W6=403D)
ECN(R=N)
T1(R=Y%DF=N%T=3A-44%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3A-44%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(R=N)

# Sagem F@ST 3302 (C-BOX Upgraded to AliceBox)
Fingerprint Sagem F@st 3302 DSL router
Class Sagem Communication | embedded || broadband router
SEQ(SP=14-1E%GCD=7A00|F400|16E00|1E800|26200%ISR=90-9A%TI=I%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4074%W5=4180%W6=403D)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(R=N)

# SAGEM My Dual Radio 700
Fingerprint Sagem My du@l radio 700 Internet radio
Class Sagem Communication | embedded || media device
SEQ(R=N)
OPS(O1=M5B4%O2=%O3=%O4=%O5=%O6=)
WIN(W1=4470%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=%CC=N%Q=U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Samsung LE32B651 LCD TV with embedded lan card
Fingerprint Samsung LE32B651 TV
Class Samsung | embedded || media device
SEQ(SP=FA-104%GCD=1-6%ISR=103-10D%TI=I%CI=Z%II=I%SS=O%TS=7)
OPS(O1=M5B4NW8ST11%O2=M5B4NW8ST11%O3=M5B4NW8NNT11%O4=M5B4NW8ST11%O5=M5B4NW8ST11%O6=M5B4ST11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=2000%O=M5B4NW8NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Samsung CLX-3160FN Colour Laser Multi-Function
Fingerprint Samsung CLX-3160FN printer
Class Samsung | embedded || printer
SEQ(SP=E-18%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%TI=I%II=I%SS=S%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Samsung CLX-3175FW
Fingerprint Samsung CLX-3175RW printer
Class Samsung | embedded || printer
SEQ(SP=0-5%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=94-9E%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Samsung Office Serve 7200 Phone System
Fingerprint Samsung OfficeServ 7200 VoIP gateway
Class Samsung | embedded || VoIP adapter
SEQ(SP=100-10A%GCD=1-6%ISR=106-110%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=3354%W2=3354%W3=3354%W4=3354%W5=3354%W6=3354)
ECN(R=Y%DF=N%T=3C%TG=40%W=3354%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=3354%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=150%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=Z)

# Samsung i8910 HD phone, running Symbian 9.4, S60 5th Edition. 
Fingerprint Samsung i8910 mobile phone (Symbian OS 9.4)
Class Samsung | Symbian OS | 9.X | phone
SEQ(SP=A2-B0%GCD=1-6%ISR=AB-B5%TI=I%CI=I%II=I%SS=S%TS=14)
OPS(O1=M5B4NNT11NW0NNS%O2=M5B4NNT11NW0NNS%O3=M5B4NNT11NW0%O4=M5B4NNT11NW0NNS%O5=M5B4NNT11NW0NNS%O6=M5B4NNT11NNS)
WIN(W1=FAF0%W2=FAF0%W3=FAF0%W4=FAF0%W5=FAF0%W6=FAF0)
ECN(R=Y%DF=Y%T=40-4A%TG=80%W=FAF0%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=40-4A%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=40-4A%TG=80%W=FAF0%S=O%A=S+%F=AS%O=M5B4NNT11NW0NNS%RD=0%Q=)
T4(R=Y%DF=N%T=40-4A%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=40-4A%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=40-4A%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=40-4A%TG=80%CD=S)

# Sanyo PLC-XU88 network-attached video projector.
Fingerprint Sanyo PLC-XU88 digital video projector
Class Sanyo | embedded || media device
SEQ(SP=0-93%GCD=1000|2000|3000|4000|5000%ISR=36-EA%TI=I%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=80%W2=80%W3=80%W4=80%W5=80%W6=80)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(R=N)

# Savin 8025e
Fingerprint Savin 8025e multifunction printer
Class Savin | embedded || printer
SEQ(SP=D1-DD%GCD=1-6%ISR=D8-E2%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# SEL-2701 ethernet add on card
Fingerprint Schweitzer Engineering SEL-2701 Ethernet processor
Class Schweitzer Engineering | embedded || specialized
SEQ(R=N)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=Z%A=S+%F=AR%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Scientific Alanta WebSTAR DPC2100 v2.0.2r1242-040825
Fingerprint Scientific Atlanta WebSTAR DPC2100 cable modem
Class Scientific Atlanta | embedded || broadband router
SEQ(SP=CD-D7%GCD=1-6%ISR=106-110%TI=RD%II=RI%TS=A)
OPS(O1=M5B4NW0NNT11SLL%O2=M5B4NW0NNT11SLL%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11SLL%O5=M5B4NW0NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FECC%W2=FECC%W3=FECC%W4=FECC%W5=FECC%W6=FECC)
ECN(R=Y%DF=Y%T=41%TG=40%W=FECC%O=M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=41%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=B15|6266|B058|D453|DC21%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# WebSTAR EPC2203 epc2203-E10-5-v202r1257-060605
Fingerprint Scientific Atlanta WebSTAR EPC2203 cable modem
Class Scientific Atlanta | embedded || broadband router
SEQ(SP=FE-108%GCD=1-6%ISR=106-110%TI=I%II=I%SS=S%TS=8)
OPS(O1=|NNT11|M5B4NW0NNT11%O2=|NNT11|M5B4NW0NNT11%O3=|NNT11|M5B4NW0NNT11%O4=|NNT11|M5B4NW0NNT11%O5=|NNT11|M5B4NW0NNT11%O6=|NNT11|M5B4NNT11)
WIN(W1=0|43E0%W2=0|4110%W3=0|423C%W4=0|4074%W5=0|4180%W6=0|403D)
ECN(R=Y%DF=N|Y%T=3B-45%TG=40%W=0|4470%O=|M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N|Y%T=3B-45%TG=40%S=O|Z%A=O|S+%F=A|AR|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N|Y%T=3B-45%TG=40%W=0|403D%S=O|Z%A=O|S+%F=A|AR|AS%O=|NNT11|M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# SCO OpenServer 5.0.4
# SCO OpenServer, SCO_SV host 3.2 5.0.5 i386
# Unixware 7.0.1
# SCO OpenServer 5.0.2
Fingerprint SCO OpenServer 5.0.2 - 5.0.5
Class SCO | OpenServer | 5.X | general purpose
SEQ(SP=95-B7%GCD=1-6%ISR=A8-C0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=60F4%W2=60F4%W3=60F4%W4=60F4%W5=60F4%W6=60F4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=60F4%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=6041%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# SCO OpenServer (SCO_SV scosysv 3.2 5.0.7 i386) (VMWare)
# SCO OpenServer(TM) Release 5 (scosysv) (ttyp0), SCO_SV scosysv 3.2 5.0.7 i386 - on vmware
Fingerprint SCO OpenServer 5.0.7
Class SCO | OpenServer | 5.X | general purpose
SEQ(SP=FE-10C%GCD=1-6%ISR=104-10E%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=832C%W2=832C%W3=832C%W4=832C%W5=832C%W6=832C)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=832C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=8058%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# SCO Open Server 5.0.7 (sysv 3.2r5.0.7) i386 Kernel 2003-02-18
Fingerprint SCO OpenServer 5.0.7 (x86)
Class SCO | OpenServer | 5.X | general purpose
SEQ(SP=F3-FF%GCD=1-6%ISR=102-10C%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=60F4%W2=60F4%W3=60F4%W4=60F4%W5=60F4%W6=60F4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=60F4%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=6041%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# SCO Open Server 5.05
Fingerprint SCO OpenServer 5.05
Class SCO | OpenServer | 5.X | general purpose
SEQ(SP=AD-B7%GCD=1-6%ISR=B7-C1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=111C%W2=111C%W3=111C%W4=111C%W5=111C%W6=111C)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=111C%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=108C%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# SCO OpenServer 6.0 (VMware)
Fingerprint SCO OpenServer 6.0
Class SCO | OpenServer | 5.X | general purpose
SEQ(SP=A5-B9%GCD=1-6%ISR=B1-C3%TI=I%II=I%SS=S%TS=7|8)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=60F4%W2=60F4%W3=60F4%W4=60F4%W5=60F4%W6=60F4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=60F4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# SCO_SV 3.2 2 i386
# SCO openserver 3.2/5.0.5 i386
Fingerprint SCO UNIX 3.2
Class SCO | SCO UNIX | 3.X | general purpose
SEQ(SP=AF-B9%GCD=1-6%ISR=B4-C2%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=60F4%W2=60F4%W3=60F4%W4=60F4%W5=60F4%W6=60F4)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=60F4%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=6041%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=3B-45%TG=40%CD=S)

# SCO UNIX, SCO_SV 3.2v5.0.7 2003-02-18
Fingerprint SCO UNIX 3.2v5.0.7
Class SCO | SCO UNIX | 3.X | general purpose
SEQ(SP=FA-10C%GCD=1-6%ISR=106-110%TI=I%II=I%SS=S%TS=U)
OPS(O1=M564%O2=M564%O3=M564%O4=M564%O5=M564%O6=M564)
WIN(W1=60F4%W2=60F4%W3=60F4%W4=60F4%W5=60F4%W6=60F4)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=60F4%O=M564%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=6019%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=Y%T=3B-45%TG=40%CD=S)

# UnixWare 5 7.1.1 i386 x86at SCO UNIX_SVR5
Fingerprint SCO UnixWare 7.1.1
Class SCO | UnixWare | 7.X | general purpose
SEQ(SP=AC-B8%GCD=1-6%ISR=B4-BE%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=60F4%W2=60F4%W3=60F4%W4=60F4%W5=60F4%W6=60F4)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=60F4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=6041%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=3B-45%TG=40%CD=S)

# SCO Unixware 7.1.3
Fingerprint SCO UnixWare 7.1.3
Class SCO | UnixWare | 7.X | general purpose
SEQ(SP=9D-B7%GCD=1-6%ISR=A3-BD%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=60F4%W2=60F4%W3=60F4%W4=60F4%W5=60F4%W6=60F4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=60F4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=6041%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# SCO UnixWare 8.0.0
Fingerprint SCO UnixWare 8.0.0
Class SCO | UnixWare | 8.X | general purpose
SEQ(SP=A9-B9%GCD=1-6%ISR=B2-C0%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=60F4%W2=60F4%W3=60F4%W4=60F4%W5=60F4%W6=60F4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=60F4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# SecureComputing/SG550 Version 3.2.2, Linux version 2.4.31-uc0 (build@sgbuild)(gcc version 3.0.4)
Fingerprint Secure Computing SG550 firewall (Linux 2.4.31)
Class Secure Computing | Linux | 2.4.X | firewall
SEQ(SP=C3-CD%GCD=1-6%ISR=C8-D2%TI=Z%CI=Z%II=I%TS=7)
OPS(O1=M5ACST11NW0%O2=M5ACST11NW0%O3=M5ACNNT11NW0%O4=M5ACST11NW0%O5=M5ACST11NW0%O6=M5ACST11)
WIN(W1=1680%W2=1680%W3=1680%W4=1680%W5=1680%W6=1680)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16B0%O=M5ACNNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Secure Computing Firewall (SecureOS) Version: "Sidewinder 6.1.1.05"
Fingerprint Secure Computing Sidewinder firewall (SecureOS 6.1.1.05)
Class Secure Computing | SecureOS | 6.X | firewall
SEQ(SP=FD-10B%GCD=1-6%ISR=105-111%TI=RI%TS=1)
OPS(O1=M5B4NW4NNT11%O2=M5B4NW0NNT11%O3=M5B4NW4NNT11%O4=M5B4NW4NNT11%O5=M5B4NW4NNT11%O6=M5B4NNT11)
WIN(W1=4470%W2=41A0%W3=4100%W4=4000%W5=40E8%W6=402E)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4470%O=M5B4NW4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=402E%S=O%A=O|S+%F=AS%O=M5B4NW4NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Sidewinder G2 appliance running version 6.1.2.0.3
Fingerprint Secure Computing Sidewinder G2 firewall (SecureOS 6.1.2.0.3)
Class Secure Computing | SecureOS | 6.X| firewall
SEQ(SP=100-10A%GCD=1-6%ISR=105-10F%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW4NNT11%O2=M5B4NW0NNT11%O3=M5B4NW4NNT11%O4=M5B4NW4NNT11%O5=M5B4NW4NNT11%O6=M5B4NNT11)
WIN(W1=4470%W2=41A0%W3=4100%W4=4000%W5=40E8%W6=402E)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4470%O=M5B4NW4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# SecureOS 7.0.0.06 SW_OPS_SMP Mon Mar 31 15:47:25 CDT 2008 70006-b_0  i386
Fingerprint Secure Computing SecureOS 7.0.0.04
Class Secure Computing | SecureOS | 7.X | firewall
SEQ(SP=FA-108%GCD=1-6%ISR=107-111%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNT11SLL%O2=M5B4NW0NNT11SLL%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11SLL%O5=M5B4NW0NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3C-46%TG=40%W=8000%O=M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3C-46%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3C-46%TG=40%W=8000%S=O%A=S+%F=AS%O=M5B4NW0NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3C-46%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3C-46%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3C-46%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3C-46%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C-46%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=BBE8%RUD=G)
IE(DFI=S%T=3C-46%TG=40%CD=S)

# Secure Computing Sidewinder Firewall (SecureOS 7.0.0.04)
Fingerprint Secure Computing Sidewinder firewall (SecureOS 7.0.0.04)
Class Secure Computing | SecureOS | 7.X | firewall
SEQ(SP=FE-10D%GCD=1-6%ISR=103-10D%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NW0NNT11SLL%O2=M5B4NW0NNT11SLL%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11SLL%O5=M5B4NW0NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8000%O=M5B4NW0SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=8000%S=O%A=S+%F=AS%O=M5B4NW0NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Seiko NS2232 Terminal/Communications Server
# Seiko Instruments NS2232 (terminal server) Firmware version 2.0B2
Fingerprint Seiko NS-2232 serial-to-IP bridge
Class Seiko | embedded || bridge
SEQ(SP=20-B0%GCD=1-6%ISR=7B-85%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=800%W2=800%W3=800%W4=800%W5=800%W6=800)
ECN(R=Y%DF=N%T=3C%TG=40%W=800%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=0|800%S=O|Z%A=O%F=A|AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=S)

# Senao NL-2611CB3 Plus Deluxe, firmware version 2.0.2
Fingerprint Senao NL-2611CB3 PLUS WAP
Class Senao | embedded || WAP
SEQ(SP=A5-AF%GCD=1-6%ISR=AB-B5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=800%W2=800%W3=800%W4=800%W5=800%W6=800)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=800%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=800%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# The device is a Sensatronics Temperature Monitor, model E4.
Fingerprint Sensatronics E4 temperature monitor
Class Sensatronics | embedded || specialized
SEQ(SP=43-B7%GCD=200|400|600|800|A00|10000|20000|30000|40000|50000%ISR=10B-115%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=400%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Sensatronics Model: EM1 Firmware Version: 5.3
Fingerprint Sensatronics EM1 environmental monitor
Class Sensatronics | embedded || specialized
SEQ(SP=6A-7A%GCD=10000|20000|30000|40000|50000%ISR=10A-114%TI=I%II=I%SS=S%TS=U)
OPS(O1=M230%O2=M230%O3=M230%O4=M218%O5=M218%O6=M109)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=400%O=M230%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Sequent Dynix.
Fingerprint Sequent DYNIX (BSD-based Unix)
Class Sequent | DYNIX || general purpose
SEQ(SP=0-5%GCD=61A8|C350|124F8|186A0|1E848%ISR=8A-94%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=G%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# SGI Indigo running IRIX 4.0.5F uname: IRIX 4.0.5F 08280217 IP20
Fingerprint SGI IRIX 4.0.5F
Class SGI | IRIX | 4.X | general purpose
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=96-A0%TI=I%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=EF88%W2=EB28%W3=F000%W4=F000%W5=EEB0%W6=EF1F)
ECN(R=Y%DF=N%T=3C%TG=40%W=EF88%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=EF1F%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=F000%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IRIX 5.2 02282013 IP12 mips
Fingerprint SGI IRIX 5.2
Class SGI | IRIX | 5.X | general purpose
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%CI=I%II=I%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=ED90%W2=EE90%W3=EDF4%W4=F000%W5=EF7C%W6=EF2A)
ECN(R=Y%DF=N%T=37-41%TG=40%W=EF88%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=37-41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=37-41%TG=40%W=EF2A%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=37-41%TG=40%W=F000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=37-41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=37-41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=37-41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# SGI 5.3 1109812 IP22 mips, SGI indy, R4600, 133MHz.  Fresh install of IRIX 5.3
Fingerprint SGI IRIX 5.3
Class SGI | IRIX | 5.X | general purpose
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=1|2)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=ED90%W2=EE90%W3=EDF4%W4=F000%W5=EF7C%W6=EF2A)
ECN(R=Y%DF=N%T=3C%TG=40%W=EF88%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=EF2A%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=F000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IRIX 6.5 10070056 IP32
# IRIX 6.5 07202013 IP32
Fingerprint SGI IRIX 6.5
Class SGI | IRIX | 6.X | general purpose
SEQ(SP=36-46%GCD=3E8|7D0|BB8|FA0|1388|FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11NNS%O2=M5B4NW0NNT11NNS%O3=M5B4NW0NNT11NNS%O4=M5B4NW0NNT11NNS%O5=M5B4NW0NNT11NNS%O6=M5B4NNT11NNS)
WIN(W1=ED90%W2=EE90%W3=EDF4%W4=F000%W5=EF7C%W6=EF2A)
ECN(R=Y%DF=Y%T=3C%TG=40%W=EF88%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=EF2A%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IRIX 6.5 6.5.15m 01091821 IP32
Fingerprint SGI IRIX 6.5.15m
Class SGI | IRIX | 6.X | general purpose
SEQ(SP=C-9C%GCD=80|100|180|200|280|FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11NNS%O2=M5B4NW0NNT11NNS%O3=M5B4NW0NNT11NNS%O4=M5B4NW0NNT11NNS%O5=M5B4NW0NNT11NNS%O6=M5B4NNT11NNS)
WIN(W1=ED90%W2=EE90%W3=EDF4%W4=F000%W5=EF7C%W6=EF2A)
ECN(R=Y%DF=Y%T=3C%TG=40%W=EF88%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=EF2A%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IRIX 6.5.22m on an SGI Indigo2
# IRIX 6.5; uname: IRIX 6.5 6.5.22m IP22; on: Silicon Graphics Indigo2 Impact R4400
# IRIX 6.5 10070056 IP32
# IRIX 6.5 6.5.30f 07202013 IP32
Fingerprint SGI IRIX 6.5.22m - 6.5.30f
Class SGI | IRIX | 6.X | general purpose
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=95-9F%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11NNS|M2048NW0NNT11NNS%O2=M5B4NW0NNT11NNS|M2048NW0NNT11NNS%O3=M5B4NW0NNT11NNS|M2048NW0NNT11NNS%O4=M5B4NW0NNT11NNS|M2048NW0NNT11NNS%O5=M5B4NW0NNT11NNS|M2048NW0NNT11NNS%O6=M5B4NNT11NNS|M2048NNT11NNS)
WIN(W1=ED90%W2=EE90%W3=EDF4%W4=F000%W5=EF7C%W6=EF2A)
ECN(R=Y%DF=Y%T=3C%TG=40%W=EF88%O=M5B4NW0NNS|M2048NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=EF2A%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IRIX 6.5 07202013 IP32 (6.5.30)
Fingerprint SGI IRIX 6.5.30
Class SGI | IRIX | 6.X | general purpose
SEQ(SP=8A-94%GCD=1-6|8%ISR=97-A1%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11NNS%O2=M5B4NW0NNT11NNS%O3=M5B4NW0NNT11NNS%O4=M5B4NW0NNT11NNS%O5=M5B4NW0NNT11NNS%O6=M5B4NNT11NNS)
WIN(W1=ED90%W2=EE90%W3=EDF4%W4=F000%W5=EF7C%W6=EF2A)
ECN(R=Y%DF=Y%T=3C%TG=40%W=EF88%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=EF2A%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IRIX 6.5 10181058 IP22, Indigo2 with a R4400 processor, running IRIX 6.5.6m.
Fingerprint SGI IRIX 6.5.6m
Class SGI | IRIX | 6.X | general purpose
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=ED90%W2=EE90%W3=EDF4%W4=F000%W5=EF7C%W6=EF2A)
ECN(R=Y%DF=Y%T=3B%TG=40%W=EF88%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B%TG=40%W=EF2A%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FE%TG=FF%CD=S)

# IRIX64 iris11 6.5 04101931 IP30
Fingerprint SGI IRIX64 6.5
Class SGI | IRIX | 6.X | general purpose
SEQ(SP=4E-C0%GCD=1-6|50|A0|F0|140|190%ISR=97-A1%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11NNS%O2=M5B4NW0NNT11NNS%O3=M5B4NW0NNT11NNS%O4=M5B4NW0NNT11NNS%O5=M5B4NW0NNT11NNS%O6=M5B4NNT11NNS)
WIN(W1=C000%W2=C000%W3=C000%W4=C000%W5=C000%W6=C000)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C000%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IRIX64 6.5 10181058 IP30
Fingerprint SGI IRIX64 6.5
Class SGI | IRIX | 6.X | general purpose
SEQ(SP=58-62%GCD=50|A0|F0|140|190%ISR=97-A1%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=C000%W2=C000%W3=C000%W4=C000%W5=C000%W6=C000)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=C000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IRIX64 6.5 07202013 IP30
Fingerprint SGI IRIX64 6.5
Class SGI | IRIX | 6.X | general purpose
SEQ(SP=6D-77%GCD=10|20|30|40|50%ISR=98-A2%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11NNS%O2=M5B4NW0NNT11NNS%O3=M5B4NW0NNT11NNS%O4=M5B4NW0NNT11NNS%O5=M5B4NW0NNT11NNS%O6=M5B4NNT11NNS)
WIN(W1=C000%W2=C000%W3=C000%W4=C000%W5=C000%W6=C000)
ECN(R=Y%DF=Y%T=38-42%TG=40%W=C000%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=38-42%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=38-42%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=38-42%TG=40%W=C000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=38-42%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=38-42%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=38-42%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=38-42%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=100%TG=FF%CD=S)

# IRIX64 6.5 07202013 IP35
Fingerprint SGI IRIX64 6.5
Class SGI | IRIX | 6.X | general purpose
SEQ(SP=3F-87%GCD=20|40|60|80|A0|320|640|960|C80|FA0%ISR=97-A1%CI=I%II=I%TS=1)
OPS(O1=M5B4NW2NNT11NNS%O2=M5B4NW2NNT11NNS%O3=M5B4NW2NNT11NNS%O4=M5B4NW3NNT11NNS%O5=M5B4NW2NNT11NNS%O6=M5B4NW2NNT11NNS)
WIN(W1=C000%W2=C000%W3=C000%W4=C000%W5=C000%W6=C000)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C000%O=M5B4NW2NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=C000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IRIX64 6.5 07202013 IP35
Fingerprint SGI IRIX64 6.5
Class SGI | IRIX | 6.X | general purpose
SEQ(SP=FE-10C%GCD=1-6%ISR=106-110%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW2NNT11NNS%O2=M5B4NW2NNT11NNS%O3=M5B4NW2NNT11NNS%O4=M5B4NW3NNT11NNS%O5=M5B4NW2NNT11NNS%O6=M5B4NW2NNT11NNS)
WIN(W1=C000%W2=C000%W3=C000%W4=C000%W5=C000%W6=C000)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C000%O=M5B4NW2NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=C000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# SGI IRIX64 6.5.15m
# IRIX64 6.5 01091821 IP35
Fingerprint SGI IRIX64 6.5.15m
Class SGI | IRIX | 6.X | general purpose
SEQ(SP=3E-8E%GCD=20|40|50|60|80|A0|C0|320|640|960|C80|FA0|12C0|1900|1F40|2580%ISR=97-A1%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11NNS%O2=M5B4NW0NNT11NNS%O3=M5B4NW0NNT11NNS%O4=M5B4NW0NNT11NNS%O5=M5B4NW0NNT11NNS%O6=M5B4NNT11NNS)
WIN(W1=C000%W2=C000%W3=C000%W4=C000%W5=C000%W6=C000)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C000%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=C000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IRIX64 6.5.19f 01100601 IP30
Fingerprint SGI IRIX64 6.5.19f
Class SGI | IRIX | 6.X | general purpose
SEQ(SP=53-65%GCD=50|A0|F0|140|190%ISR=97-A1%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11NNS%O2=M5B4NW0NNT11NNS%O3=M5B4NW0NNT11NNS%O4=M5B4NW0NNT11NNS%O5=M5B4NW0NNT11NNS%O6=M5B4NNT11NNS)
WIN(W1=C000%W2=C000%W3=C000%W4=C000%W5=C000%W6=C000)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C000%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=C000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# IRIX64 6.5.22f 10070055 IP30
Fingerprint SGI IRIX64 6.5.22f
Class SGI | IRIX | 6.X | general purpose
SEQ(SP=57-C1%GCD=1-6|50|A0|F0|140|190%ISR=97-A1%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11NNS%O2=M5B4NW0NNT11NNS%O3=M5B4NW0NNT11NNS%O4=M5B4NW0NNT11NNS%O5=M5B4NW0NNT11NNS%O6=M5B4NNT11NNS)
WIN(W1=C000%W2=C000%W3=C000%W4=C000%W5=C000%W6=C000)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C000%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=C000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# SGI Octane2 running IRIX uname: IRIX64 6.5 6.5.30m 07202013 IP30
Fingerprint SGI IRIX64 6.5.30m
Class SGI | IRIX | 6.X | general purpose
SEQ(SP=ED-109%GCD=1-6%ISR=105-10F%TI=I%TS=1|2)
OPS(O1=M5B4NW6NNT11NNS%O2=M5B4NW6NNT11NNS%O3=M5B4NW6NNT11NNS%O4=M5B4NW6NNT11NNS%O5=M5B4NW6NNT11NNS%O6=M5B4NW6NNT11NNS)
WIN(W1=C000%W2=C000%W3=C000%W4=C000%W5=C000%W6=C000)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C000%O=M5B4NW6NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=C000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Sharp AR-M351N Printer
# Sharp AR-C260M copier/printer
Fingerprint Sharp AR-C260M or AR-M351N printer
Class Sharp | embedded || printer
SEQ(SP=0-5A%GCD=1-6|10001|20002|30003|40004|50005|60006%ISR=94-9E%TI=I%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=C00%W2=C00%W3=C00%W4=C00%W5=C00%W6=C00)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=C00%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=C00%S=A|O%A=O|S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=C00%S=A|O%A=O|S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=C00%S=A|O%A=O|S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A|O%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A|O%A=O|S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A|O%A=O|S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=FA-104%TG=FF%CD=Z)

# Sharp Network Printer AR-M236
Fingerprint Sharp AR-M236 printer
Class Sharp | embedded || printer
SEQ(SP=0-5%GCD=6B6C|D6D8|14244|1ADB0|2191C%ISR=8B-95%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=O%A=O|S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Sharp AR-M237 printer.
Fingerprint Sharp AR-M237 printer
Class Sharp | embedded || printer
SEQ(SP=0-5%GCD=61A8|C350|124F8|186A0|1E848%ISR=8A-94%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=2000%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# ShoteTel ShoteGear T1
Fingerprint ShoreTel ShoreGear-T1 VoIP switch
Class ShoreTel | embedded || VoIP adapter
SEQ(R=N)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=N)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Shoretel 8800 Conference phone
Fingerprint ShoreTel 8800 VoIP phone (Linux 2.4)
Class ShoreTel | Linux | 2.4.X | VoIP phone
SEQ(SP=C7-D1%GCD=1-6%ISR=C9-D3%TI=Z%CI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Siemens C2-010-I ADSL2+ modem with firmware R100B01.0B_HN_20060406
Fingerprint Siemens C2-010-I ADSL modem
Class Siemens | embedded || broadband router
SEQ(SP=F9-105%GCD=1-6%ISR=FF-109%TI=I%II=I%SS=O|S%TS=U)
OPS(O1=|M58C%O2=|M58C%O3=|M58C%O4=|M58C%O5=|M58C%O6=|M58C)
WIN(W1=3E80%W2=3E80%W3=3E80%W4=3E80%W5=3E80%W6=3E80)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3E80%O=|M58C%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS|RF%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=ARF%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=3E80%S=O%A=O|S+%F=AS|RF%O=|M58C%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=RF%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=ARF%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=RF%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=ARF%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Siemens Gigaset SE567 (local adsl router from TELUS Communications)
# Efficient Networks/Siemens Speedstream 4200
# Siemens 4200 ADSL2+ Modem / Router
# SpeedStream 4200 ADSL router
# SpeadStream 4200-series Firmware Part #:  004-D241-A0U
Fingerprint Siemens Gigaset SE567 WAP or SpeedStream 4200 ADSL modem
Class Siemens | embedded || broadband router
Class Siemens | embedded || WAP
SEQ(SP=F4-10A%GCD=1-6%ISR=EB-101%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5AC%O2=M5AC%O3=M5AC%O4=M5AC%O5=M5AC%O6=M5AC)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5AC%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# SpeedStream 4200 router from Siemens.
Fingerprint Siemens SpeedStream 4200 ADSL modem
Class Siemens | embedded || broadband router
SEQ(SP=E4-10E%GCD=1-6%ISR=DB-105%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5AC%O2=M5AC%O3=M5AC%O4=M5AC%O5=M5AC%O6=M5AC)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5AC%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# HiPath 3000 PABX
Fingerprint Siemens HiPath 3000 PBX
Class Siemens | embedded || PBX
SEQ(SP=13-1D%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%TI=I%II=I%SS=S%TS=1)
OPS(O1=M4B0NW0NNT11%O2=M4B0NW0NNT11%O3=M4B0NW0NNT11%O4=M4B0NW0NNT11%O5=M4B0NW0NNT11%O6=M4B0NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M4B0NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1E-36%TG=20|40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# AEM100 Version V3.6/6(010418)SIE
Fingerprint Siemens AEM100 remote management unit
Class Siemens | embedded || remote management
SEQ(SP=73-7D%GCD=1-6%ISR=90-9A%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=E00%W2=E00%W3=E00%W4=E00%W5=E00%W6=E00)
ECN(R=Y%DF=N%T=3C%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3C%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=Z)

# Central Telephone server HI-PATH4000
Fingerprint Siemens HiPath 4000 VoIP gateway
Class Siemens | embedded || VoIP adapter
SEQ(SP=AE-B8%GCD=1-6%ISR=B4-BE%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=60F4%W2=60F4%W3=60F4%W4=60F4%W5=60F4%W6=60F4)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=60F4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=3B-45%TG=40%CD=S)

# HiPath optiPoint 400 Standard HFA
Fingerprint Siemens HiPath optiPoint 400 VoIP phone
Class Siemens | embedded || VoIP phone
SEQ(SP=12-1C%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M200%O2=M200%O3=M200%O4=M200%O5=M200%O6=M200)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=41%TG=40%W=2000%O=M200%CC=N%Q=)
T1(R=Y%DF=N%T=41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=7E-88%TG=80%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=41%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=41%TG=40%CD=S)

# Siemens Gigaset SE551 WLAN dsl/cable router
Fingerprint Siemens Gigaset SE551 wireless broadband router
Class Siemens | embedded || WAP
SEQ(SP=0-5%GCD=68|D0|138|1A0|208%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=5000%W2=5000%W3=5000%W4=5000%W5=5000%W6=5000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=5000%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=5000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# Siemens Gigaset SE551, Firmware Version: v1.608 (Jun 13 2006 11:51:54)
Fingerprint Siemens Gigaset SE551 wireless broadband router
Class Siemens | embedded || WAP
SEQ(SP=F-1B%GCD=1-6%ISR=4B-55%TI=I|RD%II=I%SS=O%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=5000%W2=5000%W3=5000%W4=5000%W5=5000%W6=5000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=5000%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=Z)

# SINIX-D (SVR4 derivative made by Fujitsu Siemens, running on i486 hardware)
Fingerprint Siemens SINIX-D on x86
Class Siemens | SINIX || general purpose
SEQ(SP=E-18%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1C84%W2=1C84%W3=1C84%W4=1C84%W5=1C84%W6=1C84)
ECN(R=Y%DF=N%T=19-23%TG=20%W=1C84%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=134%RID=G%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# SINIX-Z (SVR4 derivative made by Fujitsu Siemens, running on i686 hardware)
Fingerprint Siemens SINIX-Z on RM400
Class Siemens | SINIX || general purpose
SEQ(SP=91-9B%GCD=1-6%ISR=9A-A4%TI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=6000%W2=6000%W3=6000%W4=6000%W5=6000%W6=6000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=6000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=6000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=134%RID=G%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Silicon Dust HDHomerun
Fingerprint Silicondust HDHomeRun set top box
Class Silicondust | embedded || media device
SEQ(SP=A3-AD%GCD=1-6%ISR=AC-B6%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5B4%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=5B4%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# Sipura SPA-1001 VoIP adapter; Software Version 2.0.10(e); Hardware Version 2.0.1(9799)
# Sipura SPA-3000 VoIP adapter
Fingerprint Sipura SPA-1001 or SPA-3000 VoIP adapter
Class Sipura | embedded || VoIP adapter
SEQ(SP=E7-107%GCD=1-6%ISR=105-111%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=3E80%W2=3E80%W3=3E80%W4=3E80%W5=3E80%W6=3E80)
ECN(R=Y%DF=N%T=F5-FF%TG=FF%W=3E80%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=F5-FF%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=F5-FF%TG=FF%W=0%S=Z%A=S%F=ARF%O=%RD=0%Q=)
T3(R=Y%DF=N%T=F5-FF%TG=FF%W=3E80%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=F5-FF%TG=FF%W=0%S=A%A=Z%F=RF%O=%RD=0%Q=)
T5(R=Y%DF=N%T=F5-FF%TG=FF%W=0%S=Z%A=S+%F=ARF%O=%RD=0%Q=)
T6(R=Y%DF=N%T=F5-FF%TG=FF%W=0%S=A%A=Z%F=RF%O=%RD=0%Q=)
T7(R=Y%DF=N%T=F5-FF%TG=FF%W=0%S=Z%A=S%F=ARF%O=%RD=0%Q=)
U1(DF=N%T=F5-FF%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=F5-FF%TG=FF%CD=S)

# LinkSys/Sipura SPA3000, software version 3.1.10(GWd), hardware version 2.0.1(1448).
Fingerprint Sipura SPA-3000 VoIP adapter
Class Sipura | embedded || VoIP adapter
SEQ(SP=103-10D%GCD=1-6%ISR=101-111%TI=RD%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=3E80%W2=3E80%W3=3E80%W4=3E80%W5=3E80%W6=3E80)
ECN(R=Y%DF=N%T=FA%TG=FF%W=3E80%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=FA%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FA%TG=FF%W=0%S=Z%A=O|S+%F=ARF%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA%TG=FF%CD=S)

# Sitecom ADSL2+ Modem/Router 54G Turbo WL-174
# ZyXEL AIR B-3000
Fingerprint Sitecom WL-174 wireless ADSL router or ZyXEL B-3000 WAP
Class Sitecom | embedded || WAP
Class ZyXEL | embedded || WAP
SEQ(R=N)
OPS(O1=M200%O2=%O3=%O4=%O5=%O6=)
WIN(W1=400%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=FE%TG=FF%W=0%O=%CC=Y%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# Sitecom 300N Wireless Router, according to the box. Sitecom wireless broadband router WL-342, according to the web config page.
Fingerprint Sitecom WL-342 WAP
Class Sitecom | embedded || WAP
SEQ(SP=0-5%GCD=64|C8|12C|190|1F4%ISR=4B-55%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=1770%W2=1770%W3=1770%W4=1770%W5=1770%W6=1770)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1770%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=3B-45%TG=40%CD=Z)

# Slingbox Classic
Fingerprint Slingbox Classic TV over IP gateway
Class Sling | embedded || media device
SEQ(SP=0-5%GCD=1F400|3E800|5DC00|7D000|9C400%ISR=9D-A7%TI=I%CI=I%II=RI%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=%O6=)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=0%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Slingbox Classic Firmware 1.0.89
Fingerprint Slingbox Classic TV over IP gateway (Firmware 1.0.89)
Class Sling | embedded || media device
SEQ(SP=0%GCD=1F400|3E800|5DC00|7D000|9C400|BB800%ISR=9D-A7%TI=I%II=RI%SS=O|S%TS=U)
OPS(O1=M5AC%O2=M578%O3=M280%O4=M5AC%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5AC%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Slingbox PRO
Fingerprint Slingbox PRO TV over IP gateway
Class Sling | embedded || media device
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=9D-A7%TI=I%CI=I%II=RI%SS=O|S%TS=U)
OPS(O1=M5B4SNN%O2=M578SNN%O3=M280%O4=M5B4SNN%O5=M218SNN%O6=M109SNN)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4SNN%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Slingbox Solo UK
# Slingbox Pro
Fingerprint Slingbox SOLO or PRO TV over IP gateway
Class Sling | embedded || media device
SEQ(SP=0-1D%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=9D-A7%TI=I%II=RI%SS=O|S%TS=U)
OPS(O1=M5B4SNN%O2=M578SNN%O3=M280%O4=M5B4SNN%O5=M218SNN%O6=M109SNN)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4SNN%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Slingbox Tuner - Latest firmware (as of 10/25/2008).
Fingerprint Slingbox Tuner TV over IP gateway
Class Sling | embedded || media device
SEQ(SP=0-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=9E-A8%TI=I%II=RI%SS=S%TS=U)
OPS(O1=M5B4SNN%O2=M578SNN%O3=M280%O4=M5B4SNN%O5=M218SNN%O6=M109SNN)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4SNN%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Slingbox Hardware Rev 1.107.2 Firmware 1.3.80
# Slingbox Tuner - Firmware 1.2.9
Fingerprint Slingbox TV over IP gateway (Firmware 1.2.9 - 1.3.80)
Class Sling | embedded || media device
SEQ(SP=0-5%GCD=1F400|3E800|5DC00|7D000|9C400%ISR=9D-A7%TI=I%CI=I%II=RI%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Slingmedia Slingbox AV Hardware 1.2.0 Firmware 1.0.1
Fingerprint Slingmedia Slingbox AV TV over IP gateway
Class Sling | embedded || media device
SEQ(SP=E-18%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=9E-A8%TI=I%II=RI%SS=O%TS=U)
OPS(O1=|M5AC%O2=|M578%O3=|M280%O4=|M5AC%O5=%O6=)
WIN(W1=0|2000%W2=0|2000%W3=0|2000%W4=0|2000%W5=0%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O|Z%A=O|S+%F=AR|AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Original (1st edition) Slingbox
Fingerprint Slingmedia Slingbox AV TV over IP gateway
Class Sling | embedded || media device
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=9E-A8%TI=I%CI=I%II=RI%SS=O%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# SMC8014WG, Hardware Version 1B, Firmware Version 4.01.21-CCR
# SMC SMC8014WG cable modem
Fingerprint SMC SMC8014WG WAP
Class SMC | embedded || broadband router
SEQ(CI=I%II=I%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# smc8014wgccr
Fingerprint SMC SMC8014WG WAP
Class SMC | embedded || broadband router
SEQ(CI=I%II=I%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# SMCWBR14S-N2 - SMC Barricade N Wireless Broadband Router
Fingerprint SMC SMCWBR14-G2 Barricade N WAP
Class SMC | embedded || broadband router
SEQ(SP=12-1C%GCD=1-6%ISR=4B-55%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=1770%W2=1770%W3=1770%W4=1770%W5=1770%W6=1770)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1770%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N|Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N|S%T=3B-45%TG=40%CD=Z)

# SMC Barricade Broadband Router (7004BR) with firmware R1.96h2
Fingerprint SMC Barricade 7004BR router
Class SMC | embedded || router
SEQ(SP=0-1D%GCD=32|64|96|C8|FA%ISR=4B-55%TI=BI%II=BI%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3%O=%CC=N%Q=U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=80%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=100%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=400%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# SMC7908A-ISP
Fingerprint SMC SMC7908A-ISP router
Class SMC | embedded || router
SEQ(SP=22-30%GCD=1-6%ISR=4B-55%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=5000%W2=5000%W3=5000%W4=5000%W5=5000%W6=5000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=5000%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=5000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# SMC Networks 8024L2 switch
Fingerprint SMC 8024L2 switch
Class SMC | embedded || switch
SEQ(SP=E-18%GCD=A|14|1E|28|32%ISR=1F-2F%TI=I%II=RI%SS=O|S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=600%W2=600%W3=600%W4=600%W5=600%W6=600)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=600%O=M5B4%CC=N%Q=U)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FA-104%TG=FF%W=80%S=A%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=100%S=A%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=400%S=A%A=S+%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=7A69%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=8000%S=A%A=S+%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=FFFF%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# SMC SMC7724M/VSW, Loader version: 0.0.6.4, Boot rom version: 0.0.6.6, Operation code version: 1.8.2.18
# SMC TigerSwitch 10/100 - SMC6750L2
Fingerprint SMC SMC6750L2 or SMC7724M/VSW switch
Class SMC | embedded || switch
SEQ(SP=8C-96%GCD=1-6%ISR=91-9B%TI=I%II=RI%SS=O%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=M5B4NW0NNT11NNLLLLLLLLLL%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# SMC TigerStack III 10/100 - 6824M Managed 24+2 Stackable Switch
Fingerprint SMC TigerStack III 6824M switch
Class SMC | embedded || switch
SEQ(SP=8C-96%GCD=1-6%ISR=92-9C%TI=I%CI=I%II=RI%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=M5B4NW0NNT11NNLLLLLLLLLL%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# SMC7008ABR Barricade 8-port Broadband Router
# Belkin F5D7230-4 router
# Belkin Wireless G Router F5D7230-4
Fingerprint Belkin F5D7230-4 WAP or SMC SMC7008ABR router
Class SMC | embedded || WAP
Class SMC | embedded || router
SEQ(SP=0-16%GCD=1-6|A|14|1E|28|32%ISR=30-3A%TI=I%II=I%SS=O%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=1770%W2=1770%W3=1770%W4=1770%W5=1770%W6=1770)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1770%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1770%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N|O%T=3B-45%TG=40%CD=Z)

# SMC 7904WBRA Wireless ADSL2+ Router
Fingerprint SMC 7904WBRA-N wireless ADSL router
Class SMC | embedded || WAP
SEQ(SP=16-30%GCD=1-6%ISR=4B-55%TI=I|RD%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=5000%W2=5000%W3=5000%W4=5000%W5=5000%W6=5000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=5000%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N|S%T=41%TG=40%CD=Z)

# SMC broadband router / WAP - model SMC2804WBRP-G ; Runtime Code Version: v2.08
Fingerprint SMC SMC2804WBRP-G wireless broadband router
Class SMC | embedded || WAP
SEQ(SP=0%GCD=1-6|A|14|1E|28|32|3C%ISR=30-3A%TI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=1770%W2=1770%W3=1770%W4=1770%W5=1770%W6=1770)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1770%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1770%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N|O|Y%T=3B-45%TG=40%CD=Z)

# Speedport W 700V, firmware version 1.22.000
# SMC, device model: SMC7904WBRA
Fingerprint SMC SMC7904WBRA wireless ADSL router or T-Home Speedport W 700V WAP
Class SMC | embedded || WAP
Class T-Home | embedded || WAP
SEQ(SP=0-1C%GCD=1-6|64|C8|12C|190|1F4%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=5000%W2=5000%W3=5000%W4=5000%W5=5000%W6=5000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=5000%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=5000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# SMC7904WBRB2 Firmware v0.08b
Fingerprint SMC SMC7904WBRB2 wireless broadband router
Class SMC | embedded || WAP
SEQ(SP=0-5%GCD=68|D0|138|1A0|208|270%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=1770%W2=1770%W3=1770%W4=1770%W5=1770%W6=1770)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1770%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1770%S=O%A=O|S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N|S%T=3B-45%TG=40%CD=Z)

# SMCWBR14-G2 EU Barricade g Wireless Broadband Router
Fingerprint SMC SMCWBR14-G2 EU Barricade g WAP
Class SMC | embedded || WAP
SEQ(SP=0-1A%GCD=1-6|B|16|21|2C|37%ISR=30-3A%TI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=1770%W2=1770%W3=1770%W4=1770%W5=1770%W6=1770)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1770%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=1770%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N|S%T=3B-45%TG=40%CD=Z)

# Aventail EX-1500 SSL VPN Appliance, Version: 8.6.1-192
Fingerprint SonicWALL Aventail EX-1500 SSL VPN appliance
Class SonicWALL | embedded || firewall
SEQ(SP=C2-CC%GCD=1-6%ISR=CA-D4%TI=Z%II=I%TS=A)
OPS(O1=M564ST11NW2%O2=M564ST11NW2%O3=M564NNT11NW2%O4=M564ST11NW2%O5=M564ST11NW2%O6=M564ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M564NNSNW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=1F-3D%TG=20|40%W=400%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=1D-30%TG=20|40%W=8000%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Sonicwall TZ 170 Unlimited (Firmware unknown)
Fingerprint SonicWALL TZ 170 Unlimited firewall (SonicOS)
Class SonicWALL | embedded || firewall
SEQ(SP=90-9E%GCD=1-6%ISR=96-A2%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Aventail EX-6000 v9.0 Firmware
Fingerprint SonicWALL Aventail EX-6000 VPN appliance
Class SonicWALL | embedded || proxy server
SEQ(SP=C6-D0%GCD=1-6%ISR=CE-D8%TI=Z%CI=Z%TS=8)
OPS(O1=M5B4ST11NW2%O2=M5B4ST11NW2%O3=M5B4NNT11NW2%O4=M5B4ST11NW2%O5=M5B4ST11NW2%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Sonicwall TZ 170 Standard - Firmware: SonicOS Standard 2.0.0.2 - ROM Version: SonicROM 2.0.0.3
Fingerprint SonicWALL TZ 170 Standard firewall (SonicOS 2.0)
Class SonicWALL | SonicOS | 2.X | firewall
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# SonicWALL PRO 2040 (SonicOS Standard 3.1)
Fingerprint SonicWALL PRO 2040 firewall (SonicOS 3.1)
Class SonicWALL | SonicOS | 3.X | firewall
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# SonicWall Pro 4060 running SonicOS Enhanced 3.2.0.3-54e
Fingerprint SonicWALL PRO 4060 firewall (SonicOS 3.2)
Class SonicWALL | SonicOS | 3.X | firewall
SEQ(SP=FF-109%GCD=1-6%ISR=109-113%II=I%TS=U)
OPS(O1=M5B4NW0%O2=M578NW0%O3=M280NW0%O4=M22CNW0%O5=M218NW0%O6=M109)
WIN(W1=5B4%W2=578%W3=280%W4=22C%W5=218%W6=109)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# TZ 170 Standard, Firmware Version: SonicOS Standard 3.1.6.3-4s
Fingerprint SonicWALL TZ 170 Standard firewall (SonicOS 3.1)
Class SonicWALL | SonicOS | 3.X | firewall
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# SonicWALL TZ 170 Standard (VPN Router) running firmware SonicOS Standard 3.1.0.11-85s  with ROM SonicROM 3.0.0.6
Fingerprint SonicWALL TZ 170 Standard firewall (SonicOS 3.1)
Class SonicWALL | SonicOS | 3.X | firewall
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=99-A3%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# TZ 180 Standard. SonicROM 4.0.1.1, SonicOS Standard 3.8.0.1-27s.
# Version 5.2 (Build 3790.srv03_sp1_rtm.050324-1477 : Service Pack 1)
Fingerprint SonicWALL TZ 180 Standard firewall (SonicOS 3.8)
Class SonicWALL | SonicOS | 3.X | firewall
SEQ(SP=13-1D%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%II=I%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# SonicOS Enhanced 4.0.0.12-64e on PRO 3060 Enhanced
Fingerprint SonicWALL PRO 3060 Enhanced firewall (SonicOS 4.0.0.12)
Class SonicWALL | SonicOS | 4.X | firewall
SEQ(SP=FF-109%GCD=1-6%ISR=106-110%TI=I%CI=RI%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M578NW0%O3=M280NW0%O4=M22CNW0%O5=M218NW0%O6=M109)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# SonicOS Enhanced 4.0.1.1-41e, SonicWALL TZ190, but I believe the OS is hardware non-specific.
Fingerprint SonicWALL TZ 190 firewall (SonicOS Enhanced 4.0)
Class SonicWALL | SonicOS | 4.X | firewall
SEQ(SP=F9-103%GCD=1-6%ISR=104-10E%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M578NW0NNT11%O3=M280NW0NNT11%O4=M22CNW0NNT11%O5=M218NW0NNT11%O6=M109NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=N)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# SonicOS Enhanced 5.2.0.1-21o
Fingerprint SonicWALL SonicOS Enhanced 5.2
Class SonicWALL | SonicOS | 5.2 | firewall
SEQ(SP=101-10B%GCD=1-6%ISR=106-110%TI=I%CI=RI%II=I%SS=S%TS=6)
OPS(O1=M5B4NW0NNT11%O2=M578NW0NNT11%O3=M280NW0NNT11%O4=M22CNW0NNT11%O5=M218NW0NNT11%O6=M109NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Model: TELE3 SP (CPU: Toshiba 3927 H2 / 133 Mhz) Firmware version: 6.6.3.0-3s
Fingerprint SonicWALL TELE3 firewall (SonicOS 6.6.3.0)
Class SonicWALL | SonicOS | 6.X | firewall
SEQ(SP=FF-109%GCD=1-6%ISR=104-10E%TI=I%CI=Z%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=1B-25|3B-45%TG=20|40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=1B-25%TG=20%W=80%S=A%A=Z%F=R%O=%RD=44BD347E%Q=)
T3(R=N)
T4(R=Y%DF=N%T=1B-25%TG=20%W=400%S=A%A=Z%F=R%O=%RD=44BD347E%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=75444779%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=8000%S=A%A=Z%F=R%O=%RD=44BD347E%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%S=A%A=Z%F=R%O=%RD=44BD347E%Q=)
U1(R=N)
IE(R=N)

# sonicwall pro 230
Fingerprint SonicWALL PRO 230 firewall (SonicOS)
Class SonicWALL | SonicOS || firewall
SEQ(SP=85-9F%GCD=1-6%ISR=97-A1%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Sonos ZonePlayer version 2.6 (build 9166130) m16: 1.0-12170 r8: 0.8-16
Fingerprint Sonos ZonePlayer audio distribution unit
Class Sonos | embedded || media device
SEQ(SP=C7-D1%GCD=1-6%ISR=CD-D7%TI=Z%II=I%TS=A)
OPS(O1=M5B4ST11NW7%O2=M5B4ST11NW7%O3=M5B4NNT11NW7%O4=M5B4ST11NW7%O5=M5B4ST11NW7%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=41%TG=40%W=16D0%O=M5B4NNSNW7%CC=N%Q=)
T1(R=Y%DF=Y%T=41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=41%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=41%TG=40%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=41%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=41%TG=40%CD=S)

# Sony Ericsson AINO  mobile phone on wlan network
Fingerprint Sony Ericsson Aino mobile phone
Class Sony Ericsson | embedded || phone
SEQ(SP=F1-FB%GCD=1-6%ISR=104-10E%TI=I%CI=RD%II=I%SS=S%TS=9)
OPS(O1=M5ACSW0NT11%O2=M5ACSW0NT11%O3=M5ACSW0NT11%O4=M5ACSW0NT11%O5=M5ACSW0NT11%O6=M5ACST11)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=8000%O=M5ACSW0LLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Sony Ericsson W910i mobile phone
# Sony Ericsson C902, Software version: R3BA035
# Sony Ericsson Z780i GSM/UMTS phone
Fingerprint Sony Ericsson C902, W910i, or Z780i mobile phone
Class Sony Ericsson | embedded || phone
SEQ(SP=F3-10F%GCD=1-6%ISR=104-112%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4SW0NT11%O2=M5B4SW0NT11%O3=M5B4SW0NT11%O4=M5B4SW0NT11%O5=M5B4SW0NT11%O6=M5B4ST11)
WIN(W1=FAF0%W2=FAF0%W3=FAF0%W4=FAF0%W5=FAF0%W6=FAF0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FAF0%O=M5B4SW0LLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Sony Ericsson G900. I believe it is running Symbian OS.
Fingerprint Sony Ericsson G900 mobile phone
Class Sony Ericsson | embedded || phone
SEQ(SP=A7-B5%GCD=1-6%ISR=AE-B8%TI=I%II=I%SS=S%TS=14)
OPS(O1=M5ACT11W0SL%O2=M5ACT11W0SL%O3=M5ACT11W0LLL%O4=M5ACT11W0SL%O5=M5ACT11W0SL%O6=M5ACT11S)
WIN(W1=BB2C%W2=BB2C%W3=BB2C%W4=BB2C%W5=BB2C%W6=BB2C)
ECN(R=Y%DF=Y%T=45%TG=80%W=BB2C%O=M5ACW0SLLL%CC=N%Q=)
T1(R=Y%DF=N|Y%T=45%TG=80%S=Z%A=S+%F=AR|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=45%TG=80%W=BB2C%S=O%A=S+%F=AS%O=M5ACT11W0SL%RD=0%Q=)
T4(R=Y%DF=N%T=45%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=45%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=45%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=45%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=45%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=45%TG=80%CD=S)

# Sony Ericsson Hazel (J20i)
Fingerprint Sony Ericsson Hazel (J10i) or Elm mobile phone
Class Sony Ericsson | embedded || phone
SEQ(SP=100-10A%GCD=1-6%ISR=107-111%TI=I%CI=RD|RI%II=I%SS=S%TS=9|A)
OPS(O1=M5ACSW1NT11%O2=M5ACSW1NT11%O3=M5ACSW1NT11%O4=M5ACSW1NT11%O5=M5ACSW1NT11%O6=M5ACST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5ACSW1LLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Sony Ericsson K850i, Version 1200-4398 R1CA037 071012 SonyEricsson
Fingerprint Sony Ericsson K850i mobile phone
Class Sony Ericsson | embedded || phone
SEQ(SP=102-10C%GCD=1-6%ISR=106-110%TI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4SW0NT11%O2=M5B4SW0NT11%O3=M5B4SW0NT11%O4=M5B4SW0NT11%O5=M5B4SW0NT11%O6=M5B4ST11)
WIN(W1=FAF0%W2=FAF0%W3=FAF0%W4=FAF0%W5=FAF0%W6=FAF0)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=FAF0%O=M5B4SW0LLL%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Sony Ericsson W715 Luxury Silver programversion: 1217-2243-R1DA029 090126
# Sony Ericsson W705
Fingerprint Sony Ericsson W705 or W715 Walkman mobile phone
Class Sony Ericsson | embedded || phone
SEQ(CI=RD%II=I)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=N)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Sony Ericsson W995
# Sony Ericsson W705 Walkman mobile phone
Fingerprint Sony Ericsson W705 or W995 Walkman mobile phone
Class Sony Ericsson | embedded || phone
SEQ(SP=101-10B%GCD=1-6%ISR=101-113%TI=I%CI=RD%II=I%SS=S%TS=A)
OPS(O1=M5ACSW0NT11%O2=M5ACSW0NT11%O3=M5ACSW0NT11%O4=M5ACSW0NT11%O5=M5ACSW0NT11%O6=M5ACST11)
WIN(W1=FAF0%W2=FAF0%W3=FAF0%W4=FAF0%W5=FAF0%W6=FAF0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FAF0%O=M5ACSW0LLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Sony Ericsson M600i Symbian OS 9.1 UIQ 3.0 firmware R9A002
Fingerprint Sony Ericsson M600i mobile phone (Symbian OS 9.1)
Class Sony Ericsson | Symbian OS | 9.X | phone
SEQ(SP=A6-B0%GCD=1-6%ISR=AB-B5%TI=I%II=I%SS=S%TS=14)
OPS(O1=|M5ACT11W0SL%O2=|M5ACT11W0SL%O3=|M5ACT11W0LLL%O4=|M5ACT11W0SL%O5=|M5ACT11W0SL%O6=|M5ACT11S)
WIN(W1=0|BB2C%W2=0|BB2C%W3=0|BB2C%W4=0|BB2C%W5=0|BB2C%W6=0|BB2C)
ECN(R=Y%DF=Y%T=40-4A%TG=80%W=BB2C%O=M5ACW0SLLL%CC=N%Q=)
T1(R=Y%DF=N|Y%T=40-4A%TG=80%S=O|Z%A=S+%F=AR|AS%RD=0%Q=)
T2(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=40-4A%TG=80%W=BB2C%S=O%A=S+%F=AS%O=M5ACT11W0SL%RD=0%Q=)
T4(R=Y%DF=N%T=40-4A%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=40-4A%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=40-4A%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=40-4A%TG=80%CD=S)

# Sony Ericsson P1i handheld. OS is Symbian OS v9.1 UIQ3
Fingerprint Sony Ericsson P1i mobile phone (Symbian OS 9.1)
Class Sony Ericsson | Symbian OS | 9.X | phone
SEQ(SP=A1-B1%GCD=1-6%ISR=A8-B2%TI=I%II=I%SS=S%TS=14)
OPS(O1=|M5ACT11W0SL%O2=|M5ACT11W0SL%O3=|M5ACT11W0LLL%O4=|M5ACT11W0SL%O5=|M5ACT11W0SL%O6=|M5ACT11S)
WIN(W1=0|BB2C%W2=0|BB2C%W3=0|BB2C%W4=0|BB2C%W5=0|BB2C%W6=0|BB2C)
ECN(R=Y%DF=N|Y%T=40-4A%TG=80%W=0|BB2C%O=|M5ACW0SLLL%CC=N%Q=)
T1(R=Y%DF=N|Y%T=40-4A%TG=80%S=O|Z%A=S+%F=AR|AS%RD=0%Q=)
T2(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N|Y%T=40-4A%TG=80%W=0|BB2C%S=O|Z%A=O|S+%F=A|AR|AS%O=|M5ACT11W0SL%RD=0%Q=)
T4(R=Y%DF=N%T=40-4A%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=40-4A%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=40-4A%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=40-4A%TG=80%CD=S)

# Sony PlayStation 2 game console
Fingerprint Sony PlayStation 2 game console
Class Sony | embedded || game console
SEQ(SP=12-40%GCD=1-6%ISR=5F-69%TI=I%CI=I%II=RI%SS=O%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=8000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=FA-104%TG=FF%W=8000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=8000%S=A+%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=8000%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=8000%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=20-3A%TG=40%CD=S)

# this is the ps2 linux kit cony released, 2.2.1(ps2-linux)
Fingerprint Sony PlayStation 2 game console test kit 2.2.1
Class Sony | embedded || game console
SEQ(SP=BA-C4%GCD=1-6%ISR=CA-D4%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4ST10NW0%O2=M578ST10NW0%O3=M280NNT10NW0%O4=M218ST10NW0%O5=M218ST10NW0%O6=M109ST10)
WIN(W1=7D78%W2=7DC8%W3=7F80%W4=7FB8%W5=7FB8%W6=7F53)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=7D78%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=7F53%S=O%A=S+%F=AS%O=M109ST10NW0%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=AO%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Sony PlayStation 3
Fingerprint Sony PlayStation 3 game console
Class Sony | embedded || game console
SEQ(SP=F7-101%GCD=1-6%ISR=FC-106%TI=RD%TS=21)
OPS(O1=M5B4NNSNW1NNT11%O2=M5B4NNSNW1NNT11%O3=M5B4NW1NNT11%O4=M5B4NNSNW1NNT11%O5=M5B4NNSNW1NNT11%O6=M5B4NNSNNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=41%TG=40%W=FFFF%O=M5B4NNSNW1%CC=N%Q=)
T1(R=Y%DF=N%T=41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=41%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=41%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NNSNW1NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=41%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Jailbroken PS3 With firmware 3.31
Fingerprint Sony PlayStation 3 game console
Class Sony | embedded || game console
SEQ(CI=RD%II=RI)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=N)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Sony PS3 Test Kit
Fingerprint Sony PlayStation 3 game console test kit
Class Sony | embedded || game console
SEQ(SP=D2-DC%GCD=1-6%ISR=DA-E4%TI=RD%II=RI%TS=0)
OPS(O1=M5B4NW0NNT01%O2=M5B4NW0NNT01%O3=M5B4NW0NNT01%O4=M5B4NW0NNT01%O5=M5B4NW0NNT01%O6=M5B4NNT01)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M5B4NW0NNT01|M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Modified Sony PSP running 3.90M33-2 custom firmware
# Playstation Portable (PSP), running a FTP server.
# Sony PSP, 5.50 GEN-D (Full), hacked version of the m33 (Dark-Alex) firmware, running PSP FTPd
Fingerprint Sony PSP game console (modified, running Custom Firmware 3.90 - 5.50)
Class Sony | embedded || game console
SEQ(SP=C9-D9%GCD=1-6%ISR=D8-E2%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Sony Blu-ray Player S370
# BluRay Player, Sony BDP-370. Calls itself "FedoraCore/2" Server in UPnP Multicast Messages... (doubt it)
Fingerprint Sony BDP-S370 Blu-ray player
Class Sony | embedded || media device
SEQ(SP=84-8E%GCD=1-6%ISR=94-9E%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0NNS%O2=M578NW0NNS%O3=M280NW0%O4=M218NW0NNS%O5=M218NW0NNS%O6=M109NNS)
WIN(W1=FAF0%W2=FAF0%W3=FAF0%W4=FAF0%W5=FAF0%W6=FAF0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FAF0%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FAF0%S=O%A=S+%F=AS%O=M109NW0NNS%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# Sony Bravia BE2 LCD TV (KDL-40X4500)
Fingerprint Sony Bravia BE2 LCD TV
Class Sony | embedded || media device
SEQ(SP=CA-D6%GCD=1-6%ISR=D6-E0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=72%TG=80%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=72%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=72%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=72%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=72%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=72%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=15B2%RUD=G)
IE(DFI=N%T=72%TG=80%CD=Z)

# Bravia KDL-32V5500 TV
Fingerprint Sony Bravia KDL-32V5500 TV
Class Sony | embedded || media device
SEQ(SP=C8-D2%GCD=1-6%ISR=D5-DF%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=Y%T=6A-74%TG=80%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=6A-74%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=6A-74%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=6A-74%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=6A-74%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=6A-74%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=856D%RUD=G)
IE(DFI=N%T=6A-74%TG=80%CD=Z)

# Sony Bravia 52" LCD-TV KDL-52W5500
Fingerprint Sony Bravia KDL-32W5500 TV
Class Sony | embedded || media device
SEQ(SP=CA-D4%GCD=4|8|C|10|14%ISR=D7-E1%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=Y%T=6D-77%TG=80%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=6D-77%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=6D-77%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=6D-77%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=6D-77%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=6D-77%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=1550%RUD=G)
IE(DFI=N%T=6D-77%TG=80%CD=Z)

# Television Sony Bravia embedded OS (Applicast enabled), port 52323: Server: RTOS/1.0 UPnP/1.0 KDL-32W5500/1.7
Fingerprint Sony Bravia LCD TV
Class Sony | embedded || media device
SEQ(SP=CD-D7%GCD=1-6%ISR=D5-DF%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4W3L%O2=M5B4W3L%O3=M5B4W3L%O4=M5B4W3L%O5=M5B4W3L%O6=M5B4)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=75-7F%TG=80%W=FFFF%O=M5B4W3L%CC=N%Q=)
T1(R=Y%DF=Y%T=75-7F%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=75-7F%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=75-7F%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=75-7F%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=75-7F%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=75-7F%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=8398%RUD=G)
IE(DFI=N%T=75-7F%TG=80%CD=Z)

# FWD-40LX2F, embedded card inside a LCD/Projector/etc. Used as a part of sonys embedded signage system called Zirius.
Fingerprint Sony FWD-40LX2F display card
Class Sony | embedded || specialized
SEQ(SP=C9-D3%GCD=1-6%ISR=D7-E1%TI=I%II=I%SS=O|S%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=N%T=73-7D%TG=80%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=73-7D%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=73-7D%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=73-7D%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=73-7D%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=73-7D%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=97F3%RUD=G)
IE(DFI=N%T=73-7D%TG=80%CD=Z)

# This is a Sony PCS-TL30 Video Conferencing Unit
Fingerprint Sony PCS-TL30 video conferencing system
Class Sony | embedded || webcam
SEQ(SP=0-5%GCD=1E848|3D090|5B8D8|7A120|98968%ISR=9C-A6%TI=I%II=I%SS=O|S%TS=U)
OPS(O1=|M5B4NW4%O2=|M578NW4%O3=|M280NW4%O4=|M5B4NW4%O5=%O6=)
WIN(W1=8052|FFFF%W2=802C|FFFF%W3=8020|FFFF%W4=8052|FFFF%W5=0%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# Source Technologies ST-9650 printer, Firmware Version: NR.APS.N370 (Probably Linux --Ed.)
Fingerprint Source Technologies ST-9650 printer
Class Source Technologies | embedded || printer
SEQ(SP=BB-CB%GCD=1-6%ISR=C6-D0%TI=Z%CI=Z%II=I%TS=A)
OPS(O1=M5B4ST11NW2%O2=M5B4ST11NW2%O3=M5B4NNT11NW2%O4=M5B4ST11NW2%O5=M5B4ST11NW2%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=FE%TG=FF%W=16D0%O=M5B4NNSNW2%CC=N%Q=)
T1(R=Y%DF=Y%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=FE%TG=FF%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW2%RD=0%Q=)
T4(R=Y%DF=Y%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# Specialix JETSTREAM 8500 RS232 Network Access Server, Version 2.2.7
Fingerprint Specialix JetStream 8500 RS232 remote access server
Class Specialix | embedded || terminal server
SEQ(SP=E-18%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=9A-A4%TI=I%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=800%W2=800%W3=800%W4=800%W5=800%W6=800)
ECN(R=Y%DF=N%T=3C%TG=40%W=800%O=M400%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=7FC%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# sphairon turbolink iad dsl modem. tarballs contains a linux 2.4.20 kernel. http://www.sphairon.com/fld3530/fld2820/e_serv_turbolink_iad_03.html
# Sphairon Turbolink IAD ADSL-Modem/VoIP-Gateway (distributed by the German ISP "Alice")
Fingerprint Sphairon Turbolink IAD DSL modem
Class Sphairon | embedded || broadband router
SEQ(SP=C9-D3%GCD=1-6%ISR=C9-D3%TI=Z%II=I%TS=7)
OPS(O1=M5B4ST11NW0%O2=M5B4ST11NW0%O3=M5B4NNT11NW0%O4=M5B4ST11NW0%O5=M5B4ST11NW0%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3D%TG=40%W=16D0%O=M5B4NNSNW0%CC=Y%Q=)
T1(R=Y%DF=Y%T=3D%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3D%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=3D%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3D%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3D%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3D%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3D%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=38-42%TG=40%CD=S)

# Star Micronics TSP100 (small thermal receipt printer)
Fingerprint Star Micronics TSP100 receipt printer
Class Star Micronics | embedded || printer
SEQ(SP=0-5%GCD=388|710|A98|E20|11A8%ISR=64-6E%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=800%W2=800%W3=800%W4=800%W5=800%W6=800)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=800%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=800%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# Stonewater Control Systems - Environmental monitoring appliance
Fingerprint Stonewater Control Systems environmental monitoring appliance
Class Stonewater Control Systems | embedded || specialized
SEQ(SP=3C-46%GCD=100|200|300|400|500%ISR=8D-97%TI=I%II=A780|A78F|A79C|A7AC|A7B8%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=|M400)
WIN(W1=1FF%W2=1FF%W3=1FF%W4=1FF%W5=1FF%W6=0|1FF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1FF%O=M400%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=28-3E%TG=40%CD=S)

# StorageTek SN3250 Router, Version 3.06 2009v
Fingerprint StorageTek SN3250 router
Class StorageTek | embedded || router
SEQ(SP=13-1D%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5B4%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Virtual Technician Module of Stratus ftServer, It runs something from RMC - Server: RMC Webserver 2.0
Fingerprint Stratus ftServer Virtual Technician Module
Class Stratus | embedded || remote management
SEQ(SP=C-16%GCD=FA7F|1F4FE|2EF7D|3E9FC|4E47B%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B0%O2=M578%O3=M280%O4=M5B0%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2000%O=M5B0%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=19-23%TG=20%CD=S)

# Sun Solaris RSC (Remote System Control) version 2.2.3
# Sun-Fire-890 RSC remote console RSC version 2.2.3
Fingerprint Sun Remote System Control (RSC) 2.2.3
Class Sun | embedded || remote management
SEQ(SP=13-1D%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=98-A2%TI=I%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=Y%T=3B-45%TG=40%CD=S)

# Sun Storage 7210 Unified Storage System
Fingerprint Sun Storage 7210 NAS device
Class Sun | embedded || storage-misc
SEQ(SP=94-9E%GCD=1-6%ISR=9F-A9%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M5B4NW5NNS%O2=NNT11M5B4NW5NNS%O3=NNT11M5B4NW5%O4=NNT11M5B4NW5NNS%O5=NNT11M5B4NW5NNS%O6=NNT11M5B4NNS)
WIN(W1=8026%W2=8017%W3=8005%W4=800E%W5=800E%W6=FFF7)
ECN(R=Y%DF=Y%T=3C%TG=40%W=8024%O=M5B4NW5NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# Sun StorageTek 6140 Array
Fingerprint Sun StorageTek 6140 NAS device
Class Sun | embedded || storage-misc
SEQ(SP=95-9F%GCD=1-6%ISR=99-A3%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Sun StorEdge 3510 FC
Fingerprint Sun StorEdge 3510 FC storage array
Class Sun | embedded || storage-misc
SEQ(SP=C-16%GCD=1-6%ISR=2B-35%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NNSLLLL%O2=M5B4NNSLLLL%O3=M5B4NNSLLLL%O4=M5B4NNSLLLL%O5=M5B4NNSLLLL%O6=M5B4NNSLLLL)
WIN(W1=5C8%W2=5C8%W3=5C8%W4=5C8%W5=5C8%W6=5C8)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5C8%O=M5B4NNSLLLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# SunOS spot 5.11 snv_101b i86pc i386 i86pc Solaris
Fingerprint Sun OpenSolaris 2008.11
Class Sun | OpenSolaris || general purpose
SEQ(SP=91-9F%GCD=1-6%ISR=A0-AA%TI=I%II=I%SS=S%TS=5)
OPS(O1=NNT11M5B4NW0NNS%O2=NNT11M5B4NW0NNS%O3=NNT11M5B4NW0%O4=NNT11M5B4NW0NNS%O5=NNT11M5B4NW0NNS%O6=NNT11M5B4NNS)
WIN(W1=C050%W2=C330%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C1E8%O=M5B4NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# OpenSolaris 2008.11
Fingerprint Sun OpenSolaris 2008.11
Class Sun | OpenSolaris || general purpose
SEQ(SP=93-9D%GCD=1-6%ISR=9F-A9%TI=I%CI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M1B30NW0NNS%O2=NNT11M1B30NW0NNS%O3=NNT11M1B30NW0%O4=NNT11M1B30NW0NNS%O5=NNT11M1B30NW0NNS%O6=NNT11M1B30NNS)
WIN(W1=C050%W2=C330%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C1E8%O=M1B30NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# OpenSolaris 08/11
Fingerprint Sun OpenSolaris 2008.11
Class Sun | OpenSolaris || general purpose
SEQ(SP=8C-9C%GCD=1-6%ISR=9E-A8%TI=I%CI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M4BENW0NNS%O2=NNT11M4BENW0NNS%O3=NNT11M4BENW0%O4=NNT11M4BENW0NNS%O5=NNT11M4BENW0NNS%O6=NNT11M4BENNS)
WIN(W1=C082%W2=C082%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C26E%O=M4BENW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS vmOpenSolaris 5.11 snv_111b i86pc i386 i86pc Solaris (VirtualBox)
Fingerprint Sun OpenSolaris 2009.06
Class Sun | OpenSolaris || general purpose
SEQ(SP=82-9E%GCD=1-6%ISR=9F-A9%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M5B4NW0NNS%O2=NNT11M5B4NW0NNS%O3=NNT11M5B4NW0%O4=NNT11M5B4NW0NNS%O5=NNT11M5B4NW0NNS%O6=NNT11M5B4NNS)
WIN(W1=C050%W2=C330%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=N)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS vmOpenSolaris 5.11 snv_111b i86pc i386 i86pc Solaris (VirtualBox)
Fingerprint Sun OpenSolaris 2009.06
Class Sun | OpenSolaris || general purpose
SEQ(SP=8D-9D%GCD=1-6%ISR=9F-A9%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M5B4NW1NNS%O2=NNT11M5B4NW1NNS%O3=NNT11M5B4NW1%O4=NNT11M5B4NW1NNS%O5=NNT11M5B4NW1NNS%O6=NNT11M5B4NNS)
WIN(W1=FBB4%W2=FC1E%W3=FA38%W4=FABE%W5=FABE%W6=FFF7)
ECN(R=Y%DF=Y%T=37-41%TG=40%W=FAF0%O=M5B4NW1NNS%CC=Y%Q=U)
T1(R=Y%DF=Y%T=37-41%TG=40%S=O%A=S+%F=AS%RD=0%Q=U)
T2(R=N)
T3(R=Y%DF=Y%T=37-41%TG=40%W=FA09%S=O%A=S+%F=AS%O=NNT11M5B4NW1NNS%RD=0%Q=U)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.11 snv_130
# Nexenta 3.0 Beta (OpenSolaris kernel, Ubuntu Hardy userland)
# SunOS 5.11 snv_134 i86pc i386 i86pc Solaris
# SunOS superfluid 5.11 NexentaOS_134e i86pc i386 i86pc Solaris, Nexenta GNU/OpenSolaris 3.0 RC2
Fingerprint Sun OpenSolaris snv_130 - snv_134
Class Sun | OpenSolaris || general purpose
SEQ(SP=93-A1%GCD=1-6%ISR=A0-AA%TI=I%CI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M5B4NW1NNS%O2=NNT11M5B4NW1NNS%O3=NNT11M5B4NW1%O4=NNT11M5B4NW1NNS%O5=NNT11M5B4NW1NNS%O6=NNT11M5B4NNS)
WIN(W1=FBB4%W2=FC1E%W3=FA38%W4=FABE%W5=FABE%W6=FFF7)
ECN(R=Y%DF=Y%T=37-41%TG=40%W=FAF0%O=M5B4NW1NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=37-41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=37-41%TG=40%W=FA09%S=O%A=S+%F=AS%O=NNT11M5B4NW1NNS%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.10 Generic_120012-14 i86pc i386 i86pc
Fingerprint Sun Solaris 10
Class Sun | Solaris | 10 | general purpose
SEQ(SP=8F-99%GCD=1-6%ISR=9F-A9%TI=I%II=I%SS=S%TS=6)
OPS(O1=NNT11M5B4NW0NNS%O2=NNT11M5B4NW0NNS%O3=NNT11M5B4NW0%O4=NNT11M5B4NW0NNS%O5=NNT11M5B4NW0NNS%O6=NNT11M5B4NNS)
WIN(W1=C050%W2=C330%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C1E8%O=M5B4NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.10 Generic_137112-02 i86pc i386 i86pc
# SunOS 5.10 Generic_120011-14 sun4u sparc SUNW,Sun-Blade-1500
Fingerprint Sun Solaris 10
Class Sun | Solaris | 10 | general purpose
SEQ(SP=8E-A2%GCD=1-6%ISR=9E-A8%TI=I%TS=7)
OPS(O1=NNT11M5B4NW0NNS%O2=NNT11M5B4NW0NNS%O3=NNT11M5B4NW0%O4=NNT11M5B4NW0NNS%O5=NNT11M5B4NW0NNS%O6=NNT11M5B4NNS)
WIN(W1=C050%W2=C330%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=5B-65%TG=80%W=C1E8%O=M5B4NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=5B-65%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=5F-69%TG=80%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=5F-69%TG=80%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=5F-69%TG=80%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=250-25A%TG=FF%IPL=70%UN=0%RIPL=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=250-25A%TG=FF%CD=S)

# SunOS 5.10 Generic_137111-01 sun4v sparc SUNW,Sun-Fire-T200
Fingerprint Sun Solaris 10
Class Sun | Solaris | 10 | general purpose
SEQ(SP=8D-D7%GCD=1-6%ISR=9F-D3%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M564NW0NNS%O2=NNT11M564NW0NNS%O3=NNT11M564NW0%O4=NNT11M564NW0NNS%O5=NNT11M564NW0NNS%O6=NNT11M564NNS)
WIN(W1=C060%W2=C060%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=C210%O=M564NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=20-3E%TG=40%W=80%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=20-3C%TG=40%W=100%S=A%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=20-35%TG=40%W=400%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=23-3F%TG=40%W=8000%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=21-32%TG=40%W=FFFF%S=A%A=S+%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=Y%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=D56A%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.10 Generic_137112-03 i86pc i386 i86pc
# SunOS 5.10 Generic_137138-09 i86pc i386 i86pc
# SunOS 5.10 Generic_127127-11 sun4u sparc SUNW,Sun-Fire-V880
Fingerprint Sun Solaris 10
Class Sun | Solaris | 10 | general purpose
SEQ(SP=90-B2%GCD=1-6%ISR=9E-C8%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M5B4NW0NNS%O2=NNT11M5B4NW0NNS%O3=NNT11M5B4NW0%O4=NNT11M5B4NW0NNS%O5=NNT11M5B4NW0NNS%O6=NNT11M5B4NNS)
WIN(W1=C050%W2=C330%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=C1E8%O=M5B4NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.10 Generic_138889-05 i86pc i386 i86pc
Fingerprint Sun Solaris 10
Class Sun | Solaris | 10 | general purpose
SEQ(SP=90-A4%GCD=1-6%ISR=9F-A9%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M2300NW0NNS%O2=NNT11M2300NW0NNS%O3=NNT11M2300NW0%O4=NNT11M2300NW0NNS%O5=NNT11M2300NW0NNS%O6=NNT11M2300NNS)
WIN(W1=C050%W2=C330%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C1E8%O=M2300NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS OUD 5.10 Generic_138889-07 i86pc i386 i86pc
Fingerprint Sun Solaris 10
Class Sun | Solaris | 10 | general purpose
SEQ(SP=FC-106%GCD=1-6%ISR=104-10E%TI=I%CI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M1D8NW0NNS%O2=NNT11M1D8NW0NNS%O3=NNT11M1D8NW0%O4=NNT11M1D8NW0NNS%O5=NNT11M1D8NW0NNS%O6=NNT11M1D8NNS)
WIN(W1=C044%W2=C044%W3=C044%W4=C044%W5=C044%W6=C0B7)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C198%O=M1D8NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.10 Generic_139555-08 sun4v sparc SUNW,SPARC-Enterprise-T5120
Fingerprint Sun Solaris 10
Class Sun | Solaris | 10 | general purpose
SEQ(SP=95-9F%GCD=1-6%ISR=9E-A8%TI=I%TS=7)
OPS(O1=NNT11M4B0NW0NNS%O2=NNT11M4B0NW0NNS%O3=NNT11M4B0NW0%O4=NNT11M4B0NW0NNS%O5=NNT11M4B0NW0NNS%O6=NNT11M4B0NNS)
WIN(W1=C050%W2=C330%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=3B%TG=40%W=C1E8%O=M4B0NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3F%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3F%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3F%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FE%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=D101%RUD=G)
IE(R=N)

# SunOS 5.10 Generic_138888-03 sun4v sparc SUNW,Sun-Blade-T6320
Fingerprint Sun Solaris 10
Class Sun | Solaris | 10 | general purpose
SEQ(SP=FA-108%GCD=1-6%ISR=F8-110%TI=I%CI=RD|RI%II=I%SS=S%TS=7)
OPS(O1=NNT11M564NW0NNS%O2=NNT11M564NW0NNS%O3=NNT11M564NW0%O4=NNT11M564NW0NNS%O5=NNT11M564NW0NNS%O6=NNT11M564NNS)
WIN(W1=C060%W2=C060%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=37-41%TG=40%W=C210%O=M564NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=37-41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=21-38%TG=40%W=80%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=25-3C%TG=40%W=100%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=29-3E%TG=40%W=400%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=1F-3D%TG=20|40%W=8000%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=28-3E%TG=40%W=FFFF%S=A%A=S%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.10 Generic_142901-07 i86pc i386 i86pc
Fingerprint Sun Solaris 10
Class Sun | Solaris | 10 | general purpose
SEQ(SP=94-9E%GCD=1-6%ISR=9F-A9%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M5B0NW0NNS%O2=NNT11M5B0NW0NNS%O3=NNT11M5B0NW0%O4=NNT11M5B0NW0NNS%O5=NNT11M5B0NW0NNS%O6=NNT11M5B0NNS)
WIN(W1=C56C%W2=C330%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=38-42%TG=40%W=C160%O=M5B0NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=38-42%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3C-46%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.10 Generic_127111-03 sun4v sparc SUNW,SPARC-Enterprise-T5220
Fingerprint Sun Solaris 10
Class Sun | Solaris | 10 | general purpose
SEQ(SP=101-10B%GCD=1-6%ISR=108-112%TI=I%TS=7)
OPS(O1=NNT11M5B4NW3NNS%O2=NNT11M5B4NW3NNS%O3=NNT11M5B4NW3%O4=NNT11M5B4NW3NNS%O5=NNT11M5B4NW3NNS%O6=NNT11M5B4NNS)
WIN(W1=80AE%W2=8017%W3=802D%W4=802F%W5=802F%W6=FFF7)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8052%O=M5B4NW3NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.10 HW3/05 Generic_118833-24 sun4u sparc SUNW,Sun-Fire-880
# SunOS 5.10 Generic_127111-03 sun4v sparc SUNW,Sun-Fire-T200
Fingerprint Sun Solaris 10 (SPARC)
Class Sun | Solaris | 10 | general purpose
SEQ(SP=F3-10B%GCD=1-6%ISR=107-111%TI=I%TS=A)
OPS(O1=NNT11M5B4NW0NNS%O2=NNT11M5B4NW0NNS%O3=NNT11M5B4NW0%O4=NNT11M5B4NW0NNS%O5=NNT11M5B4NW0NNS%O6=NNT11M5B4NNS)
WIN(W1=C050%W2=C330%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C1E8%O=M5B4NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS nj-web20 5.10 Generic_118833-24 sun4u sparc SUNW,Sun-Fire-V210
Fingerprint Sun Solaris 10 (SPARC)
Class Sun | Solaris | 10 | general purpose
SEQ(SP=8F-A3%GCD=1-6%ISR=9E-A8%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M564NW0NNS%O2=NNT11M564NW0NNS%O3=NNT11M564NW0%O4=NNT11M564NW0NNS%O5=NNT11M564NW0NNS%O6=NNT11M564NNS)
WIN(W1=C060%W2=C060%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C210%O=M564NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=23-33%TG=40%W=80%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=22-40%TG=40%W=100%S=A%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=27-3D%TG=40%W=400%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=23-3F%TG=40%W=8000%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=23-40%TG=40%W=FFFF%S=A%A=S+%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=2F22%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.10 Generic_125100-10 sun4u sparc SUNW,UltraAX-i2
Fingerprint Sun Solaris 10 (SPARC)
Class Sun | Solaris | 10 | general purpose
SEQ(SP=100-10A%GCD=1-6%ISR=103-10D%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M564NW0NNS%O2=NNT11M564NW0NNS%O3=NNT11M564NW0%O4=NNT11M564NW0NNS%O5=NNT11M564NW0NNS%O6=NNT11M564NNS)
WIN(W1=C060%W2=C060%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C210%O=M564NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=22-30%TG=40%W=80%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=22-39%TG=40%W=100%S=A%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=1F-3B%TG=20|40%W=400%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=1F-2C|30-3D%TG=20|40%W=8000%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=1F-30|34-3E%TG=20|40%W=FFFF%S=A%A=S+%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.10 Generic_125100-10 sun4v sparc SUNW,Sun-Fire-T200
Fingerprint Sun Solaris 10 (SPARC)
Class Sun | Solaris | 10 | general purpose
SEQ(SP=92-A0%GCD=1-6%ISR=9E-A8%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M5B4NW0NNS%O2=NNT11M5B4NW0NNS%O3=NNT11M5B4NW0%O4=NNT11M5B4NW0NNS%O5=NNT11M5B4NW0NNS%O6=NNT11M5B4NNS)
WIN(W1=C050%W2=C330%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C1E8%O=M5B4NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=1F-3C%TG=20|40%W=80%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=1F-36%TG=20|40%W=100%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=27-3A%TG=40%W=400%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=1F-38%TG=20|40%W=8000%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=1F-2A|2D-3C%TG=20|40%W=FFFF%S=A%A=S%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.10 Generic_127127-11 sun4u sparc SUNW,Ultra-5_10
Fingerprint Sun Solaris 10 (SPARC)
Class Sun | Solaris | 10 | general purpose
SEQ(SP=8B-95%GCD=1-6%ISR=9F-A9%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M5B4NW0NNS%O2=NNT11M5B4NW0NNS%O3=NNT11M5B4NW0%O4=NNT11M5B4NW0NNS%O5=NNT11M5B4NW0NNS%O6=NNT11M5B4NNS)
WIN(W1=C050%W2=C330%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C1E8%O=M5B4NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=370F%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS unknown 5.10 Generic_118855-15 i86pc i386 i86pc
Fingerprint Sun Solaris 10 (x86)
Class Sun | Solaris | 10 | general purpose
SEQ(SP=83-A3%GCD=1-6%ISR=9D-A7%TI=I%TS=7)
OPS(O1=NNT11M564NW0NNS%O2=NNT11M564NW0NNS%O3=NNT11M564NW0%O4=NNT11M564NW0NNS%O5=NNT11M564NW0NNS%O6=NNT11M564NNS)
WIN(W1=C060%W2=C060%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C210%O=M564NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=22-41%TG=40%W=80%S=A|O%A=O|S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=Y%T=22-40%TG=40%W=100%S=A|O%A=O|S+%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=27-3E%TG=40%W=400%S=A|O%A=O|S%F=AR%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=26-41%TG=40%W=8000%S=A|O%A=O|S%F=AR%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=Y%T=2B-3E%TG=40%W=FFFF%S=A|O%A=O|S+%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# OpenIndiana SunOS 5.11      oi_147  September 2010
# SunOS 5.11 oi_147 i86pc i386 i86pc Solaris
# Sun Blade 1000 Solaris 11
# SunOS 5.11 snv_151a i86pc i386 i86pc Solaris
# SunOS 5.11 snv_151a sun4u sparc SUNW,Sun-Blade-100 Solaris
Fingerprint Sun Solaris 11 (snv_151a) or OpenIndiana oi_147
Class Sun | Solaris | 11 | general purpose
Class OpenIndiana | OpenIndiana || general purpose
SEQ(SP=94-9E%GCD=1-6%ISR=A0-AA%TI=I%CI=I%II=I%SS=S%TS=7)
OPS(O1=ST11M5B4NW1%O2=ST11M5B4NW1%O3=NNT11M5B4NW1%O4=ST11M5B4NW1%O5=ST11M5B4NW1%O6=ST11M5B4)
WIN(W1=FBB4%W2=FC1E%W3=FA38%W4=FABE%W5=FABE%W6=FFF7)
ECN(R=Y%DF=Y%T=37-41%TG=40%W=FAF0%O=M5B4NNSNW1%CC=Y%Q=)
T1(R=Y%DF=Y%T=37-41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=37-41%TG=40%W=FA09%S=O%A=S+%F=AS%O=ST11M5B4NW1%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.5.1 Generic_103640-36 sun4m sparc SUNW,SPARCstation-10 Solaris
# SunOS 5.5.1 Generic_103640-31 sun4m sparc
Fingerprint Sun Solaris 2.5.1 (SPARC)
Class Sun | Solaris | 2.X | general purpose
SEQ(SP=8E-A2%GCD=1-6%ISR=99-A7%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=2238%W2=2648%W3=2300%W4=2398%W5=2398%W6=2332)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=2238%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=26-3A%TG=29-39%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=26-3A%TG=27-39%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=26-3A%TG=27-3A%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=26-3A%TG=26-39%W=0%S=Z%A=O|S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.5.1 Generic_103640-42 sun4m sparc SUNW,SPARCstation-20
Fingerprint Sun Solaris 2.5.1 (SPARC)
Class Sun | Solaris | 2.X | general purpose
SEQ(SP=8F-99%GCD=1-6%ISR=95-9F%TI=I%II=I%SS=S%TS=U)
OPS(O1=M564%O2=M564%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=25BC%W2=25BC%W3=2300%W4=2398%W5=2398%W6=2332)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=25BC%O=M564%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=21-34%TG=40%W=80%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=22-33%TG=40%W=100%S=A%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=21-39%TG=40%W=400%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=Y%T=1F-3D%TG=20|40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=27-40%TG=40%W=8000%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=23-3A%TG=40%W=FFFF%S=A%A=S+%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=436C%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.6 Generic_105181-15 sun4u sparc SUNW,Ultra-5_10
# SunOS 5.6 Generic_105181-33 sun4u sparc SUNW,Ultra-Enterprise
# SunOS 5.6 Generic_105182-35 i86pc i386 i86pc
# SunOS 5.6 Generic_105181-26 sun4u sparc SUNW,Ultra-1 Solaris
# SunOS 5.6 Generic_105181-31 sun4u sparc SUNW,Ultra-Enterprise
Fingerprint Sun Solaris 2.6
Class Sun | Solaris | 2.X | general purpose
SEQ(SP=8D-AB%GCD=1-6%ISR=97-AB%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11NW0M5B4%O2=NNT11NW0M578%O3=NNT11NW0M280%O4=NNT11NW0M218%O5=NNT11NW0M218%O6=NNT11M109)
WIN(W1=2798%W2=25F4%W3=2258%W4=22CC%W5=22CC%W6=2297)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=2238%O=NW0M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=23-3B%TG=20|40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=23-3B%TG=20|40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=23-3B%TG=20|40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=23-3B%TG=20|40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# 5.10 Generic_127111-03 sun4v sparc
Fingerprint Sun Solaris 5.10
Class Sun | Solaris | 5.X | general purpose
SEQ(SP=102-10C%GCD=1-6%ISR=106-110%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=NNT11M5B4NW0NNS%O2=NNT11M5B4NW0NNS%O3=NNT11M5B4NW0%O4=NNT11M5B4NW0NNS%O5=NNT11M5B4NW0NNS%O6=NNT11M5B4NNS)
WIN(W1=C050%W2=C330%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=C1E8%O=M5B4NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# Sun OS 5.7
Fingerprint Sun Solaris 7
Class Sun | Solaris | 7 | general purpose
SEQ(SP=8E-98%GCD=1-6%ISR=98-A4%TI=I%CI=RD%II=I%SS=S%TS=7)
OPS(O1=NNT11NW0NNSM564%O2=NNT11NW0NNSM564%O3=NNT11NW0M280%O4=NNT11NW0NNSM218%O5=NNT11NW0NNSM218%O6=NNT11NNSM109)
WIN(W1=2568%W2=2568%W3=2258%W4=22CC%W5=22CC%W6=2297)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=25BC%O=NW0NNSM564%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=25-3D%TG=40%W=80%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=20-3F%TG=40%W=100%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=27-3F%TG=40%W=400%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=Y%T=22-36%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=22-30%TG=40%W=8000%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=20-32%TG=40%W=FFFF%S=A%A=S%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS hostname 5.7 Generic_Patch sun4u sparc SUNW,Ultra-1 Solaris
Fingerprint Sun Solaris 7 (SPARC)
Class Sun | Solaris | 7 | general purpose
SEQ(SP=84-A0%GCD=1-6%ISR=93-A1%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11NW0NNSM5B4%O2=NNT11NW0NNSM578%O3=NNT11NW0M280%O4=NNT11NW0NNSM218%O5=NNT11NW0NNSM218%O6=NNT11NNSM109)
WIN(W1=2798%W2=25F4%W3=2258%W4=22CC%W5=22CC%W6=2297)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=2238%O=NW0NNSM5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=21-3F%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=21-3D%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=22-40%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=20-3F%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS <hostname> 5.7 Generic_106541-23 sun4u sparc SUNW,Ultra-5_10
Fingerprint Sun Solaris 7 (SPARC)
Class Sun | Solaris | 7 | general purpose
SEQ(SP=FB-105%GCD=1-6%ISR=108-112%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11|NNT11NW0NNSM5B4%O2=NNT11|NNT11NW0NNSM578%O3=NNT11|NNT11NW0M280%O4=NNT11|NNT11NW0NNSM218%O5=NNT11|NNT11NW0NNSM218%O6=NNT11|NNT11NNSM109)
WIN(W1=2798%W2=25F4%W3=2258%W4=22CC%W5=22CC%W6=2297)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=2238%O=|NW0NNSM5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=20-3D%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=24-3F%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=28-3D%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=23-3E%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.7 Generic sun4u sparc SUNW,Ultra-1
Fingerprint Sun Solaris 7 (SPARC)
Class Sun | Solaris | 7 | general purpose
SEQ(SP=EA-106%GCD=1-6%ISR=100-110%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11NW0NNSM564%O2=NNT11NW0NNSM564%O3=NNT11NW0M280%O4=NNT11NW0NNSM218%O5=NNT11NW0NNSM218%O6=NNT11NNSM109)
WIN(W1=2568%W2=2568%W3=2258%W4=22CC%W5=22CC%W6=2297)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=25BC%O=NW0NNSM564%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=22-2C|2E-3F%TG=40%W=80%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=2B-3A%TG=40%W=100%S=A%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=25-40%TG=40%W=400%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=N%T=34-3E%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=24-3F%TG=40%W=8000%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=21-38%TG=40%W=FFFF%S=A%A=S+%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.8 Generic_108528-11 sun4u sparc SUNW,Ultra-5_10 Solaris
# SunOS unknown 5.8 Generic_108528-13 sun4u sparc SUNW,Sun-Blade-100
Fingerprint Sun Solaris 8 (SPARC)
Class Sun | Solaris | 8 | general purpose
SEQ(SP=8D-9F%GCD=1-6%ISR=A0-AA%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11NW0NNSM5B4%O2=NNT11NW0NNSM5B4%O3=NNT11NW0M5B4%O4=NNT11NW0NNSM5B4%O5=NNT11NW0NNSM5B4%O6=NNT11NNSM5B4)
WIN(W1=6028%W2=6198%W3=6220%W4=6034%W5=6034%W6=60DA)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=60F4%O=NW0NNSM5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS  5.8 Generic_108528-19 sun4u sparc SUNW,Ultra-5_10
Fingerprint Sun Solaris 8 (SPARC)
Class Sun | Solaris | 8 | general purpose
SEQ(SP=DF-E9%GCD=1-6%ISR=108-112%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11NW0NNSM5B4%O2=NNT11NW0NNSM5B4%O3=NNT11NW0M5B4%O4=NNT11NW0NNSM5B4%O5=NNT11NW0NNSM5B4%O6=NNT11NNSM5B4)
WIN(W1=6028%W2=6198%W3=6220%W4=6034%W5=6034%W6=60DA)
ECN(R=Y%DF=Y%T=3A-44%TG=40%W=60F4%O=NW0NNSM5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3A-44%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3A-44%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=38-42%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=38-42%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=38-42%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FE%TG=FF%CD=S)

# Solaris 8: SunOS 5.8 Generic_117350-39
Fingerprint Sun Solaris 8 (SPARC)
Class Sun | Solaris | 8 | general purpose
SEQ(SP=F8-102%GCD=1-6%ISR=F7-10D%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11NW0NNSM5B4%O2=NNT11NW0NNSM5B4%O3=NNT11NW0M5B4%O4=NNT11NW0NNSM5B4%O5=NNT11NW0NNSM5B4%O6=NNT11NNSM5B4)
WIN(W1=6028%W2=6198%W3=6220%W4=6034%W5=6034%W6=60DA)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=60F4%O=NW0NNSM5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.8 Generic_108528-15 sun4u sparc SUNW,Ultra-250
# SunOS 5.8 Generic_108529-01 i86pc i386 i86pc (on vmware)
Fingerprint Sun Solaris 8 (SPARC)
Class Sun | Solaris | 8 | general purpose
SEQ(SP=92-A6%GCD=1-6%ISR=A2-AC%TI=I%II=I%SS=S%TS=8)
OPS(O1=NNT11NW0NNSM5B4%O2=NNT11NW0NNSM5B4%O3=NNT11NW0M5B4%O4=NNT11NW0NNSM5B4%O5=NNT11NW0NNSM5B4%O6=NNT11NNSM5B4)
WIN(W1=6028%W2=6198%W3=6220%W4=6034%W5=6034%W6=60DA)
ECN(R=Y%DF=Y%T=37-45%TG=40%W=60F4%O=NW0NNSM5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=37-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.8 Generic_108528-29 sun4u sparc SUNW,Sun-Fire-280R
# SunOS 5.8 Generic_117350-39 sun4u sparc SUNW,Sun-Fire-480R
Fingerprint Sun Solaris 8 (SPARC)
Class Sun | Solaris | 8 | general purpose
SEQ(SP=92-160%GCD=1-6%ISR=98-140%TI=I%II=I%SS=S%TS=7|9)
OPS(O1=NNT11|NNT11NW0NNSM5B4%O2=NNT11|NNT11NW0NNSM5B4%O3=NNT11NW0M5B4%O4=NNT11|NNT11NW0NNSM5B4%O5=NNT11NW0NNSM5B4%O6=NNT11NNSM5B4)
WIN(W1=6028%W2=6198%W3=6220%W4=6034%W5=6034%W6=60DA)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=60F4%O=NW0NNSM5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.8 Generic_117350-20 sun4u sparc SUNW,Sun-Fire-V440
Fingerprint Sun Solaris 8 (SPARC)
Class Sun | Solaris | 8 | general purpose
SEQ(SP=96-A6%GCD=1-6%ISR=A1-AB%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11NW1NNSM5B4%O2=NNT11NW1NNSM5B4%O3=NNT11NW1M5B4%O4=NNT11NW1NNSM5B4%O5=NNT11NW1NNSM5B4%O6=NNT11NNSM5B4)
WIN(W1=8218%W2=8220%W3=80CA%W4=80F4%W5=80F4%W6=FFF7)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=8052%O=NW1NNSM5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# SunOS 5.8 Generic_117350-45 sun4u sparc SUNW,UltraAX-i2
# SunOS 5.8 Generic_117350-46 sun4u sparc SUNW,Ultra-4
Fingerprint Sun Solaris 8 (SPARC)
Class Sun | Solaris | 8 | general purpose
SEQ(SP=FA-104%GCD=1-6%ISR=100-114%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11NW0NNSM5B4%O2=NNT11NW0NNSM5B4%O3=NNT11NW0M5B4%O4=NNT11NW0NNSM5B4%O5=NNT11NW0NNSM5B4%O6=NNT11NNSM5B4)
WIN(W1=6028%W2=6198%W3=6220%W4=6034%W5=6034%W6=60DA)
ECN(R=Y%DF=Y%T=3C%TG=40%W=60F4%O=NW0NNSM5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.8 Generic_117350-24 sun4u sparc SUNW,Sun-Fire-880
# SunOS 5.8 Generic_117350-13 sun4u sparc SUNW,Sun-Blade-1000
Fingerprint Sun Solaris 8 (SPARC)
Class Sun | Solaris | 8 | general purpose
SEQ(SP=95-AF%GCD=1-6%ISR=9D-AB%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11NW0NNSM5B4%O2=NNT11NW0NNSM5B4%O3=NNT11NW0M5B4%O4=NNT11NW0NNSM5B4%O5=NNT11NW0NNSM5B4%O6=NNT11NNSM5B4)
WIN(W1=6028%W2=6198%W3=6220%W4=6034%W5=6034%W6=60DA)
ECN(R=Y%DF=Y%T=3C%TG=40%W=60F4%O=NW0NNSM5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.8 Generic_117350-33 sun4u sparc SUNW,Sun-Blade-1000
# SunOS 5.8 Generic_117350-39 sun4u sparc SUNW,Ultra-5_10
Fingerprint Sun Solaris 8 (SPARC)
Class Sun | Solaris | 8 | general purpose
SEQ(SP=89-9F%GCD=1-6%ISR=9E-A8%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11NW0NNSM5B4%O2=NNT11NW0NNSM5B4%O3=NNT11NW0M5B4%O4=NNT11NW0NNSM5B4%O5=NNT11NW0NNSM5B4%O6=NNT11NNSM5B4)
WIN(W1=6028%W2=6198%W3=6220%W4=6034%W5=6034%W6=60DA)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=60F4%O=NW0NNSM5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS  5.8 Generic_117350-39 sun4u sparc SUNW,Sun-Fire-V210
Fingerprint Sun Solaris 8 (SPARC)
Class Sun | Solaris | 8 | general purpose
SEQ(SP=91-A1%GCD=1-6%ISR=9E-A8%TI=I%TS=7)
OPS(O1=NNT11NW0NNSM5B4%O2=NNT11NW0NNSM5B4%O3=NNT11NW0M5B4%O4=NNT11NW0NNSM5B4%O5=NNT11NW0NNSM5B4%O6=NNT11NNSM5B4)
WIN(W1=6028%W2=6198%W3=6220%W4=6034%W5=6034%W6=60DA)
ECN(R=Y%DF=Y%T=5B-65%TG=80%W=60F4%O=NW0NNSM5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=5B-65%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=5F-69%TG=80%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=5F-69%TG=80%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=5F-69%TG=80%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=250-25A%TG=FF%IPL=70%UN=0%RIPL=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=250-25A%TG=FF%CD=S)

# SunOS 5.8 Generic_108528-25 sun4u sparc SUNW,Ultra-80
Fingerprint Sun Solaris 8 (SPARC)
Class Sun | Solaris | 8 | general purpose
SEQ(SP=A0-AC%GCD=1-6%ISR=A6-B7%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11NW1NNSM5AC%O2=NNT11NW1NNSM5AC%O3=NNT11NW1M5AC%O4=NNT11NW1NNSM5AC%O5=NNT11NW1NNSM5AC%O6=NNT11NNSM5AC)
WIN(W1=8160%W2=8220%W3=80CA%W4=80F4%W5=80F4%W6=FFF7)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8274%O=NW1NNSM5AC%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.8 Generic_108528-29 sun4u sparc SUNW,Ultra-60
Fingerprint Sun Solaris 8 (SPARC)
Class Sun | Solaris | 8 | general purpose
SEQ(SP=93-E7%GCD=1-6%ISR=A5-C9%TI=I%TS=7)
OPS(O1=NNT11NW1NNSM5B4%O2=NNT11NW1NNSM5B4%O3=NNT11NW1M5B4%O4=NNT11NW1NNSM5B4%O5=NNT11NW1NNSM5B4%O6=NNT11NNSM5B4)
WIN(W1=8218%W2=8220%W3=80CA%W4=80F4%W5=80F4%W6=FFF7)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8052%O=NW1NNSM5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.8 Generic_117350-45 sun4u sparc SUNW,Sun-Fire-480R
# SunOS 5.8 Generic_117350-46 sun4u sparc SUNW,Sun-Fire-15000
Fingerprint Sun Solaris 8 (SPARC)
Class Sun | Solaris | 8 | general purpose
SEQ(SP=8A-9F%GCD=1-6%ISR=9E-A8%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11NW0NNSM5B4%O2=NNT11NW0NNSM5B4%O3=NNT11NW0M5B4%O4=NNT11NW0NNSM5B4%O5=NNT11NW0NNSM5B4%O6=NNT11NNSM5B4)
WIN(W1=8218%W2=8220%W3=8204%W4=80F4%W5=80F4%W6=807A)
ECN(R=Y%DF=Y%T=3C%TG=40%W=832C%O=NW0NNSM5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.8 Generic_117350-61 sun4u sparc SUNW,Ultra-1
Fingerprint Sun Solaris 8 (SPARC)
Class Sun | Solaris | 8 | general purpose
SEQ(SP=8C-A2%GCD=1-6%ISR=9F-A9%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11NW0NNSM5B4%O2=NNT11NW0NNSM5B4%O3=NNT11NW0M5B4%O4=NNT11NW0NNSM5B4%O5=NNT11NW0NNSM5B4%O6=NNT11NNSM5B4)
WIN(W1=6028%W2=6198%W3=6220%W4=6034%W5=6034%W6=60DA)
ECN(R=Y%DF=Y%T=3C%TG=40%W=60F4%O=NW0NNSM5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=N)
T6(R=N)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.8 Generic_108529-11 i86pc i386 i86pc Solaris
Fingerprint Sun Solaris 8 (x86)
Class Sun | Solaris | 8 | general purpose
SEQ(SP=8A-9E%GCD=1-6%ISR=9F-A9%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11NW1NNSM5B4%O2=NNT11NW1NNSM5B4%O3=NNT11NW1M5B4%O4=NNT11NW1NNSM5B4%O5=NNT11NW1NNSM5B4%O6=NNT11NNSM5B4)
WIN(W1=8218%W2=8220%W3=80CA%W4=80F4%W5=80F4%W6=FFF7)
ECN(R=Y%DF=Y%T=37-45%TG=40%W=8052%O=NW1NNSM5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=37-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.9 Generic_118559-39 i86pc i386 i86pc
Fingerprint Sun Solaris 9
Class Sun | Solaris | 9 | general purpose
SEQ(SP=FF-109%GCD=1-6%ISR=101-10B%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M5B4NW1NNS%O2=NNT11M5B4NW1NNS%O3=NNT11M5B4NW1%O4=NNT11M5B4NW1NNS%O5=NNT11M5B4NW1NNS%O6=NNT11M5B4NNS)
WIN(W1=8140%W2=8220%W3=80CA%W4=80F4%W5=80F4%W6=FFF7)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=825A%O=M5B4NW1NNS%CC=Y%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# SunOS 5.9 Generic_122300-36 sun4u sparc SUNW,Sun-Fire
Fingerprint Sun Solaris 9
Class Sun | Solaris | 9 | general purpose
SEQ(SP=83-A9%GCD=1-6%ISR=A2-AC%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M5B4NW0NNS%O2=NNT11M5B4NW0NNS%O3=NNT11M5B4NW0%O4=NNT11M5B4NW0NNS%O5=NNT11M5B4NW0NNS%O6=NNT11M5B4NNS)
WIN(W1=8218%W2=8220%W3=8204%W4=80F4%W5=80F4%W6=807A)
ECN(R=Y%DF=Y%T=38-42%TG=40%W=832C%O=M5B4NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=38-42%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=41%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=41%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=100%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=100%TG=FF%CD=S)

# SunOS 5.9 Generic_118558-34 sun4u sparc SUNW,Sun-Blade-100
Fingerprint Sun Solaris 9
Class Sun | Solaris | 9 | general purpose
SEQ(SP=7B-A5%GCD=1-6%ISR=A1-AB%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M5B4NW0NNS%O2=NNT11M5B4NW0NNS%O3=NNT11M5B4NW0%O4=NNT11M5B4NW0NNS%O5=NNT11M5B4NW0NNS%O6=NNT11M5B4NNS)
WIN(W1=C050%W2=C330%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=37-41%TG=40%W=C1E8%O=M5B4NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=37-41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=N)
T6(R=N)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.9 Generic_118558-28 sun4u sparc SUNW,Sun-Blade-1500
Fingerprint Sun Solaris 9 (SPARC)
Class Sun | Solaris | 9 | general purpose
SEQ(SP=FC-106%GCD=1-6%ISR=FD-113%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M5B4NW0NNS%O2=NNT11M5B4NW0NNS%O3=NNT11M5B4NW0%O4=NNT11M5B4NW0NNS%O5=NNT11M5B4NW0NNS%O6=NNT11M5B4NNS)
WIN(W1=C050%W2=C330%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=C1E8%O=M5B4NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=1B-25|3B-45%TG=20|40%W=80%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=1B-25|3B-45%TG=20|40%W=100%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=1B-25|3B-45%TG=20|40%W=400%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=1B-25|3B-45%TG=20|40%W=8000%S=A%A=S%F=AR%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25|3B-45%TG=20|40%W=FFFF%S=A%A=S%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(R=N)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.9 Generic_112234-05 i86pc i386 i86pc Solaris
Fingerprint Sun Solaris 9 (x86)
Class Sun | Solaris | 9 | general purpose
SEQ(SP=8A-A2%GCD=1-6%ISR=A1-AB%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M5B4NW1NNS%O2=NNT11M5B4NW1NNS%O3=NNT11M5B4NW1%O4=NNT11M5B4NW1NNS%O5=NNT11M5B4NW1NNS%O6=NNT11M5B4NNS)
WIN(W1=8218%W2=8220%W3=80CA%W4=80F4%W5=80F4%W6=FFF7)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=8052%O=M5B4NW1NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.9 Generic_118559-11 i86pc i386 i86pc
# solaris 10 x86
Fingerprint Sun Solaris 9 or 10
Class Sun | Solaris | 9 | general purpose
SEQ(SP=92-9C%GCD=1-6%ISR=9D-A7%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M5B4NW1NNS%O2=NNT11M5B4NW1NNS%O3=NNT11M5B4NW1%O4=NNT11M5B4NW1NNS%O5=NNT11M5B4NW1NNS%O6=NNT11M5B4NNS)
WIN(W1=8218%W2=8220%W3=80CA%W4=80F4%W5=80F4%W6=FFF7)
ECN(R=Y%DF=Y%T=3C%TG=40%W=8052%O=M5B4NW1NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.9 Generic_118558-10 sun4u sparc SUNW,Sun-Fire-15000
# Solaris 10; uname: SunOS 5.10 Generic_118855-33 i86pc i386 i86pc
# SunOS 5.11 snv_64a sun4u sparc SUNW,Sun-Blade-1000
Fingerprint Sun Solaris 9 or 10
Class Sun | Solaris | 9 | general purpose
Class Sun | Solaris | 10 | general purpose
SEQ(SP=90-A4%GCD=1-6%ISR=9F-A9%TI=I%II=I%SS=O%TS=7)
OPS(O1=NNT11M5B4NW0NNS%O2=NNT11M5B4NW0NNS%O3=NNT11M5B4NW0%O4=NNT11M5B4NW0NNS%O5=NNT11M5B4NW0NNS%O6=NNT11M5B4NNS)
WIN(W1=C050%W2=C330%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=3C%TG=40%W=C1E8%O=M5B4NW0NNS%CC=N|Y%Q=)
T1(R=Y%DF=Y%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.9 Generic_118558-39 sun4u sparc SUNW,Sun-Fire-V215
# SunOS 5.10 Generic_118833-24 sun4u sparc SUNW,Sun-Fire-V210
# SunOS 5.9 Generic_122300-10 sun4u sparc SUNW,A70
# SunOS 5.9 Generic_112233-12 sun4u sparc SUNW,Sun-Fire-280R
# Solaris 10; uname: SunOS 5.10 Generic_118822-25 sun4u sparc SUNW,Sun-Blade-1000
# SunOS 5.10 Generic sun4u sparc SUNW,Sun-Blade-1500
# SunOS 5.10 Generic_118833-18 sun4u sparc SUNW,Sun-Fire-280R
# SunOS 5.9 Generic_118558-30 sun4u sparc SUNW,Sun-Fire-V440
# SunOS 5.10 Generic_125100-10 sun4u sparc SUNW,Sun-Fire-280R
Fingerprint Sun Solaris 9 or 10 (SPARC)
Class Sun | Solaris | 9 | general purpose
Class Sun | Solaris | 10 | general purpose
SEQ(SP=F3-10B%GCD=1-6%ISR=101-10F%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M5B4NW0NNS%O2=NNT11M5B4NW0NNS%O3=NNT11M5B4NW0%O4=NNT11M5B4NW0NNS%O5=NNT11M5B4NW0NNS%O6=NNT11M5B4NNS)
WIN(W1=C050%W2=C330%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=C1E8%O=M5B4NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 5.10 Generic_127112-05 i86pc i386 i86pc
# Solaris 10 on UltraSPARC T1
# SunOS 5.9 Generic_122300-03 sun4us sparc FJSV,GPUZC-M
# SunOS 5.10 Generic_125101-10 i86pc i386 i86pc
# OpenSolaris 2009.06 snv_111b X86, SunOS 5.11 snv_111b i86pc i386 i86pc
# Ultra 10 uni-processor
# SunOS sparc10 5.10 Generic_118822-30 sun4u sparc SUNW,Ultra-5_10 Solaris
# Solaris 10 x86
# OpenSolaris (aka Solaris Nevada)
# SunOS 5.10 Generic_142910-17 i86pc i386 i86pc
Fingerprint Sun Solaris 9 or 10, or OpenSolaris 2009.06 snv_111b
Class Sun | Solaris | 9 | general purpose
Class Sun | Solaris | 10 | general purpose
Class Sun | OpenSolaris || general purpose
SEQ(SP=8C-D4%GCD=1-6%ISR=9E-D2%TI=I%II=I%SS=S%TS=7)
OPS(O1=NNT11M5B4NW0NNS%O2=NNT11M5B4NW0NNS%O3=NNT11M5B4NW0%O4=NNT11M5B4NW0NNS%O5=NNT11M5B4NW0NNS%O6=NNT11M5B4NNS)
WIN(W1=C050%W2=C330%W3=C1CC%W4=C068%W5=C068%W6=C0B7)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=C1E8%O=M5B4NW0NNS%CC=Y%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=Y%T=FA-104%TG=FF%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=Y%T=FA-104%TG=FF%CD=S)

# SunOS 4.1.3 sun4m on SuperSPARC
Fingerprint Sun SunOS 4.1.3 (SPARC)
Class Sun | SunOS | 4.X | general purpose
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3C%TG=40%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3C%TG=40%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# symantec firewall appliance 100, Firmware V1 Rel 62
# Symantec Firewall/VPN 200, Firmware-Version V1 Rel 4I
Fingerprint Symantec Firewall/VPN 100 or 200
Class Symantec | embedded || firewall
SEQ(SP=1F-43%GCD=1000|2000|3000|4000|5000%ISR=85-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4T11NN%O2=M5B4%O3=M5B4T11NN%O4=M5B4T11NN%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3C%TG=40%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=16D0%S=O%A=S+%F=AS%O=M5B4T11NN%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=70%UN=5DC%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3C%TG=40%CD=Z)

# Symantec Security Gateway 5620 Firewall
Fingerprint Symantec Security Gateway 5620 firewall
Class Symantec | embedded || firewall
SEQ(SP=FF-109%GCD=1-6%ISR=FC-106%TI=Z%TS=U)
OPS(O1=M5B4NNSNW0%O2=M5B4NNSNW0%O3=M5B4NW0%O4=M5B4NNSNW0%O5=M5B4NNSNW0%O6=M5B4NNS)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=1A-24%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1A-24%TG=20%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1A-24%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Symantec VelociRaptor 1.5
Fingerprint Symantec VelociRaptor 1.5 firewall
Class Symantec | embedded || firewall
SEQ(SP=FE-10A%GCD=1-6%ISR=106-110%TI=I%TS=U)
OPS(O1=M5B4NNSNW0%O2=M578NNSNW0%O3=M280NW0%O4=M218NNSNW0%O5=M218NNSNW0%O6=M109NNS)
WIN(W1=7D78%W2=7DC8%W3=7F80%W4=7FB8%W5=7FB8%W6=7F53)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=7D78%O=M5B4NNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=1A-24%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1A-24%TG=20%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1A-24%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Nokia Symbian^3
Fingerprint Symbian^3
Class Symbian OS | Symbian OS | 3 | phone
SEQ(SP=A7-B1%GCD=1-6%ISR=B2-BC%TI=I%CI=I%II=I%SS=S%TS=A)
OPS(O1=M5B4NNT11NW2NNS%O2=M5B4NNT11NW2NNS%O3=M5B4NNT11NW2%O4=M5B4NNT11NW2NNS%O5=M5B4NNT11NW2NNS%O6=M5B4NNT11NNS)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FAF0)
ECN(R=Y%DF=N%T=40-4A%TG=80%W=FFFF%O=M5B4NW2NNS%CC=N%Q=)
T1(R=Y%DF=N%T=40-4A%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=40-4A%TG=80%W=FFFF%S=O%A=S+%F=AS%O=M5B4NNT11NW2NNS%RD=0%Q=)
T4(R=Y%DF=N%T=40-4A%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=40-4A%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=40-4A%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=40-4A%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=40-4A%TG=80%CD=S)

# Symbol WAP, firmware version 04.00-25 Model AP-2411
Fingerprint Symbol AP-2411 switch
Class Symbol | embedded || switch
SEQ(SP=0-5%GCD=64|C8|12C|190|1F4%ISR=4B-55%TI=RD%TS=U)
OPS(O1=|M5B4%O2=|M5B4%O3=|M5B4%O4=|M5B4%O5=|M5B4%O6=|M5B4)
WIN(W1=1|16D0%W2=3F|16D0%W3=4|16D0%W4=4|16D0%W5=10|16D0%W6=200|16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3%O=%CC=N%Q=U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O|Z%A=O|S+%F=AR|AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=80%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=100%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=400%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Symbol AP-3021 firmware 04.02-19
Fingerprint Symbol AP-3021 switch
Class Symbol | embedded || switch
SEQ(SP=0-5%GCD=64|C8|12C|190|1F4%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=|M5B4%O2=|M5B4%O3=|M5B4%O4=|M5B4%O5=|M5B4%O6=|M5B4)
WIN(W1=1|16D0%W2=3F|16D0%W3=4|16D0%W4=4|16D0%W5=10|16D0%W6=200|16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3%O=%CC=N%Q=U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O|Z%A=S+%F=AR|AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=80%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=100%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=400%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Symbol ES3000 24-port ethernet PoE switch v1.0.0.0-012R / Apr 26 2004 11:44:48
Fingerprint Symbol ES3000 switch
Class Symbol | embedded || switch
SEQ(SP=0-5%GCD=388|710|A98|E20|11A8%ISR=64-6E%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M218%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=2400%W2=2400%W3=2400%W4=2400%W5=2400%W6=2400)
ECN(R=Y%DF=N%T=3C%TG=40%W=2400%O=M578%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=2400%S=O%A=O%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Symbol Spectrum24 4131 Access Point
# Model AP-4131; AP firmware: 03.70-72; RF firmware: F3.70-32
Fingerprint Symbol Spectrum24 4131 Access Point
Class Symbol | embedded || WAP
SEQ(SP=B-15%GCD=32|64|96|C8|FA|12C%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=|M514%O2=|M514%O3=|M514%O4=|M514%O5=|M514%O6=|M514)
WIN(W1=1|16D0%W2=3F|16D0%W3=4|16D0%W4=4|16D0%W5=10|16D0%W6=200|16D0)
ECN(R=Y%DF=N%T=41%TG=40%W=3%O=%CC=N%Q=U)
T1(R=Y%DF=N%T=41%TG=40%S=O|Z%A=S+%F=AR|AS%RD=0%Q=)
T2(R=Y%DF=N%T=41%TG=40%W=80%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=41%TG=40%W=100%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=41%TG=40%W=400%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=41%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=41%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=41%TG=40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=41%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=41%TG=40%CD=S)

# Symbol WS500 Wireless Switch
Fingerprint Symbol WS500 wireless switch
Class Symbol | embedded || WAP
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4470%W2=41A0%W3=4100%W4=4000%W5=40E8%W6=402E)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4470%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=402E%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Symbol WS5000 Wireless Switch
# Software 1.4.3.0-012R, firmware 2.2 (7/9/02)
Fingerprint Symbol WS5000 wireless switch
Class Symbol | embedded || WAP
SEQ(SP=5-15%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=96-A0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4204%W2=4204%W3=4100%W4=4000%W5=40E8%W6=402E)
ECN(R=Y%DF=N%T=3D-47%TG=40%W=4204%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3D-47%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3D-47%TG=40%W=402E%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3D-47%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3D-47%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3D-47%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3D-47%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FC-106%TG=FF%IPL=38%UN=0%RIPL=15C%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FC-106%TG=FF%CD=S)

# Symbol WS5000 Wireless Switch
Fingerprint Symbol WS5000 wireless switch
Class Symbol | embedded || WAP
SEQ(SP=0-15%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=96-A0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=4470%W2=41A0%W3=4100%W4=4000%W5=40E8%W6=402E)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4470%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Microsoft Windows CE .NET 4.20 running on a Symbol MC9060-G (XScale PXA255 400 MHz)
# This is some sort of specialized mobile computer for data entry, etc.
Fingerprint Symbol MC9060-G mobile computer (runs Microsoft Windows CE .NET 4.20)
Class Symbol | Windows | PocketPC/CE | specialized
SEQ(SP=82-8C%GCD=1-6%ISR=95-9F%TI=I%II=I%SS=S%TS=0)
OPS(O1=M514NW0NNT00NNS%O2=M514NW0NNT00NNS%O3=M514NW0NNT00%O4=M514NW0NNT00NNS%O5=M514NW0NNT00NNS%O6=M514NNT00NNS)
WIN(W1=8000%W2=8000%W3=8000%W4=8000%W5=8000%W6=8000)
ECN(R=Y%DF=Y%T=7C-86%TG=80%W=8000%O=M514NW0NNS%CC=N%Q=)
T1(R=Y%DF=Y%T=7C-86%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=7C-86%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=7C-86%TG=80%W=8000%S=O%A=S+%F=AS%O=M514NW0NNT00NNS%RD=0%Q=)
T4(R=Y%DF=N%T=7C-86%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7C-86%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7C-86%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7C-86%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7C-86%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=7C-86%TG=80%CD=Z)

# Linux DiskStation 2.4.22-uc0 #375 Thu Jul 20 21:03:01 CST 2006 ppc unknown
# Linksys NSLU2 FW:V2.3R63-uNSLUng-6.8-beta (Kernel 2.4.22, Busybox 1.5.0)
Fingerprint Embedded Linux 2.4.22 (Linksys NSLU2 NAS device or Synology DS-106j NAS server)
Class Synology | Linux | 2.4.X | storage-misc
SEQ(SP=BA-D0%GCD=1-6%ISR=C8-D2%TI=Z%II=I%TS=7)
OPS(O1=M400CST11NW0%O2=M400CST11NW0%O3=M400CNNT11NW0%O4=M400CST11NW0%O5=M400CST11NW0%O6=M400CST11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=400C%O=M400CNNSNW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M400CST11NW0%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# T-Home Speedport W 700V WAP
# T-Com Speedport w700V Router,ADSL-Modem,ADSL2-Modem,WAP
Fingerprint T-Home Speedport W 700V WAP
Class T-Home | embedded || WAP
SEQ(SP=0-5%GCD=68|6C|D0|D8|138|144|1A0|1B0|208|21C%ISR=4B-55%TI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=5000%W2=5000%W3=5000%W4=5000%W5=5000%W6=5000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=5000%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=5000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N|O|S|Y%T=3B-45%TG=40%CD=Z)

# Arcadyan Router W700V (Deutsche Telekom)
Fingerprint T-Home Speedport W 700V WAP
Class T-Home | embedded || WAP
SEQ(SP=18-22%GCD=1-6%ISR=4B-55%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=5000%W2=5000%W3=5000%W4=5000%W5=5000%W6=5000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=5000%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N|S%T=3B-45%TG=40%CD=Z)

# Tahoe 8216 - Remote Power Management System. http://www.tahoe.pl/tahoe_8216.php
Fingerprint Tahoe 8216 power management system
Class Tahoe | embedded || power-device
SEQ(SP=9F-E9%GCD=3|6|9|C|F%ISR=A7-D3%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M240%O2=M240%O3=M240%O4=M240%O5=M218%O6=M109)
WIN(W1=C00%W2=C00%W3=C00%W4=C00%W5=C00%W6=C00)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=C00%O=M240%CC=N%Q=U)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=C00%S=O%A=S+%F=ASF%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=150%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=Z)

# Tandberg TT1222 satellite receiver
Fingerprint Tandberg TT 1122 video receiver
Class Tandberg | embedded || media device
SEQ(SP=0-19%GCD=1-6|58|B0|108|160|1B8%ISR=49-53%TI=Z%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5DC%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=FA-104%TG=FF%W=2000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=2000%S=A+%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=2000%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=2000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=2000%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=1BD8|1E8F|216B|247B|27B6%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=27-40%TG=40%CD=S)

# TANDBERG 990 MXP Video Conferencing Unit
# Tandberg T1000 [TTC7-02] integrated Video Conferencing Unit
# Tandberg Codec 2500, also known as: Tandberg 2500 Classic, Firmware=B10.3
# Tandberg T1000 portable video conference codec
Fingerprint Tandberg video conferencing system (1000, 2500, or 990 MXP)
Class Tandberg | embedded || webcam
SEQ(SP=FD-109%GCD=1-6%ISR=101-111%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=3E80%W2=3E80%W3=3E80%W4=3E80%W5=3E80%W6=3E80)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3E80%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=ARF%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=3E80%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=RF%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=ARF%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=RF%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=ARF%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Tandem Himalaya K2000, Guardian 90 (Operating System D30, Release D39.02)
Fingerprint Tandem Himalaya K2000 server (Guardian 90)
Class Tandem | Guardian || general purpose
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Technisat Digicoder HD S2, sat receiver
Fingerprint TechniSat Digicorder HD S2 satellite receiver
Class TechniSat | embedded || media device
SEQ(SP=C5-D9%GCD=1-6%ISR=D7-E1%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4W0L%O2=M5B4W0L%O3=M5B4W0L%O4=M5B4W0L%O5=M5B4W0L%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=6E-78%TG=80%W=2000%O=M5B4W0L%CC=N%Q=)
T1(R=Y%DF=N%T=6E-78%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=6E-78%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=6E-78%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=6E-78%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=6E-78%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=6E-78%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=82A0%RUD=G)
IE(DFI=N%T=6E-78%TG=80%CD=Z)

# Tektronix Phaser 8200DP, firmware: OS 3.106 laser printer
Fingerprint Tektronix Phaser 8200DP laser printer
Class Tektronix | embedded || printer
SEQ(R=N)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=7A-84%TG=80%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=7A-84%TG=80%S=Z%A=S+%F=AR%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7A-84%TG=80%W=0%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=7A-84%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7A-84%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7A-84%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7A-84%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7A-84%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7A-84%TG=80%CD=S)

# Telekom T-Sinus 130 DSL Router
Fingerprint T-Sinus 130 DSL router
Class Telekom | embedded || broadband router
SEQ(SP=8A-9A%GCD=1-6%ISR=96-A0%TI=I%II=I%SS=O%TS=0)
OPS(O1=NNT11|M57ENW0NNT00NNS%O2=NNT11|M57ENW0NNT00NNS%O3=NNT11|M57ENW0NNT00%O4=NNT11|M57ENW0NNT00NNS%O5=NNT11|M57ENW0NNT00NNS%O6=)
WIN(W1=7FFF%W2=7FFF%W3=7FFF%W4=7FFF%W5=7FFF%W6=0)
ECN(R=Y%DF=N%T=3A-44%TG=40%W=0%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3A-44%TG=40%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=1AF8%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# Telewell TW-EA501 (version 1) ADSL modem/router, Firmware Version: 2.7.0.38(UE0.B1C)3.5.12.4, ADSL Firmware Version: FwVer:3.5.12.4_A_TC3084 HwVer:T14.F7_0.0
Fingerprint Telewell TW-EA501 ADSL modem
Class Telewell | embedded || broadband router
SEQ(SP=0-16%GCD=A000|14000|1E000|28000|32000|64000|C8000|12C000|190000|1F4000%ISR=AB-B5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M578%O4=M578%O5=M578%O6=M578)
WIN(W1=AF0%W2=AF0%W3=AF0%W4=AF0%W5=AF0%W6=AF0)
ECN(R=Y%DF=N%T=FE%TG=FF%W=AF0%O=M578%CC=N%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# TELEX IP-223  Radio over IP interface device
Fingerprint Telex IP-223 radio IP adapter
Class Telex | embedded || bridge
SEQ(SP=CE-D8%GCD=1-6%ISR=D4-DE%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4W0L%O2=M5B4W0L%O3=M5B4W0L%O4=M5B4W0L%O5=M5B4W0L%O6=M5B4)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=6C-76%TG=80%W=4000%O=M5B4W0L%CC=N%Q=)
T1(R=Y%DF=N%T=6C-76%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=6C-76%TG=80%W=4000%S=O%A=S+%F=AS%O=M5B4W0L%RD=0%Q=)
T4(R=Y%DF=N%T=6C-76%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=6C-76%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=6C-76%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=6C-76%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=6C-76%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=2389%RUD=G)
IE(DFI=N%T=6C-76%TG=80%CD=Z)

# Telsey Videostation provided by an italian internet provider called Fastweb. It runs on a 2.4.19 linux kernel customized by Fastweb.
Fingerprint Telsey IP Video Station media server
Class Telsey | embedded || media device
SEQ(SP=C-16%GCD=9C4|1388|1D4C|2710|30D4%ISR=5D-67%TI=I%TS=U)
OPS(O1=M578%O2=M578%O3=M578%O4=M578%O5=M578%O6=M578)
WIN(W1=578%W2=578%W3=578%W4=578%W5=578%W6=578)
ECN(R=Y%DF=N%T=20-36%TG=40%W=578%O=M578%CC=N%Q=)
T1(R=Y%DF=N%T=22-39%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=28-3C%TG=40%W=578%S=O%A=S+%F=AS%O=M578%RD=0%Q=)
T4(R=Y%DF=N%T=22-3B%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=21-3B%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=Y%DF=N%T=27-3E%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Teltronics NET-PATH <http://www.teltronics.com/products_services/ism/text.asp?id=SEBNETPATH> OS Version: 3.0.1.1047 Application Version: 3.1.1.1057
Fingerprint Teltronics NET-PATH intrusion detection system
Class Teltronics | embedded || firewall
SEQ(SP=46-95%GCD=FA|1F4|2EE|3E8|4E2%ISR=8C-BA%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5A2%O2=M5A2%O3=M5A2%O4=M5A2%O5=M5A2%O6=M5A2)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=400%O=M5A2%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# iRMX III R2.2 (for MS-DOS)
Fingerprint TenAsys iRMX III 2.2
Class TenAsys | iRMX | 2.X | specialized
SEQ(R=N)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4074%W5=4180%W6=403D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=403D%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Thecus N5200 Pro NAS
Fingerprint Thecus N52000PRO NAS device
Class Thecus | embedded || storage-misc
SEQ(SP=AE-B8%GCD=1-6%ISR=B5-BF%TI=Z%CI=I%II=I%TS=8)
OPS(O1=M3E58ST11NW5%O2=M3E58ST11NW5%O3=M3E58NNT11NW5%O4=M3E58ST11NW5%O5=M3E58ST11NW5%O6=M3E58ST11)
WIN(W1=7C98%W2=7C98%W3=7C98%W4=7C98%W5=7C98%W6=7C98)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=7CB0%O=M3E58NNSNW5%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=7C98%S=O%A=S+%F=AS%O=M3E58ST11NW5%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# SpeedTouch 510 SW-Version  : 4.2.7.16.0
Fingerprint Thomson SpeedTouch 510 DSL modem
Class Thomson | embedded || broadband router
SEQ(SP=100-10A%GCD=1-6%ISR=102-10C%TI=I%TS=1)
OPS(O1=M200NW0NNT11%O2=M200NW0NNT11%O3=M200NW0NNT11%O4=M200NW0NNT11%O5=M200NW0NNT11%O6=M200NNT11)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M200NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Broadband Router; Thompson SpeedTouch 530
# Speedtouch 580
# Thomson Telecom Belgium Speedtouch 530
# Thomson SpeedTouch 510i
# SpeedTouch 510 ADSL modem/router Firmware version 4.2.7.16.0
Fingerprint Thomson SpeedTouch 510/510i/530/580 DSL modem
Class Thomson | embedded || broadband router
SEQ(SP=FD-107%GCD=1-6%ISR=105-10F%TI=I%II=I%SS=S%TS=1)
OPS(O1=M200NW0NNT11%O2=M200NW0NNT11%O3=M200NW0NNT11%O4=M200NW0NNT11%O5=M200NW0NNT11%O6=M200NNT11)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M200NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Thomson (formerly called Speedtouch) ST536i. The firmware is common to models ST516, ST536 and ST546, and these models with "i" appended.
Fingerprint Thomson ST 536i ADSL modem
Class Thomson | embedded || broadband router
SEQ(SP=102-10C%GCD=1-6%ISR=109-113%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=48%UN=0%RIPL=134%RID=G%RIPCK=I%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Thomson cable modem tcm390
Fingerprint Thomson TCM390 cable modem
Class Thomson | embedded || broadband router
SEQ(SP=7B-89%GCD=1-6%ISR=83-91%TI=I%II=I%SS=S%TS=U)
OPS(O1=M200NW0%O2=M200NW0%O3=M200NW0%O4=M200NW0%O5=M200NW0%O6=M200)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M200NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Thomson TCW 710
Fingerprint Thomson TCW710 wireless cable modem
Class Thomson | embedded || broadband router
SEQ(SP=DF-101%GCD=1-6%ISR=E2-10A%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4074%W5=4180%W6=403D)
ECN(R=N)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Thomson ST2030
# Thomson ST2030 VoIP Phone
Fingerprint Thomson ST 2030 VoIP phone
Class Thomson | embedded || VoIP phone
SEQ(SP=F3-10D%GCD=1-6%ISR=FB-113%TI=I%II=I%SS=S%TS=9)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Thomson Symbio phone.
Fingerprint Thomson Symbio VoIP phone
Class Thomson | embedded || VoIP phone
SEQ(SP=BD-C7%GCD=1-6%ISR=C3-CD%TI=Z%TS=8)
OPS(O1=M5ACST11NW1%O2=M5ACST11NW1%O3=M5ACNNT11NW1%O4=M5ACST11NW1%O5=M5ACST11NW1%O6=M5ACST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5ACNNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=D563%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Topfield TF6000PVR ES (Satellite based digital video recorder)
# Topfield TF600PVRc
# Topfield TF600PVR
Fingerprint Topfield TF6000PVR set top box
Class Topfield | embedded || media device
SEQ(SP=0-5F%GCD=1-6|7FC|FF8|17F4|1FF0|27EC%ISR=56-94%TI=Z%CI=Z%II=RI%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=4E20%W2=4E20%W3=4E20%W4=4E20%W5=4E20%W6=4E20)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=4E20%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=FA-104%TG=FF%W=4E20%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=4E20%S=A+%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=4E20%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=4E20%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=4E20%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=20-3F%TG=40%CD=S)

# Toshiba Digital television set (REGZA series)
Fingerprint Toshiba REGZA TV
Class Toshiba | embedded || media device
SEQ(SP=BE-C8%GCD=1-6%ISR=C4-CE%TI=Z%II=I%TS=A|C)
OPS(O1=NNT11|M5B4ST11NW1%O2=NNT11|M5B4ST11NW1%O3=NNT11|M5B4NNT11NW1%O4=NNT11|M5B4ST11NW1%O5=NNT11|M5B4ST11NW1%O6=NNT11|M5B4ST11)
WIN(W1=10F8%W2=10F8%W3=10F8%W4=10F8%W5=10F8%W6=10F8)
ECN(R=Y%DF=Y%T=3B-45|7B-85%TG=40|80%W=111C%O=|M5B4NNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45|7B-85%TG=40|80%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45|7B-85%TG=40|80%W=10F8%S=O%A=O|S+%F=A|AS%O=NNT11|M5B4ST11NW1%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Toshiba e-Studio20 printer, ROM Version 6.19 TA
Fingerprint Toshiba e-STUDIO 20 printer
Class Toshiba | embedded || printer
SEQ(R=N)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3C%TG=40%W=1000%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=3C%TG=40%S=Z%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3C%TG=40%W=1000%S=Z%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3C%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3C%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3C%TG=40%CD=S)

# Toshiba e-STUDIO280 (network copier/printer)
Fingerprint Toshiba e-STUDIO 280 multifunction printer
Class Toshiba | embedded || printer
SEQ(SP=CB-13B%GCD=1-6%ISR=D7-11D%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=71-7B%TG=80%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=71-7B%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=71-7B%TG=80%W=2000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=71-7B%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=71-7B%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=71-7B%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=71-7B%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=71-7B%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=2A39%RUD=G)
IE(DFI=N%T=71-7B%TG=80%CD=Z)

# TOSHIBA e-STUDIO 4511
Fingerprint Toshiba e-STUDIO 4511 multifunction printer
Class Toshiba | embedded || printer
SEQ(SP=C9-135%GCD=1-6%ISR=D6-120%TI=I%II=I%SS=O|S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M200%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=72-7C%TG=80%W=2000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=72-7C%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=72-7C%TG=80%W=2000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=72-7C%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=72-7C%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=72-7C%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=72-7C%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=72-7C%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=84B7%RUD=G)
IE(DFI=N%T=72-7C%TG=80%CD=Z)

# Toshiba Magnia SG10, Linux toshiba.toshiba.loc 2.4.18-3custom #3 Tue Aug 13 15:10:18 PDT 2002 i686 unknown
Fingerprint Toshiba Magnia SG10 server appliance (Linux 2.4.18)
Class Toshiba | Linux | 2.4.X | general purpose
SEQ(SP=C9-D3%GCD=1-6%ISR=CD-D7%TI=Z%II=I%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AP|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%S=O%A=O|S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=A|O%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=0%S=Z%A=O|S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# TP-Link TL-WA5210G 2.4 GHz high Power Wireless Outdoor CPE, Firmware Version: 4.4.3 Build 100510 Rel.33448n [VxWorks? --Ed.]
Fingerprint TP-Link TL-WA5210G WAP
Class TP-Link | embedded || WAP
SEQ(SP=97-A1%GCD=1-6%ISR=9C-A6%TI=I%CI=I%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O%F=AS%RD=0)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(R=N)

# TP-LINK TL-WR941N (Probably Linux --Ed.)
# TP-LINK WR941N v2/v3 00000000, 3.11.8 Build 100609 Rel.61214n
# Model: TL-WR841ND v5 Firmware Version: 3.11.7 Build 100603 Rel.56412n
# TP-Link TL-WA801N Wireless Access Point Firmware Version: 3.10.6 Build 100408 Rel.37896n
# TP-Link TL-WR1043N(D) Firmware 3.12.2 Build 100820 Rel.41891n
Fingerprint TP-Link WAP: TL-WA801N, TL-WR841ND, TL-WR941N, or TL-WR1043N
Class TP-Link | embedded || WAP
SEQ(SP=C6-D0%GCD=1-6%ISR=C9-D3%TI=Z%CI=I%II=I%TS=A)
OPS(O1=M5B4ST11NW1%O2=M5B4ST11NW1%O3=M5B4NNT11NW1%O4=M5B4ST11NW1%O5=M5B4ST11NW1%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Trendware Broadband Router TW100-BRF114, Version 2.0 Release 04
Fingerprint TRENDnet TW100-BRF114 broadband router
Class TRENDnet | embedded || broadband router
SEQ(SP=0-5%GCD=80|100|180|200|280%ISR=4D-57%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M564%O3=M5B4%O4=M5B4%O5=M204%O6=MF5)
WIN(W1=C00%W2=C00%W3=C00%W4=C00%W5=C00%W6=C00)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=C00%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=C00%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=ECA7%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# Trendnet TW-100-S4W1CA/RO router
Fingerprint TRENDnet TW100-S4W1CA router
Class TRENDnet | embedded || router
SEQ(SP=8D-9F%GCD=1-6%ISR=98-A2%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5A8NW0NNT11%O2=M5A8NW0NNT11%O3=M5A8NW0NNT11%O4=M5A8NW0NNT11%O5=M5A8NW0NNT11%O6=M5A8NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=43E0%W5=4180%W6=403D)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=403D%S=O%A=S+%F=AS%O=M5A8NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=134%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# TRENDnet TV-IP100 Internet camera
Fingerprint TRENDnet TV-IP100 Internet camera
Class TRENDnet | embedded || webcam
SEQ(SP=C-16%GCD=37|6E|A5|DC|113%ISR=4B-55%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=16D0%O=M5B4%CC=N%Q=U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=16D0%S=O%A=S+%F=ASF%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=N%T=FA-104%TG=FF%CD=Z)

# TRIPP LITE SMART1500SLT, Firmware Version: 12.04.0045
# TRIPP LITE SMART1500SLT with network card.
Fingerprint Tripp Lite SMART1500SLT UPS
Class Tripp Lite | embedded || power-device
SEQ(SP=CC-F4%GCD=1-6%ISR=D5-E7%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4W0L%O2=M5B4W0L%O3=M5B4W0L%O4=M5B4W0L%O5=M5B4W0L%O6=M5B4)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=74-7E%TG=80%W=4000%O=M5B4W0L%CC=N%Q=)
T1(R=Y%DF=N%T=74-7E%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=74-7E%TG=80%W=4000%S=O%A=S+%F=AS%O=M5B4W0L%RD=0%Q=)
T4(R=Y%DF=N%T=74-7E%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=74-7E%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=74-7E%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=74-7E%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=74-7E%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=8532|8564%RUD=G)
IE(DFI=N%T=74-7E%TG=80%CD=Z)

# TUT Systems SMS2000
Fingerprint Tut Systems SMS2000 subscriber management system
Class Tut Systems | embedded || router
SEQ(SP=FD-107%GCD=1-6%ISR=10A-114%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=7FE0%W2=7FE0%W3=7FE0%W4=7FE0%W5=7FE0%W6=7FE0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=7FE0%O=M5B4%CC=N%Q=U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45|FA-104%TG=40|FF%W=0|7FE0%S=O|Z%A=O|S+%F=AR|ASF%O=|M109%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=2466%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Ubicom ipOS (IP3023 network processor).
Fingerprint Ubicom ipOS
Class Ubicom | ipOS || specialized
SEQ(SP=9E-AE%GCD=1-6%ISR=AE-BC%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=10%W2=10%W3=10%W4=10%W5=10%W6=10)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=10%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=10%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=Z)

# AirOS on a rebranded NanoStation
Fingerprint Ubiquity AirOS (Linux)
Class Ubiquiti | Linux || WAP
SEQ(SP=C9-D3%GCD=1-6%ISR=CA-D4%TI=Z%CI=I%TS=A)
OPS(O1=M5B4ST11NW1%O2=M5B4ST11NW1%O3=M5B4NNT11NW1%O4=M5B4ST11NW1%O5=M5B4ST11NW1%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16A0%S=O%A=S+%F=AS%O=M5B4ST11NW1%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=8C73%RUD=G)
IE(R=N)

# USRobotics USR8000 broadband router, Firmware Version 1.25 German
Fingerprint USRobotics USR8000 broadband router
Class USRobotics | embedded || router
SEQ(SP=0-5%GCD=64|C8|12C|190|1F4%ISR=4A-54%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3%O=%CC=N%Q=U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=80%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=100%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=400%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Firmware version: R1.95j, Model Number: USR998000
Fingerprint USRobotics USR8000 broadband router
Class USRobotics | embedded || router
SEQ(SP=0-5%GCD=64|C8|12C|190|1F4%ISR=4B-55%TI=BI%II=BI%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=860%W2=860%W3=860%W4=860%W5=860%W6=860)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3%O=%CC=N%Q=U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=80%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=100%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=400%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# USR5450 access point
Fingerprint USRobotics USR5450 WAP
Class USRobotics | embedded || WAP
SEQ(SP=B9-C3%GCD=1-6%ISR=C1-CB%TI=Z%II=I%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=Y%T=41%TG=40%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=41%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=7A-84%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=7A-84%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7A-84%TG=80%CD=S)

# vantage digital 7100s satellite decoder with software version 2.44.
Fingerprint Vantage HD7100S satellite receiver
Class Vantage | embedded || media device
SEQ(SP=C-16%GCD=7D00|FA00|17700|1F400|27100%ISR=96-A0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=16D0%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# System Description VBrick Systems Inc., Model 4300. This is a network based video encoder.
Fingerprint VBrick 4300 video encoder
Class VBrick | embedded || media device
SEQ(SP=97-A1%GCD=1-6%ISR=9D-A7%II=I%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=2000%S=O%A=O%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Hardware Platform  : Vega 400  H323 Firmware Rev 08.00 for H/W Type 10
Fingerprint Vegastream Vega 400 VoIP Gateway
Class Vegastream | embedded || VoIP adapter
SEQ(SP=E7-103%GCD=1-6%ISR=106-110%TI=I|RD%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=3E80%W2=3E80%W3=3E80%W4=3E80%W5=3E80%W6=3E80)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3E80%O=|M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=3E80%S=O%A=O|S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Vegastream, Express Logic's ThreadX RTOS
Fingerprint Vegastream VoIP Gateway
Class Vegastream | ThreadX || VoIP adapter
SEQ(SP=FB-10B%GCD=1-6%ISR=107-111%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=3E80%W2=3E80%W3=3E80%W4=3E80%W5=3E80%W6=3E80)
ECN(R=Y%DF=N%T=19-23%TG=20%W=3E80%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=19-23%TG=20%W=3E80%S=O%A=S+%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=19-23%TG=20%CD=S)

# Vilar IPCamera's OS is based on Linux 2.6 kernel
Fingerprint Vilar IP Camera (Linux 2.6)
Class Vilar | Linux | 2.6.X | webcam
SEQ(SP=C0-CA%GCD=1-6%ISR=C6-D0%TI=Z%CI=I%II=I%TS=U)
OPS(O1=M5B4NNSNW1%O2=M5B4NNSNW1%O3=M5B4NW1%O4=M5B4NNSNW1%O5=M5B4NNSNW1%O6=M5B4NNS)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%S=O%A=S+%F=AS%O=M5B4NNSNW1%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Visual UpTime Select IP Transport DS3/E3 Inline ASE Software version:     I 3.1.011 - May 10 2009
Fingerprint Visual Network Systems Visual UpTime Select IP Transport DS3/E3 inline ASE
Class Visual Network Systems | embedded || specialized
SEQ(CI=I%II=I)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=1%W2=3F%W3=4%W4=4%W5=10%W6=200)
ECN(R=Y%DF=N%T=26-35%TG=40%W=3%O=%CC=N%Q=U)
T1(R=Y%DF=N%T=29-37%TG=40%S=Z%A=S+%F=AR%RD=0%Q=)
T2(R=Y%DF=Y%T=20-3B%TG=40%W=80%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=25-36%TG=40%W=100%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=20-30|33-3F%TG=40%W=400%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=27-3D%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=20-2C|2E-3B%TG=40%W=8000%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1F-33|35-3F%TG=20|40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=19-23%TG=20%CD=S)

# Visual UpTime Select IP Transport NxT1 Inline ASE Software version:     I 3.1.011 - May 10 2009
Fingerprint Visual Network Systems Visual UpTime Select IP Transport NxT1 inline ASE
Class Visual Network Systems | embedded || specialized
SEQ(SP=FA-106%GCD=1-6%ISR=100-10E%TI=I%CI=I%II=I%SS=O%TS=U)
OPS(O1=M564%O2=M564%O3=M564%O4=M564%O5=M564%O6=M564)
WIN(W1=7FF%W2=7FF%W3=7FF%W4=7FF%W5=7FF%W6=7FF)
ECN(R=Y%DF=N%T=19-2D%TG=20%W=FFFF%O=|M564%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=22-34%TG=40%W=80%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=19-30%TG=20|40%W=100|7FE%S=O|Z%A=O%F=AR|AS%O=|M564%RD=0%Q=)
T4(R=Y%DF=Y%T=21-3C%TG=40%W=400%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=22-36%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=20-3E%TG=40%W=8000%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=26-40%TG=40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=19-23%TG=20%CD=S)

# Visual UpTime Select IP Transport T1 CSU DROP & INSERT ASE Software version:     I 3.1.011 - May 10 2009
Fingerprint Visual Network Systems Visual UpTime Select IP Transport T1 CSU DROP & INSERT ASE
Class Visual Network Systems | embedded || specialized
SEQ(CI=I%II=I)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=1%W2=3F%W3=4%W4=4%W5=10%W6=200)
ECN(R=Y%DF=N%T=20-39%TG=40%W=3%O=%CC=N%Q=U)
T1(R=Y%DF=N%T=27-39%TG=40%S=Z%A=S+%F=AR%RD=0%Q=)
T2(R=Y%DF=Y%T=28-3F%TG=40%W=80%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=25-3F%TG=40%W=100%S=Z%A=O%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=20-3E%TG=40%W=400%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=23-3F%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=21-3D%TG=40%W=8000%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=25-3D%TG=40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=19-23%TG=20%IPL=38%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=19-23%TG=20%CD=S)

# VMware ESX 3.0.1 vmkernel ip stack
# VMWARE ESX-Server 3.0.1 (VMotion Interface)
# VMWare ESX Server,3.0.1,42829 (VMKernel Port)
# VMWare ESX 3.5 entreprise server, "vmotion" IP address
# ESX Server 3i Update 2 build 110271
# ESXi Server 3.5.0u2-110271
# ESX 3.5.0 v120505
# ESXi 3.5 Update 4
# VMKernel for ESX 3.5.0 build 110268
Fingerprint VMware ESX Server 3.0.1 - 3.5.0
Class VMware | ESX Server | 3.X | specialized
SEQ(SP=F0-108%GCD=1-6%ISR=FF-111%TI=Z%II=RI%TS=7)
OPS(O1=M5B4NW1NNT11%O2=M5B4NW1NNT11%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11%O5=M5B4NW1NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# ESX Server 3.0.2 (default firewall configuration)
Fingerprint VMware ESX Server 3.0.2
Class VMware | ESX Server | 3.X | specialized
SEQ(SP=FD-107%GCD=1-6%ISR=105-113%TI=Z%II=I%TS=7)
OPS(O1=M5B4NW1NNT11%O2=M5B4NW1NNT11%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11%O5=M5B4NW1NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(R=N)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# VMWare ESXi, Update 3 (embedded version of VMWare ESX)
# VMWare ESX version 3.5.0 (build 64607), Linux 2.4.21-47.0.1.ELvmnix #1 Thu Nov 29 17:50:29 PST 2007 i686 i686 i386 GNU/Linux
# VMware ESXi 3.5 Installable Update 3, Version: 3.5 Update 3 | 2008/11/06 | Build: 123629
# ESXi 3.5 U2
# ESX server 3i 3.5.0 build-123629 2008-10-15 21:03:57.000
Fingerprint VMware ESX Server 3.5.0
Class VMware | ESX Server | 3.X | specialized
SEQ(SP=F4-10C%GCD=1-6%ISR=100-111%TI=Z%II=RI%TS=7)
OPS(O1=M5B4NW1NNT11%O2=M5B4NW1NNT11%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11%O5=M5B4NW1NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M5B4NW1NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# VMware ESXi 3.5 Server
Fingerprint VMware ESXi Server 3.5
Class VMware | ESX Server | 3.X | specialized
SEQ(SP=F6-106%GCD=1-6%ISR=104-10E%TI=Z%CI=RI%TS=7)
OPS(O1=M5B4NW1NNT11%O2=M5B4NW1NNT11%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11%O5=M5B4NW1NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=0-FFFF%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# ESX 4.0.1 vkernel interface, jumbo frames enabled
Fingerprint VMware ESX Server 4.0.1
Class VMware | ESX Server | 4.X | specialized
SEQ(SP=FE-108%GCD=1-6%ISR=107-113%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW3NNT11SLL%O2=M5B4NW3NNT11SLL%O3=M5B4NW3NNT11%O4=M5B4NW3NNT11SLL%O5=M5B4NW3NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW3SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW3NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# VMware ESXi 4
Fingerprint VMware ESXi Server 3.0 - 4.0
Class VMware | ESX Server | 4.X | specialized
SEQ(SP=FC-10A%GCD=1-6%ISR=105-10F%TI=RI%TS=7)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# VMWare ESXi 4
Fingerprint VMware ESXi Server 4.0
Class VMware | ESX Server | 4.X | specialized
SEQ(SP=FB-107%GCD=1-6%ISR=105-10F%TI=I%II=I%SS=S%TS=7)
OPS(O1=M564NW1NNT11%O2=M564NW1NNT11%O3=M564NW1NNT11%O4=M564NW1NNT11%O5=M564NW1NNT11%O6=M564NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M564NW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=O%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# VMware ESXi 4
Fingerprint VMware ESXi Server 4.0
Class VMware | ESX Server | 4.X | specialized
SEQ(SP=F7-101%GCD=1-6%ISR=FF-109%TI=I%II=I%SS=O|S%TS=7)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# VMware ESXi 4.0.0 build 208167
Fingerprint VMware ESXi Server 4.0.0
Class VMware | ESX Server | 4.X | specialized
SEQ(SP=EA-10C%GCD=1-6%ISR=109-113%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# ESXi 4.0 Update 1
Fingerprint VMware ESXi Server 4.0.1
Class VMware | ESX Server | 4.X | specialized
SEQ(SP=FC-108%GCD=1-6%ISR=108-112%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW1NNT11SLL%O2=M5B4NW1NNT11SLL%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11SLL%O5=M5B4NW1NNT11SLL%O6=M5B4NNT11SLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW1SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11SLL%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# VMware ESXi 4.1
# vSphere ESXi 4.1
# VMWare ESXi, 4.1.0, 260247
Fingerprint VMware ESXi Server 4.1
Class VMware | ESX Server | 4.X | specialized
SEQ(SP=80-EC%GCD=1-6%ISR=F4-FE%TI=I%CI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW4ST11%O2=M578NW4ST11%O3=M280NW4NNT11%O4=M5B4NW4ST11%O5=M218NW4ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW4SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW4ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# VMWare ESXi Server 4.1
Fingerprint VMware ESXi Server 4.1
Class VMware | ESX Server | 4.X | specialized
SEQ(SP=96-B0%GCD=1-6%ISR=F7-101%TI=RI%CI=I%TS=7)
OPS(O1=M5B4NW4ST11%O2=M578NW4ST11%O3=M280NW4NNT11%O4=M5B4NW4ST11%O5=M218NW4ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW4SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW4ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# vSphere ESXi 4.1
Fingerprint VMware ESXi Server 4.1
Class VMware | ESX Server | 4.X | specialized
SEQ(SP=84-B4%GCD=2|4|6|8|A%ISR=F5-FF%TI=I%CI=I%II=I%SS=O%TS=7)
OPS(O1=M5B4NW4ST11%O2=M578NW4ST11%O3=M280NW4NNT11%O4=M5B4NW4ST11%O5=M218NW4ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW4SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N|Y%T=3B-45%TG=40%W=FFFF%S=O%A=O|S+%F=AS%O=M109NW4ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# ESXi 4.1.0
Fingerprint VMware ESXi Server 4.1
Class VMware | ESX Server | 4.X | specialized
SEQ(SP=BA-F4%GCD=3|6|9|C|F%ISR=F4-FE%TI=I%TS=7)
OPS(O1=M5B4NW4ST11%O2=M578NW4ST11%O3=M280NW4NNT11%O4=M5B4NW4ST11%O5=M218NW4ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW4SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# VMware ESXi, 4.1.0, 260247
Fingerprint VMware ESXi Server 4.1
Class VMware | ESX Server | 4.X | specialized
SEQ(SP=BA-D8%GCD=8|10|18|20|28%ISR=F5-FF%CI=I%II=I%TS=7)
OPS(O1=M5B4NW4ST11%O2=M578NW4ST11%O3=M280NW4NNT11%O4=M5B4NW4ST11%O5=M218NW4ST11%O6=M109ST11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%O=M5B4NW4SLL%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=FFFF%S=O%A=S+%F=AS%O=M109NW4ST11%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%RD=0)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%RD=0)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%RD=0)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S|O%F=AR%RD=0)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Vodafone DSL-Easybox A601 WLAN
Fingerprint Vodafone EasyBox A601 wireless ADSL router
Class Vodafone | embedded || WAP
SEQ(SP=11-1F%GCD=1-6%ISR=4B-55%TI=I%CI=I%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=5000%W2=5000%W3=5000%W4=5000%W5=5000%W6=5000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=5000%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=5000%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=CFC2%RUD=G)
IE(R=N)

# Vodavi XTS-IP PBX (it's Vodavi's newer class of PBX's)
Fingerprint Vodavi XTS-IP PBX
Class Vodavi | embedded || PBX
SEQ(R=N)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=Y%T=FE%TG=FF%S=O%A=O|S+%F=AS|RF%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# Vonage V-Portal device.
Fingerprint Vonage V-Portal VoIP gateway
Class Vonage | embedded || VoIP adapter
SEQ(SP=101-10B%GCD=1-6%ISR=103-10D%TI=I%TS=7)
OPS(O1=M5ACNW0NNT11%O2=M5ACNW0NNT11%O3=M5ACNW0NNT11%O4=M5ACNW0NNT11%O5=M5ACNW0NNT11%O6=M5ACNNT11)
WIN(W1=4380%W2=4110%W3=423C%W4=4074%W5=4180%W6=403D)
ECN(R=N)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=Y%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(R=N)

# HP Procurve 2650 (firmware H.07.50)
# Xerox Phaser 8550DT. Operating System: 4.302. PostScript: 4.8.0
# Xerox Phaser 7400N network printer
# Cisco C1230B running vxWorks 12.01T1
# Cisco 1200 Series AP 12.01T1 (AIR-AP-1220B-E-K9) running VxWorks 12.01A
# Remote System Controller (RSC) card of a Sun Fire 280R server, RSC Version: 2.2.3
# Nortel Ethernet Switch 470-48T-PWR. FW:3.6.0.6   SW:v3.6.3.04 ISVN:2.
# 3COM wireless Access Point 7250
# Nortel Business Policy Switch 2000, FW:3.0.0.5   SW:v3.1.0.78 ISVN:2
# sun rsc (Remote Sytem Control) card. It runs RSC version 2.2.
Fingerprint VxWorks 12.0
Class VxWorks | VxWorks | 12.X | general purpose
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=99-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# W&T Web-Thermometer #57101
Fingerprint W&T Web-IO Thermometer model 57101
Class W&T | embedded || specialized
SEQ(SP=0-5%GCD=1-6%ISR=16-20%TI=I%II=I%SS=S%TS=U)
OPS(O1=M200%O2=M200%O3=M200%O4=M200%O5=M200%O6=M200)
WIN(W1=200%W2=200%W3=200%W4=200%W5=200%W6=200)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=200%O=M200%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=22-3F%TG=40%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=22-40%TG=40%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=21-37%TG=40%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=21-3A%TG=40%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=23-40%TG=40%W=0%S=A%A=S%F=APR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=22-3D%TG=40%W=0%S=A%A=S+%F=APR%O=%RD=0%Q=)
U1(DF=N%T=32-45%TG=40%IPL=38%UN=128%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=2C-40%TG=40%CD=S)

# W&T Web-Thermograph NTC, 10/100BT, 12-24V, firmware version '1.50/1.30'
Fingerprint W&T Web-Thermograph NTC
Class W&T | embedded || specialized
SEQ(SP=70-7A%GCD=2|4|6|8|A%ISR=69-73%TI=I|RD%CI=I%II=I%SS=O%TS=U)
OPS(O1=M200%O2=M200%O3=M200%O4=M200%O5=M200%O6=)
WIN(W1=200%W2=200%W3=200%W4=200%W5=200%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=200%O=M200%CC=N%Q=|U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=AR|AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=128%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# W&T Web-Thermograph NTC, 10/100BT, 12-24V, firmware version '1.53'
Fingerprint W&T Web-Thermograph NTC
Class W&T | embedded || specialized
SEQ(SP=86-90%GCD=1-6%ISR=83-8D%TI=I|RD%CI=I%II=I%SS=O%TS=U)
OPS(O1=M230%O2=M230%O3=M230%O4=M230%O5=M230%O6=)
WIN(W1=230%W2=230%W3=230%W4=230%W5=230%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=%CC=N%Q=U)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=O|S+%F=A|AR|AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=128%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# WAGO IO System 750 Ethernet fieldbus coupler. Firmware revision 02.02.00(04)
Fingerprint WAGO-I/O-SYSTEM 750 automation system
Class WAGO | embedded || specialized
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4LLW1NT11%O2=M5B4LLW1NT11%O3=M5B4LLW1NT11%O4=M5B4LLW1NT11%O5=M5B4LLW1NT11%O6=M5B4NNT11)
WIN(W1=5DC%W2=5DC%W3=5DC%W4=5DC%W5=5DC%W6=5DC)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=5DC%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=5DC%S=O%A=O%F=A%O=NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=5DC%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Watchguard Firebox II 500
Fingerprint WatchGuard FireBox 500 firewall
Class WatchGuard | embedded || firewall
SEQ(SP=101-10B%GCD=1-6%ISR=106-110%TI=I%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4%CC=S%Q=RU)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=S+%F=ASF%O=M109%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# WatchGuard FireBox 700
# WatchGuard Firebox X700, OS Fireware 7.5
Fingerprint WatchGuard FireBox 700 or X700 firewall
Class WatchGuard | embedded || firewall
SEQ(SP=EF-10F%GCD=1-6%ISR=108-112%TI=I%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=3FE0%W2=3FE0%W3=3FE0%W4=3FE0%W5=3FE0%W6=3FE0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=3FE0%O=M5B4%CC=S%Q=RU)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=3FE0%S=O%A=S+%F=ASF%O=M109%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Watchguard Firebox x5 Wireless
# Watchguard Firebox x5 firewall version  7.5.2  Boot ROM  7.2.1
Fingerprint WatchGuard Firebox X5w firewall/WAP
Class WatchGuard | embedded || firewall
Class WatchGuard | embedded || WAP
SEQ(SP=EA-FC%GCD=1-6%ISR=FE-112%TI=RD%II=RI%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=16D0%W2=16D0%W3=16D0%W4=16D0%W5=16D0%W6=16D0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=16D0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=80%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=100%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=400%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=8000%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Westell WireSpeed Dual Connect 6100 DSL Modem
Fingerprint Westell WireSpeed Dual Connect 6100 DSL router
Class Westell | embedded || broadband router
SEQ(SP=95-9F%GCD=1-6%ISR=9C-A6%TI=I%CI=I%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=2000%S=O%A=O%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(R=N)

# Westermo EDW-100 Ethernet Serial Controller
Fingerprint Westermo EDW-100 Ethernet-to-serial bridge
Class Westermo | embedded || bridge
SEQ(SP=CE-D8%GCD=1-6%ISR=D5-DF%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4W0L%O2=M5B4W0L%O3=M5B4W0L%O4=M5B4W0L%O5=M5B4W0L%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=6D-77%TG=80%W=2000%O=M5B4W0L%CC=N%Q=)
T1(R=Y%DF=N%T=6D-77%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=6D-77%TG=80%W=2000%S=O%A=S+%F=AS%O=M5B4W0L%RD=0%Q=)
T4(R=Y%DF=N%T=6D-77%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=6D-77%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=6D-77%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=6D-77%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=6D-77%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=94B6%RUD=G)
IE(DFI=N%T=6D-77%TG=80%CD=Z)

# Linux 2.6.17.14 #1 PREEMPT Fri Jan 18 10:40:25 GMT 2008 armv5tejl GNU/Linux, MyBook World Edition 2 NAS, Fireware: 02.00.18
Fingerprint Western Digital MyBook World Edition 2 NAS device (Linux 2.6.17.14)
Class Western Digital | Linux | 2.6.X | storage-misc
SEQ(SP=C6-D0%GCD=1-6%ISR=C7-D1%TI=Z%II=I%TS=9)
OPS(O1=M5B4ST11NW1%O2=M5B4ST11NW1%O3=M5B4NNT11NW1%O4=M5B4ST11NW1%O5=M5B4ST11NW1%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M5B4NNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=8806%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Dell laser printer 1600n V1.11(1600n)
# Dell Laser MFP 1600n OS Ver. 1.21 Nic ver. 1.11
# samsung ML-2150 series printer
# "Samsung KS32C" microcontroller. This device uses for sure "pSOSystem". http://www.windriver.com/products/run-time_technologies/Real-Time_Operating_Systems/pSOS/
Fingerprint Wind River pSOSystem
Class Wind River | pSOSystem || specialized
SEQ(SP=C-46%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-BB%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Netgear SC101 Storage Central
# Compex WPE54G Wireless Access Point
# Xerox Phaser 6120/N Laser Printer
# Inter-Tel model 8662 VoIP phone, SW v. 2.0.06
# Hitachi WMS 100 SAN Controller, OS Version 0070/G-X
# Hitachi WMS 100 SAN Controller, OS Version 0770/G-X
# ALOM 1.6.3 on Sun Fire V210.
# Sun(tm) Advanced Lights Out Manager CMT v1.2.4
# Sony LocationFree device (used to transmit television broadcasts within a home)
# Allen-Bradley ControlLogix 1756-EWEB
# Harmonic Inc. HLT7806R-D7-AS-AC-5, Firmware: 1.3.0. Its a device for optical video transmission.
# Aastra 9133i IP Phone firmware version 1.4.1.1077
# Canon iR2570CI
# Aastra 480i GT
# Scopus IVG-7100 - Intelligent Video Remultiplexer
# WireSpeed Dual Connect DSL Modem
# Westell WireSpeed Dual Connect, model E90-610015-06, software version VER:04.00.00.02
# Sunfire T2000 Service controller
# Avaya T3 IP II.3 Compact (IP Phone), SW Version: T441_0DE.a3i, Bootloader Version: B02.03
# Nortel Ethernet Routing Switch 5520-48T-PWR  HW:32       FW:4.2.0.12  SW:v4.2.0.002
# Philips SOPHO iS3000 PBX system
# [Sun ALOM is VxWorks for sure. --Ed.]
Fingerprint VxWorks
Class Wind River | VxWorks || printer
Class Wind River | VxWorks || WAP
Class Wind River | VxWorks || storage-misc
Class Wind River | VxWorks || VoIP phone
Class Wind River | VxWorks || media device
Class Wind River | VxWorks || remote management
Class Wind River | VxWorks || switch
SEQ(SP=96-A0%GCD=1-6%ISR=9B-BF%TI=I%CI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=2000%S=O%A=O%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Apple Airport Express V6.3
# Added another Airport express, no version #
# CANON iR C5185
# Canon iR3045 Laser Printer
# Canon iR5055
# Canon imageRUNNER multifunction printer C3380
# Apple Airport Extreme Base Station. Version 5.7.
# Xerox Phaser 8860MFP
# AMX NI-3100 NetLinx Integrated Controller
# VxWorks based firmware for the AMX NI-4100 NetLinx Integrated Controller
# Nortel Communication Server 1000 PBX
# KYOCERA MITA FS-4020DN printer.
# Canon imageRUNNER multifunction printer C10221
# Dell 3130cn Color Laser, Firmware Version 200903231111, Network Firmware Version 13.161
# Xerox Phaser 8560DN
# Kyocera Mita FS-1350DN
Fingerprint VxWorks
Class Wind River | VxWorks || WAP
Class Wind River | VxWorks || printer
SEQ(SP=D1-110%GCD=1-6%ISR=F7-111%TI=I%II=I%SS=S%TS=6)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=4000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=4000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=70%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# WIZnet W3150A, a "Fully Hardwired TCP/IP Chip" that exposes a 4-socket TCP/IP stack to the host as a series of memory-mapped registers.
Fingerprint WIZnet W3150A TCP/IP chip
Class WIZnet | embedded || specialized
SEQ(R=N)
OPS(O1=M5B4%O2=%O3=%O4=%O5=%O6=)
WIN(W1=800%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=0|800%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=7B-85%TG=80%W=0|800%S=A%A=S+%F=R|AS%O=|M109%RD=0%Q=)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
U1(DF=Y%T=7B-85%TG=80%IPL=38%UN=5DC%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Sonicview Ihub with version 1.4 rom
# Arduino board and optional ethernet shield based on Wiznet W5100 chip. Mac address DEADBE.
Fingerprint WIZnet W5100 TCP/IP chip
Class WIZnet | embedded || specialized
SEQ(SP=56-68%GCD=1-6%ISR=C0-CA%TI=I%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M5B4%O5=M218%O6=M109)
WIN(W1=800%W2=800%W3=800%W4=800%W5=800%W6=800)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=800%O=M5B4%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=7B-85%TG=80%W=800%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
U1(DF=Y%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# W5100 in Arduino Ethernet shield. MAC address DEADBE. http://www.arduino.cc/en/Main/ArduinoEthernetShield
Fingerprint WIZnet W5100 TCP/IP chip
Class WIZnet | embedded || specialized
SEQ(R=N)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=0%O=%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=A%A=O%F=R%RD=0%Q=)
T2(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T3(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=7B-85%TG=80%W=0%S=A%A=O%F=R%O=%RD=0%Q=)
U1(DF=Y%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# WowWee Rovio UI v3.97 | Evo v4.72b.201 http://www.wowwee.com/en/support/rovio, runs eCos on a 200MHz ARM9 processor, according to coverage on DeviceGuru
Fingerprint WowWee Rovio mobile webcam
Class WowWee | embedded || webcam
SEQ(SP=92-A0%GCD=1-6%ISR=98-A4%II=I%TS=1)
OPS(O1=M5A8NW0NNT11%O2=M5A8NW0NNT11%O3=M5A8NW0NNT11%O4=M5A8NW0NNT11%O5=M5A8NW0NNT11%O6=M5A8NNT11)
WIN(W1=9310%W2=9264%W3=90BC%W4=9310%W5=9154%W6=904A)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=9448%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=904A%S=O%A=S+%F=AS%O=M5A8NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=9000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=3401%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# thin client Wyse Model SX0
# Wyse S10 Thin Client
# Wyse Winterm 1200 LE terminal
Fingerprint Wyse S10, SX0, or 1200LE terminal
Class Wyse | embedded || terminal
SEQ(SP=90-9A%GCD=1-6%ISR=9D-A7%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=S)

# Wyse V10L thin client
# Wyse 1200LE running Wyse "Thin OS" (Blazer) firmware version 5.2.0_39
Fingerprint Wyse V10L or 1200LE thin client
Class Wyse | embedded || terminal
SEQ(SP=E-18%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=9A-A4%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NNLL%O2=M5B4NNLL%O3=M5B4NNLL%O4=M5B4NNLL%O5=M5B4NNLL%O6=M5B4NNLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%O=M5B4NNLL%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=S)

# Wyse V10L Thin Client running Wyse Thin OS
Fingerprint Wyse V10L thin client
Class Wyse | embedded || terminal
SEQ(SP=8E-98%GCD=1-6%ISR=9A-A4%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NNLL%O2=M5B4NNLL%O3=M5B4NNLL%O4=M5B4NNLL%O5=M5B4NNLL%O6=M5B4NNLL)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%O=M5B4NNLL%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=FFFF%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=S)

# Wyse Linux V6
Fingerprint Wyse S50 thin client (Linux 2.6)
Class Wyse | Linux | 2.6.X | terminal
SEQ(SP=E-18%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=9A-A4%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=7800%W2=7800%W3=7800%W4=7800%W5=7800%W6=7800)
ECN(R=Y%DF=N%T=1B-25%TG=20%W=7800%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=1B-25%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=1B-25%TG=20%W=7800%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=1B-25%TG=20%W=7800%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=7B-85%TG=80%CD=S)

# Xavi 7001 Modem
Fingerprint XAVi 7001 DSL modem
Class XAVi | embedded || broadband router
SEQ(SP=0-5%GCD=61A8|C350|124F8|186A0|1E848|249F0%ISR=8A-94%TI=I%TS=U)
OPS(O1=|M5B4%O2=|M5B4%O3=|M5B4%O4=|M5B4%O5=|M5B4%O6=|M5B4)
WIN(W1=0|1FB0%W2=0|1FB0%W3=0|1FB0%W4=0|1FB0%W5=0|1FB0%W6=0|1FB0)
ECN(R=Y%DF=N|Y%T=3C%TG=40%W=0|1FB0%O=|M5B4%CC=N%Q=)
T1(R=Y%DF=N|Y%T=3C%TG=40%S=O|Z%A=S|S+%F=AR|AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3C%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3C%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3C%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=19-23%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(R=N)

# Device Vendor: XAVi Technologies Corporation Model Number: X7721r+ Device: DSL router
Fingerprint XAVi Technologies X7721r+ DSL router
Class XAVi | embedded || broadband router
SEQ(SP=75-8B%GCD=1-6%ISR=7F-8F%TI=I%TS=U)
OPS(O1=M58C%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=4000%O=M58C%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=7B-85%TG=80%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=Z%F=R%O=%RD=0%Q=)
U1(DF=N%T=96-A0%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)

# Xavi Wireless x7868r
Fingerprint XAVi X7868r wireless ADSL modem
Class XAVi | embedded || WAP
SEQ(SP=7F-8B%GCD=1-6%ISR=81-8D%TI=I%TS=U)
OPS(O1=M58C%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=FDE8%W2=FDE8%W3=FDE8%W4=FDE8%W5=FDE8%W6=FDE8)
ECN(R=Y%DF=Y%T=7B-85%TG=80%W=FDE8%O=M58C%CC=N%Q=)
T1(R=Y%DF=Y%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=7B-85%TG=80%W=FDE8%S=A%A=Z%F=R%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=Y%T=7B-85%TG=80%W=FDE8%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=Z%F=R%O=%RD=0%Q=)
U1(DF=N%T=96-A0%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(R=N)

# Xerox DC220 printer
Fingerprint Xerox DC220 printer
Class Xerox | embedded || printer
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=96-A0%TI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=1000%O=M400%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Xerox DC440 printer
Fingerprint Xerox Document Centre 440 or WorkCentre Pro 55 printer
Class Xerox | embedded || printer
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=96-A0%TI=I|RD%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=4000%W2=4000%W3=4100%W4=4000%W5=40E8%W6=402E)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M400%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Fuji Xerox Document Centre 706 CP. web service reports itself as a "Document Centre 706/606/506"
Fingerprint Xerox Document Centre 706 CP printer
Class Xerox | embedded || printer
SEQ(SP=B-15%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=96-A0%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=1000%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=O|S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Fuji-XEROX DocuPrint C525 A
Fingerprint Xerox DocuPrint C525 A printer
Class Xerox | embedded || printer
SEQ(R=N)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=3000%W2=3000%W3=3000%W4=3000%W5=3000%W6=3000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=3000%O=%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=Z%A=S+%F=AR%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=3000%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=3000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=4E4%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# xerox phaser 3150 printer
Fingerprint Xerox Phaser 3150 printer
Class Xerox | embedded || printer
SEQ(SP=E-18%GCD=FA00|1F400|2EE00|3E800|4E200|5DC00%ISR=99-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=%O2=%O3=%O4=%O5=%O6=)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3A-44%TG=40%W=1000%O=%CC=N%Q=)
T1(R=Y%DF=N%T=3A-44%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3A-44%TG=40%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3A-44%TG=40%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3A-44%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3A-44%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3A-44%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FE%TG=FF%CD=S)

# Xerox Phaser 3300MFP. Operating System  OS 1.50.00.14 07-16-2009, Networking V4.02.06(P3300MFP) 07-16-2009.
Fingerprint Xerox Phaser 3300MFP printer
Class Xerox | embedded || printer
SEQ(SP=0-5%GCD=FA01|1F402|2EE03|3E804|4E205%ISR=95-9F%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=NNM5A0SNW0%O2=NNM5A0SNW0%O3=M5A0NW0%O4=NNM5A0SNW0%O5=NNM5A0SNW0%O6=NNM5A0S)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=1000%O=NNM5A0SNW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=A%A=S+%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=0%S=Z%A=S+%F=R%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=138%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=Z)

# Pinter model 6110
Fingerprint Xerox Phaser 6110 printer
Class Xerox | embedded || printer
SEQ(SP=E-18%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=98-A2%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(R=N)
WIN(R=N)
ECN(R=N)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Phaser 6180N
Fingerprint Xerox Phaser 6180N printer
Class Xerox | embedded || printer
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=3000%W2=3000%W3=3000%W4=3000%W5=3000%W6=3000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=3000%O=%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O|Z%A=S+%F=AR|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=3000%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=3000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=4E4%RID=G%RIPCK=Z%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Xerox Phaser 6250DP
Fingerprint Xerox Phaser 6250DP printer
Class Xerox | embedded || printer
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%CI=RD%II=I%SS=S%TS=U)
OPS(O1=M200NW0%O2=M200NW0%O3=M200NW0%O4=M200NW0%O5=M200NW0%O6=M200)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M200NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=3B-45%TG=40%W=80%S=A%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=100%S=A%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=400%S=A%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=7A69%S=A%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=8000%S=A%A=S+%F=AR%O=WANM109T10S%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=FFFF%S=A%A=S+%F=AR%O=WFNM109T10S%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Xerox Phaser 8560MFP, Operating System: 8.26, Networking: 33.16.05.04.2007
Fingerprint Xerox Phaser 8560 multifunction printer
Class Xerox | embedded || printer
SEQ(SP=14-1E%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=99-A3%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4NW0%O2=M5B4NW0%O3=M5B4NW0%O4=M5B4NW0%O5=M5B4NW0%O6=M5B4)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=2000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Xerox Phaser 860N
# Operating system: 3.38; Networking  12.86.04.06.2001
# Xerox Phaser 8200N
Fingerprint Xerox Phaser 860N or 8200N printer
Class Xerox | embedded || printer
SEQ(SP=0-5%GCD=186A0|30D40|493E0|61A80|7A120|927C0%ISR=9A-A4%TI=I%II=I%SS=S%TS=U)
OPS(O1=M5B4%O2=M578%O3=M280%O4=M218%O5=M218%O6=M109)
WIN(W1=B68%W2=AF0%W3=F00%W4=EA8%W5=EA8%W6=F87)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=B68%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=7B-85%TG=80%W=FFFF%S=O%A=O%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=7B-85%TG=80%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=7B-85%TG=80%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=7B-85%TG=80%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=7B-85%TG=80%CD=S)

# Xerox WorkCentre 7245
Fingerprint Xerox WorkCentre Pro 7245 printer
Class Xerox | embedded || printer
SEQ(SP=95-9F%GCD=1-6%ISR=9B-A5%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=2000%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=2000%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=N)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# Xerox WorkCentre Pro C2128, v1 Multifunction System
Fingerprint Xerox WorkCentre Pro C2128 printer
Class Xerox | embedded || printer
SEQ(SP=C-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=4000%W2=4000%W3=4100%W4=4000%W5=40E8%W6=402E)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4000%O=M400%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=402E%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=15C%RID=4210%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Xirrus XS8 Wi-Fi Array, System software 3.5 (Feb 23 2009), Build: 0706
# Xirrus XS8, System Software version 3.5, Build 0724
Fingerprint Xirrus XS8 WAP
Class Xirrus | embedded || WAP
SEQ(SP=BE-CA%GCD=1-6%ISR=C5-CF%TI=Z%CI=I%II=I%TS=A)
OPS(O1=M5B8ST11NW2%O2=M5B8ST11NW2%O3=M5B8NNT11NW2%O4=M5B8ST11NW2%O5=M5B8ST11NW2%O6=M5B8ST11)
WIN(W1=16B0%W2=16B0%W3=16B0%W4=16B0%W5=16B0%W6=16B0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=1128%O=M5B8NNSNW2%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=16B0%S=O%A=S+%F=AS%O=M5B8ST11NW2%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# XMOS (www.xmos.com) XC-2 development card for their XS1G4 multicore multithreaded processor.
Fingerprint XMOS XC-2 development card
Class XMOS | embedded || specialized
SEQ(SP=0-29%GCD=1-6|BC|CC|178|198|234|264|2F0|330|3AC|3FC%ISR=52-5C%TI=I%II=RI%SS=O%TS=U)
OPS(O1=M80%O2=M80%O3=M80%O4=M80%O5=M80%O6=M80)
WIN(W1=1C0%W2=1C0%W3=1C0%W4=1C0%W5=1C0%W6=1C0)
ECN(R=Y%DF=N%T=FA-104%TG=FF%W=1C0%O=M80%CC=N%Q=)
T1(R=Y%DF=N%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FA-104%TG=FF%W=1C0%S=O%A=S+%F=AS%O=M80%RD=0%Q=)
T4(R=Y%DF=N%T=FA-104%TG=FF%W=1C0%S=A+%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FA-104%TG=FF%W=1C0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FA-104%TG=FF%W=1C0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FA-104%TG=FF%W=1C0%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=2591|2B68|3164|3793|3DEA%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=FA-104%TG=FF%CD=S)

# Xylan OmniStack OS-4024CF running Version 3.4.2
Fingerprint Xylan OmniStack 4024CF switch
Class Xylan | embedded || switch
SEQ(SP=0-16%GCD=FA00|1F400|2EE00|3E800|4E200%ISR=97-A1%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=1000%W2=1000%W3=1000%W4=1000%W5=1000%W6=1000)
ECN(R=Y%DF=N%T=19-23%TG=20%W=1000%O=M400%CC=N%Q=)
T1(R=Y%DF=N%T=19-23%TG=20%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=19-23%TG=20%W=1000%S=O%A=O%F=A%O=%RD=0%Q=)
T4(R=Y%DF=N%T=19-23%TG=20%W=1000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=1B-25%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=Z%RUCK=0%RUD=G)
IE(DFI=S%T=1B-25%TG=20%CD=S)

# Xylan OmniStack! Version 3.2.5
Fingerprint Xylan OmniStack switch (version 3.2.5)
Class Xylan | embedded || switch
SEQ(SP=FF-109%GCD=1-6%ISR=104-10E%TI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT00NNS%O2=M5B4NW0NNT00NNS%O3=M5B4NW0NNT00%O4=M5B4NW0NNT00NNS%O5=M5B4NW0NNT00NNS%O6=M5B4NNT00NNS)
WIN(W1=4470%W2=41A0%W3=4100%W4=40E8%W5=40E8%W6=402E)
ECN(R=Y%DF=N%T=7C-86%TG=80%W=4470%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=7C-86%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=1B-25%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=6A1D%RUD=G)
IE(DFI=S%T=1B-25%TG=20%CD=S)

# Xylan OmniStack! Version 3.4.7
Fingerprint Xylan OmniStack switch (version 3.4.7)
Class Xylan | embedded || switch
SEQ(SP=FF-109%GCD=1-6%ISR=104-10E%TI=I%II=I%SS=S%TS=0)
OPS(O1=M5B4NW0NNT00NNS%O2=M5B4NW0NNT00NNS%O3=M5B4NW0NNT00%O4=M5B4NW0NNT00NNS%O5=M5B4NW0NNT00NNS%O6=M5B4NNT00NNS)
WIN(W1=4470%W2=41A0%W3=4100%W4=40E8%W5=40E8%W6=402E)
ECN(R=Y%DF=N%T=7C-86%TG=80%W=4470%O=M5B4NW0NNS%CC=N%Q=)
T1(R=Y%DF=N%T=7C-86%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=19-23%TG=20%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=19-23%TG=20%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=1B-25%TG=20%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=I%RUCK=3D87%RUD=G)
IE(DFI=S%T=1B-25%TG=20%CD=S)

# AV-Receiver RX-V2065
Fingerprint Yamaha RX-V2065 audio/video receiver
Class Yamaha | embedded || media device
SEQ(SP=F1-103%GCD=1-6%ISR=FE-10A%TI=Z%CI=Z%II=RI%TS=U)
OPS(O1=M578%O2=M578%O3=M280%O4=M578%O5=M218%O6=M109)
WIN(W1=E998%W2=E998%W3=E998%W4=E998%W5=E998%W6=E998)
ECN(R=Y%DF=Y%T=FA-104%TG=FF%W=E998%O=M578%CC=N%Q=)
T1(R=Y%DF=Y%T=FA-104%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=FA-104%TG=FF%W=E998%S=O%A=S+%F=AS%O=M109%RD=0%Q=)
T4(R=Y%DF=Y%T=FA-104%TG=FF%W=E998%S=A+%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=FA-104%TG=FF%W=E998%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=FA-104%TG=FF%W=E998%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=FA-104%TG=FF%W=E998%S=A%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=Y%T=FA-104%TG=FF%IPL=38%UN=6D6C%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=S%T=23-3D%TG=40%CD=S)

# Yamaha Network capable audio receiver, model RX-V3900
Fingerprint Yamaha RX-V3900 audio receiver
Class Yamaha | embedded || media device
SEQ(CI=RD|RI%II=RI%TS=U)
OPS(O1=M5B4%O2=M5B4%O3=M5B4%O4=M5B4%O5=M5B4%O6=M5B4)
WIN(W1=0%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=0%O=M5B4%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=3B-45%TG=40%W=0%S=O%A=O%F=AS%O=M5B4%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Router YAMAHA NETVOLANTE RT58i Rev.9.01.13
Fingerprint Yamaha NetVolante RT58i router
Class Yamaha | embedded || router
SEQ(SP=F1-103%GCD=1-6%ISR=FE-10E%TI=I%II=I%SS=S%TS=7)
OPS(O1=M5B4NW1NNT11%O2=M5B4NW1NNT11%O3=M5B4NW1NNT11%O4=M5B4NW1NNT11%O5=M5B4NW1NNT11%O6=M5B4NNT11)
WIN(W1=FFFF%W2=FFFF%W3=FFFF%W4=FFFF%W5=FFFF%W6=FFFF)
ECN(R=Y%DF=N%T=100%TG=FF%W=FFFF%O=M5B4NW1%CC=N%Q=)
T1(R=Y%DF=N%T=100%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=100%TG=FF%W=FFFF%S=O%A=S+%F=AS%O=M5B4NW1NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=100%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=100%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=100%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=100%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=100%TG=FF%CD=S)

# Zebra LP 2844-Z Label Printer with integrated ethernet, F/W Version: 7.02 (3111A)
Fingerprint Zebra LP 2844-Z label printer
Class Zebra | embedded || printer
SEQ(SP=0-5%GCD=0%ISR=0-5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M218%O2=M218%O3=M218%O4=M218%O5=M218%O6=M218)
WIN(W1=5B4%W2=5B4%W3=5B4%W4=5B4%W5=5B4%W6=5B4)
ECN(R=Y%DF=N%T=7B-85%TG=80%W=5B4%O=M218%CC=N%Q=)
T1(R=Y%DF=N%T=7B-85%TG=80%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=Y%T=1B-25%TG=20%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=7B-85%TG=80%W=5B4%S=O%A=S+%F=AS%O=M218%RD=0%Q=)
T4(R=Y%DF=Y%T=1B-25%TG=20%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=1B-25%TG=20%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=Y%DF=N%T=1B-25%TG=20%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
U1(R=N)
IE(DFI=S%T=3B-45%TG=40%CD=S)

# ZELAX MM-201R-UNI.1, CPU:MPC852, revA, Communication software version 1.2.11
Fingerprint Zelax MM-201R-UNI router
Class Zelax | embedded || router
SEQ(SP=95-9F%GCD=1-6%ISR=9B-A5%TI=I%II=I%SS=S%TS=1)
OPS(O1=M5B4NW0NNT11%O2=M5B4NW0NNT11%O3=M5B4NW0NNT11%O4=M5B4NW0NNT11%O5=M5B4NW0NNT11%O6=M5B4NNT11)
WIN(W1=43E0%W2=4110%W3=423C%W4=4074%W5=4180%W6=403D)
ECN(R=Y%DF=N%T=3B-45%TG=40%W=4470%O=M5B4NW0%CC=N%Q=)
T1(R=Y%DF=N%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=3B-45%TG=40%W=403D%S=O%A=S+%F=AS%O=M5B4NW0NNT11%RD=0%Q=)
T4(R=Y%DF=N%T=3B-45%TG=40%W=4000%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=3B-45%TG=40%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FA-104%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=0%RUD=G)
IE(DFI=N%T=FA-104%TG=FF%CD=S)

# (ADSL Router) ZHONE Firmware: 03.01.08 Product Name: 6211-I3-xxx, Software Version: 3-10-02-2100.A2pB024k1.d20h
Fingerprint Zhone 6211-I3 series ADSL2+ modem
Class Zhone | embedded || broadband router
SEQ(SP=CA-D4%GCD=1-6%ISR=C8-D2%TI=Z%II=I%TS=8)
OPS(O1=M5ACST11NW7%O2=M5ACST11NW7%O3=M5ACNNT11NW7%O4=M5ACST11NW7%O5=M5ACST11NW7%O6=M5ACST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=N)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=B0D8%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Zonealarm Z100G firewall/router (home version of the Checkpoint UTM-1 Edge), running OS version 8.0.42x
Fingerprint ZoneAlarm Z100G WAP
Class ZoneAlarm | embedded || WAP
SEQ(SP=BA-CE%GCD=1-6%ISR=C7-D1%TI=Z%CI=Z%II=I%TS=A)
OPS(O1=M5B4ST11NW7%O2=M5B4ST11NW7%O3=M5B4NNT11NW7%O4=M5B4ST11NW7%O5=M5B4ST11NW7%O6=M5B4ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=37%TG=40%W=16D0%O=M5B4NNSNW7%CC=N%Q=)
T1(R=Y%DF=Y%T=37%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# ZyXEL Model P-2602H-D1A broadband router
Fingerprint ZyXEL P-2602H-D1A DSL modem
Class ZyXEL | embedded || broadband router
SEQ(SP=0-16%GCD=A000|14000|1E000|28000|32000|64000|C8000|12C000|190000|1F4000%ISR=AB-B5%TI=I%CI=RI%II=I%SS=S%TS=U)
OPS(O1=M200%O2=M200%O3=M200%O4=M200%O5=M200%O6=M200)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FE%TG=FF%W=400%O=M200%CC=N%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=3B-45%TG=40%W=0%S=A%A=S%F=AR%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# Zyxel Prestige 660R-61C ADSL router
Fingerprint ZyXEL Prestige 660R ADSL router
Class ZyXEL | embedded || broadband router
SEQ(CI=I%II=I%TS=U)
OPS(O1=M200%O2=|M200%O3=%O4=%O5=%O6=)
WIN(W1=400%W2=0|800%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=FE%TG=FF%W=0%O=%CC=Y%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O%A=O%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# ZyXEL NSA220
Fingerprint ZyXEL NSA-200 NAS device
Class ZyXEL | embedded || storage-misc
SEQ(SP=C9-D3%GCD=1-6%ISR=CA-D4%TI=Z%II=I%TS=7)
OPS(O1=M550ST11NW1%O2=M550ST11NW1%O3=M550NNT11NW1%O4=M550ST11NW1%O5=M550ST11NW1%O6=NNT11|M550ST11)
WIN(W1=16A0%W2=16A0%W3=16A0%W4=16A0%W5=16A0%W6=16A0)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=16D0%O=M550NNSNW1%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# Zyxel ES-3024A switch
Fingerprint ZyXEL ES-3024A switch
Class ZyXEL | embedded || switch
SEQ(SP=0-1D%GCD=A000|14000|1E000|28000|32000|64000|C8000|12C000|190000|1F4000%ISR=AB-B5%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M578%O4=M578%O5=M578%O6=M578)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=FE%TG=FF%W=4000%O=M578%CC=N%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FE%TG=FF%W=4000%S=O%A=O|S+%F=AS%O=M578%RD=0%Q=)
T4(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# Linux version 2.6.17.14_stm22_0041-STB1001H (hhchang@ipav5) (gcc version 4.1.1 (STMicroelectronics/Linux Base 4.1.1-23)) #1 PREEMPT Wed jul 21 14:19:46 CST 2010, Zyxel STB-1001H device provided by http://www.sgtsa.pl/jambox for IPTV 
Fingerprint ZyXEL STB-1001H set-top box (Linux 2.6.17)
Class ZyXEL | Linux | 2.6.X | media device
SEQ(SP=BB-C5%GCD=1-6%ISR=C4-CE%TI=Z%CI=Z%II=I%TS=A)
OPS(O1=M5B4ST11NW4%O2=M5B4ST11NW4%O3=M5B4NNT11NW4%O4=M5B4ST11NW4%O5=M5B4ST11NW4%O6=M5B4ST11)
WIN(W1=5A8%W2=5A8%W3=5A8%W4=5A8%W5=5A8%W6=5A8)
ECN(R=Y%DF=Y%T=3B-45%TG=40%W=5B4%O=M5B4NNSNW4%CC=N%Q=)
T1(R=Y%DF=Y%T=3B-45%TG=40%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=Y%T=3B-45%TG=40%W=5A8%S=O%A=S+%F=AS%O=M5B4ST11NW4%RD=0%Q=)
T4(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=Y%T=3B-45%TG=40%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
U1(DF=N%T=3B-45%TG=40%IPL=164%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=3B-45%TG=40%CD=S)

# ZyXEL Prestige 202 DSS1, ZyNOS version: V2.41(N.01) | 12/20/1999, bootbase version: V1.13 | 4/14/2000
Fingerprint ZyXEL Prestige 202 ISDN router (ZyNOS 2.41)
Class ZyXEL | ZyNOS | 2.X | router
SEQ(SP=0-5%GCD=6C000|D8000|144000|1B0000|21C000%ISR=AB-B5%TI=I%II=I%SS=S%TS=U)
OPS(O1=|M200%O2=|M200%O3=|M200%O4=|M200%O5=|M200%O6=|M200)
WIN(W1=0|2000%W2=0|2000%W3=0|2000%W4=0|2000%W5=0|2000%W6=0|2000)
ECN(R=Y%DF=N%T=FE%TG=FF%W=0|2000%O=|M200%CC=N|Y%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O|Z%A=S+%F=AR|AS%RD=0%Q=)
T2(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FE%TG=FF%W=2000%S=O%A=O|S+%F=AS%O=M200%RD=0%Q=)
T4(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# G-2000PLUS ZyNOS Firmware Version: V3.60(HU.4) | 06/01/2006
Fingerprint ZyXEL G-2000 Plus WAP
Class ZyXEL | ZyNOS | 3.X | broadband router
SEQ(SP=0-16%GCD=A000|14000|1E000|28000|32000|64000|C8000|12C000|190000|1F4000%ISR=AB-B5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M400%O2=M400%O3=M400%O4=M400%O5=M400%O6=M400)
WIN(W1=4000%W2=4000%W3=4000%W4=4000%W5=4000%W6=4000)
ECN(R=Y%DF=N%T=FE%TG=FF%W=4000%O=M400%CC=N%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# P-2602HW-D1A, ZyNOS F/W Version: V3.40(ADQ.4)b1_IPPR_0307 | 03/07/2007
Fingerprint ZyXEL P-2602HW-D1A wireless DSL modem (ZyNOS 3.40)
Class ZyXEL | ZyNOS | 3.X | broadband router
SEQ(SP=D-17%GCD=A000|14000|1E000|28000|32000%ISR=AB-B5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M546%O2=M546%O3=M546%O4=M546%O5=M546%O6=M546)
WIN(W1=5500%W2=5500%W3=5500%W4=5500%W5=5500%W6=5500)
ECN(R=Y%DF=N%T=FE%TG=FF%W=5500%O=M546%CC=N%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# ZyNOS F/W Version: V3.40(AHF.0)b12 | 7/30/2007, DSL FW Version:TI AR7 06.02.00.7b
Fingerprint ZyXEL ZyNOS 3.40
Class ZyXEL | ZyNOS | 3.X | broadband router
SEQ(SP=0-5%GCD=64000|C8000|12C000|190000|1F4000%ISR=AB-B5%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M200%O2=M200%O3=M200%O4=M200%O5=M200%O6=M200)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FE%TG=FF%W=400%O=M200%CC=N%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=N)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# Model Name : ZyWALL 10W, ZyNOS Firmware Version: V3.62(WH.1) | 02/26/2004
Fingerprint ZyXEL ZyWALL 10W firewall (ZyNOS 3.62)
Class ZyXEL | ZyNOS | 3.X | firewall
SEQ(SP=0-2B%GCD=1000|2000|3000|4000|5000|68000|D0000|138000|1A0000|208000%ISR=AB-B5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M578%O2=M578%O3=M578%O4=M578%O5=M578%O6=M578)
WIN(W1=5780%W2=5780%W3=5780%W4=5780%W5=5780%W6=5780)
ECN(R=Y%DF=N%T=FE%TG=FF%W=5780%O=M578%CC=N%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# ZyNOS Firmware Version: V3.62(WK.16) ZyWALL 2
# ZerXEL Prestige 660HW-61
Fingerprint ZyXEL ZyWALL 2 firewall or Prestige 660HW-61 ADSL router (ZyNOS 3.62)
Class ZyXEL | ZyNOS | 3.X | firewall
SEQ(SP=0-29%GCD=1000|2000|3000|4000|5000|6000|64000|C8000|12C000|190000|1F4000|258000%ISR=AB-B5%TI=I%II=I%SS=S%TS=U)
OPS(O1=|M200%O2=|M200%O3=|M200%O4=|M200%O5=|M200%O6=|M200)
WIN(W1=0|400%W2=0|400%W3=0|400%W4=0|400%W5=0|400%W6=0|400)
ECN(R=Y%DF=N%T=FE%TG=FF%W=0|400%O=|M200%CC=N|Y%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O|Z%A=S+%F=AR|AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# ZyXEL ZyWALL 70 Internet Security Appliance, firmware 3.65(WM.8)C0
Fingerprint ZyXEL ZyWALL 70 firewall (ZyNOS 3.65)
Class ZyXEL | ZyNOS | 3.X | firewall
SEQ(R=N)
OPS(O1=M200%O2=%O3=%O4=%O5=%O6=)
WIN(W1=2000%W2=0%W3=0%W4=0%W5=0%W6=0)
ECN(R=Y%DF=N%T=FE%TG=FF%W=0%O=%CC=Y%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# ZyXEL G-3000H WLAN access point, ZyNOS Firmware Version: V3.50(AAC.5)C0 | 03/28/2007
Fingerprint ZyXEL G-3000H WAP (ZyNOS 3.50)
Class ZyXEL | ZyNOS | 3.X | WAP
SEQ(SP=0-5%GCD=A000|14000|1E000|28000|32000|64000|C8000|12C000|190000|1F4000%ISR=AB-B5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M200%O2=M200%O3=M200%O4=M200%O5=M200%O6=M200)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FE%TG=FF%W=400%O=M200%CC=N%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# ZyWALL 2 Plus, Bootbase Version V1.12, Firmware Version V4.04(XU.2)
# Zyxel Zywall 70 UTM
# zyxel zywall 5
Fingerprint ZyXEL ZyWALL 2, 5, or 70 firewall (ZyNOS 4.04)
Class ZyXEL | ZyNOS | 4.X | firewall
SEQ(SP=0-B%GCD=A000|14000|1E000|28000|32000|64000|C8000|12C000|190000|1F4000%ISR=AB-B5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M200%O2=M200%O3=M200%O4=M200%O5=M200%O6=M200)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FE%TG=FF%W=2000%O=M200%CC=N%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# Zyxel Prestige 2602R-D1A
Fingerprint ZyXEL Prestige 2602R-D1A ADSL router
Class ZyXEL | ZyNOS || broadband router
SEQ(SP=D-17%GCD=A000|14000|1E000|28000|32000%ISR=AB-B5%TI=I%CI=I%II=I%SS=S%TS=U)
OPS(O1=M550%O2=M550%O3=M550%O4=M550%O5=M550%O6=M550)
WIN(W1=800%W2=800%W3=800%W4=800%W5=800%W6=800)
ECN(R=Y%DF=N%T=FE%TG=FF%W=800%O=M550%CC=N%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# ZyXEL Prestige 600 series router.
Fingerprint ZyXEL Prestige 600-series ADSL router
Class ZyXEL | ZyNOS || broadband router
SEQ(SP=0-5%GCD=68000|D0000|138000|1A0000|208000%ISR=AB-B5%TI=I%II=I%SS=S%TS=U)
OPS(O1=|M200%O2=|M200%O3=|M200%O4=|M200%O5=|M200%O6=|M200)
WIN(W1=0|400%W2=0|400%W3=0|400%W4=0|400%W5=0|400%W6=0|400)
ECN(R=Y%DF=N%T=FE%TG=FF%W=0|400%O=|M200%CC=N|Y%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O|Z%A=S+%F=AR|AS%RD=0%Q=)
T2(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
T3(R=Y%DF=N%T=FE%TG=FF%W=400%S=O%A=O|S+%F=AS%O=M200%RD=0%Q=)
T4(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# ZyXEL Prestige 660HW-61 ADSL router; ZyNOS F/W Version: V3.40(PE.10) | 10/28/2005
Fingerprint ZyXEL Prestige 660HW-61 ADSL router (ZyNOS 3.40)
Class ZyXEL | ZyNOS || broadband router
SEQ(SP=4-14%GCD=A000|14000|1E000|28000|32000|3C000%ISR=AF-B1%TI=I%II=I%SS=S%TS=U)
OPS(O1=M200%O2=M200%O3=M200%O4=M200%O5=M200%O6=M200)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FE%TG=FF%W=400%O=M200%CC=N%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# zyxel P-660HW-D1, ADSL+LAN+WLAN router with default configurations.
Fingerprint ZyXEL Prestige 660HW-D1 wireless ADSL router
Class ZyXEL | ZyNOS || broadband router
SEQ(SP=0-5%GCD=6E000|DC000|14A000|1B8000|226000%ISR=AB-B5%TI=I|RD%II=I%SS=S%TS=U)
OPS(O1=|M200%O2=|M200%O3=|M200%O4=|M200%O5=|M200%O6=|M200)
WIN(W1=400%W2=400%W3=400%W4=400%W5=400%W6=400)
ECN(R=Y%DF=N%T=FE%TG=FF%W=400%O=M200%CC=N%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O%A=O|S+%F=A|AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# zyxel zywall 2 plus
Fingerprint ZyXEL ZyWALL 2 Plus firewall
Class ZyXEL | ZyNOS || firewall
SEQ(SP=B-15%GCD=A000|14000|1E000|28000|32000%ISR=AB-B5%TI=I%II=I%SS=S%TS=U)
OPS(O1=|M584%O2=|M584%O3=|M584%O4=|M584%O5=|M584%O6=|M584)
WIN(W1=0|5B40%W2=0|5B40%W3=0|5B40%W4=0|5B40%W5=0|5B40%W6=0|5B40)
ECN(R=Y%DF=N%T=FE%TG=FF%W=0|5B40%O=|M584%CC=N|Y%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O|Z%A=S+%F=AR|AS%RD=0%Q=)
T2(R=N)
T3(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T4(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=Y%DF=N%T=FE%TG=FF%W=0%S=A%A=Z%F=R%O=%RD=0%Q=)
T7(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S%F=AR%O=%RD=0%Q=)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=D624%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)

# ZyWALL 5, Bootbase Version V1.08, Firmware Version V4.04(XD.0)
Fingerprint ZyXEL ZyWALL 5 firewall
Class ZyXEL | ZyNOS || firewall
SEQ(SP=0-12%GCD=A000|14000|1E000|28000|32000|6E000|DC000|14A000|1B8000|226000%ISR=AB-B5%TI=I%II=I%SS=S%TS=U)
OPS(O1=M200%O2=M200%O3=M200%O4=M200%O5=M200%O6=M200)
WIN(W1=2000%W2=2000%W3=2000%W4=2000%W5=2000%W6=2000)
ECN(R=Y%DF=N%T=FE%TG=FF%W=0|2000%O=|M200%CC=N|Y%Q=)
T1(R=Y%DF=N%T=FE%TG=FF%S=O%A=S+%F=AS%RD=0%Q=)
T2(R=N)
T3(R=N)
T4(R=N)
T5(R=Y%DF=N%T=FE%TG=FF%W=0%S=Z%A=S+%F=AR%O=%RD=0%Q=)
T6(R=N)
T7(R=N)
U1(DF=N%T=FE%TG=FF%IPL=38%UN=0%RIPL=G%RID=G%RIPCK=G%RUCK=G%RUD=G)
IE(DFI=N%T=FE%TG=FF%CD=S)
